{"text_format":"1","workbook":"xlsx","n_sheets":54,"sheets":["Performance_Outputs_0","Instructions","Definitions","General Information","1 - Multiple Buildings Details","2a - Schedules","2b - EFLH Calculator","3 - Multifamily Details","4 - Shading and Fenestration","5 - Opaque Assemblies","DropdownData","Envelope Assumptions","Envelope Lookup 90.1-2007","Envelope Lookup 90.1-2013","Envelope Lookup 90.1-2010","6a - Lighting Counts","6b - General Lighting","Lighting Assumptions","Lighting Assumptions 90.1-2007","Lighting Assumptions 90.1-2013","Lighting Assumptions 90.1-2010","7 - Process Loads","8 - Service Water Heating","SWH Lookup","9 - General HVAC","10a - Baseline Air-Side HVAC","10b - Proposed Air-Side HVAC","11 - Water-Side HVAC","P4P - LEED Inputs","Results from eQuest","ECM","Detailed Measures","Results from Trace","12 - Performance_Outputs_1","90.1-2004 Site EUI","90.1-2013 Site EUI","Revision Notes","Quality Assurance Checks","Performance_Outputs_0 old","Performance_Outputs_Summary","BPF 2013BM","BPF 2007","BPF 2010","BPF 2013","BPF 2016","Summary","Revision Log","Version Update Checklist","Rating System Descriptions","HVAC Lookup","HVAC Lookup 90.1-2007","HVAC Lookup 90.1-2013","HVAC Lookup 90.1-2010","District Energy Path 3"],"not_rendered":{"charts":6,"images":72,"macros":1,"external_links":21,"defined_names":1603,"comments":7,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Performance_Outputs_0","index":0,"n_rows":588,"n_cols":61,"rows_kept":588,"cut":false,"hidden":true,"merged":[[492,2,492,3],[492,6,492,7],[492,10,492,12],[513,2,513,3],[513,10,513,11],[304,2,304,3],[304,10,304,11],[325,2,325,3],[325,4,325,6],[325,7,325,9],[325,10,325,12],[345,2,345,3],[345,10,345,11],[379,2,379,3],[379,10,379,11],[487,2,487,3],[487,6,487,7],[487,10,487,12],[374,2,374,3],[374,10,374,11],[397,2,397,3],[397,10,397,11],[418,2,418,3],[418,10,418,11],[439,2,439,3],[439,10,439,11],[463,2,463,3],[463,10,463,11],[486,2,486,3],[486,6,486,7],[486,10,486,12],[393,2,393,3],[95,1,95,5],[95,9,95,10],[95,11,95,12],[112,1,112,5],[112,9,112,10],[112,11,112,12],[202,1,202,3],[202,10,202,12],[223,1,223,4],[223,10,223,12],[120,1,120,12],[123,1,123,12],[124,1,124,12],[126,1,126,12],[128,1,128,12],[130,1,130,12],[140,1,140,12],[160,1,161,2],[160,3,161,3],[160,4,161,4],[160,10,160,12],[161,10,161,12],[162,1,163,2],[162,3,163,3],[162,4,163,4],[162,10,162,12],[163,10,163,12],[164,1,165,2],[164,3,165,3],[164,4,165,4],[164,10,164,12],[165,10,165,12],[299,2,299,3],[299,10,299,11],[298,2,298,3],[298,10,298,11],[131,1,131,12],[135,1,135,12],[136,1,136,12],[137,1,137,12],[138,1,138,12],[139,1,139,12],[148,1,149,2],[148,3,149,3],[148,4,149,4],[148,10,148,12],[149,10,149,12],[150,1,151,2],[150,3,151,3],[154,1,155,2],[154,3,155,3],[154,4,155,4],[154,10,154,12],[155,10,155,12],[156,1,157,2],[156,3,157,3],[156,4,157,4],[156,10,156,12],[157,10,157,12],[158,1,159,2],[158,3,159,3],[158,4,159,4],[158,10,158,12],[159,10,159,12],[416,2,416,3],[416,10,416,11],[429,1,429,3],[429,10,429,11],[430,1,430,11],[432,1,433,1],[432,2,433,3],[90,1,90,5],[90,9,90,10],[90,11,90,12],[89,1,89,5],[89,9,89,10],[89,11,89,12],[39,1,39,12],[40,1,40,12],[42,1,42,3],[42,5,42,6],[52,1,52,3],[52,7,52,8],[52,9,52,12],[65,1,65,5],[65,7,65,8],[65,9,65,12],[50,1,50,3],[42,7,42,8],[42,9,42,12],[44,1,44,3],[44,9,44,12],[45,1,45,3],[45,9,45,12],[46,1,46,12],[373,2,373,3],[15,2,15,3],[16,2,16,3],[319,2,319,3],[319,4,319,6],[319,7,319,9],[319,10,319,12],[16,5,16,6],[16,7,16,9],[16,10,16,11],[17,2,17,3],[17,5,17,6],[17,7,17,9],[17,10,17,11],[32,1,32,10],[32,11,32,12],[18,2,18,3],[18,5,18,6],[18,7,18,9],[18,10,18,11],[31,1,31,10],[31,11,31,12],[19,2,19,3],[19,5,19,6],[19,7,19,9],[24,10,24,11],[25,2,25,3],[25,5,25,6],[25,7,25,9],[25,10,25,11],[50,7,50,8],[50,9,50,12],[51,1,51,3],[373,10,373,11],[320,2,320,3],[320,4,320,6],[320,7,320,9],[320,10,320,12],[340,2,340,3],[340,10,340,11],[338,2,338,3],[338,10,338,11],[351,1,351,3],[351,10,351,11],[353,1,353,11],[354,1,354,12],[370,2,370,3],[370,10,370,11],[372,2,372,3],[372,10,372,11],[367,10,367,12],[371,2,371,3],[371,10,371,11],[343,2,343,3],[332,1,332,11],[333,1,334,1],[333,2,334,3],[333,4,333,6],[333,7,333,9],[333,10,333,12],[326,10,326,12],[323,2,323,3],[323,4,323,6],[323,7,323,9],[323,10,323,12],[4,7,4,12],[6,1,6,12],[7,1,7,12],[8,1,8,12],[9,1,9,12],[10,1,10,12],[11,1,11,12],[12,1,12,12],[13,1,14,1],[13,2,14,3],[13,4,14,4],[13,5,14,6],[13,7,14,9],[13,10,13,12],[14,10,14,11],[19,10,19,11],[47,1,48,3],[47,4,47,6],[47,7,48,8],[47,9,48,12],[48,4,48,5],[21,2,21,3],[21,5,21,6],[21,7,21,9],[21,10,21,11],[20,2,20,3],[20,5,20,6],[20,7,20,9],[20,10,20,11],[24,2,24,3],[24,5,24,6],[24,7,24,9],[51,7,51,8],[51,9,51,12],[53,1,53,3],[53,7,53,8],[53,9,53,12],[66,1,66,8],[66,9,66,12],[55,1,55,3],[55,7,55,8],[55,9,55,12],[54,1,54,3],[54,7,54,8],[54,9,54,12],[58,1,58,3],[58,7,58,8],[58,9,58,12],[59,1,59,3],[59,7,59,8],[59,9,59,12],[67,1,67,11],[72,1,72,12],[75,1,75,12],[77,1,78,1],[77,2,78,2],[77,3,78,4],[77,5,78,5],[77,6,77,10],[81,3,81,4],[81,9,81,10],[81,11,81,12],[82,3,82,4],[82,9,82,10],[82,11,82,12],[77,11,78,12],[78,6,78,7],[78,9,78,10],[79,3,79,4],[80,3,80,4],[80,9,80,10],[80,11,80,12],[87,1,87,5],[87,9,87,10],[87,11,87,12],[88,1,88,5],[88,9,88,10],[88,11,88,12],[83,3,83,4],[83,9,83,10],[83,11,83,12],[84,1,84,4],[86,1,86,5],[86,9,86,10],[86,11,86,12],[105,1,105,5],[105,9,105,10],[105,11,105,12],[118,1,118,5],[118,9,118,10],[118,11,118,12],[101,1,101,4],[103,1,103,5],[103,9,103,10],[103,11,103,12],[104,1,104,5],[104,9,104,10],[104,11,104,12],[106,1,106,5],[106,9,106,10],[106,11,106,12],[107,1,107,5],[107,9,107,10],[107,11,107,12],[141,57,141,60],[142,1,142,2],[142,10,142,12],[144,1,145,2],[144,3,145,3],[144,4,145,4],[144,10,144,12],[145,10,145,12],[146,1,147,2],[146,3,147,3],[146,4,147,4],[146,10,146,12],[147,10,147,12],[150,4,151,4],[150,10,150,12],[151,10,151,12],[152,1,153,2],[152,3,153,3],[152,4,153,4],[152,10,152,12],[153,10,153,12],[166,1,167,2],[166,3,167,3],[166,4,167,4],[166,10,166,12],[167,10,167,12],[168,1,169,2],[168,3,169,3],[168,4,169,4],[168,10,168,12],[169,10,169,12],[170,1,171,2],[170,3,171,3],[170,4,171,4],[170,10,170,12],[171,10,171,12],[172,1,173,2],[172,3,173,3],[172,4,173,4],[172,10,172,12],[173,10,173,12],[191,10,191,12],[193,10,193,12],[186,1,187,2],[186,3,187,3],[186,4,187,4],[186,10,186,12],[187,10,187,12],[188,1,189,2],[188,3,189,3],[188,4,189,4],[188,10,188,12],[189,10,189,12],[174,1,175,2],[174,3,175,3],[174,4,175,4],[174,10,174,12],[175,10,175,12],[176,1,177,2],[176,3,177,3],[176,4,177,4],[176,10,176,12],[177,10,177,12],[178,1,179,2],[178,3,179,3],[178,4,179,4],[178,10,178,12],[179,10,179,12],[180,1,181,2],[180,3,181,3],[180,4,181,4],[180,10,180,12],[181,10,181,12],[233,1,233,12],[234,1,234,12],[235,1,235,12],[236,1,236,12],[237,1,237,12],[238,1,238,12],[215,1,215,4],[215,10,215,12],[216,1,216,4],[216,10,216,12],[229,1,229,5],[229,10,229,12],[217,1,217,4],[217,10,217,12],[218,1,218,4],[218,10,218,12],[220,1,220,4],[220,10,220,12],[221,1,221,4],[221,10,221,12],[239,57,239,60],[240,1,240,2],[240,10,240,11],[242,1,243,2],[242,3,243,3],[242,4,243,4],[242,9,243,9],[242,10,243,11],[242,12,243,12],[242,31,243,32],[244,31,245,32],[246,1,247,2],[246,3,247,3],[246,4,247,4],[246,9,247,9],[246,10,247,11],[246,12,247,12],[246,31,247,32],[244,1,245,2],[244,3,245,3],[244,4,245,4],[244,9,245,9],[244,10,245,11],[244,12,245,12],[248,31,249,32],[250,1,251,2],[250,3,251,3],[250,4,251,4],[250,9,251,9],[250,10,251,11],[250,12,251,12],[250,31,251,32],[248,1,249,2],[248,3,249,3],[248,4,249,4],[248,9,249,9],[248,10,249,11],[248,12,249,12],[252,31,253,32],[254,1,255,2],[254,3,255,3],[254,4,255,4],[254,9,255,9],[254,10,255,11],[254,12,255,12],[254,31,255,32],[252,1,253,2],[252,3,253,3],[252,4,253,4],[252,9,253,9],[252,10,253,11],[252,12,253,12],[256,31,257,32],[258,1,259,2],[258,3,259,3],[258,4,259,4],[258,9,259,9],[258,10,259,11],[258,12,259,12],[258,31,259,32],[256,1,257,2],[256,3,257,3],[256,4,257,4],[256,9,257,9],[256,10,257,11],[256,12,257,12],[260,31,261,32],[262,1,263,2],[262,3,263,3],[262,4,263,4],[262,9,263,9],[262,10,263,11],[262,12,263,12],[262,31,263,32],[260,1,261,2],[260,3,261,3],[260,4,261,4],[260,9,261,9],[260,10,261,11],[260,12,261,12],[264,31,265,32],[266,1,267,2],[266,3,267,3],[266,4,267,4],[266,9,267,9],[266,10,267,11],[266,12,267,12],[266,31,267,32],[264,1,265,2],[264,3,265,3],[264,4,265,4],[264,9,265,9],[264,10,265,11],[264,12,265,12],[268,31,269,32],[270,1,271,2],[270,3,271,3],[270,4,271,4],[270,9,271,9],[270,10,271,11],[270,12,271,12],[270,31,271,32],[268,1,269,2],[268,3,269,3],[268,4,269,4],[268,9,269,9],[268,10,269,11],[268,12,269,12],[286,31,287,32],[284,1,285,2],[284,3,285,3],[284,4,285,4],[284,9,285,9],[284,10,285,11],[284,12,285,12],[272,31,273,32],[274,1,275,2],[274,3,275,3],[274,4,275,4],[274,9,275,9],[274,10,275,11],[274,12,275,12],[274,31,275,32],[272,1,273,2],[272,3,273,3],[272,4,273,4],[272,9,273,9],[272,10,273,11],[272,12,273,12],[276,31,277,32],[278,1,279,2],[278,3,279,3],[278,4,279,4],[278,9,279,9],[278,10,279,11],[278,12,279,12],[278,31,279,32],[276,1,277,2],[276,3,277,3],[276,4,277,4],[288,31,289,32],[292,1,293,1],[292,2,293,3],[292,4,292,6],[292,7,292,9],[292,10,292,12],[293,10,293,11],[288,1,289,2],[288,3,289,3],[288,4,289,4],[288,9,289,9],[288,10,289,11],[288,12,289,12],[280,31,281,32],[282,1,283,2],[282,3,283,3],[282,4,283,4],[282,9,283,9],[282,10,283,11],[282,12,283,12],[282,31,283,32],[280,1,281,2],[280,3,281,3],[280,4,281,4],[280,9,281,9],[280,10,281,11],[280,12,281,12],[284,31,285,32],[286,1,287,2],[286,3,287,3],[286,4,287,4],[286,9,287,9],[342,2,342,3],[342,10,342,11],[316,2,316,3],[316,4,316,6],[316,7,316,9],[316,10,316,12],[317,2,317,3],[317,4,317,6],[317,7,317,9],[317,10,317,12],[310,1,310,3],[310,10,310,11],[313,1,313,11],[314,1,314,3],[314,4,314,6],[314,7,314,9],[314,10,314,12],[318,2,318,3],[318,4,318,6],[318,7,318,9],[318,10,318,12],[409,1,409,11],[411,1,412,1],[411,2,412,3],[411,4,411,6],[411,7,411,9],[411,10,411,12],[396,2,396,3],[396,10,396,11],[398,2,398,3],[398,10,398,11],[401,2,401,3],[333,13,333,15],[334,10,334,11],[336,2,336,3],[336,10,336,11],[337,2,337,3],[337,10,337,11],[367,13,367,15],[368,10,368,11],[359,2,359,3],[360,2,360,3],[362,1,362,3],[363,2,363,3],[364,2,364,3],[366,1,366,3],[355,1,356,1],[355,2,356,3],[355,4,355,6],[355,7,355,9],[355,10,355,11],[358,1,358,3],[367,1,368,1],[419,10,419,11],[420,2,420,3],[420,10,420,11],[421,2,421,3],[421,10,421,11],[422,2,422,3],[422,10,422,11],[423,2,423,3],[423,10,423,11],[444,2,444,3],[444,10,444,11],[390,13,390,15],[391,10,391,11],[385,1,385,3],[385,10,385,11],[386,1,386,3],[388,1,388,12],[390,1,391,1],[390,2,391,3],[390,4,390,6],[390,7,390,9],[390,10,390,12],[411,13,411,15],[412,10,412,11],[414,2,414,3],[414,10,414,11],[415,2,415,3],[415,10,415,11],[395,2,395,3],[395,10,395,11],[408,1,408,3],[408,10,408,11],[451,1,451,11],[452,1,452,9],[452,10,452,12],[432,13,432,15],[433,10,433,11],[435,2,435,3],[435,10,435,11],[436,2,436,3],[436,10,436,11],[438,2,438,3],[438,10,438,11],[440,2,440,3],[440,10,440,11],[441,2,441,3],[441,10,441,11],[442,2,442,3],[442,10,442,11],[432,4,432,6],[432,7,432,9],[432,10,432,12],[443,2,443,3],[443,10,443,11],[447,2,447,3],[447,10,447,11],[448,2,448,3],[448,10,448,11],[449,2,449,3],[449,10,449,11],[437,2,437,3],[437,10,437,11],[450,1,450,3],[450,10,450,11],[456,13,456,15],[457,10,457,11],[459,2,459,3],[459,10,459,11],[460,2,460,3],[460,10,460,11],[453,1,453,9],[453,10,453,12],[456,1,457,1],[456,2,457,3],[456,4,456,6],[456,7,456,9],[456,10,456,12],[478,13,478,15],[479,6,479,7],[479,10,479,12],[481,2,481,3],[481,6,481,7],[481,10,481,12],[461,2,461,3],[461,10,461,11],[474,1,474,3],[474,10,474,11],[477,1,477,12],[478,1,479,1],[478,2,479,3],[478,4,478,7],[478,8,478,12],[462,2,462,3],[462,10,462,11],[464,2,464,3],[464,10,464,11],[465,10,465,11],[466,2,466,3],[466,10,466,11],[467,2,467,3],[484,2,484,3],[484,6,484,7],[484,10,484,12],[485,2,485,3],[485,6,485,7],[485,10,485,12],[482,1,482,3],[482,6,482,7],[482,10,482,12],[483,2,483,3],[483,6,483,7],[483,10,483,12],[468,2,468,3],[468,10,468,11],[467,10,467,11],[471,2,471,3],[471,10,471,11],[472,2,472,3],[472,10,472,11],[473,2,473,3],[473,10,473,11],[519,1,519,3],[519,10,519,11],[520,1,520,11],[521,1,521,11],[525,1,525,4],[525,5,525,7],[525,8,525,12],[504,2,504,3],[504,10,504,11],[505,2,505,3],[505,10,505,11],[506,2,506,3],[506,10,506,11],[508,2,508,3],[508,10,508,11],[507,2,507,3],[507,10,507,11],[511,2,511,3],[511,10,511,11],[546,1,549,1],[551,1,551,7],[551,8,551,12],[552,1,552,7],[552,8,552,12],[553,1,553,7],[553,8,553,12],[560,1,560,7],[560,8,560,12],[561,1,561,7],[561,8,561,12],[528,8,528,12],[529,1,529,4],[529,5,529,12],[530,2,530,6],[526,1,526,4],[526,5,526,7],[526,8,526,12],[527,1,527,4],[527,5,527,7],[527,8,527,12],[532,1,533,1],[534,1,535,1],[536,1,537,1],[537,3,537,4],[538,1,543,1],[544,1,545,1],[545,3,545,4],[528,1,528,4],[528,5,528,7],[566,1,566,7],[566,8,566,12],[567,1,567,7],[567,8,567,12],[568,1,568,7],[568,8,568,12],[563,1,563,7],[563,8,563,12],[564,1,564,7],[564,8,564,12],[565,1,565,7],[565,8,565,12],[554,1,554,7],[554,8,554,12],[555,1,555,7],[555,8,555,12],[556,1,556,7],[556,8,556,12],[183,10,183,12],[184,1,185,2],[184,3,185,3],[184,4,185,4],[184,10,184,12],[185,10,185,12],[190,1,191,2],[190,3,191,3],[190,4,191,4],[190,10,190,12],[571,1,571,7],[571,8,571,12],[578,1,578,7],[578,8,578,12],[579,1,579,7],[579,8,579,12],[580,1,580,7],[580,8,580,12],[575,1,575,7],[575,8,575,12],[576,1,576,7],[576,8,576,12],[577,1,577,7],[577,8,577,12],[562,1,562,7],[562,8,562,12],[557,1,557,7],[557,8,557,12],[558,1,558,7],[558,8,558,12],[559,1,559,7],[559,8,559,12],[569,1,569,7],[569,8,569,12],[570,1,570,7],[570,8,570,12],[469,10,469,11],[493,2,493,3],[493,6,493,7],[493,10,493,12],[514,2,514,3],[514,10,514,11],[91,1,91,5],[91,9,91,10],[91,11,91,12],[108,1,108,5],[108,9,108,10],[108,11,108,12],[198,1,198,3],[198,10,198,12],[219,1,219,4],[219,10,219,12],[93,11,93,12],[109,1,109,5],[109,9,109,10],[109,11,109,12],[110,1,110,5],[110,9,110,10],[110,11,110,12],[199,1,199,3],[182,1,183,2],[182,3,183,3],[182,4,183,4],[182,10,182,12],[587,1,587,7],[587,8,587,12],[584,1,584,7],[584,8,584,12],[585,1,585,7],[585,8,585,12],[586,1,586,7],[586,8,586,12],[581,1,581,7],[581,8,581,12],[582,1,582,7],[582,8,582,12],[583,1,583,7],[583,8,583,12],[572,1,572,7],[572,8,572,12],[573,1,573,7],[573,8,573,12],[574,1,574,7],[574,8,574,12],[199,10,199,12],[200,1,200,3],[200,10,200,12],[209,1,209,5],[209,10,209,12],[212,1,212,5],[300,2,300,3],[300,10,300,11],[321,2,321,3],[321,4,321,6],[321,7,321,9],[321,10,321,12],[341,2,341,3],[341,10,341,11],[375,2,375,3],[375,10,375,11],[301,2,301,3],[301,10,301,11],[302,2,302,3],[302,10,302,11],[322,2,322,3],[322,4,322,6],[322,7,322,9],[326,4,326,6],[326,7,326,9],[367,2,368,3],[367,4,367,6],[367,7,367,9],[346,2,346,3],[346,10,346,11],[339,2,339,3],[339,10,339,11],[194,1,194,3],[194,10,194,12],[195,1,195,3],[195,10,195,12],[208,1,208,5],[208,10,208,12],[488,2,488,3],[488,6,488,7],[488,10,488,12],[509,2,509,3],[509,10,509,11],[22,2,22,3],[22,5,22,6],[22,7,22,9],[22,10,22,11],[23,2,23,3],[23,5,23,6],[23,7,23,9],[23,10,23,11],[56,1,56,3],[56,7,56,8],[56,9,56,12],[57,1,57,3],[57,7,57,8],[57,9,57,12],[92,1,92,5],[92,9,92,10],[92,11,92,12],[93,1,93,5],[93,9,93,10],[343,10,343,11],[376,2,376,3],[489,2,489,3],[489,6,489,7],[489,10,489,12],[490,2,490,3],[490,6,490,7],[490,10,490,12],[510,2,510,3],[510,10,510,11],[305,2,305,3],[305,10,305,11],[326,2,326,3],[400,10,400,11],[393,10,393,11],[394,2,394,3],[394,10,394,11],[498,1,498,3],[498,6,498,7],[498,10,498,12],[501,1,502,1],[501,2,502,3],[501,4,501,6],[501,7,501,9],[501,10,501,12],[502,10,502,11],[322,10,322,12],[376,10,376,11],[377,2,377,3],[377,10,377,11],[399,2,399,3],[399,10,399,11],[400,2,400,3],[465,2,465,3],[26,2,26,3],[26,5,26,6],[26,7,26,9],[26,10,26,11],[60,1,60,3],[60,7,60,8],[60,9,60,12],[96,1,96,5],[96,9,96,10],[96,11,96,12],[113,1,113,5],[113,9,113,10],[113,11,113,12],[203,1,203,3],[203,10,203,12],[224,1,224,4],[224,10,224,12],[196,1,196,3]],"merged_total":1206,"flags":["merged_cut"]}
["G"]
["G","Performance Rating Method Outputs"]
["G"]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Multiplier"]
["G","Energy Model ID",null,null,null,null,null,{"$f":"INDEX(MBD_EMI_Table,2,1)","v":0},null,null,null,null,null,null,null,null,{"$f":"IFERROR(INDEX(MBD_EMI_Table,MATCH($H$5,MBD_EMI_Index,0),MATCH('1 - Multiple Buildings Details'!$J$16,MBD_EMI_Hdr,0)),\"ERROR\")","v":0}]
["G"]
["G","Energy Sources"]
["G"]
["G","Enter each energy source serving the project, the units for the energy consumption and demand, and the associated utility rate name and tariff structure. Default EIA Rates may be used in lieu of local utility rates at the discretion of the energy modeler.  All project energy types and the demand and consumption units must be entered before entering energy simulation output data. Also enter the units used to report energy consumption totals (the sum of all energy types) for site energy consumption and source energy consumption (generally, the IP units are Btu x 10^6, the SI site energy units are kWh, and the SI source energy units are MJ).\n\n\n",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","DES Path 1: If the project is using campus or district thermal energy using ASHRAE 90.1-2010 without Addenda (District Energy Modeling Path 1), select District Cooling, District Hot Water, or District Steam as applicable and all other energy sources serving the building "]
["G","DES Path 2: If the project is modeling campus or district thermal energy using the Full DES Performance Accounting method (District Energy Modeling Path 2) include each energy source serving the building except District Energy, AND include each energy source in the district or campus plant (e.g. electricity, natural gas, etc.) if different from the energy sources serving the building. Do not select District Cooling, District Hot Water, or District Steam. "]
["G","DES Path 3: If the project is modeling campus or district thermal energy using the Streamlined DES Accounting Method (District Energy Modeling Path 3), select District Cooling, District Hot Water, or District Steam as applicable, AND each energy source serving the building, AND each energy source in the district or campus plant if different from the energy sources serving the building (e.g. electricity, natural gas, etc.).\n"]
["G"]
["G","Energy Type","Energy Consumption Units",null,"Demand Units","Utility Rate Name",null,"Utility Rate Structure",null,null,"Unit Conversion Factors"]
["G",null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Energy Type Consumption Units to Site Energy Consumption (\",PO_SiteUnits,\")\")","v":"Energy Type Consumption Units to Site Energy Consumption (Btu x 10^6)"},null,{"$f":"CONCATENATE(\"Energy Type Consumption Units to Source Energy Consumption (\",PO_SourceUnits,\")\")","v":"Energy Type Consumption Units to Source Energy Consumption (Btu x 10^6)"}]
["G","Energy_Type","Energy_Consumption_Units",null,"Demand_Units","Utility_Rate_Name",null,"Utility_Rate_Structure",null,null,"Site_Energy_Conversion_Factor",null,"Source_Energy_Conversion_Factor"]
["G","Electricity","kWh",null,"kW",null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(\"kBtu\",EnergyUnitsTable,3,FALSE)/VLOOKUP(PO_SiteUnits,EnergyUnitsTable,3,FALSE)*VLOOKUP($C17,EnergyUnitsTable,3,FALSE),\"\")","v":3.4120000000000001E-3},null,{"$f":"IFERROR(VLOOKUP(\"kBtu\",EnergyUnitsTable,3,FALSE)/VLOOKUP(PO_SourceUnits,EnergyUnitsTable,3,FALSE)*VLOOKUP($C17,EnergyUnitsTable,3,FALSE)*VLOOKUP($B17,FuelTypesTable,2,FALSE),\"\")","v":8.7005999999999993E-3}]
["G","Natural Gas","therm",null,"Btuh x 10^6",null,null,null,null,null,0.1,null,0.10500000000000001]
["G","District Cooling","MWh",null,"MW",null,null,null,null,null,3.4119999999999999,null,3.4119999999999999]
["G","District Cooling","MWh",null,"MW",null,null,null,null,null,3.4119999999999999,null,3.4119999999999999]
["G","District Cooling","MWh",null,"MW",null,null,null,null,null,3.4119999999999999,null,3.4119999999999999]
["G","District Cooling","MWh",null,"MW",null,null,null,null,null,3.4119999999999999,null,3.4119999999999999]
["G","District Cooling","MWh",null,"MW",null,null,null,null,null,3.4119999999999999,null,3.4119999999999999]
["G","District Cooling","MWh",null,"MW",null,null,null,null,null,3.4119999999999999,null,3.4119999999999999]
["G","District Cooling","MWh",null,"MW",null,null,null,null,null,3.4119999999999999,null,3.4119999999999999]
["G","District Cooling","MWh",null,"MW",null,null,null,null,null,3.4119999999999999,null,3.4119999999999999]
["G","District Cooling","MWh",null,"MW",null,null,null,null,null,3.4119999999999999,null,3.4119999999999999]
["G","District Cooling","MWh",null,"MW",null,null,null,null,null,3.4119999999999999,null,3.4119999999999999]
["G","District Cooling","MWh",null,"MW",null,null,null,null,null,3.4119999999999999,null,3.4119999999999999]
["G","District Cooling","MWh",null,"MW",null,null,null,null,null,3.4119999999999999,null,3.4119999999999999]
["G","District Cooling","MWh",null,"MW",null,null,null,null,null,3.4119999999999999,null,3.4119999999999999]
["G","Site energy consumption units used to report energy consumption totals (sum of energy types)",null,null,null,null,null,null,null,null,null,{"$f":"IF(SI_IP_Units=\"SI\",\"MWh\",\"Btu x 10^6\")","v":"Btu x 10^6"}]
["G","Source energy consumption units used to report energy consumption totals (sum of energy types)",null,null,null,null,null,null,null,null,null,{"$f":"IF(SI_IP_Units=\"SI\",\"MWh\",\"Btu x 10^6\")","v":"Btu x 10^6"}]
["G"]
["G"]
["G","On-Site Renewable Energy Production"]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Site-generated renewable energy?"]
["G","The project building uses on-site renewable energy systems. (Optional)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,true]
["G"]
["G","Table: On-Site Renewable energy source summary"]
["G","Renewable energy production should be reported in the table below. Note: This calculator will automatically reduce the proposed energy consumption and cost to accurately reflect the revised results. Therefore, any site-generated renewable energy production should NOT be included in the Performance Rating Method tables below.\n\nSelect the site-generated renewable energy source. Enter the rated capacity of the site-generated renewable source including the units (e.g. for photovoltaics 10 kW). Include all relevant capacities (i.e for solar thermal, both the storage tank capacity and the solar thermal panel capacity).\n\nThe cost of the Site-generated renewable cost will be automatically determined using the virtual rate once the output data (consumption and cost) is entered below. The cost may be overridden by the user, however this may generate an issue on the Quality Checks and the user should be prepared to justify the entered cost value."]
["G"]
["G","On-Site Renewable Source",null,null,"Offset \nEnergy Type","Rated Capacity ",null,"Annual Site Energy Generated",null,"Annual Energy Cost Offset with \nSite-Generated Renewables \n($/year)",null,null,null,null,null,null,null,null,null,"Default_Cost","Rate_Variance"]
["G","Renewable_Source",null,null,"Offset_Energy_Type","Rated_Capacity",null,"Annual_Site_Energy",null,"Cost",null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion","EFLH","Default_Cost","Rate_Variance"]
["A","Photovoltaic system",null,null,"Electricity",null,{"$f":"IFERROR(IF(ISBLANK($E45),\"\",VLOOKUP($E45,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":"kW"},null,{"$f":"IFERROR(IF(ISBLANK($E45),\"\",VLOOKUP($E45,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":"kWh"},{"$f":"IFERROR($H45*VLOOKUP($E45,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},"","","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E45),\"\",VLOOKUP($E45,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($E45),\"\",VLOOKUP($E45,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3},{"$f":"IFERROR((H45*VLOOKUP(I45,EnergyUnitsTable,3,FALSE))/(F45*VLOOKUP(G45,DemandTable,3,FALSE)),\"\")","v":""},{"$f":"IFERROR($H45*VLOOKUP($E45,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(1-$J45/$T45,0)","v":0}]
[null,"Solar thermal system",null,null,"Natural Gas",null,{"$f":"IFERROR(IF(ISBLANK($E46),\"\",VLOOKUP($E46,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":"Btuh x 10^6"},null,{"$f":"IFERROR(IF(ISBLANK($E46),\"\",VLOOKUP($E46,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":"therm"},"","","","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E46),\"\",VLOOKUP($E46,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":0.1},{"$f":"IFERROR(IF(ISBLANK($E46),\"\",VLOOKUP($E46,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":0.10500000000000001},{"$f":"IFERROR((H46*VLOOKUP(I46,EnergyUnitsTable,3,FALSE))/(F46*VLOOKUP(G46,DemandTable,3,FALSE)),\"\")","v":""},{"$f":"IFERROR($H46*VLOOKUP($E46,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(1-$J46/$T46,0)","v":0}]
[null,"Renewable Summary"]
[null,"Offset Energy Type",null,null,"Annual Site Energy Generated",null,null,{"$f":"CONCATENATE(\"Annual Source Energy Generated\n (\", PO_SourceUnits, \")\")","v":"Annual Source Energy Generated\n (Btu x 10^6)"},null,"Annual Energy Cost Offset with \nSite-Generated Renewables \n($/year)"]
[null,null,null,null,"Units per Energy Type",null,{"$f":"CONCATENATE(\"Units = \", PO_SiteUnits,\")\")","v":"Units = Btu x 10^6)"}]
[null,"Energy_Type",null,null,"Site_Energy_Ind_Units","Site_Ind_Units","Site_Energy_Same_Units","Source_Energy",null,"Cost",null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
[null,{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},null,null,{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,SUMIF(INDEX(PO_renewable_table,0,MATCH($E$44,PO_renewable_hdr,0)),$B51,INDEX(PO_renewable_table,0,MATCH($H$44,PO_renewable_hdr,0))),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(ISBLANK($B51),\"\",VLOOKUP($B51,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":"kWh"},{"$f":"IFERROR($E51*$Q51,\"\")","v":0},{"$f":"IFERROR($E51*$R51,\"\")","v":0},null,{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,SUMIF($E$45:$E$46,$B51,$J$45:$J$46),0),\"\")","v":0},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B51),\"\",VLOOKUP($B51,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B51),\"\",VLOOKUP($B51,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3}]
[null,"Natural Gas",null,null,0,"therm",0,0,null,0,null,null,null,null,null,null,0.1,0.10500000000000001]
[null,"District Cooling",null,null,0,"MWh",0,0,null,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,0,"MWh",0,0,null,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,0,"MWh",0,0,null,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,0,"MWh",0,0,null,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,0,"MWh",{"$f":"IFERROR($E57*$Q57,\"\")","v":0},{"$f":"IFERROR($E57*$R57,\"\")","v":0},null,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,0,"MWh",0,0,null,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,0,"MWh",0,0,null,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,0,"MWh",0,0,null,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,0,"MWh",0,0,null,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,0,"MWh",0,0,null,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
[null,{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},null,null,0,"MWh",0,0,null,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,0,"MWh",0,0,null,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,0,"MWh",0,0,null,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"Total",null,null,null,null,{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_2_Table,0,MATCH($G$50,PO_Enrgy_2_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_2_Table,0,MATCH($H$50,PO_Enrgy_2_Hdr,0))),\"\")","v":0},{"$f":"SUM(I50:I52)","v":0},{"$f":"IFERROR(SUM(J44:J46),\"\")","v":0}]
[null,"Percent renewable energy (by cost)",null,null,null,null,null,null,null,{"$f":"IF(Datacenter_Avg=TRUE,IFERROR($J66/$J$451,\"\"),IFERROR($J66/$J$386,\"\"))","v":""}]
["G"]
["G"]
["G","Exceptional Calculation Methods",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Exceptional Calculations?"]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,true]
["G","The building energy analysis includes exceptional calculation methods. (Optional)"]
["G","Data Centers:  If using the Data Center Calculator to document energy improvements in IT loads, the checkbox stating that the building energy analysis includes exceptional calculation methods must be checked.  In the table below, select the checkbox “Apply to Baseline?” for each end-use impacted, and provide:\n•  The completed Data Center Calculator (found under the prerequisite's \"Resources\" tab in the Credit Library), as well as copies of any other spreadsheets used to perform the calculations\n•  If energy efficiency credit is applied for any future IT equipment, electrical infrastructure, and/or for future server room cooling equipment that will serve unfinished spaces (meaning that the IT equipment, electrical infrastructure, and/or unfinished space cooling equipment will not be installed during Startup Occupancy), provide a binding Owner commitment letter and (for any tenants) sample lease agreements with binding tenant requirements that confirms that the future installed IT equipment will be at least as efficient as the equipment modeled in the Data Center Calculator. Note that the future equipment may not be modeled as being more efficient than the equipment installed for Startup occupancy.\n•  If taking credit for the impact of IT equipment load reductions on HVAC energy consumption, upload the simulation input summary and simulation output reports, and Performance Rating summary with the baseline model revised to include the baseline IT and electrical infrastructure from the Data Center Calculator.\n"]
["G"]
["G","Table: Exceptional calculation methods energy summary"]
["G","Report Exceptional calculation methods in the table below.\n\nSelect \"Add to Baseline\" if the exceptional calculation adjusts the Baseline building energy consumption and cost up, or \"Subtract from Proposed\" if the exceptional calculation adjusts the Proposed building energy consumption and cost down.\n\nThis calculator will automatically reduce the proposed energy consumption and cost, or increase the baseline energy consumption and cost to accurately reflect the revised results. Therefore, any exceptional calculation methods should NOT be included in the Performance Rating Method Compliance report below.  If any single Exceptional Calculation Method results in energy penalties for a given energy type (i.e. increased proposed case electricity energy usage, or decreased baseline case fossil fuel energy usage), that penalty should be entered as a negative number. If any single Exceptional Calculation Method affects more than one energy type, please add additional rows to capture the method's impact to that energy type. If taking credit for Data Center Equipment or Retail Process Loads, those savings must be recorded here and the supplemental spreadsheets associated with that equipment must be uploaded as part of the submittal documents.\n\nThe cost of the Exceptional Calculation Method will be automatically determined using the virtual rate once the output data (consumption and cost) is entered below. The cost may be overridden by the user, however this may generate an issue on the Quality Checks and the user should be prepared to justify the entered cost value."]
["G"]
["G","Exceptional \nCalculation \nNumber","Exceptional \nCalculation \nMethod ID","Energy Type(s)",null,"Add to Baseline?\nSubtract from Proposed?","Annual Energy Difference by Energy Type",null,null,null,null,"Annual Energy Cost Difference"]
["G",null,null,null,null,null,"Site Energy \n(Units per Energy Type)",null,{"$f":"CONCATENATE(\"Site Energy \n(Units = \", PO_SiteUnits,\")\")","v":"Site Energy \n(Units = Btu x 10^6)"},{"$f":"\"Source Energy Consumption \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Consumption \n(Btu x 10^6)"}]
["G","Ex_Calc_Number","Ex_Calc_ID","Energy_Type",null,"Add_Baseline_Subtract_Proposed","Site_Energy_Ind_Units","Site_Ind_Units","Site_Energy_Same_Units","Source_Energy",null,"Cost",null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",null,"Default_Cost","Rate_Variance"]
["B",null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D81),\"\",VLOOKUP($D81,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D81,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)*$G81,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D81,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)*$G81,\"\")","v":""},null,{"$f":"IFERROR($G81*IF($F81=\"Subtract from Proposed\",VLOOKUP($D81,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D81,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D81),\"\",VLOOKUP($D81,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($D81),\"\",VLOOKUP($D81,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR($G81*IF($F81=\"Subtract from Proposed\",VLOOKUP($D81,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D81,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(1-$J81/$T81,0)","v":0},null,null,null,null,null,null,""]
[null,1,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D82),\"\",VLOOKUP($D82,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D82,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)*$G82,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D82,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)*$G82,\"\")","v":""},null,{"$f":"IFERROR($G82*IF($F82=\"Subtract from Proposed\",VLOOKUP($D82,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D82,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D82),\"\",VLOOKUP($D82,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($D82),\"\",VLOOKUP($D82,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR($G82*IF($F82=\"Subtract from Proposed\",VLOOKUP($D82,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D82,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(1-$J82/$T82,0)","v":0}]
[null,2,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D83),\"\",VLOOKUP($D83,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D83,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)*$G83,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D83,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)*$G83,\"\")","v":""},null,{"$f":"IFERROR($G83*IF($F83=\"Subtract from Proposed\",VLOOKUP($D83,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D83,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D83),\"\",VLOOKUP($D83,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($D83),\"\",VLOOKUP($D83,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR($G83*IF($F83=\"Subtract from Proposed\",VLOOKUP($D83,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D83,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(1-$J83/$T83,0)","v":0},null,null,null,null,null,null,""]
[null,3,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D84),\"\",VLOOKUP($D84,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D84,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)*$G84,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D84,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)*$G84,\"\")","v":""},null,{"$f":"IFERROR($G84*IF($F84=\"Subtract from Proposed\",VLOOKUP($D84,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D84,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D84),\"\",VLOOKUP($D84,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($D84),\"\",VLOOKUP($D84,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR($G84*IF($F84=\"Subtract from Proposed\",VLOOKUP($D84,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D84,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(1-$J84/$T84,0)","v":0},null,null,null,null,null,null,""]
[null,"Subtotals added to baseline"]
[null,"Energy_Type",null,null,null,null,"Site_Energy_Ind_Units","Site_Ind_Units","Site_Energy_Same_Units","Source_Energy",null,"Cost",null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
[null,{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($G$80,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$80,PO_ExCalc_Hdr,0)),$B87,INDEX(PO_ExCalc_Table,0,MATCH($F$80,PO_ExCalc_Hdr,0)),\"Add to Baseline\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(ISBLANK($B87),\"\",VLOOKUP($B87,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":"kWh"},{"$f":"IFERROR($G87*$Q87,\"\")","v":0},{"$f":"IFERROR($G87*$R87,\"\")","v":0},{"$f":"IFERROR($G87*$Q87,\"\")","v":0},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($L$80,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$80,PO_ExCalc_Hdr,0)),$B87,INDEX(PO_ExCalc_Table,0,MATCH($F$80,PO_ExCalc_Hdr,0)),\"Add to Baseline\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(M$81:M$84,$D$81:$D$84,$B87,$F$81:$F$84,\"Add to Baseline\"),\"\"),\"\")","v":0},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B87),\"\",VLOOKUP($B87,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B87),\"\",VLOOKUP($B87,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3}]
[null,"Natural Gas",null,null,null,null,0,"therm",0,0,0,0,0,null,null,null,0.1,0.10500000000000001]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",{"$f":"IFERROR($G93*$Q93,\"\")","v":0},{"$f":"IFERROR($G93*$R93,\"\")","v":0},{"$f":"IFERROR($G93*$Q93,\"\")","v":0},0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"Subtotals subtracted from proposed"]
[null,"Energy_Type",null,null,null,null,"Site_Energy_Ind_Units","Site_Ind_Units","Site_Energy_Same_Units","Source_Energy",null,"Cost",null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
[null,{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($G$80,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$80,PO_ExCalc_Hdr,0)),$B104,INDEX(PO_ExCalc_Table,0,MATCH($F$80,PO_ExCalc_Hdr,0)),\"Subtract from Proposed\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(ISBLANK($B104),\"\",VLOOKUP($B104,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":"kWh"},{"$f":"IFERROR($G104*$Q104,\"\")","v":0},{"$f":"IFERROR($G104*$R104,\"\")","v":0},{"$f":"IFERROR($G104*$Q104,\"\")","v":0},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($L$80,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$80,PO_ExCalc_Hdr,0)),$B104,INDEX(PO_ExCalc_Table,0,MATCH($F$80,PO_ExCalc_Hdr,0)),\"Subtract from Proposed\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(M$81:M$84,$D$81:$D$84,$B104,$F$81:$F$84,\"Add to Baseline\"),\"\"),\"\")","v":0},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B104),\"\",VLOOKUP($B104,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B104),\"\",VLOOKUP($B104,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3}]
[null,"Natural Gas",null,null,null,null,0,"therm",0,0,0,0,0,null,null,null,0.1,0.10500000000000001]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",{"$f":"IFERROR($G110*$Q110,\"\")","v":0},{"$f":"IFERROR($G110*$R110,\"\")","v":0},{"$f":"IFERROR($G110*$Q110,\"\")","v":0},0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"District Cooling",null,null,null,null,0,"MWh",0,0,0,0,0,null,null,null,3.4119999999999999,3.4119999999999999]
[null,"Total Exceptional Calculation Method Adjustment",null,null,null,null,null,null,{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_3_Table,0,MATCH($I86,PO_Enrgy_3_Hdr,0)),INDEX(PO_Enrgy_4_Table,0,MATCH($I103,PO_Enrgy_4_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_3_Table,0,MATCH($J86,PO_Enrgy_3_Hdr,0)),INDEX(PO_Enrgy_4_Table,0,MATCH($J103,PO_Enrgy_4_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(K$47:K$105),0)","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_3_Table,0,MATCH($L86,PO_Enrgy_3_Hdr,0)),INDEX(PO_Enrgy_4_Table,0,MATCH($L103,PO_Enrgy_4_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(M$47:M$105),0)","v":0}]
["G"]
["G","Upload: Exceptional calculation \nProvide a detailed narrative explaining the exceptional calculation method(s) performed, including all end-uses affected by the exceptional calculation method. If more than one exceptional calculation method is used, the exceptional calculation ID in the narrative must match the values listed in the table above.  The exceptional calculation method must include:\n•  Step-by-step documentation of the exceptional calculation method(s) performed detailed enough to reproduce the results\n•  Copies of all spreadsheets used to perform the calculations, or simulation energy model input and output summaries documenting the calculations performed\n•  For methods that significantly impact HVAC or refrigeration energy, the calculations shall be performed on a time step basis consistent with the simulation program used\n•  The Performance Rating calculated with and without the exceptional calculation method\n•  Documentation of the baseline and proposed assumptions. Documentation of baseline assumptions verify that the efficiency measure is not conventional practice by including, but not limited to:\n    ○  a recently published study (published within five years of the project registration date) with researched tabulations or monitored data establishing standard practice for the given application in similar newly constructed facilities\n    ○  a new construction utility or government program that incentivizes the measure\n    ○  a document showing the systems used to perform the same function in other newly constructed facilities (for example, three similar facilities built within the past five years). These systems would be treated as the baseline system in the analysis, and evidence must be provided to demonstrate how the energy for the baseline and proposed buildings are determined \n    ○  use any of the prescriptive requirements from 90.1-2013 as the baseline requirement without further justification to substantiate conventional practice, but only for the specific component addressed by the prescriptive requirement"]
["G"]
["G","Energy Modeling Output Reporting Method"]
["G","Select one of the following before entering any simulation output data:\nNote: If this is selected after data has been entered in the tables below, the energy types, baseline energy by end use, and baseline cost data will be cleared from these tables."]
["G","Complete the baseline results for each of the four building orientations, in addition to the proposed results.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
["G"]
["G","Report the averaged baseline results, in addition to the proposed results. In the EAp2 form uploads, provide simulation output summaries from the simulation output software that include the energy consumption by end-use, total energy consumption by energy type, and total energy cost by energy type, reported separately  for each of the four baseline rotations, and the average baseline energy consumption by end-use, energy consumption by energy type, and energy cost by energy type. (The simulation software must report this average as a standard report in order to use this option)."]
["G"]
["G","The project is not required to simulate four baseline orientations because (a) the vertical fenestration area on each orientation varies by less than 5%, (b) the energy code used does not require simulation of four baseline orientations, or (c) the building is more than 50% existing based on conditioned floor area. Report the non-rotated baseline results, in addition to the proposed results.\n"]
["G"]
["G","The project is not required to simulate four baseline orientations because the building orientation is dictated by site consideration, as allowed by Table G3.1.5 (a) (baseline) Exception 1. Report the non-rotated baseline results, in addition to the proposed results."]
["G"]
["G"]
["G","Performance Rating Method Compliance Report"]
["G","Table: Baseline energy summary by end use"]
["G","Complete the table below for the proposed, providing information on baseline energy consumption and peak demand by end-use. This data will be used to autopopulate the Performance tables below. If an end-use has two energy types (e.g. proposed space heating includes both fossil fuel and electric), enter the end-use twice in the table, and list the two different energy types.When linking to the Results from eQUEST or Results from Trace tabs, scroll to the right to customize the linked rows/columns for each end-use. For those using the 'Results from Trace' tab, note that TRACE uses a unit conversion factor of 3.413 btu/W, wherease this worksheet uses a conversion factor of 3.412 btu/W. As a result, model results will differ by 0.03% versus those shown in Trace output reports."]
["G","ASHRAE 90.1-2010 without Addenda (District Energy Modeling Path 1): Report the district energy type (District Cooling, District Hot Water, or District Steam) for the cooling and heating end-uses as applicable for both the baseline and proposed.  "]
["G","Full DES Performance Accounting method (District Energy Modeling Path 2): Report the baseline energy as if the thermal energy is produced in the building.  Report the proposed energy used to generate and distribute the district thermal energy serving the building based on calculated average district thermal efficiencies (e.g. report the electricity used to generate and distribute chilled water to the building).\n"]
["G","Streamlined DES Accounting Method (District Energy Modeling Path 3): Report the energy type (District Cooling, District Hot Water, or District Steam for the cooling and heating end-uses as applicable for both the baseline and proposed. "]
["G","Data Centers: The energy consumption for IT equipment must be metered and reported separately from other end-uses in the energy model, and in the tables below to allow the proper determination of the PUE. Complete the table below for the baseline using the full build-out IT loads for the proposed design.\n"]
["G","Retail: The energy consumption for cooking, refrigeration, and kitchen ventilation fans must be metered and reported separately from other end-uses in the energy model and in the tables below. Energy savings or consumption attributable to unregulated equipment, other than Commercial Kitchen Equipment, Supermarket Refrigeration, Walk-in Coolers and Freezers, or Commercial Kitchen Ventilation listed in Tables 1 – 4 of the LEED v4 BD+C:Retail and ID+C: Retail Rating System Appendix 3 must be claimed via Exceptional Calculation Methodology."]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Software Links"]
["G","End Use",null,"Unregulated?","Energy Type","Units of \nAnnual Energy and Peak Demand","Baseline 0° rotation","Baseline 90° rotation","Baseline 180° rotation","Baseline 270° rotation","Baseline Design Total\n (Average of 4 rotations)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"\"Results from eQUEST\" End Use Column","\"Results from Trace\" End Use Label","\"Results from Trace\" End Use Fuel Label","\"Results from Trace\" End Use Row"]
["G","End_Use",null,"Unregulated","Energy_Type","Energy_Units","Baseline_0_Rotation","Baseline_90_Rotation","Baseline_180_Rotation","Baseline_270_Rotation","Base_Consumption_Demand",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion","EFLH"]
["G","Interior lighting",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E145),\"\",\"Consumption (\" & VLOOKUP($E145,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF145&\"8\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!C\"&$BI145)/$Q145,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF145&\"9\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!D\"&$BI145)/$Q145,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF145&\"10\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!E\"&$BI145)/$Q145,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF145&\"11\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!F\"&$BI145)/$Q145,\"\")),\"\")","v":0},{"$f":"IFERROR(AVERAGEIF(G145:J145,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E145),\"\",VLOOKUP($E145,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($E145),\"\",VLOOKUP($E145,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3},{"$f":"IFERROR(IF(FIND(\"Consumption\",F145),(K145*VLOOKUP(MID(F145,FIND(\"(\",F145)+1,LEN(F145)-FIND(\"(\",F145)-1),EnergyUnitsTable,3,FALSE))/(K146*VLOOKUP(MID(F146,FIND(\"(\",F146)+1,LEN(F146)-FIND(\"(\",F146)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L","Lighting - Conditioned","Electricity",{"$f":"IF(BG145<>\"\",IFERROR(MATCH(BG145&BH145,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":7}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E145),\"\",\"Demand (\" & VLOOKUP($E145,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},0,0,0,0,{"$f":"IFERROR(AVERAGEIF(G146:J146,\"<>0\"),\"\")","v":""},null,null,null,null,null,"","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y"]
["G","Exterior lighting",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E147),\"\",\"Consumption (\" & VLOOKUP($E147,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},0,0,0,0,"",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W","Stand-alone Base Utilities","Electricity",{"$f":"IF(BG147<>\"\",IFERROR(MATCH(BG147&BH147,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":15}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E147),\"\",\"Demand (\" & VLOOKUP($E147,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},0,0,0,0,"",null,null,null,null,null,"","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AJ"]
["G","Space heating",null,null,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E149),\"\",\"Consumption (\" & VLOOKUP($E149,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (therm)"},0,0,0,0,"",null,null,null,null,null,0.1,0.10500000000000001,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BA","Space Heating","Gas",{"$f":"IF(BG149<>\"\",IFERROR(MATCH(BG149&BH149,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":9}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E149),\"\",\"Demand (\" & VLOOKUP($E149,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (Btuh x 10^6)"},"","","","","",null,null,null,null,null,"","",""]
["G","Space cooling",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E151),\"\",\"Consumption (\" & VLOOKUP($E151,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},0,0,0,0,"",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"P","Space Cooling","Electricity",{"$f":"IF(BG151<>\"\",IFERROR(MATCH(BG151&BH151,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":10}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E151),\"\",\"Demand (\" & VLOOKUP($E151,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},0,0,0,0,"",null,null,null,null,null,"","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AC"]
["G","Pumps",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E153),\"\",\"Consumption (\" & VLOOKUP($E153,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},0,0,0,0,"",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R","Pumps","Electricity",{"$f":"IF(BG153<>\"\",IFERROR(MATCH(BG153&BH153,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":11}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E153),\"\",\"Demand (\" & VLOOKUP($E153,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},0,0,0,0,"",null,null,null,null,null,"","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AE"]
["G","Heat rejection",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E155),\"\",\"Consumption (\" & VLOOKUP($E155,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},0,0,0,0,"",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Q","Heat Rejection","Electricity",{"$f":"IF(BG155<>\"\",IFERROR(MATCH(BG155&BH155,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":12}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E155),\"\",\"Demand (\" & VLOOKUP($E155,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},0,0,0,0,"",null,null,null,null,null,"","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AD"]
["G","Fans - interior ventilation",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E157),\"\",\"Consumption (\" & VLOOKUP($E157,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},0,0,0,0,"",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S","Fans - Conditioned","Electricity",{"$f":"IF(BG157<>\"\",IFERROR(MATCH(BG157&BH157,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":13}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E157),\"\",\"Demand (\" & VLOOKUP($E157,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},0,0,0,0,"",null,null,null,null,null,"","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AF"]
["G","Fans - parking garage",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E159),\"\",\"Consumption (\" & VLOOKUP($E159,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},"","","","","",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG159<>\"\",IFERROR(MATCH(BG159&BH159,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E159),\"\",\"Demand (\" & VLOOKUP($E159,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},"","","","","",null,null,null,null,null,"","",""]
["G","Service water heating",null,null,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E161),\"\",\"Consumption (\" & VLOOKUP($E161,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (therm)"},0,0,0,0,"",null,null,null,null,null,0.1,0.10500000000000001,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BH","Stand-alone Base Utilities","Gas",{"$f":"IF(BG161<>\"\",IFERROR(MATCH(BG161&BH161,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":16}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E161),\"\",\"Demand (\" & VLOOKUP($E161,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (Btuh x 10^6)"},"","","","","",null,null,null,null,null,"","",""]
["G","Receptacle equipment",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E163),\"\",\"Consumption (\" & VLOOKUP($E163,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},0,0,0,0,"",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N","Receptacles - Conditioned","Electricity",{"$f":"IF(BG163<>\"\",IFERROR(MATCH(BG163&BH163,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":14}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E163),\"\",\"Demand (\" & VLOOKUP($E163,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},0,0,0,0,"",null,null,null,null,null,"","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AA"]
["G","IT equipment",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E165),\"\",\"Consumption (\" & VLOOKUP($E165,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},"","","","","",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG165<>\"\",IFERROR(MATCH(BG165&BH165,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E165),\"\",\"Demand (\" & VLOOKUP($E165,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},"","","","","",null,null,null,null,null,"","",""]
["G","Interior lighting - process",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E167),\"\",\"Consumption (\" & VLOOKUP($E167,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},"","","","","",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG167<>\"\",IFERROR(MATCH(BG167&BH167,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E167),\"\",\"Demand (\" & VLOOKUP($E167,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},"","","","","",null,null,null,null,null,"","",""]
["G","Refrigeration equipment",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E169),\"\",\"Consumption (\" & VLOOKUP($E169,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},"","","","","",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG169<>\"\",IFERROR(MATCH(BG169&BH169,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E169),\"\",\"Demand (\" & VLOOKUP($E169,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},"","","","","",null,null,null,null,null,"","",""]
["G","Fans - Kitchen Ventilation",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E171),\"\",\"Consumption (\" & VLOOKUP($E171,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},"","","","","",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG171<>\"\",IFERROR(MATCH(BG171&BH171,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E171),\"\",\"Demand (\" & VLOOKUP($E171,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},"","","","","",null,null,null,null,null,"","",""]
["G","Cooking",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E173),\"\",\"Consumption (\" & VLOOKUP($E173,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},"","","","","",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG173<>\"\",IFERROR(MATCH(BG173&BH173,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E173),\"\",\"Demand (\" & VLOOKUP($E173,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},"","","","","",null,null,null,null,null,"","",""]
["G","Industrial Process",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E175),\"\",\"Consumption (\" & VLOOKUP($E175,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},"","","","","",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG175<>\"\",IFERROR(MATCH(BG175&BH175,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E175),\"\",\"Demand (\" & VLOOKUP($E175,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},"","","","","",null,null,null,null,null,"","",""]
["G","Elevators and escalators",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E177),\"\",\"Consumption (\" & VLOOKUP($E177,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},"","","","","",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG177<>\"\",IFERROR(MATCH(BG177&BH177,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E177),\"\",\"Demand (\" & VLOOKUP($E177,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},"","","","","",null,null,null,null,null,"","",""]
["G","Heat Pump Supplementary",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E179),\"\",\"Consumption (\" & VLOOKUP($E179,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},0,0,0,0,"",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"U",null,null,{"$f":"IF(BG179<>\"\",IFERROR(MATCH(BG179&BH179,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E179),\"\",\"Demand (\" & VLOOKUP($E179,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},0,0,0,0,"",null,null,null,null,null,"","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AH"]
["G","Space Heating",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E181),\"\",\"Consumption (\" & VLOOKUP($E181,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},0,0,0,0,"",null,null,null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O",null,null,{"$f":"IF(BG181<>\"\",IFERROR(MATCH(BG181&BH181,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E181),\"\",\"Demand (\" & VLOOKUP($E181,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},0,0,0,0,"",null,null,null,null,null,"","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AB"]
["G","Misc Equipment (Gas)",null,null,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E183),\"\",\"Consumption (\" & VLOOKUP($E183,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (therm)"},0,0,0,0,"",null,null,null,null,null,0.1,0.10500000000000001,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AZ",null,null,{"$f":"IF(BG183<>\"\",IFERROR(MATCH(BG183&BH183,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E183),\"\",\"Demand (\" & VLOOKUP($E183,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (Btuh x 10^6)"},"","","","","",null,null,null,null,null,"","",""]
["G","Auxilary (Gas)",null,null,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E185),\"\",\"Consumption (\" & VLOOKUP($E185,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (therm)"},0,0,0,0,"",null,null,null,null,null,0.1,0.10500000000000001,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BD",null,null,{"$f":"IF(BG185<>\"\",IFERROR(MATCH(BG185&BH185,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E185),\"\",\"Demand (\" & VLOOKUP($E185,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (Btuh x 10^6)"},"","","","","",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E187),\"\",\"Consumption (\" & VLOOKUP($E187,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG187<>\"\",IFERROR(MATCH(BG187&BH187,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E187),\"\",\"Demand (\" & VLOOKUP($E187,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E189),\"\",\"Consumption (\" & VLOOKUP($E189,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG189<>\"\",IFERROR(MATCH(BG189&BH189,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E189),\"\",\"Demand (\" & VLOOKUP($E189,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E191),\"\",\"Consumption (\" & VLOOKUP($E191,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG191<>\"\",IFERROR(MATCH(BG191&BH191,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E191),\"\",\"Demand (\" & VLOOKUP($E191,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","",""]
["G",null,null,null,"Energy_Type","Energy_Units","Baseline_0_Rotation","Baseline_90_Rotation","Baseline_180_Rotation","Baseline_270_Rotation","Baseline_Total",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",""]
["G","Total energy consumption by energy type ",null,null,{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E194),\"\",VLOOKUP($E194,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"kWh"},{"$f":"IFERROR(SUMIFS(INDEX(PO_baseline_table,0,MATCH(G$144,PO_baseline_hdr,0)),INDEX(PO_baseline_table,0,MATCH($E$144,PO_baseline_hdr,0)),$E194,INDEX(PO_baseline_table,0,MATCH($F$144,PO_baseline_hdr,0)),\"=Con*\"),\"\")","v":0},0,0,0,0,"","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E194),\"\",VLOOKUP($E194,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($E194),\"\",VLOOKUP($E194,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3}]
["G",null,null,null,"Natural Gas","therm",0,0,0,0,0,"","",null,null,null,0.1,0.10500000000000001]
["G",null,null,null,"District Cooling","MWh",0,0,0,0,0,"","",null,null,null,3.4119999999999999,3.4119999999999999]
["G",null,null,null,"District Cooling","MWh",0,0,0,0,0,"","",null,null,null,3.4119999999999999,3.4119999999999999]
["G",null,null,null,"District Cooling","MWh",0,0,0,0,0,"","",null,null,null,3.4119999999999999,3.4119999999999999]
["G",null,null,null,"District Cooling","MWh",0,0,0,0,0,"","",null,null,null,3.4119999999999999,3.4119999999999999]
["G",null,null,null,"District Cooling","MWh",0,0,0,0,0,"","",null,null,null,3.4119999999999999,3.4119999999999999]
["G",null,null,null,"District Cooling","MWh",0,0,0,0,0,"","",null,null,null,3.4119999999999999,3.4119999999999999]
["G",null,null,null,"District Cooling",{"$f":"IFERROR(IF(ISBLANK(E202),\"\",VLOOKUP($E202,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"MWh"},0,0,0,0,0,"","",null,null,null,3.4119999999999999,3.4119999999999999]
["G",null,null,null,"District Cooling",{"$f":"IFERROR(IF(ISBLANK(E203),\"\",VLOOKUP($E203,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"MWh"},0,0,0,0,0,"","",null,null,null,3.4119999999999999,3.4119999999999999]
["G",null,null,null,"District Cooling",{"$f":"IFERROR(IF(ISBLANK(E204),\"\",VLOOKUP($E204,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"MWh"},0,0,0,0,0,"","",null,null,null,3.4119999999999999,3.4119999999999999]
["G",null,null,null,"District Cooling",{"$f":"IFERROR(IF(ISBLANK(E205),\"\",VLOOKUP($E205,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"MWh"},0,0,0,0,0,"","",null,null,null,3.4119999999999999,3.4119999999999999]
["G",null,null,null,{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},{"$f":"IFERROR(IF(ISBLANK(E206),\"\",VLOOKUP($E206,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"MWh"},0,0,0,0,0,"","",null,null,null,3.4119999999999999,3.4119999999999999]
["G",null,null,null,"District Cooling","MWh",0,0,0,0,0,"","",null,null,null,3.4119999999999999,3.4119999999999999]
["G",null,null,null,"District Cooling","MWh",0,0,0,0,0,"","",null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"\"Total site energy (\" & PO_SiteUnits & \")\"","v":"Total site energy (Btu x 10^6)"},null,null,null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_5_Table,0,MATCH(G$193,PO_Enrgy_5_Hdr,0)),INDEX(PO_Enrgy_5_Table,0,MATCH($Q193,PO_Enrgy_5_Hdr,0))),\"\")","v":0},0,0,0,0,"",""]
["G",{"$f":"\"Total source energy (\" & PO_SourceUnits & \")\"","v":"Total source energy (Btu x 10^6)"},null,null,null,null,{"$f":"IFERROR(SUMPRODUCT(G$194:G$195,$R$194:$R$195),0)","v":0},0,0,0,0,0,0]
["G"]
["G","Table: Baseline building annual energy cost by energy type "]
["G","Energy Type",null,null,null,null,"Baseline 0° rotation","Baseline 90° rotation","Baseline 180° rotation","Baseline 270° rotation","Baseline Design Total"]
["G","Energy_Type",null,null,null,null,"Baseline_0_Rotation","Baseline_90_Rotation","Baseline_180_Rotation","Baseline_270_Rotation","Base_Cost",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B215),\"\",VLOOKUP($B215,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"kWh"},null,null,null,null,{"$f":"IFERROR((AVERAGE(G215:J215)),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B215),\"\",VLOOKUP($B215,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B215),\"\",VLOOKUP($B215,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3}]
["G","Natural Gas",null,null,null,"therm",null,null,null,null,"",null,null,null,null,null,0.1,0.10500000000000001]
["G","District Cooling",null,null,null,"MWh",null,null,null,null,"",null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling",null,null,null,"MWh",null,null,null,null,"",null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling",null,null,null,"MWh",null,null,null,null,"",null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling",null,null,null,"MWh",null,null,null,null,"",null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling",null,null,null,"MWh",null,null,null,null,{"$f":"IFERROR((AVERAGE(G221:J221)),\"\")","v":""},null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling",null,null,null,"MWh",null,null,null,null,"",null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling",null,null,null,"MWh",null,null,null,null,{"$f":"IFERROR((AVERAGE(G223:J223)),\"\")","v":""},null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling",null,null,null,"MWh",null,null,null,null,{"$f":"IFERROR((AVERAGE(G224:J224)),\"\")","v":""},null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling",null,null,null,"MWh",null,null,null,null,{"$f":"IFERROR((AVERAGE(G225:J225)),\"\")","v":""},null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling",null,null,null,"MWh",null,null,null,null,{"$f":"IFERROR((AVERAGE(G226:J226)),\"\")","v":""},null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},null,null,null,"MWh",null,null,null,null,{"$f":"IFERROR((AVERAGE(G227:J227)),\"\")","v":""},null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling",null,null,null,"MWh",null,null,null,null,"",null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling",null,null,null,"MWh",null,null,null,null,"",null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","Baseline annual energy cost",null,null,null,null,{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_6_Table,0,MATCH(G$214,PO_Enrgy_6_Hdr,0))),\"\")","v":0},0,0,0,0,"",""]
["G"]
["G"]
["G","Table: Proposed energy summary by end use"]
["G","Complete the table below, providing information on energy consumption and demand by end-use. If an end-use has two energy types (e.g. proposed case space heating includes both fossil fuel and electric), enter the end-use twice in the table, and list the two different energy types."]
["G","ASHRAE 90.1-2010 without Addenda (District Energy Modeling Path 1): Report the district energy type (District Cooling, District Hot Water, or District Steam) for the cooling and heating end-uses as applicable for both the baseline and proposed."]
["G","Full DES Performance Accounting method (District Energy Modeling Path 2): Report the baseline energy as if the thermal energy is produced in the building.  Report the proposed energy used to generate and distribute the district thermal energy serving the building based on calculated average district thermal efficiencies (e.g. report the electricity used to generate and distribute chilled water to the building).\n"]
["G","Streamlined DES Accounting Method (District Energy Modeling Path 3): Report the energy type (District Cooling, District Hot Water, or District Steam for the cooling and heating end-uses as applicable for both the baseline and proposed. "]
["G","Data Centers: The energy consumption for IT equipment must be metered and reported separately from other end-uses in the energy model, and in the tables below to allow the proper determination of the PUE. Complete the table below for the baseline using the full build-out IT loads for the proposed design.\n"]
["G","Retail: The energy consumption for cooking, refrigeration, and kitchen ventilation fans must be metered and reported separately from other end-uses in the energy model and in the tables below. Energy savings or consumption attributable to unregulated equipment, other than Commercial Kitchen Equipment, Supermarket Refrigeration, Walk-in Coolers and Freezers, or Commercial Kitchen Ventilation listed in Tables 1 – 4 of the LEED v4 BD+C: Retail and ID+C: Retail Rating System Appendix 3 must be claimed via Exceptional Calculation Methodology."]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Software Link References"]
["G","End Use",null,"Unregulated?","Energy Type","Units of \nAnnual Energy and Peak Demand","Baseline","Proposed","Energy / Demand Savings \nper End-Use","End Use \nPercent Contribution to Total Energy Savings","End Use \nPercent \nContribution to \nTotal Cost Savings",null,"Percent of Total Proposed  \nSite Energy Consumption",null,null,null,null,null,null,null,null,null,"contribution rank",null,"Rank with ties","rank no ties",null,null,null,null,null,null,"QC_EFLH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eQUEST Outputs End Use Column","TRACE End Use Label","TRACE End Use Fuel Label","TRACE Output End Use Row"]
["G","End_Use",null,"Unregulated","Energy_Type","Energy_Units","Base_Consumption_Demand","Design_Consumption_Demand","End_Use_Savings","End_Use_Contribution_to_Energy_Savings","End_Use_Contribution_to_Cost_Savings",null,"Percent_Design_Site_Consumption",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion","Base_EFLH","Design_EFLH",null,null,"contribution rank",null,"Rank with ties","rank no ties"]
["G","Interior lighting",null,{"$f":"INDEX(PO_baseline_table,1, 3)","v":0},{"$f":"INDEX(PO_baseline_table,1, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E243),\"\",\"Consumption (\" & VLOOKUP($E243,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,1, 10)","v":""},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF243&\"13\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!H\"&$BI243)/$Q243,\"\")),\"\")","v":0},{"$f":"IFERROR(1-H243/G243,\"\")","v":""},{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G243-$H243)*VLOOKUP($E243,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G243*VLOOKUP($E243,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H243*VLOOKUP($E243,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H243*VLOOKUP($E243,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($E243),\"\",VLOOKUP($E243,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($E243),\"\",VLOOKUP($E243,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3},{"$f":"IFERROR(IF(FIND(\"Consumption\",F243),(G243*VLOOKUP(MID(F243,FIND(\"(\",F243)+1,LEN(F243)-FIND(\"(\",F243)-1),EnergyUnitsTable,3,FALSE))/(G244*VLOOKUP(MID(F244,FIND(\"(\",F244)+1,LEN(F244)-FIND(\"(\",F244)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",$F243),(H243*VLOOKUP(MID($F243,FIND(\"(\",$F243)+1,LEN($F243)-FIND(\"(\",$F243)-1),EnergyUnitsTable,3,FALSE))/(H244*VLOOKUP(MID($F244,FIND(\"(\",$F244)+1,LEN($F244)-FIND(\"(\",$F244)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IFERROR($AN243*H243,0)","v":0},{"$f":"IFERROR(G243*VLOOKUP($AE243,PO_Enrgy_8_Table,4,FALSE),0)","v":0},{"$f":"IFERROR(H243*VLOOKUP($AE243,PO_Enrgy_8_Table,7,FALSE),0)","v":0},{"$f":"IFERROR(IF(D243=\"x\",IF(OR(G243/H243>1.03,G243/H243<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J243*100,)","v":0},null,{"$f":"RANK(Z243,$Z$243:$Z$290,0)","v":1},{"$f":"AB243","v":1},{"$f":"B243","v":"Interior lighting"},null,{"$f":"IFERROR(G243/'6b - General Lighting'!#REF!,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BF145","v":"L"},"Lighting - Conditioned","Electricity",{"$f":"IF(BG243<>\"\",IFERROR(MATCH(BG243&BH243,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":7}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E243),\"\",\"Demand (\" & VLOOKUP($E243,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,2, 10)","v":""},0,{"$f":"IFERROR(1-H244/G244,\"\")","v":""},null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y",0,0]
["G","Exterior lighting",null,{"$f":"INDEX(PO_baseline_table,3, 3)","v":0},{"$f":"INDEX(PO_baseline_table,3, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E245),\"\",\"Consumption (\" & VLOOKUP($E245,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,3, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G245-$H245)*VLOOKUP($E245,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G245*VLOOKUP($E245,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H245*VLOOKUP($E245,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H245*VLOOKUP($E245,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D245=\"x\",IF(OR(G245/H245>1.03,G245/H245<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J245*100,)","v":0},null,{"$f":"RANK(Z245,$Z$243:$Z$290,0)","v":1},{"$f":"AB245+COUNTIF($AB$243:$AB244,AB245)","v":2},{"$f":"B245","v":"Exterior lighting"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W","Stand-alone Base Utilities","Electricity",{"$f":"IF(BG245<>\"\",IFERROR(MATCH(BG245&BH245,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":15}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E245),\"\",\"Demand (\" & VLOOKUP($E245,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,4, 10)","v":""},0,"",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AJ",0,0]
["G","Space heating",null,{"$f":"INDEX(PO_baseline_table,5, 3)","v":0},{"$f":"INDEX(PO_baseline_table,5, 4)","v":"Natural Gas"},{"$f":"IFERROR(IF(ISBLANK(E247),\"\",\"Consumption (\" & VLOOKUP($E247,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (therm)"},{"$f":"INDEX(PO_baseline_table,5, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G247-$H247)*VLOOKUP($E247,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G247*VLOOKUP($E247,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H247*VLOOKUP($E247,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H247*VLOOKUP($E247,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,0.1,0.10500000000000001,"","",null,0,0,0,{"$f":"IFERROR(IF(D247=\"x\",IF(OR(G247/H247>1.03,G247/H247<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J247*100,)","v":0},null,{"$f":"RANK(Z247,$Z$243:$Z$290,0)","v":1},{"$f":"AB247+COUNTIF($AB$243:$AB246,AB247)","v":3},{"$f":"B247","v":"Space heating"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BA","Space Heating","Gas",{"$f":"IF(BG247<>\"\",IFERROR(MATCH(BG247&BH247,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":9}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E247),\"\",\"Demand (\" & VLOOKUP($E247,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (Btuh x 10^6)"},{"$f":"INDEX(PO_baseline_table,6, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G","Space cooling",null,{"$f":"INDEX(PO_baseline_table,7, 3)","v":0},{"$f":"INDEX(PO_baseline_table,7, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E249),\"\",\"Consumption (\" & VLOOKUP($E249,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,7, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G249-$H249)*VLOOKUP($E249,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G249*VLOOKUP($E249,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H249*VLOOKUP($E249,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H249*VLOOKUP($E249,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D249=\"x\",IF(OR(G249/H249>1.03,G249/H249<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J249*100,)","v":0},null,{"$f":"RANK(Z249,$Z$243:$Z$290,0)","v":1},{"$f":"AB249+COUNTIF($AB$243:$AB248,AB249)","v":4},{"$f":"B249","v":"Space cooling"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"P","Space Cooling","Electricity",{"$f":"IF(BG249<>\"\",IFERROR(MATCH(BG249&BH249,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":10}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E249),\"\",\"Demand (\" & VLOOKUP($E249,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,8, 10)","v":""},0,"",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AC",0,0]
["G","Pumps",null,{"$f":"INDEX(PO_baseline_table,9, 3)","v":0},{"$f":"INDEX(PO_baseline_table,9, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E251),\"\",\"Consumption (\" & VLOOKUP($E251,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,9, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G251-$H251)*VLOOKUP($E251,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G251*VLOOKUP($E251,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H251*VLOOKUP($E251,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H251*VLOOKUP($E251,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D251=\"x\",IF(OR(G251/H251>1.03,G251/H251<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J251*100,)","v":0},null,{"$f":"RANK(Z251,$Z$243:$Z$290,0)","v":1},{"$f":"AB251+COUNTIF($AB$243:$AB250,AB251)","v":5},{"$f":"B251","v":"Pumps"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R","Pumps","Electricity",{"$f":"IF(BG251<>\"\",IFERROR(MATCH(BG251&BH251,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":11}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E251),\"\",\"Demand (\" & VLOOKUP($E251,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,10, 10)","v":""},0,"",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AE",0,0]
["G","Heat rejection",null,{"$f":"INDEX(PO_baseline_table,11, 3)","v":0},{"$f":"INDEX(PO_baseline_table,11, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E253),\"\",\"Consumption (\" & VLOOKUP($E253,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,11, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G253-$H253)*VLOOKUP($E253,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G253*VLOOKUP($E253,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H253*VLOOKUP($E253,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H253*VLOOKUP($E253,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D253=\"x\",IF(OR(G253/H253>1.03,G253/H253<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J253*100,)","v":0},null,{"$f":"RANK(Z253,$Z$243:$Z$290,0)","v":1},{"$f":"AB253+COUNTIF($AB$243:$AB252,AB253)","v":6},{"$f":"B253","v":"Heat rejection"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Q","Heat Rejection","Electricity",{"$f":"IF(BG253<>\"\",IFERROR(MATCH(BG253&BH253,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":12}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E253),\"\",\"Demand (\" & VLOOKUP($E253,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,12, 10)","v":""},0,"",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AD",0,0]
["G","Fans - interior ventilation",null,{"$f":"INDEX(PO_baseline_table,13, 3)","v":0},{"$f":"INDEX(PO_baseline_table,13, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E255),\"\",\"Consumption (\" & VLOOKUP($E255,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,13, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G255-$H255)*VLOOKUP($E255,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G255*VLOOKUP($E255,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H255*VLOOKUP($E255,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H255*VLOOKUP($E255,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D255=\"x\",IF(OR(G255/H255>1.03,G255/H255<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J255*100,)","v":0},null,{"$f":"RANK(Z255,$Z$243:$Z$290,0)","v":1},{"$f":"AB255+COUNTIF($AB$243:$AB254,AB255)","v":7},{"$f":"B255","v":"Fans - interior ventilation"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S","Fans - Conditioned","Electricity",{"$f":"IF(BG255<>\"\",IFERROR(MATCH(BG255&BH255,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":13}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E255),\"\",\"Demand (\" & VLOOKUP($E255,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,14, 10)","v":""},0,"",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AF",0,0]
["G","Fans - parking garage",null,{"$f":"INDEX(PO_baseline_table,15, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,15, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E257),\"\",\"Consumption (\" & VLOOKUP($E257,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,15, 10)","v":""},"","",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G257-$H257)*VLOOKUP($E257,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G257*VLOOKUP($E257,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H257*VLOOKUP($E257,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H257*VLOOKUP($E257,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D257=\"x\",IF(OR(G257/H257>1.03,G257/H257<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J257*100,)","v":0},null,{"$f":"RANK(Z257,$Z$243:$Z$290,0)","v":1},{"$f":"AB257+COUNTIF($AB$243:$AB256,AB257)","v":8},{"$f":"B257","v":"Fans - parking garage"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,{"$f":"IF(BG257<>\"\",IFERROR(MATCH(BG257&BH257,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E257),\"\",\"Demand (\" & VLOOKUP($E257,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,16, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G","Service water heating",null,{"$f":"INDEX(PO_baseline_table,17, 3)","v":0},{"$f":"INDEX(PO_baseline_table,17, 4)","v":"Natural Gas"},{"$f":"IFERROR(IF(ISBLANK(E259),\"\",\"Consumption (\" & VLOOKUP($E259,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (therm)"},{"$f":"INDEX(PO_baseline_table,17, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G259-$H259)*VLOOKUP($E259,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G259*VLOOKUP($E259,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H259*VLOOKUP($E259,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H259*VLOOKUP($E259,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,0.1,0.10500000000000001,"","",null,0,0,0,{"$f":"IFERROR(IF(D259=\"x\",IF(OR(G259/H259>1.03,G259/H259<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J259*100,)","v":0},null,{"$f":"RANK(Z259,$Z$243:$Z$290,0)","v":1},{"$f":"AB259+COUNTIF($AB$243:$AB258,AB259)","v":9},{"$f":"B259","v":"Service water heating"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BH","Stand-alone Base Utilities","Gas",{"$f":"IF(BG259<>\"\",IFERROR(MATCH(BG259&BH259,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":16}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E259),\"\",\"Demand (\" & VLOOKUP($E259,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (Btuh x 10^6)"},{"$f":"INDEX(PO_baseline_table,18, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G","Receptacle equipment",null,{"$f":"INDEX(PO_baseline_table,19, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,19, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E261),\"\",\"Consumption (\" & VLOOKUP($E261,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,19, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G261-$H261)*VLOOKUP($E261,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G261*VLOOKUP($E261,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H261*VLOOKUP($E261,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H261*VLOOKUP($E261,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D261=\"x\",IF(OR(G261/H261>1.03,G261/H261<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J261*100,)","v":0},null,{"$f":"RANK(Z261,$Z$243:$Z$290,0)","v":1},{"$f":"AB261+COUNTIF($AB$243:$AB260,AB261)","v":10},{"$f":"B261","v":"Receptacle equipment"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N","Receptacles - Conditioned","Electricity",{"$f":"IF(BG261<>\"\",IFERROR(MATCH(BG261&BH261,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":14}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E261),\"\",\"Demand (\" & VLOOKUP($E261,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,20, 10)","v":""},0,"",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AA",0,0]
["G","IT equipment",null,{"$f":"INDEX(PO_baseline_table,21, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,21, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E263),\"\",\"Consumption (\" & VLOOKUP($E263,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,21, 10)","v":""},"","",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G263-$H263)*VLOOKUP($E263,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G263*VLOOKUP($E263,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H263*VLOOKUP($E263,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H263*VLOOKUP($E263,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D263=\"x\",IF(OR(G263/H263>1.03,G263/H263<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J263*100,)","v":0},null,{"$f":"RANK(Z263,$Z$243:$Z$290,0)","v":1},{"$f":"AB263+COUNTIF($AB$243:$AB262,AB263)","v":11},{"$f":"B263","v":"IT equipment"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BF165","v":0},0,0,{"$f":"IF(BG263<>\"\",IFERROR(MATCH(BG263&BH263,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E263),\"\",\"Demand (\" & VLOOKUP($E263,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,22, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G","Interior lighting - process",null,{"$f":"INDEX(PO_baseline_table,23, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,23, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E265),\"\",\"Consumption (\" & VLOOKUP($E265,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,23, 10)","v":""},"","",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G265-$H265)*VLOOKUP($E265,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G265*VLOOKUP($E265,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H265*VLOOKUP($E265,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H265*VLOOKUP($E265,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D265=\"x\",IF(OR(G265/H265>1.03,G265/H265<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J265*100,)","v":0},null,{"$f":"RANK(Z265,$Z$243:$Z$290,0)","v":1},{"$f":"AB265+COUNTIF($AB$243:$AB264,AB265)","v":12},{"$f":"B265","v":"Interior lighting - process"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,{"$f":"IF(BG265<>\"\",IFERROR(MATCH(BG265&BH265,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E265),\"\",\"Demand (\" & VLOOKUP($E265,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,24, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G","Refrigeration equipment",null,{"$f":"INDEX(PO_baseline_table,25, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,25, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E267),\"\",\"Consumption (\" & VLOOKUP($E267,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,25, 10)","v":""},"","",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G267-$H267)*VLOOKUP($E267,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G267*VLOOKUP($E267,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H267*VLOOKUP($E267,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H267*VLOOKUP($E267,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D267=\"x\",IF(OR(G267/H267>1.03,G267/H267<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J267*100,)","v":0},null,{"$f":"RANK(Z267,$Z$243:$Z$290,0)","v":1},{"$f":"AB267+COUNTIF($AB$243:$AB266,AB267)","v":13},{"$f":"B267","v":"Refrigeration equipment"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,{"$f":"IF(BG267<>\"\",IFERROR(MATCH(BG267&BH267,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E267),\"\",\"Demand (\" & VLOOKUP($E267,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,26, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G","Fans - Kitchen Ventilation",null,{"$f":"INDEX(PO_baseline_table,27, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,27, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E269),\"\",\"Consumption (\" & VLOOKUP($E269,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,27, 10)","v":""},"","",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G269-$H269)*VLOOKUP($E269,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G269*VLOOKUP($E269,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H269*VLOOKUP($E269,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H269*VLOOKUP($E269,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D269=\"x\",IF(OR(G269/H269>1.03,G269/H269<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J269*100,)","v":0},null,{"$f":"RANK(Z269,$Z$243:$Z$290,0)","v":1},{"$f":"AB269+COUNTIF($AB$243:$AB268,AB269)","v":14},{"$f":"B269","v":"Fans - Kitchen Ventilation"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,{"$f":"IF(BG269<>\"\",IFERROR(MATCH(BG269&BH269,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E269),\"\",\"Demand (\" & VLOOKUP($E269,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,28, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G","Cooking",null,{"$f":"INDEX(PO_baseline_table,29, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,29, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E271),\"\",\"Consumption (\" & VLOOKUP($E271,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,29, 10)","v":""},"","",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G271-$H271)*VLOOKUP($E271,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G271*VLOOKUP($E271,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H271*VLOOKUP($E271,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H271*VLOOKUP($E271,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D271=\"x\",IF(OR(G271/H271>1.03,G271/H271<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J271*100,)","v":0},null,{"$f":"RANK(Z271,$Z$243:$Z$290,0)","v":1},{"$f":"AB271+COUNTIF($AB$243:$AB270,AB271)","v":15},{"$f":"B271","v":"Cooking"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,{"$f":"IF(BG271<>\"\",IFERROR(MATCH(BG271&BH271,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E271),\"\",\"Demand (\" & VLOOKUP($E271,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,30, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G","Industrial Process",null,{"$f":"INDEX(PO_baseline_table,31, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,31, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E273),\"\",\"Consumption (\" & VLOOKUP($E273,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,31, 10)","v":""},"","",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G273-$H273)*VLOOKUP($E273,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G273*VLOOKUP($E273,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H273*VLOOKUP($E273,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H273*VLOOKUP($E273,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D273=\"x\",IF(OR(G273/H273>1.03,G273/H273<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J273*100,)","v":0},null,{"$f":"RANK(Z273,$Z$243:$Z$290,0)","v":1},{"$f":"AB273+COUNTIF($AB$243:$AB272,AB273)","v":16},{"$f":"B273","v":"Industrial Process"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,{"$f":"IF(BG273<>\"\",IFERROR(MATCH(BG273&BH273,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E273),\"\",\"Demand (\" & VLOOKUP($E273,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,32, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G","Elevators and escalators",null,{"$f":"INDEX(PO_baseline_table,33, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,33, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E275),\"\",\"Consumption (\" & VLOOKUP($E275,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,33, 10)","v":""},"","",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G275-$H275)*VLOOKUP($E275,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G275*VLOOKUP($E275,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H275*VLOOKUP($E275,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H275*VLOOKUP($E275,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D275=\"x\",IF(OR(G275/H275>1.03,G275/H275<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J275*100,)","v":0},null,{"$f":"RANK(Z275,$Z$243:$Z$290,0)","v":1},{"$f":"AB275+COUNTIF($AB$243:$AB274,AB275)","v":17},{"$f":"B275","v":"Elevators and escalators"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,{"$f":"IF(BG275<>\"\",IFERROR(MATCH(BG275&BH275,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E275),\"\",\"Demand (\" & VLOOKUP($E275,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,34, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G","Heat Pump Supplementary",null,{"$f":"INDEX(PO_baseline_table,35, 3)","v":0},{"$f":"INDEX(PO_baseline_table,35, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E277),\"\",\"Consumption (\" & VLOOKUP($E277,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,35, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G277-$H277)*VLOOKUP($E277,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G277*VLOOKUP($E277,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H277*VLOOKUP($E277,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H277*VLOOKUP($E277,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D277=\"x\",IF(OR(G277/H277>1.03,G277/H277<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J277*100,)","v":0},null,{"$f":"RANK(Z277,$Z$243:$Z$290,0)","v":1},{"$f":"AB277+COUNTIF($AB$243:$AB276,AB277)","v":18},{"$f":"B277","v":"Heat Pump Supplementary"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"U",0,0,{"$f":"IF(BG277<>\"\",IFERROR(MATCH(BG277&BH277,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E277),\"\",\"Demand (\" & VLOOKUP($E277,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,36, 10)","v":""},0,"",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AH",0,0]
["G",{"$f":"INDEX(PO_base_Add_EndUses,1, 1)","v":"Space Heating"},null,{"$f":"INDEX(PO_baseline_table,37, 3)","v":0},{"$f":"INDEX(PO_baseline_table,37, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E279),\"\",\"Consumption (\" & VLOOKUP($E279,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (kWh)"},{"$f":"INDEX(PO_baseline_table,37, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G279-$H279)*VLOOKUP($E279,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G279*VLOOKUP($E279,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H279*VLOOKUP($E279,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H279*VLOOKUP($E279,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,3.4120000000000001E-3,8.7005999999999993E-3,"","",null,0,0,0,{"$f":"IFERROR(IF(D279=\"x\",IF(OR(G279/H279>1.03,G279/H279<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J279*100,)","v":0},null,{"$f":"RANK(Z279,$Z$243:$Z$290,0)","v":1},{"$f":"AB279+COUNTIF($AB$243:$AB278,AB279)","v":19},{"$f":"B279","v":"Space Heating"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O",0,0,{"$f":"IF(BG279<>\"\",IFERROR(MATCH(BG279&BH279,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E279),\"\",\"Demand (\" & VLOOKUP($E279,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (kW)"},{"$f":"INDEX(PO_baseline_table,38, 10)","v":""},0,"",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AB",0,0]
["G",{"$f":"INDEX(PO_base_Add_EndUses,3, 1)","v":"Misc Equipment (Gas)"},null,{"$f":"INDEX(PO_baseline_table,39, 3)","v":0},{"$f":"INDEX(PO_baseline_table,39, 4)","v":"Natural Gas"},{"$f":"IFERROR(IF(ISBLANK(E281),\"\",\"Consumption (\" & VLOOKUP($E281,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (therm)"},{"$f":"INDEX(PO_baseline_table,39, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G281-$H281)*VLOOKUP($E281,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G281*VLOOKUP($E281,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H281*VLOOKUP($E281,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H281*VLOOKUP($E281,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,0.1,0.10500000000000001,"","",null,0,0,0,{"$f":"IFERROR(IF(D281=\"x\",IF(OR(G281/H281>1.03,G281/H281<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J281*100,)","v":0},null,{"$f":"RANK(Z281,$Z$243:$Z$290,0)","v":1},{"$f":"AB281+COUNTIF($AB$243:$AB280,AB281)","v":20},{"$f":"B281","v":"Misc Equipment (Gas)"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AZ",0,0,{"$f":"IF(BG281<>\"\",IFERROR(MATCH(BG281&BH281,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E281),\"\",\"Demand (\" & VLOOKUP($E281,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (Btuh x 10^6)"},{"$f":"INDEX(PO_baseline_table,40, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_base_Add_EndUses,5, 1)","v":"Auxilary (Gas)"},null,{"$f":"INDEX(PO_baseline_table,41, 3)","v":0},{"$f":"INDEX(PO_baseline_table,41, 4)","v":"Natural Gas"},{"$f":"IFERROR(IF(ISBLANK(E283),\"\",\"Consumption (\" & VLOOKUP($E283,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Consumption (therm)"},{"$f":"INDEX(PO_baseline_table,41, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G283-$H283)*VLOOKUP($E283,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G283*VLOOKUP($E283,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H283*VLOOKUP($E283,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H283*VLOOKUP($E283,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,0.1,0.10500000000000001,"","",null,0,0,0,{"$f":"IFERROR(IF(D283=\"x\",IF(OR(G283/H283>1.03,G283/H283<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J283*100,)","v":0},null,{"$f":"RANK(Z283,$Z$243:$Z$290,0)","v":1},{"$f":"AB283+COUNTIF($AB$243:$AB282,AB283)","v":21},{"$f":"B283","v":"Auxilary (Gas)"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BF185","v":"BD"},0,0,{"$f":"IF(BG283<>\"\",IFERROR(MATCH(BG283&BH283,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E283),\"\",\"Demand (\" & VLOOKUP($E283,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":"Demand (Btuh x 10^6)"},{"$f":"INDEX(PO_baseline_table,42, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_base_Add_EndUses,7, 1)","v":0},null,{"$f":"INDEX(PO_baseline_table,43, 3)","v":0},{"$f":"INDEX(PO_baseline_table,43, 4)","v":0},{"$f":"IFERROR(IF(ISBLANK(E285),\"\",\"Consumption (\" & VLOOKUP($E285,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,43, 10)","v":""},"","",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G285-$H285)*VLOOKUP($E285,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G285*VLOOKUP($E285,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H285*VLOOKUP($E285,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H285*VLOOKUP($E285,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D285=\"x\",IF(OR(G285/H285>1.03,G285/H285<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J285*100,)","v":0},null,{"$f":"RANK(Z285,$Z$243:$Z$290,0)","v":1},{"$f":"AB285+COUNTIF($AB$243:$AB284,AB285)","v":22},{"$f":"B285","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,{"$f":"IF(BG285<>\"\",IFERROR(MATCH(BG285&BH285,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E285),\"\",\"Demand (\" & VLOOKUP($E285,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,44, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_base_Add_EndUses,9, 1)","v":0},null,{"$f":"INDEX(PO_baseline_table,45, 3)","v":0},{"$f":"INDEX(PO_baseline_table,45, 4)","v":0},{"$f":"IFERROR(IF(ISBLANK(E287),\"\",\"Consumption (\" & VLOOKUP($E287,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,45, 10)","v":""},"","",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G287-$H287)*VLOOKUP($E287,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G287*VLOOKUP($E287,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H287*VLOOKUP($E287,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H287*VLOOKUP($E287,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D287=\"x\",IF(OR(G287/H287>1.03,G287/H287<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J287*100,)","v":0},null,{"$f":"RANK(Z287,$Z$243:$Z$290,0)","v":1},{"$f":"AB287+COUNTIF($AB$243:$AB286,AB287)","v":23},{"$f":"B287","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,{"$f":"IF(BG287<>\"\",IFERROR(MATCH(BG287&BH287,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E287),\"\",\"Demand (\" & VLOOKUP($E287,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,46, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_base_Add_EndUses,11, 1)","v":0},null,{"$f":"INDEX(PO_baseline_table,47, 3)","v":0},{"$f":"INDEX(PO_baseline_table,47, 4)","v":0},{"$f":"IFERROR(IF(ISBLANK(E289),\"\",\"Consumption (\" & VLOOKUP($E289,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,47, 10)","v":""},"","",{"$f":"IFERROR(IF($E$520-$H$520<0,\"\",($G289-$H289)*VLOOKUP($E289,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$520-$H$520)),\"\")","v":""},{"$f":"IFERROR(IF($G$520-$J$520<0,\"\",($G289*VLOOKUP($E289,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)-($H289*VLOOKUP($E289,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)))/($G$520-$J$520)),\"\")","v":""},null,{"$f":"IFERROR(H289*VLOOKUP($E289,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$311,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D289=\"x\",IF(OR(G289/H289>1.03,G289/H289<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J289*100,)","v":0},null,{"$f":"RANK(Z289,$Z$243:$Z$290,0)","v":1},{"$f":"AB289+COUNTIF($AB$243:$AB288,AB289)","v":24},{"$f":"B289","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,{"$f":"IF(BG289<>\"\",IFERROR(MATCH(BG289&BH289,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E289),\"\",\"Demand (\" & VLOOKUP($E289,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,48, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G"]
["G","Table: Performance rating energy consumption and cost by fuel type"]
["G","Energy Type","Site Energy Units",null,"Baseline",null,null,"Proposed",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site_Energy",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK($B296),\"\",VLOOKUP($B296,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"kWh"},{"$f":"IF(C296=\"\",\"\",VLOOKUP(C296,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(SUMIFS(G$243:G$290,$F$243:$F$290,\"=Con*\",$E$243:$E$290,$B296), 0)","v":0},{"$f":"IFERROR(SUMIFS(G$243:G$290,$F$243:$F$290,\"=Con*\",$E$243:$E$290,$B296)*VLOOKUP($B296,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE), 0)","v":0},{"$f":"INDEX(PO_Enrgy_6_Table,1, 10)","v":""},{"$f":"IFERROR(SUMIFS(H$243:H$290,$F$243:$F$290,\"=Con*\",$E$243:$E$290,$B296), 0)","v":0},{"$f":"IFERROR(SUMIFS(H$243:H$290,$F$243:$F$290,\"=Con*\",$E$243:$E$290,$B296)*VLOOKUP($B296,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE), 0)","v":0},null,{"$f":"IFERROR(1-H296/E296,\"\")","v":""},null,{"$f":"IFERROR(1-J296/G296,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B296),\"\",VLOOKUP($B296,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B296),\"\",VLOOKUP($B296,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3}]
["G","Natural Gas","therm",{"$f":"IF(C297=\"\",\"\",VLOOKUP(C297,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,{"$f":"INDEX(PO_Enrgy_6_Table,2, 10)","v":""},0,0,null,"",null,"",null,null,null,0.1,0.10500000000000001]
["G","District Cooling","MWh",{"$f":"IF(C298=\"\",\"\",VLOOKUP(C298,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,{"$f":"INDEX(PO_Enrgy_6_Table,3, 10)","v":""},0,0,null,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C299=\"\",\"\",VLOOKUP(C299,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,{"$f":"INDEX(PO_Enrgy_6_Table,4, 10)","v":""},0,0,null,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C300=\"\",\"\",VLOOKUP(C300,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,{"$f":"INDEX(PO_Enrgy_6_Table,5, 10)","v":""},0,0,null,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C301=\"\",\"\",VLOOKUP(C301,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,{"$f":"INDEX(PO_Enrgy_6_Table,6, 10)","v":""},0,0,null,{"$f":"IFERROR(1-H301/E301,\"\")","v":""},null,{"$f":"IFERROR(1-J301/G301,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C302=\"\",\"\",VLOOKUP(C302,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(SUMIFS(G$243:G$290,$F$243:$F$290,\"=Con*\",$E$243:$E$290,$B302), 0)","v":0},0,{"$f":"INDEX(PO_Enrgy_6_Table,7, 10)","v":""},{"$f":"IFERROR(SUMIFS(H$243:H$290,$F$243:$F$290,\"=Con*\",$E$243:$E$290,$B302), 0)","v":0},0,null,{"$f":"IFERROR(1-H302/E302,\"\")","v":""},null,{"$f":"IFERROR(1-J302/G302,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C303=\"\",\"\",VLOOKUP(C303,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,{"$f":"INDEX(PO_Enrgy_6_Table,8, 10)","v":""},0,0,null,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C304=\"\",\"\",VLOOKUP(C304,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(SUMIFS(G$243:G$290,$F$243:$F$290,\"=Con*\",$E$243:$E$290,$B304), 0)","v":0},0,{"$f":"INDEX(PO_Enrgy_6_Table,9, 10)","v":""},0,0,null,{"$f":"IFERROR(1-H304/E304,\"\")","v":""},null,{"$f":"IFERROR(1-J304/G304,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C305=\"\",\"\",VLOOKUP(C305,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(SUMIFS(G$243:G$290,$F$243:$F$290,\"=Con*\",$E$243:$E$290,$B305), 0)","v":0},0,{"$f":"INDEX(PO_Enrgy_6_Table,10, 10)","v":""},0,0,null,{"$f":"IFERROR(1-H305/E305,\"\")","v":""},null,{"$f":"IFERROR(1-J305/G305,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C306=\"\",\"\",VLOOKUP(C306,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(SUMIFS(G$243:G$290,$F$243:$F$290,\"=Con*\",$E$243:$E$290,$B306), 0)","v":0},0,{"$f":"INDEX(PO_Enrgy_6_Table,11, 10)","v":""},0,0,null,{"$f":"IFERROR(1-H306/E306,\"\")","v":""},null,{"$f":"IFERROR(1-J306/G306,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C307=\"\",\"\",VLOOKUP(C307,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(SUMIFS(G$243:G$290,$F$243:$F$290,\"=Con*\",$E$243:$E$290,$B307), 0)","v":0},0,{"$f":"INDEX(PO_Enrgy_6_Table,12, 10)","v":""},0,0,null,{"$f":"IFERROR(1-H307/E307,\"\")","v":""},null,{"$f":"IFERROR(1-J307/G307,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},"MWh",{"$f":"IF(C308=\"\",\"\",VLOOKUP(C308,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(SUMIFS(G$243:G$290,$F$243:$F$290,\"=Con*\",$E$243:$E$290,$B308), 0)","v":0},0,{"$f":"INDEX(PO_Enrgy_6_Table,13, 10)","v":""},0,0,null,{"$f":"IFERROR(1-H308/E308,\"\")","v":""},null,{"$f":"IFERROR(1-J308/G308,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C309=\"\",\"\",VLOOKUP(C309,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,{"$f":"INDEX(PO_Enrgy_6_Table,14, 10)","v":""},0,0,null,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C310=\"\",\"\",VLOOKUP(C310,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,{"$f":"INDEX(PO_Enrgy_6_Table,15, 10)","v":""},0,0,null,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_7_Table,0,MATCH(E$295,PO_Enrgy_7_Hdr,0)),INDEX(PO_Enrgy_7_Table,0,MATCH($Q$295,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(F$295,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(G$295,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_7_Table,0,MATCH(H$295,PO_Enrgy_7_Hdr,0)),INDEX(PO_Enrgy_7_Table,0,MATCH($Q$295,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(I$295,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(J$295,PO_Enrgy_7_Hdr,0))),\"\")","v":0},"",null,""]
["G"]
["G"]
["G","Table: Virtual rate (average energy cost per unit energy)"]
["G","Energy Type",null,null,"Baseline",null,null,"Proposed",null,null,"Percent Variance"]
["G","Energy_Type","Units",null,"Base_Virtual_Rate",null,null,"Design_Virtual_Rate",null,null,"Percent_Variance",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",null,"Default_Base","Default_Proposed"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},{"$f":"IFERROR(CONCATENATE(\"$ / \",VLOOKUP($B317,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":"$ / kWh"},{"$f":"IF(C317=\"\",\"\",VLOOKUP(C317,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B317=\"District Cooling\",$B317=\"District Steam\",$B317=\"District Hot Water\")),IF($B317=\"District Cooling\",$V$359,$W$359),VLOOKUP($B317,PO_Enrgy_7_Table,MATCH($G$295,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B317,PO_Enrgy_7_Table,MATCH($E$295,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},"","",{"$f":"IFERROR(IF(AND(DESPath=3,OR($B317=\"District Cooling\",$B317=\"District Steam\",$B317=\"District Hot Water\")),IF($B317=\"District Cooling\",$V$363,$W$363),VLOOKUP($B317,PO_Enrgy_7_Table,MATCH($J$295,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B317,PO_Enrgy_7_Table,MATCH($H$295,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},"","",{"$f":"IFERROR(ABS(1-H317/E317),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B317),\"\",VLOOKUP($B317,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B317),\"\",VLOOKUP($B317,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3},null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B317=\"District Cooling\",$B317=\"District Steam\",$B317=\"District Hot Water\")),IF($B317=\"District Cooling\",$V$359,$W$359),VLOOKUP($B317,PO_Enrgy_7_Table,MATCH($G$295,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B317,PO_Enrgy_7_Table,MATCH($E$295,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B317=\"District Cooling\",$B317=\"District Steam\",$B317=\"District Hot Water\")),IF($B317=\"District Cooling\",$V$363,$W$363),VLOOKUP($B317,PO_Enrgy_7_Table,MATCH($J$295,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B317,PO_Enrgy_7_Table,MATCH($H$295,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""}]
["G","Natural Gas","$ / therm",{"$f":"IF(C318=\"\",\"\",VLOOKUP(C318,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","","",null,null,null,null,null,0.1,0.10500000000000001,null,"",""]
["G","District Cooling","$ / MWh",{"$f":"IF(C319=\"\",\"\",VLOOKUP(C319,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","","",null,null,null,null,null,3.4119999999999999,3.4119999999999999,null,"",""]
["G","District Cooling","$ / MWh",{"$f":"IF(C320=\"\",\"\",VLOOKUP(C320,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","","",null,null,null,null,null,3.4119999999999999,3.4119999999999999,null,"",""]
["G","District Cooling","$ / MWh",{"$f":"IF(C321=\"\",\"\",VLOOKUP(C321,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","","",null,null,null,null,null,3.4119999999999999,3.4119999999999999,null,"",""]
["G","District Cooling","$ / MWh",{"$f":"IF(C322=\"\",\"\",VLOOKUP(C322,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","","",null,null,null,null,null,3.4119999999999999,3.4119999999999999,null,"",""]
["G","District Cooling","$ / MWh",{"$f":"IF(C323=\"\",\"\",VLOOKUP(C323,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","",{"$f":"IFERROR(ABS(1-H323/E323),\"\")","v":""},null,null,null,null,null,3.4119999999999999,3.4119999999999999,null,"",""]
["G","District Cooling","$ / MWh",{"$f":"IF(C324=\"\",\"\",VLOOKUP(C324,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","","",null,null,null,null,null,3.4119999999999999,3.4119999999999999,null,"",""]
["G","District Cooling","$ / MWh",{"$f":"IF(C325=\"\",\"\",VLOOKUP(C325,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","",{"$f":"IFERROR(ABS(1-H325/E325),\"\")","v":""},null,null,null,null,null,3.4119999999999999,3.4119999999999999,null,"",""]
["G","District Cooling","$ / MWh",{"$f":"IF(C326=\"\",\"\",VLOOKUP(C326,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","",{"$f":"IFERROR(ABS(1-H326/E326),\"\")","v":""},null,null,null,null,null,3.4119999999999999,3.4119999999999999,null,"",""]
["G","District Cooling","$ / MWh",{"$f":"IF(C327=\"\",\"\",VLOOKUP(C327,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","",{"$f":"IFERROR(ABS(1-H327/E327),\"\")","v":""},null,null,null,null,null,3.4119999999999999,3.4119999999999999,null,"",""]
["G","District Cooling","$ / MWh",{"$f":"IF(C328=\"\",\"\",VLOOKUP(C328,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","",{"$f":"IFERROR(ABS(1-H328/E328),\"\")","v":""},null,null,null,null,null,3.4119999999999999,3.4119999999999999,null,"",""]
["G",{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},"$ / MWh",{"$f":"IF(C329=\"\",\"\",VLOOKUP(C329,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","",{"$f":"IFERROR(ABS(1-H329/E329),\"\")","v":""},null,null,null,null,null,3.4119999999999999,3.4119999999999999,null,"",""]
["G","District Cooling","$ / MWh",{"$f":"IF(C330=\"\",\"\",VLOOKUP(C330,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","","",null,null,null,null,null,3.4119999999999999,3.4119999999999999,null,"",""]
["G","District Cooling","$ / MWh",{"$f":"IF(C331=\"\",\"\",VLOOKUP(C331,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","","",null,null,null,null,null,3.4119999999999999,3.4119999999999999,null,"",""]
["G"]
["G","Table: Exceptional calculation methods"]
["G","Energy Type","Site Energy Units",null,"Baseline Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site_Energy",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK($B337),\"\",VLOOKUP($B337,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"kWh"},{"$f":"IF(C337=\"\",\"\",VLOOKUP(C337,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(VLOOKUP($B337,PO_Enrgy_7_Table,MATCH($E$295,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B337,PO_Enrgy_3_Table,MATCH($G$86,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B337,PO_Enrgy_7_Table,MATCH($F$295,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B337,PO_Enrgy_3_Table,MATCH($J$86,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B337,PO_Enrgy_7_Table,MATCH($G$295,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B337,PO_Enrgy_3_Table,MATCH($L$86,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B337,PO_Enrgy_7_Table,MATCH($H$295,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B337,PO_Enrgy_4_Table,MATCH($G$86,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B337,PO_Enrgy_7_Table,MATCH($I$295,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B337,PO_Enrgy_4_Table,MATCH($J$86,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B337,PO_Enrgy_7_Table,MATCH($J$295,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B337,PO_Enrgy_4_Table,MATCH($L$86,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(1-H337/E337,\"\")","v":""},null,{"$f":"IFERROR(1-J337/G337,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B337),\"\",VLOOKUP($B337,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B337),\"\",VLOOKUP($B337,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3}]
["G","Natural Gas","therm",{"$f":"IF(C338=\"\",\"\",VLOOKUP(C338,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,{"$f":"IFERROR(VLOOKUP($B338,PO_Enrgy_7_Table,MATCH($J$295,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B338,PO_Enrgy_4_Table,MATCH($L$86,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},"",null,"",null,null,null,0.1,0.10500000000000001]
["G","District Cooling","MWh",{"$f":"IF(C339=\"\",\"\",VLOOKUP(C339,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C340=\"\",\"\",VLOOKUP(C340,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C341=\"\",\"\",VLOOKUP(C341,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C342=\"\",\"\",VLOOKUP(C342,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,{"$f":"IFERROR(1-H342/E342,\"\")","v":""},null,{"$f":"IFERROR(1-J342/G342,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C343=\"\",\"\",VLOOKUP(C343,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,{"$f":"IFERROR(1-H343/E343,\"\")","v":""},null,{"$f":"IFERROR(1-J343/G343,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C344=\"\",\"\",VLOOKUP(C344,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C345=\"\",\"\",VLOOKUP(C345,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,{"$f":"IFERROR(1-H345/E345,\"\")","v":""},null,{"$f":"IFERROR(1-J345/G345,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C346=\"\",\"\",VLOOKUP(C346,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,{"$f":"IFERROR(1-H346/E346,\"\")","v":""},null,{"$f":"IFERROR(1-J346/G346,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C347=\"\",\"\",VLOOKUP(C347,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,{"$f":"IFERROR(1-H347/E347,\"\")","v":""},null,{"$f":"IFERROR(1-J347/G347,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C348=\"\",\"\",VLOOKUP(C348,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,{"$f":"IFERROR(1-H348/E348,\"\")","v":""},null,{"$f":"IFERROR(1-J348/G348,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},"MWh",{"$f":"IF(C349=\"\",\"\",VLOOKUP(C349,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,{"$f":"IFERROR(1-H349/E349,\"\")","v":""},null,{"$f":"IFERROR(1-J349/G349,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C350=\"\",\"\",VLOOKUP(C350,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C351=\"\",\"\",VLOOKUP(C351,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_9_Table,0,MATCH(E$336,PO_Enrgy_9_Hdr,0)),INDEX(PO_Enrgy_9_Table,0,MATCH($Q$336,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(F$336,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(G$336,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_9_Table,0,MATCH(H$336,PO_Enrgy_9_Hdr,0)),INDEX(PO_Enrgy_9_Table,0,MATCH($Q$336,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(I$336,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(J$336,PO_Enrgy_9_Hdr,0))),\"\")","v":0},"",null,""]
["G"]
["G","Table: Streamlined DES Accounting Method (DES Path 3) - District Energy Allocation to Project Based on Average Efficiencies"]
["G","Select the fossil fuel energy type used to generate any district heating or cooling.  Enter the proposed average District Cooling and District Heating efficiencies as applicable. For District Cooling, include chillers, cooling towers, chilled water and condenser water pumps, thermal distribution losses, and any other end-uses contributing towards the energy used to generate and distribute chilled water to the building. For District Heating, include boilers, pumps, thermal distribution losses, and any other end-uses contributing towards the energy used to generate and distribute heating to the building. In the Uploads section of the form, provide details regarding the calculations and or monitoring used to determine the proposed District Energy average efficiency, including any energy simulation outputs for the district plant if using the modeling method.\n\n* Average DES efficiency (COP) per energy source is equal to one unit of thermal energy divided by the input energy for the energy source associated with generating one unit of thermal energy and delivering it to the building. Baseline average efficiency is determined based on chilled water or hot water capacity and ASHRAE 90.1 Appendix G Baseline requirements for on-site CHW and HHW generation equipment (see District Energy Path 3 tab for details)."]
["G","Fuel Source for District Cooling and/or Heating","Site Energy Units",null,"District Cooling ",null,null,"District Heating"]
["G",null,null,null,"Average \nEfficiency \n(COP)*","Site Energy Use \n(Units shown per energy type)","Cost","Average \nEfficiency \n(COP)*","Site Energy Use (Units shown per energy type)","Cost"]
["G","Energy_Type","Energy_Units",null,"Cooling_Avg_Efficiency","Cooling_Site_Energy","Cooling_Cost","Heating_Avg_Effiicency","Heating_Site_Energy","Heating_Cost",null,null,null,null,null,null,null,null,null,null,"Total Baseline","Cost/Unit District Cooling","Cost/Unit District Heating"]
["G","Baseline",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",null,null,null,{"$f":"IFERROR(V361+V360,\"\")","v":""},{"$f":"IFERROR(W361+W360,\"\")","v":""}]
["G",{"$f":"IFERROR(IF(DESPath=3,\"Electricity\",\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B360),\"\",VLOOKUP($B360,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C360=\"\",\"\",VLOOKUP(C360,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(AND(DESPath=3,DistrictCooling,$B$360=\"Electricity\"),DESPath3_Cooling_COP,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(DESPath=3,VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($E$336,PO_Enrgy_9_Hdr,0),FALSE)/$E360*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C360,EnergyUnitsTable,3,FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(F360*VLOOKUP($B360,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(IF(AND(DESPath=3,DistrictHeating,$B$360=\"Electricity\"),DESPath3_Heating_eCOP,\"\"),\"\")","v":""},{"$f":"IF(DESPath = 3,IFERROR(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($E$336,PO_Enrgy_9_Hdr,0),FALSE)/$H360*VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C360,EnergyUnitsTable,3,FALSE),0)+IFERROR(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($E$336,PO_Enrgy_9_Hdr,0),FALSE)/$H360*VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($H360,EnergyUnitsTable,3,FALSE),0),0)","v":0},{"$f":"IFERROR(I360*VLOOKUP($B360,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B360),\"\",VLOOKUP($B360,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B360),\"\",VLOOKUP($B360,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,null,"Elec",{"$f":"IFERROR(VLOOKUP($B360,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)/$E$360*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C360,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B360,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)/$H$360*(IFERROR(VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1)+IFERROR(VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1))/VLOOKUP($C360,EnergyUnitsTable,3,FALSE),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(DESPath=3,IF(MATCH(\"Natural Gas\",PO_Enrgy_1_Index,0)>0,\"Natural Gas\",IF(MATCH(\"Fuel Oil / Diesel\",PO_Enrgy_1_Table,0)>1,\"Fuel Oil / Diesel\",\"\")),\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B361),\"\",VLOOKUP($B361,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C361=\"\",\"\",VLOOKUP(C361,ProjectEnergyTypeTable,3,FALSE))","v":""},null,null,null,{"$f":"IFERROR(IF(AND(DESPath=3,DistrictHeating,$B$360=\"Electricity\"),DESPath3_Heating_fCOP,\"\"),\"\")","v":""},{"$f":"IF(DESPath = 3,IFERROR(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($E$336,PO_Enrgy_9_Hdr,0),FALSE)/$H361*VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C361,EnergyUnitsTable,3,FALSE),0)+IFERROR(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($E$336,PO_Enrgy_9_Hdr,0),FALSE)/$H361*VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($H361,EnergyUnitsTable,3,FALSE),0),0)","v":0},{"$f":"IFERROR(I361*VLOOKUP($B361,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B361),\"\",VLOOKUP($B361,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B361),\"\",VLOOKUP($B361,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,null,"Fuel",{"$f":"IFERROR(VLOOKUP($B361,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)/$E$360*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C361,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B361,PO_Enrgy_8_Table,MATCH($E$316,PO_Enrgy_8_Hdr,0),FALSE)/$H$360*(IFERROR(VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1)+IFERROR(VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1))/VLOOKUP($C361,EnergyUnitsTable,3,FALSE),\"\")","v":""}]
["G","Energy_Type","Energy_Units",null,"Cooling_Avg_Efficiency","Cooling_Site_Energy","Cooling_Cost","Heating_Avg_Effiicency","Heating_Site_Energy","Heating_Cost",null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",null,null,null,"Cost/Unit District Cooling","Cost/Unit District Heating"]
["G","Proposed",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Total Proposed",{"$f":"IFERROR(V364+V365,\"\")","v":""},{"$f":"IFERROR(W364+W365,\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK($B364),\"\",VLOOKUP($B364,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"kWh"},{"$f":"IF(C364=\"\",\"\",VLOOKUP(C364,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,{"$f":"IFERROR(VLOOKUP($B364,PO_Enrgy_9_Table,MATCH($E$336,PO_Enrgy_9_Hdr,0),FALSE)/$E$364*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C364,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(F364*VLOOKUP($B364,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,{"$f":"IF(DESPath = 3,IFERROR(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($H$336,PO_Enrgy_9_Hdr,0),FALSE)/$H364*VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C364,EnergyUnitsTable,3,FALSE),0)+IFERROR(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($H$336,PO_Enrgy_9_Hdr,0),FALSE)/$H364*VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($H364,EnergyUnitsTable,3,FALSE),0),0)","v":0},{"$f":"IFERROR(I364*VLOOKUP($B364,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B364),\"\",VLOOKUP($B364,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B364),\"\",VLOOKUP($B364,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3},null,null,"Elec",{"$f":"IFERROR(VLOOKUP($B364,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)/$E$364*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C364,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B364,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)/$H$364*(IFERROR(VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1)+IFERROR(VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1))/VLOOKUP($C364,EnergyUnitsTable,3,FALSE),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK($B$361),\"\",$B$361),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B365),\"\",VLOOKUP($B365,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C365=\"\",\"\",VLOOKUP(C365,ProjectEnergyTypeTable,3,FALSE))","v":""},null,{"$f":"IFERROR(VLOOKUP($B365,PO_Enrgy_9_Table,MATCH($E$336,PO_Enrgy_9_Hdr,0),FALSE)/$E$364*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C365,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(F365*VLOOKUP($B365,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,{"$f":"IF(DESPath = 3,IFERROR(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($H$336,PO_Enrgy_9_Hdr,0),FALSE)/$H365*VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C365,EnergyUnitsTable,3,FALSE),0)+IFERROR(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($H$336,PO_Enrgy_9_Hdr,0),FALSE)/$H365*VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($H365,EnergyUnitsTable,3,FALSE),0),0)","v":0},{"$f":"IFERROR(I365*VLOOKUP($B365,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B365),\"\",VLOOKUP($B365,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B365),\"\",VLOOKUP($B365,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,null,"Fuel",{"$f":"IFERROR(VLOOKUP($B365,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)/$E$364*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C365,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B365,PO_Enrgy_8_Table,MATCH($H$316,PO_Enrgy_8_Hdr,0),FALSE)/$H$364*(IFERROR(VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1)+IFERROR(VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$336,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1))/VLOOKUP($C365,EnergyUnitsTable,3,FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(G365/E365,\"\")","v":""},{"$f":"IFERROR(J365/H365,\"\")","v":""}]
["G",null,null,null,null,null,null,null,"("]
["G"]
["G","Energy Type","Site Energy Units",null,"Baseline Energy Consumption \nwith District Energy Average Efficiencies \n(if DES Path 3 is used)",null,null,"Proposed Energy Consumption \nwith District Energy Average Efficiencies \n(if DES Path 3 is used)",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK($B371),\"\",VLOOKUP($B371,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"kWh"},{"$f":"IF(C371=\"\",\"\",VLOOKUP(C371,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B371,PO_DESbase_Enrgy_Table,MATCH($F$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B371,PO_DESbase_Enrgy_Table,MATCH($I$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B371<>\"District Cooling\",B371<>\"District Hot Water\",B371<>\"District Steam\")),VLOOKUP($B371,PO_Enrgy_9_Table,MATCH($E$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E371*$R371,\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B371,PO_DESbase_Enrgy_Table,MATCH($G$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B371,PO_DESbase_Enrgy_Table,MATCH($J$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B371<>\"District Cooling\",B371<>\"District Hot Water\",B371<>\"District Steam\")),VLOOKUP($B371,PO_Enrgy_9_Table,MATCH($G$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B371,PO_DESdesign_Enrgy_Table,MATCH($F$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B371,PO_DESdesign_Enrgy_Table,MATCH($I$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B371<>\"District Cooling\",B371<>\"District Hot Water\",B371<>\"District Steam\")),VLOOKUP($B371,PO_Enrgy_9_Table,MATCH($H$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(H371*$R371,\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B371,PO_DESdesign_Enrgy_Table,MATCH($G$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B371,PO_DESdesign_Enrgy_Table,MATCH($J$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B371<>\"District Cooling\",B371<>\"District Hot Water\",B371<>\"District Steam\")),VLOOKUP($B371,PO_Enrgy_9_Table,MATCH($J$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(1-H371/E371,\"\")","v":""},null,{"$f":"IFERROR(1-J371/G371,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B371),\"\",VLOOKUP($B371,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B371),\"\",VLOOKUP($B371,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3}]
["G","Natural Gas","therm",{"$f":"IF(C372=\"\",\"\",VLOOKUP(C372,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,0.1,0.10500000000000001]
["G","District Cooling","MWh",{"$f":"IF(C373=\"\",\"\",VLOOKUP(C373,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C374=\"\",\"\",VLOOKUP(C374,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C375=\"\",\"\",VLOOKUP(C375,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C376=\"\",\"\",VLOOKUP(C376,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,{"$f":"IFERROR(1-H376/E376,\"\")","v":""},null,{"$f":"IFERROR(1-J376/G376,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C377=\"\",\"\",VLOOKUP(C377,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E377*$R377,\"\")","v":0},0,0,{"$f":"IFERROR(H377*$R377,\"\")","v":0},0,{"$f":"IFERROR(1-H377/E377,\"\")","v":""},null,{"$f":"IFERROR(1-J377/G377,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C378=\"\",\"\",VLOOKUP(C378,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C379=\"\",\"\",VLOOKUP(C379,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B379,PO_DESbase_Enrgy_Table,MATCH($F$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B379,PO_DESbase_Enrgy_Table,MATCH($I$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B379<>\"District Cooling\",B379<>\"District Hot Water\",B379<>\"District Steam\")),VLOOKUP($B379,PO_Enrgy_9_Table,MATCH($E$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E379*$R379,\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B379,PO_DESbase_Enrgy_Table,MATCH($G$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B379,PO_DESbase_Enrgy_Table,MATCH($J$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B379<>\"District Cooling\",B379<>\"District Hot Water\",B379<>\"District Steam\")),VLOOKUP($B379,PO_Enrgy_9_Table,MATCH($G$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B379,PO_DESdesign_Enrgy_Table,MATCH($F$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B379,PO_DESdesign_Enrgy_Table,MATCH($I$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B379<>\"District Cooling\",B379<>\"District Hot Water\",B379<>\"District Steam\")),VLOOKUP($B379,PO_Enrgy_9_Table,MATCH($H$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(H379*$R379,\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B379,PO_DESdesign_Enrgy_Table,MATCH($G$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B379,PO_DESdesign_Enrgy_Table,MATCH($J$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B379<>\"District Cooling\",B379<>\"District Hot Water\",B379<>\"District Steam\")),VLOOKUP($B379,PO_Enrgy_9_Table,MATCH($J$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(1-H379/E379,\"\")","v":""},null,{"$f":"IFERROR(1-J379/G379,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C380=\"\",\"\",VLOOKUP(C380,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B380,PO_DESbase_Enrgy_Table,MATCH($F$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B380,PO_DESbase_Enrgy_Table,MATCH($I$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B380<>\"District Cooling\",B380<>\"District Hot Water\",B380<>\"District Steam\")),VLOOKUP($B380,PO_Enrgy_9_Table,MATCH($E$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E380*$R380,\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B380,PO_DESbase_Enrgy_Table,MATCH($G$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B380,PO_DESbase_Enrgy_Table,MATCH($J$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B380<>\"District Cooling\",B380<>\"District Hot Water\",B380<>\"District Steam\")),VLOOKUP($B380,PO_Enrgy_9_Table,MATCH($G$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B380,PO_DESdesign_Enrgy_Table,MATCH($F$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B380,PO_DESdesign_Enrgy_Table,MATCH($I$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B380<>\"District Cooling\",B380<>\"District Hot Water\",B380<>\"District Steam\")),VLOOKUP($B380,PO_Enrgy_9_Table,MATCH($H$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(H380*$R380,\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B380,PO_DESdesign_Enrgy_Table,MATCH($G$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B380,PO_DESdesign_Enrgy_Table,MATCH($J$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B380<>\"District Cooling\",B380<>\"District Hot Water\",B380<>\"District Steam\")),VLOOKUP($B380,PO_Enrgy_9_Table,MATCH($J$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(1-H380/E380,\"\")","v":""},null,{"$f":"IFERROR(1-J380/G380,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C381=\"\",\"\",VLOOKUP(C381,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B381,PO_DESbase_Enrgy_Table,MATCH($F$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B381,PO_DESbase_Enrgy_Table,MATCH($I$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B381<>\"District Cooling\",B381<>\"District Hot Water\",B381<>\"District Steam\")),VLOOKUP($B381,PO_Enrgy_9_Table,MATCH($E$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E381*$R381,\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B381,PO_DESbase_Enrgy_Table,MATCH($G$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B381,PO_DESbase_Enrgy_Table,MATCH($J$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B381<>\"District Cooling\",B381<>\"District Hot Water\",B381<>\"District Steam\")),VLOOKUP($B381,PO_Enrgy_9_Table,MATCH($G$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B381,PO_DESdesign_Enrgy_Table,MATCH($F$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B381,PO_DESdesign_Enrgy_Table,MATCH($I$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B381<>\"District Cooling\",B381<>\"District Hot Water\",B381<>\"District Steam\")),VLOOKUP($B381,PO_Enrgy_9_Table,MATCH($H$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(H381*$R381,\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B381,PO_DESdesign_Enrgy_Table,MATCH($G$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B381,PO_DESdesign_Enrgy_Table,MATCH($J$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B381<>\"District Cooling\",B381<>\"District Hot Water\",B381<>\"District Steam\")),VLOOKUP($B381,PO_Enrgy_9_Table,MATCH($J$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(1-H381/E381,\"\")","v":""},null,{"$f":"IFERROR(1-J381/G381,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C382=\"\",\"\",VLOOKUP(C382,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B382,PO_DESbase_Enrgy_Table,MATCH($F$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B382,PO_DESbase_Enrgy_Table,MATCH($I$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B382<>\"District Cooling\",B382<>\"District Hot Water\",B382<>\"District Steam\")),VLOOKUP($B382,PO_Enrgy_9_Table,MATCH($E$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E382*$R382,\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B382,PO_DESbase_Enrgy_Table,MATCH($G$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B382,PO_DESbase_Enrgy_Table,MATCH($J$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B382<>\"District Cooling\",B382<>\"District Hot Water\",B382<>\"District Steam\")),VLOOKUP($B382,PO_Enrgy_9_Table,MATCH($G$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B382,PO_DESdesign_Enrgy_Table,MATCH($F$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B382,PO_DESdesign_Enrgy_Table,MATCH($I$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B382<>\"District Cooling\",B382<>\"District Hot Water\",B382<>\"District Steam\")),VLOOKUP($B382,PO_Enrgy_9_Table,MATCH($H$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(H382*$R382,\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B382,PO_DESdesign_Enrgy_Table,MATCH($G$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B382,PO_DESdesign_Enrgy_Table,MATCH($J$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B382<>\"District Cooling\",B382<>\"District Hot Water\",B382<>\"District Steam\")),VLOOKUP($B382,PO_Enrgy_9_Table,MATCH($J$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(1-H382/E382,\"\")","v":""},null,{"$f":"IFERROR(1-J382/G382,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},"MWh",{"$f":"IF(C383=\"\",\"\",VLOOKUP(C383,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B383,PO_DESbase_Enrgy_Table,MATCH($F$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B383,PO_DESbase_Enrgy_Table,MATCH($I$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B383<>\"District Cooling\",B383<>\"District Hot Water\",B383<>\"District Steam\")),VLOOKUP($B383,PO_Enrgy_9_Table,MATCH($E$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E383*$R383,\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B383,PO_DESbase_Enrgy_Table,MATCH($G$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B383,PO_DESbase_Enrgy_Table,MATCH($J$358,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B383<>\"District Cooling\",B383<>\"District Hot Water\",B383<>\"District Steam\")),VLOOKUP($B383,PO_Enrgy_9_Table,MATCH($G$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B383,PO_DESdesign_Enrgy_Table,MATCH($F$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B383,PO_DESdesign_Enrgy_Table,MATCH($I$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B383<>\"District Cooling\",B383<>\"District Hot Water\",B383<>\"District Steam\")),VLOOKUP($B383,PO_Enrgy_9_Table,MATCH($H$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(H383*$R383,\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B383,PO_DESdesign_Enrgy_Table,MATCH($G$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B383,PO_DESdesign_Enrgy_Table,MATCH($J$362,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B383<>\"District Cooling\",B383<>\"District Hot Water\",B383<>\"District Steam\")),VLOOKUP($B383,PO_Enrgy_9_Table,MATCH($J$336,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(1-H383/E383,\"\")","v":""},null,{"$f":"IFERROR(1-J383/G383,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C384=\"\",\"\",VLOOKUP(C384,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C385=\"\",\"\",VLOOKUP(C385,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"\"Energy Model Subtotal (\" & PO_SiteUnits & \")\"","v":"Energy Model Subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_10_Table,0,MATCH(E$370,PO_Enrgy_10_Hdr,0)),INDEX(PO_Enrgy_10_Table,0,MATCH($Q$370,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_10_Table,0,MATCH(F$370,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_10_Table,0,MATCH(G$370,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_10_Table,0,MATCH(H$370,PO_Enrgy_10_Hdr,0)),INDEX(PO_Enrgy_10_Table,0,MATCH($Q$370,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_10_Table,0,MATCH(I$370,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_10_Table,0,MATCH(J$370,PO_Enrgy_10_Hdr,0))),\"\")","v":0},"",null,""]
["G"]
["G","Data Center - Performance Rating Method Results"]
["G",{"$f":"CONCATENATE(\"Startup IT Loads: Enter the simulated energy consumption and cost for the Data Center based on Startup IT Loads as defined in the LEED Reference Guide.\",\" Report exceptional calculations and results from the Data Center calculator in the startup load results below,\",\" but do not include renewable energy in these reported results. Provide separate exceptional calculation method uploads as applicable for Startup Loads and for Full build-out.\", \" Also upload simulation outputs and performance rating method calculations with and without the exceptional calculation methods for both Startup IT Loads, and the full buildout IT loads.\",\"\n\n\",IF(DESPath=3,\" Note: The calculations using DES Path 3 must be performed manually for the Startup IT Load method, and supplemental documentation uploaded for the project must show these calculations.\",\"\"))","v":"Startup IT Loads: Enter the simulated energy consumption and cost for the Data Center based on Startup IT Loads as defined in the LEED Reference Guide. Report exceptional calculations and results from the Data Center calculator in the startup load results below, but do not include renewable energy in these reported results. Provide separate exceptional calculation method uploads as applicable for Startup Loads and for Full build-out. Also upload simulation outputs and performance rating method calculations with and without the exceptional calculation methods for both Startup IT Loads, and the full buildout IT loads.\n\n"}]
["G","Table: Performance rating data center - Startup IT loads"]
["G","Energy Type","Site Energy Units",null,"Baseline Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK($B394),\"\",VLOOKUP($B394,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"kWh"},{"$f":"IF(C394=\"\",\"\",VLOOKUP(C394,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,{"$f":"IFERROR(E394*$Q394,\"\")","v":0},null,null,{"$f":"IFERROR(H394*$Q394,\"\")","v":0},null,{"$f":"IFERROR(1-H394/E394,\"\")","v":""},null,{"$f":"IFERROR(1-J394/G394,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B394),\"\",VLOOKUP($B394,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B394),\"\",VLOOKUP($B394,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3}]
["G","Natural Gas","therm",{"$f":"IF(C395=\"\",\"\",VLOOKUP(C395,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,0,null,null,0,null,"",null,"",null,null,null,0.1,0.10500000000000001]
["G","District Cooling","MWh",{"$f":"IF(C396=\"\",\"\",VLOOKUP(C396,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,0,null,null,0,null,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C397=\"\",\"\",VLOOKUP(C397,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,0,null,null,0,null,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C398=\"\",\"\",VLOOKUP(C398,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,0,null,null,0,null,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C399=\"\",\"\",VLOOKUP(C399,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,0,null,null,0,null,{"$f":"IFERROR(1-H399/E399,\"\")","v":""},null,{"$f":"IFERROR(1-J399/G399,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C400=\"\",\"\",VLOOKUP(C400,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,{"$f":"IFERROR(E400*$Q400,\"\")","v":0},null,null,{"$f":"IFERROR(H400*$Q400,\"\")","v":0},null,{"$f":"IFERROR(1-H400/E400,\"\")","v":""},null,{"$f":"IFERROR(1-J400/G400,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C401=\"\",\"\",VLOOKUP(C401,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,0,null,null,0,null,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C402=\"\",\"\",VLOOKUP(C402,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,{"$f":"IFERROR(E402*$Q402,\"\")","v":0},null,null,{"$f":"IFERROR(H402*$Q402,\"\")","v":0},null,{"$f":"IFERROR(1-H402/E402,\"\")","v":""},null,{"$f":"IFERROR(1-J402/G402,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C403=\"\",\"\",VLOOKUP(C403,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,{"$f":"IFERROR(E403*$Q403,\"\")","v":0},null,null,{"$f":"IFERROR(H403*$Q403,\"\")","v":0},null,{"$f":"IFERROR(1-H403/E403,\"\")","v":""},null,{"$f":"IFERROR(1-J403/G403,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C404=\"\",\"\",VLOOKUP(C404,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,{"$f":"IFERROR(E404*$Q404,\"\")","v":0},null,null,{"$f":"IFERROR(H404*$Q404,\"\")","v":0},null,{"$f":"IFERROR(1-H404/E404,\"\")","v":""},null,{"$f":"IFERROR(1-J404/G404,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C405=\"\",\"\",VLOOKUP(C405,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,{"$f":"IFERROR(E405*$Q405,\"\")","v":0},null,null,{"$f":"IFERROR(H405*$Q405,\"\")","v":0},null,{"$f":"IFERROR(1-H405/E405,\"\")","v":""},null,{"$f":"IFERROR(1-J405/G405,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},"MWh",{"$f":"IF(C406=\"\",\"\",VLOOKUP(C406,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,{"$f":"IFERROR(E406*$Q406,\"\")","v":0},null,null,{"$f":"IFERROR(H406*$Q406,\"\")","v":0},null,{"$f":"IFERROR(1-H406/E406,\"\")","v":""},null,{"$f":"IFERROR(1-J406/G406,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C407=\"\",\"\",VLOOKUP(C407,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,0,null,null,0,null,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C408=\"\",\"\",VLOOKUP(C408,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,0,null,null,0,null,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_11_Table,0,MATCH(E$393,PO_Enrgy_11_Hdr,0)),INDEX(PO_Enrgy_11_Table,0,MATCH($Q$393,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_11_Table,0,MATCH(F$393,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_11_Table,0,MATCH(G$393,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_11_Table,0,MATCH(H$393,PO_Enrgy_11_Hdr,0)),INDEX(PO_Enrgy_11_Table,0,MATCH($Q$393,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_11_Table,0,MATCH(I$393,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_11_Table,0,MATCH(J$393,PO_Enrgy_11_Hdr,0))),\"\")","v":0},"",null,""]
["G"]
["G","Table: Performance rating data center - Full load IT loads (tabulated from spreadsheet data entered above)"]
["G","Energy Type","Site Energy Units",null,"Baseline Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK($B415),\"\",VLOOKUP($B415,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"kWh"},{"$f":"IF(C415=\"\",\"\",VLOOKUP(C415,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(VLOOKUP($B415,PO_Enrgy_10_Table,MATCH($E$370,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(E415*$R415,\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B415,PO_Enrgy_10_Table,MATCH($G$370,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B415,PO_Enrgy_10_Table,MATCH($H$370,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(H415*$R415,\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B415,PO_Enrgy_10_Table,MATCH($J$370,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(1-H415/E415,\"\")","v":""},null,{"$f":"IFERROR(1-J415/G415,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B415),\"\",VLOOKUP($B415,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B415),\"\",VLOOKUP($B415,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3}]
["G","Natural Gas","therm",{"$f":"IF(C416=\"\",\"\",VLOOKUP(C416,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,0.1,0.10500000000000001]
["G","District Cooling","MWh",{"$f":"IF(C417=\"\",\"\",VLOOKUP(C417,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C418=\"\",\"\",VLOOKUP(C418,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C419=\"\",\"\",VLOOKUP(C419,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C420=\"\",\"\",VLOOKUP(C420,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,{"$f":"IFERROR(1-H420/E420,\"\")","v":""},null,{"$f":"IFERROR(1-J420/G420,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C421=\"\",\"\",VLOOKUP(C421,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E421*$R421,\"\")","v":0},0,0,{"$f":"IFERROR(H421*$R421,\"\")","v":0},0,{"$f":"IFERROR(1-H421/E421,\"\")","v":""},null,{"$f":"IFERROR(1-J421/G421,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C422=\"\",\"\",VLOOKUP(C422,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C423=\"\",\"\",VLOOKUP(C423,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E423*$R423,\"\")","v":0},0,0,{"$f":"IFERROR(H423*$R423,\"\")","v":0},0,{"$f":"IFERROR(1-H423/E423,\"\")","v":""},null,{"$f":"IFERROR(1-J423/G423,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C424=\"\",\"\",VLOOKUP(C424,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E424*$R424,\"\")","v":0},0,0,{"$f":"IFERROR(H424*$R424,\"\")","v":0},0,{"$f":"IFERROR(1-H424/E424,\"\")","v":""},null,{"$f":"IFERROR(1-J424/G424,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C425=\"\",\"\",VLOOKUP(C425,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E425*$R425,\"\")","v":0},0,0,{"$f":"IFERROR(H425*$R425,\"\")","v":0},0,{"$f":"IFERROR(1-H425/E425,\"\")","v":""},null,{"$f":"IFERROR(1-J425/G425,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C426=\"\",\"\",VLOOKUP(C426,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E426*$R426,\"\")","v":0},0,0,{"$f":"IFERROR(H426*$R426,\"\")","v":0},0,{"$f":"IFERROR(1-H426/E426,\"\")","v":""},null,{"$f":"IFERROR(1-J426/G426,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},"MWh",{"$f":"IF(C427=\"\",\"\",VLOOKUP(C427,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E427*$R427,\"\")","v":0},0,0,{"$f":"IFERROR(H427*$R427,\"\")","v":0},0,{"$f":"IFERROR(1-H427/E427,\"\")","v":""},null,{"$f":"IFERROR(1-J427/G427,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C428=\"\",\"\",VLOOKUP(C428,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C429=\"\",\"\",VLOOKUP(C429,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_12_Table,0,MATCH(E$414,PO_Enrgy_12_Hdr,0)),INDEX(PO_Enrgy_12_Table,0,MATCH($Q$414,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_12_Table,0,MATCH(F$414,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_12_Table,0,MATCH(G$414,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_12_Table,0,MATCH(H$414,PO_Enrgy_12_Hdr,0)),INDEX(PO_Enrgy_12_Table,0,MATCH($Q$414,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_12_Table,0,MATCH(I$414,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_12_Table,0,MATCH(J$414,PO_Enrgy_12_Hdr,0))),\"\")","v":0},"",null,""]
["G"]
["G","Table: Performance rating data center - Average between full Load IT loads and startup IT loads"]
["G","Energy Type","Site Energy Units",null,"Baseline Building Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Building Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK($B436),\"\",VLOOKUP($B436,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"kWh"},{"$f":"IF(C436=\"\",\"\",VLOOKUP(C436,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B436,PO_Enrgy_11_Table,MATCH($E$393,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B436,PO_Enrgy_12_Table,MATCH($E$414,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B436,PO_Enrgy_12_Table,MATCH($E$414,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(E436*$R436,\"\")","v":0},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B436,PO_Enrgy_11_Table,MATCH($G$393,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B436,PO_Enrgy_12_Table,MATCH($G$414,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B436,PO_Enrgy_12_Table,MATCH($G$414,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B436,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B436,PO_Enrgy_12_Table,MATCH($H$414,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B436,PO_Enrgy_12_Table,MATCH($H$414,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(H436*$R436,\"\")","v":0},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B436,PO_Enrgy_11_Table,MATCH($J$393,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B436,PO_Enrgy_12_Table,MATCH($J$414,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B436,PO_Enrgy_12_Table,MATCH($J$414,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(1-H436/E436,\"\")","v":""},null,{"$f":"IFERROR(1-J436/G436,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B436),\"\",VLOOKUP($B436,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B436),\"\",VLOOKUP($B436,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3}]
["G","Natural Gas","therm",{"$f":"IF(C437=\"\",\"\",VLOOKUP(C437,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,0.1,0.10500000000000001]
["G","District Cooling","MWh",{"$f":"IF(C438=\"\",\"\",VLOOKUP(C438,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C439=\"\",\"\",VLOOKUP(C439,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C440=\"\",\"\",VLOOKUP(C440,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C441=\"\",\"\",VLOOKUP(C441,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,{"$f":"IFERROR(1-H441/E441,\"\")","v":""},null,{"$f":"IFERROR(1-J441/G441,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C442=\"\",\"\",VLOOKUP(C442,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E442*$R442,\"\")","v":0},0,0,{"$f":"IFERROR(H442*$R442,\"\")","v":0},0,{"$f":"IFERROR(1-H442/E442,\"\")","v":""},null,{"$f":"IFERROR(1-J442/G442,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C443=\"\",\"\",VLOOKUP(C443,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C444=\"\",\"\",VLOOKUP(C444,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E444*$R444,\"\")","v":0},0,0,{"$f":"IFERROR(H444*$R444,\"\")","v":0},0,{"$f":"IFERROR(1-H444/E444,\"\")","v":""},null,{"$f":"IFERROR(1-J444/G444,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C445=\"\",\"\",VLOOKUP(C445,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E445*$R445,\"\")","v":0},0,0,{"$f":"IFERROR(H445*$R445,\"\")","v":0},0,{"$f":"IFERROR(1-H445/E445,\"\")","v":""},null,{"$f":"IFERROR(1-J445/G445,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C446=\"\",\"\",VLOOKUP(C446,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E446*$R446,\"\")","v":0},0,0,{"$f":"IFERROR(H446*$R446,\"\")","v":0},0,{"$f":"IFERROR(1-H446/E446,\"\")","v":""},null,{"$f":"IFERROR(1-J446/G446,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C447=\"\",\"\",VLOOKUP(C447,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E447*$R447,\"\")","v":0},0,0,{"$f":"IFERROR(H447*$R447,\"\")","v":0},0,{"$f":"IFERROR(1-H447/E447,\"\")","v":""},null,{"$f":"IFERROR(1-J447/G447,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},"MWh",{"$f":"IF(C448=\"\",\"\",VLOOKUP(C448,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E448*$R448,\"\")","v":0},0,0,{"$f":"IFERROR(H448*$R448,\"\")","v":0},0,{"$f":"IFERROR(1-H448/E448,\"\")","v":""},null,{"$f":"IFERROR(1-J448/G448,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C449=\"\",\"\",VLOOKUP(C449,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C450=\"\",\"\",VLOOKUP(C450,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"\"Energy Model Subtotal (\" & PO_SiteUnits & \")\"","v":"Energy Model Subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_13_Table,0,MATCH(E$435,PO_Enrgy_13_Hdr,0)),INDEX(PO_Enrgy_13_Table,0,MATCH($Q$435,PO_Enrgy_13_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(F$435,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(G$435,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_13_Table,0,MATCH(H$435,PO_Enrgy_13_Hdr,0)),INDEX(PO_Enrgy_13_Table,0,MATCH($Q$435,PO_Enrgy_13_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(I$435,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(J$435,PO_Enrgy_12_Hdr,0))),\"\")","v":0},"",null,""]
["G"]
["G","Total energy cost savings (excluding site-generated renewable energy) (%)",null,null,null,null,null,null,null,null,{"$f":"$M$451","v":""}]
["G","Performance Cost Index (PCI) (excluding site-generated renewable energy)",null,null,null,null,null,null,null,null,{"$f":"IFERROR(1-K453,\"\")","v":""}]
["G"]
["G","Table: Renewable energy production"]
["G","Energy Type","Site Energy Units",null,"On-Site Renewable Savings",null,null,"Proposed with On-Site Renewable Energy",null,null,"Percent Cost Savings"]
["G",null,null,null,"Site Energy Use Savings ",{"$f":"\"Source Energy Use Savings \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use Savings \n(Btu x 10^6)"},"Cost Savings","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Renewable_Site_Savings","Renewable_Source_Savings","Renewable_Cost_Savings","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion","Virtual Rate"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK($B460),\"\",VLOOKUP($B460,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"kWh"},{"$f":"IF(C460=\"\",\"\",VLOOKUP(C460,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,VLOOKUP($B460,PO_Enrgy_2_Table,MATCH($E$50,PO_Enrgy_2_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E460*$R460,\"\")","v":0},{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,VLOOKUP($B460,PO_Enrgy_2_Table,MATCH($J$50,PO_Enrgy_2_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B460,PO_Enrgy_13_Table,MATCH($H$435,PO_Enrgy_13_Hdr,0),FALSE)-IF(PO_SiteRenewable=TRUE,VLOOKUP($B460,PO_Enrgy_2_Table,MATCH($E$50,PO_Enrgy_2_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(H460*$R460,\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B460,PO_Enrgy_13_Table,MATCH($J$435,PO_Enrgy_13_Hdr,0),FALSE)-IF(PO_SiteRenewable=TRUE,VLOOKUP($B460,PO_Enrgy_2_Table,MATCH($J$50,PO_Enrgy_2_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(1-$H460/VLOOKUP($B460,PO_Enrgy_13_Table,MATCH($E$435,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},null,{"$f":"IFERROR(1-$J460/VLOOKUP($B460,PO_Enrgy_13_Table,MATCH($G$435,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B460),\"\",VLOOKUP($B460,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B460),\"\",VLOOKUP($B460,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3},{"$f":"IFERROR(G460/E460,\"\")","v":""}]
["G","Natural Gas","therm",{"$f":"IF(C461=\"\",\"\",VLOOKUP(C461,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,0.1,0.10500000000000001,""]
["G","District Cooling","MWh",{"$f":"IF(C462=\"\",\"\",VLOOKUP(C462,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999,""]
["G","District Cooling","MWh",{"$f":"IF(C463=\"\",\"\",VLOOKUP(C463,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999,""]
["G","District Cooling","MWh",{"$f":"IF(C464=\"\",\"\",VLOOKUP(C464,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999,""]
["G","District Cooling","MWh",{"$f":"IF(C465=\"\",\"\",VLOOKUP(C465,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999,""]
["G","District Cooling","MWh",{"$f":"IF(C466=\"\",\"\",VLOOKUP(C466,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E466*$R466,\"\")","v":0},0,0,{"$f":"IFERROR(H466*$R466,\"\")","v":0},0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999,{"$f":"IFERROR(G466/E466,\"\")","v":""}]
["G","District Cooling","MWh",{"$f":"IF(C467=\"\",\"\",VLOOKUP(C467,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999,""]
["G","District Cooling","MWh",{"$f":"IF(C468=\"\",\"\",VLOOKUP(C468,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E468*$R468,\"\")","v":0},0,0,{"$f":"IFERROR(H468*$R468,\"\")","v":0},0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999,{"$f":"IFERROR(G468/E468,\"\")","v":""}]
["G","District Cooling","MWh",{"$f":"IF(C469=\"\",\"\",VLOOKUP(C469,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E469*$R469,\"\")","v":0},0,0,{"$f":"IFERROR(H469*$R469,\"\")","v":0},0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999,{"$f":"IFERROR(G469/E469,\"\")","v":""}]
["G","District Cooling","MWh",{"$f":"IF(C470=\"\",\"\",VLOOKUP(C470,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E470*$R470,\"\")","v":0},0,0,{"$f":"IFERROR(H470*$R470,\"\")","v":0},0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999,{"$f":"IFERROR(G470/E470,\"\")","v":""}]
["G","District Cooling","MWh",{"$f":"IF(C471=\"\",\"\",VLOOKUP(C471,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E471*$R471,\"\")","v":0},0,0,{"$f":"IFERROR(H471*$R471,\"\")","v":0},0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999,{"$f":"IFERROR(G471/E471,\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},"MWh",{"$f":"IF(C472=\"\",\"\",VLOOKUP(C472,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E472*$R472,\"\")","v":0},0,0,{"$f":"IFERROR(H472*$R472,\"\")","v":0},0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999,{"$f":"IFERROR(G472/E472,\"\")","v":""}]
["G","District Cooling","MWh",{"$f":"IF(C473=\"\",\"\",VLOOKUP(C473,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999,""]
["G","District Cooling","MWh",{"$f":"IF(C474=\"\",\"\",VLOOKUP(C474,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999,""]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_14_Table,0,MATCH(E$459,PO_Enrgy_14_Hdr,0)),INDEX(PO_Enrgy_14_Table,0,MATCH($Q$459,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(F$459,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(G$459,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_14_Table,0,MATCH(H$459,PO_Enrgy_14_Hdr,0)),INDEX(PO_Enrgy_14_Table,0,MATCH($Q$459,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(I$459,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(J$459,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-$H475/$E$451,\"\")","v":""},null,{"$f":"IFERROR(1-$J475/$G$451,\"\")","v":""}]
["G"]
["G","Table: Data center PUE3 of startup and full buildout IT loads "]
["G",{"$f":"\"Enter the IT equipment energy consumption \" & IF(Datacenter_Avg=FALSE, \" and total building consumption by end-use including renewable energy \",\"\") & \"for the Startup IT loads.  The information for the full buildout loads is tabulated from the data above.  PUE3 is calculated based on source energy.\"","v":"Enter the IT equipment energy consumption  and total building consumption by end-use including renewable energy for the Startup IT loads.  The information for the full buildout loads is tabulated from the data above.  PUE3 is calculated based on source energy."}]
["G","Energy Type","Site Energy Units",null,"Startup IT Loads\nBuilding energy consumption with Startup IT loads \nincluding Data Center Calculator and exceptional calculation measures",null,null,null,"Full Buildout IT Loads\nBuilding energy consumption with Full Buildout IT loads \nincluding Data Center Calculator and exceptional calculation measures"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"PUE3",null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"PUE3"]
["G","Energy_Type","Energy_Units",null,"Startup_Site_Energy","Startup_Source_Energy","Startup_PUE",null,"Buildout_Site_Energy","Buildout_Source_Energy","Buildoout_PUE",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"B263","v":"IT equipment"},"kWh",{"$f":"IF(C482=\"\",\"\",VLOOKUP(C482,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,{"$f":"IFERROR(E482*$R482,\"\")","v":0},null,null,{"$f":"IFERROR(VLOOKUP(B482,PO_design_table,MATCH($H$242,PO_design_hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(I482*$R482,\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(\"Electricity\",PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(VLOOKUP(\"electricity\",PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE),\"\")","v":8.7005999999999993E-3}]
["G","Total building consumption by end-use",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK($B484),\"\",VLOOKUP($B484,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"kWh"},{"$f":"IF(C484=\"\",\"\",VLOOKUP(C484,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B484,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B484,PO_Enrgy_14_Table,MATCH($E459,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(E484*$R484,\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP($B484,PO_Enrgy_12_Table,MATCH($H$414,PO_Enrgy_12_Hdr,0),FALSE)-VLOOKUP($B484,PO_Enrgy_14_Table,MATCH($E$459,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(I484*$R484,\"\")","v":0},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B484),\"\",VLOOKUP($B484,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B484),\"\",VLOOKUP($B484,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3}]
["G","Natural Gas","therm",{"$f":"IF(C485=\"\",\"\",VLOOKUP(C485,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B485,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B485,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},"",null,null,0,0,null,null,null,null,null,null,0.1,0.10500000000000001]
["G","District Cooling","MWh",{"$f":"IF(C486=\"\",\"\",VLOOKUP(C486,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B486,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B486,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},"",null,null,0,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C487=\"\",\"\",VLOOKUP(C487,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B487,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B487,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},"",null,null,0,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C488=\"\",\"\",VLOOKUP(C488,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B488,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B488,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},"",null,null,0,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C489=\"\",\"\",VLOOKUP(C489,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B489,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B489,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},"",null,null,0,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C490=\"\",\"\",VLOOKUP(C490,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B490,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B490,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(E490*$R490,\"\")","v":""},null,null,0,{"$f":"IFERROR(I490*$R490,\"\")","v":0},null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C491=\"\",\"\",VLOOKUP(C491,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B491,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B491,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},"",null,null,0,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C492=\"\",\"\",VLOOKUP(C492,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B492,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B492,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(E492*$R492,\"\")","v":""},null,null,0,{"$f":"IFERROR(I492*$R492,\"\")","v":0},null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C493=\"\",\"\",VLOOKUP(C493,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B493,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B493,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(E493*$R493,\"\")","v":""},null,null,0,{"$f":"IFERROR(I493*$R493,\"\")","v":0},null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C494=\"\",\"\",VLOOKUP(C494,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B494,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B494,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(E494*$R494,\"\")","v":""},null,null,0,{"$f":"IFERROR(I494*$R494,\"\")","v":0},null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C495=\"\",\"\",VLOOKUP(C495,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B495,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B495,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(E495*$R495,\"\")","v":""},null,null,0,{"$f":"IFERROR(I495*$R495,\"\")","v":0},null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},"MWh",{"$f":"IF(C496=\"\",\"\",VLOOKUP(C496,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B496,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B496,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(E496*$R496,\"\")","v":""},null,null,0,{"$f":"IFERROR(I496*$R496,\"\")","v":0},null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C497=\"\",\"\",VLOOKUP(C497,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B497,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B497,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},"",null,null,0,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C498=\"\",\"\",VLOOKUP(C498,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B498,PO_Enrgy_11_Table,MATCH($H$393,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B498,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},"",null,null,0,0,null,null,null,null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_15_Table,0,MATCH(E$481,PO_Enrgy_15_Hdr,0)),INDEX(PO_Enrgy_15_Table,0,MATCH($Q$481,PO_Enrgy_15_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_15_Table,0,MATCH(F$481,PO_Enrgy_15_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(F499/F482,\"\")","v":""},null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_15_Table,0,MATCH(I$481,PO_Enrgy_15_Hdr,0)),INDEX(PO_Enrgy_15_Table,0,MATCH($Q$481,PO_Enrgy_15_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_15_Table,0,MATCH(J$481,PO_Enrgy_15_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(J499/J482,\"\")","v":""}]
["G"]
["G","Table: Total energy usage"]
["G","Energy Type","Site Energy Units",null,"Baseline",null,null,"Proposed",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK($B505),\"\",VLOOKUP($B505,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":"kWh"},{"$f":"IF(C505=\"\",\"\",VLOOKUP(C505,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(VLOOKUP($B505,PO_Enrgy_13_Table,MATCH($E$435,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(E505*$R505,\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B505,PO_Enrgy_13_Table,MATCH($G$435,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B505,PO_Enrgy_14_Table,MATCH($H$435,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(H505*$R505,\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B505,PO_Enrgy_14_Table,MATCH($J$435,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(1-H505/E505,\"\")","v":""},null,{"$f":"IFERROR(1-J505/G505,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B505),\"\",VLOOKUP($B505,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":3.4120000000000001E-3},{"$f":"IFERROR(IF(ISBLANK($B505),\"\",VLOOKUP($B505,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":8.7005999999999993E-3}]
["G","Natural Gas","therm",{"$f":"IF(C506=\"\",\"\",VLOOKUP(C506,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,0.1,0.10500000000000001]
["G","District Cooling","MWh",{"$f":"IF(C507=\"\",\"\",VLOOKUP(C507,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C508=\"\",\"\",VLOOKUP(C508,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C509=\"\",\"\",VLOOKUP(C509,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C510=\"\",\"\",VLOOKUP(C510,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,{"$f":"IFERROR(1-H510/E510,\"\")","v":""},null,{"$f":"IFERROR(1-J510/G510,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C511=\"\",\"\",VLOOKUP(C511,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E511*$R511,\"\")","v":0},0,0,{"$f":"IFERROR(H511*$R511,\"\")","v":0},0,{"$f":"IFERROR(1-H511/E511,\"\")","v":""},null,{"$f":"IFERROR(1-J511/G511,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C512=\"\",\"\",VLOOKUP(C512,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C513=\"\",\"\",VLOOKUP(C513,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E513*$R513,\"\")","v":0},0,0,{"$f":"IFERROR(H513*$R513,\"\")","v":0},0,{"$f":"IFERROR(1-H513/E513,\"\")","v":""},null,{"$f":"IFERROR(1-J513/G513,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C514=\"\",\"\",VLOOKUP(C514,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E514*$R514,\"\")","v":0},0,0,{"$f":"IFERROR(H514*$R514,\"\")","v":0},0,{"$f":"IFERROR(1-H514/E514,\"\")","v":""},null,{"$f":"IFERROR(1-J514/G514,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C515=\"\",\"\",VLOOKUP(C515,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E515*$R515,\"\")","v":0},0,0,{"$f":"IFERROR(H515*$R515,\"\")","v":0},0,{"$f":"IFERROR(1-H515/E515,\"\")","v":""},null,{"$f":"IFERROR(1-J515/G515,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C516=\"\",\"\",VLOOKUP(C516,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E516*$R516,\"\")","v":0},0,0,{"$f":"IFERROR(H516*$R516,\"\")","v":0},0,{"$f":"IFERROR(1-H516/E516,\"\")","v":""},null,{"$f":"IFERROR(1-J516/G516,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G",{"$f":"IFERROR(IF(ISBLANK(B29),\"\",B29),\"\")","v":"District Cooling"},"MWh",{"$f":"IF(C517=\"\",\"\",VLOOKUP(C517,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,{"$f":"IFERROR(E517*$R517,\"\")","v":0},0,0,{"$f":"IFERROR(H517*$R517,\"\")","v":0},0,{"$f":"IFERROR(1-H517/E517,\"\")","v":""},null,{"$f":"IFERROR(1-J517/G517,\"\")","v":""},null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C518=\"\",\"\",VLOOKUP(C518,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","District Cooling","MWh",{"$f":"IF(C519=\"\",\"\",VLOOKUP(C519,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},0,0,0,0,0,0,"",null,"",null,null,null,3.4119999999999999,3.4119999999999999]
["G","Totals",null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_16_Table,0,MATCH(E$504,PO_Enrgy_16_Hdr,0)),INDEX(PO_Enrgy_16_Table,0,MATCH($Q$504,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(F$504,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(G$504,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_16_Table,0,MATCH(H$504,PO_Enrgy_16_Hdr,0)),INDEX(PO_Enrgy_16_Table,0,MATCH($Q$504,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(I$504,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(J$504,PO_Enrgy_16_Hdr,0))),\"\")","v":0},"",null,""]
["G","Total energy cost savings (including site-generated renewable energy) (%)",null,null,null,null,null,null,null,null,null,null,{"$f":"$M$520","v":""}]
[null,"Performance Cost Indeix (PCI) (including site-generated renewable energy)",null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(1-M521,\"\")","v":""}]
["G"]
["G","Unmet Loads"]
[null,"Enter the non-coincident unmet load hours, consistent with the energy simulation output reports."]
["G","Unmet Loads",null,null,null,"Baseline",null,null,"Proposed"]
["G","Number of hours heating loads not met"]
["G","Number of hours cooling loads not met"]
["G","Totals",null,null,null,{"$f":"IF(ISERROR(F527+F528),0,F527+F528)","v":0},null,null,{"$f":"IF(ISERROR(I527+I528),0,I527+I528)","v":0}]
["G","Compliance",null,null,null,{"$f":"IF(ISERROR(OR(F527+F528,I527+I528)),\"Enter numbers only\",\n     IF(OR(F529>300,I529>300),\"No\",\"Yes\"))","v":"Yes"}]
[null,null,{"$f":"IF(ISERROR(F529+I529),\"\",IF(OR(I529>300,F529>300),\"Revise the model so that the unmet load hours for both the baseline and proposed case are 300 hours or less\",\"\"))","v":""}]
[null,"Quality Assurance Checks"]
[null,{"$f":"IF(MultipleBuildingsExist=\"No\",\"General information\",\"Multiple Building Details\")","v":"General information"},{"$f":"\"Total Area \"&IF(SI_IP_Units=\"IP\",\"(sq ft)\",\"(sq m)\")","v":"Total Area (sq ft)"}]
[null,null,{"$f":"IFERROR(IF(MultipleBuildingsExist=\"No\",\nGI_BldgArea,\nSUMIF(MBD_BS_Index,$H$5,OFFSET(MBD_BS_Index,0,MATCH('1 - Multiple Buildings Details'!$G$22,MBD_BS_Hdr,0)-1,1,1))+SUMIF(MBD_BS_Index,$H$5,OFFSET(MBD_BS_Index,0,MATCH('1 - Multiple Buildings Details'!$H$22,MBD_BS_Hdr,0)-1,1,1))),\"\")","v":0}]
[null,"Lighting",{"$f":"\"Total Area \"&IF(SI_IP_Units=\"IP\",\"(sq ft)\",\"(sq m)\")","v":"Total Area (sq ft)"},"Base Lighting Demand",null,"Design Lighting Demand","Base Exterior Lighting Demand","Design Exterior Lighting Demand","Base Non Tradeable Exterior Lighting Maximum","Design Non Tradeable Exterior Lighting Maximum"]
[null,null,{"$f":"IFERROR(TotalArea,\"\")","v":0},{"$f":"IFERROR(OFFSET(L_IL_SumTable,MATCH($H$5,L_IL_SumIndex,0)-1,MATCH('6b - General Lighting'!$L$107,L_IL_SumHdr,0)-1,1,1),\"\")","v":"Base_Power"},null,{"$f":"IFERROR(OFFSET(L_IL_SumTable,MATCH($H$5,L_IL_SumIndex,0)-1,MATCH('6b - General Lighting'!$O$107,L_IL_SumHdr,0)-1,1,1),\"\")","v":"Design_Power"},{"$f":"IFERROR(OFFSET(L_ExtSum_Table,1,MATCH('6b - General Lighting'!$J$171,L_ExtSum_Hdr,0)-1,1,1),\"\")","v":0},{"$f":"IFERROR(OFFSET(L_ExtSum_Table,1,MATCH('6b - General Lighting'!$M$171,L_ExtSum_Hdr,0)-1,1,1),\"\")","v":0},{"$f":"IFERROR(OFFSET(L_LtgZone_Table,1,MATCH('6b - General Lighting'!$M$134,L_LtgZone_Hdr,0)-1,1,1)+OFFSET(L_NTSurface_Table,MATCH('6b - General Lighting'!$B$165,L_NTSurface_Index,0)-1,MATCH('6b - General Lighting'!$J$158,L_NTSurface_Hdr,0)-1,1,1),\"\")","v":""},{"$f":"IFERROR(OFFSET(L_NTSurface_Table,MATCH('6b - General Lighting'!$B$165,L_NTSurface_Index,0)-1,MATCH('6b - General Lighting'!$M$158,L_NTSurface_Hdr,0)-1,1,1),\"\")","v":0}]
[null,"Shading and Fenestration","Zones Modeled","Baseline Above 40%",null,"App G. Baseline %","Entered Baseline %"]
[null,null,{"$f":"IFERROR(OFFSET('4 - Shading and Fenestration'!S:U,MATCH(CONCATENATE($H$5, \" zones\"),'4 - Shading and Fenestration'!S:S,0)-1,1,1,1),\"\")","v":""},{"$f":"IF(IFERROR(COUNTIFS('4 - Shading and Fenestration'!S:S,$H$5,'4 - Shading and Fenestration'!U:U,TRUE),\"\")>0,TRUE,FALSE)","v":false},null,{"$f":"ROUND('4 - Shading and Fenestration'!D53,3)","v":0},{"$f":"ROUND('4 - Shading and Fenestration'!B53,3)","v":{"$error":"#VALUE!"}}]
[null,"Performance Outputs","Baseline Lighting EFLHs","Design Lighting EFLHs",null,"Base Lighting Demand","Design Lighting Demand","Base Exterior Lighitng Consumption","Design Exterior Lighting Consumption","Base Exterior EFLH","Design Ext EFLH"]
[null,null,{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$243,PO_design_index,0)-2,MATCH($S$242,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$243,PO_design_index,0)-2,MATCH($T$242,PO_design_hdr,0)-1,1,1)),\"\")","v":0},null,{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$243,PO_design_index,0)-1,MATCH($G$242,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$243,PO_design_index,0)-1,MATCH($H$242,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$245,PO_design_index,0)-2,MATCH($G$242,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$245,PO_design_index,0)-2,MATCH($H$242,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$245,PO_design_index,0)-2,MATCH($S$242,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$245,PO_design_index,0)-2,MATCH($T$242,PO_design_hdr,0)-1,1,1)),\"\")","v":0}]
[null,null,"Base Exterior Lighting Demand","Design Exterior Lighting Demand",null,"Base Miscellaneous % of Total","Design Miscellaneous % of Total","Unregulated Load Difference","Base Service Hot Waters % of Total","Design Service Hot Water % of Total","Base Pump Consumption",null,"Base Fan EFLH"]
[null,null,{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$245,PO_design_index,0)-1,MATCH($G$242,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$245,PO_design_index,0)-1,MATCH($H$242,PO_design_hdr,0)-1,1,1)),\"\")","v":0},null,{"$f":"IFERROR((OFFSET(PO_design_table,MATCH($B$261,PO_design_index,0)-2,MATCH($G$242,PO_design_hdr,0)-1,1,1)*OFFSET(PO_design_table,MATCH($B$261,PO_design_index,0)-2,MATCH($Q$242,PO_design_hdr,0)-1,1,1))/OFFSET(PO_ModelSubtotal,0,4,1,1),\"\")","v":""},{"$f":"IFERROR((OFFSET(PO_design_table,MATCH($B$261,PO_design_index,0)-2,MATCH($H$242,PO_design_hdr,0)-1,1,1)*OFFSET(PO_design_table,MATCH($B$261,PO_design_index,0)-2,MATCH($Q$242,PO_design_hdr,0)-1,1,1))/OFFSET(PO_ModelSubtotal,0,7,1,1),\"\")","v":""},null,{"$f":"IFERROR((OFFSET(PO_design_table,MATCH($B$259,PO_design_index,0)-2,MATCH($G$242,PO_design_hdr,0)-1,1,1)*OFFSET(PO_design_table,MATCH($B$259,PO_design_index,0)-2,MATCH($Q$242,PO_design_hdr,0)-1,1,1))/OFFSET(PO_ModelSubtotal,0,4,1,1),\"\")","v":""},{"$f":"IFERROR((OFFSET(PO_design_table,MATCH($B$259,PO_design_index,0)-2,MATCH($H$242,PO_design_hdr,0)-1,1,1)*OFFSET(PO_design_table,MATCH($B$259,PO_design_index,0)-2,MATCH($Q$242,PO_design_hdr,0)-1,1,1))/OFFSET(PO_ModelSubtotal,0,7,1,1),\"\")","v":""},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$251,PO_design_index,0)-2,MATCH($G$242,PO_design_hdr,0)-1,1,1)),\"\")","v":0},null,{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$255,PO_design_index,0)-2,MATCH($S$242,PO_design_hdr,0)-1,1,1)),\"\")","v":0}]
[null,null,"Design Fan EFLH","Base Fan Demand",null,"Design Fan Demand","PV EFLH","Renewable Rate Difference","Proposed Electric Rate","Proposed Gas Rate","Total Baseline Exterior Lighting Demand",null,"Total Design Exterior Lighting Demand"]
[null,null,{"$f":"IFERROR(IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$255,PO_design_index,0)-2,MATCH($T$242,PO_design_hdr,0)-1,1,1)),\"\"),\"\")","v":0},{"$f":"IFERROR(IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$255,PO_design_index,0)-1,MATCH($G$242,PO_design_hdr,0)-1,1,1)),\"\"),\"\")","v":0},null,{"$f":"IFERROR(IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$255,PO_design_index,0)-1,MATCH($H$242,PO_design_hdr,0)-1,1,1)),\"\"),\"\")","v":0},{"$f":"IFERROR(MAX(IFERROR(OFFSET(PO_renewable_table,MATCH(\"Photovoltaic system\",PO_renewable_Index,0)-2,MATCH($S$44,PO_renewable_hdr,0)-1,1,1),0),\nIFERROR(OFFSET(PO_renewable_table,MATCH(\"Solar thermal system\",PO_renewable_Index,0)-2,MATCH($S$44,PO_renewable_hdr,0)-1,1,1),0)),\"\")","v":""},null,{"$f":"IFERROR(OFFSET(PO_Enrgy_8_Table,MATCH(\"Electricity\",PO_Enrgy_8_Index,0)-2,MATCH($H$316,PO_Enrgy_8_Hdr,0)-1,1,1),\"\")","v":""},{"$f":"IFERROR(OFFSET(PO_Enrgy_8_Table,MATCH(\"Natural Gas\",PO_Enrgy_8_Index,0)-2,MATCH($H$316,PO_Enrgy_8_Hdr,0)-1,1,1),\"\")","v":""},{"$f":"IFERROR(GetPerformanceOutputRangeSums(\"PO_QA_BaseExtLtgDem\"),\"\")","v":"Error"},null,{"$f":"IFERROR(GetPerformanceOutputRangeSums(\"PO_QA_DesignExtLtgDem\"),\"\")","v":"Error"}]
[null,"General HVAC","Base non-water systems","Base water systems"]
[null,null,{"$f":"isbasehvac(2)+isbasehvac(3)+isbasehvac(4)+isbasehvac(6)+isbasehvac(9)+isbasehvac(10)","v":0},{"$f":"isbasehvac(1)+isbasehvac(5)+isbasehvac(7)+isbasehvac(8)+isbasehvac(11)+isbasehvac(12)+isbasehvac(13)","v":0}]
[null,"Air-Side HVAC","Base Fan Flow","Design Fan Flow",null,"Base Fan Power","Design Fan Power","Base Cooling Capacity","Design Cooling Capacity","Base Heating Capacity","Design Heating Capacity"]
[null,null,{"$f":"IFERROR(SUMIFS(AHVAC_Base_FanFlow,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_FanFlow,AHVAC_Design_ID,$H$5),\"\")","v":0},null,{"$f":"IFERROR(SUMIFS(AHVAC_Base_FanPower,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_FanPower,AHVAC_Design_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Base_CoolingCap,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_CoolingCap,AHVAC_Design_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Base_HeatingCap,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_HeatingCap,AHVAC_Design_ID,$H$5),\"\")","v":0}]
[null,null,"Base OA","Design OA"]
[null,null,{"$f":"IFERROR(SUMIFS(AHVAC_Base_OAFlow,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_OAFlow,AHVAC_Design_ID,$H$5),\"\")","v":0}]
[]
[null,"Issue",null,null,null,null,null,null,"Project Team Respone",null,null,null,null,null,null,null,"Trigger","Issue Applicable"]
[null,{"$f":"\"The total building area reported in the \"&IF(MultipleBuildingsExist=\"No\",\"General Information\", \"Multiple Building Details\")& \" tab differs from the total building area reported in the Lighting tab (Interior Lighting section) by more than 10%. Please check for consistency and verify that the building areas reported are accurate.\"","v":"The total building area reported in the General Information tab differs from the total building area reported in the Lighting tab (Interior Lighting section) by more than 10%. Please check for consistency and verify that the building areas reported are accurate."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ABS(C534-C536)/MIN(C534,C536)>0.1,TRUE,FALSE),TRUE)","v":true}]
[null,"The vertical glazing areas in the baseline differs from what is required in Table G3.1.1-1.  Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(F538=G538,FALSE,TRUE),FALSE)","v":false}]
[null,"The baseline vertical glazing area is greater than 40% (as reported in the Shading and Fenestration tab, Shading section), which is inconsistent with the requirement of Table G3.1.5(c) (baseline).  Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(D538=TRUE,TRUE,FALSE),TRUE)","v":false}]
[null,"The baseline and/or proposed interior lighting equivalent full load hours (determined by dividing the total annual lighting consumption by the total lighting power as reported in the Performance Outputs tab) is greater than 4,000 hours/year, which is unexpectedly high. Ensure that the lighting models reflect all mandatory controls from Section 9 and reflect the anticipated schedule of operation for the building.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(C540>4000,D540>4000),TRUE,FALSE),TRUE)","v":false}]
[null,"The baseline and/or proposed interior lighting equivalent full load hours (determined by dividing the total annual lighting consumption by the total lighting power as reported in the Performance Outputs tab) differs by more than 10%, which is unexpected.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(ABS(C540-D540)/MIN(C540,D540)>0.1,MIN(C540,D540)=0),TRUE,FALSE),TRUE)","v":true}]
[null,"The interior lighting demand (as reported in the Performance Outputs tab for the baseline and/or proposed) exceeds the lighting power as reported in the Lighting sheet (Summary section) by more than 5%. Ensure that the values reflected in the Lighting sheet are accurate and appropriately reflect the modeled interior lighting power density.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(((F540-D536)/MIN(F540,D536))>0.05,((G540-F536)/MIN(G540,F536))>0.05),TRUE,FALSE),TRUE)","v":true}]
[null,"The Performance Outputs tab shows zero consumption for exterior lighting power in the baseline and/or proposed model.  Confirm that no exterior lighting is included in the building site. Verify that the proposed exterior lighting reflects the actual building design, and the baseline reflects the allowed lighting power from Table G3.6. Ensure that no credit is taken in the proposed for lighting reductions on non‐tradable surfaces.  (Note that additional lighting power allowance cannot be claimed in the baseline for surfaces that are not provided with lighting in the actual design, and that lighting fixtures cannot be double counted for different exterior surfaces).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(H540=0,I540=0),TRUE,FALSE),TRUE)","v":true}]
[null,"The baseline and/or proposed exterior lighting equivalent full load hours (determined by dividing the total annual lighting consumption by the total lighting power as reported in the Performance Outputs tab) is greater than 5,110 hours/year (approximately 14 hours per day) or less than 3,650 hours/year (approximately 10 hours per day). Ensure that the lighting models reflect all mandatory controls from Section 9.4.1.4.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(J540>5110,K540>5110),TRUE,FALSE),TRUE)","v":false}]
[null,"The baseline and/or proposed exterior lighting equivalent full load hours (determined by dividing the total annual lighting consumption by the total lighting power as reported in the Performance Outputs tab) differs by more than 5%, which is unexpected. Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ABS(J540-K540)/MIN(J540,K540)>0.05,TRUE,FALSE),TRUE)","v":true}]
[null,"The baseline and proposed exterior lighting consumption values are within 1% of each other, as reported in the Performance Outputs tab, indicating that the lighting has been modeled nearly identically. Verify that the proposed exterior lighting reflects the actual building design, and the baseline reflects the allowed lighting power from Table G3.6. Ensure that no credit is taken in the proposed for lighting reductions on non‐tradable surfaces. (Note that additional lighting power allowance cannot be claimed in the baseline for surfaces that are not provided with lighting in the actual design, and  that lighting fixtures cannot be double counted for different exterior surfaces.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ABS(H540-I540)/MIN(H540,I540)<0.01,TRUE,FALSE),TRUE)","v":true}]
[null,"The receptacle equipment consumption for the baseline and/or proposed building (as reported in the Performance Outputs tab) is greater than 40% (less than 10%) of the total building site energy usage, which is unexpectedly high (low). This check was made using the Performance rating energy consumption and cost by fuel type table (i.e. before adjustments were made for renewable energy production or an exceptional calculation method). Verify that the receptacle equipment has been modeled as accurately as possible.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(F542>0.4,G542>0.4,F542<0.1,G542<0.1),TRUE,FALSE),TRUE)","v":true}]
[null,"One (or more) of the unregulated end uses differs by more than 3% between the baseline and proposed as reported in the Performance Outputs tab. If savings are being attempted for an unregulated end use, the Exceptional Calculation Method must be followed.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(COUNTIFS(INDEX(PO_design_table,,MATCH($D$242,PO_design_hdr,0)),\"x\",INDEX(PO_design_table,,MATCH($I$242,PO_design_hdr,0)),\">0.03\")+COUNTIFS(INDEX(PO_design_table,,MATCH($D$242,PO_design_hdr,0)),\"x\",INDEX(PO_design_table,,MATCH($I$242,PO_design_hdr,0)),\"<-0.03\")>0,TRUE,FALSE),TRUE)","v":false}]
[null,"The service water heating consumption for the baseline and/or proposed building constitutes more than 15% of the total building site energy usage (as reported in the Performance Outputs tab), which is unexpected. This check was made using the Performance Rating - Energy Consumption and Cost by Fuel Type table (i.e. before any adjustments were made for renewable energy production or an exceptional calculation method). Verify that the service water heating has been modeled as designed, in accordance with Table G3.1.11 (b) (proposed) and that the schedule is typical of the building type in accordance with Table G3.1#4.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(I542>0.15,J542>0.15),TRUE,FALSE),TRUE)","v":true}]
[null,"Pump consumption is reflected in the baseline outputs (as reported in the Performance Outputs tab), even though the baseline HVAC system type is 2, 3, 4, 6, 8, 9, or 10, none of which include an HVAC circulation loop.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AND(C546>0,D546<1),TRUE,FALSE),TRUE)","v":false}]
[null,"The total baseline and proposed air flow rates differ by more than 35% (as reported in the Air-Side HVAC sheet), making it unclear whether the baseline fan air flow rate was sized based on a 20 deg. F supply-air-to-room-air temperature difference, as required by G3.1.2.8.1 for each baseline system. Verify that the proposed has been modeled as designed in accordance with Table G3.1.10(b) (proposed) and that the baseline has been correctly sized in accordance with Appendix G requirements.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ABS(C548-D548)/MIN(C548,D548),TRUE,FALSE),TRUE)","v":true}]
[null,"The baseline and/or proposed fans equivalent full load hours (determined by dividing the total annual fan consumption by the total fan power as reported in the Performance Outputs tab) is greater than 4,000 hours/year, which is unexpectedly high. Ensure that the HVAC system models reflect all mandatory controls from Section 6, and reflect the anticipated schedule of operation for the building. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(M542>4000,C544>4000),TRUE,FALSE),TRUE)","v":false}]
[null,"The baseline and/or proposed fan equivalent full load hours (determined by dividing the total annual fan consumption by the total fan power as reported in the Performance Outputs tab) differs by more than 25%, which is unexpected. Ensure that the HVAC system models reflect all mandatory controls from Section 6, and reflect the anticipated schedule of operation for the building. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ABS(M542-C544)/MIN(M542,C544)>0.25,TRUE,FALSE),TRUE)","v":true}]
[null,"The fan demand (as reported in the Performance Outputs tab) for the baseline and/or proposed exceeds the fan power as reported in the Air-Side HVAC tab (total system fan power) by more than 5%. Ensure that the values reflected in the Air-Side HVAC sheet are accurate and appropriately reflect the modeled fans.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(((D544-F548)/MIN(D544,F548))>0.05,((F544-G548)/MIN(F544,G548))>0.05),TRUE,FALSE),TRUE)","v":true}]
[null,"The fan demand (as reported in the Performance Outputs tab) for the baseline and/or proposed is 60% less than the fan power as reported in the Air-Side HVAC tab, which is unexpected. Ensure that the values reflected in the Air-Side HVAC tab are accurate and appropriately reflect the modeled fans.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(1-(D544/F548)>0.6,1-(F544/G548)>0.6),TRUE,FALSE),TRUE)","v":true}]
[null,"The total baseline and proposed capacities for the cooling and/or heating (as reported in the Air-Side HVAC tab) differ by more than 35%, making it unclear whether the baseline cooling and heating capacities meet the G3.1.2.2 requirement for oversizing by 15% for cooling and 25% for heating. Verify that the proposed has been modeled as designed in accordance with Table G3.1.10(b) and that the baseline has been sized in accordance with Appendix G requirements. Additionally, verify that the baseline capacities were oversized either at the system level or plant level, but not both, and that any other safety factors have been excluded from the baseline.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(ABS(H548-I548)/MIN(H548,I548)>0.35,ABS(J548-K548)/MIN(J548,K548)>0.35),TRUE,FALSE),TRUE)","v":true}]
[null,"The outdoor airflow rate is higher in the baseline model compared to the proposed (as reported in the Air-Side HVAC tab). Section G3.1.2.5 exception (3) requires that if the proposed design has more outdoor air than required by the rating authority (in this case USGBC/GBCI), then the baseline must be modeled with the amount required per EQ Prerequisite Minimum Indoor Air Quality Performance, and will be less than the rate modeled in the proposed. Ensure that the baseline outdoor airflow rate is consistent with that required by EQ Prerequisite Minimum Indoor Air Quality Performance. If applying G3.1.2.5 exception (2), and using an Ez value of 1.0 for the Baseline Case, upload baseline design ventilation rate procedure calculations as described in Standard 62.1 and as required by ASHRAE 90.1 in order to claim credit for this exception.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(C550>D550,TRUE,FALSE),TRUE)","v":false}]
[null,"The equivalent full load hours (determined by dividing the total annual consumption by the total rated capacity/power as reported in the Performance Outputs tab) for the photovoltaic system is greater than 1,500 hours/year, which is unexpectedly high. Provide documentation explaining the calculation method used to estimate the annual energy generated, and indicate all factors influencing the performance, such as derate factor, tilt, orientation, etc.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(G544>1500,TRUE,FALSE),TRUE)","v":true}]
[null,"The virtual energy rate for one or more of the energy types varies by more than 10% (as reported in the Performance Outputs tab). Ensure that the energy rates have been determined using either actual rates or state average energy prices published by DOE's Energy Information Administration. Provide information regarding the utility rate structure including all demand and energy charges and the seasonal and time-of-use structure of the utility tariff.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(COUNTIF(INDEX(PO_Enrgy_8_Table,,MATCH($K$316,PO_Enrgy_8_Hdr,0)),\">0.1\")+COUNTIF(INDEX(PO_Enrgy_8_Table,,MATCH($K$316,PO_Enrgy_8_Hdr,0)),\"<-0.1\")>0,TRUE,FALSE),TRUE)","v":false}]
[null,"The virtual energy rate for the renewable energy varies from the virtual energy rate for the proposed by more than 5% (as reported in the Performance Outputs tab), which is unexpected.  Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,IF(COUNTIF(INDEX(PO_renewable_table,,MATCH($U$44,PO_renewable_hdr,0)),\">0.05\")+COUNTIF(INDEX(PO_renewable_table,,MATCH($U$44,PO_renewable_hdr,0)),\"<-0.05\")>0,TRUE,FALSE),FALSE),TRUE)","v":false}]
[null,"The virtual energy rate for one or more exceptional calculation measures varies from the virtual energy rate for the proposed by more than 10% (as reported in the Performance Outputs tab), which is unexpected.  Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,IF(COUNTIF(INDEX(PO_ExCalc_Table,,MATCH($U$80,PO_ExCalc_Hdr,0)),\">0.05\")+COUNTIF(INDEX(PO_ExCalc_Table,,MATCH($U$80,PO_ExCalc_Hdr,0)),\"<-0.05\")>0,TRUE,FALSE),FALSE),TRUE)","v":false}]
[null,"The proposed virtual energy rate for electricity is less than $0.06 per kWh or greater than $0.25 per kWh (as reported in the Performance Outputs tab), which is unexpected. Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(I544<0.06,I544>0.25),TRUE,FALSE),TRUE)","v":true}]
[null,"The proposed virtual energy rate for natural gas is less than $0.50 per therm or greater than $2.00 per therm (as reported in the Performance Outputs tab), which is unexpected.  Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(J544<0.5,J544>2),TRUE,FALSE),TRUE)","v":true}]
[null,"The Energy Modeling Output Reporting Method (as reported in the Performance Outputs tab) indicates that the baseline has not been rotated because the building orientation is dictated by site considerations, as allowed by Table G3.1 #5 (a) (baseline) Exception 1. Provide a detailed narrative (and additional documentation as necessary) describing why this exception has been applied.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(PO_EnergyReportingMethod>2,TRUE,FALSE),FALSE)","v":false}]
[null,"Two different types of heating consumption (e.g. electricity and natural gas) are reported in the baseline results in the Performance Outputs tab, which is unexpected. If modeling system type 3, note that there should be no crankcase heating or electric space heaters modeled in the baseline. If modeling system type 1, 5, or 7, note that the hot water boiler must be modeled as a natural draft boiler and there should be no electric space heaters modeled in the baseline. Please note that there are some exceptions (e.g. G3.1.1 (b)) which allow this situation; therefore, please be cautious before changing the model as a result of this comment.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AND(COUNTIFS(INDEX(PO_design_table,,MATCH($E$242,PO_design_hdr,0)),\"Electricity\",INDEX(PO_design_table,,MATCH($B$242,PO_design_hdr,0)),\"Space Heating\",INDEX(PO_design_table,,MATCH($G$242,PO_design_hdr,0)),\">0\")>0,COUNTIFS(INDEX(PO_design_table,,MATCH($E$242,PO_design_hdr,0)),\"<>Electricity\",INDEX(PO_design_table,,MATCH($B$242,PO_design_hdr,0)),\"Space Heating\",INDEX(PO_design_table,,MATCH($G$242,PO_design_hdr,0)),\">0\")>0),TRUE,FALSE),TRUE)","v":false}]
[null,"The unmet load hours exceed 300 hours for the baseline and/or proposed (as reported in the Performance Outputs tab), which is not in compliance with G3.1.2.3.  Please correct.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(MAX(F529:M529)>300,TRUE,FALSE),TRUE)","v":false}]
[null,{"$f":"\"The three largest end use contributors to the cost savings are \"&CONCATENATE(VLOOKUP(1,QCEnSaveRank,2,FALSE),\", \", VLOOKUP(2,QCEnSaveRank,2,FALSE), \", \",VLOOKUP(3,QCEnSaveRank,2,FALSE))&\" (as reported in the Performance Outputs tab). Please provide a narrative to justify the savings of these end uses, such as the energy conservation measures which contribute to the savings claimed.\"","v":"The three largest end use contributors to the cost savings are Interior lighting, Exterior lighting, Space heating (as reported in the Performance Outputs tab). Please provide a narrative to justify the savings of these end uses, such as the energy conservation measures which contribute to the savings claimed."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"TRUE","v":true}]
[null,"The rating system requires that a minimum of 2% of the energy savings must come from building power and cooling infrastructure. Provide a narrative describing how this requirement has been met. If necessary, include additional modeling output reports.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(RatingSystemSelection=\"LEED v4 BD+C: Data Centers\",TRUE,FALSE)","v":false}]
[null,"Inputs for the Shading and Fenestration tab indicate that less than 10 zones were modeled for the building.  This is unusually low for a standard submission.  Revise the quantity of zones input or provide a narrative justifying the number of zones used.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(C538<10,TRUE,FALSE),TRUE)","v":false}]
[null,"The exterior lighting demand as reported in the Performance Outputs tab for the baseline and/or proposed exceeds the lighting power reported on the Lighting sheet (Summary section) by more than 5%. Ensure that the values reflected in the Lighting sheet are accurate and appropriately reflect the modeled exterior lighting power density.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"TRUE","v":true}]
[null,"The total exterior lighting power allowance, including the base site allowance, is less than the designed lighting power as reported in the Lighting tab, violating mandatory Section 9.4.2. Verify that the inputs are accurate and modify the exterior lighting design as necessary to show compliance.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"TRUE","v":true}]
[null,"The value for nontradable exterior lighting power (building facades, ATMs and night depositories, entrances and gatehouse inspection stations at guarded facilities, loading areas for law enforcement, fire, ambulance, and other emergency service vehicles, drive-through windows at fast food restaurants, and/or parking near 24-hour retail entrances) is less than the designed lighting power after adding in the unrestricted lighting power allowance as reported in the Lighting sheet, violating mandatory Section 9.4.2. Verify that the inputs are accurate and modify the exterior lighting design as necessary to show compliance.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"TRUE","v":true}]

{"sheet":"Instructions","index":1,"n_rows":50,"n_cols":2,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[null,{"$f":"IF(RatingSystemSelection=\"ENERGY STAR MFHR\",\"ESMFHR Performance Path Calculator (90.1-2016 Appendix G)\",IF(RatingSystemSelection=\"ECCCNYS ASHRAE Standard 90.1 Appendix G\",\"ECCCNYS ASHRAE Standard 90.1 Appendix G\",\"Minimum Energy Performance Calculator\"))","v":"ESMFHR Performance Path Calculator (90.1-2016 Appendix G)"}]
[null,"Whole Building Template"]
[null,"LEED v4 EA Prerequisite Minimum Energy Performance and EA Credit Optimize Energy Performance"]
[null,"2020-05-01"]
[null,"Version 1.4"]
[null,"Background\nThis Calculator is an update to the version released on June 7th, 2016 and reflects the following changes:\n\na. Updated all tabs to reflect simulation rules of ASHRAE Standard 90.1 2016 Appendix G. The previous version was based on the ASHRAE Standard 90.1 2013 Appendix G Excerpts.\n\nb. Expanded functionality to includes additional calculators, including but not limited to conversion from CFM75 air-leakage test results to simulation inputs and many others.\n\nc. Added support for the EPA ENERGY STAR Multifamily High Rise Program (New Construction) Performance Path, by incorporating the areas where EPA Simulation Guidelines – Appendix G 90.1 2016 deviates from 90.1 2016. These EPA-specific features are enabled when user selects “Energy Star MFHR” from the list of rating systems on the General Information tab.\n\nd. The Quality Assurance Checks tab has been expanded since the previous release, as well as the Air-Side HVAC Baseline and Proposed tabs being split. Other updates include, but are not limited to, bug fixes, automatic calculations, spaces for drawing/specifications etc."]
[null,"General Instructions\nComplete this calculator to document the LEED Minimum Energy Performance prerequisite, or ENERGY STAR MFHR compliance when using ASHRAE 90.1 or a LEED approved alternative energy standard.\n\nWhere the template references LEED Reference Guide or LEED rating system requirements, the appropriate programs Simulation Guidelines must be used instead. "]
[]
[null,"Step 1:  Enable macros\nIn order for the template to function correctly, when prompted with a Security Warning, enable macros by clicking Enable Content (Excel 2010, 2013) or by clicking Options -> Enable this content (Excel 2007)"]
[null,"Note: This calculator is for use with Excel for Mac 2011 and Excel 2007 or later."]
[]
[null,"Step 2: Complete all tabs except for Performance Outputs \nComplete the General Info tab before completing any other tabs, since this will show or hide some project-specific information. \n\nProjects participating in EPA Energy Star Multifamily High-rise Program cannot have multiple buildings included in a single project. \n\nThis template is intended to assist energy modelers in developing the ASHRAE 90.1 Appendix G baseline and proposed design models. Many cells with the baseline design inputs are auto-populated based on the appropriate 90.1 requirements. There are also built-in calculators to convert project information into simulation tool inputs. These sheets provide the greatest value to the project team if they are completed during the design process, prior to creating the baseline and proposed design models, and are updated as necessary to reflect changes to the design. \n\nIf the energy modeler and project team waits to fill out the spreadsheet until near the completion of the building design, the team may discover some ASHRAE 90.1 mandatory requirements that have been overlooked, modeling requirements that have not been addressed, and additional time may be required to revise the model and show compliance. Please note that some ASHRAE 90.1 mandatory requirements may not be required by the ENERGY STAR Multifamily High Rise program. Please be sure to refer to the programs Simulation Guidelines. "]
[]
[null,"Step 3: Complete Performance_Outputs tab\nEnter simulation results for the baseline and proposed design models on the Performance_Outputs tab. \n\nFor projects modeled in eQUEST and Trane Trace, the Performance_Outputs tab can be auto-populated by copying simulation reports generated by the software into \"Results from eQUEST\" or \"Results from Trace\" tabs, as appropriate, following instructions on these tabs."]
[]
[null,"Step 4: Review Quality Assurance Checks tab\nPrior to submitting project for review, the energy modeler must confirm that the model inputs listed are consistent with those modeled. \n\nReview the Quality Assurance Checks tab, and address all the areas that are flagged and highlighted in red. Modify inputs in the template and/or the models as appropriate to address the issues, or include explanation why the flagged area is correct for the project.   "]
[null,"If you have any questions or comments regarding the Whole Building Template, please contact Maria Karpman at maria.karpman@karpmanconsulting.net"]
[]
[null,"Instructions for LEED Projects"]
[null,"LEED D+C projects can use this workbook and models in lieu of the LEED Minimum Energy Performance Calculator to document LEED NC v4 or v4.1 Prerequisite: Minimum Energy Performance and Credit: Optimize Energy Performance Credit.\n \n- LEED 2009 or LEED v4 BD+C – Register for and follow requirements for LEED Pilot Credit: Alternative Performance Rating Method. Upload all additional documentation indicated in the Pilot ACP, and in the instructions tab of the LEED v4 Minimum Energy Performance Calculator."]
[]
[null,"\n- LEED v4.1 – Upload all documentation indicated in the relevant LEED v4.1 Guide, and in the instructions tab of the LEED v4.1 Minimum Energy Performance Calculator.\n\nNote: If LEED published requirements vary from the details provided in this calculator, follow the LEED published requirements when submitting for LEED Certification."]
[]
[]
[null,"Color Legend"]
[]
[null,"Tab Heading"]
[]
[null,"Table Headings"]
[]
[null,"User Input"]
[]
[null,"Non-editable cells that auto-populate "]
[]
[null,"Aspects of Proposed Design that are worse than prescriptive requirements of 90.1 that project aspires to exceed (conditional formatting)"]
[]
[null,"Aspects of Proposed Design that are better than prescriptive requirements of 90.1 that project aspires to exceed (conditional formatting)"]
[]
[null,"Aspects of Proposed Design with no conditional formatting implemented"]
[]
[null,"Aspects of Proposed Design that are worse than Baseline requirements of 90.1 (conditional formatting)"]
[]
[null,"Aspects of Proposed Design that are better than Baseline requirements of 90.1  (conditional formatting)"]
[]
[null,"Tab Color Legend"]
[null,"Instructions Tab"]
[null,"Mandatory Baseline and Proposed Design Description Tabs"]
[null,"Mandatory Simulation Outputs Tabs"]
[null,"Non-Mandatory Supporting Tabs"]

{"sheet":"Definitions","index":2,"n_rows":18,"n_cols":3,"rows_kept":18,"cut":false,"hidden":true,"merged":[]}
[]
[null,"DEFINITIONS"]
[]
[]
[null,"baseline building performance","The annual energy cost for a building design, used as a baseline for comparison with above-standard design"]
[]
[null,"combined heat and power","An integrated system that captures the heat, otherwise unused, generated by a single fuel source in the production of electrical power. Also known as cogeneration. (Adapted from U.S. Environmental Protection Agency)"]
[null,"district energy system (DES)","A central energy conversion plant and transmission and distribution system that provides thermal energy to a group of buildings (e.g., a central cooling plant on a university campus). It does not include central energy systems that provide only electricity."]
[null,"DES: downstream equipment","The heating and cooling systems, equipment, and controls located in the project building or on the project site and associated with transporting the thermal energy of the district energy system (DES) into heated and cooled spaces. Downstream equipment includes the thermal connection or interface with the DES, secondary distribution systems in the building, and terminal units."]
[null,"DES: upstream equipment","A heating or cooling system or control associated with the district energy system (DES) but not part of the thermal connection or interface with the DES. Upstream equipment includes the thermal energy conversion plant and all the transmission and distribution equipment associated with transporting the thermal energy to the project building or site."]
[null,"DES Modeling Paths:"]
[null,"DES Path 1: ASHRAE 90.1-2013","Purchased heating and cooling (as applicable) are modeled as cost-neutral in the baseline and proposed case. Local rates for purchased heating and cooling are used to establish the purchased heating and cooling costs. The energy model's scope accounts for only downstream equipment, plus purchased heating and cooling. (Refer to ASHRAE 90.1-2013 for details)."]
[null,"DES Path 2: Full DES Performance Accounting","A virtual DES-equivalent plant for the Proposed case is constructed and compared to code-compliant on-site equipment for the Baseline Case. The Baseline case system type is modeled consistent with an on-site system in ASHRAE 90.1 Appendix G. Average efficiencies for the proposed case are modeled or monitored. (Refer to the LEED v4 Building Design & Construction Reference Guide, Minimum Energy Performance Prerequisite for details.)"]
[null,"DES Path 3: Streamlined DES Modeling","The district thermal energy is metered in both the Baseline and Proposed Case models and reported in this spreadsheet. This spreadsheet assigns default average efficiencies for the baseline case calculated using ASHRAE 90.1-2013 prescriptive requirements for DES equipment. Average efficiencies for the proposed case are modeled or monitored. (Refer to the LEED v4 Building Design & Construction Reference Guide, Minimum Energy Performance Prerequisite for details.)"]
[null,"IT annual energy","Electricity consumption by information technology and telecom equipment which includes servers, networking, and storage equipment over the course of a year"]
[null,"Power Utilization Effectiveness (PUE)","a measure of how efficiently a data center uses its power; specifically, how much power is used by computing equipment rather than for cooling and other overhead"]
[null,"Regulated load","Any building end use that has either a mandatory or a prescriptive requirement in ANSI/ASHRAE/IES Standard 90.1–2013"]
[null,"Server input","the information technology (IT) load as measured at the point of connection (e.g., power receptacle ) of the IT device to the electrical power system. Server input captures the actual power load of the IT device exclusive of any power distribution losses and non-IT loads (e.g., rack-mounted fans)."]

{"sheet":"General Information","index":3,"n_rows":72,"n_cols":27,"rows_kept":72,"cut":false,"hidden":false,"merged":[[11,15,14,15],[11,16,14,16],[11,17,14,17],[2,1,2,5],[43,2,43,5],[41,2,41,5],[4,4,4,5],[6,4,6,5],[34,2,34,5],[36,1,36,5],[37,1,37,5],[8,4,8,5],[32,2,32,5],[71,1,71,5],[70,2,70,5],[53,1,53,5],[63,3,63,5],[63,1,63,2],[69,1,69,5],[65,1,65,5],[67,1,67,3],[67,4,67,5],[66,1,66,3],[66,4,66,5],[61,1,61,2],[60,1,60,2],[57,1,57,5],[39,2,39,4],[50,1,50,5],[45,2,45,5],[49,1,49,5],[52,1,52,5],[47,6,47,9],[48,2,48,5],[62,1,62,2],[62,3,62,5],[61,3,61,5],[47,2,47,5],[58,1,58,5],[48,6,49,9]]}
[null,"General Information"]
[]
[null,"Complete the General Information tab before completing any other tabs. Note that the selections in this tab will determine the selections available within other tabs, including multiple building selections, residential dwelling unit selections, rating system dependent selections, and district energy selections.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional)"]
[]
[null,{"$f":"IF(RatingSystemSelection=\"ENERGY STAR MFHR\",\"LEED Project ID # (please mark as N/A)\",\"LEED Project ID #\")","v":"LEED Project ID # (please mark as N/A)"},null,null,{"$f":"IF(RatingSystemSelection=\"ENERGY STAR MFHR\",\"N/A\",IF(RatingSystemSelection=\"2016 NYS Energy Code ASHRAE 90.1 Appendix G\",\"N/A\",\"\"))","v":"N/A"}]
[]
[null,"Project Name",null,null,null,null,null,null,null,null,{"$f":"C48","v":"ASHRAE 90.1-2013"}]
[]
[null,"Rating system",null,null,"ENERGY STAR MFHR",null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(E9,DropdownData!W:X,2,FALSE),\"\")","v":"Homes"},{"$f":"IF(RatingSystemSelection=\"ENERGY STAR MFHR\",0,1)","v":0}]
[]
[null,"Unit of measurement",null,null,null,"IP units",null,null,null,null,{"$f":"IF(F11=\"SI units\",\"SI\",\"IP\")","v":"IP"},{"$f":"CONCATENATE(C46,\" (\",'General Information'!K11,\")\")","v":"4A (IP)"}]
[null,"Note: The selections above must match the rating system and unit of measurement chosen during project registration.",null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED average BPF (2010,2013,2016)","ES Actual BPF (2007,2010,2013,2016)","NYS Actual BPF(2016)"]
[null,"Project has multiple buildings?",null,null,null,"No",{"$f":"IF(AND(RatingSystemSelection=\"2016 NYS Energy Code ASHRAE 90.1 Appendix G\",MultipleBuildingsExist=\"Yes\"),\"Project should not have multiple buildings.\",\"\")","v":""},null,null,null,null,null,null,null,null,null,"ES Actual BPF (2007,2010,2013,2016)","NYS Actual BPF(2016)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N16=\"Multifamily\",TRUE,FALSE)","v":false},null,null,"ES Actual BPF (2007,2010,2013,2016)","NYS Actual BPF(2016)",null,null,"EFLH","EFLH","EFLH"]
[null,{"$f":"IF(MultipleBuildingsExist=\"Yes\",\"Note: After completing the General Info tab, complete the Multiple Building Details Tab before proceeding to the other tabs.\",\"\")","v":""},null,null,null,"Select Building Type(s)",{"$f":"IF($K$11=\"IP\",\"New Construction Conditioned (sq ft)\",\"New Construction Conditioned (sq m)\")","v":"New Construction Conditioned (sq ft)"},{"$f":"IF($K$11=\"IP\",\"Renovation Conditioned (sq ft)\",\"Renovation Conditioned (sq m)\")","v":"Renovation Conditioned (sq ft)"},{"$f":"IF($K$11=\"IP\",\"New Construction Unconditioned (sq ft)\",\"New Construction Unconditioned (sq m)\")","v":"New Construction Unconditioned (sq ft)"},{"$f":"IF($K$11=\"IP\",\"Renovation Unconditioned (sq ft)\",\"Renovation Unconditioned (sq m)\")","v":"Renovation Unconditioned (sq ft)"},"BPF","Conditioned total",null,{"$f":"INDEX(F17:F20,MATCH(MAX(L17:L20),L17:L20,0))","v":0},{"$f":"SUM(G17:H20)+SUM(I17:J20)","v":0},null,null,null,"Misc. Building Type","Misc. EUI","Lighting","SHW","Misc Load"]
["D",{"$f":"\"Building Type \"&F17","v":"Building Type "},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(RatingSystemSelection=\"ECCCNYS ASHRAE Standard 90.1 Appendix G\",R17,IF(RatingSystemSelection=\"ENERGY STAR MFHR\",Q17,P17)),\"\")","v":""},{"$f":"G17+H17","v":0},{"$f":"SUM(G17:J17)","v":0},null,{"$f":"M17/BuildingArea","v":{"$error":"#DIV/0!"}},{"$f":"IF($K$49=2010,INDEX('BPF 2010'!$C$3:$T$12,MATCH(F17,'BPF 2010'!$B$3:$B$12,0),MATCH(\"Average\",'BPF 2010'!$C$3:$T$3,0)),IF($K$49=2016,INDEX('BPF 2016'!$C$3:$T$12,MATCH(F17,'BPF 2016'!$B$3:$B$12,0),MATCH(\"Average\",'BPF 2016'!$C$3:$T$3,0)),IF($K$49=2013,INDEX('BPF 2013'!$C$3:$T$12,MATCH(F17,'BPF 2013'!$B$3:$B$12,0),MATCH(\"Average\",'BPF 2007'!$C$3:$T$3,0)),IF($K$49=2007,INDEX('BPF 2007'!$C$3:$T$12,MATCH(F17,'BPF 2007'!$B$3:$B$12,0),MATCH(\"Average\",'BPF 2007'!$C$3:$T$3,0)),\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF($K$49=2013,INDEX('BPF 2013'!$C$3:$T$12,MATCH(F17,'BPF 2013'!$B$3:$B$12,0),MATCH($C$46,'BPF 2013'!$C$3:$T$3,0)),IF($K$49=2007,INDEX('BPF 2007'!$C$3:$T$12,MATCH(F17,'BPF 2007'!$B$3:$B$12,0),MATCH($C$46,'BPF 2007'!$C$3:$T$3,0)),IF($K$49=2010,INDEX('BPF 2010'!$C$3:$T$12,MATCH(F17,'BPF 2010'!$B$3:$B$12,0),MATCH($C$46,'BPF 2010'!$C$3:$T$3,0)),IF($K$49=2016,INDEX('BPF 2016'!$C$3:$T$12,MATCH(F17,'BPF 2016'!$B$3:$B$12,0),MATCH($C$46,'BPF 2016'!$C$3:$T$3,0))))))","v":{"$error":"#N/A"}},{"$f":"IF($K$49=2016,INDEX('BPF 2016'!$C$3:$T$12,MATCH(F17,'BPF 2016'!$B$3:$B$12,0),MATCH($C$46,'BPF 2016'!$C$3:$T$3,0)))","v":false},{"$f":"IFERROR(VLOOKUP(F17,'Quality Assurance Checks'!DW2:EU26,1,0),VLOOKUP(\"Office\",'Quality Assurance Checks'!DW2:EU26,1,0))","v":"Office"},{"$f":"IFERROR(O17*VLOOKUP(F17,'Quality Assurance Checks'!DW2:EU26,9,0),O17*VLOOKUP(\"Office\",'Quality Assurance Checks'!DW2:EU26,9,0))","v":{"$error":"#DIV/0!"}},{"$f":"O17*VLOOKUP(F17,'Quality Assurance Checks'!DM2:DU26,5,0)","v":{"$error":"#DIV/0!"}},{"$f":"O17*VLOOKUP(F17,'Quality Assurance Checks'!DM2:DU26,9,0)","v":{"$error":"#DIV/0!"}},{"$f":"O17*VLOOKUP(F17,'Quality Assurance Checks'!DM2:DU26,6,0)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(G17:I17)","v":0}]
["D",{"$f":"\"Building Type \"&F18","v":"Building Type "},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(RatingSystemSelection=\"ECCCNYS ASHRAE Standard 90.1 Appendix G\",R18,IF(RatingSystemSelection=\"ENERGY STAR MFHR\",Q18,P18)),\"\")","v":""},{"$f":"G18+H18","v":0},{"$f":"SUM(G18:J18)","v":0},null,{"$f":"M18/BuildingArea","v":{"$error":"#DIV/0!"}},{"$f":"IF($K$49=2010,INDEX('BPF 2010'!$C$3:$T$12,MATCH(F18,'BPF 2010'!$B$3:$B$12,0),MATCH(\"Average\",'BPF 2010'!$C$3:$T$3,0)),IF($K$49=2016,INDEX('BPF 2016'!$C$3:$T$12,MATCH(F18,'BPF 2016'!$B$3:$B$12,0),MATCH(\"Average\",'BPF 2016'!$C$3:$T$3,0)),IF($K$49=2013,INDEX('BPF 2013'!$C$3:$T$12,MATCH(F18,'BPF 2013'!$B$3:$B$12,0),MATCH(\"Average\",'BPF 2007'!$C$3:$T$3,0)),IF($K$49=2007,INDEX('BPF 2007'!$C$3:$T$12,MATCH(F18,'BPF 2007'!$B$3:$B$12,0),MATCH(\"Average\",'BPF 2007'!$C$3:$T$3,0)),\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF($K$49=2013,INDEX('BPF 2013'!$C$3:$T$12,MATCH(F18,'BPF 2013'!$B$3:$B$12,0),MATCH($C$46,'BPF 2013'!$C$3:$T$3,0)),IF($K$49=2007,INDEX('BPF 2007'!$C$3:$T$12,MATCH(F18,'BPF 2007'!$B$3:$B$12,0),MATCH($C$46,'BPF 2007'!$C$3:$T$3,0)),IF($K$49=2010,INDEX('BPF 2010'!$C$3:$T$12,MATCH(F18,'BPF 2010'!$B$3:$B$12,0),MATCH($C$46,'BPF 2010'!$C$3:$T$3,0)),IF($K$49=2016,INDEX('BPF 2016'!$C$3:$T$12,MATCH(F18,'BPF 2016'!$B$3:$B$12,0),MATCH($C$46,'BPF 2016'!$C$3:$T$3,0))))))","v":{"$error":"#N/A"}},{"$f":"IF($K$49=2016,INDEX('BPF 2016'!$C$3:$T$12,MATCH(F18,'BPF 2016'!$B$3:$B$12,0),MATCH($C$46,'BPF 2016'!$C$3:$T$3,0)))","v":false},{"$f":"IFERROR(VLOOKUP(F18,'Quality Assurance Checks'!DW3:EU27,1,0),VLOOKUP(\"Office\",'Quality Assurance Checks'!DW3:EU27,1,0))","v":"Office"},{"$f":"IFERROR(O18*VLOOKUP(F18,'Quality Assurance Checks'!DW3:EU27,9,0),O18*VLOOKUP(\"Office\",'Quality Assurance Checks'!DW3:EU27,9,0))","v":{"$error":"#DIV/0!"}},{"$f":"O18*VLOOKUP(F18,'Quality Assurance Checks'!DM3:DU27,5,0)","v":{"$error":"#DIV/0!"}},{"$f":"O18*VLOOKUP(F18,'Quality Assurance Checks'!DM3:DU27,9,0)","v":{"$error":"#DIV/0!"}},{"$f":"O18*VLOOKUP(F18,'Quality Assurance Checks'!DM3:DU27,6,0)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(G18:I18)","v":0}]
["D","Building Type ",null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(RatingSystemSelection=\"ECCCNYS ASHRAE Standard 90.1 Appendix G\",R19,IF(RatingSystemSelection=\"ENERGY STAR MFHR\",Q19,P19)),\"\")","v":""},0,0,null,{"$f":"M19/BuildingArea","v":{"$error":"#DIV/0!"}},{"$f":"IF($K$49=2010,INDEX('BPF 2010'!$C$3:$T$12,MATCH(F19,'BPF 2010'!$B$3:$B$12,0),MATCH(\"Average\",'BPF 2010'!$C$3:$T$3,0)),IF($K$49=2016,INDEX('BPF 2016'!$C$3:$T$12,MATCH(F19,'BPF 2016'!$B$3:$B$12,0),MATCH(\"Average\",'BPF 2016'!$C$3:$T$3,0)),IF($K$49=2013,INDEX('BPF 2013'!$C$3:$T$12,MATCH(F19,'BPF 2013'!$B$3:$B$12,0),MATCH(\"Average\",'BPF 2007'!$C$3:$T$3,0)),IF($K$49=2007,INDEX('BPF 2007'!$C$3:$T$12,MATCH(F19,'BPF 2007'!$B$3:$B$12,0),MATCH(\"Average\",'BPF 2007'!$C$3:$T$3,0)),\"\"))))","v":{"$error":"#N/A"}},{"$f":"IF($K$49=2013,INDEX('BPF 2013'!$C$3:$T$12,MATCH(F19,'BPF 2013'!$B$3:$B$12,0),MATCH($C$46,'BPF 2013'!$C$3:$T$3,0)),IF($K$49=2007,INDEX('BPF 2007'!$C$3:$T$12,MATCH(F19,'BPF 2007'!$B$3:$B$12,0),MATCH($C$46,'BPF 2007'!$C$3:$T$3,0)),IF($K$49=2010,INDEX('BPF 2010'!$C$3:$T$12,MATCH(F19,'BPF 2010'!$B$3:$B$12,0),MATCH($C$46,'BPF 2010'!$C$3:$T$3,0)),IF($K$49=2016,INDEX('BPF 2016'!$C$3:$T$12,MATCH(F19,'BPF 2016'!$B$3:$B$12,0),MATCH($C$46,'BPF 2016'!$C$3:$T$3,0))))))","v":{"$error":"#N/A"}},{"$f":"IF($K$49=2016,INDEX('BPF 2016'!$C$3:$T$12,MATCH(F19,'BPF 2016'!$B$3:$B$12,0),MATCH($C$46,'BPF 2016'!$C$3:$T$3,0)))","v":false},{"$f":"IFERROR(VLOOKUP(F19,'Quality Assurance Checks'!DW4:EU28,1,0),VLOOKUP(\"Office\",'Quality Assurance Checks'!DW4:EU28,1,0))","v":"Office"},{"$f":"IFERROR(O19*VLOOKUP(F19,'Quality Assurance Checks'!DW4:EU28,9,0),O19*VLOOKUP(\"Office\",'Quality Assurance Checks'!DW4:EU28,9,0))","v":{"$error":"#DIV/0!"}},{"$f":"O19*VLOOKUP(F19,'Quality Assurance Checks'!DM4:DU28,5,0)","v":{"$error":"#DIV/0!"}},{"$f":"O19*VLOOKUP(F19,'Quality Assurance Checks'!DM4:DU28,9,0)","v":{"$error":"#DIV/0!"}},{"$f":"O19*VLOOKUP(F19,'Quality Assurance Checks'!DM4:DU28,6,0)","v":{"$error":"#DIV/0!"}},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(G20:I20)","v":0}]
[]
[null,null,null,null,null,"Total",{"$f":"G16","v":"New Construction Conditioned (sq ft)"},{"$f":"H16","v":"Renovation Conditioned (sq ft)"},{"$f":"I16","v":"New Construction Unconditioned (sq ft)"},null,"Total Conditioned Area"]
[null,{"$f":"IF($K$11=\"IP\",\"Total building area (sq ft)\",\"Total building area (sq m)\")","v":"Total building area (sq ft)"},null,null,null,{"$f":"O16","v":0},{"$f":"SUM(G17:G20)","v":0},{"$f":"SUM(H17:H20)","v":0},{"$f":"SUM(I17:I20)","v":0},null,{"$f":"SUM(G23:H23)","v":0}]
[null,"Percent of Conditioned Area (%)",null,null,null,"NA",{"$f":"IFERROR(G23/K23,\"-\")","v":"-"},{"$f":"IFERROR(H23/K23,\"-\")","v":"-"},"NA"]
[]
[null,"Project has residential Dwelling Units?",null,null,null,"Yes"]
[]
[null,null,null,null,null,"Above Grade","Below Grade"]
[null,"Number of floors"]
[]
[null,"Energy Model Information"]
[]
[null,"Energy modeler"]
[]
[null,"Energy model based on"]
[]
[null,"Please describe the phase in which the Energy model is based on"]
[null,"NY HP Case study description Rev15"]
[]
[null,"Simulation program","eQuest",null,null,"<Specify Version Number>",{"$f":"IF(F40=\"\",\"Please specify simulation program version number.\",IF(F40=\"<Specify Version Number>\",\"Please specify simulation program version number.\",\"\"))","v":"Please specify simulation program version number."}]
[]
[null,"Energy Modeling Protocol","ASHRAE 90.1 2016 Appendix G",null,null,null,null,null,null,null,{"$f":"IF(C42=\"California Title-24 2013, Part 6\",\"TRUE\",\"FALSE\")","v":"FALSE"}]
[]
[null,"Simulation weather file "]
[]
[null,"Climate zone","4A",null,null,null,null,null,null,null,{"$f":"IF(C46=\"\",\"\",LEFT(C46,1))","v":"4"},{"$f":"IF(OR(C46=\"3B\",C46=\"3C\",C46=\"4A\",C46=\"4B\",C46=\"4C\",C46=\"5A\",C46=\"5B\",C46=\"5C\",C46=\"6A\",C46=\"6B\",C46=\"7A\",C46=\"7B\",C46=\"8\"),\"Gas\",\"Electric\")","v":"Gas"}]
[]
[null,"Version of ASHRAE 90.1 to exceed (reference edition of 90.1)",{"$f":"IF(OR(C49=\"ASHRAE 90.1-2016\",C49=\"ASHRAE 90.1-2013\"),\"ASHRAE 90.1-2013\",C49)","v":"ASHRAE 90.1-2013"},null,null,null,{"$f":"IF(OR(AND(RatingSystemSelection=\"2016 NYS Energy Code ASHRAE 90.1 Appendix G\",C48=\"ASHRAE 90.1-2007\"),AND(RatingSystemSelection=\"2016 NYS Energy Code ASHRAE 90.1 Appendix G\",C48=\"ASHRAE 90.1-2010\")),\"ASHRAE 90.1-2013 is the version of ASHRAE 90.1 to exceed. Please update.\",IF(AND(C48=\"ASHRAE 90.1-2007\",L9=1),\"ASHRAE 90.1-2007 is only supported for the ENERGY STAR HRMF program.\",\"\"))","v":""},null,null,null,{"$f":"IF(AND(C48=\"ASHRAE 90.1-2007\",RatingSystemSelection=\"ENERGY STAR MFHR\"),2007,IF(C48=\"ASHRAE 90.1-2013\",2013,IF(C48=\"ASHRAE 90.1-2010\",2010,\"\")))","v":2013},{"$f":"IF(G48=\"\",\"\",1)","v":""}]
[null,"Version of ASHRAE 90.1 to exceed (reference edition of 90.1)","ASHRAE 90.1-2013",null,null,null,{"$f":"IF(OR(AND(RatingSystemSelection=\"2016 NYS Energy Code ASHRAE 90.1 Appendix G\",C49=\"ASHRAE 90.1-2007\"),AND(RatingSystemSelection=\"2016 NYS Energy Code ASHRAE 90.1 Appendix G\",C49=\"ASHRAE 90.1-2010\")),\"ASHRAE 90.1-2013 is the version of ASHRAE 90.1 to exceed. Please update.\",IF(AND(C49=\"ASHRAE 90.1-2007\",L10=1),\"ASHRAE 90.1-2007 is only supported for the ENERGY STAR HRMF program.\",IF(C49=\"ASHRAE 90.1-2016\",\"Note that the prescriptive and mandatory requirements shown throughout this tool will be for ASHRAE 90.1-2013 as this feature is not supported for 90.1-2016.\",\"\")))","v":""},null,null,null,{"$f":"IF(AND(C48=\"ASHRAE 90.1-2007\",RatingSystemSelection=\"ENERGY STAR MFHR\"),2007,IF(OR(RIGHT(C49,4)=\"2016\",AND(K48=2013,RatingSystemSelection=\"2016 NYS Energy Code ASHRAE 90.1 Appendix G\")),2016,IF(C48=\"ASHRAE 90.1-2013\",2013,IF(C48=\"ASHRAE 90.1-2010\",2010,\"\"))))","v":2013},"BPF"]
[null,"ASHRAE 90.1 2016 Addenda used in the energy model(s), if any.  Addenda are not required to be used for the project. However, each addenda must be used in its entirety if applied to the project, and must be consistent across all relevant LEED Credits."]
[]
[]
[null,"Compliant energy simulation software. The energy simulation software used for this project has all capabilities described in EITHER section \"G2 Simulation General Requirements\" in Appendix G of ASHRAE 90.1 OR the analogous section of the alternative qualifying energy code used."]
[null,"Compliant energy modeling methodology.   Energy simulation runs for both the baseline and proposed use the assumptions and modeling methodology described in EITHER ASHRAE 90.1 Appendix G OR the analogous section of the alternative qualifying energy code used."]
[]
[null,"Are there error or warning messages noted in the simulation program output?",null,null,{"$f":"IF(C56=\"Yes\",\"Please include an explanation of any error messages in the submitted package.\",\"\")","v":""}]
[]
[null,"District Energy Systems"]
[null,"The project is connected to a district or campus thermal energy system. For projects connected to a district or campus thermal energy system where thermal energy is produced for or distributed to multiple buildings, complete the applicable fields below. "]
[null,null,null,null,null,null,null,null,null,null,false]
[null,"The district energy system includes (select all that apply)",null,null,null,null,null,null,null,null,false,false,false]
[null,"Select how the district energy system has been modeled (see Definitions Tab)",null,null,null,null,null,null,null,null,{"$f":"IF(AND(K60=TRUE,LEFT(D62,6)=\"Path 1\"),TRUE,FALSE)","v":false},{"$f":"IF(AND(K60=TRUE,LEFT(D62,6)=\"Path 2\"),TRUE,FALSE)","v":false},{"$f":"IF(AND(K60=TRUE,LEFT(D62,6)=\"Path 3\"),TRUE,FALSE)","v":false},{"$f":"IF(AND(K60=TRUE,LEFT(D62,6)=\"Path 4\"),TRUE,FALSE)","v":false}]
[null,"For DES Paths 2 or 3, identify the method for evaluating the district plant average efficiency.",null,null,null,null,null,null,null,null,{"$f":"IF(D63=\"Modeling Method\",TRUE,FALSE)","v":false},{"$f":"IF(D63=\"Monitoring Method\",TRUE,FALSE)","v":false}]
[null,"If using the DES Path 2 or 3 and the Modeling Method, describe how the average efficiency was determined. Include information about how the thermal distribution losses and distribution pump energy was accounted for. If using the modeling method, upload summary simulation files or spreadsheet calculations as supporting documentation."]
[]
[null,"Rating System Variation",null,null,null,null,null,null,null,null,{"$f":"IF(OR(K67=TRUE,K68=TRUE),TRUE,FALSE)","v":false}]
[null,"An ID+C rating system has been selected. Provide a detailed narrative regarding the method for assigning relative contribution of base building HVAC and service water heating systems. Refer to the LEED v4 ID+C Reference Guide for additional information.",null,null,null,null,null,null,null,null,{"$f":"IF(OR($E$9=\"LEED v4 ID+C: Commercial Interiors\",$E$9=\"LEED v4 ID+C: Retail\",$E$9=\"LEED v4 ID+C: Hospitality\"),TRUE,FALSE)","v":false}]
[null,"The BD+C: Data Center rating system has been selected. By default, the full buildout IT loads are used to determine prerequisite and credit compliance. Select \"Avg of Full IT Load + Startup IT Load\" to the right in order to use the average of the energy modeling results for the full buildout IT loads and the energy modeling results for the startup IT loads to determine prerequisite and credit compliance.",null,null,null,null,null,null,null,null,{"$f":"IF($E$9=\"LEED v4 BD+C: Data Centers\",TRUE,FALSE)","v":false},null,{"$f":"IF(AND(K68=TRUE,E68=\"Avg of Full IT Load + Startup IT Load\"),TRUE,FALSE)","v":false},{"$f":"K68","v":false},{"$f":"IF(OR($E$9=\"LEED v4 ID+C: Retail\",$E$9=\"LEED v4 BD+C: Retail\"),TRUE,FALSE)","v":false}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Data Center Avg.","Data Center","Retail"]
[null,"Unfinished Spaces"]
[null,"Select how any unfinished spaces have been modeled"]
[null,"Refer to the Tenant Lease and Sales Agreement section of the LEED Reference Guide. Upload all required documentation to substantiate the savings claimed for the unfinished spaces."]

{"sheet":"1 - Multiple Buildings Details","index":4,"n_rows":35,"n_cols":18,"rows_kept":35,"cut":false,"hidden":true,"merged":[[33,1,33,4],[14,9,14,10],[31,1,32,2],[14,1,14,8],[9,1,9,10],[10,1,10,10],[22,1,22,3],[24,1,24,3],[16,1,16,8],[16,9,16,10],[23,1,23,3]]}
["G"]
["G","Multiple Building Energy Model Information"]
["G"]
["G"]
["G","How are the buildings modeled?"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
[]
[]
[]
["G",{"$f":"IF(proj_RatingSystem=\"ND\",CONCATENATE(\"The minimum average building energy improvement over ASHRAE 90.1-2010 must be 5% for new buildings, 3% for major building renovations, or 2% for core and shell buildings.\",\" Multiple buildings may be grouped into a single energy model, provided (1) the building type (new construction, major renovation, or core and shell) is consistent for all buildings included in the energy model, \",\"or (2) an average 5% improvement is demonstrated for the entire energy model.\", \"If only a subset of the building energy model details is reported, check the box below, and for the buildings without the details reported here, \",\"report the sum total energy  consumption for the buildings not reported here in the Performance_Output_Residual tab.\",\" Provide a narrative confirming that at least 90% of the building area for ND non-residential, mixed-use and multiunit residential buildings 4 stories or more were modeled\",\", and briefly describing the energy efficiency measures for any buildings where energy model details are not reported here.\"),CONCATENATE(\"The documentation must be sufficient to show that each building individually complies with the prerequisite performance improvement requirements.\",\" If not modeling each building in a separate energy model to show individual compliance, complete the narrative below to justify that all buildings meet the prerequisite performance improvement requirements. \",\"Note: if insufficient information is available in the narrative and input data to prove that all buildings individually meet the prerequisite performance improvement requirements, \",\"additional energy simulation outputs including submetered data per building may be required during the review process to confirm prerequisite compliance per building.\"))","v":"The documentation must be sufficient to show that each building individually complies with the prerequisite performance improvement requirements. If not modeling each building in a separate energy model to show individual compliance, complete the narrative below to justify that all buildings meet the prerequisite performance improvement requirements. Note: if insufficient information is available in the narrative and input data to prove that all buildings individually meet the prerequisite performance improvement requirements, additional energy simulation outputs including submetered data per building may be required during the review process to confirm prerequisite compliance per building."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
["G","Table 1.1: Energy Model Information"]
["G"]
["G","Energy Simulation ID",null,null,null,null,null,null,null,"Multiplier"]
["G","Simulation ID",null,null,null,null,null,null,null,"Multiplier"]
[null,{"$f":"INDEX(MBD_BS_Table,3,1)","v":0},null,null,null,null,null,null,null,{"$f":"INDEX(MBD_BS_Table,3, 5)","v":0}]
[]
["G"]
[null,"Table 1.2: Building Information for Multiple Building Projects"]
["G",null,null,null,"Energy Model",{"$f":"\"Modeled Building Area \"&IF(SI_IP_Units=\"IP\",\"(sq. ft.)\",\"(sq. m.)\")","v":"Modeled Building Area (sq. ft.)"},null,null,"Percent Construction"]
["G","Building ID",null,null,"Simulation ID","Multiplier","Conditioned","Unconditioned","New","Renovation/Existing"]
[null,"Residual Project",null,null,{"$f":"INDEX(MBD_BS_Table,2, 1)","v":"Residual Project"},null,null,null,null,{"$f":"I23","v":0}]
["G",{"$f":"GI_Project_Name","v":0},null,null,1,null,null,null,null,{"$f":"1-I24","v":1}]
["G",{"$f":"GI_Project_Name","v":0},null,null,1,null,null,null,null,{"$f":"1-I25","v":1}]
["G","All"]
[]
["G"]
["G"]
["G","Table 1.3: Project Summary"]
["G"]
["G",null,null,null,null,{"$f":"\"Modeled Building Area \"&IF(SI_IP_Units=\"IP\",\"(sq. ft.)\",\"(sq. m.)\")","v":"Modeled Building Area (sq. ft.)"},null,null,"Percent Construction"]
["G",null,null,null,null,"Total Buildings","Conditioned","Unconditioned","New","Renovation/Existing"]
["G"," Total",null,null,null,{"$f":"SUM(OFFSET(MBD_BS_Index,1,MATCH($F$22,MBD_BS_Hdr,0)-1,ROWS(MBD_BS_Index)-1,1))","v":0},{"$f":"SUM(OFFSET(MBD_BS_Index,1,MATCH($G$22,MBD_BS_Hdr,0)-1,ROWS(MBD_BS_Index)-1,1))","v":0},{"$f":"SUM(OFFSET(MBD_BS_Index,1,MATCH($H$22,MBD_BS_Hdr,0)-1,ROWS(MBD_BS_Index)-1,1))","v":0},{"$f":"(SUMPRODUCT(OFFSET(MBD_BS_Index,1,MATCH($F$22,MBD_BS_Hdr,0)-1,ROWS(MBD_BS_Index)-1,1),OFFSET(MBD_BS_Index,1,MATCH($G$22,MBD_BS_Hdr,0)-1,ROWS(MBD_BS_Index)-1,1),OFFSET(MBD_BS_Index,1,MATCH($I$22,MBD_BS_Hdr,0)-1,ROWS(MBD_BS_Index)-1,1))+SUMPRODUCT(OFFSET(MBD_BS_Index,1,MATCH($F$22,MBD_BS_Hdr,0)-1,ROWS(MBD_BS_Index)-1,1),OFFSET(MBD_BS_Index,1,MATCH($H$22,MBD_BS_Hdr,0)-1,ROWS(MBD_BS_Index)-1,1),OFFSET(MBD_BS_Index,1,MATCH($I$22,MBD_BS_Hdr,0)-1,ROWS(MBD_BS_Index)-1,1)))/(SUMPRODUCT(OFFSET(MBD_BS_Index,1,MATCH($F$22,MBD_BS_Hdr,0)-1,ROWS(MBD_BS_Index)-1,1),OFFSET(MBD_BS_Index,1,MATCH($G$22,MBD_BS_Hdr,0)-1,ROWS(MBD_BS_Index)-1,1))+SUMPRODUCT(OFFSET(MBD_BS_Index,1,MATCH($F$22,MBD_BS_Hdr,0)-1,ROWS(MBD_BS_Index)-1,1),OFFSET(MBD_BS_Index,1,MATCH($H$22,MBD_BS_Hdr,0)-1,ROWS(MBD_BS_Index)-1,1)))","v":{"$error":"#DIV/0!"}},{"$f":"1-I34","v":{"$error":"#DIV/0!"}}]
["G"]

{"sheet":"2a - Schedules","index":5,"n_rows":108,"n_cols":22,"rows_kept":108,"cut":false,"hidden":false,"merged":[[7,21,9,21],[8,11,9,11],[4,1,4,18],[5,1,5,18],[7,1,9,1],[7,2,9,2],[7,3,7,13],[7,14,9,14],[7,15,7,16],[7,17,7,18],[8,3,9,3],[8,4,9,4],[8,6,9,6],[8,7,9,7],[8,8,9,8],[8,9,9,9],[8,5,9,5],[8,18,9,18],[8,10,9,10],[8,12,8,13],[8,15,9,15],[8,16,9,16],[8,17,9,17]]}
["G"]
["G","Schedules"]
["G"]
["G"]
["G",{"$f":"CONCATENATE(\"Complete the table for each building in the project. Provide information for the \",IF(proj_RatingSystem=\"Homes\",\"Dwelling Units\",\"Main Building Schedules\"),\" and for each additional area or set of areas where the schedules differ significantly. Ensure that the reported schedules are consistent with the energy-model entered values, and that schedules account for all mandatory controls. \",IF(proj_RatingSystem=\"Homes\",CONCATENATE(\"Residential lighting shall be for two to four hours per day (700 to 1500 equivalent full load hours per year). See the EFLH Calculator for default Residential Dwelling Unit Schedules that may be input into the energy model.\", \" Corridors and parking garages shall be lit 24 hours per day; parking garages shall include schedule adjustments for occupant sensor controls.\"),\"\" ),\"\",\" Ensure that schedules account for all mandatory controls.\",CHAR(10),\"*Note: The following Equivalent full load schedule information may be optionally excluded from the Table: \",\"(1) End-uses that do not significantly influence overall energy consumption for the project building type (i.e. service water heating for an office building < 5% of total energy consumption),\",\" (2) Spaces modeled with differing schedules that contribute minimally to overall building energy consumption (i.e. electrical/mechanical rooms in a school building that contribute < 5% of total building energy consumption\")","v":"Complete the table for each building in the project. Provide information for the Dwelling Units and for each additional area or set of areas where the schedules differ significantly. Ensure that the reported schedules are consistent with the energy-model entered values, and that schedules account for all mandatory controls. Residential lighting shall be for two to four hours per day (700 to 1500 equivalent full load hours per year). See the EFLH Calculator for default Residential Dwelling Unit Schedules that may be input into the energy model. Corridors and parking garages shall be lit 24 hours per day; parking garages shall include schedule adjustments for occupant sensor controls. Ensure that schedules account for all mandatory controls.\n*Note: The following Equivalent full load schedule information may be optionally excluded from the Table: (1) End-uses that do not significantly influence overall energy consumption for the project building type (i.e. service water heating for an office building < 5% of total energy consumption), (2) Spaces modeled with differing schedules that contribute minimally to overall building energy consumption (i.e. electrical/mechanical rooms in a school building that contribute < 5% of total building energy consumption"}]
["G","Note: The EFLH Calculator tab in this spreadsheet may be used as an optional tool for determining Equivalent Full Load hours of operation"]
["G","Table 2.1: Schedules"]
["G","Building ID","Areas Served","Equivalent Full Load Hours of Operation Per Year (maximum of 8,760). \nLeave blank or enter N/A if not applicable.",null,null,null,null,null,null,null,null,null,null,"Hours per Year HVAC Runs in Occupied Mode",{"$f":"IF(proj_RatingSystem=\"Homes\",\"Active Mode Setpoint\",\"Occupied Mode Setpoint\")","v":"Active Mode Setpoint"},null,"Setback Mode Setpoint",null,null,null,"Additional Notes (Optional):"]
["G",null,null,"Interior Lighting","Service Water Heating","Appliances","Receptacle Equipment","Refriger-ation","Server Equip-ment","Cooking Equip-ment","Elevators / Escalators","Exterior Lighting","Other Loads (Indicate Loads)",null,null,{"$f":"CONCATENATE(\"Cooling\",IF(SI_IP_Units=\"IP\",\" (degrees F)\",\" (degrees C)\"))","v":"Cooling (degrees F)"},{"$f":"CONCATENATE(\"Heating\",IF(SI_IP_Units=\"IP\",\" (degrees F)\",\" (degrees C)\"))","v":"Heating (degrees F)"},{"$f":"CONCATENATE(\"Cooling\",IF(SI_IP_Units=\"IP\",\" (degrees F)\",\" (degrees C)\"))","v":"Cooling (degrees F)"},{"$f":"CONCATENATE(\"Heating\",IF(SI_IP_Units=\"IP\",\" (degrees F)\",\" (degrees C)\"))","v":"Heating (degrees F)"}]
["G"]
[null,{"$f":"B8","v":"Building ID"},{"$f":"C8","v":"Areas Served"},{"$f":"D9","v":"Interior Lighting"},{"$f":"E9","v":"Service Water Heating"},"Appliances","Receptacle Equipment","Refriger-ation","Server Equip-ment","Cooking Equip-ment","Elevators / Escalators","Exterior Lighting","Other Loads (Indicate Loads)",0,{"$f":"O8","v":"Hours per Year HVAC Runs in Occupied Mode"},"Cooling (degrees F)","Heating (degrees F)","Cooling (degrees F)","Heating (degrees F)"]
[{"$f":"IF(RatingSystemSelection=\"ENERGY STAR MFHR\",1,0)","v":1},{"$f":"IF(MultipleBuildingsExist=\"Yes\",\"All\",GI_Project_Name)","v":0},"Dwelling Units",{"$f":"2.34*365","v":854.09999999999991},2628,{"$f":"365*24","v":8760},{"$f":"5.8*365","v":2117},{"$f":"365*24","v":8760},"N/A",{"$f":"365*24","v":8760},"N/A",{"$f":"12*365","v":4380},"N/A","N/A",8760,78,72,80,70]
[{"$f":"IF(RatingSystemSelection=\"ENERGY STAR MFHR\",1,0)","v":1},{"$f":"IF(MultipleBuildingsExist=\"Yes\",\"All\",GI_Project_Name)","v":0},"Common Spaces",{"$f":"365*24","v":8760},null,null,{"$f":"9*365","v":3285},null,null,null,null,{"$f":"12*365","v":4380},null,null,{"$f":"365*24","v":8760},78,72,80,70]
[{"$f":"IF(RatingSystemSelection=\"ENERGY STAR MFHR\",0,1)","v":0},{"$f":"IF(MultipleBuildingsExist=\"Yes\",\"All\",GI_Project_Name)","v":0},"Main Building Schedule",{"$f":"365*24","v":8760},null,null,{"$f":"9*365","v":3285},null,null,null,null,{"$f":"12*365","v":4380},null,null,{"$f":"365*24","v":8760},78,72,80,70]
["G"]
["A",{"$f":"GI_Project_Name","v":0}]
["A",0]
["A",0]
[null,0]
[null,0]
[null,0]
[null,0]
["A"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]

{"sheet":"2b - EFLH Calculator","index":6,"n_rows":532,"n_cols":31,"rows_kept":532,"cut":false,"hidden":false,"merged":[[515,2,515,27],[522,1,522,26],[524,2,524,27],[531,1,531,26],[488,2,488,27],[495,1,495,26],[497,2,497,27],[504,1,504,26],[506,2,506,27],[513,1,513,26],[484,1,484,26],[432,2,432,27],[439,1,439,26],[441,2,441,27],[448,1,448,26],[450,2,450,27],[457,1,457,26],[459,2,459,27],[466,1,466,26],[468,2,468,27],[475,1,475,26],[477,2,477,27],[428,1,428,26],[374,2,374,27],[381,1,381,26],[385,2,385,27],[392,1,392,26],[394,2,394,27],[401,1,401,26],[403,2,403,27],[410,1,410,26],[412,2,412,27],[419,1,419,26],[421,2,421,27],[372,1,372,26],[318,2,318,27],[325,1,325,26],[329,2,329,27],[336,1,336,26],[338,2,338,27],[345,1,345,26],[347,2,347,27],[354,1,354,26],[356,2,356,27],[363,1,363,26],[365,2,365,27],[316,1,316,26],[262,2,262,27],[269,1,269,26],[273,2,273,27],[280,1,280,26],[282,2,282,27],[289,1,289,26],[291,2,291,27],[298,1,298,26],[300,2,300,27],[307,1,307,26],[309,2,309,27],[260,1,260,26],[206,2,206,27],[213,1,213,26],[217,2,217,27],[224,1,224,26],[226,2,226,27],[233,1,233,26],[235,2,235,27],[242,1,242,26],[244,2,244,27],[251,1,251,26],[253,2,253,27],[204,1,204,26],[153,1,153,26],[161,2,161,27],[168,1,168,26],[170,2,170,27],[177,1,177,26],[179,2,179,27],[186,1,186,26],[188,2,188,27],[195,1,195,26],[197,2,197,27],[157,1,157,14],[147,2,147,27],[65,1,65,26],[108,1,108,26],[117,2,117,27],[123,2,123,27],[129,1,129,26],[131,2,131,27],[137,1,137,26],[139,2,139,27],[145,1,145,26],[87,2,87,14],[93,1,93,26],[78,2,78,14],[84,1,84,26],[69,2,69,14],[75,1,75,26],[59,2,59,14],[97,2,97,14],[51,1,51,26],[4,1,4,25],[5,1,5,27],[26,1,26,26],[20,2,20,14],[40,2,40,14],[30,2,30,14],[36,1,36,26]]}
[]
[null,"(OPTIONAL) Equivalent Full Load Hours Calculator"]
[]
[]
[null,{"$f":"CONCATENATE(\"THIS CALCULATOR IS OPTIONAL FOR USE DETERMIING THE EQUIVALENT FULL LOAD HOUR INFORMATION FOR THE SCHEDULES TAB. THE CALCULATOR IS NOT REQUIRED TO BE COMPLETED OR SUBMITTED.\n\", IF(proj_RatingSystem=\"Homes\",\"Default schedules required for LEED-Homes Midrise are shown below for reference. \",IF(ResDwellingUnitsExist=\"Yes\",\"Default schedules for residential dwelling units are shown below for reference.\",\"\")), \" Some of the sample schedules from the ASHRAE 90.1-2013 User's Manual are shown below for reference.\")","v":"THIS CALCULATOR IS OPTIONAL FOR USE DETERMIING THE EQUIVALENT FULL LOAD HOUR INFORMATION FOR THE SCHEDULES TAB. THE CALCULATOR IS NOT REQUIRED TO BE COMPLETED OR SUBMITTED.\nDefault schedules required for LEED-Homes Midrise are shown below for reference.  Some of the sample schedules from the ASHRAE 90.1-2013 User's Manual are shown below for reference."}]
[]
[null,null,"Days per Year"]
[null,"Holiday ",11]
[null,"Monday",50]
[null,"Tuesday",50]
[null,"Wednesday",50]
[null,"Thursday",50]
[null,"Friday",50]
[null,"Saturday",52]
[null,"Sunday",52]
[null,"Total (must equal 365 days/year)",{"$f":"SUM(C8:C15)","v":365}]
[]
[null,"On/Off Schedules"]
[null,"Enter 1 for \"On\", 0 for \"Off."]
[]
[null,"Schedule Name:"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","Hours/day","Hours/year",null,null,"Additional Notes (Optional):"]
[null,"Weekday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(C24:Z24)","v":0},{"$f":"AA24*SUM($C$9:$C$13)","v":0}]
[null,"Weekend",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(C25:Z25)","v":0},{"$f":"AA25*SUM($C$14:$C$15)","v":0}]
[null,"Holiday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(C26:Z26)","v":0},{"$f":"AA26*$C$8","v":0}]
[null,"Total hours of operation per year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB24:AB26)","v":0}]
[]
[]
[]
[null,"Schedule Name:"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","Hours/day","Hours/year"]
[null,"Weekday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(C34:Z34)","v":0},{"$f":"AA34*SUM($C$9:$C$13)","v":0}]
[null,"Weekend",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(C35:Z35)","v":0},{"$f":"AA35*SUM($C$14:$C$15)","v":0}]
[null,"Holiday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(C36:Z36)","v":0},{"$f":"AA36*$C$8","v":0}]
[null,"Total hours of operation per year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB34:AB36)","v":0}]
[]
[]
[]
[null,"Schedule Name:"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","Hours/day","Hours/year"]
[null,"Holiday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(C44:Z44)","v":0},{"$f":"AA44*$C$8","v":0}]
[null,"Monday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA45*$C$9","v":0}]
[null,"Tuesday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA46*$C$10","v":0}]
[null,"Wednesday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA47*$C$11","v":0}]
[null,"Thursday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA48*$C$12","v":0}]
[null,"Friday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA49*$C$13","v":0}]
[null,"Saturday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA50*$C$14","v":0}]
[null,"Sunday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA51*$C$15","v":0}]
[null,"Total hours of operation per year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB44:AB51)","v":0}]
[]
[]
[]
[]
[null,"Fraction / Percentage Schedules"]
[null,"Enter a percentage value between 0% and 100%"]
[]
[null,"Schedule Name:"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0,0,0,0,0,0.1,0.3,0.3,0,0,0,0,0,0,0,0,0,0,0.5,0.5,0.5,0.1,0.04,0,{"$f":"SUM(C63:Z63)","v":2.3400000000000003},{"$f":"AA63*SUM($C$9:$C$13)","v":585.00000000000011}]
[null,"Weekend",0,0,0,0,0,0.1,0.3,0.3,0,0,0,0,0,0,0,0,0,0,0.5,0.5,0.5,0.1,0.04,0,{"$f":"SUM(C64:Z64)","v":2.3400000000000003},{"$f":"AA64*SUM($C$14:$C$15)","v":243.36000000000004}]
[null,"Holiday",0,0,0,0,0,0.1,0.3,0.3,0,0,0,0,0,0,0,0,0,0,0.5,0.5,0.5,0.1,0.04,0,{"$f":"SUM(C65:Z65)","v":2.3400000000000003},{"$f":"AA65*$C$8","v":25.740000000000002}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB63:AB65)","v":854.10000000000014}]
[]
[]
[]
[null,"Schedule Name:"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.12,0.12,0.12,0.12,0.12,0.12,0.36,0.36,0.36,0.36,0.24,0.24,0.24,0.24,0.24,0.24,0.24,0.24,0.36,0.36,0.36,0.36,0.12,0.12,{"$f":"SUM(C73:Z73)","v":5.7600000000000025},{"$f":"AA73*SUM($C$9:$C$13)","v":1440.0000000000007}]
[null,"Weekend",0.12,0.12,0.12,0.12,0.12,0.12,0.36,0.36,0.36,0.36,0.24,0.24,0.24,0.24,0.24,0.24,0.24,0.24,0.36,0.36,0.36,0.36,0.12,0.12,{"$f":"SUM(C74:Z74)","v":5.7600000000000025},{"$f":"AA74*SUM($C$14:$C$15)","v":599.0400000000003}]
[null,"Holiday",0.12,0.12,0.12,0.12,0.12,0.12,0.36,0.36,0.36,0.36,0.24,0.24,0.24,0.24,0.24,0.24,0.24,0.24,0.36,0.36,0.36,0.36,0.12,0.12,{"$f":"SUM(C75:Z75)","v":5.7600000000000025},{"$f":"AA75*$C$8","v":63.360000000000028}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB73:AB75)","v":2102.400000000001}]
[]
[]
[null,"Schedule Name:"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.2,0.2,0.2,0.2,0.2,0.2,0.6,0.6,0.6,0.6,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.6,0.6,0.6,0.6,0.2,0.2,{"$f":"SUM(C82:Z82)","v":9.6},{"$f":"AA82*SUM($C$9:$C$13)","v":2400}]
[null,"Weekend",0.2,0.2,0.2,0.2,0.2,0.2,0.6,0.6,0.6,0.6,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.6,0.6,0.6,0.6,0.2,0.2,{"$f":"SUM(C83:Z83)","v":9.6},{"$f":"AA83*SUM($C$14:$C$15)","v":998.4}]
[null,"Holiday",0.2,0.2,0.2,0.2,0.2,0.2,0.6,0.6,0.6,0.6,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.6,0.6,0.6,0.6,0.2,0.2,{"$f":"SUM(C84:Z84)","v":9.6},{"$f":"AA84*$C$8","v":105.6}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB82:AB84)","v":3504}]
[]
[]
[null,"Schedule Name:"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.05,0.29649999999999999,0.78900000000000003,0.9,0.9,0.9,0.9,0.9,0.9,0.9,0.9,0.78900000000000003,0.50049999999999994,0.29649999999999999,0.29649999999999999,0.10100000000000001,0.10100000000000001,0.05,0.05,{"$f":"SUM(C91:Z91)","v":10.770000000000005},{"$f":"AA91*SUM($C$9:$C$13)","v":2692.5000000000014}]
[null,"Weekend",1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,{"$f":"SUM(C92:Z92)","v":0.36000000000000021},{"$f":"AA92*SUM($C$14:$C$15)","v":37.440000000000019}]
[null,"Holiday",1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,1.4999999999999999E-2,{"$f":"SUM(C93:Z93)","v":0.36000000000000021},{"$f":"AA93*$C$8","v":3.9600000000000022}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB91:AB93)","v":2733.9000000000015}]
[]
[]
[]
[null,"Schedule Name:"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/day"]
[null,"Holiday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(C101:Z101)","v":0},{"$f":"AA101*$C$8","v":0}]
[null,"Monday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA102*$C$9","v":0}]
[null,"Tuesday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA103*$C$10","v":0}]
[null,"Wednesday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA104*$C$11","v":0}]
[null,"Thursday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA105*$C$12","v":0}]
[null,"Friday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA106*$C$13","v":0}]
[null,"Saturday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA107*$C$14","v":0}]
[null,"Sunday",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"AA108*$C$15","v":0}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB101:AB108)","v":0}]
[]
[]
[]
[]
[null,"Default Schedules"]
[]
[null,"Residential Dwelling Unit Default Schedules"]
[]
[null,"Schedule Name:","Dwelling Unit Thermostat setpoint schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","Hours/day","Hours/year"]
[null,"Daily Heating Setpoint",{"$f":"IF(SI_IP_Units=\"IP\",70,CONVERT(70,\"F\",\"C\"))","v":70},70,70,70,70,70,{"$f":"IF(SI_IP_Units=\"IP\",72,CONVERT(72,\"F\",\"C\"))","v":72},72,72,72,72,72,72,72,72,72,72,72,72,72,72,72,72,{"$f":"IF(SI_IP_Units=\"IP\",70,CONVERT(70,\"F\",\"C\"))","v":70},24,8760]
[null,"Daily Cooling Setpoint",{"$f":"IF(SI_IP_Units=\"IP\",78,CONVERT(78,\"F\",\"C\"))","v":78},78,78,78,78,78,78,78,78,{"$f":"IF(SI_IP_Units=\"IP\",80,CONVERT(80,\"F\",\"C\"))","v":80},80,80,80,80,80,{"$f":"IF(SI_IP_Units=\"IP\",78,CONVERT(78,\"F\",\"C\"))","v":78},78,78,78,78,78,78,78,78,24,8760]
[]
[null,"Schedule Name:","Dwelling Unit Lighting Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",1.6E-2,1.6E-2,1.6E-2,1.6E-2,1.6E-2,1.6E-2,7.6999999999999999E-2,0.14000000000000001,0.14000000000000001,0.108,0.108,0.108,7.6999999999999999E-2,7.6999999999999999E-2,7.6999999999999999E-2,7.6999999999999999E-2,7.6999999999999999E-2,0.108,0.217,0.217,0.217,0.217,0.186,1.6E-2,{"$f":"SUM(C127:Z127)","v":2.3400000000000003},{"$f":"AA127*SUM($C$9:$C$13)","v":585.00000000000011}]
[null,"Weekend",1.6E-2,1.6E-2,1.6E-2,1.6E-2,1.6E-2,1.6E-2,7.6999999999999999E-2,0.14000000000000001,0.14000000000000001,0.108,0.108,0.108,7.6999999999999999E-2,7.6999999999999999E-2,7.6999999999999999E-2,7.6999999999999999E-2,7.6999999999999999E-2,0.108,0.217,0.217,0.217,0.217,0.186,1.6E-2,{"$f":"SUM(C128:Z128)","v":2.3400000000000003},{"$f":"AA128*SUM($C$14:$C$15)","v":243.36000000000004}]
[null,"Holiday",1.6E-2,1.6E-2,1.6E-2,1.6E-2,1.6E-2,1.6E-2,7.6999999999999999E-2,0.14000000000000001,0.14000000000000001,0.108,0.108,0.108,7.6999999999999999E-2,7.6999999999999999E-2,7.6999999999999999E-2,7.6999999999999999E-2,7.6999999999999999E-2,0.108,0.217,0.217,0.217,0.217,0.186,1.6E-2,{"$f":"SUM(C129:Z129)","v":2.3400000000000003},{"$f":"AA129*$C$8","v":25.740000000000002}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB127:AB129)","v":854.10000000000014}]
[]
[null,"Schedule Name:","Dwelling Unit Miscellaneous Equipment Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.5,0.5,0.5,0.5,0.3,0.5,0.5,0.5,0.5,0.5,0.35,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C135:Z135)","v":5.799999999999998},{"$f":"AA135*SUM($C$9:$C$13)","v":1449.9999999999995}]
[null,"Weekend",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.5,0.5,0.5,0.5,0.3,0.5,0.5,0.5,0.5,0.5,0.35,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C136:Z136)","v":5.799999999999998},{"$f":"AA136*SUM($C$14:$C$15)","v":603.19999999999982}]
[null,"Holiday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.5,0.5,0.5,0.5,0.3,0.5,0.5,0.5,0.5,0.5,0.35,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C137:Z137)","v":5.799999999999998},{"$f":"AA137*$C$8","v":63.799999999999976}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB135:AB137)","v":2116.9999999999995}]
[]
[null,"Schedule Name:","Residential Common Area Miscellaneous Equipment Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.1,0.1,0.1,0.1,0.1,0.3,0.45,0.45,0.45,0.45,0.3,0.3,0.3,0.3,0.3,0.3,0.3,0.3,0.6,0.8,0.9,0.8,0.6,0.3,{"$f":"SUM(C143:Z143)","v":9},{"$f":"AA143*SUM($C$9:$C$13)","v":2250}]
[null,"Weekend",0.1,0.1,0.1,0.1,0.1,0.3,0.45,0.45,0.45,0.45,0.3,0.3,0.3,0.3,0.3,0.3,0.3,0.3,0.6,0.8,0.9,0.8,0.6,0.3,{"$f":"SUM(C144:Z144)","v":9},{"$f":"AA144*SUM($C$14:$C$15)","v":936}]
[null,"Holiday",0.1,0.1,0.1,0.1,0.1,0.3,0.45,0.45,0.45,0.45,0.3,0.3,0.3,0.3,0.3,0.3,0.3,0.3,0.6,0.8,0.9,0.8,0.6,0.3,{"$f":"SUM(C145:Z145)","v":9},{"$f":"AA145*$C$8","v":99}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB143:AB145)","v":3285}]
[]
[null,"Schedule Name:","Residential DHW Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.05,0.3,0.5,0.4,0.3,0.3,0.35,0.4,0.35,0.35,0.3,0.3,0.5,0.5,0.4,0.35,0.45,0.3,0.05,{"$f":"SUM(C151:Z151)","v":6.7},{"$f":"AA151*SUM($C$9:$C$13)","v":1675}]
[null,"Weekend",0.05,0.05,0.05,0.05,0.05,0.05,0.3,0.5,0.4,0.3,0.3,0.35,0.4,0.35,0.35,0.3,0.3,0.5,0.5,0.4,0.35,0.45,0.3,0.05,{"$f":"SUM(C152:Z152)","v":6.7},{"$f":"AA152*SUM($C$14:$C$15)","v":696.80000000000007}]
[null,"Holiday",0.05,0.05,0.05,0.05,0.05,0.05,0.3,0.5,0.4,0.3,0.3,0.35,0.4,0.35,0.35,0.3,0.3,0.5,0.5,0.4,0.35,0.45,0.3,0.05,{"$f":"SUM(C153:Z153)","v":6.7},{"$f":"AA153*$C$8","v":73.7}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB151:AB153)","v":2445.5}]
[]
[]
[null,"ASHRAE 90.1-2010 User's Manual Schedules"]
[null,"Below is a subset of sample schedules provided in the ASHRAE 90.1-2010 User's Manual. Refer to the ASHRAE User's Manual Tables G-D through G-M for additional schedules. (Note: Holiday schedules are added, and are assumed to be equal to the Sunday schedules; therefore annual equivalent full load hours will differ slightly from those reported in the default ASHRAE schedules)."]
[]
[null,"Office Occupancy"]
[]
[null,"Schedule Name:","Office HVAC System - ON/OFF Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","Hours/day","Hours/year"]
[null,"Weekday",0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0,0,{"$f":"SUM(C165:Z165)","v":16},{"$f":"AA165*SUM($C$9:$C$13)","v":4000}]
[null,"Saturday",0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,0,0,0,0,0,0,{"$f":"SUM(C166:Z166)","v":12},{"$f":"AA166*SUM($C$14)","v":624}]
[null,"Sunday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C167:Z167)","v":0},{"$f":"AA167*$C$15","v":0}]
[null,"Holiday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C168:Z168)","v":0},{"$f":"AA168*SUM($C$8)","v":0}]
[null,"Total hours of operation per year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB165:AB168)","v":4624}]
[]
[null,"Schedule Name:","Office Occupancy Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0,0,0,0,0,0,0.1,0.2,0.95,0.95,0.95,0.95,0.5,0.95,0.95,0.95,0.95,0.3,0.1,0.1,0.1,0.1,0.05,0.05,{"$f":"SUM(C174:Z174)","v":9.2000000000000011},{"$f":"AA174*SUM($C$9:$C$13)","v":2300.0000000000005}]
[null,"Saturday",0,0,0,0,0,0,0.1,0.1,0.3,0.3,0.3,0.3,0.1,0.1,0.1,0.1,0.1,0.05,0.05,0,0,0,0,0,{"$f":"SUM(C175:Z175)","v":2.0000000000000004},{"$f":"AA175*SUM($C$14)","v":104.00000000000003}]
[null,"Sunday",0,0,0,0,0,0,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0,0,0,0,0,0,{"$f":"SUM(C176:Z176)","v":0.6},{"$f":"AA176*$C$15","v":31.2}]
[null,"Holiday",0,0,0,0,0,0,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0,0,0,0,0,0,{"$f":"SUM(C177:Z177)","v":0.6},{"$f":"AA177*SUM($C$8)","v":6.6}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB174:AB177)","v":2441.8000000000002}]
[]
[null,"Schedule Name:","Office Lighting Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.1,0.1,0.3,0.65,0.65,0.65,0.65,0.55000000000000004,0.65,0.65,0.65,0.65,0.35,0.3,0.3,0.2,0.2,0.1,0.05,{"$f":"SUM(C183:Z183)","v":8},{"$f":"AA183*SUM($C$9:$C$13)","v":2000}]
[null,"Saturday",0.05,0.05,0.05,0.05,0.05,0.05,0.1,0.1,0.3,0.3,0.3,0.3,0.15,0.15,0.15,0.15,0.15,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C184:Z184)","v":2.7999999999999985},{"$f":"AA184*SUM($C$14)","v":145.59999999999991}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C185:Z185)","v":1.2000000000000004},{"$f":"AA185*$C$15","v":62.40000000000002}]
[null,"Holiday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C186:Z186)","v":1.2000000000000004},{"$f":"AA186*SUM($C$8)","v":13.200000000000005}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB183:AB186)","v":2221.1999999999998}]
[]
[null,"Schedule Name:","Office Receptacle Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.1,0.1,0.3,0.9,0.9,0.9,0.9,0.8,0.9,0.9,0.9,0.9,0.5,0.3,0.3,0.2,0.2,0.1,0.05,{"$f":"SUM(C192:Z192)","v":10.4},{"$f":"AA192*SUM($C$9:$C$13)","v":2600}]
[null,"Saturday",0.05,0.05,0.05,0.05,0.05,0.05,0.1,0.1,0.3,0.3,0.3,0.3,0.15,0.15,0.15,0.15,0.15,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C193:Z193)","v":2.7999999999999985},{"$f":"AA193*SUM($C$14)","v":145.59999999999991}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C194:Z194)","v":1.2000000000000004},{"$f":"AA194*$C$15","v":62.40000000000002}]
[null,"Holiday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C195:Z195)","v":1.2000000000000004},{"$f":"AA195*SUM($C$8)","v":13.200000000000005}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB192:AB195)","v":2821.2}]
[]
[null,"Schedule Name:","Office DHW Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.08,7.0000000000000007E-2,0.19,0.35,0.38,0.39,0.47,0.56999999999999995,0.54,0.34,0.33,0.44,0.26,0.21,0.15,0.17,0.08,0.05,0.05,{"$f":"SUM(C201:Z201)","v":5.3699999999999992},{"$f":"AA201*SUM($C$9:$C$13)","v":1342.4999999999998}]
[null,"Saturday",0.05,0.05,0.05,0.05,0.05,0.08,7.0000000000000007E-2,0.11,0.15,0.21,0.19,0.23,0.2,0.19,0.15,0.12,0.14000000000000001,7.0000000000000007E-2,7.0000000000000007E-2,7.0000000000000007E-2,7.0000000000000007E-2,0.09,0.05,0.05,{"$f":"SUM(C202:Z202)","v":2.5599999999999987},{"$f":"AA202*SUM($C$14)","v":133.11999999999995}]
[null,"Sunday",0.04,0.04,0.04,0.04,0.04,7.0000000000000007E-2,0.04,0.04,0.04,0.04,0.04,0.06,0.06,0.09,0.06,0.04,0.04,0.04,0.04,0.04,0.04,7.0000000000000007E-2,0.04,0.04,{"$f":"SUM(C203:Z203)","v":1.1300000000000001},{"$f":"AA203*$C$15","v":58.760000000000005}]
[null,"Holiday",0.04,0.04,0.04,0.04,0.04,7.0000000000000007E-2,0.04,0.04,0.04,0.04,0.04,0.06,0.06,0.09,0.06,0.04,0.04,0.04,0.04,0.04,0.04,7.0000000000000007E-2,0.04,0.04,{"$f":"SUM(C204:Z204)","v":1.1300000000000001},{"$f":"AA204*SUM($C$8)","v":12.430000000000001}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB201:AB204)","v":1546.8099999999997}]
[]
[null,"Schedule Name:","Office Elevator Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0,0,0,0,0,0,0,0.35,0.69,0.43,0.37,0.43,0.57999999999999996,0.48,0.37,0.37,0.46,0.62,0.2,0.12,0.04,0.04,0,0,{"$f":"SUM(C210:Z210)","v":5.5500000000000007},{"$f":"AA210*SUM($C$9:$C$13)","v":1387.5000000000002}]
[null,"Saturday",0,0,0,0,0,0,0,0.16,0.14000000000000001,0.21,0.18,0.25,0.21,0.13,0.08,0.04,0.05,0.06,0,0,0,0,0,0,{"$f":"SUM(C211:Z211)","v":1.51},{"$f":"AA211*SUM($C$14)","v":78.52}]
[null,"Sunday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C212:Z212)","v":0},{"$f":"AA212*$C$15","v":0}]
[null,"Holiday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C213:Z213)","v":0},{"$f":"AA213*SUM($C$8)","v":0}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB210:AB213)","v":1466.0200000000002}]
[]
[null,"School Occupancy"]
[]
[null,"Schedule Name:","School HVAC System - ON/OFF Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","Hours/day","Hours/year"]
[null,"Weekday",0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0,0,{"$f":"SUM(C221:Z221)","v":15},{"$f":"AA221*SUM($C$9:$C$13)","v":3750}]
[null,"Saturday",0,0,0,0,0,0,0,0,1,1,1,1,1,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C222:Z222)","v":5},{"$f":"AA222*SUM($C$14)","v":260}]
[null,"Sunday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C223:Z223)","v":0},{"$f":"AA223*$C$15","v":0}]
[null,"Holiday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C224:Z224)","v":0},{"$f":"AA224*SUM($C$8)","v":0}]
[null,"Total hours of operation per year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB221:AB224)","v":4010}]
[]
[null,"Schedule Name:","School Occupancy Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0,0,0,0,0,0,0,0.05,0.75,0.9,0.9,0.8,0.8,0.8,0.8,0.45,0.15,0.05,0.15,0.2,0.2,0.1,0,0,{"$f":"SUM(C230:Z230)","v":7.1000000000000005},{"$f":"AA230*SUM($C$9:$C$13)","v":1775.0000000000002}]
[null,"Saturday",0,0,0,0,0,0,0,0,0.1,0.1,0.1,0.1,0.1,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C231:Z231)","v":0.5},{"$f":"AA231*SUM($C$14)","v":26}]
[null,"Sunday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C232:Z232)","v":0},{"$f":"AA232*$C$15","v":0}]
[null,"Holiday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C233:Z233)","v":0},{"$f":"AA233*SUM($C$8)","v":0}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB230:AB233)","v":1801.0000000000002}]
[]
[null,"Schedule Name:","School Lighting Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.3,0.6,0.65,0.65,0.65,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.5,0.35,0.35,0.35,0.35,0.35,0.3,0.05,0.05,{"$f":"SUM(C239:Z239)","v":7.4999999999999973},{"$f":"AA239*SUM($C$9:$C$13)","v":1874.9999999999993}]
[null,"Saturday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.15,0.15,0.15,0.15,0.15,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C240:Z240)","v":1.7000000000000004},{"$f":"AA240*SUM($C$14)","v":88.40000000000002}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C241:Z241)","v":1.2000000000000004},{"$f":"AA241*$C$15","v":62.40000000000002}]
[null,"Holiday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C242:Z242)","v":1.2000000000000004},{"$f":"AA242*SUM($C$8)","v":13.200000000000005}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB239:AB242)","v":2038.9999999999995}]
[]
[null,"Schedule Name:","School Receptacle Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.3,0.85,0.95,0.95,0.95,0.8,0.8,0.8,0.7,0.5,0.5,0.35,0.35,0.35,0.3,0.05,0.05,{"$f":"SUM(C248:Z248)","v":9.9},{"$f":"AA248*SUM($C$9:$C$13)","v":2475}]
[null,"Saturday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.15,0.15,0.15,0.15,0.15,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C249:Z249)","v":1.7000000000000004},{"$f":"AA249*SUM($C$14)","v":88.40000000000002}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C250:Z250)","v":1.2000000000000004},{"$f":"AA250*$C$15","v":62.40000000000002}]
[null,"Holiday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C251:Z251)","v":1.2000000000000004},{"$f":"AA251*SUM($C$8)","v":13.200000000000005}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB248:AB251)","v":2639}]
[]
[null,"Schedule Name:","School DHW Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.1,0.34,0.6,0.63,0.72,0.79,0.83,0.61,0.65,0.1,0.1,0.19,0.25,0.22,0.22,0.12,0.09,{"$f":"SUM(C257:Z257)","v":6.91},{"$f":"AA257*SUM($C$9:$C$13)","v":1727.5}]
[null,"Saturday",0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.05,0.05,0.05,0.05,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,{"$f":"SUM(C258:Z258)","v":0.80000000000000027},{"$f":"AA258*SUM($C$14)","v":41.600000000000016}]
[null,"Sunday",0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.05,0.05,0.05,0.05,0.05,0.05,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,{"$f":"SUM(C259:Z259)","v":0.8400000000000003},{"$f":"AA259*$C$15","v":43.680000000000014}]
[null,"Holiday",0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.05,0.05,0.05,0.05,0.05,0.05,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,0.03,{"$f":"SUM(C260:Z260)","v":0.8400000000000003},{"$f":"AA260*SUM($C$8)","v":9.2400000000000038}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB257:AB260)","v":1822.02}]
[]
[null,"Schedule Name:","School Elevator Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0,0,0,0,0,0,0,0,0.3,0.3,0.3,0.3,0.3,0.3,0.3,0.15,0,0,0,0,0,0,0,0,{"$f":"SUM(C266:Z266)","v":2.25},{"$f":"AA266*SUM($C$9:$C$13)","v":562.5}]
[null,"Saturday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C267:Z267)","v":0},{"$f":"AA267*SUM($C$14)","v":0}]
[null,"Sunday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C268:Z268)","v":0},{"$f":"AA268*$C$15","v":0}]
[null,"Holiday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C269:Z269)","v":0},{"$f":"AA269*SUM($C$8)","v":0}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB266:AB269)","v":562.5}]
[]
[null,"Health Occupancy"]
[]
[null,"Schedule Name:","Health HVAC System - ON/OFF Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","Hours/day","Hours/year"]
[null,"Weekday",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,{"$f":"SUM(C277:Z277)","v":24},{"$f":"AA277*SUM($C$9:$C$13)","v":6000}]
[null,"Saturday",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,{"$f":"SUM(C278:Z278)","v":24},{"$f":"AA278*SUM($C$14)","v":1248}]
[null,"Sunday",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,{"$f":"SUM(C279:Z279)","v":24},{"$f":"AA279*$C$15","v":1248}]
[null,"Holiday",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,{"$f":"SUM(C280:Z280)","v":24},{"$f":"AA280*SUM($C$8)","v":264}]
[null,"Total hours of operation per year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB277:AB280)","v":8760}]
[]
[null,"Schedule Name:","Health Occupancy Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0,0,0,0,0,0,0,0.1,0.5,0.8,0.8,0.8,0.8,0.8,0.8,0.8,0.8,0.5,0.3,0.3,0.2,0.2,0,0,{"$f":"SUM(C286:Z286)","v":8.4999999999999982},{"$f":"AA286*SUM($C$9:$C$13)","v":2124.9999999999995}]
[null,"Saturday",0,0,0,0,0,0,0,0.1,0.3,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.1,0.1,0,0,0,0,0,{"$f":"SUM(C287:Z287)","v":3.8},{"$f":"AA287*SUM($C$14)","v":197.6}]
[null,"Sunday",0,0,0,0,0,0,0,0,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0,0,0,0,0,0,0,0,{"$f":"SUM(C288:Z288)","v":0.39999999999999997},{"$f":"AA288*$C$15","v":20.799999999999997}]
[null,"Holiday",0,0,0,0,0,0,0,0,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0,0,0,0,0,0,0,0,{"$f":"SUM(C289:Z289)","v":0.39999999999999997},{"$f":"AA289*SUM($C$8)","v":4.3999999999999995}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB286:AB289)","v":2347.7999999999997}]
[]
[null,"Schedule Name:","Health Lighting Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.45,0.8,0.8,0.8,0.8,0.8,0.8,0.8,0.8,0.3,0.3,0.3,0.3,0.3,0.3,0.3,0.1,{"$f":"SUM(C295:Z295)","v":9.7500000000000018},{"$f":"AA295*SUM($C$9:$C$13)","v":2437.5000000000005}]
[null,"Saturday",0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.2,0.35,0.35,0.35,0.35,0.35,0.35,0.35,0.35,0.35,0.35,0.1,0.1,0.1,0.1,0.1,0.1,{"$f":"SUM(C296:Z296)","v":4.9999999999999982},{"$f":"AA296*SUM($C$14)","v":259.99999999999989}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C297:Z297)","v":1.6000000000000003},{"$f":"AA297*$C$15","v":83.200000000000017}]
[null,"Holiday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C298:Z298)","v":1.6000000000000003},{"$f":"AA298*SUM($C$8)","v":17.600000000000005}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB295:AB298)","v":2798.3}]
[]
[null,"Schedule Name:","Health Receptacle Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.5,0.9,0.9,0.9,0.9,0.9,0.9,0.9,0.9,0.3,0.3,0.3,0.3,0.3,0.3,0.3,0.1,{"$f":"SUM(C304:Z304)","v":10.600000000000005},{"$f":"AA304*SUM($C$9:$C$13)","v":2650.0000000000014}]
[null,"Saturday",0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.2,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.1,0.1,0.1,0.1,0.1,0.1,{"$f":"SUM(C305:Z305)","v":5.4999999999999982},{"$f":"AA305*SUM($C$14)","v":285.99999999999989}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C306:Z306)","v":1.6000000000000003},{"$f":"AA306*$C$15","v":83.200000000000017}]
[null,"Holiday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C307:Z307)","v":1.6000000000000003},{"$f":"AA307*SUM($C$8)","v":17.600000000000005}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB304:AB307)","v":3036.8000000000011}]
[]
[null,"Schedule Name:","Health DHW Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.17,0.57999999999999996,0.66,0.78,0.82,0.71,0.82,0.78,0.74,0.63,0.41,0.18,0.18,0.18,0.1,0.01,0.01,{"$f":"SUM(C313:Z313)","v":7.8299999999999983},{"$f":"AA313*SUM($C$9:$C$13)","v":1957.4999999999995}]
[null,"Saturday",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.2,0.28000000000000003,0.3,0.3,0.24,0.24,0.23,0.23,0.23,0.1,0.01,0.01,0.01,0.01,0.01,0.01,{"$f":"SUM(C314:Z314)","v":2.4899999999999989},{"$f":"AA314*SUM($C$14)","v":129.47999999999993}]
[null,"Sunday",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,{"$f":"SUM(C315:Z315)","v":0.24000000000000007},{"$f":"AA315*$C$15","v":12.480000000000004}]
[null,"Holiday",0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,0.01,{"$f":"SUM(C316:Z316)","v":0.24000000000000007},{"$f":"AA316*SUM($C$8)","v":2.640000000000001}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB313:AB316)","v":2102.0999999999995}]
[]
[null,"Schedule Name:","Health Elevator Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0,0,0,0,0,0,0,0.02,0.75,1,1,1,0.75,1,1,1,1,1,0.52,0.52,0.52,0.28000000000000003,0,0,{"$f":"SUM(C322:Z322)","v":11.359999999999998},{"$f":"AA322*SUM($C$9:$C$13)","v":2839.9999999999995}]
[null,"Saturday",0,0,0,0,0,0,0,0.02,0.46,0.7,0.7,0.7,0.51,0.51,0.51,0.51,0.51,0.25,0.02,0,0,0,0,0,{"$f":"SUM(C323:Z323)","v":5.3999999999999986},{"$f":"AA323*SUM($C$14)","v":280.79999999999995}]
[null,"Sunday",0,0,0,0,0,0,0,0,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0,0,0,0,0,0,0,0,{"$f":"SUM(C324:Z324)","v":0.16},{"$f":"AA324*$C$15","v":8.32}]
[null,"Holiday",0,0,0,0,0,0,0,0,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0,0,0,0,0,0,0,0,{"$f":"SUM(C325:Z325)","v":0.16},{"$f":"AA325*SUM($C$8)","v":1.76}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB322:AB325)","v":3130.8799999999997}]
[]
[null,"Retail Occupancy"]
[]
[null,"Schedule Name:","Retail HVAC System - ON/OFF Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","Hours/day","Hours/year"]
[null,"Weekday",0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0,0,0,{"$f":"SUM(C333:Z333)","v":15},{"$f":"AA333*SUM($C$9:$C$13)","v":3750}]
[null,"Saturday",0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0,0,{"$f":"SUM(C334:Z334)","v":16},{"$f":"AA334*SUM($C$14)","v":832}]
[null,"Sunday",0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,0,0,0,0,0,0,0,{"$f":"SUM(C335:Z335)","v":9},{"$f":"AA335*$C$15","v":468}]
[null,"Holiday",0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,0,0,0,0,0,0,0,{"$f":"SUM(C336:Z336)","v":9},{"$f":"AA336*SUM($C$8)","v":99}]
[null,"Total hours of operation per year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB333:AB336)","v":5149}]
[]
[null,"Schedule Name:","Retail Occupancy Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0,0,0,0,0,0,0,0.1,0.2,0.5,0.5,0.7,0.7,0.7,0.7,0.8,0.7,0.5,0.5,0.3,0.3,0,0,0,{"$f":"SUM(C342:Z342)","v":7.2},{"$f":"AA342*SUM($C$9:$C$13)","v":1800}]
[null,"Saturday",0,0,0,0,0,0,0,0.1,0.2,0.5,0.6,0.8,0.8,0.8,0.8,0.8,0.8,0.6,0.2,0.2,0.2,0.1,0,0,{"$f":"SUM(C343:Z343)","v":7.4999999999999991},{"$f":"AA343*SUM($C$14)","v":389.99999999999994}]
[null,"Sunday",0,0,0,0,0,0,0,0,0,0.1,0.2,0.2,0.4,0.4,0.4,0.4,0.4,0.2,0.1,0,0,0,0,0,{"$f":"SUM(C344:Z344)","v":2.8000000000000003},{"$f":"AA344*$C$15","v":145.60000000000002}]
[null,"Holiday",0,0,0,0,0,0,0,0,0,0.1,0.2,0.2,0.4,0.4,0.4,0.4,0.4,0.2,0.1,0,0,0,0,0,{"$f":"SUM(C345:Z345)","v":2.8000000000000003},{"$f":"AA345*SUM($C$8)","v":30.800000000000004}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB342:AB345)","v":2366.4}]
[]
[null,"Schedule Name:","Retail Lighting Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.2,0.5,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.55000000000000004,0.55000000000000004,0.5,0.2,0.05,0.05,{"$f":"SUM(C351:Z351)","v":10.600000000000001},{"$f":"AA351*SUM($C$9:$C$13)","v":2650.0000000000005}]
[null,"Saturday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.1,0.3,0.55000000000000004,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.5,0.3,0.3,0.1,0.05,0.05,{"$f":"SUM(C352:Z352)","v":9.4000000000000021},{"$f":"AA352*SUM($C$14)","v":488.80000000000013}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.1,0.1,0.4,0.4,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.4,0.2,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C353:Z353)","v":4.9999999999999991},{"$f":"AA353*$C$15","v":259.99999999999994}]
[null,"Holiday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.1,0.1,0.4,0.4,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.4,0.2,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C354:Z354)","v":4.9999999999999991},{"$f":"AA354*SUM($C$8)","v":54.999999999999993}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB351:AB354)","v":3453.8000000000006}]
[]
[null,"Schedule Name:","Retail Receptacle Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.2,0.5,0.9,0.9,0.9,0.9,0.9,0.9,0.9,0.9,0.9,0.6,0.6,0.5,0.2,0.05,0.05,{"$f":"SUM(C360:Z360)","v":11.150000000000002},{"$f":"AA360*SUM($C$9:$C$13)","v":2787.5000000000005}]
[null,"Saturday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.1,0.3,0.6,0.9,0.9,0.9,0.9,0.9,0.9,0.9,0.9,0.5,0.3,0.3,0.1,0.05,0.05,{"$f":"SUM(C361:Z361)","v":9.8500000000000032},{"$f":"AA361*SUM($C$14)","v":512.20000000000016}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.1,0.1,0.4,0.4,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.4,0.2,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C362:Z362)","v":4.9999999999999991},{"$f":"AA362*$C$15","v":259.99999999999994}]
[null,"Holiday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.1,0.1,0.4,0.4,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.4,0.2,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C363:Z363)","v":4.9999999999999991},{"$f":"AA363*SUM($C$8)","v":54.999999999999993}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB360:AB363)","v":3614.7000000000007}]
[]
[null,"Schedule Name:","Retail DHW Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.04,0.05,0.05,0.04,0.04,0.04,0.04,0.15,0.23,0.32,0.41,0.56999999999999995,0.62,0.61,0.5,0.45,0.46,0.47,0.42,0.34,0.33,0.23,0.13,0.08,{"$f":"SUM(C369:Z369)","v":6.62},{"$f":"AA369*SUM($C$9:$C$13)","v":1655}]
[null,"Saturday",0.11,0.1,0.08,0.06,0.06,0.06,7.0000000000000007E-2,0.2,0.24,0.27,0.42,0.54,0.59,0.6,0.49,0.48,0.47,0.46,0.44,0.36,0.28999999999999998,0.22,0.16,0.13,{"$f":"SUM(C370:Z370)","v":6.8999999999999995},{"$f":"AA370*SUM($C$14)","v":358.79999999999995}]
[null,"Sunday",7.0000000000000007E-2,7.0000000000000007E-2,7.0000000000000007E-2,0.06,0.06,0.06,7.0000000000000007E-2,0.1,0.12,0.14000000000000001,0.28999999999999998,0.31,0.36,0.36,0.34,0.35,0.37,0.34,0.25,0.27,0.21,0.16,0.1,0.06,{"$f":"SUM(C371:Z371)","v":4.59},{"$f":"AA371*$C$15","v":238.68}]
[null,"Holiday",7.0000000000000007E-2,7.0000000000000007E-2,7.0000000000000007E-2,0.06,0.06,0.06,7.0000000000000007E-2,0.1,0.12,0.14000000000000001,0.28999999999999998,0.31,0.36,0.36,0.34,0.35,0.37,0.34,0.25,0.27,0.21,0.16,0.1,0.06,{"$f":"SUM(C372:Z372)","v":4.59},{"$f":"AA372*SUM($C$8)","v":50.489999999999995}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB369:AB372)","v":2302.9699999999998}]
[]
[null,"Schedule Name:","Retail Elevator Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0,0,0,0,0,0,0,0.12,0.22,0.64,0.74,0.68,0.68,0.71,0.72,0.72,0.73,0.68,0.68,0.57999999999999996,0.54,0,0,0,{"$f":"SUM(C378:Z378)","v":8.4399999999999977},{"$f":"AA378*SUM($C$9:$C$13)","v":2109.9999999999995}]
[null,"Saturday",0,0,0,0,0,0,0,0.09,0.21,0.56000000000000005,0.66,0.68,0.68,0.69,0.7,0.69,0.66,0.57999999999999996,0.47,0.43,0.43,0.08,0,0,{"$f":"SUM(C379:Z379)","v":7.61},{"$f":"AA379*SUM($C$14)","v":395.72}]
[null,"Sunday",0,0,0,0,0,0,0,0,0,0.11,0.13,0.35,0.37,0.37,0.39,0.41,0.38,0.34,0.03,0,0,0,0,0,{"$f":"SUM(C380:Z380)","v":2.88},{"$f":"AA380*$C$15","v":149.76}]
[null,"Holiday",0,0,0,0,0,0,0,0,0,0.11,0.13,0.35,0.37,0.37,0.39,0.41,0.38,0.34,0.03,0,0,0,0,0,{"$f":"SUM(C381:Z381)","v":2.88},{"$f":"AA381*SUM($C$8)","v":31.68}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB378:AB381)","v":2687.1599999999994}]
[]
[null,"Restaurant Occupancy"]
[]
[null,"Schedule Name:","Restaurant HVAC System - ON/OFF Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","Hours/day","Hours/year"]
[null,"Weekday",1,1,1,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,{"$f":"SUM(C389:Z389)","v":20},{"$f":"AA389*SUM($C$9:$C$13)","v":5000}]
[null,"Saturday",1,1,1,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,{"$f":"SUM(C390:Z390)","v":18},{"$f":"AA390*SUM($C$14)","v":936}]
[null,"Sunday",1,1,1,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,{"$f":"SUM(C391:Z391)","v":17},{"$f":"AA391*$C$15","v":884}]
[null,"Holiday",1,1,1,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,{"$f":"SUM(C392:Z392)","v":17},{"$f":"AA392*SUM($C$8)","v":187}]
[null,"Total hours of operation per year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB389:AB392)","v":7007}]
[]
[null,"Schedule Name:","Restaurant Occupancy Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.15,0.15,0.05,0,0,0,0,0.05,0.05,0.05,0.2,0.5,0.8,0.7,0.4,0.2,0.25,0.5,0.8,0.8,0.8,0.5,0.35,0.2,{"$f":"SUM(C398:Z398)","v":7.5},{"$f":"AA398*SUM($C$9:$C$13)","v":1875}]
[null,"Saturday",0.3,0.25,0.05,0,0,0,0,0,0,0.05,0.2,0.45,0.5,0.5,0.35,0.3,0.3,0.3,0.7,0.9,0.7,0.65,0.55000000000000004,0.35,{"$f":"SUM(C399:Z399)","v":7.3999999999999995},{"$f":"AA399*SUM($C$14)","v":384.79999999999995}]
[null,"Sunday",0.2,0.2,0.05,0,0,0,0,0,0,0,0.1,0.2,0.25,0.25,0.15,0.2,0.25,0.35,0.55000000000000004,0.65,0.7,0.35,0.2,0.2,{"$f":"SUM(C400:Z400)","v":4.8499999999999996},{"$f":"AA400*$C$15","v":252.2}]
[null,"Holiday",0.2,0.2,0.05,0,0,0,0,0,0,0,0.1,0.2,0.25,0.25,0.15,0.2,0.25,0.35,0.55000000000000004,0.65,0.7,0.35,0.2,0.2,{"$f":"SUM(C401:Z401)","v":4.8499999999999996},{"$f":"AA401*SUM($C$8)","v":53.349999999999994}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB398:AB401)","v":2565.35}]
[]
[null,"Schedule Name:","Restaurant Lighting Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.15,0.15,0.15,0.15,0.15,0.2,0.35,0.35,0.55000000000000004,0.55000000000000004,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.45,0.3,{"$f":"SUM(C407:Z407)","v":13.699999999999998},{"$f":"AA407*SUM($C$9:$C$13)","v":3424.9999999999995}]
[null,"Saturday",0.2,0.15,0.15,0.15,0.15,0.15,0.3,0.3,0.55000000000000004,0.55000000000000004,0.75,0.75,0.75,0.75,0.75,0.75,0.75,0.85,0.85,0.85,0.85,0.85,0.45,0.3,{"$f":"SUM(C408:Z408)","v":12.899999999999999},{"$f":"AA408*SUM($C$14)","v":670.8}]
[null,"Sunday",0.2,0.15,0.15,0.15,0.15,0.15,0.3,0.3,0.45,0.45,0.65,0.65,0.65,0.65,0.65,0.65,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.45,0.3,{"$f":"SUM(C409:Z409)","v":10.400000000000004},{"$f":"AA409*$C$15","v":540.80000000000018}]
[null,"Holiday",0.2,0.15,0.15,0.15,0.15,0.15,0.3,0.3,0.45,0.45,0.65,0.65,0.65,0.65,0.65,0.65,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.45,0.3,{"$f":"SUM(C410:Z410)","v":10.400000000000004},{"$f":"AA410*SUM($C$8)","v":114.40000000000005}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB407:AB410)","v":4750.9999999999991}]
[]
[null,"Schedule Name:","Restaurant Receptacle Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.15,0.15,0.15,0.15,0.15,0.2,0.4,0.4,0.6,0.6,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.85,0.45,0.3,{"$f":"SUM(C416:Z416)","v":13.899999999999997},{"$f":"AA416*SUM($C$9:$C$13)","v":3474.9999999999991}]
[null,"Saturday",0.2,0.15,0.15,0.15,0.15,0.15,0.3,0.3,0.55000000000000004,0.55000000000000004,0.75,0.75,0.75,0.75,0.75,0.75,0.75,0.85,0.85,0.85,0.85,0.85,0.45,0.3,{"$f":"SUM(C417:Z417)","v":12.899999999999999},{"$f":"AA417*SUM($C$14)","v":670.8}]
[null,"Sunday",0.2,0.15,0.15,0.15,0.15,0.15,0.3,0.3,0.45,0.45,0.65,0.65,0.65,0.65,0.65,0.65,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.45,0.3,{"$f":"SUM(C418:Z418)","v":10.400000000000004},{"$f":"AA418*$C$15","v":540.80000000000018}]
[null,"Holiday",0.2,0.15,0.15,0.15,0.15,0.15,0.3,0.3,0.45,0.45,0.65,0.65,0.65,0.65,0.65,0.65,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.45,0.3,{"$f":"SUM(C419:Z419)","v":10.400000000000004},{"$f":"AA419*SUM($C$8)","v":114.40000000000005}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB416:AB419)","v":4800.9999999999991}]
[]
[null,"Schedule Name:","Restaurant DHW Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.2,0.15,0.15,0,0,0,0,0.6,0.55000000000000004,0.45,0.4,0.45,0.4,0.35,0.3,0.3,0.3,0.4,0.55000000000000004,0.6,0.5,0.55000000000000004,0.45,0.25,{"$f":"SUM(C425:Z425)","v":7.8999999999999995},{"$f":"AA425*SUM($C$9:$C$13)","v":1974.9999999999998}]
[null,"Saturday",0.2,0.15,0.15,0,0,0,0,0,0,0.5,0.45,0.5,0.5,0.45,0.4,0.4,0.35,0.4,0.55000000000000004,0.55000000000000004,0.5,0.55000000000000004,0.4,0.3,{"$f":"SUM(C426:Z426)","v":7.3},{"$f":"AA426*SUM($C$14)","v":379.59999999999997}]
[null,"Sunday",0.25,0.2,0.2,0,0,0,0,0,0,0,0.5,0.5,0.4,0.4,0.3,0.3,0.3,0.4,0.5,0.5,0.4,0.5,0.4,0.2,{"$f":"SUM(C427:Z427)","v":6.25},{"$f":"AA427*$C$15","v":325}]
[null,"Holiday",0.25,0.2,0.2,0,0,0,0,0,0,0,0.5,0.5,0.4,0.4,0.3,0.3,0.3,0.4,0.5,0.5,0.4,0.5,0.4,0.2,{"$f":"SUM(C428:Z428)","v":6.25},{"$f":"AA428*SUM($C$8)","v":68.75}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB425:AB428)","v":2748.35}]
[]
[null,"Warehouse Occupancy"]
[]
[null,"Schedule Name:","Warehouse HVAC System - ON/OFF Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","Hours/day","Hours/year"]
[null,"Weekday",0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,0,0,0,0,0,0,0,{"$f":"SUM(C436:Z436)","v":10},{"$f":"AA436*SUM($C$9:$C$13)","v":2500}]
[null,"Saturday",0,0,0,0,0,0,0,0,1,1,1,1,1,1,1,1,0,0,0,0,0,0,0,0,{"$f":"SUM(C437:Z437)","v":8},{"$f":"AA437*SUM($C$14)","v":416}]
[null,"Sunday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C438:Z438)","v":0},{"$f":"AA438*$C$15","v":0}]
[null,"Holiday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C439:Z439)","v":0},{"$f":"AA439*SUM($C$8)","v":0}]
[null,"Total hours of operation per year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB436:AB439)","v":2916}]
[]
[null,"Schedule Name:","Warehouse Occupancy Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0,0,0,0,0,0,0,0.15,0.7,0.9,0.9,0.9,0.5,0.85,0.85,0.85,0.2,0,0,0,0,0,0,0,{"$f":"SUM(C445:Z445)","v":6.7999999999999989},{"$f":"AA445*SUM($C$9:$C$13)","v":1699.9999999999998}]
[null,"Saturday",0,0,0,0,0,0,0,0,0.2,0.2,0.2,0.2,0.1,0.1,0.1,0.1,0,0,0,0,0,0,0,0,{"$f":"SUM(C446:Z446)","v":1.2000000000000002},{"$f":"AA446*SUM($C$14)","v":62.400000000000006}]
[null,"Sunday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C447:Z447)","v":0},{"$f":"AA447*$C$15","v":0}]
[null,"Holiday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C448:Z448)","v":0},{"$f":"AA448*SUM($C$8)","v":0}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB445:AB448)","v":1762.3999999999999}]
[]
[null,"Schedule Name:","Warehouse Lighting Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.25,0.45,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.5,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.3,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C454:Z454)","v":5.9999999999999982},{"$f":"AA454*SUM($C$9:$C$13)","v":1499.9999999999995}]
[null,"Saturday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.08,0.24,0.24,0.24,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C455:Z455)","v":1.8000000000000005},{"$f":"AA455*SUM($C$14)","v":93.600000000000023}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C456:Z456)","v":1.2000000000000004},{"$f":"AA456*$C$15","v":62.40000000000002}]
[null,"Holiday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C457:Z457)","v":1.2000000000000004},{"$f":"AA457*SUM($C$8)","v":13.200000000000005}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB454:AB457)","v":1669.1999999999996}]
[]
[null,"Schedule Name:","Warehouse Receptacle Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.4,0.7,0.9,0.9,0.9,0.8,0.9,0.9,0.9,0.9,0.3,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C463:Z463)","v":9.1500000000000057},{"$f":"AA463*SUM($C$9:$C$13)","v":2287.5000000000014}]
[null,"Saturday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.08,0.24,0.24,0.24,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C464:Z464)","v":1.8000000000000005},{"$f":"AA464*SUM($C$14)","v":93.600000000000023}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C465:Z465)","v":1.2000000000000004},{"$f":"AA465*$C$15","v":62.40000000000002}]
[null,"Holiday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.05,{"$f":"SUM(C466:Z466)","v":1.2000000000000004},{"$f":"AA466*SUM($C$8)","v":13.200000000000005}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB463:AB466)","v":2456.7000000000012}]
[]
[null,"Schedule Name:","Warehouse DHW Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.02,0.02,0.02,0.02,0.05,7.0000000000000007E-2,7.0000000000000007E-2,0.1,0.3,0.36,0.36,0.46,0.56999999999999995,0.43,0.38,0.4,0.3,0.18,0.03,0.03,0.03,0.03,0.03,0.03,{"$f":"SUM(C472:Z472)","v":4.2900000000000009},{"$f":"AA472*SUM($C$9:$C$13)","v":1072.5000000000002}]
[null,"Saturday",0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.06,0.12,0.12,0.17,0.04,0.04,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,{"$f":"SUM(C473:Z473)","v":0.91000000000000025},{"$f":"AA473*SUM($C$14)","v":47.320000000000014}]
[null,"Sunday",0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.04,0.04,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,{"$f":"SUM(C474:Z474)","v":0.52000000000000013},{"$f":"AA474*$C$15","v":27.040000000000006}]
[null,"Holiday",0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.04,0.04,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,0.02,{"$f":"SUM(C475:Z475)","v":0.52000000000000013},{"$f":"AA475*SUM($C$8)","v":5.7200000000000015}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB472:AB475)","v":1152.5800000000002}]
[]
[null,"Schedule Name:","Warehouse Elevator Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0,0,0,0,0,0,0,0,0,0,0.3,0,0,0,0,0.4,0,0,0,0,0,0,0,0,{"$f":"SUM(C481:Z481)","v":0.7},{"$f":"AA481*SUM($C$9:$C$13)","v":175}]
[null,"Saturday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C482:Z482)","v":0},{"$f":"AA482*SUM($C$14)","v":0}]
[null,"Sunday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C483:Z483)","v":0},{"$f":"AA483*$C$15","v":0}]
[null,"Holiday",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUM(C484:Z484)","v":0},{"$f":"AA484*SUM($C$8)","v":0}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB481:AB484)","v":175}]
[]
[null,"Assembly Occupancy"]
[]
[null,"Schedule Name:","Assembly HVAC System - ON/OFF Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","Hours/day","Hours/year"]
[null,"Weekday",0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0,{"$f":"SUM(C492:Z492)","v":18},{"$f":"AA492*SUM($C$9:$C$13)","v":4500}]
[null,"Saturday",0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0,{"$f":"SUM(C493:Z493)","v":17},{"$f":"AA493*SUM($C$14)","v":884}]
[null,"Sunday",0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0,{"$f":"SUM(C494:Z494)","v":17},{"$f":"AA494*$C$15","v":884}]
[null,"Sunday",0,0,0,0,0,0,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,0,{"$f":"SUM(C495:Z495)","v":17},{"$f":"AA495*SUM($C$8)","v":187}]
[null,"Total hours of operation per year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB492:AB495)","v":6455}]
[]
[null,"Schedule Name:","Assembly Occupancy Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0,0,0,0,0,0,0,0,0.2,0.2,0.2,0.8,0.8,0.8,0.8,0.8,0.8,0.8,0.2,0.2,0.2,0.2,0.1,0,{"$f":"SUM(C501:Z501)","v":7.1},{"$f":"AA501*SUM($C$9:$C$13)","v":1775}]
[null,"Saturday",0,0,0,0,0,0,0,0,0.2,0.2,0.2,0.6,0.6,0.6,0.6,0.6,0.6,0.6,0.6,0.6,0.6,0.8,0.1,0,{"$f":"SUM(C502:Z502)","v":7.4999999999999982},{"$f":"AA502*SUM($C$14)","v":389.99999999999989}]
[null,"Sunday",0,0,0,0,0,0,0,0,0.1,0.1,0.1,0.1,0.1,0.7,0.7,0.7,0.7,0.7,0.7,0.7,0.7,0.7,0.2,0,{"$f":"SUM(C503:Z503)","v":7.0000000000000009},{"$f":"AA503*$C$15","v":364.00000000000006}]
[null,"Sunday",0,0,0,0,0,0,0,0,0.1,0.1,0.1,0.1,0.1,0.7,0.7,0.7,0.7,0.7,0.7,0.7,0.7,0.7,0.2,0,{"$f":"SUM(C504:Z504)","v":7.0000000000000009},{"$f":"AA504*SUM($C$8)","v":77.000000000000014}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB501:AB504)","v":2606}]
[]
[null,"Schedule Name:","Assembly Lighting Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.05,0.35,0.35,0.35,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.25,0.05,{"$f":"SUM(C510:Z510)","v":10.100000000000003},{"$f":"AA510*SUM($C$9:$C$13)","v":2525.0000000000009}]
[null,"Saturday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.3,0.3,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.4,0.05,{"$f":"SUM(C511:Z511)","v":6.6000000000000014},{"$f":"AA511*SUM($C$14)","v":343.20000000000005}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.3,0.3,0.3,0.3,0.3,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.05,0.05,{"$f":"SUM(C512:Z512)","v":7.4499999999999984},{"$f":"AA512*$C$15","v":387.39999999999992}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.3,0.3,0.3,0.3,0.3,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.05,0.05,{"$f":"SUM(C513:Z513)","v":7.4499999999999984},{"$f":"AA513*SUM($C$8)","v":81.949999999999989}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB510:AB513)","v":3337.5500000000006}]
[]
[null,"Schedule Name:","Assembly Receptacle Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0.05,0.05,0.05,0.05,0.05,0.05,0.4,0.4,0.4,0.75,0.75,0.75,0.75,0.75,0.75,0.75,0.75,0.75,0.75,0.75,0.75,0.75,0.25,0.05,{"$f":"SUM(C519:Z519)","v":11.55},{"$f":"AA519*SUM($C$9:$C$13)","v":2887.5}]
[null,"Saturday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.3,0.3,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.05,{"$f":"SUM(C520:Z520)","v":8},{"$f":"AA520*SUM($C$14)","v":416}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.3,0.3,0.3,0.3,0.3,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.05,0.05,{"$f":"SUM(C521:Z521)","v":8.4500000000000028},{"$f":"AA521*$C$15","v":439.40000000000015}]
[null,"Sunday",0.05,0.05,0.05,0.05,0.05,0.05,0.05,0.3,0.3,0.3,0.3,0.3,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.65,0.05,0.05,{"$f":"SUM(C522:Z522)","v":8.4500000000000028},{"$f":"AA522*SUM($C$8)","v":92.950000000000031}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB519:AB522)","v":3835.85}]
[]
[null,"Schedule Name:","Assembly DHW Schedule"]
[]
[null,null,"12-1AM","1-2AM","2-3AM","3-4AM","4-5AM","5-6AM","6-7AM","7-8AM","8-9 AM","9-10AM","10-11AM","11AM-12PM","12-1PM","1-2PM","2-3PM","3-4PM","4-5PM","5-6PM","6-7PM","7-8PM","8-9PM","9-10PM","10-11PM","11-12PM","EFLH/day","EFLH/year"]
[null,"Weekday",0,0,0,0,0,0,0,0,0,0.05,0.05,0.35,0.05,0.05,0.05,0.05,0.05,0,0,0,0,0,0,0,{"$f":"SUM(C528:Z528)","v":0.70000000000000007},{"$f":"AA528*SUM($C$9:$C$13)","v":175.00000000000003}]
[null,"Saturday",0,0,0,0,0,0,0,0,0,0.05,0.05,0.2,0,0,0,0,0,0,0,0.65,0.3,0,0,0,{"$f":"SUM(C529:Z529)","v":1.25},{"$f":"AA529*SUM($C$14)","v":65}]
[null,"Sunday",0,0,0,0,0,0,0,0,0,0.05,0.05,0.1,0,0,0,0,0,0,0,0.65,0.3,0,0,0,{"$f":"SUM(C530:Z530)","v":1.1500000000000001},{"$f":"AA530*$C$15","v":59.800000000000004}]
[null,"Sunday",0,0,0,0,0,0,0,0,0,0.05,0.05,0.1,0,0,0,0,0,0,0,0.65,0.3,0,0,0,{"$f":"SUM(C531:Z531)","v":1.1500000000000001},{"$f":"AA531*SUM($C$8)","v":12.650000000000002}]
[null,"Total Equivalent Full Load Hours of Operation per Year",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AB528:AB531)","v":312.45}]

{"sheet":"3 - Multifamily Details","index":7,"n_rows":130,"n_cols":33,"rows_kept":130,"cut":false,"hidden":false,"merged":[[101,1,101,20],[119,1,119,20],[8,25,9,25],[25,1,25,20],[54,19,55,19],[54,20,55,20],[84,1,84,20],[86,1,88,1],[86,2,88,2],[86,10,87,11],[86,12,87,13],[86,14,87,15],[86,16,87,17],[87,7,88,7],[87,8,88,8],[54,12,54,13],[54,14,55,14],[54,15,55,15],[54,17,55,17],[54,18,55,18],[82,2,82,16],[82,19,82,20],[53,16,55,16],[53,17,53,20],[54,7,54,8],[54,9,55,9],[54,10,55,10],[79,1,79,16],[79,17,79,20],[80,2,80,16],[80,19,80,20],[53,1,55,1],[53,2,55,2],[53,3,55,3],[53,4,55,4],[53,5,55,5],[53,6,55,6],[53,7,53,10],[53,11,55,11],[53,12,53,15],[81,2,81,16],[81,19,81,20],[67,1,67,20],[69,1,71,1],[69,2,71,2],[69,3,71,3],[69,4,71,4],[69,5,69,10],[69,11,71,11],[69,12,69,17],[69,18,71,18],[69,19,70,20],[70,5,70,7],[70,8,70,10],[70,12,70,14],[70,15,70,17],[40,1,40,21],[42,1,44,1],[42,2,44,2],[42,3,44,3],[42,4,44,4],[42,11,44,11],[42,12,42,17],[43,12,43,14],[43,15,43,17],[42,18,44,18],[42,19,43,20],[27,2,29,2],[27,3,29,3],[27,4,29,4],[27,5,29,5],[28,15,29,15],[28,16,29,16],[28,17,29,17],[27,6,29,6],[28,7,28,8],[28,11,29,11],[28,9,29,9],[28,10,29,10],[28,18,29,18],[20,16,20,20],[8,19,8,20],[8,13,8,14],[8,15,8,16],[14,1,14,18],[8,3,8,4],[8,5,8,6],[12,1,12,18],[28,19,29,19],[28,20,29,20],[28,12,28,13],[13,1,13,18],[8,9,8,10],[8,11,8,12],[8,7,8,8],[15,1,15,18],[16,1,16,18],[17,1,17,18],[18,1,18,18],[8,17,8,18],[8,1,9,2],[28,14,29,14],[27,1,29,1],[98,3,98,4],[98,5,98,6],[98,7,98,8],[98,9,98,10],[98,11,98,12],[98,13,98,14],[98,15,98,16],[98,17,98,18],[98,19,98,20],[102,9,102,10],[103,9,103,10],[104,9,104,10],[102,11,102,12],[103,11,103,12],[104,11,104,12],[102,1,102,2],[103,1,103,2],[104,1,104,2],[102,3,102,4],[103,3,103,4],[104,3,104,4],[102,5,102,6],[103,5,103,6],[104,5,104,6],[102,19,102,20],[103,19,103,20],[104,19,104,20],[107,3,107,4],[107,5,107,6],[107,7,107,8],[107,9,107,10],[107,11,107,12],[107,13,107,14],[107,15,107,16],[107,17,107,18],[107,19,107,20],[102,13,102,14],[103,13,103,14],[104,13,104,14],[102,15,102,16],[103,15,103,16],[104,15,104,16],[102,17,102,18],[103,17,103,18],[104,17,104,18],[102,7,102,8],[103,7,103,8],[104,7,104,8],[106,13,106,14],[106,15,106,16],[106,17,106,18],[106,19,106,20],[107,1,108,1],[108,3,108,4],[108,5,108,6],[108,7,108,8],[108,9,108,10],[108,11,108,12],[108,13,108,14],[108,15,108,16],[108,17,108,18],[105,1,106,1],[106,3,106,4],[106,5,106,6],[106,7,106,8],[106,9,106,10],[106,11,106,12],[111,3,111,4],[111,5,111,6],[111,7,111,8],[111,9,111,10],[111,11,111,12],[105,19,105,20],[109,3,109,4],[109,5,109,6],[109,7,109,8],[109,9,109,10],[109,11,109,12],[109,13,109,14],[109,15,109,16],[109,17,109,18],[109,19,109,20],[105,3,105,4],[105,5,105,6],[105,7,105,8],[105,9,105,10],[105,11,105,12],[105,13,105,14],[105,15,105,16],[105,17,105,18],[108,19,108,20],[111,15,111,16],[114,19,114,20],[112,13,112,14],[112,15,112,16],[112,17,112,18],[112,19,112,20],[113,13,113,14],[113,15,113,16],[113,17,113,18],[113,19,113,20],[117,13,117,14],[117,15,117,16],[112,9,112,10],[116,19,116,20],[115,19,115,20],[112,11,112,12],[114,13,114,14],[114,15,114,16],[109,1,110,1],[110,15,110,16],[111,1,112,1],[113,1,114,1],[114,5,114,6],[114,7,114,8],[114,9,114,10],[114,11,114,12],[113,3,113,4],[113,5,113,6],[113,7,113,8],[113,9,113,10],[110,3,110,4],[110,5,110,6],[110,7,110,8],[110,9,110,10],[125,17,125,18],[121,1,121,2],[121,3,121,4],[121,5,121,6],[121,7,121,8],[121,9,121,10],[121,11,121,12],[121,13,121,14],[121,15,121,16],[121,17,121,18],[125,1,125,2],[125,3,125,4],[125,5,125,6],[125,7,125,8],[125,9,125,10],[125,11,125,12],[125,13,125,14],[125,15,125,16],[123,1,123,2],[123,3,123,4],[123,5,123,6],[123,7,123,8],[122,9,122,10],[122,11,122,12],[124,19,124,20],[120,1,120,2],[120,3,120,4],[120,5,120,6],[118,3,118,4],[118,5,118,6],[118,7,118,8],[118,9,118,10],[118,11,118,12],[118,13,118,14],[118,15,118,16],[122,13,122,14],[122,15,122,16],[122,17,122,18],[124,1,124,2],[124,3,124,4],[124,5,124,6],[124,7,124,8],[124,9,124,10],[124,11,124,12],[124,13,124,14],[124,15,124,16],[124,17,124,18],[122,1,122,2],[126,17,126,18],[126,19,126,20],[53,21,55,21],[42,21,44,21],[27,21,29,21],[69,21,71,21],[123,11,123,12],[123,13,123,14],[123,15,123,16],[123,17,123,18],[123,19,123,20],[121,19,121,20],[110,13,110,14],[120,11,120,12],[120,13,120,14],[125,19,125,20],[122,19,122,20],[120,15,120,16],[120,17,120,18],[120,19,120,20],[117,17,117,18],[117,19,117,20],[118,17,118,18],[118,19,118,20],[126,3,126,4],[126,5,126,6],[126,7,126,8],[126,9,126,10],[126,11,126,12],[126,13,126,14],[126,15,126,16],[120,7,120,8],[120,9,120,10],[122,3,122,4],[122,5,122,6],[122,7,122,8],[123,9,123,10],[117,1,118,1],[113,11,113,12],[112,3,112,4],[112,5,112,6],[112,7,112,8],[117,3,117,4],[117,5,117,6],[117,7,117,8],[117,9,117,10],[117,11,117,12],[114,3,114,4],[115,1,116,1],[115,3,115,4],[115,5,115,6],[115,7,115,8],[115,9,115,10],[115,11,115,12],[116,5,116,6],[116,7,116,8],[86,21,87,22],[86,3,86,6],[87,3,87,4],[87,5,87,6],[86,7,86,9],[87,9,88,9],[86,18,87,19],[86,20,88,20],[116,3,116,4],[110,11,110,12],[110,17,110,18],[110,19,110,20],[115,13,115,14],[115,15,115,16],[115,17,115,18],[116,9,116,10],[116,11,116,12],[116,13,116,14],[116,15,116,16],[116,17,116,18],[114,17,114,18],[111,17,111,18],[111,19,111,20],[111,13,111,14]]}
["G"]
["G","Multifamily Home Details"]
["G"]
["G"]
["G","Complete the table for each building in the project.  Input the number of units and the average floor area for units with the corresponding bedroom number. "]
["G"]
["G","Table 3.1: Building Unit summary"]
["G"]
["G","Building ID",null,"Studio",null,"1 Bedroom",null,"2 Bedrooms",null,"3 Bedrooms",null,"4 Bedrooms",null,"5 Bedrooms",null,"6 Bedrooms",null,"7 Bedrooms",null,"8 Bedrooms",null,null,null,null,null,"Additional Notes (Optional):"]
["G",null,null,"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"}]
["G","Building ID",null,"S_Unit","S_Area","1B_Unit","1B_Area","2B_Unit","2B_Area","3B_Unit","3B_Area","4B_Unit","4B_Area","5B_Unit","5B_Area","6B_Unit","6B_Area","7B_Unit","7B_Area","8B_Unit","8B_Area"]
["G",{"$f":"'1 - Multiple Buildings Details'!B24","v":0}]
["G","Total number of units",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(OFFSET(MD_BUS_Index,1,MATCH($D$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($F$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($H$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($J$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($L$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($N$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($P$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($R$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($T$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\n)","v":0}]
["G","Total number of bedrooms",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(OFFSET(MD_BUS_Index,1,MATCH($D$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($F$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($H$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*2,\nOFFSET(MD_BUS_Index,1,MATCH($J$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*3,\nOFFSET(MD_BUS_Index,1,MATCH($L$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*4,\nOFFSET(MD_BUS_Index,1,MATCH($N$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*5,\nOFFSET(MD_BUS_Index,1,MATCH($P$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*6,\nOFFSET(MD_BUS_Index,1,MATCH($R$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*7,\nOFFSET(MD_BUS_Index,1,MATCH($T$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*8,\n)","v":0}]
["G",{"$f":"CONCATENATE(\"Total Area of Dwelling Units\",IF(SI_IP_Units=\"IP\",\" (square feet)\",\" (square meters)\"))","v":"Total Area of Dwelling Units (square feet)"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(OFFSET(MD_BUS_Index,1,MATCH($D$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*OFFSET(MD_BUS_Index,1,MATCH($E$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($F$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*OFFSET(MD_BUS_Index,1,MATCH($G$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($H$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*OFFSET(MD_BUS_Index,1,MATCH($I$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($J$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*OFFSET(MD_BUS_Index,1,MATCH($K$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($L$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*OFFSET(MD_BUS_Index,1,MATCH($M$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($N$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*OFFSET(MD_BUS_Index,1,MATCH($O$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($P$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*OFFSET(MD_BUS_Index,1,MATCH($Q$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($R$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*OFFSET(MD_BUS_Index,1,MATCH($S$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\nOFFSET(MD_BUS_Index,1,MATCH($T$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1)*OFFSET(MD_BUS_Index,1,MATCH($U$11,MD_BUS_Hdr,0)-1,COUNTA(MD_BUS_Index),1),\n)","v":0}]
["G","Average Number of Bedrooms Per Unit",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(1/U13),0,U14/U13)","v":0}]
["G",{"$f":"CONCATENATE(\"Average Floor Area Per Unit\",IF(SI_IP_Units=\"IP\",\" (square feet)\",\" (square meters)\"))","v":"Average Floor Area Per Unit (square feet)"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(1/U13),0,U15/U13)","v":0}]
["G",{"$f":"CONCATENATE(\"Average Floor Area Per Unit for Reference Building\",IF(SI_IP_Units=\"IP\",\" (square feet)\",\" (square meters)\"))","v":"Average Floor Area Per Unit for Reference Building (square feet)"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(1/Avg_Bedrooms),0,ROUNDDOWN((Avg_Bedrooms-1)*(IF(SI_IP_Units=\"IP\",600,55.6)),0)+IF(SI_IP_Units=\"IP\",1000,93))","v":0}]
["G","Point Adjustment (1 point credit per 4% reduction in floor area versus reference; 1 point deduction per 4% increase in floor area versus reference).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(1/U18),0,ROUNDDOWN((U18-Avg_Bedroom_Area)/(U18*4%),0))","v":0}]
["G"]
["G","Building ID",null,"Total Number of Units",null,"Total Number of Bedrooms",null,"Total Area of Dwelling Units (square feet)",null,null,"Average Number of Bedrooms Per Unit",null,null,{"$f":"CONCATENATE(\"Average Floor Area per Unit\",IF(SI_IP_Units=\"IP\",\" (square feet)\",\" (square meter)\"))","v":"Average Floor Area per Unit (square feet)"},null,null,{"$f":"CONCATENATE(\"Average Floor Area Per Unit for Reference Building\",IF(SI_IP_Units=\"IP\",\" (square feet)\",\" (square meter)\"))","v":"Average Floor Area Per Unit for Reference Building (square feet)"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Point Adjustment (1 point credit per 4% reduction in floor area versus reference; 1 point deduction per 4% increase in floor area versus reference).","Avg Occupants/bedroom"]
["G",{"$f":"'1 - Multiple Buildings Details'!B24","v":0},null,{"$f":"SUM(INDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($D$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($F$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($H$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($J$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($L$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($N$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($P$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($R$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($T$11,MD_BUS_Hdr,0)),\n)","v":0},null,{"$f":"SUM(INDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($D$11,MD_BUS_Hdr,0))*1,\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($F$11,MD_BUS_Hdr,0))*1,\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($H$11,MD_BUS_Hdr,0))*2,\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($J$11,MD_BUS_Hdr,0))*3,\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($L$11,MD_BUS_Hdr,0))*4,\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($N$11,MD_BUS_Hdr,0))*5,\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($P$11,MD_BUS_Hdr,0))*6,\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($R$11,MD_BUS_Hdr,0))*7,\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($T$11,MD_BUS_Hdr,0))*8,\n)","v":0},null,{"$f":"SUM(INDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($D$11,MD_BUS_Hdr,0))*INDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($E$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($F$11,MD_BUS_Hdr,0))*INDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($G$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($H$11,MD_BUS_Hdr,0))*INDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($I$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($J$11,MD_BUS_Hdr,0))*INDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($K$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($L$11,MD_BUS_Hdr,0))*INDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($M$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($N$11,MD_BUS_Hdr,0))*INDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($O$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($P$11,MD_BUS_Hdr,0))*INDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($Q$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($R$11,MD_BUS_Hdr,0))*INDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($S$11,MD_BUS_Hdr,0)),\nINDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($T$11,MD_BUS_Hdr,0))*INDEX(MD_BUS_Table,MATCH($B22,MD_BUS_Index,0),MATCH($U$11,MD_BUS_Hdr,0)),\n)","v":0},null,null,{"$f":"IF(ISERROR(1/D22),0,F22/D22)","v":0},null,null,{"$f":"IF(ISERROR(1/D22),0,H22/D22)","v":0},null,null,{"$f":"IF(ISERROR(1/K22),0,ROUNDDOWN((K22-1)*(IF(SI_IP_Units=\"IP\",600,55.6)),0)+IF(SI_IP_Units=\"IP\",1000,93))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(1/Q22),0,ROUNDDOWN((Q22-N22)/(Q22*4%),0))","v":0},{"$f":"(D12*1+F12*2+H12*3+J12*4+L12*5+N12*6+P12*7+R12*8+T12*9)/F22","v":{"$error":"#DIV/0!"}}]
["G"]
["G","Table 3.2: Homes Dwelling Unit Equipment Calculator"]
["G"]
["G","Enter the appliances and equipment that is present in the residential dwelling units for the project. For clothes washers and dryers, enter the quantity of each unit installed within the project scope of work. "]
["G"]
["G","Building ID","Load Source","Quantity","ENERGY STAR Eqp?","Average bedrooms per dwelling unit",null,"Electric Loads",null,null,null,null,"Natural Gas Loads",null,null,null,null,{"$f":"CONCATENATE(\"Annual Service Hot Water Load \",IF(SI_IP_Units=\"IP\",\"(gallons/year)\",\"(Liters/year)\"))","v":"Annual Service Hot Water Load (gallons/year)"},null,null,null,"Measure #"]
["G",null,null,null,null,null,null,{"$f":"CONCATENATE(\"Annual Consumption \",IF(SI_IP_Units=\"IP\",\"(kWh/year)\",\"kWh/year\"))","v":"Annual Consumption (kWh/year)"},null,"Sensible Ratio","Latent Ratio",null,{"$f":"CONCATENATE(\"Annual Consumption \",IF(SI_IP_Units=\"IP\",\"(therms/year)\",\"kWh/year\"))","v":"Annual Consumption (therms/year)"},null,"Sensible Ratio","Latent Ratio",null,"Baseline Per Equipment","Proposed Design Per Equipment","Baseline Total","Proposed Design Total"]
["G",null,null,null,null,null,null,"Baseline","Proposed",null,null,null,"Baseline","Proposed"]
["G","Building ID","Load_Source","Qty","Energy_Star","Avg_Bedrooms_DU","Blank1","Base_Elec_Consumption","Design_Elec_Consumption","Elec_Sens_Ratio","Elec_Latent_Ratio","Blank2","Base_Ng_Consumption","Design_Ng_Consumption","NG_Sens_Ratio","NG_Latent_Ratio","Blank3","Base_DHW_Equip","Design_DHW_Equip","Base_DHW_Annual","Design_DHW_Annual"]
["A",{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IFERROR(INDEX(MD_BUS_SumTable,MATCH($B32,MD_BUS_SumIndex,0),MATCH($K$21,MD_BUS_SumHdr,0)),\"\")","v":0},null,{"$f":"IFERROR($D32*((VLOOKUP($C32,Homes_DwellingEqpLookup,2,FALSE)+VLOOKUP($C32,Homes_DwellingEqpLookup,6,FALSE)*$F32)*VLOOKUP($C32,Homes_DwellingEqpLookup,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(IF($E32=\"No\",$H32,$D32*(VLOOKUP($C32,Homes_DwellingEqpLookup,3,FALSE)+VLOOKUP($C32,Homes_DwellingEqpLookup,6,FALSE)*$F32)*VLOOKUP($C32,Homes_DwellingEqpLookup,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C32,Homes_DwellingEqpLookup,4,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C32,Homes_DwellingEqpLookup,5,0),\"\")","v":""},null,{"$f":"IFERROR($D32*((VLOOKUP($C32,Homes_DwellingEqpLookup,7,FALSE)+VLOOKUP($C32,Homes_DwellingEqpLookup,11,FALSE)*$F32)*VLOOKUP($C32,Homes_DwellingEqpLookup,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(IF($E32=\"No\",$M32,$D32*(VLOOKUP($C32,Homes_DwellingEqpLookup,8,FALSE)+VLOOKUP($C32,Homes_DwellingEqpLookup,11,FALSE)*$F32)*VLOOKUP($C32,Homes_DwellingEqpLookup,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C32,Homes_DwellingEqpLookup,9,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C32,Homes_DwellingEqpLookup,10,0),\"\")","v":""},null,{"$f":"IFERROR(VLOOKUP($C32,Homes_DwellingEqpLookup,13,0),\"\")","v":""},{"$f":"IFERROR(IF($E32=\"No\",$R32,VLOOKUP($C32,Homes_DwellingEqpLookup,14,0)),\"\")","v":""},{"$f":"IFERROR($R32*$D32,\"\")","v":""},{"$f":"IFERROR($S32*$D32,\"\")","v":""}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IFERROR(INDEX(MD_BUS_SumTable,MATCH($B33,MD_BUS_SumIndex,0),MATCH($K$21,MD_BUS_SumHdr,0)),\"\")","v":0},null,{"$f":"IFERROR($D33*((VLOOKUP($C33,Homes_DwellingEqpLookup,2,FALSE)+VLOOKUP($C33,Homes_DwellingEqpLookup,6,FALSE)*$F33)*VLOOKUP($C33,Homes_DwellingEqpLookup,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(IF($E33=\"No\",$H33,$D33*(VLOOKUP($C33,Homes_DwellingEqpLookup,3,FALSE)+VLOOKUP($C33,Homes_DwellingEqpLookup,6,FALSE)*$F33)*VLOOKUP($C33,Homes_DwellingEqpLookup,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C33,Homes_DwellingEqpLookup,4,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C33,Homes_DwellingEqpLookup,5,0),\"\")","v":""},null,{"$f":"IFERROR($D33*((VLOOKUP($C33,Homes_DwellingEqpLookup,7,FALSE)+VLOOKUP($C33,Homes_DwellingEqpLookup,11,FALSE)*$F33)*VLOOKUP($C33,Homes_DwellingEqpLookup,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(IF($E33=\"No\",$M33,$D33*(VLOOKUP($C33,Homes_DwellingEqpLookup,8,FALSE)+VLOOKUP($C33,Homes_DwellingEqpLookup,11,FALSE)*$F33)*VLOOKUP($C33,Homes_DwellingEqpLookup,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C33,Homes_DwellingEqpLookup,9,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C33,Homes_DwellingEqpLookup,10,0),\"\")","v":""},null,{"$f":"IFERROR(VLOOKUP($C33,Homes_DwellingEqpLookup,13,0),\"\")","v":""},{"$f":"IFERROR(IF($E33=\"No\",$R33,VLOOKUP($C33,Homes_DwellingEqpLookup,14,0)),\"\")","v":""},{"$f":"IFERROR($R33*$D33,\"\")","v":""},{"$f":"IFERROR($S33*$D33,\"\")","v":""}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IFERROR(INDEX(MD_BUS_SumTable,MATCH($B34,MD_BUS_SumIndex,0),MATCH($K$21,MD_BUS_SumHdr,0)),\"\")","v":0},null,{"$f":"IFERROR($D34*((VLOOKUP($C34,Homes_DwellingEqpLookup,2,FALSE)+VLOOKUP($C34,Homes_DwellingEqpLookup,6,FALSE)*$F34)*VLOOKUP($C34,Homes_DwellingEqpLookup,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(IF($E34=\"No\",$H34,$D34*(VLOOKUP($C34,Homes_DwellingEqpLookup,3,FALSE)+VLOOKUP($C34,Homes_DwellingEqpLookup,6,FALSE)*$F34)*VLOOKUP($C34,Homes_DwellingEqpLookup,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C34,Homes_DwellingEqpLookup,4,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C34,Homes_DwellingEqpLookup,5,0),\"\")","v":""},null,{"$f":"IFERROR($D34*((VLOOKUP($C34,Homes_DwellingEqpLookup,7,FALSE)+VLOOKUP($C34,Homes_DwellingEqpLookup,11,FALSE)*$F34)*VLOOKUP($C34,Homes_DwellingEqpLookup,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(IF($E34=\"No\",$M34,$D34*(VLOOKUP($C34,Homes_DwellingEqpLookup,8,FALSE)+VLOOKUP($C34,Homes_DwellingEqpLookup,11,FALSE)*$F34)*VLOOKUP($C34,Homes_DwellingEqpLookup,12,FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C34,Homes_DwellingEqpLookup,9,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C34,Homes_DwellingEqpLookup,10,0),\"\")","v":""},null,{"$f":"IFERROR(VLOOKUP($C34,Homes_DwellingEqpLookup,13,0),\"\")","v":""},{"$f":"IFERROR(IF($E34=\"No\",$R34,VLOOKUP($C34,Homes_DwellingEqpLookup,14,0)),\"\")","v":""},{"$f":"IFERROR($R34*$D34,\"\")","v":""},{"$f":"IFERROR($S34*$D34,\"\")","v":""}]
[]
[]
["G"]
["G"]
["G","Table 3.3: Homes Dwelling Unit Equipment Modeling Summary"]
["G"]
["G",{"$f":" CONCATENATE(\"Report the modeled Receptacle Equipment and Appliances Equivalent Full Load Hours of Operation in the Schedules tab before referring to the table below.\",\" The Equivalent Full Load Hours of Operation is used to calculate the equipment power density for resdential dwelling units that must be modeled based on the building equipment reported for the building.\",\" After confirming the Equivalent Full Load Hours of Operation in the schedules tab, use the values below for the Baseline and Proposed Miscellaneous Equipment Loads in the Dwelling Units. These loads include \",IF(SI_IP_Units=\"IP\",\"0.5 Watts per square foot \",\"5.38 Watts per square meter\"), \" of electric miscellaneous equipment load with a 0.9 sensible ratio and 0.1 latent ratio in addition to the equipment load sources selected above.\")","v":"Report the modeled Receptacle Equipment and Appliances Equivalent Full Load Hours of Operation in the Schedules tab before referring to the table below. The Equivalent Full Load Hours of Operation is used to calculate the equipment power density for resdential dwelling units that must be modeled based on the building equipment reported for the building. After confirming the Equivalent Full Load Hours of Operation in the schedules tab, use the values below for the Baseline and Proposed Miscellaneous Equipment Loads in the Dwelling Units. These loads include 0.5 Watts per square foot  of electric miscellaneous equipment load with a 0.9 sensible ratio and 0.1 latent ratio in addition to the equipment load sources selected above."}]
["G"]
["G","Building ID","Equipment Type",{"$f":"CONCATENATE(\"Total Area of Dwelling Units\",IF(SI_IP_Units=\"IP\",\" (square feet)\",\" (square meters)\"))","v":"Total Area of Dwelling Units (square feet)"},"Equivalent Full Load Hours of Dwelling Unit Miscellaneous Equipment Operation Per Year","Electric Miscellaneous Loads in Dwelling Unit (including appliances and equipment listed above)",null,null,null,null,null,null,"Natural Gas Miscellaneous Loads in Dwelling Unit (including appliances and equipment listed above)",null,null,null,null,null,null,{"$f":"CONCATENATE(\"Dwelling Unit Equipment Hot Water Loads \",IF(SI_IP_Units=\"IP\",\"(gallons/year)\",\"(Liters/year)\"))","v":"Dwelling Unit Equipment Hot Water Loads (gallons/year)"},null,"Measure #"]
["G",null,null,null,null,"Baseline",null,null,"Proposed",null,null,null,"Baseline",null,null,"Proposed"]
["G",null,null,null,null,{"$f":"CONCATENATE(\"Equipment Power Density \", IF(SI_IP_Units=\"IP\",\"(Watts/ sq ft)\",\"(Watts/ sq m)\"))","v":"Equipment Power Density (Watts/ sq ft)"},"Sensible Ratio","Latent Ratio",{"$f":"CONCATENATE(\"Equipment Power Density \", IF(SI_IP_Units=\"IP\",\"(Watts/ sq ft)\",\"(Watts/ sq m)\"))","v":"Equipment Power Density (Watts/ sq ft)"},"Sensible Ratio","Latent Ratio",null,{"$f":"CONCATENATE(\"Equipment Power Density \", IF(SI_IP_Units=\"IP\",\"(Btu/ sq ft)\",\"(Watts/ sq m)\"))","v":"Equipment Power Density (Btu/ sq ft)"},"Sensible Ratio","Latent Ratio",{"$f":"CONCATENATE(\"Equipment Power Density \",  IF(SI_IP_Units=\"IP\",\"(Btu/ sq ft)\",\"(Watts/ sq m)\"))","v":"Equipment Power Density (Btu/ sq ft)"},"Sensible Ratio","Latent Ratio",null,"Base","Proposed"]
["G",{"$f":"B43","v":"Building ID"},"EFLH","Total_Area","Blank1","Base_EPD_Elecric","Base_Elec_Sens_Ratio","Base_Elec_Latent_Ratio","Prop_EPD_Elecric","Prop_Elec_Sens_Ratio","Prop_Elec_Latent_Ratio","Blank2","Base_Ng_EPD","Base_Ng_Sens_Ratio","Base_Ng_Latent_Ratio","Prop_Ng_EPD","Prop_Ng_Sens_Ratio","Prop_Ng_Latent_Ratio","Blank3","Base_HW_Loads","Proposed_HW_Loads"]
["G",{"$f":"'1 - Multiple Buildings Details'!B24","v":0},"Summary of Equipment in Table 3.2",{"$f":"INDEX(MD_BUS_SumTable,MATCH($B47,MD_BUS_SumIndex,0),MATCH($H$21,MD_BUS_SumHdr,0))","v":0},8760,{"$f":"IFERROR((SUM(H32:H35))/E47*1000/D47,\"\")","v":""},{"$f":"IFERROR(SUMPRODUCT(H32:H35,J32:J35)/SUM(H32:H35),\"\")","v":""},{"$f":"IFERROR(SUMPRODUCT(H32:H35,K32:K35)/SUM(H32:H35),\"\")","v":""},{"$f":"IFERROR((SUM(I32:I35))/E47*1000/D47,\"\")","v":""},{"$f":"IFERROR(SUMPRODUCT(I32:I35,J32:J35)/SUM(I32:I35),\"\")","v":""},{"$f":"IFERROR(SUMPRODUCT(I32:I35,K32:K35)/SUM(I32:I35),\"\")","v":""},null,{"$f":"IFERROR((SUM(M32:M35))/E47/D47*IF(SI_IP_Units=\"IP\",100000,1000),\"\")","v":""},{"$f":"IFERROR(IF(SUM(O34:O35)=0,0,SUMPRODUCT(M32:M35,O32:O35)/SUM(M32:M35)),\"\")","v":0},{"$f":"IFERROR(IF(SUM(P34:P35)=0,0,SUMPRODUCT(M32:M35,P32:P35)/SUM(M32:M35)),\"\")","v":0},{"$f":"IFERROR((SUM(N32:N35))/E47/D47*IF(SI_IP_Units=\"IP\",100000,1000),\"\")","v":""},{"$f":"IFERROR(IF(SUM(O34:O35)=0,0,SUMPRODUCT(N32:N35,O32:O35)/SUM(N32:N35)),\"\")","v":0},{"$f":"IFERROR(IF(SUM(P34:P35)=0,0,SUMPRODUCT(N32:N35,P32:P35)/SUM(N32:N35)),\"\")","v":0},null,{"$f":"IFERROR(SUMIF(MD_HDUEC_Index1,$B47,OFFSET(MD_HDUEC_Index1,0,MATCH($T$31,MD_HDUEC_Hdr,0)-1,ROWS(MD_HDUEC_Index1),1)),\"\")","v":0},{"$f":"IFERROR(SUMIF(MD_HDUEC_Index1,$B47,OFFSET(MD_HDUEC_Index1,0,MATCH($U$31,MD_HDUEC_Hdr,0)-1,ROWS(MD_HDUEC_Index1),1)),\"\")","v":0}]
["G",{"$f":"'1 - Multiple Buildings Details'!B25","v":0},"All Other Dwelling Unit Receptacle Loads",{"$f":"INDEX(MD_BUS_SumTable,MATCH($B48,MD_BUS_SumIndex,0),MATCH($H$21,MD_BUS_SumHdr,0))","v":0},{"$f":"'2a - Schedules'!G12","v":2117},{"$f":"0.5*(IF(SI_IP_Units=\"IP\",1,10.76))","v":0.5},0.9,0.1,{"$f":"0.5*(IF(SI_IP_Units=\"IP\",1,10.76))","v":0.5},0.9,0.1,null,0,0,0,0,0,0,null,{"$f":"IFERROR(SUMIF(MD_HDUEC_Index1,$B48,OFFSET(MD_HDUEC_Index1,0,MATCH($T$31,MD_HDUEC_Hdr,0)-1,ROWS(MD_HDUEC_Index1),1)),\"\")","v":0},{"$f":"IFERROR(SUMIF(MD_HDUEC_Index1,$B48,OFFSET(MD_HDUEC_Index1,0,MATCH($U$31,MD_HDUEC_Hdr,0)-1,ROWS(MD_HDUEC_Index1),1)),\"\")","v":0}]
["G"]
["G","Table 3.4: Homes Laundry Room Equipment Calculator"]
["G"]
["G","If the project has one or more laundry rooms serving multiple dwelling units, enter the equipment that is present in the laundry rooms. Leave blank if the project has no laundry rooms."]
["G"]
["G","Building ID","Load Source","Quantity","Energy Star Equip-ment?","Average Bedrooms per Dwelling Unit",null,"Electric Loads",null,null,null,null,"Natural Gas Loads",null,null,null,null,{"$f":"CONCATENATE(\"Annual Service Hot Water Load \",IF(SI_IP_Units=\"IP\",\"(gallons/year)\",\"(Liters/year)\"))","v":"Annual Service Hot Water Load (gallons/year)"},null,null,null,"Measure #"]
["G",null,null,null,null,null,null,{"$f":"CONCATENATE(\"Annual Consumption \",IF(SI_IP_Units=\"IP\",\"(kWh/year)\",\"kWh/year\"))","v":"Annual Consumption (kWh/year)"},null,"Sensible Ratio","Latent Ratio",null,{"$f":"CONCATENATE(\"Annual Consumption \",IF(SI_IP_Units=\"IP\",\"(therms/year)\",\"kWh/year\"))","v":"Annual Consumption (therms/year)"},null,"Sensible Ratio","Latent Ratio",null,"Baseline Per Equipment","Proposed Design Per Equipment","Baseline Total","Proposed Design Total"]
["G",null,null,null,null,null,null,"Baseline","Proposed",null,null,null,"Baseline","Proposed"]
["G","Building ID","Load_Source","Qty","Energy_Star","Avg_Bedrooms_DU",null,"Base_Elec_Consumption","Design_Elec_Consumption","Elec_Sens_Ratio","Elec_Latent_Ratio",null,"Base_Ng_Consumption","Design_Ng_Consumption","NG_Sens_Ratio","NG_Latent_Ratio",null,"Base_DHW_Equip","Design_DHW_Equip","Base_DHW_Annual","Design_DHW_Annual"]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IFERROR(INDEX(MD_BUS_SumTable,MATCH($B58,MD_BUS_SumIndex,0),MATCH($K$21,MD_BUS_SumHdr,0)),\"\")","v":0},null,{"$f":"IFERROR((VLOOKUP($C58,Homes_LaundryEqpLookup,2,FALSE)+VLOOKUP($C58,Homes_LaundryEqpLookup,6,FALSE)*$F58)*VLOOKUP($C58,Homes_LaundryEqpLookup,12,FALSE)*D58,\"\")","v":""},{"$f":"IFERROR(IF($E58=\"No\",$H58,(VLOOKUP($C58,Homes_LaundryEqpLookup,3,FALSE)+VLOOKUP($C58,Homes_LaundryEqpLookup,6,FALSE)*$F58)*VLOOKUP($C58,Homes_LaundryEqpLookup,12,FALSE))*D58,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C58,Homes_LaundryEqpLookup,4,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C58,Homes_LaundryEqpLookup,5,0),\"\")","v":""},null,{"$f":"IFERROR((VLOOKUP($C58,Homes_LaundryEqpLookup,7,FALSE)+VLOOKUP($C58,Homes_LaundryEqpLookup,11,FALSE)*$F58)*VLOOKUP($C58,Homes_LaundryEqpLookup,12,FALSE)*D58,\"\")","v":""},{"$f":"IFERROR(IF($E58=\"No\",$M58,(VLOOKUP($C58,Homes_LaundryEqpLookup,8,FALSE)+VLOOKUP($C58,Homes_LaundryEqpLookup,11,FALSE)*$F58)*VLOOKUP($C58,Homes_LaundryEqpLookup,12,FALSE))*D58,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C58,Homes_LaundryEqpLookup,9,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C58,Homes_LaundryEqpLookup,10,0),\"\")","v":""},null,{"$f":"IFERROR(VLOOKUP($C58,Homes_LaundryEqpLookup,13,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C58,Homes_LaundryEqpLookup,14,0),\"\")","v":""},{"$f":"IFERROR($R58*$D58,\"\")","v":""},{"$f":"IFERROR($S58*$D58,\"\")","v":""}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IFERROR(INDEX(MD_BUS_SumTable,MATCH($B59,MD_BUS_SumIndex,0),MATCH($K$21,MD_BUS_SumHdr,0)),\"\")","v":0},null,{"$f":"IFERROR((VLOOKUP($C59,Homes_LaundryEqpLookup,2,FALSE)+VLOOKUP($C59,Homes_LaundryEqpLookup,6,FALSE)*$F59)*VLOOKUP($C59,Homes_LaundryEqpLookup,12,FALSE)*D59,\"\")","v":""},{"$f":"IFERROR(IF($E59=\"No\",$H59,(VLOOKUP($C59,Homes_LaundryEqpLookup,3,FALSE)+VLOOKUP($C59,Homes_LaundryEqpLookup,6,FALSE)*$F59)*VLOOKUP($C59,Homes_LaundryEqpLookup,12,FALSE))*D59,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C59,Homes_LaundryEqpLookup,4,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C59,Homes_LaundryEqpLookup,5,0),\"\")","v":""},null,{"$f":"IFERROR((VLOOKUP($C59,Homes_LaundryEqpLookup,7,FALSE)+VLOOKUP($C59,Homes_LaundryEqpLookup,11,FALSE)*$F59)*VLOOKUP($C59,Homes_LaundryEqpLookup,12,FALSE)*D59,\"\")","v":""},{"$f":"IFERROR(IF($E59=\"No\",$M59,(VLOOKUP($C59,Homes_LaundryEqpLookup,8,FALSE)+VLOOKUP($C59,Homes_LaundryEqpLookup,11,FALSE)*$F59)*VLOOKUP($C59,Homes_LaundryEqpLookup,12,FALSE))*D59,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C59,Homes_LaundryEqpLookup,9,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C59,Homes_LaundryEqpLookup,10,0),\"\")","v":""},null,{"$f":"IFERROR(VLOOKUP($C59,Homes_LaundryEqpLookup,13,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C59,Homes_LaundryEqpLookup,14,0),\"\")","v":""},{"$f":"IFERROR($R59*$D59,\"\")","v":""},{"$f":"IFERROR($S59*$D59,\"\")","v":""}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IFERROR(INDEX(MD_BUS_SumTable,MATCH($B60,MD_BUS_SumIndex,0),MATCH($K$21,MD_BUS_SumHdr,0)),\"\")","v":0},null,{"$f":"IFERROR((VLOOKUP($C60,Homes_LaundryEqpLookup,2,FALSE)+VLOOKUP($C60,Homes_LaundryEqpLookup,6,FALSE)*$F60)*VLOOKUP($C60,Homes_LaundryEqpLookup,12,FALSE)*D60,\"\")","v":""},{"$f":"IFERROR(IF($E60=\"No\",$H60,(VLOOKUP($C60,Homes_LaundryEqpLookup,3,FALSE)+VLOOKUP($C60,Homes_LaundryEqpLookup,6,FALSE)*$F60)*VLOOKUP($C60,Homes_LaundryEqpLookup,12,FALSE))*D60,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C60,Homes_LaundryEqpLookup,4,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C60,Homes_LaundryEqpLookup,5,0),\"\")","v":""},null,{"$f":"IFERROR((VLOOKUP($C60,Homes_LaundryEqpLookup,7,FALSE)+VLOOKUP($C60,Homes_LaundryEqpLookup,11,FALSE)*$F60)*VLOOKUP($C60,Homes_LaundryEqpLookup,12,FALSE)*D60,\"\")","v":""},{"$f":"IFERROR(IF($E60=\"No\",$M60,(VLOOKUP($C60,Homes_LaundryEqpLookup,8,FALSE)+VLOOKUP($C60,Homes_LaundryEqpLookup,11,FALSE)*$F60)*VLOOKUP($C60,Homes_LaundryEqpLookup,12,FALSE))*D60,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C60,Homes_LaundryEqpLookup,9,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C60,Homes_LaundryEqpLookup,10,0),\"\")","v":""},null,{"$f":"IFERROR(VLOOKUP($C60,Homes_LaundryEqpLookup,13,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C60,Homes_LaundryEqpLookup,14,0),\"\")","v":""},{"$f":"IFERROR($R60*$D60,\"\")","v":""},{"$f":"IFERROR($S60*$D60,\"\")","v":""}]
["B",null,null,null,null,{"$f":"IFERROR(INDEX(MD_BUS_SumTable,MATCH($B61,MD_BUS_SumIndex,0),MATCH($K$21,MD_BUS_SumHdr,0)),\"\")","v":0},null,{"$f":"IFERROR((VLOOKUP($C61,Homes_LaundryEqpLookup,2,FALSE)+VLOOKUP($C61,Homes_LaundryEqpLookup,6,FALSE)*$F61)*VLOOKUP($C61,Homes_LaundryEqpLookup,12,FALSE)*D61,\"\")","v":""},{"$f":"IFERROR(IF($E61=\"No\",$H61,(VLOOKUP($C61,Homes_LaundryEqpLookup,3,FALSE)+VLOOKUP($C61,Homes_LaundryEqpLookup,6,FALSE)*$F61)*VLOOKUP($C61,Homes_LaundryEqpLookup,12,FALSE))*D61,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C61,Homes_LaundryEqpLookup,4,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C61,Homes_LaundryEqpLookup,5,0),\"\")","v":""},null,{"$f":"IFERROR((VLOOKUP($C61,Homes_LaundryEqpLookup,7,FALSE)+VLOOKUP($C61,Homes_LaundryEqpLookup,11,FALSE)*$F61)*VLOOKUP($C61,Homes_LaundryEqpLookup,12,FALSE)*D61,\"\")","v":""},{"$f":"IFERROR(IF($E61=\"No\",$M61,(VLOOKUP($C61,Homes_LaundryEqpLookup,8,FALSE)+VLOOKUP($C61,Homes_LaundryEqpLookup,11,FALSE)*$F61)*VLOOKUP($C61,Homes_LaundryEqpLookup,12,FALSE))*D61,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C61,Homes_LaundryEqpLookup,9,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C61,Homes_LaundryEqpLookup,10,0),\"\")","v":""},null,{"$f":"IFERROR(VLOOKUP($C61,Homes_LaundryEqpLookup,13,0),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($C61,Homes_LaundryEqpLookup,14,0),\"\")","v":""},{"$f":"IFERROR($R61*$D61,\"\")","v":""},{"$f":"IFERROR($S61*$D61,\"\")","v":""}]
["G"]
["G"]
["G"]
["G"]
["G","Table 3.5: Homes Laundry Room Equipment Modeling Summary"]
["G"]
["G",{"$f":" CONCATENATE(\"Identify the equivalent full load hours of operation and building area for the landury room(s) below. \",\"In the energy model(s), use the values below for the Baseline and Proposed Miscellaneous Equipment Loads in the Laundry Rooms. These loads include \",IF(SI_IP_Units=\"IP\",\"0.2 Watts per square foot \",\"2.15 Watts per square meter\"), \" of electric miscellaneous equipment load with a 1.0 sensible ratio and 0.0 latent ratio in addition to the equipment load sources selected above.\",\" Note that the Equivalent Full Load Hours of operation noted here must be consistent with that of the energy model in order for the equipment power densities\",\" listed here to appropriately calculate the annual laundry miscellaneous energy consumption in the energy model.\")","v":"Identify the equivalent full load hours of operation and building area for the landury room(s) below. In the energy model(s), use the values below for the Baseline and Proposed Miscellaneous Equipment Loads in the Laundry Rooms. These loads include 0.2 Watts per square foot  of electric miscellaneous equipment load with a 1.0 sensible ratio and 0.0 latent ratio in addition to the equipment load sources selected above. Note that the Equivalent Full Load Hours of operation noted here must be consistent with that of the energy model in order for the equipment power densities listed here to appropriately calculate the annual laundry miscellaneous energy consumption in the energy model."}]
["G"]
["G","Building ID","Equivalent Full Load Hours of Dwelling Unit Miscellaneous Equipment Operation Per Year",{"$f":"CONCATENATE(\"Total Area of Laundry Rooms\",IF(SI_IP_Units=\"IP\",\" (square feet)\",\" (square meters)\"))","v":"Total Area of Laundry Rooms (square feet)"},null,"Electric Loads in Laundry Room (including appliances and equipment listed above)",null,null,null,null,null,null,"Natural Gas Loads in Laundry Room (including appliances and equipment listed above)",null,null,null,null,null,null,{"$f":"CONCATENATE(\"Laundry Room Equipment Hot Water Loads \",IF(SI_IP_Units=\"IP\",\"(gallons/year)\",\"(Liters/year)\"))","v":"Laundry Room Equipment Hot Water Loads (gallons/year)"},null,"Measure #"]
["G",null,null,null,null,"Baseline",null,null,"Proposed",null,null,null,"Baseline",null,null,"Proposed"]
["G",null,null,null,null,{"$f":"CONCATENATE(\"Equipment Power Density \", IF(SI_IP_Units=\"IP\",\"(Watts/ sq ft)\",\"(Watts/ sq m)\"))","v":"Equipment Power Density (Watts/ sq ft)"},"Sensible Ratio","Latent Ratio",{"$f":"CONCATENATE(\"Equipment Power Density \", IF(SI_IP_Units=\"IP\",\"(Watts/ sq ft)\",\"(Watts/ sq m)\"))","v":"Equipment Power Density (Watts/ sq ft)"},"Sensible Ratio","Latent Ratio",null,{"$f":"CONCATENATE(\"Equipment Power Density \",  IF(SI_IP_Units=\"IP\",\"(Btu/ sq ft)\",\"(Watts/ sq m)\"))","v":"Equipment Power Density (Btu/ sq ft)"},"Sensible Ratio","Latent Ratio",{"$f":"CONCATENATE(\"Equipment Power Density \", IF(SI_IP_Units=\"IP\",\"(Btu/ sq ft)\",\"(Watts/ sq m)\"))","v":"Equipment Power Density (Btu/ sq ft)"},"Sensible Ratio","Latent Ratio",null,"Base","Proposed"]
["G","Building ID","EFLH","Total_Area","Blank1","Base_EPD_Elecric","Base_Elec_Sens_Ratio","Base_Elec_Latent_Ratio","Prop_EPD_Elecric","Prop_Elec_Sens_Ratio","Prop_Elec_Latent_Ratio","Blank2","Base_Ng_EPD","Base_Ng_Sens_Ratio","Base_Ng_Latent_Ratio","Prop_Ng_EPD","Prop_Ng_Sens_Ratio","Prop_Ng_Latent_Ratio","Blank3","Base_HW_Loads","Proposed_HW_Loads"]
["G",{"$f":"'1 - Multiple Buildings Details'!B24","v":0},null,null,null,{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B74,OFFSET(MD_Laundry_Index,0,MATCH($H$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1))/$D74*1000/$C74+0.2*(IF(SI_IP_Units=\"IP\",1,2.15)),\"\")","v":""},{"$f":"IFERROR((SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($H$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($J$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B74))*1000/$C74+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D74*1)/(SUMIF(MD_Laundry_Index,$B74,(OFFSET(MD_Laundry_Index,0,MATCH($H$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)))*1000/$C74+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D74),\"\")","v":""},{"$f":"IFERROR((SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($H$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($K$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B74))*1000/$C74+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D74*0)/(SUMIF(MD_Laundry_Index,$B74,(OFFSET(MD_Laundry_Index,0,MATCH($H$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)))*1000/$C74+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D74),\"\")","v":""},{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B74,OFFSET(MD_Laundry_Index,0,MATCH($I$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1))/$D74*1000/$C74+0.2*(IF(SI_IP_Units=\"IP\",1,10.76)),\"\")","v":""},{"$f":"IFERROR((SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($I$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($J$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B74))*1000/$C74+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D74*1)/(SUMIF(MD_Laundry_Index,$B74,(OFFSET(MD_Laundry_Index,0,MATCH($I$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)))*1000/$C74+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D74),\"\")","v":""},{"$f":"IFERROR((SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($I$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($K$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B74))*1000/$C74+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D74*0)/(SUMIF(MD_Laundry_Index,$B74,(OFFSET(MD_Laundry_Index,0,MATCH($I$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)))*1000/$C74+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D74),\"\")","v":""},null,{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B74,OFFSET(MD_Laundry_Index,0,MATCH($M$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1))/$D74/$C74*IF(SI_IP_Units=\"IP\",100000,1000),\"\")","v":""},{"$f":"IFERROR(SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($M$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($O$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B74))/SUMIF(MD_Laundry_Index,$B74,OFFSET(MD_Laundry_Index,0,MATCH($M$57,MD_Laundry_Hdr,0)-1)),\"\")","v":""},{"$f":"IFERROR(SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($M$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($P$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B74))/SUMIF(MD_Laundry_Index,$B74,OFFSET(MD_Laundry_Index,0,MATCH($M$57,MD_Laundry_Hdr,0)-1)),\"\")","v":""},{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B74,OFFSET(MD_Laundry_Index,0,MATCH($N$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1))/$D74/$C74*IF(SI_IP_Units=\"IP\",100000,1000),\"\")","v":""},{"$f":"IFERROR(SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($N$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($O$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B74))/SUMIF(MD_Laundry_Index,$B74,OFFSET(MD_Laundry_Index,0,MATCH($N$57,MD_Laundry_Hdr,0)-1)),\"\")","v":""},{"$f":"IFERROR(SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($N$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($P$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B74))/SUMIF(MD_Laundry_Index,$B74,OFFSET(MD_Laundry_Index,0,MATCH($N$57,MD_Laundry_Hdr,0)-1)),\"\")","v":""},null,{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B74,OFFSET(MD_Laundry_Index,0,MATCH($T$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)),\"\")","v":0},{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B74,OFFSET(MD_Laundry_Index,0,MATCH($U$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)),\"\")","v":0}]
["C",{"$f":"'1 - Multiple Buildings Details'!B24","v":0},null,null,null,{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B75,OFFSET(MD_Laundry_Index,0,MATCH($H$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1))/$D75*1000/$C75+0.2*(IF(SI_IP_Units=\"IP\",1,2.15)),\"\")","v":""},{"$f":"IFERROR((SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($H$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($J$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B75))*1000/$C75+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D75*1)/(SUMIF(MD_Laundry_Index,$B75,(OFFSET(MD_Laundry_Index,0,MATCH($H$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)))*1000/$C75+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D75),\"\")","v":""},{"$f":"IFERROR((SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($H$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($K$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B75))*1000/$C75+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D75*0)/(SUMIF(MD_Laundry_Index,$B75,(OFFSET(MD_Laundry_Index,0,MATCH($H$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)))*1000/$C75+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D75),\"\")","v":""},{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B75,OFFSET(MD_Laundry_Index,0,MATCH($I$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1))/$D75*1000/$C75+0.2*(IF(SI_IP_Units=\"IP\",1,10.76)),\"\")","v":""},{"$f":"IFERROR((SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($I$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($J$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B75))*1000/$C75+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D75*1)/(SUMIF(MD_Laundry_Index,$B75,(OFFSET(MD_Laundry_Index,0,MATCH($I$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)))*1000/$C75+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D75),\"\")","v":""},{"$f":"IFERROR((SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($I$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($K$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B75))*1000/$C75+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D75*0)/(SUMIF(MD_Laundry_Index,$B75,(OFFSET(MD_Laundry_Index,0,MATCH($I$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)))*1000/$C75+IF(SI_IP_Units=\"IP\",0.2,0.2*10.76)*$D75),\"\")","v":""},null,{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B75,OFFSET(MD_Laundry_Index,0,MATCH($M$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1))/$D75/$C75*IF(SI_IP_Units=\"IP\",100000,1000),\"\")","v":""},{"$f":"IFERROR(SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($M$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($O$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B75))/SUMIF(MD_Laundry_Index,$B75,OFFSET(MD_Laundry_Index,0,MATCH($M$57,MD_Laundry_Hdr,0)-1)),\"\")","v":""},{"$f":"IFERROR(SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($M$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($P$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B75))/SUMIF(MD_Laundry_Index,$B75,OFFSET(MD_Laundry_Index,0,MATCH($M$57,MD_Laundry_Hdr,0)-1)),\"\")","v":""},{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B75,OFFSET(MD_Laundry_Index,0,MATCH($N$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1))/$D75/$C75*IF(SI_IP_Units=\"IP\",100000,1000),\"\")","v":""},{"$f":"IFERROR(SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($N$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($O$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B75))/SUMIF(MD_Laundry_Index,$B75,OFFSET(MD_Laundry_Index,0,MATCH($N$57,MD_Laundry_Hdr,0)-1)),\"\")","v":""},{"$f":"IFERROR(SUMPRODUCT(OFFSET(MD_Laundry_Index,0,MATCH($N$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),OFFSET(MD_Laundry_Index,0,MATCH($P$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1),--(MD_Laundry_Index=$B75))/SUMIF(MD_Laundry_Index,$B75,OFFSET(MD_Laundry_Index,0,MATCH($N$57,MD_Laundry_Hdr,0)-1)),\"\")","v":""},null,{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B75,OFFSET(MD_Laundry_Index,0,MATCH($T$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)),\"\")","v":0},{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B75,OFFSET(MD_Laundry_Index,0,MATCH($U$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)),\"\")","v":0}]
["G"]
["G"]
["G","Table 3.6: Homes Service Water Heating Load Summary"]
["G"]
["G","Residential Usage Profile Dependent on Project Demographics",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Baseline Residential Usage per person\nExcluding Clothes / Dish Washers"]
["G","Low","Demographics such as all occupants working, seniors, middle income, and higher population density.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SI_IP_Units=\"IP\",12,45)","v":12},{"$f":"IF(SI_IP_Units=\"IP\",\"gallons/day\",\"liters/day\")","v":"gallons/day"}]
["G","Medium","Demographics such as mixture of working / non-working occupants, mixture of age groups, medium population densities.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SI_IP_Units=\"IP\",25,95)","v":25},{"$f":"IF(SI_IP_Units=\"IP\",\"gallons/day\",\"liters/day\")","v":"gallons/day"}]
["G","High","Demographics such high percentages of children, low income, public assistance, or no occupants working.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SI_IP_Units=\"IP\",44,167)","v":44},{"$f":"IF(SI_IP_Units=\"IP\",\"gallons/day\",\"liters/day\")","v":"gallons/day"}]
["G"]
["G",{"$f":"CONCATENATE(\"Report the modeled Service Water Heating Full Load Hours of Operation in the Schedules tab before referring to the table below.\",\" The Equivalent Full Load Hours of Operation is used to calculate the DHW modeled peak residential flow a the DHW Heater that must be modeled to be consistent with the annual hot water consumption calculated here.\",\" After confirming the Equivalent Full Load Hours of Operation in the schedules tab,\",\"Identify the residential service water heating usage profile, and the weighted average fixture flows for sink and shower fixtures. Supply temperature at fixture point of use shall be \",IF(SI_IP_Units=\"IP\",\"120 degrees F\",\"49 degrees C\"),\". If the modeled supply DHW temperature from the DHW heater is higher than this,\",\" indicate the supply DHW temperature from the DHW heater and the average cold water input temperature below.\",\"\n\nThis information along with the appliance information entered above and the schedule data from the schedules tab is used to determine the DHW modeled Peak Flow at DHW heater,\",\"which should be input into the energy model.\")","v":"Report the modeled Service Water Heating Full Load Hours of Operation in the Schedules tab before referring to the table below. The Equivalent Full Load Hours of Operation is used to calculate the DHW modeled peak residential flow a the DHW Heater that must be modeled to be consistent with the annual hot water consumption calculated here. After confirming the Equivalent Full Load Hours of Operation in the schedules tab,Identify the residential service water heating usage profile, and the weighted average fixture flows for sink and shower fixtures. Supply temperature at fixture point of use shall be 120 degrees F. If the modeled supply DHW temperature from the DHW heater is higher than this, indicate the supply DHW temperature from the DHW heater and the average cold water input temperature below.\n\nThis information along with the appliance information entered above and the schedule data from the schedules tab is used to determine the DHW modeled Peak Flow at DHW heater,which should be input into the energy model."}]
["G"]
["G","Building ID","Residential Usage Profile",{"$f":"CONCATENATE(\"Average Fixture Flows \",IF(SI_IP_Units=\"IP\",\"(gallons/minute)\",\"(Liters/second)\"))","v":"Average Fixture Flows (gallons/minute)"},null,null,null,{"$f":"CONCATENATE(\"DHW Temperature Settings \",IF(SI_IP_Units=\"IP\",\"(degrees F)\",\"(degrees C)\"))","v":"DHW Temperature Settings (degrees F)"},null,null,{"$f":"CONCATENATE(\"DHW Sink and Shower Fixture Loads at Point of Use\",IF(SI_IP_Units=\"IP\",\" (gallons / year)\", \"(Liters / year)\"))","v":"DHW Sink and Shower Fixture Loads at Point of Use (gallons / year)"},null,{"$f":"CONCATENATE(\"DHW In-Unit Appliance Loads at Point of Use\",IF(SI_IP_Units=\"IP\",\" (gallons / year)\", \"(Liters / year)\"))","v":"DHW In-Unit Appliance Loads at Point of Use (gallons / year)"},null,{"$f":"CONCATENATE(\"DHW Laundry Room Equipment Loads at Point of Use\",IF(SI_IP_Units=\"IP\",\" (gallons / year)\", \"(Liters / year)\"))","v":"DHW Laundry Room Equipment Loads at Point of Use (gallons / year)"},null,{"$f":"CONCATENATE(\"DHW Total Residential Loads at Point of Use\",IF(SI_IP_Units=\"IP\",\" (gallons / year)\", \"(Liters / year)\"))","v":"DHW Total Residential Loads at Point of Use (gallons / year)"},null,{"$f":"CONCATENATE(\"DHW Total Residential Loads at DHW Heater\",IF(SI_IP_Units=\"IP\",\" (gallons / year)\", \"(Liters / year)\"))","v":"DHW Total Residential Loads at DHW Heater (gallons / year)"},null,"DHW Equivalent Full Load Hours of Operation",{"$f":"CONCATENATE(\"DHW Modeled Peak Residential Flow at DHW Heater\",IF(SI_IP_Units=\"IP\",\" (gallons / minute)\", \"(Liters / second)\"))","v":"DHW Modeled Peak Residential Flow at DHW Heater (gallons / minute)"},null,"Measure #"]
["G",null,null,"Baseline",null,"Proposed",null,"DHW Supply Temp","Average Cold Water Temp","DHW Temp at Fixture Point of Use"]
["G",null,null,"Showers","Sinks","Showers","Sinks",null,null,null,"Baseline","Proposed","Baseline","Proposed","Baseline","Proposed","Baseline","Proposed","Baseline","Proposed",null,"Baseline","Proposed"]
["G","Building ID","Res_Usage_Profile","Shower_Flow_Avg","Sink_Flow_Avg","Shower_Flow_Avg","Sink_Flow_Avg","DHW_Supply_Temp","DHW_Cold_Water_Temp","DHW_Fixture_Temp","DHW_Base_Fixture_flow","DHW_Design_Fixture_flow","DHW_Base_Appliance_Flow","DHW_Design_Appliance_Flow","DHW_Base_Laundry_Flow","DHW_Proposed_Laundry_Flow","DHW_Base_Total_Flow","DHW_Design_Total_Flow","DHW_Heater_Base_Flow","DHW_Heater_Design_Flow","DHW_EFLH","DHW_Base_Modeled_Flowrate","DHW_Design_Modeled_Flowrate"]
["G",{"$f":"'1 - Multiple Buildings Details'!B24","v":0},null,{"$f":"IF('General Information'!F11=\"IP Units\",2.5,0.16)","v":2.5},{"$f":"IF('General Information'!F11=\"IP Units\",2.5,0.14)","v":2.5},null,null,null,null,{"$f":"IF(SI_IP_Units=\"IP\",120,CONVERT(120,\"F\",\"C\"))","v":120},{"$f":"IFERROR(VLOOKUP($C91,Res_Usage_Profile_Table,18,FALSE)*365*INDEX(MD_BUS_SumTable,MATCH($B91,MD_BUS_SumIndex,0),MATCH($F$21,MD_BUS_SumHdr,0)),\"N/A\")","v":"N/A"},{"$f":"IF(ISERROR(1/$F91/$G91),$K91,IFERROR($K91*IF(SI_IP_Units=\"IP\",(0.36+0.54*$F91/D91+0.1*$G91/E91),(0.36+0.54*$F91/D91+0.1*$G91/E91)),$K91))","v":"N/A"},{"$f":"IFERROR(SUMIF(MD_HDUEC_Index1,$B91,OFFSET(MD_HDUEC_Index1,0,MATCH($T$31,MD_HDUEC_Hdr,0)-1,ROWS(MD_HDUEC_Index1),1)),\"N/A\")","v":0},{"$f":"IFERROR(SUMIF(MD_HDUEC_Index1,$B91,OFFSET(MD_HDUEC_Index1,0,MATCH($U$31,MD_HDUEC_Hdr,0)-1,ROWS(MD_HDUEC_Index1),1)),\"N/A\")","v":0},{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B91,OFFSET(MD_Laundry_Index,0,MATCH($T$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)),\"N/A\")","v":0},{"$f":"IFERROR(SUMIF(MD_Laundry_Index,$B91,OFFSET(MD_Laundry_Index,0,MATCH($U$57,MD_Laundry_Hdr,0)-1,ROWS(MD_Laundry_Index),1)),\"N/A\")","v":0},{"$f":"IFERROR(SUM(K91,M91,O91),0)","v":0},{"$f":"IFERROR(SUM(L91,N91,P91),0)","v":0},{"$f":"IFERROR(IF(ISERROR(1/$I91),Q91,($J91-$I91)/($H91-$I91)*Q91),Q91)","v":0},{"$f":"IFERROR(IF(ISERROR(1/$I91),R91,($J91-$I91)/($H91-$I91)*R91),R91)","v":0},{"$f":"'2a - Schedules'!$E$12","v":2628},{"$f":"IFERROR(IF(SI_IP_Units=\"IP\",S91/$U91/60,S91/$U91/60/60),\"N/A\")","v":0},{"$f":"IFERROR(IF(SI_IP_Units=\"IP\",T91/$U91/60,T91/$U91/60/60),\"N/A\")","v":0}]
["G","Note:  Flow rates are based on Energy Star Multifamily Simulation Guidance. One person is assumed per bedroom."]
[]
[]
[null,"Table 3.7: Ventilation in Dwelling Units"]
[]
[null,"Enter values in the grey editable cells to populate the ventilation in dwelling units per ASHRAE 62.2-2013."]
[]
[null,null,null,"Studio",null,"1 Bedroom",null,"2 Bedrooms",null,"3 Bedrooms",null,"4 Bedrooms",null,"5 Bedrooms",null,"6 Bedrooms",null,"7 Bedrooms",null,"8 Bedrooms"]
[null,null,null,"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"},"Qty",{"$f":"CONCATENATE(\"Average Floor Area\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Average Floor Area (sq ft)"}]
[null,null,null,{"$f":"IF(D12=\"\",\"-\",D12)","v":"-"},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Local Exhaust"]
[null,"Kitchen Area (sf)"]
[null,"Kitchen Ceiling Height (ft)"]
[null,"Continuous CFM equivalent to 5ACH (62.2-2013):",null,{"$f":"ROUNDUP(5*D103*D104/60,0)","v":0},null,0,null,{"$f":"ROUNDUP(5*H103*H104/60,0)","v":0},null,{"$f":"ROUNDUP(5*J103*J104/60,0)","v":0},null,{"$f":"ROUNDUP(5*L103*L104/60,0)","v":0},null,{"$f":"ROUNDUP(5*N103*N104/60,0)","v":0},null,{"$f":"ROUNDUP(5*P103*P104/60,0)","v":0},null,{"$f":"ROUNDUP(5*R103*R104/60,0)","v":0},null,{"$f":"ROUNDUP(5*T103*T104/60,0)","v":0}]
[null,"Intermittent or Continuous?","Kitchen"]
[null,null,"Bathroom"]
[null,{"$f":"\"ASHRAE 62.2-2013 Requirements: \"&D106&\n\" Baseline Exhaust Ventilation\"","v":"ASHRAE 62.2-2013 Requirements:  Baseline Exhaust Ventilation"},"Kitchen (CFM, each)",null,null,{"$f":"IF(F106=\"Continuous\",F105,IF(F106=\"Intermittent\",100,\"-\"))","v":"-"},null,{"$f":"IF(H106=\"Continuous\",H105,IF(H106=\"Intermittent\",100,\"-\"))","v":"-"},null,{"$f":"IF(J106=\"Continuous\",J105,IF(J106=\"Intermittent\",100,\"-\"))","v":"-"},null,{"$f":"IF(L106=\"Continuous\",L105,IF(L106=\"Intermittent\",100,\"-\"))","v":"-"},null,{"$f":"IF(N106=\"Continuous\",N105,IF(N106=\"Intermittent\",100,\"-\"))","v":"-"},null,{"$f":"IF(P106=\"Continuous\",P105,IF(P106=\"Intermittent\",100,\"-\"))","v":"-"},null,{"$f":"IF(R106=\"Continuous\",R105,IF(R106=\"Intermittent\",100,\"-\"))","v":"-"},null,{"$f":"IF(T106=\"Continuous\",T105,IF(T106=\"Intermittent\",100,\"-\"))","v":"-"}]
[null,null,"Bathroom (CFM, each)",null,null,{"$f":"IF(F107=\"Continuous\",20,IF(F107=\"Intermittent\",50,\"-\"))","v":"-"},null,{"$f":"IF(H107=\"Continuous\",20,IF(H107=\"Intermittent\",50,\"-\"))","v":"-"},null,{"$f":"IF(J107=\"Continuous\",20,IF(J107=\"Intermittent\",50,\"-\"))","v":"-"},null,{"$f":"IF(L107=\"Continuous\",20,IF(L107=\"Intermittent\",50,\"-\"))","v":"-"},null,{"$f":"IF(N107=\"Continuous\",20,IF(N107=\"Intermittent\",50,\"-\"))","v":"-"},null,{"$f":"IF(P107=\"Continuous\",20,IF(P107=\"Intermittent\",50,\"-\"))","v":"-"},null,{"$f":"IF(R107=\"Continuous\",20,IF(R107=\"Intermittent\",50,\"-\"))","v":"-"},null,{"$f":"IF(T107=\"Continuous\",20,IF(T107=\"Intermittent\",50,\"-\"))","v":"-"}]
[null,"Proposed Design Fan Type","Kitchen"]
[null,null,"Bathroom"]
[null,"Proposed Design CFM per Apartment","Kitchen (CFM)"]
[null,null,"Bathroom (CFM)"]
[null,"Proposed Design CFM Total","Kitchen (CFM)",{"$f":"IFERROR(D112*D101,\"-\")","v":"-"},null,{"$f":"IFERROR(F112*F101,\"-\")","v":"-"},null,{"$f":"IFERROR(H112*H101,\"-\")","v":"-"},null,{"$f":"IFERROR(J112*J101,\"-\")","v":"-"},null,{"$f":"IFERROR(L112*L101,\"-\")","v":"-"},null,{"$f":"IFERROR(N112*N101,\"-\")","v":"-"},null,{"$f":"IFERROR(P112*P101,\"-\")","v":"-"},null,{"$f":"IFERROR(R112*R101,\"-\")","v":"-"},null,{"$f":"IFERROR(T112*T101,\"-\")","v":"-"}]
[null,null,"Bathroom (CFM)",{"$f":"IFERROR(D113*D101,\"-\")","v":"-"},null,{"$f":"IFERROR(F113*F101,\"-\")","v":"-"},null,{"$f":"IFERROR(H113*H101,\"-\")","v":"-"},null,{"$f":"IFERROR(J113*J101,\"-\")","v":"-"},null,{"$f":"IFERROR(L113*L101,\"-\")","v":"-"},null,{"$f":"IFERROR(N113*N101,\"-\")","v":"-"},null,{"$f":"IFERROR(P113*P101,\"-\")","v":"-"},null,{"$f":"IFERROR(R113*R101,\"-\")","v":"-"},null,{"$f":"IFERROR(T113*T101,\"-\")","v":"-"}]
[null,"Baseline CFM per Apartment (Minimum of ASHRAE 62.2-2013 or Proposed Value)","Per Kitchen (CFM)",{"$f":"IFERROR(IF(D112<D108,D112,D108),\"-\")","v":0},null,{"$f":"IFERROR(IF(F112<F108,F112,F108),\"-\")","v":0},null,{"$f":"IFERROR(IF(H112<H108,H112,H108),\"-\")","v":0},null,{"$f":"IFERROR(IF(J112<J108,J112,J108),\"-\")","v":0},null,{"$f":"IFERROR(IF(L112<L108,L112,L108),\"-\")","v":0},null,{"$f":"IFERROR(IF(N112<N108,N112,N108),\"-\")","v":0},null,{"$f":"IFERROR(IF(P112<P108,P112,P108),\"-\")","v":0},null,{"$f":"IFERROR(IF(R112<R108,R112,R108),\"-\")","v":0},null,{"$f":"IFERROR(IF(T112<T108,T112,T108),\"-\")","v":0}]
[null,null,"Per Bathroom (CFM)",{"$f":"IFERROR(IF(D113<D109,D113,D109),\"-\")","v":0},null,{"$f":"IFERROR(IF(F113<F109,F113,F109),\"-\")","v":0},null,{"$f":"IFERROR(IF(H113<H109,H113,H109),\"-\")","v":0},null,{"$f":"IFERROR(IF(J113<J109,J113,J109),\"-\")","v":0},null,{"$f":"IFERROR(IF(L113<L109,L113,L109),\"-\")","v":0},null,{"$f":"IFERROR(IF(N113<N109,N113,N109),\"-\")","v":0},null,{"$f":"IFERROR(IF(P113<P109,P113,P109),\"-\")","v":0},null,{"$f":"IFERROR(IF(R113<R109,R113,R109),\"-\")","v":0},null,{"$f":"IFERROR(IF(T113<T109,T113,T109),\"-\")","v":0}]
[null,"Baseline CFM Total","Kitchen (CFM)",{"$f":"IFERROR(D116*D101,\"-\")","v":"-"},null,{"$f":"IFERROR(F116*F101,\"-\")","v":"-"},null,{"$f":"IFERROR(H116*H101,\"-\")","v":"-"},null,{"$f":"IFERROR(J116*J101,\"-\")","v":"-"},null,{"$f":"IFERROR(L116*L101,\"-\")","v":"-"},null,{"$f":"IFERROR(N116*N101,\"-\")","v":"-"},null,{"$f":"IFERROR(P116*P101,\"-\")","v":"-"},null,{"$f":"IFERROR(R116*R101,\"-\")","v":"-"},null,{"$f":"IFERROR(T116*T101,\"-\")","v":"-"}]
[null,null,"Bathroom (CFM) \n(Assuming 1 Bathroom)",{"$f":"IFERROR(D117*D101,\"-\")","v":"-"},null,{"$f":"IFERROR(F117*F101,\"-\")","v":"-"},null,{"$f":"IFERROR(H117*H101,\"-\")","v":"-"},null,{"$f":"IFERROR(J117*J101,\"-\")","v":"-"},null,{"$f":"IFERROR(L117*L101,\"-\")","v":"-"},null,{"$f":"IFERROR(N117*N101,\"-\")","v":"-"},null,{"$f":"IFERROR(P117*P101,\"-\")","v":"-"},null,{"$f":"IFERROR(R117*R101,\"-\")","v":"-"},null,{"$f":"IFERROR(T117*T101,\"-\")","v":"-"}]
[null,"Whole Unit Ventilation"]
[null,"OA Supply Method"]
[null,"For non-mechanical OA supply method, does the intermittent exhaust run on a timer per 62.2-2013?"]
[null,"Proposed Design Mechanical OA Supply CFM per Apartment",null,{"$f":"IF(OR(D121=\"Trickle Vent\",D121=\"Natural Ventilation\"),\"N/A\",\"\")","v":""},null,"",null,{"$f":"IF(OR(H121=\"Trickle Vent\",H121=\"Natural Ventilation\"),\"N/A\",\"\")","v":""},null,{"$f":"IF(OR(J121=\"Trickle Vent\",J121=\"Natural Ventilation\"),\"N/A\",\"\")","v":""},null,{"$f":"IF(OR(L121=\"Trickle Vent\",L121=\"Natural Ventilation\"),\"N/A\",\"\")","v":""},null,{"$f":"IF(OR(N121=\"Trickle Vent\",N121=\"Natural Ventilation\"),\"N/A\",\"\")","v":""},null,{"$f":"IF(OR(P121=\"Trickle Vent\",P121=\"Natural Ventilation\"),\"N/A\",\"\")","v":""},null,{"$f":"IF(OR(R121=\"Trickle Vent\",R121=\"Natural Ventilation\"),\"N/A\",\"\")","v":""},null,{"$f":"IF(OR(T121=\"Trickle Vent\",T121=\"Natural Ventilation\"),\"N/A\",\"\")","v":""}]
[null,"Proposed Design Mechanical OA Supply CFM Total",null,{"$f":"IFERROR(D123*D101,\"\")","v":""},null,{"$f":"IFERROR(F123*F101,\"\")","v":""},null,{"$f":"IFERROR(H123*H101,\"\")","v":""},null,{"$f":"IFERROR(J123*J101,\"\")","v":""},null,{"$f":"IFERROR(L123*L101,\"\")","v":""},null,{"$f":"IFERROR(N123*N101,\"\")","v":""},null,{"$f":"IFERROR(P123*P101,\"\")","v":""},null,{"$f":"IFERROR(R123*R101,\"\")","v":""},null,{"$f":"IFERROR(T123*T101,\"\")","v":""}]
[null,"Baseline CFM per Apartment  (Minimum of ASHRAE 62.2-2013 or Proposed Value)",null,{"$f":"IFERROR(IF(D123=\"N/A\",0,MIN(D123,(0.03*E101+7.5*(1)))),\"-\")","v":"-"},null,{"$f":"IFERROR(IF(F123=\"N/A\",0,MIN(F123,(0.03*G101+7.5*(2)))),\"-\")","v":"-"},null,{"$f":"IFERROR(IF(H123=\"N/A\",0,MIN(H123,(0.03*I101+7.5*(3)))),\"-\")","v":"-"},null,{"$f":"IFERROR(IF(J123=\"N/A\",0,MIN(J123,(0.03*K101+7.5*(4)))),\"-\")","v":"-"},null,{"$f":"IFERROR(IF(L123=\"N/A\",0,MIN(L123,(0.03*M101+7.5*(5)))),\"-\")","v":"-"},null,{"$f":"IFERROR(IF(N123=\"N/A\",0,MIN(N123,(0.03*O101+7.5*(6)))),\"-\")","v":"-"},null,{"$f":"IFERROR(IF(P123=\"N/A\",0,MIN(P123,(0.03*Q101+7.5*(7)))),\"-\")","v":"-"},null,{"$f":"IFERROR(IF(R123=\"N/A\",0,MIN(R123,(0.03*S101+7.5*(8)))),\"-\")","v":"-"},null,{"$f":"IFERROR(IF(T123=\"N/A\",0,MIN(T123,(0.03*U101+7.5*(9)))),\"-\")","v":"-"}]
[null,"Baseline CFM Total (per 62.2-2013)",null,{"$f":"IFERROR(D101*D125,\"-\")","v":"-"},null,{"$f":"IFERROR(F101*F125,\"-\")","v":"-"},null,{"$f":"IFERROR(H101*H125,\"-\")","v":"-"},null,{"$f":"IFERROR(J101*J125,\"-\")","v":"-"},null,{"$f":"IFERROR(L101*L125,\"-\")","v":"-"},null,{"$f":"IFERROR(N101*N125,\"-\")","v":"-"},null,{"$f":"IFERROR(P101*P125,\"-\")","v":"-"},null,{"$f":"IFERROR(R101*R125,\"-\")","v":"-"},null,{"$f":"IFERROR(T101*T125,\"-\")","v":"-"}]
[null,null,null,{"$f":"IF(AND(D129=1,D130>0),\"Warning: Proposed Design mechanical OA supply CFM is noted for a non-mechanical system.\",\"\")","v":""},null,{"$f":"IF(AND(F129=1,F130>0),\"Warning: Proposed Design mechanical OA supply CFM is noted for a non-mechanical system.\",\"\")","v":""},null,{"$f":"IF(AND(H129=1,H130>0),\"Warning: Proposed Design mechanical OA supply CFM is noted for a non-mechanical system.\",\"\")","v":""},null,{"$f":"IF(AND(J129=1,J130>0),\"Warning: Proposed Design mechanical OA supply CFM is noted for a non-mechanical system.\",\"\")","v":""},null,{"$f":"IF(AND(L129=1,L130>0),\"Warning: Proposed Design mechanical OA supply CFM is noted for a non-mechanical system.\",\"\")","v":""},null,{"$f":"IF(AND(N129=1,N130>0),\"Warning: Proposed Design mechanical OA supply CFM is noted for a non-mechanical system.\",\"\")","v":""},null,{"$f":"IF(AND(P129=1,P130>0),\"Warning: Proposed Design mechanical OA supply CFM is noted for a non-mechanical system.\",\"\")","v":""},null,{"$f":"IF(AND(R129=1,R130>0),\"Warning: Proposed Design mechanical OA supply CFM is noted for a non-mechanical system.\",\"\")","v":""},null,{"$f":"IF(AND(T129=1,T130>0),\"Warning: Proposed Design mechanical OA supply CFM is noted for a non-mechanical system.\",\"\")","v":""}]
[]
[null,null,null,{"$f":"IF(OR(D121=\"Trickle Vent\",D121=\"Natural Ventilation\"),1,0)","v":0},{"$f":"IF(OR(E121=\"Trickle Vent\",E121=\"Natural Ventilation\"),1,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,{"$f":"IF(D123=\"N/A\",0,D123)","v":""},{"$f":"IF(E123=\"N/A\",0,E123)","v":0},"",0,"",0,"",0,"",0,"",0,"",0,"",0,"",0]

{"sheet":"4 - Shading and Fenestration","index":8,"n_rows":93,"n_cols":34,"rows_kept":93,"cut":false,"hidden":false,"merged":[[16,1,16,10],[11,1,11,10],[12,1,12,10],[13,1,13,10],[14,1,14,10],[34,1,34,2],[35,1,35,2],[36,1,36,2],[63,1,63,3],[63,5,63,7],[55,1,55,11],[31,6,31,7],[31,8,32,8],[31,9,31,10],[54,1,54,10],[56,1,56,9],[44,6,44,7],[44,8,45,8],[33,1,33,2],[29,1,32,2],[29,3,32,3],[49,1,49,6],[49,7,49,11],[22,1,22,11],[84,1,84,11],[47,1,48,3],[5,1,5,9],[29,5,29,7],[29,8,29,10],[6,1,6,10],[8,1,8,10],[9,1,9,10],[19,1,19,11],[20,1,20,11],[44,9,44,10],[31,5,32,5],[80,1,80,6],[72,5,72,7],[80,7,80,11],[7,1,7,10],[10,1,10,10],[44,1,46,3],[44,5,45,5],[30,8,30,10],[17,1,17,6],[17,7,17,11],[30,5,30,7],[15,1,15,10],[66,26,66,27],[65,26,65,27],[74,26,74,27],[74,5,74,7],[75,26,75,27],[66,24,66,25],[75,24,75,25],[67,24,67,25],[68,24,68,25],[67,26,67,27],[68,26,68,27],[65,5,65,7],[72,17,74,17],[63,17,65,17],[73,8,73,9],[63,16,64,16],[72,16,73,16],[35,12,35,13],[36,12,36,13],[37,12,37,13],[38,12,38,13],[61,1,61,10],[51,1,51,2],[52,1,52,2],[50,1,50,11],[51,4,51,11],[52,4,52,11],[39,1,39,2],[39,12,39,13],[43,1,43,3],[42,1,42,2],[42,12,42,13],[43,12,43,13],[37,1,37,2],[38,1,38,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[77,8,77,9],[74,8,74,14],[41,1,41,2],[40,1,40,2],[40,12,40,13],[76,8,76,9],[65,8,65,14],[63,8,63,14],[72,8,72,14],[72,1,72,3],[64,1,65,1],[64,2,65,2],[64,3,65,3],[73,1,74,1],[73,2,74,2],[73,3,74,3],[33,12,33,13],[34,12,34,13],[29,12,32,13],[41,12,41,13]]}
["G"]
["G","Shading and Fenestration"]
["G"]
["G"]
["G","Building Massing and Zoning"]
["G","Instructions: Provide the following shading and orientation information. An example of the expected level of detail has been provided for each input. For any information not applicable to the project, simply enter \"N/A\".",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional)"]
[null,"Modeled baseline vertical fenestration areas for new buildings and additions reflects Window to Wall (WWR) ratio in Table G3.1.1-1 based on the area of gross above-grade walls that separate conditioned spaces and semiheated spaces from the exterior. For building areas not shown in Table G3.1.1-1, vertical fenestration areas is equal that in the proposed design or 40% of gross above-grade wall area, whichever is smaller."]
[null,"Modeled baseline vertical fenestration is distributed on each face of the building in the same proportion as in the proposed design."]
[null,"Modeled baseline fenestration area for an existing building is equal the existing fenestration area prior to the proposed work and distributed on each face of the building in the same proportions as the existing building."]
[null,"Modeled baseline skylight area is equal to that in the proposed design or 3%, whichever is smaller. Skylight orientation and tilt is the same as in the proposed design."]
[null,"Shading by adjacent structures and terrain was modeled the same in the baseline and proposed design models. All elements whose effective height is greater than their distance from a proposed building and whose width facing the proposed building is greater than one-third that of the proposed building were accounted for in both simulations. "]
[null,{"$f":"IF('General Information'!E9=\"ENERGY STAR MFHR\",\"For ENERGY STAR MFHR projects, manual shading such as blinds or shades have not been modeled in either the baseline or proposed design.\",\"Manual fenestration shading devices such as blinds or shades have been modeled or not modeled, the same in the baseline and proposed design.\")","v":"For ENERGY STAR MFHR projects, manual shading such as blinds or shades have not been modeled in either the baseline or proposed design."}]
[null,"Automatically controlled fenestration shades or blinds have been modeled in the proposed design but not in the baseline."]
[null,"Permanent shading devices such as fins, overhangs, and light shelves were modeled in the proposed design but not in the baseline."]
[null,"The baseline is modeled as an average of four orientations."]
[null,"All baseline fenestration for new buildings, existing buildings, and additions was modeled with assembly U-factor and SHGC from Tables G3.4-1 through G3.4-8."]
[null,"Thermal Blocks were modeled consistent with Table G3.1#7 and Table G3.1#8 as applicable, and were modeled identically in the Baseline and Proposed design models."]
[null,"All proposed fenestration was modeled based on the assembly U-factor and SHGC determined using the following method: (If more than one method used, list additional methods in the Note, and describe and fenestration products to which it was applied.)"]
[]
[null,"For each item entered as “No” above, describe the applicable ASHRAE 90.1 Appendix G exception(s) that apply, or the circumstances preventing the building massing modeling parameters from being modeled as required. If the energy simulation software is not capable of modeling the required parameters, describe the adjustments that were made to provide a thermodynamically similar representation or provide a narrative justifying why the predicted energy performance results will not be influenced."]
[]
[]
[null,"Please select the Building Area Types which will be used in the below Table 4.1, based on ASHRAE 90.1-2016 Appendix G Table G3.1.1-1."]
[]
[]
[]
[]
[]
[null,"Table 4.1: Envelope Area Summary"]
[null,"Building Area Type",null,"Orientation",null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,"Proposed Design",null,null,null,"Measure #"]
[null,null,null,null,null,"Helpful Hints\n•  All vertical glazing flush with exterior wall and no shading projections per Table G3.1#5(d)\n•  Manual shading devices such as blinds or shades may be modeled per Table G3.1#5(d)\n•  No self-shading per Table G3.1#5\n•  Total vertical fenestration areas for new construction and additions shall equal that in Table G3.1.1-1 based on gross above-grade exterior wall area. For buildings areas not shown in Table G3.1.1-1, vertical fenestration shall equal that in the proposed design or the maximum allowed in Tables G3.4-1 through G3.4-8 for the applicable glazing percentage for U-fixed, whichever is smaller, per Table G3.1#5(c)\n•  Total vertical fenestration areas for existing construction shall equal the existing fenestration area prior to the proposed work and shall be distributed on each face of the building in the same proportions as the existing building per Table G3.1#5(c)",null,null,"Helpful Hints\n•  Manual shading devices such as blinds or shades may be modeled and must be consistent with the baseline per Table G3.1#5(4)\n•  Permanent shading devices (such as fins, overhangs, and light shelves) and automatically controlled shades or blinds must be modeled per Table G3.1#5(4)"]
[null,null,null,null,null,{"$f":"CONCATENATE(\"Gross Above-Grade Wall Area\n\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Gross Above-Grade Wall Area\n (sq ft)"},"Vertical Glazing Area",null,{"$f":"CONCATENATE(\"Gross Above-Grade Wall Area\n\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Gross Above-Grade Wall Area\n (sq ft)"},"Vertical Glazing Area"]
[null,null,null,null,null,null,{"$f":"IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\")","v":" (sq ft)"},"(%)",null,{"$f":"IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\")","v":" (sq ft)"},"(%)"]
[null,null,null,"North",null,"Identical to Proposed",{"$f":"IFERROR(J34/(SUMIF($B$40:$C$43,B34,$J$40:$J$43))*(SUMIF($B$40:$C$43,B34,$G$40:$G$43)),\"-\")","v":"-"},{"$f":"IFERROR(G34/I34,\"\")","v":""},null,null,{"$f":"IFERROR(J34/I34,\"\")","v":""}]
[null,null,null,"East",null,{"$f":"$F$34","v":"Identical to Proposed"},"-",{"$f":"IFERROR(G35/I35,\"\")","v":""},null,null,{"$f":"IFERROR(J35/I35,\"\")","v":""}]
[null,null,null,"South",null,{"$f":"$F$34","v":"Identical to Proposed"},"-","",null,null,""]
[null,null,null,"West",null,"Identical to Proposed","-","",null,null,""]
["D",null,null,null,null,"Identical to Proposed","-","",null,null,""]
[null,null,null,null,null,"Identical to Proposed","-","",null,null,""]
[null,{"$f":"IF(B24=\"\",\"-\",B24)","v":"-"},null,"Total",null,{"$f":"I40","v":0},{"$f":"F40*H40","v":0},{"$f":"MIN(SUMIF(BuildingAreaType,'4 - Shading and Fenestration'!B40,'Envelope Assumptions'!$CJ$3:$CJ$18),K40)","v":0},{"$f":"SUMIF($B$34:$C$39,B40,$I$34:$I$39)","v":0},{"$f":"SUMIF($B$34:$C$39,B40,$J$34:$J$39)","v":0},{"$f":"IFERROR(J40/I40,0)","v":0}]
[null,{"$f":"IF(B25=\"\",\"-\",B25)","v":"-"},null,"Total",null,{"$f":"I41","v":0},{"$f":"F41*H41","v":0},{"$f":"MIN(SUMIF(BuildingAreaType,'4 - Shading and Fenestration'!B41,'Envelope Assumptions'!$CJ$3:$CJ$18),K41)","v":0},{"$f":"SUMIF($B$34:$C$39,B41,$I$34:$I$39)","v":0},{"$f":"SUMIF($B$34:$C$39,B41,$J$34:$J$39)","v":0},{"$f":"IFERROR(J41/I41,0)","v":0}]
[null,"-",null,"Total",null,{"$f":"I42","v":0},{"$f":"F42*H42","v":0},{"$f":"MIN(SUMIF(BuildingAreaType,'4 - Shading and Fenestration'!B42,'Envelope Assumptions'!$CJ$3:$CJ$18),K42)","v":0},{"$f":"SUMIF($B$34:$C$39,B42,$I$34:$I$39)","v":0},{"$f":"SUMIF($B$34:$C$39,B42,$J$34:$J$39)","v":0},{"$f":"IFERROR(J42/I42,0)","v":0}]
[null,"-",null,"Total",null,{"$f":"I43","v":0},{"$f":"F43*H43","v":0},{"$f":"MIN(SUMIF(BuildingAreaType,'4 - Shading and Fenestration'!B43,'Envelope Assumptions'!$CJ$3:$CJ$18),K43)","v":0},{"$f":"SUMIF($B$34:$C$39,B43,$I$34:$I$39)","v":0},{"$f":"SUMIF($B$34:$C$39,B43,$J$34:$J$39)","v":0},{"$f":"IFERROR(J43/I43,0)","v":0}]
[null,"Building Total",null,null,null,{"$f":"SUM(F40:F43)","v":0},{"$f":"SUM(G40:G43)","v":0},{"$f":"IFERROR(G44/F44,\"-\")","v":"-"},{"$f":"SUM(I40:I43)","v":0},{"$f":"SUM(J40:J43)","v":0},{"$f":"IFERROR(J44/I44,\"-\")","v":"-"}]
[null,"Roof and skylight area",null,null,null,{"$f":"CONCATENATE(\"Roof Area\n\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Roof Area\n (sq ft)"},"Skylight Area",null,{"$f":"CONCATENATE(\"Roof Area\n\",IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\"))","v":"Roof Area\n (sq ft)"},"Skylight Area"]
[null,null,null,null,null,null,{"$f":"IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\")","v":" (sq ft)"},"(%)",null,{"$f":"IF(SI_IP_Units=\"IP\",\" (sq ft)\",\" (sq m)\")","v":" (sq ft)"},"(%)"]
[null,null,null,null,null,"Identical to Proposed",{"$f":"IF(J47=\"\",\"-\",(MIN(J47,(0.05*I47))))","v":"-"},{"$f":"IFERROR(G47/I47,\"-\")","v":"-"},null,null,{"$f":"IFERROR(J47/F47,0)","v":0}]
["G","Number of Thermal Blocks",null,null,null,"Conditioned","Semi-heated","Unconditioned","Conditioned","Semi-heated","Unconditioned"]
["G",null,null,null,null,"Identical to Proposed","Identical to Proposed","Identical to Proposed",null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(INDEX(MBD_BS_Table,MATCH(OFFSET(S49,-14,-11,1,1),MBD_BS_Index,0),MATCH('1 - Multiple Buildings Details'!$E$22,MBD_BS_Hdr,0)),\" zones\")","v":{"$error":"#N/A"}},{"$f":"SUM(IFERROR(VALUE(IF(ISNUMBER(F49:H49),F49:H49,IFERROR(LEFT(F49:H49,IFERROR(FIND(\"to\",F49:H49)-1,\"\")),\"\"))),\"\"))+SUM(IFERROR(FIND(\">100\",F49:H49)*100,\"\"))","v":0}]
[]
[null,{"$f":"\"Baseline Vertical Glazing\"&\"-\"&'General Information'!$C$42","v":"Baseline Vertical Glazing-ASHRAE 90.1 2016 Appendix G"}]
[null,"Baseline Vertical Glazing % calculated from table above",null,"Modeled Baseline Vertical Glazing % ","If the baseline vertical glazing percentage does not match the Vertical Glazing % per G3.1#5(c) and Table G3.1.1-1, \nplease provide an explanation in the space below."]
[null,{"$f":"IFERROR($H$44,\"-\")","v":"-"}]
[]
["G","Reason for exemption from modeling the additional building orientations."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Total",{"$f":"MAX(T47:T55)","v":0},{"$f":"IF(COUNTIF(U47:U55,TRUE)>0,TRUE,FALSE)","v":false}]
[null,{"$f":"IF(IFERROR(FIND(\"*\",B56),FALSE),\"* Please ensure that the site plan provided for the Project Information forms clearly indicate the constraints to comply with Table G3.1.5 (a) (baseline) Exception 1\",\"\")","v":""}]
[]
[]
[]
["G","Fenestration"]
["G","Instructions: Describe each unique fenestration assembly on a separate row in the following table. Please refer to the column header notes for information about Appendix G modeling protocol. For any information not applicable to the project, simply enter \"N/A\". Baseline information will autogenerate for new construction."]
["G","Table 4.2: Vertical Glazing"]
["G","General Information",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,"Proposed Design",null,null,null,null,null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
["G","Building ID","New or \nExisting Construction","Space-Conditioning Category",null,"Description","Assembly U-factor","SHGC","Type","Description","Assembly \nU-factor","SHGC","VLT","Area (sf)","Plans / Specs"]
["G",null,null,null,null,"Helpful Hints\n• New/Existing vertical glazing: \n     • Select a description\n     • Assembly U-factor and SHGC from  Table G3.4-1 through G3.4-8 per Table G3.1#5(d). \n     • (SHGC). Please note that this is not equivalent to the shading coefficient (SC).\n\n",null,null,"Helpful Hints\n• Proposed vertical glazing assembly U-factor should be as-designed and account for the impact of the frames on the whole assembly. Reference Table A8.2 of ASHRAE 90.1 as necessary.\n• Describe the Proposed vertical glazing assembly (for example: double glazing, argon filled, low-e coating, aluminum frame with thermal break)\n• Enter the Proposed vertical glazing assembly solar heat gain coefficient (SHGC). Please note that this is not equivalent to the shading coefficient (SC).\n• Enter the Proposed vertical glazing assembly visual light transmittance (VLT)\n• If the Proposed design includes building envelope assemblies of different U-values, please specify surface area, square feet, for each envelope assembly.\n•Reference specific place in the submitted design documents (e.g. drawing & detail number) where relevant parameters are listed to support review.",null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2013,\"In accordance with Prescriptive Requirements of 90.1-2013 \"&INDEX(DropdownData!AW2:AW19,MATCH('General Information'!C46,AshraeClimate,0)),\"In accordance with Prescriptive Requirements of 90.1-2010 \"&INDEX(DropdownData!AX2:AX19,MATCH('General Information'!C46,AshraeClimate,0)))","v":"In accordance with Prescriptive Requirements of 90.1-2013 Table 5.5-4"}]
["G",{"$f":"B65","v":"Building ID"},{"$f":"C65","v":"New or \nExisting Construction"},{"$f":"D65","v":"Space-Conditioning Category"},null,{"$f":"F65","v":"Description"},"Base_Assembly_U-factor","Base_SHGC",null,{"$f":"J65","v":"Description"},{"$f":"K65","v":"Assembly \nU-factor"},{"$f":"L65","v":"SHGC"},{"$f":"M65","v":"VLT"},{"$f":"N65","v":"Area (sf)"},"Plans / Specs",null,"Prescriptive Requirement",null,null,null,null,"Default_Assembly_U-factor","Default_SHGC",null,"Prescriptive Requirement 90.1-2013",null,"Prescriptive Requirement 90.1-2010",null,null,"Prescriptive Requirement 90.1-2013","Prescriptive Requirement 90.1-2010"]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,null,{"$f":"IF(D68=\"Unconditioned\",K68,IF($T68<>0,$T68,\"\"))","v":""},{"$f":"IF(D68=\"Unconditioned\",L68,IF($U68<>0,$U68,\"\"))","v":""},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF('General Information'!$K$48=2013,Y68,IF('General Information'!$K$48=2010,AA68,IF('General Information'!$K$48=2007,\"Not Supported\"))),\"-\")","v":""},null,{"$f":"D68&F68","v":""},{"$f":"IFERROR(INDEX('Envelope Assumptions'!$AT$2:$BE$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(S68,'Envelope Assumptions'!$AT$2:$BE$2,0)),0)","v":0},{"$f":"IFERROR(INDEX('Envelope Assumptions'!$BF$2:$BQ$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(S68,'Envelope Assumptions'!$BF$2:$BQ$2,0)),0)","v":0},{"$f":"IF($C68=\"Existing\",\"Provide U-Factor\",IF($T68<>0,$T68,\"\"))","v":""},{"$f":"IF($C68=\"Existing\", \"Provide SHGC\",IF($U68<>0,$U68,\"\"))","v":""},{"$f":"'General Information'!$K$46&\"-\"&I68","v":"4-"},{"$f":"IF(D68=\"\",\"\",INDEX(Env_Lookup_2013_Windows,MATCH(X68,Env_Lookup_2013_Windows_CZ,0),MATCH(D68,Env_Lookup_2013_Windows_BT,0)))","v":""},null,{"$f":"IF(D68=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!DI$2:DL$16,MATCH(X68,'Envelope Lookup 90.1-2010'!DI$2:DI$16,0),MATCH(D68,'Envelope Lookup 90.1-2010'!DI$2:DL$2,0)))","v":""},null,{"$f":"D68&\" \"&I68","v":" "},{"$f":"IFERROR(INDEX('Envelope Lookup 90.1-2013'!$BR$2:$CC$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(AC68,'Envelope Lookup 90.1-2013'!$BR$2:$CC$2,0)),0)","v":0},{"$f":"IFERROR(INDEX('Envelope Lookup 90.1-2010'!$BR$2:$CC$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(AC68,'Envelope Lookup 90.1-2010'!$BR$2:$CC$2,0)),0)","v":0}]
["A",{"$f":"GI_Project_Name","v":0},null,null,null,null,{"$f":"IF(D69=\"Unconditioned\",K69,IF($T69<>0,$T69,\"\"))","v":""},{"$f":"IF(D69=\"Unconditioned\",L69,IF($U69<>0,$U69,\"\"))","v":""},null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF('General Information'!$K$48=2013,Y69,IF('General Information'!$K$48=2010,AA69,IF('General Information'!$K$48=2007,\"Not Supported\"))),\"-\")","v":""},null,{"$f":"D69&F69","v":""},{"$f":"IFERROR(INDEX('Envelope Assumptions'!$AT$2:$BE$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(S69,'Envelope Assumptions'!$AT$2:$BE$2,0)),0)","v":0},{"$f":"IFERROR(INDEX('Envelope Assumptions'!$BF$2:$BQ$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(S69,'Envelope Assumptions'!$BF$2:$BQ$2,0)),0)","v":0},{"$f":"IF($C69=\"Existing\",\"Provide U-Factor\",IF($T69<>0,$T69,\"\"))","v":""},{"$f":"IF($C69=\"Existing\", \"Provide SHGC\",IF($U69<>0,$U69,\"\"))","v":""},{"$f":"'General Information'!$K$46&\"-\"&I69","v":"4-"},{"$f":"IF(D69=\"\",\"\",INDEX(Env_Lookup_2013_Windows,MATCH(X69,Env_Lookup_2013_Windows_CZ,0),MATCH(D69,Env_Lookup_2013_Windows_BT,0)))","v":""},null,{"$f":"IF(D69=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!DI$2:DL$16,MATCH(X69,'Envelope Lookup 90.1-2010'!DI$2:DI$16,0),MATCH(D69,'Envelope Lookup 90.1-2010'!DI$2:DL$2,0)))","v":""},null,{"$f":"D69&\" \"&I69","v":" "},{"$f":"IFERROR(INDEX('Envelope Lookup 90.1-2013'!$BR$2:$CC$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(AC69,'Envelope Lookup 90.1-2013'!$BR$2:$CC$2,0)),0)","v":0},{"$f":"IFERROR(INDEX('Envelope Lookup 90.1-2010'!$BR$2:$CC$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(AC69,'Envelope Lookup 90.1-2010'!$BR$2:$CC$2,0)),0)","v":0}]
["G"]
["G"]
["G","Table 4.3: Skylights"]
["G","General Information",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,"Proposed Design",null,null,null,null,null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
["G","Building ID","New or \nExisting Construction","Space-Conditioning Category",null,"Description","Assembly \nU-factor","SHGC","Description",null,"Assembly \nU-factor","SHGC","VLT","Area (sf)","Plans / Specs"]
["G",null,null,null,null,"Helpful Hints\n• New/Existing skylights: assembly U-factor and SHGC from Table G3.4-1 through G3.4-8 using the value for skylights without curb; sky lighting area per G3.1#5(e). \n\n(SHGC). Please note that this is not equivalent to the shading coefficient (SC).",null,null,"Helpful Hints\n• Proposed skylight assembly U-factor should be as-designed and account for the impact of the frames on the whole assembly. Reference Tables A8.1-1 and A8.1-2 of ASHRAE 90.1 as necessary.\n• Describe the Proposed skylight assembly (for example: glass with curb, double glazing, argon filled, low-e coating, aluminum frame with thermal break)\n• Enter the Proposed skylight assembly solar heat gain coefficient (SHGC). Please note that this is not equivalent to the shading coefficient (SC).\n• Enter the Proposed skylight assembly visual light transmittance (VLT)\n• If the Proposed design includes building envelope assemblies of different U-values, please specify surface area, square feet, for each envelope assembly.\n•Reference specific place in the submitted design documents (e.g. drawing & detail number) where relevant parameters are listed to support review.",null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2013,\"In accordance with Prescriptive Requirements of 90.1-2013 \"&INDEX(DropdownData!AW2:AW19,MATCH('General Information'!C46,AshraeClimate,0)),\"In accordance with Prescriptive Requirements of 90.1-2010 \"&INDEX(DropdownData!AX2:AX19,MATCH('General Information'!C46,AshraeClimate,0)))","v":"In accordance with Prescriptive Requirements of 90.1-2013 Table 5.5-4"}]
["G",{"$f":"B74","v":"Building ID"},{"$f":"C74","v":"New or \nExisting Construction"},{"$f":"D74","v":"Space-Conditioning Category"},null,"Base_Description","Base_Assembly_U-factor","Base_SHGC",null,"Proposed_Description",{"$f":"K74","v":"Assembly \nU-factor"},{"$f":"L74","v":"SHGC"},{"$f":"M74","v":"VLT"},{"$f":"N74","v":"Area (sf)"},{"$f":"O74","v":"Plans / Specs"},null,"Prescriptive Requirement",null,null,null,null,"Default_Assembly_U-factor","Default_SHGC",null,"Prescriptive Requirement 90.1-2013",null,"Prescriptive Requirement 90.1-2010"]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,null,{"$f":"IF(D77=\"Unconditioned\",K77,IF($T77<>0,$T77,\"\"))","v":""},{"$f":"IF(D77=\"Unconditioned\",L77,IF($U77<>0,$U77,\"\"))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D77=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Y77<>0,$Z77<>0),\"U-\"&$Y77&\", SHGC-\"&$Z77,\"\"),IF(AND($AA77<>0,$AB77<>0),\"U-\"&$AA77&\", SHGC-\"&$AB77,\"\"))))","v":""},null,{"$f":"D77&F77","v":""},{"$f":"IFERROR(INDEX('Envelope Assumptions'!$BR$2:$BW$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(S77,'Envelope Assumptions'!$BR$2:$BW$2,0)),0)","v":0},{"$f":"IFERROR(INDEX('Envelope Assumptions'!$BX$2:$CC$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(S77,'Envelope Assumptions'!$BX$2:$CC$2,0)),0)","v":0},{"$f":"IF($C77=\"Existing\",\"Provide U-Factor\",IF($T77<>0,$T77,\"\"))","v":""},{"$f":"IF($C77=\"Existing\", \"Provide SHGC\",IF($U77<>0,$U77,\"\"))","v":""},null,{"$f":"IFERROR(INDEX('Envelope Lookup 90.1-2013'!$CP$2:$CU$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(S77,'Envelope Lookup 90.1-2013'!$CP$2:$CU$2,0)),0)","v":0},{"$f":"IFERROR(INDEX('Envelope Lookup 90.1-2013'!$CV$2:$DA$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(S77,'Envelope Lookup 90.1-2013'!$CV$2:$DA$2,0)),0)","v":0},{"$f":"IFERROR(INDEX('Envelope Lookup 90.1-2010'!$CP$2:$CU$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(S77,'Envelope Lookup 90.1-2010'!$CP$2:$CU$2,0)),0)","v":0},{"$f":"IFERROR(INDEX('Envelope Lookup 90.1-2010'!$CV$2:$DA$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(S77,'Envelope Lookup 90.1-2010'!$CV$2:$DA$2,0)),0)","v":0}]
["B",{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D78=\"Unconditioned\",J78,\"\")","v":""},{"$f":"IF(D78=\"Unconditioned\",K78,IF($T78<>0,$T78,\"\"))","v":""},{"$f":"IF(D78=\"Unconditioned\",L78,IF($U78<>0,$U78,\"\"))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D78=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Y78<>0,$Z78<>0),\"U-\"&$Y78&\", SHGC-\"&$Z78,\"\"),IF(AND($AA78<>0,$AB78<>0),\"U-\"&$AA78&\", SHGC-\"&$AB78,\"\"))))","v":""},null,{"$f":"D78&F78","v":""},{"$f":"IFERROR(INDEX('Envelope Assumptions'!$BR$2:$BW$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(S78,'Envelope Assumptions'!$BR$2:$BW$2,0)),0)","v":0},{"$f":"IFERROR(INDEX('Envelope Assumptions'!$BX$2:$CC$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(S78,'Envelope Assumptions'!$BX$2:$CC$2,0)),0)","v":0},{"$f":"IF($C78=\"Existing\",\"Provide U-Factor\",IF($T78<>0,$T78,\"\"))","v":""},{"$f":"IF($C78=\"Existing\", \"Provide SHGC\",IF($U78<>0,$U78,\"\"))","v":""},null,{"$f":"IFERROR(INDEX('Envelope Lookup 90.1-2013'!$CP$2:$CU$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(S78,'Envelope Lookup 90.1-2013'!$CP$2:$CU$2,0)),0)","v":0},{"$f":"IFERROR(INDEX('Envelope Lookup 90.1-2013'!$CV$2:$DA$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(S78,'Envelope Lookup 90.1-2013'!$CV$2:$DA$2,0)),0)","v":0},{"$f":"IFERROR(INDEX('Envelope Lookup 90.1-2010'!$CP$2:$CU$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(S78,'Envelope Lookup 90.1-2010'!$CP$2:$CU$2,0)),0)","v":0},{"$f":"IFERROR(INDEX('Envelope Lookup 90.1-2010'!$CV$2:$DA$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(S78,'Envelope Lookup 90.1-2010'!$CV$2:$DA$2,0)),0)","v":0}]
["G"]
["G"]
["G","How were the proposed framed assembly fenestration U-factors determined?"]
["G"]
["G"]
["G","Additional notes:"]
["G"]
[]
[]
[null,null,null,null,null,null,null,"NFRC testing for site-assembled fenestration"]
[null,null,null,null,null,null,null,"NFRC testing for manufactured fenestration assemblies"]
[null,null,null,null,null,null,null,"Table A8.2 (windows) and Table A8.1 (skylights)"]
[null,null,null,null,null,null,null,"LBNL Window 5 or Window 6 calculations"]
[null,null,null,null,null,null,null,"Energy simulation includes separate frame and glazing"]
[null,null,null,null,null,null,null,"Other (Describe)"]

{"sheet":"5 - Opaque Assemblies","index":9,"n_rows":110,"n_cols":31,"rows_kept":110,"cut":false,"hidden":false,"merged":[[39,1,39,4],[39,5,39,6],[39,7,39,8],[43,1,43,4],[43,5,43,6],[43,7,43,8],[58,1,59,1],[58,2,59,2],[58,3,59,3],[41,1,41,4],[47,5,47,6],[57,5,57,6],[47,1,47,3],[49,5,49,6],[48,1,49,1],[48,2,49,2],[48,3,49,3],[41,5,41,6],[40,5,40,8],[41,7,41,8],[42,7,42,8],[42,1,42,4],[40,1,40,4],[47,7,47,11],[87,5,87,6],[98,1,99,1],[98,2,99,2],[98,3,99,3],[68,2,69,2],[68,3,69,3],[78,1,79,1],[78,2,79,2],[78,3,79,3],[88,1,89,1],[88,2,89,2],[88,3,89,3],[33,7,33,8],[30,5,30,6],[30,7,30,8],[31,5,31,6],[31,7,31,8],[30,9,34,10],[34,5,34,6],[34,7,34,8],[29,1,29,10],[32,1,32,4],[32,5,32,6],[32,7,32,8],[33,1,33,4],[33,5,33,6],[34,1,34,4],[35,7,35,8],[36,1,36,4],[36,5,36,6],[36,7,36,8],[37,7,37,8],[4,1,4,10],[10,1,10,5],[12,1,12,5],[14,1,14,5],[16,1,16,9],[8,1,8,5],[8,6,8,11],[10,6,10,11],[12,6,12,11],[14,6,14,11],[16,10,16,11],[18,10,18,11],[20,10,20,11],[22,10,22,11],[24,1,24,11],[25,1,25,11],[20,1,20,9],[22,1,22,9],[18,1,18,9],[35,9,42,10],[109,1,109,11],[69,5,69,6],[79,5,79,6],[59,5,59,6],[99,5,99,6],[67,5,67,6],[77,1,77,3],[87,1,87,3],[97,1,97,3],[89,5,89,6],[97,5,97,6],[38,1,38,4],[37,5,37,6],[42,5,42,6],[57,1,57,3],[67,1,67,3],[68,1,69,1],[77,5,77,6],[37,1,37,4],[38,7,38,8],[38,5,38,6],[35,1,35,4],[35,5,35,6],[87,14,90,14],[97,7,97,11],[99,7,99,11],[97,13,98,13],[97,14,100,14],[49,7,49,11],[47,16,48,16],[47,17,49,17],[57,7,57,11],[59,7,59,11],[57,13,58,13],[57,14,60,14],[69,7,69,11],[67,13,68,13],[67,14,70,14],[67,7,67,11],[77,7,77,11],[79,7,79,11],[77,13,78,13],[87,7,87,11],[89,7,89,11],[87,13,88,13],[77,14,80,14],[47,13,47,14]]}
["G"]
["G","Opaque Assemblies"]
["G"]
["G"]
["G","Instructions: Complete the Opaque Building Envelope Requirements section, then describe each unique opaque building envelope construction on a separate row in the Opaque Building Envelope Constructions table. Please refer to the column header notes for information about Appendix G modeling protocol. For any information not applicable to the project, simply enter \"N/A\". Baseline information will autogenerate for new construction when the space conditioning category is selected."]
["G"]
["G","Opaque Building Envelope Requirements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G"]
["G","All residential spaces (guest rooms, living quarters, private living space, in-patient rooms, and sleeping quarters) have been modeled with the required residential construction types from Tables G3.4-1 through G3.4-8 per ASHRAE 90.1-2016 Appendix G. "]
["G"]
["G","For existing spaces, have there been any changes to the space conditioning category (for example, previously unconditioned spaces becoming fully conditioned)?"]
["G"]
["G","All spaces qualifying as semiheated are not defined as heated per Table 3.2 or indirectly conditioned (see Section 3.2 definition of space)."]
["G"]
["G","Opaque envelope assemblies separating conditioned space from unconditioned or semiheated space in the baseline are modeled using semiheated envelope assemblies per the ASHRAE 90.1-2013 User's Manual, Section 5.1.2, Space Conditioning Categories (Page 5-1). Refer to Figure 5-B."]
["G"]
["G","All baseline new construction opaque envelope assemblies were modeled as required by Tables G3.4-1 through G3.4-8 per ASHRAE 90.1 2016 Appendix G for the project's climate zone and Table G3.1#5(b) as lightweight assembly types."]
["G"]
["G",{"$f":"IF(RatingSystem_IDC,CONCATENATE(\"All existing envelope opaque assemblies were modeled as required by Tables G3.4-1 through G3.4-8 per ASHRAE 90.1-2016 Appendix G for the project's climate zone and Table G3.1#5(Proposed)(b) as lightweight assembly types,\",\" and are not modeled using Exception (f) per Rating system requirements\"),CONCATENATE(\"All baseline existing roofs, above-grade exterior walls, below-grade exterior walls, exposed floors, slab-on-grade floors, and opaque doors were modeled\",\" using Tables G3.4-1 through G3.4-8 per ASHRAE 90.1-2016 Appendix G.\"))","v":"All baseline existing roofs, above-grade exterior walls, below-grade exterior walls, exposed floors, slab-on-grade floors, and opaque doors were modeled using Tables G3.4-1 through G3.4-8 per ASHRAE 90.1-2016 Appendix G."}]
["G"]
["G","All proposed roofs, above-grade exterior walls, below-grade exterior walls, exposed floors, slab-on-grade floors, and opaque doors were modeled as-designed and with assembly U-factors, C-factors, and F-factors consistent with Appendix A values."]
["G"]
["G",{"$f":"IF('General Information'!E9=\"ENERGY STAR MFHR\",DropdownData!DV2,DropdownData!DW2)","v":"Infiltration rates and schedules have been modeled identically in the baseline and proposed, unless whole-building or compartmentalization air leakage testing, in accordance with ASTM e779, is specified during design and completed after construction (per Table G3.1#5). If performance credit is modeled for infiltration reduction, complete the Infiltration table below."}]
["G"]
["G","For each item entered as “No” above, describe the applicable ASHRAE 90.1 Appendix G exception(s) that apply, or the circumstances preventing the opaque envelope parameters from being modeled as required. If the energy simulation software is not capable of modeling the required parameters, describe the adjustments that were made to provide a thermodynamically similar representation or provide a narrative justifying why the predicted energy performance results will not be influenced."]
["G"]
["G"]
[null,"Table 5.1: Infiltration"]
[]
[null,"Only required if infiltration is modeled for performance credit. If \"Individual Apartments\" is selected in cell H36, air leakage rate should be calculated in the Testing & Verification Worksheets \"8.1- INF_BLOWER DOOR TEST\" tab, and the highest air leakage rate should be entered below in cell H38."]
[null,null,null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,"Proposed Design",null,"Measure #"]
[null,null,null,null,null,"Per Table G3.1#5, the air leakage rate at a fixed building pressure differential of 0.3 in. H20 shall be 0.4 cfm/ft2, and infiltration rates must be converted into appropriate modeling inputs using one of the two methods in G3.1.1.4",null,"To claim performance credit for infiltration reduction, actual, measured infiltration, based on testing  performed in accordance with ASTM e779, must be modeled. Otherwise, proposed infiltration must be modeled identically to the baseline."]
[null,"A FLR = total gross floor area, SqFt",null,null,null,{"$f":"H33","v":0},null,{"$f":"'General Information'!F23","v":0}]
[null,"A EW = total above grade exterior wall area, SqFt",null,null,null,{"$f":"H34","v":0},null,{"$f":"'4 - Shading and Fenestration'!I44","v":0}]
[null,"S = total area of the envelope air pressure boundary (expressed in ft2), including the lowest floor, any below- or above-grade walls, and roof (or ceiling) (including windows and skylights), separating the interior conditioned space from the unconditioned environment measured",null,null,null,{"$f":"H35","v":0},null,{"$f":"'4 - Shading and Fenestration'!I44+'4 - Shading and Fenestration'!I47+'4 - Shading and Fenestration'!I47","v":0}]
[null,"Air leakage measurement type",null,null,null,"Whole Building"]
[null,"Fixed building pressure differential ",null,null,null,"75 Pa"]
[null,"I 75Pa / I 50 Pa = air leakage rate of the building envelope expressed in cfm/ft2 at the specified fixed building pressure differential.",null,null,null,0.4]
[null,"Q = Volume of air in CFM flowing through the whole building envelope when subjected to the specified fixed building pressure differential.",null,null,null,{"$f":"F38*F35","v":0},null,{"$f":"H38*H35","v":0}]
[null,"Building Volume (ft3)",null,null,null,{"$f":"H40","v":0}]
[null,null,null,null,null,"Simulation Inputs"]
[null,{"$f":"IF(SI_IP_Units=\"IP\",\" I flr = Baseline Model Infiltration as a Function of Floor Area [cfm/sf]\",\" I flr Baseline Model Infiltration as a Function of Floor Area [cfm/m2]\")","v":" I flr = Baseline Model Infiltration as a Function of Floor Area [cfm/sf]"},null,null,null,{"$f":"IFERROR(IF(F39=\"\",\"-\",(0.112*F39/F33)),\"-\")","v":"-"},null,{"$f":"IFERROR(IF(H37=\"\",\"-\",IF(H37=\"75 Pa\",0.112*H39/H33,IF(H37=\"50 Pa\",0.146*H39/H33))),\"-\")","v":"-"}]
[null,{"$f":"IF(SI_IP_Units=\"IP\",\"I ew = Baseline Model Infiltration as a Function of Exterior Wall Area  [cfm/sf]\",\"I ew -Baseline Model Infiltration as a Function of Exterior Wall Area [cfm/m2]\")","v":"I ew = Baseline Model Infiltration as a Function of Exterior Wall Area  [cfm/sf]"},null,null,null,{"$f":"IFERROR(IF(F39=\"\",\"-\",(0.112*F39/F34)),\"-\")","v":"-"},null,{"$f":"IFERROR(IF(H37=\"\",\"-\",IF(H37=\"75 Pa\",0.112*H39/H34,IF(H37=\"50 Pa\",0.146*H39/H34))),\"-\")","v":"-"}]
[null,"Air Changes Per Hour (ACH)",null,null,null,{"$f":"IFERROR(((F39*60)/F40)*0.112,\"-\")","v":"-"},null,{"$f":"IFERROR(IF(H37=\"\",\"-\",IF(H37=\"75 Pa\",0.112*((H39*60)/H40),IF(H37=\"50 Pa\",0.146*((H39*60)/H40)))),\"-\")","v":"-"}]
[]
["G","Opaque Building Envelope Constructions"]
["G","Table 5.2: Roof Constructions"]
["G","General Information",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,"Proposed Design",null,null,null,null,null,"Roof Solar Reflectance and Thermal Emittance",null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
["G","Building ID","New or \nExisting\nConstruction","Space-Conditioning Category",null,"Description","Assembly U-factor","Type","Description","Assembly \nU-factor","Area (sf)","Plans / Specs",null,"Baseline","Proposed"]
["G",null,null,null,null,"Helpful Hints\n• Describe the Baseline roof construction (for example: R-20 (R-2.6) continuous insulation entirely above metal deck).\n• New/Existing/Addition roofs: insulation entirely above deck with U-factor from Table G3.4-1 through G3.4-8 per Table G3.1#5(b). \n",null,"Helpful Hints\n• Describe the Proposed roof construction and Appendix A Table if referenced (for example: R-30 (R-5.3) continuous insulation entirely above metal deck per Table A2.2.3).  \n• Proposed construction assembly U-factor should be as-designed and consistent with Appendix A of ASHRAE 90.1.  \n• If the Proposed design includes building envelope assemblies of different U-values, please specify surface area, square feet, for each envelope assembly.\n•Reference specific place in the submitted design documents (e.g. drawing & detail number) where relevant parameters are listed to support review.",null,null,null,null,null,"Helpful Hints\n• In accordance with Section 5.5.3.1.1(a) or 0.3/0.9 per Table G3.1#5(f).",null,null,{"$f":"IF('General Information'!$K$48=2013,\"In accordance with Prescriptive Requirements of 90.1-2013 \"&INDEX(DropdownData!AW2:AW19,MATCH('General Information'!C46,AshraeClimate,0)),\"In accordance with Prescriptive Requirements of 90.1-2010 \"&INDEX(DropdownData!AX2:AX19,MATCH('General Information'!C46,AshraeClimate,0)))","v":"In accordance with Prescriptive Requirements of 90.1-2013 Table 5.5-4"}]
["G",{"$f":"B49","v":"Building ID"},{"$f":"C49","v":"New or \nExisting\nConstruction"},"Space-Conditioning Category",null,"Base_Description","Assembly U-factor",null,"Proposed_Description",{"$f":"J49","v":"Assembly \nU-factor"},{"$f":"K49","v":"Area (sf)"},"Plans / Specs",null,{"$f":"N49","v":"Baseline"},{"$f":"O49","v":"Proposed"},null,"Prescriptive Requirement",null,null,null,null,null,"Default_Description","Default_Assembly_U-factor",null,"Prescriptive Requirement 90.1-2013","Prescriptive Requirement 90.1-2010"]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D52=\"Unconditioned\",I52,IF(AND($U52<>0,$D52<>\"\"),$U52,\"\"))","v":""},{"$f":"IF(D52=\"Unconditioned\",J52,IF(AND($V52<>0,$D52<>\"\"),$V52,\"\"))","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D52=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z52<>0,$D52<>\"\"),\"U-\"&$Z52&\"; Reflectance 0.55 / Emittance 0.75\",\"\"),IF(AND($AA52<>0,$D52<>\"\"),\"U-\"&$AA52&\"; Reflectance 0.55 / Emittance 0.75\",\"\"))))","v":""},null,null,null,{"$f":"IFERROR(IF(C52=\"\",\"\",INDEX('Envelope Assumptions'!$A$2:$D$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D52,'Envelope Assumptions'!$A$2:$D$2,0))),0)","v":""},{"$f":"IFERROR(IF(C52=\"\",\"\",INDEX('Envelope Assumptions'!$X$2:$Z$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D52,'Envelope Assumptions'!$X$2:$Z$2,0))),0)","v":""},{"$f":"IF(AND($U52<>0,$D52<>\"\"),$U52,\"\")","v":""},{"$f":"IF(AND($V52<>0,$D52<>\"\"),$V52,\"\")","v":""},{"$f":"D52&\" \"&H52","v":" "},{"$f":"IFERROR(IF(C52=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$X$2:$AF$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y52,'Envelope Lookup 90.1-2013'!$X$2:$AF$2,0))),0)","v":""},{"$f":"IFERROR(IF(C52=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$X$2:$AF$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y52,'Envelope Lookup 90.1-2010'!$X$2:$AF$2,0))),0)","v":""}]
["A",{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D53=\"Unconditioned\",I53,IF(AND($U53<>0,$D53<>\"\"),$U53,\"\"))","v":""},{"$f":"IF(D53=\"Unconditioned\",J53,IF(AND($V53<>0,$D53<>\"\"),$V53,\"\"))","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D53=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z53<>0,$D53<>\"\"),\"U-\"&$Z53&\"; Reflectance 0.55 / Emittance 0.75\",\"\"),IF(AND($AA53<>0,$D53<>\"\"),\"U-\"&$AA53&\"; Reflectance 0.55 / Emittance 0.75\",\"\"))))","v":""},null,null,null,{"$f":"IFERROR(IF(C53=\"\",\"\",INDEX('Envelope Assumptions'!$A$2:$D$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D53,'Envelope Assumptions'!$A$2:$D$2,0))),0)","v":""},{"$f":"IFERROR(IF(C53=\"\",\"\",INDEX('Envelope Assumptions'!$X$2:$Z$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D53,'Envelope Assumptions'!$X$2:$Z$2,0))),0)","v":""},{"$f":"IF(AND($U53<>0,$D53<>\"\"),$U53,\"\")","v":""},{"$f":"IF(AND($V53<>0,$D53<>\"\"),$V53,\"\")","v":""},{"$f":"D53&\" \"&H53","v":" "},{"$f":"IFERROR(IF(C53=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$X$2:$AF$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y53,'Envelope Lookup 90.1-2013'!$X$2:$AF$2,0))),0)","v":""},{"$f":"IFERROR(IF(C53=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$X$2:$AF$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y53,'Envelope Lookup 90.1-2010'!$X$2:$AF$2,0))),0)","v":""}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D54=\"Unconditioned\",I54,IF(AND($U54<>0,$D54<>\"\"),$U54,\"\"))","v":""},{"$f":"IF(D54=\"Unconditioned\",J54,IF(AND($V54<>0,$D54<>\"\"),$V54,\"\"))","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D54=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z54<>0,$D54<>\"\"),\"U-\"&$Z54&\"; Reflectance 0.55 / Emittance 0.75\",\"\"),IF(AND($AA54<>0,$D54<>\"\"),\"U-\"&$AA54&\"; Reflectance 0.55 / Emittance 0.75\",\"\"))))","v":""},null,null,null,{"$f":"IFERROR(IF(C54=\"\",\"\",INDEX('Envelope Assumptions'!$A$2:$D$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D54,'Envelope Assumptions'!$A$2:$D$2,0))),0)","v":""},{"$f":"IFERROR(IF(C54=\"\",\"\",INDEX('Envelope Assumptions'!$X$2:$Z$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D54,'Envelope Assumptions'!$X$2:$Z$2,0))),0)","v":""},{"$f":"IF(AND($U54<>0,$D54<>\"\"),$U54,\"\")","v":""},{"$f":"IF(AND($V54<>0,$D54<>\"\"),$V54,\"\")","v":""}," ",{"$f":"IFERROR(IF(C54=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$X$2:$AF$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y54,'Envelope Lookup 90.1-2013'!$X$2:$AF$2,0))),0)","v":""},{"$f":"IFERROR(IF(C54=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$X$2:$AF$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y54,'Envelope Lookup 90.1-2010'!$X$2:$AF$2,0))),0)","v":""}]
["G"]
["G"]
["G","Table 5.3: Above-Grade Exterior Wall Constructions"]
["G","General Information",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,"Proposed Design",null,null,null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
["G","Building ID","New or \nExisting\nConstruction","Space-Conditioning Category",null,"Description","Assembly U-factor","Type","Description","Assembly \nU-factor","Area (sf)","Plans / Specs"]
["G",null,null,null,null,"Helpful Hints\n• Describe the Baseline above-grade exterior wall construction (for example: steel-framed with R-13.0 (R-2.3) cavity insulation and R-7.5 (R-1.3)continuous insulation).\n• New/Existing/Addition above-grade walls: steel-framed with U-factor from Table G3.4-1 through G3.4-8 per Table G3.1#5(b).",null,"Helpful Hints\n• Describe the Proposed above-grade exterior wall construction and Appendix A Table referenced (for example: 6\" (150mm) steel frames spaced 24\" (610mm) on center with R-21 cavity insulation and R-10 (R3.7)continuous insulation per Table A3.3.3.1). \n• Proposed construction assembly U-factor should be as-designed and consistent with Appendix A of ASHRAE 90.1.  \n• If the Proposed design includes building envelope assemblies of different U-values, please specify surface area, square feet, for each envelope assembly.\n•Reference specific place in the submitted design documents (e.g. drawing & detail number) where relevant parameters are listed to support review.",null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2013,\"In accordance with Prescriptive Requirements of 90.1-2013 \"&INDEX(DropdownData!AW2:AW19,MATCH('General Information'!C46,AshraeClimate,0)),\"In accordance with Prescriptive Requirements of 90.1-2010 \"&INDEX(DropdownData!AX2:AX19,MATCH('General Information'!C46,AshraeClimate,0)))","v":"In accordance with Prescriptive Requirements of 90.1-2013 Table 5.5-4"}]
["G",{"$f":"B59","v":"Building ID"},{"$f":"C59","v":"New or \nExisting\nConstruction"},{"$f":"D59","v":"Space-Conditioning Category"},null,"Base_Description",{"$f":"G59","v":"Assembly U-factor"},null,"Proposed_Description",{"$f":"J59","v":"Assembly \nU-factor"},{"$f":"K59","v":"Area (sf)"},{"$f":"L59","v":"Plans / Specs"},null,"Prescriptive Requirement",null,null,null,null,null,null,null,null,"Default_Description","Default_Assembly_U-factor",null,"Prescriptive Requirement 90.1-2013","Prescriptive Requirement 90.1-2010"]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D62=\"Unconditioned\",I62,IF(AND($U62<>0,$D62<>\"\"),$U62,\"\"))","v":""},{"$f":"IF(D62=\"Unconditioned\",J62,IF(AND($V62<>0,$D62<>\"\"),$V62,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D62=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z62<>0,$D62<>\"\"),\"U-\"&$Z62,\"\"),IF(AND($AA62<>0,$D62<>\"\"),\"U-\"&$AA62,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C62=\"\",\"\",INDEX('Envelope Assumptions'!$E$2:$G$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D62,'Envelope Assumptions'!$E$2:$G$2,0))),0)","v":""},{"$f":"IFERROR(IF(C62=\"\",\"\",INDEX('Envelope Assumptions'!$AA$2:$AC$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D62,'Envelope Assumptions'!$AA$2:$AC$2,0))),0)","v":""},{"$f":"IF(AND($U62<>0,$D62<>\"\"),$U62,\"\")","v":""},{"$f":"IF(AND($V62<>0,$D62<>\"\"),$V62,\"\")","v":""},{"$f":"D62&\" \"&H62","v":" "},{"$f":"IFERROR(IF(C62=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$AG$2:$AR$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y62,'Envelope Lookup 90.1-2013'!$AG$2:$AR$2,0))),0)","v":""},{"$f":"IFERROR(IF(C62=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$AG$2:$BG$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y62,'Envelope Lookup 90.1-2010'!$AG$2:$BG$2,0))),0)","v":""}]
["B",{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D63=\"Unconditioned\",I63,IF(AND($U63<>0,$D63<>\"\"),$U63,\"\"))","v":""},{"$f":"IF(D63=\"Unconditioned\",J63,IF(AND($V63<>0,$D63<>\"\"),$V63,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D63=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z63<>0,$D63<>\"\"),\"U-\"&$Z63,\"\"),IF(AND($AA63<>0,$D63<>\"\"),\"U-\"&$AA63,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C63=\"\",\"\",INDEX('Envelope Assumptions'!$E$2:$G$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D63,'Envelope Assumptions'!$E$2:$G$2,0))),0)","v":""},{"$f":"IFERROR(IF(C63=\"\",\"\",INDEX('Envelope Assumptions'!$AA$2:$AC$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D63,'Envelope Assumptions'!$AA$2:$AC$2,0))),0)","v":""},{"$f":"IF(AND($U63<>0,$D63<>\"\"),$U63,\"\")","v":""},{"$f":"IF(AND($V63<>0,$D63<>\"\"),$V63,\"\")","v":""},{"$f":"D63&\" \"&H63","v":" "},{"$f":"IFERROR(IF(C63=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$AG$2:$AR$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y63,'Envelope Lookup 90.1-2013'!$AG$2:$AR$2,0))),0)","v":""},{"$f":"IFERROR(IF(C63=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$AG$2:$BG$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y63,'Envelope Lookup 90.1-2010'!$AG$2:$BG$2,0))),0)","v":""}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D64=\"Unconditioned\",I64,IF(AND($U64<>0,$D64<>\"\"),$U64,\"\"))","v":""},{"$f":"IF(D64=\"Unconditioned\",J64,IF(AND($V64<>0,$D64<>\"\"),$V64,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D64=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z64<>0,$D64<>\"\"),\"U-\"&$Z64,\"\"),IF(AND($AA64<>0,$D64<>\"\"),\"U-\"&$AA64,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C64=\"\",\"\",INDEX('Envelope Assumptions'!$E$2:$G$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D64,'Envelope Assumptions'!$E$2:$G$2,0))),0)","v":""},{"$f":"IFERROR(IF(C64=\"\",\"\",INDEX('Envelope Assumptions'!$AA$2:$AC$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D64,'Envelope Assumptions'!$AA$2:$AC$2,0))),0)","v":""},{"$f":"IF(AND($U64<>0,$D64<>\"\"),$U64,\"\")","v":""},{"$f":"IF(AND($V64<>0,$D64<>\"\"),$V64,\"\")","v":""},{"$f":"D64&\" \"&H64","v":" "},{"$f":"IFERROR(IF(C64=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$AG$2:$AR$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y64,'Envelope Lookup 90.1-2013'!$AG$2:$AR$2,0))),0)","v":""},{"$f":"IFERROR(IF(C64=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$AG$2:$BG$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y64,'Envelope Lookup 90.1-2010'!$AG$2:$BG$2,0))),0)","v":""}]
["G"]
["G"]
["G","Table 5.4: Below-Grade Exterior Wall Constructions"]
["G","General Information",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,"Proposed Design",null,null,null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
["G","Building ID","New or \nExisting\nConstruction","Space-Conditioning Category",null,"Description","Assembly C-factor","Type","Description","Assembly\nC-factor","Area (sf)","Plans / Specs"]
["G",null,null,null,null,"Helpful Hints\n• Describe the Baseline below-grade exterior wall construction (for example: 8\" (200mm) medium-weight concrete block with solid grouted cores and R-7.5 (R-1.3)continuous insulation).\n• New/Existing/Addition below-grade walls: 8\" medium weight concrete block with solid grouted cores as defined in A4.1 with C-factor from Table G3.4-1 through G3.4-8 per Table G3.1#5(b). ",null,"Helpful Hints\n• Describe the Proposed below-grade exterior wall construction and Appendix A Table referenced (for example: 8\" (200mm) medium-weight concrete b-lock with solid grouted cores and R-10 (R3.7) continuous insulation per Table A4.2.1).  \n• Proposed construction assembly U-factor should be as-designed and consistent with Appendix A of ASHRAE 90.1.\n• If the Proposed design includes building envelope assemblies of different U-values, please specify surface area, square feet, for each envelope assembly.\n•Reference specific place in the submitted design documents (e.g. drawing & detail number) where relevant parameters are listed to support review.\n",null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2013,\"In accordance with Prescriptive Requirements of 90.1-2013 \"&INDEX(DropdownData!AW2:AW19,MATCH('General Information'!C46,AshraeClimate,0)),\"In accordance with Prescriptive Requirements of 90.1-2010 \"&INDEX(DropdownData!AX2:AX19,MATCH('General Information'!C46,AshraeClimate,0)))","v":"In accordance with Prescriptive Requirements of 90.1-2013 Table 5.5-4"}]
["G",{"$f":"B69","v":"Building ID"},{"$f":"C69","v":"New or \nExisting\nConstruction"},{"$f":"D69","v":"Space-Conditioning Category"},null,"Base_Description",{"$f":"G69","v":"Assembly C-factor"},null,"Proposed_Description",{"$f":"J69","v":"Assembly\nC-factor"},{"$f":"K69","v":"Area (sf)"},{"$f":"L69","v":"Plans / Specs"},null,"Prescriptive Requirement",null,null,null,null,null,null,null,null,"Default_Description","Default_Assembly_C-factor","Prescriptive Requirement 90.1-2013","Prescriptive Requirement 90.1-2010"]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D72=\"Unconditioned\",I72,IF(AND($U72<>0,$D72<>\"\"),$U72,\"\"))","v":""},{"$f":"IF(D72=\"Unconditioned\",J72,IF(AND($V72<>0,$D72<>\"\"),$V72,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D72=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Y72<>0,$D72<>\"\"),\"C-\"&$Y72,\"\"),IF(AND($Z72<>0,$D72<>\"\"),\"C-\"&$Z72,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C72=\"\",\"\",INDEX('Envelope Assumptions'!H$2:$J$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D72,'Envelope Assumptions'!$H$2:$J$2,0))),0)","v":""},{"$f":"IFERROR(IF(C72=\"\",\"\",INDEX('Envelope Assumptions'!$AD$2:$AF$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D72,'Envelope Assumptions'!$AD$2:$AF$2,0))),0)","v":""},{"$f":"IF(AND($U72<>0,$D72<>\"\"),$U72,\"\")","v":""},{"$f":"IF(AND($V72<>0,$D72<>\"\"),$V72,\"\")","v":""},{"$f":"IFERROR(IF(C72=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$AS$2:$AU$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(D72,'Envelope Lookup 90.1-2013'!$AS$2:$AU$2,0))),0)","v":""},{"$f":"IFERROR(IF(C72=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$AS$2:$AU$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(D72,'Envelope Lookup 90.1-2010'!$AS$2:$AU$2,0))),0)","v":""}]
["C",{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D73=\"Unconditioned\",I73,IF(AND($U73<>0,$D73<>\"\"),$U73,\"\"))","v":""},{"$f":"IF(D73=\"Unconditioned\",J73,IF(AND($V73<>0,$D73<>\"\"),$V73,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D73=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Y73<>0,$D73<>\"\"),\"C-\"&$Y73,\"\"),IF(AND($Z73<>0,$D73<>\"\"),\"C-\"&$Z73,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C73=\"\",\"\",INDEX('Envelope Assumptions'!H$2:$J$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D73,'Envelope Assumptions'!$H$2:$J$2,0))),0)","v":""},{"$f":"IFERROR(IF(C73=\"\",\"\",INDEX('Envelope Assumptions'!$AD$2:$AF$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D73,'Envelope Assumptions'!$AD$2:$AF$2,0))),0)","v":""},{"$f":"IF(AND($U73<>0,$D73<>\"\"),$U73,\"\")","v":""},{"$f":"IF(AND($V73<>0,$D73<>\"\"),$V73,\"\")","v":""},{"$f":"IFERROR(IF(C73=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$AS$2:$AU$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(D73,'Envelope Lookup 90.1-2013'!$AS$2:$AU$2,0))),0)","v":""},{"$f":"IFERROR(IF(C73=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$AS$2:$AU$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(D73,'Envelope Lookup 90.1-2010'!$AS$2:$AU$2,0))),0)","v":""}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D74=\"Unconditioned\",I74,IF(AND($U74<>0,$D74<>\"\"),$U74,\"\"))","v":""},{"$f":"IF(D74=\"Unconditioned\",J74,IF(AND($V74<>0,$D74<>\"\"),$V74,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D74=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Y74<>0,$D74<>\"\"),\"C-\"&$Y74,\"\"),IF(AND($Z74<>0,$D74<>\"\"),\"C-\"&$Z74,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C74=\"\",\"\",INDEX('Envelope Assumptions'!H$2:$J$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D74,'Envelope Assumptions'!$H$2:$J$2,0))),0)","v":""},{"$f":"IFERROR(IF(C74=\"\",\"\",INDEX('Envelope Assumptions'!$AD$2:$AF$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D74,'Envelope Assumptions'!$AD$2:$AF$2,0))),0)","v":""},{"$f":"IF(AND($U74<>0,$D74<>\"\"),$U74,\"\")","v":""},{"$f":"IF(AND($V74<>0,$D74<>\"\"),$V74,\"\")","v":""},{"$f":"IFERROR(IF(C74=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$AS$2:$AU$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(D74,'Envelope Lookup 90.1-2013'!$AS$2:$AU$2,0))),0)","v":""},{"$f":"IFERROR(IF(C74=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$AS$2:$AU$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(D74,'Envelope Lookup 90.1-2010'!$AS$2:$AU$2,0))),0)","v":""}]
["G"]
["G"]
["G","Table 5.5: Exposed Floor Constructions"]
["G","General Information",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,"Proposed Design",null,null,null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
["G","Building ID","New or \nExisting\nConstruction","Space-Conditioning Category",null,"Description","Assembly U-factor","Type","Description","Assembly \nU-factor","Area (sf)","Plans / Specs"]
["G",null,null,null,null,"Helpful Hints\n• Describe the Baseline floor construction (for example: steel-joist with R-30 (R-5.3) batt insulation between the floor joists)\n•  New/Existing/Addition floors: steel-joist with U-factor from Tables G3.4-1 through G3.4-8 per Table G3.1#5(b). \n•  For floor assemblies above unconditioned or semiheated space, select the space conditioning category as semiheated per 90.1-2013 User's Manual, Section 5.1.2-Space Conditioning Categories (Figure 5-B)\n",null,"Helpful Hints\n• Describe the Proposed floor construction and Appendix A Table referenced (for example: steel-joist with R-20 (R-2.6) spray-on insulation on underside of floor and joists per Table A5.3.3.1).  \n• Proposed construction assembly U-factor should be as-designed and consistent with Appendix A of ASHRAE 90.1.\n• If the Proposed design includes building envelope assemblies of different U-values, please specify surface area, square feet, for each envelope assembly.\n•Reference specific place in the submitted design documents (e.g. drawing & detail number) where relevant parameters are listed to support review.\n",null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2013,\"In accordance with Prescriptive Requirements of 90.1-2013 \"&INDEX(DropdownData!AW2:AW19,MATCH('General Information'!C46,AshraeClimate,0)),\"In accordance with Prescriptive Requirements of 90.1-2010 \"&INDEX(DropdownData!AX2:AX19,MATCH('General Information'!C46,AshraeClimate,0)))","v":"In accordance with Prescriptive Requirements of 90.1-2013 Table 5.5-4"}]
["G",{"$f":"B79","v":"Building ID"},{"$f":"C79","v":"New or \nExisting\nConstruction"},{"$f":"D79","v":"Space-Conditioning Category"},null,"Base_Description",{"$f":"G79","v":"Assembly U-factor"},null,"Proposed_Description",{"$f":"J79","v":"Assembly \nU-factor"},{"$f":"K79","v":"Area (sf)"},{"$f":"L79","v":"Plans / Specs"},null,"Prescriptive Requirement",null,null,null,null,null,null,null,null,"Default_Description","Default_Assembly_U-factor",null,"Prescriptive Requirement 90.1-2013","Prescriptive Requirement 90.1-2010"]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D82=\"Unconditioned\",I82,IF(AND($U82<>0,$D82<>\"\"),$U82,\"\"))","v":""},{"$f":"IF(D82=\"Unconditioned\",J82,IF(AND($V82<>0,$D82<>\"\"),$V82,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D82=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z82<>0,$D82<>\"\"),\"U-\"&$Z82,\"\"),IF(AND($AA82<>0,$D82<>\"\"),\"U-\"&$AA82,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C82=\"\",\"\",INDEX('Envelope Assumptions'!K$2:$M$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D82,'Envelope Assumptions'!$K$2:$M$2,0))),0)","v":""},{"$f":"IFERROR(IF(C82=\"\",\"\",INDEX('Envelope Assumptions'!$AG$2:$AI$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D82,'Envelope Assumptions'!$AG$2:$AI$2,0))),0)","v":""},{"$f":"IF(AND($U82<>0,$D82<>\"\"),$U82,\"\")","v":""},{"$f":"IF(AND($V82<>0,$D82<>\"\"),$V82,\"\")","v":""},{"$f":"D82&\" \"&H82","v":" "},{"$f":"IFERROR(IF(C82=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$AV$2:$BD$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y82,'Envelope Lookup 90.1-2013'!$AV$2:$BD$2,0))),0)","v":""},{"$f":"IFERROR(IF(C82=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$AV$2:$BM$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y82,'Envelope Lookup 90.1-2010'!$AV$2:$BM$2,0))),0)","v":""}]
["D",{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D83=\"Unconditioned\",I83,IF(AND($U83<>0,$D83<>\"\"),$U83,\"\"))","v":""},{"$f":"IF(D83=\"Unconditioned\",J83,IF(AND($V83<>0,$D83<>\"\"),$V83,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D83=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z83<>0,$D83<>\"\"),\"U-\"&$Z83,\"\"),IF(AND($AA83<>0,$D83<>\"\"),\"U-\"&$AA83,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C83=\"\",\"\",INDEX('Envelope Assumptions'!K$2:$M$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D83,'Envelope Assumptions'!$K$2:$M$2,0))),0)","v":""},{"$f":"IFERROR(IF(C83=\"\",\"\",INDEX('Envelope Assumptions'!$AG$2:$AI$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D83,'Envelope Assumptions'!$AG$2:$AI$2,0))),0)","v":""},{"$f":"IF(AND($U83<>0,$D83<>\"\"),$U83,\"\")","v":""},{"$f":"IF(AND($V83<>0,$D83<>\"\"),$V83,\"\")","v":""},{"$f":"D83&\" \"&H83","v":" "},{"$f":"IFERROR(IF(C83=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$AV$2:$BD$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y83,'Envelope Lookup 90.1-2013'!$AV$2:$BD$2,0))),0)","v":""},{"$f":"IFERROR(IF(C83=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$AV$2:$BM$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y83,'Envelope Lookup 90.1-2010'!$AV$2:$BM$2,0))),0)","v":""}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D84=\"Unconditioned\",I84,IF(AND($U84<>0,$D84<>\"\"),$U84,\"\"))","v":""},{"$f":"IF(D84=\"Unconditioned\",J84,IF(AND($V84<>0,$D84<>\"\"),$V84,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D84=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z84<>0,$D84<>\"\"),\"U-\"&$Z84,\"\"),IF(AND($AA84<>0,$D84<>\"\"),\"U-\"&$AA84,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C84=\"\",\"\",INDEX('Envelope Assumptions'!K$2:$M$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D84,'Envelope Assumptions'!$K$2:$M$2,0))),0)","v":""},{"$f":"IFERROR(IF(C84=\"\",\"\",INDEX('Envelope Assumptions'!$AG$2:$AI$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D84,'Envelope Assumptions'!$AG$2:$AI$2,0))),0)","v":""},{"$f":"IF(AND($U84<>0,$D84<>\"\"),$U84,\"\")","v":""},{"$f":"IF(AND($V84<>0,$D84<>\"\"),$V84,\"\")","v":""},{"$f":"D84&\" \"&H84","v":" "},{"$f":"IFERROR(IF(C84=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$AV$2:$BD$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y84,'Envelope Lookup 90.1-2013'!$AV$2:$BD$2,0))),0)","v":""},{"$f":"IFERROR(IF(C84=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$AV$2:$BM$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y84,'Envelope Lookup 90.1-2010'!$AV$2:$BM$2,0))),0)","v":""}]
["G"]
["G"]
["G","Table 5.6: Slab-On-Grade Floors"]
["G","General Information",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,"Proposed Design",null,null,null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
["G","Building ID","New or \nExisting\nConstruction","Space-Conditioning Category",null,"Description","Assembly F-factor","Type","Description","Assembly \nF-factor","Area (sf)","Plans / Specs"]
["G",null,null,null,null,"Helpful Hints\n• Describe the Baseline slab-on-grade floor construction (for example: unheated 6\" (150 mm) concrete slab poured directly on the earth with no insulation).\n• New/Existing/Addition slab-on-grade floors: unheated 6\" concrete slab as defined in A4.6 with F-factor from appropriate Tables G3.4-1 through G3.4-8 per Table G3.1#5(b). ",null,"Helpful Hints\n• Describe the Proposed slab-on-grade floor construction and Appendix A Table referenced (for example: unheated 6\" (150 mm) concrete slab poured directly on the earth with 24\" R-10 (610 mm R-3.7) vertical insulation per Table A6.3.1).  \n• Proposed construction assembly U-factor should be as-designed and consistent with Appendix A of ASHRAE 90.1 .\n• If the Proposed design includes building envelope assemblies of different U-values, please specify surface area, square feet, for each envelope assembly.\n•Reference specific place in the submitted design documents (e.g. drawing & detail number) where relevant parameters are listed to support review.",null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2013,\"In accordance with Prescriptive Requirements of 90.1-2013 \"&INDEX(DropdownData!AW2:AW19,MATCH('General Information'!C46,AshraeClimate,0)),\"In accordance with Prescriptive Requirements of 90.1-2010 \"&INDEX(DropdownData!AX2:AX19,MATCH('General Information'!C46,AshraeClimate,0)))","v":"In accordance with Prescriptive Requirements of 90.1-2013 Table 5.5-4"}]
["G",{"$f":"B89","v":"Building ID"},{"$f":"C89","v":"New or \nExisting\nConstruction"},{"$f":"D89","v":"Space-Conditioning Category"},null,"Base_Description",{"$f":"G89","v":"Assembly F-factor"},null,"Proposed_Description",{"$f":"J89","v":"Assembly \nF-factor"},{"$f":"K89","v":"Area (sf)"},{"$f":"L89","v":"Plans / Specs"},null,"Prescriptive Requirement",null,null,null,null,null,null,null,null,"Default_Description","Default_Assembly_F-factor",null,"Prescriptive Requirement 90.1-2013","Prescriptive Requirement 90.1-2010"]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D92=\"Unconditioned\",I92,IF(AND($U92<>0,$D92<>\"\"),$U92,\"\"))","v":""},{"$f":"IF(D92=\"Unconditioned\",J92,IF(AND($V92<>0,$D92<>\"\"),$V92,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D92=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z92<>0,$D92<>\"\"),\"F-\"&$Z92,\"\"),IF(AND($AA92<>0,$D92<>\"\"),\"F-\"&$AA92,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C92=\"\",\"\",INDEX('Envelope Assumptions'!N$2:$P$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D92,'Envelope Assumptions'!$N$2:$P$2,0))),0)","v":""},{"$f":"IFERROR(IF(C92=\"\",\"\",INDEX('Envelope Assumptions'!$AJ$2:$AL$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D92,'Envelope Assumptions'!$AJ$2:$AL$2,0))),0)","v":""},{"$f":"IF(AND($U92<>0,$D92<>\"\"),$U92,\"\")","v":""},{"$f":"IF(AND($V92<>0,$D92<>\"\"),$V92,\"\")","v":""},{"$f":"D92&\" \"&H92","v":" "},{"$f":"IFERROR(IF(C92=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$BE$2:$BJ$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y92,'Envelope Lookup 90.1-2013'!$BE$2:$BJ$2,0))),0)","v":""},{"$f":"IFERROR(IF(C92=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$BE$2:$BM$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y92,'Envelope Lookup 90.1-2010'!$BE$2:$BM$2,0))),0)","v":""}]
["E",{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D93=\"Unconditioned\",I93,IF(AND($U93<>0,$D93<>\"\"),$U93,\"\"))","v":""},{"$f":"IF(D93=\"Unconditioned\",J93,IF(AND($V93<>0,$D93<>\"\"),$V93,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D93=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z93<>0,$D93<>\"\"),\"F-\"&$Z93,\"\"),IF(AND($AA93<>0,$D93<>\"\"),\"F-\"&$AA93,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C93=\"\",\"\",INDEX('Envelope Assumptions'!N$2:$P$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D93,'Envelope Assumptions'!$N$2:$P$2,0))),0)","v":""},{"$f":"IFERROR(IF(C93=\"\",\"\",INDEX('Envelope Assumptions'!$AJ$2:$AL$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D93,'Envelope Assumptions'!$AJ$2:$AL$2,0))),0)","v":""},{"$f":"IF(AND($U93<>0,$D93<>\"\"),$U93,\"\")","v":""},{"$f":"IF(AND($V93<>0,$D93<>\"\"),$V93,\"\")","v":""},{"$f":"D93&\" \"&H93","v":" "},{"$f":"IFERROR(IF(C93=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$BE$2:$BJ$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y93,'Envelope Lookup 90.1-2013'!$BE$2:$BJ$2,0))),0)","v":""},{"$f":"IFERROR(IF(C93=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$BE$2:$BM$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y93,'Envelope Lookup 90.1-2010'!$BE$2:$BM$2,0))),0)","v":""}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D94=\"Unconditioned\",I94,IF(AND($U94<>0,$D94<>\"\"),$U94,\"\"))","v":""},{"$f":"IF(D94=\"Unconditioned\",J94,IF(AND($V94<>0,$D94<>\"\"),$V94,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D94=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z94<>0,$D94<>\"\"),\"F-\"&$Z94,\"\"),IF(AND($AA94<>0,$D94<>\"\"),\"F-\"&$AA94,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C94=\"\",\"\",INDEX('Envelope Assumptions'!N$2:$P$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D94,'Envelope Assumptions'!$N$2:$P$2,0))),0)","v":""},{"$f":"IFERROR(IF(C94=\"\",\"\",INDEX('Envelope Assumptions'!$AJ$2:$AL$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D94,'Envelope Assumptions'!$AJ$2:$AL$2,0))),0)","v":""},{"$f":"IF(AND($U94<>0,$D94<>\"\"),$U94,\"\")","v":""},{"$f":"IF(AND($V94<>0,$D94<>\"\"),$V94,\"\")","v":""},{"$f":"D94&\" \"&H94","v":" "},{"$f":"IFERROR(IF(C94=\"\",\"\",INDEX('Envelope Lookup 90.1-2013'!$BE$2:$BJ$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y94,'Envelope Lookup 90.1-2013'!$BE$2:$BJ$2,0))),0)","v":""},{"$f":"IFERROR(IF(C94=\"\",\"\",INDEX('Envelope Lookup 90.1-2010'!$BE$2:$BM$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y94,'Envelope Lookup 90.1-2010'!$BE$2:$BM$2,0))),0)","v":""}]
["G"]
["G"]
["G","Table 5.7: Opaque Doors"]
["G","General Information",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,"Proposed Design",null,null,null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
["G","Building ID","New or \nExisting\nConstruction","Space-Conditioning Category",null,"Description","Assembly U-factor","Type","Description","Assembly \nU-factor","Area (sf)","Plans / Specs"]
["G",null,null,null,null,"Helpful Hints\n• Describe the Baseline opaque door construction (for example: swinging or nonswinging).\n• Opaque door types shall match the proposed design and conform to the U-factor requirements from Table G3.4-1 through G3.4-8 per Table G3.1#5(b). \n• Swinging doors include all operable opaque panels with hinges on one side and opaque revolving doors, while nonswinging doors include roll-up, metal coiling, sliding, and all other doors that are not swinging doors.",null,"Helpful Hints\n• Describe the Proposed opaque door construction (for example: insulated metal swinging door). \n• Proposed construction assembly U-factor should be as-designed and consistent with Appendix A of ASHRAE 90.1.\n• If the Proposed design includes building envelope assemblies of different U-values, please specify surface area, square feet, for each envelope assembly.\n•Reference specific place in the submitted design documents (e.g. drawing & detail number) where relevant parameters are listed to support review.\n",null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,\"Opaque door types shall match the proposed design and confrom to the Prescriptive Requirements of 90.1-2013 \"&INDEX(DropdownData!AW2:AW19,MATCH('General Information'!C46,AshraeClimate,0))&\". Swinging doors include all operable opaque panels with hinges on one side and opaque revolving doors, while nonswinging doors include roll-up,\"&\" metal coiling, sliding, and all other doors that are not swining doors.\",\"All opaque doors shall have a U-factor not greater than listed in the Prescriptive Requirements of 90.1-2010 \"&INDEX(DropdownData!AX2:AX19,MATCH('General Information'!C46,AshraeClimate,0)&\". Swinging doors include all operable opaque panels with hinges on one side and opaque revolving doors, while nonswinging doors include roll-up,\"&\" metal coiling, sliding, and all other doors that are not swining doors.\")))","v":"Opaque door types shall match the proposed design and confrom to the Prescriptive Requirements of 90.1-2013 Table 5.5-4. Swinging doors include all operable opaque panels with hinges on one side and opaque revolving doors, while nonswinging doors include roll-up, metal coiling, sliding, and all other doors that are not swining doors."}]
["G",{"$f":"B99","v":"Building ID"},{"$f":"C99","v":"New or \nExisting\nConstruction"},{"$f":"D99","v":"Space-Conditioning Category"},null,"Base_Description",{"$f":"G99","v":"Assembly U-factor"},null,"Proposed_Description",{"$f":"J99","v":"Assembly \nU-factor"},{"$f":"K99","v":"Area (sf)"},{"$f":"L99","v":"Plans / Specs"},null,"Prescriptive Requirement",null,null,null,null,null,null,null,null,"Default_Description","Default_Assembly_U-factor",null,"Prescriptive Requirement 90.1-2013","Prescriptive Requirement 90.1-2010"]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D102=\"Unconditioned\",I102,IF(AND($U102<>0,$D102<>\"\"),$U102,\"\"))","v":""},{"$f":"IF(D102=\"Unconditioned\",J102,IF(AND($V102<>0,$D102<>\"\"),$V102,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D102=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z102<>0,$D102<>\"\"),\"U-\"&$Z102,\"\"),IF(AND($AA102<>0,$D102<>\"\"),\"U-\"&$AA102,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C102=\"\",\"\",CONCATENATE(\"Swinging Doors: \",INDEX('Envelope Assumptions'!Q$2:$S$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D102,'Envelope Assumptions'!$Q$2:$S$2,0)),\"; Nonswinging Doors: \",INDEX('Envelope Assumptions'!T$2:$V$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D102,'Envelope Assumptions'!$T$2:$V$2,0)))),0)","v":""},{"$f":"IFERROR(IF(C102=\"\",\"\",CONCATENATE(INDEX('Envelope Assumptions'!AM$2:$AO$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D102,'Envelope Assumptions'!$AM$2:$AO$2,0)),\" / \",INDEX('Envelope Assumptions'!AP$2:$AR$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D102,'Envelope Assumptions'!$AP$2:$AR$2,0)))),0)","v":""},{"$f":"IF(AND($U102<>0,$D102<>\"\"),$U102,\"\")","v":""},{"$f":"IF(AND($V102<>0,$D102<>\"\"),$V102,\"\")","v":""},{"$f":"D102&\" \"&H102","v":" "},{"$f":"IFERROR(IF(C102=\"\",\"\",CONCATENATE(INDEX('Envelope Lookup 90.1-2013'!BK$2:$BP$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y102,'Envelope Lookup 90.1-2013'!$BK$2:$BP$2,0)))),0)","v":""},{"$f":"IFERROR(IF(C102=\"\",\"\",CONCATENATE(INDEX('Envelope Lookup 90.1-2010'!BK$2:$BP$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y102,'Envelope Lookup 90.1-2010'!$BK$2:$BP$2,0)))),0)","v":""}]
["F",{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D103=\"Unconditioned\",I103,IF(AND($U103<>0,$D103<>\"\"),$U103,\"\"))","v":""},{"$f":"IF(D103=\"Unconditioned\",J103,IF(AND($V103<>0,$D103<>\"\"),$V103,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D103=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z103<>0,$D103<>\"\"),\"U-\"&$Z103,\"\"),IF(AND($AA103<>0,$D103<>\"\"),\"U-\"&$AA103,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C103=\"\",\"\",CONCATENATE(\"Swinging Doors: \",INDEX('Envelope Assumptions'!Q$2:$S$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D103,'Envelope Assumptions'!$Q$2:$S$2,0)),\"; Nonswinging Doors: \",INDEX('Envelope Assumptions'!T$2:$V$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D103,'Envelope Assumptions'!$T$2:$V$2,0)))),0)","v":""},{"$f":"IFERROR(IF(C103=\"\",\"\",CONCATENATE(INDEX('Envelope Assumptions'!AM$2:$AO$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D103,'Envelope Assumptions'!$AM$2:$AO$2,0)),\" / \",INDEX('Envelope Assumptions'!AP$2:$AR$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D103,'Envelope Assumptions'!$AP$2:$AR$2,0)))),0)","v":""},{"$f":"IF(AND($U103<>0,$D103<>\"\"),$U103,\"\")","v":""},{"$f":"IF(AND($V103<>0,$D103<>\"\"),$V103,\"\")","v":""},{"$f":"D103&\" \"&H103","v":" "},{"$f":"IFERROR(IF(C103=\"\",\"\",CONCATENATE(INDEX('Envelope Lookup 90.1-2013'!BK$2:$BP$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y103,'Envelope Lookup 90.1-2013'!$BK$2:$BP$2,0)))),0)","v":""},{"$f":"IFERROR(IF(C103=\"\",\"\",CONCATENATE(INDEX('Envelope Lookup 90.1-2010'!BK$2:$BP$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y103,'Envelope Lookup 90.1-2010'!$BK$2:$BP$2,0)))),0)","v":""}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,{"$f":"IF(D104=\"Unconditioned\",I104,IF(AND($U104<>0,$D104<>\"\"),$U104,\"\"))","v":""},{"$f":"IF(D104=\"Unconditioned\",J104,IF(AND($V104<>0,$D104<>\"\"),$V104,\"\"))","v":""},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(D104=\"Unconditioned\",\"-\",IF('General Information'!$K$48=2013,IF(AND($Z104<>0,$D104<>\"\"),\"U-\"&$Z104,\"\"),IF(AND($AA104<>0,$D104<>\"\"),\"U-\"&$AA104,\"\"))))","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(C104=\"\",\"\",CONCATENATE(\"Swinging Doors: \",INDEX('Envelope Assumptions'!Q$2:$S$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D104,'Envelope Assumptions'!$Q$2:$S$2,0)),\"; Nonswinging Doors: \",INDEX('Envelope Assumptions'!T$2:$V$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D104,'Envelope Assumptions'!$T$2:$V$2,0)))),0)","v":""},{"$f":"IFERROR(IF(C104=\"\",\"\",CONCATENATE(INDEX('Envelope Assumptions'!AM$2:$AO$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D104,'Envelope Assumptions'!$AM$2:$AO$2,0)),\" / \",INDEX('Envelope Assumptions'!AP$2:$AR$38,MATCH('General Information'!$L$11,'Envelope Assumptions'!$A$2:$A$38,0),MATCH(D104,'Envelope Assumptions'!$AP$2:$AR$2,0)))),0)","v":""},{"$f":"IF(AND($U104<>0,$D104<>\"\"),$U104,\"\")","v":""},{"$f":"IF(AND($V104<>0,$D104<>\"\"),$V104,\"\")","v":""},{"$f":"D104&\" \"&H104","v":" "},{"$f":"IFERROR(IF(C104=\"\",\"\",CONCATENATE(INDEX('Envelope Lookup 90.1-2013'!BK$2:$BP$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2013'!$A$2:$A$38,0),MATCH(Y104,'Envelope Lookup 90.1-2013'!$BK$2:$BP$2,0)))),0)","v":""},{"$f":"IFERROR(IF(C104=\"\",\"\",CONCATENATE(INDEX('Envelope Lookup 90.1-2010'!BK$2:$BP$38,MATCH('General Information'!$L$11,'Envelope Lookup 90.1-2010'!$A$2:$A$38,0),MATCH(Y104,'Envelope Lookup 90.1-2010'!$BK$2:$BP$2,0)))),0)","v":""}]
["G"]
[]
[]
["G"]
["G","Additional notes:"]
["G"]

{"sheet":"DropdownData","index":10,"n_rows":218,"n_cols":132,"rows_kept":218,"cut":false,"hidden":true,"merged":[[213,5,213,6],[213,8,213,9],[214,1,216,4],[214,5,215,6],[214,7,215,7],[214,8,214,10],[215,8,215,9],[216,5,216,6],[216,8,216,9],[206,1,206,3],[206,7,206,10],[207,1,213,2],[207,3,208,3],[207,5,208,6],[207,7,208,7],[207,8,207,10],[208,8,208,9],[209,5,209,6],[209,8,209,9],[210,5,210,6],[210,8,210,9],[211,5,211,6],[211,8,211,9],[212,5,212,6],[212,8,212,9],[204,1,205,4],[204,7,204,10],[205,7,205,10],[177,2,177,3],[178,2,178,3],[203,1,203,3],[203,5,203,6],[203,7,203,10]]}
[null,"Fuel Types","Site-to-source ratio","Considered \"Gas\" for District Plant Path 3 Calcs? (Note: Coal,coke, and wood are selected as gas to allow the lower efficiencies).","Energy Consumption Units","Units Spelled Out","Multiplier to convert to kBtu","multiplier to convert to therm","Energy Demand Units","Units Spelled Out","Multiplier to convert to MBH",null,null,null,"Area Units",null,"Utility Rate Structure",null,null,null,null,null,"LEED Rating System","LEED Rating System",null,null,null,"Thresholds per Rating System:","NC","CS",null,"Fenestration Percent","Skylight Percent","Exterior Lighting Zone",null,null,null,"Renewable Source",null,null,"Simulation Program",null,"90.1 versions","Energy Code",null,null,null,"ASHRAE Climate Zones","ASHRAE 90.1-2013 envelope table","ASHRAE 90.1-2010 envelope table","California Climate Zones",null,null,"ClimateZones",null,null,"Energy End-Uses","Unregulated?",null,"Energy Modeling Method:",null,null,null,"District Heating",null,"District Cooling",null,null,null,null,null,null,null,null,null,null,null,null,"Option Buttons:",null,null,"Start Cells for Utility Data:",null,null,null,null,null,null,null,"Output Sheet Names","BuildingNames",null,"Conversions for QC",null,null,null,"Baseline Orientation Exemptions",null,"Multifamily Dwelling Unit Equipment List",{"$f":"CONCATENATE(\"Base \",IF(SI_IP_Units=\"IP\",\"(kWh/year)\",\"kWh/year\"))","v":"Base (kWh/year)"},{"$f":"CONCATENATE(\"Energy Star \",IF(SI_IP_Units=\"IP\",\"(kWh/year)\",\"kWh/year\"))","v":"Energy Star (kWh/year)"},"Sensible ratio electric","Latent Ratio electric","Elec Nbr Multiplier",{"$f":"CONCATENATE(\"Base \",IF(SI_IP_Units=\"IP\",\"(Therms/year)\",\"kWh/year\"))","v":"Base (Therms/year)"},{"$f":"CONCATENATE(\"Energy Star \",IF(SI_IP_Units=\"IP\",\"(Therms/year)\",\"kWh/year\"))","v":"Energy Star (Therms/year)"},"Sensible ratio gas","Latent Ratio gas","Gas Nbr Multiplier","F","base Hot Water Load","Energy Star Hot Water Load",null,"Multifamily Non-Dwelling Unit Plug Loads","w/sf","kwh/sf",null,null,"General HVAC Baseline System Type List",null,null,"Building ID Lookup",null,null,null,"Long Comments",null,null,null,null,"Table G3.1.1-3"]
[1,"Electricity",{"$f":"IF(RatingSystemSelection=\"ENERGY STAR MFHR\",2.55,3.14)","v":2.5499999999999998},null,"kWh","Kilowatt hour",3.4119999999999999,{"$f":"G2/100","v":3.4119999999999998E-2},"kW","Kilowatt",3.4119999999999999,null,null,null,"square feet",null,"Default EIA Rates",null,null,null,null,null,"LEED v4 BD+C: New Construction","New Construction",null,null,null,null,null,null,null," 0%-10.0%"," 0%-2.0%","Zone 0",null,null,null,"Photovoltaic system",null,null,"EnergyPlus",null,"ASHRAE 90.1-2007","ASHRAE 90.1 2016 Appendix G",null,null,null,"1A","Table 5.5-1","Table 5.5-1","CZ1",null,null,"1A",null,null,"Interior lighting",null,null,"One model per building",null,null,null,"Each building generates its own heating",null,"Each building generates its own cooling",null,null,null,null,null,null,null,null,null,null,null,null,"rbOutputReporting",1,null,"Number of Energy Sources",5,null,null,null,null,null,null,null,"All",null,"Energy Consumption Units","convert to kWh",null,null,"Vertical Fenestration varies by less than 5%",null,"Refrigerator",529,423,1,0,null,null,null,null,null,0,1,0,0,null,"Corridors",0.2,0.7,null,null,"Primary HVAC System",null,null,{"$f":"ROWS(IF(MBD_LEEDNDEMSubsetExist=TRUE,\nOFFSET(MBD_BSTotal_Index,1,0,ROWS(MBD_BSTotal_Index)-1,1),\nIF(MultipleBuildingsExist=\"YES\",OFFSET(MBD_BSTotal_Index,2,0,ROWS(MBD_BSTotal_Index)-2,1),\nOFFSET(MBD_BSTotal_Index,2,0,ROWS(MBD_BSTotal_Index)-2,1))))","v":3},null,null,null,"Infiltration rates and schedules have been modeled identically in the baseline and proposed, unless whole-building or compartmentalization air leakage testing, in accordance with ASTM e779, is specified during design and completed after construction (per Table G3.1#5). If performance credit is modeled for infiltration reduction, complete the Infiltration table below.","Infiltration rates and schedules have been modeled identically in the baseline and proposed, unless whole-building air leakage testing, in accordance with ASTM e779, is specified during design and completed after construction (per Table G3.1#5). If performance credit is modeled for infiltration reduction, complete the Infiltration table below.","\"Instructions - LEED\" tab lookups","NFRC testing for site-assembled fenestration",null,"CZ 3B, 3C, and 4 to 8","CZ 0 to 3A"]
[2,"Natural Gas",1.05,"Yes","MWh","Megawatt hour",3412,34.119999999999997,"MW","Megawatt",3412,null,null,null,"square meters",null,"Fixed Rates per unit of consumption",null,null,null,null,null,"ENERGY STAR MFHR","Homes",null,null,null,null,null,null,null," 10.1%-20.0%"," 2.1%+","Zone 1",null,null,null,"Wind energy system",null,null,"EnergyPro",null,"ASHRAE 90.1-2010","California Title-24 2013, Part 6",null,null,null,"1B","Table 5.5-1","Table 5.5-1","CZ2",null,null,"1B",null,null,"Exterior lighting",null,null,"One energy model. Submeter buildings",null,null,null,"A central heating plant serves only buildings in this project",null,"A central cooling plant serves only the buildings in this project",null,null,null,null,null,null,null,null,null,null,null,null,"rbSiteRenewable",null,null,null,null,null,null,null,null,"NumBuildings",2,"PRM_Outputs(1)",0,null,"kWh",1,null,null,"Energy code does not require four orientations",null,"Dishwasher",206,164,0.6,0.15,0,null,null,null,null,0,1,{"$f":"IF(SI_IP_Units=\"IP\",1290,4883)","v":1290},{"$f":"IF(SI_IP_Units=\"IP\",860,3255)","v":860},null,"Restrooms",0.2,0.7,null,null,"All",null,null,{"$f":"IF(MBD_LEEDNDEMSubsetExist=TRUE,\nOFFSET(MBD_BSTotal_Index,1,0,ROWS(MBD_BSTotal_Index)-1,1),\nIF(MultipleBuildingsExist=\"YES\",OFFSET(MBD_BSTotal_Index,2,0,ROWS(MBD_BSTotal_Index)-2,1),\nOFFSET(MBD_BSTotal_Index,2,0,ROWS(MBD_BSTotal_Index)-2,1)))","v":0},null,null,null,"Mechanical ventilation was modeled following ENERGY STAR MFHR Simulation Guidelines Section 6.5.12. In the common spaces, the baseline ventilation rate was modeled the same as in the proposed design without exceeding ASHRAE 62.1-2013 (Simulation Guidelines Section 6.5.12, 1(b). \nIn apartments, the baseline ventilation method (mechanical versus natural) and controls (continuous versus intermittent) was modeled as specified for each application. The baseline local mechanical exhaust from bathrooms and kitchens, and the baseline dwelling-unit ventilation rate was modeled using the same rates as in the Proposed Design, without exceeding the minimum required by ASHRAE 62.2-2013.\nIf the same mechanical ventilation system was used to provide both local mechanical exhaust and whole-unit ventilation, the baseline ventilation rate was based on the greater of the two rates. \n","Per Section G3.1.2.5, the minimum ventilation system outdoor air intake flow was modeled the same for the proposed design and baseline building design except when modeling demand control ventilation in the proposed design (G3.1.2.5 Exception 1), for proposed designs with the zone air distribution effectiveness Ez>1.0 as defined in ASHRAE Standard 62.1 (G3.1.2.5 Exception 2), when proposed design has the minimum outdoor air intake flow in excess of the amount required by the building code or the rating authority (G3.1.2.5 Exception 3), or for the baseline systems serving certain laboratory spaces (G3.1.2.5 Exception 4). Indicate if any of the exceptions apply in the Additional Notes field.\nThe Baseline outside air volume and Proposed outside air volume values must be reported consistently with the information provided in IEQ Prerequisite: Minimum Indoor Air Quality, or supplemental documentation must be provided to support the local OA volume requirements or Baseline calculations for systems with Ez > 1.0. \n","UfactorMethod","NFRC testing for manufactured fenestration assemblies",null,"System 1 - PTAC","System 2 - PTHP"]
[3,"District Cooling",1,null,"kBtu","(British thermal unit) x 1,000",1,0.01,"Btuh","British thermal unit per hour",1E-3,null,null,null,null,null,"Fixed Rates per unit of consumption varying seasonally",null,null,null,null,null,"ECCCNYS ASHRAE Standard 90.1 Appendix G",null,null,null,null,null,null,null,null," 20.1%-30.0%",null,"Zone 2",null,null,null,"Solar thermal system",null,null,"eQuest",null,"ASHRAE 90.1-2013","Other approved code",null,null,null,"2A","Table 5.5-2","Table 5.5-2","CZ3",null,null,"2A",null,null,"Space heating",null,null,null,null,null,null,"A district heating plant serves the buildings in this project, or an on-campus heating plant provides heating to buildings outside of this project",null,"A district cooling plant serves the buildings in this project, or an on-campus cooling plant provides heating to buildings outside of this project",null,null,null,null,null,null,null,null,null,null,null,null,"rbDES",1,null,"Sheet","Start Row","Range Start Row","End Row","TargetRow",null,null,null,"PRM_Outputs(2)",0,null,"MWh",1000,null,null,"Building is more than 50% existing based on floor area",null,"Clothes Washer (In-unit)",81,57,0.8,0,0,null,null,null,null,0,1,{"$f":"IF(SI_IP_Units=\"IP\",12179,46102)*0.2","v":2435.8000000000002},{"$f":"IF(SI_IP_Units=\"IP\",5637,21338)*0.2","v":1127.4000000000001},null,"Stairs",0.2,0.7,null,null,"Other HVAC System",null,null,0,null,null,null,null,null,"NFRC testing for site-assembled fenestration","Table A8.2 (windows) and Table A8.1 (skylights)",null,"System 3 - PSZ-AC","System 4 - PSZ-HP"]
[4,"District Hot Water",1.2,null,"therm","therm",100,1,"MBH","(British thermal unit per hour) x 1,000",1,null,null,null,null,null,"Fixed Rates per unit of consumption and demand",null,null,null,null,null,"LEED v4 BD+C: Core and Shell","Core and Shell",null,null,null,null,null,null,null," 30.1%-40.0%",null,"Zone 3",null,null,null,"Geothermal heating system (not geoexchange)",null,null,"HAP",null,"ASHRAE 90.1-2016",null,null,null,null,"2B","Table 5.5-2","Table 5.5-2","CZ4",null,null,"2B",null,null,"Space cooling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rbDESguide",1,null,"Project EAp2 Summary",40,{"$f":"CE5+1","v":41},{"$f":"CE5+$CE$2-1","v":44},{"$f":"CG5","v":44},null,null,null,null,null,null,"kBtu",0.29308323563892147,null,null,"Design is dictated by site consideration*",null,"Cooking (electric stove/range)",604,604,0.4,0.3,0,null,null,null,null,0,1,0,0,null,"Support areas",0.2,0.7,null,null,null,null,null,"All",null,null,null,null,null,"NFRC testing for manufactured fenestration assemblies","LBNL Window 5 or Window 6 calculations",null,"System 5 - Packaged VAV with reheat","System 6 - Packaged VAV with PFP boxes"]
[5,"District Steam",1.2,null,"Btu x 10^6","(British thermal unit) x 1,000,000",1000,10,"Btuh x 10^3","(British thermal unit per hour) x 1,000",1,null,null,null,null,null,"Fixed Rates per unit of consumption and demand varying seasonally",null,null,null,null,null,"LEED v4 BD+C: Schools","Schools - New Construction",null,null,null,null,null,null,null,null,null,"Zone 4",null,null,null,"Geothermal electric system",null,null,"IES",null,null,null,null,null,null,"3A","Table 5.5-3","Table 5.5-3","CZ5",null,null,"3A",null,null,"Pumps",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rbDESAvg",null,null,"Project EAp2 Summary",{"$f":"CE5+CE2+22","v":67},68,71,{"$f":"CH5-CF5+CF6","v":71},null,null,null,null,null,null,"therm",29.308323563892145,null,null,null,null,"Cooking (gas stove/range)",null,null,null,null,0,45,45,0.3,0.2,0,1,0,0,null,"Offices",1.5,4.9000000000000004,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Table A8.2 (windows) and Table A8.1 (skylights)","Energy simulation includes separate frame and glazing",null,"System 7 - VAV with Reheat","System 8 - VAV with PFP boxes"]
[6,"Fuel Oil / Diesel",1.01,null,"MJ","(Joules) x 1,000,000",0.94799999999999995,9.4799999999999988E-3,"Btuh x 10^6","(British thermal unit per hour) x 1,000,000",1000,null,null,null,null,null,"Time of Use Rates per unit of consumption",null,null,null,null,null,"LEED v4 BD+C: Retail","Retail - New Construction",null,null,null,null,null,null,null,null,null,null,null,null,null,"On-site untreated wood waste - thermal",null,null,"Trace",null,null,null,null,null,null,"3B","Table 5.5-3","Table 5.5-3","CZ6",null,null,"3B",null,null,"Heat rejection",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Outputs(1) Building Performance",31,32,35,{"$f":"CH6-CF6+CF7","v":35},null,null,null,null,null,null,"Btu x 10^6",293.08323563892145,null,null,null,null,"Clothes Dryer (In-unit electric)","418","418",0.15,0.05,139,null,null,null,null,0,1,0,0,null,"Other",0.5,1.6,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LBNL Window 5 or Window 6 calculations","Other (Described below)",null,"System 9 - Heating and ventilation","System 10 - Heating and ventilation"]
[7,"Propane",1.01,"Yes","Ton Hours","Ton Hours",12,0.12,"MMBTUH","(British thermal unit per hour) x 1,000,000",1000,null,null,null,null,null,"Time of Use Rates per unit of consumption and demand",null,null,null,null,null,"LEED v4 BD+C: Data Centers","Data Centers - New Construction",null,null,null,null,null,null,null,null,null,null,null,null,null,"On-site untreated wood waste - electric generator",null,null,"Other",null,null,null,null,null,null,"3C","Table 5.5-3","Table 5.5-3","CZ7",null,null,"3C",null,null,"Fans - interior ventilation",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Outputs(1) Building Performance",{"$f":"CE7+CE2+58","v":94},95,98,{"$f":"CH7-CF7+CF8","v":98},null,null,null,null,null,null,"MJ",0.2778429073856975,null,null,null,null,"Clothes Dryer (In-unit gas)",38,38,1,0,12.7,26.5,26.5,0.1,0.05,8.8000000000000007,1,0,0,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Energy simulation includes separate frame and glazing",null,null,"System 11 - SZ-VAV","System 11 - SZ-VAV"]
[8,"Fuel Oil (No. 5 & No.6)",1.01,null,null,null,null,null,"ton","ton",12,null,null,null,null,null,"Time of Use Rates per unit of consumption varying seasonally",null,null,null,null,null,"LEED v4 BD+C: Warehouses and Distribution Centers","Warehouses and Distribution Centers - New Construction",null,null,null,null,null,null,null,null,null,null,null,null,null,"On-site agricultural crops or waste - thermal",null,null,null,null,null,null,null,null,null,"4A","Table 5.5-4","Table 5.5-4","CZ8",null,null,"4A",null,null,"Fans - parking garage",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Outputs(1) Building Performance",{"$f":"65+CE7+2*CE2","v":106},107,110,{"$f":"CH8-CF8+CF9","v":110},null,null,null,null,null,null,"Ton Hours",3.5169988276670576,null,null,null,null,{"$f":"CONCATENATE(\"Range hood, \",IF(SI_IP_Units=\"IP\",\"up to 500 cfm\",\"up to 236 L/s\"))","v":"Range hood, up to 500 cfm"},0.31739130434782614,0.26071428571428573,0,0,0,null,null,null,null,0,1,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Other (Describe)",null,null,"System 12 - SZ-CV-HW","System 13 - SZ-CV-ER"]
[9,"Kerosene",1.01,"Yes",null,null,null,null,null,null,null,null,null,null,null,null,"Time of Use Rates per unit of consumption and demand varying seasonally",null,null,null,null,null,"LEED v4 BD+C: Hospitality","Hospitality - New Construction",null,null,null,null,null,null,null,null,null,null,null,null,null,"On-site agricultural crops or waste - electric",null,null,null,null,null,"ASHRAE 90.1 2013 Appendix G Excerpt 2015",null,null,null,"4B","Table 5.5-4","Table 5.5-4","CZ9",null,null,"4B",null,null,"Service water heating",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Outputs(1) Building Performance",{"$f":"123+CE7+3*CE2","v":169},170,173,{"$f":"CH9-CF9+CF10","v":173},null,null,null,null,null,null,"Energy Demand Units","convert to kWh",null,null,null,null,{"$f":"CONCATENATE(\"Bath / Utility Fan, \",IF(SI_IP_Units=\"IP\",\"10 to 89 cfm\",\"5 to 42 L/s\"))","v":"Bath / Utility Fan, 10 to 89 cfm"},0.60833333333333339,0.52142857142857146,0,0,0,null,null,null,null,0,1,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[10,"Coal (anthracite)",1,"Yes","cf (Natural Gas)","cubic feet",1.0289999999999999,null,null,null,null,null,null,null,null,null,"Block Charges per unit of consumptoin",null,null,null,null,null,"LEED v4 BD+C: Healthcare","Healthcare",null,null,null,null,null,null,null,null,null,null,null,null,null,"On-site animal or organic waste - thermal",null,null,null,null,null,null,null,null,null,"4C","Table 5.5-4","Table 5.5-4","CZ10",null,null,"4C",null,null,"Receptacle equipment","x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kW",1,null,null,null,null,{"$f":"CONCATENATE(\"Bath / Utility Fan, \",IF(SI_IP_Units=\"IP\",\"90 to 500 cfm\",\"43 to 236 L/s\"))","v":"Bath / Utility Fan, 90 to 500 cfm"},0.31739130434782614,0.26071428571428573,0,0,0,null,null,null,null,0,1,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"General HVAC drop-down"]
[11,"Coal (bituminous)",1,"Yes","ccf (Natural Gas)","(cubic feet) x 100",102.9,null,null,null,null,null,null,null,null,null,"Block charges per unit of consumption and demand",null,null,null,null,null,"LEED v4 ID+C: Commercial Interiors","IDC",null,null,null,null,null,null,null,null,null,null,null,null,null,"On-site animal or organic waste - electric",null,null,null,null,null,null,null,null,null,"5A","Table 5.5-5","Table 5.5-5","CZ11",null,null,"5A",null,null,"IT equipment","x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MW",1000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"All equipment in the unfinished spaces not included in the project scope of work has been modeled identically in the Baseline and Proposed case using the Baseline modeling requirements"]
[12,"Coke",1,"Yes","kcf (Natural Gas)","(cubic feet) x 1,000",1029,null,null,null,null,null,null,null,null,null,"Block charges per unit of consumption varying seasonally",null,null,null,null,null,"LEED v4 ID+C: Retail","IDC",null,null,null,null,null,null,null,null,null,null,null,null,null,"On-site landfill gas - thermal",null,null,null,null,null,null,null,null,null,"5B","Table 5.5-5","Table 5.5-5","CZ12",null,null,"5B",null,null,"Interior lighting - process","x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Btuh",2.9308323563892149E-4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Credit has been modeled in the Proposed case for energy efficiency measures that are specifically identified in signed tenant sales and lease agreements (LEED Core & Shell only.  New Construction must be modeled identically in the Baseline and Proposed Case)."]
[13,"Wood",1,"Yes","Mcf (Natural Gas)","(cubic feet) x 1,000,000",1029000,null,null,null,null,null,null,null,null,null,"Block charges per unit of consumption and demand varying seasonally",null,null,null,null,null,"LEED v4 ID+C: Hospitality","IDC",null,null,null,null,null,null,null,null,null,null,null,null,null,"On-site landfill gas - electric",null,null,null,null,null,null,null,null,null,"5C","Table 5.5-5","Table 5.5-5","CZ13",null,null,"5C",null,null,"Refrigeration equipment","x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MBH",0.29308323563892147,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,"Lbs (District Steam)","Pounds (District Steam)",1.194,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4 BD+C Multifamily Midrise","Homes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6A","Table 5.5-6","Table 5.5-6","CZ14",null,null,"6A",null,null,"Cooking","x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Btuh x 10^3",0.29308323563892147,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Opaque Envelope - Construction"]
[null,null,null,null,"kLbs (District Steam)","(Pounds) x 1,000",1194,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4: Neighborhood Development","ND",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6B","Table 5.5-6","Table 5.5-6","CZ15",null,null,"6B",null,null,"Fans - Kitchen Ventilation","x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Btuh x 10^6",293.08323563892145,null,null,null,null,"Multifamily Dwelling Unit Equipment List",{"$f":"CONCATENATE(\"Base \",IF(SI_IP_Units=\"IP\",\"(kWh/year)\",\"kWh/year\"))","v":"Base (kWh/year)"},{"$f":"CONCATENATE(\"Energy Star \",IF(SI_IP_Units=\"IP\",\"(kWh/year)\",\"kWh/year\"))","v":"Energy Star (kWh/year)"},"Sensible ratio electric","Latent Ratio electric","Elec Nbr Multiplier",{"$f":"CONCATENATE(\"Base \",IF(SI_IP_Units=\"IP\",\"(Therms/year)\",\"kWh/year\"))","v":"Base (Therms/year)"},{"$f":"CONCATENATE(\"Energy Star \",IF(SI_IP_Units=\"IP\",\"(Therms/year)\",\"kWh/year\"))","v":"Energy Star (Therms/year)"},"Sensible ratio gas","Latent Ratio gas","Gas Nbr Multiplier","F","base Hot Water Load","Energy Star Hot Water Load",null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"New"]
[null,null,null,null,"MLbs (District Steam)","(Pounds) x 1,000,000",1194000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"7A","Table 5.5-7","Table 5.5-7","CZ16",null,null,"7A",null,null,"Industrial Process","x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MMBTUH",293.08323563892145,null,null,null,null,"Clothes Washer (Commercial)",196,138,0.8,0,0,null,null,null,null,0,1,{"$f":"IF(SI_IP_Units=\"IP\",29515,111726)*0.2","v":5903},{"$f":"IF(SI_IP_Units=\"IP\",13661,51712)*0.2","v":2732.2000000000003},null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Existing"]
[null,null,null,null,"liters (fuel oil/diesel)",null,36.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"7B","Table 5.5-7","Table 5.5-7",{"$f":"\"\"","v":""},null,null,"7B",null,null,"Elevators and escalators","x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ton",3.5169988276670576,null,null,null,null,"Clothes Dryer (Commercial electric)",418,418,0.15,0.05,139,null,null,null,null,0,2.423,0,0,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,"gallons (fuel oil/diesel)",null,138.69049999999999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"Table 5.5-8","Table 5.5-8",{"$f":"\"\"","v":""},null,null,8,null,null,"Cogen - Electricity generated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Clothes Dryer (Commercial gas)",38,38,0.1,0.05,12.7,26.5,26.5,0.1,0.05,8.8000000000000007,1,0,0,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Opaque Envelope - Space Conditioning"]
[null,null,null,null,"liters (fuel oil no. 5 or no. 6)",null,38.92,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cogen - Fuel Input",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Nonresidential"]
[null,null,null,null,"gallons (fuel oil no. 5 or no. 6)",null,149.69,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cogen - Parasitic energy",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Residential"]
[null,null,null,null,"gallons (propane)",null,91.65,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Other (Please Specify)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Semiheated"]
[null,null,null,null,"liters (propane)",null,23.83,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"W2","v":"LEED v4 BD+C: New Construction"},1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Unconditioned"]
[null,null,null,null,"Lbs (anth. coal)","Pounds (Anthracite Coal)",12.545,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"W3","v":"ENERGY STAR MFHR"},2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,"kLbs (anth. coal)","(Pounds Anthracite Coal) x 1,000",12545,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECCCNYS ASHRAE Standard 90.1 Appendix G",3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Climate Zone"]
[null,null,null,null,"MLbs (anth. coal)","(Pounds Anthracite Coal) x 1,000,000",12545000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4 BD+C: Core and Shell",4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"1A"]
[null,null,null,null,"Tons (anth. coal)","Tons (Anthracite Coal)",24800,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4 BD+C: Schools",5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"1B"]
[null,null,null,null,"Lbs (bit. coal)","Pounds (Bituminous Coal)",12.465,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4 BD+C: Retail",6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"2A"]
[null,null,null,null,"kLbs (bit. coal)","(Pounds Bituminous Coal) x 1,000",12465,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4 BD+C: Data Centers",7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"2B"]
[null,null,null,null,"MLbs (bit. coal)","(Pounds Bituminous Coal) x 1,000,000",12465000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4 BD+C: Warehouses and Distribution Centers",8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Campus Plant End Uses",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"3A"]
[null,null,null,null,"Tons (bit. coal)","Tons (Bituminous Coal)",24930,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4 BD+C: Hospitality",9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Campus space cooling",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"3B"]
[null,null,null,null,"Lbs (coke)","Pounds (coke)",12.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4 BD+C: Healthcare",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Campus heat rejection",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"3C"]
[null,null,null,null,"kLbs (coke)","(Pounds coke) x 1,000",12400,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4 ID+C: Commercial Interiors",11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Campus pumps: Cooling & Heat Rejection",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"4A"]
[null,null,null,null,"MLbs (coke)","(Pounds coke) x 1,000,000",12400000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4 ID+C: Retail",12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Campus space heating",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"4B"]
[null,null,null,null,"Tons (coke)","Tons (coke)",24800,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4 ID+C: Hospitality",13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Campus pumps: Heating",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"4C"]
[null,null,null,null,"Lbs (wood)","Pounds (wood)",7.69,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4 BD+C Multifamily Midrise",14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Campus Cogen - Electricity generated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"5A"]
[null,null,null,null,"Tons (wood)","Tons (wood)",15380,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEED v4: Neighborhood Development",15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Campus Cogen - Fuel Input",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"5B"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Campus Cogen - Parasitic energy",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"5C"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"6A"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"6B"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"7A"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"7B"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Air-Side HVAC adjustment drop-down (IP)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,0.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,2.15]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED Rating System"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED v4 BD+C: New Construction"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED v4 BD+C: Core and Shell"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED v4 BD+C: Schools"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED v4 BD+C: Retail"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED v4 BD+C: Data Centers"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED v4 BD+C: Warehouses and Distribution Centers"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED v4 BD+C: Hospitality"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED v4 BD+C: Healthcare"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED v4 ID+C: Commercial Interiors"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED v4 ID+C: Retail"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED v4 ID+C: Hospitality"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED v4 BD+C: Multifamily Midrise"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED v4: Neighborhood Development"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"LEED project phase completeness"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"90% Construction Documents"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"100% Construction Documents"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"As-built Construction Documents"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"},null,null,null,null,null,"Other - Please Describe"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,"DESPath",{"$f":"IFERROR(IF('General Information'!K62,1,IF('General Information'!L62,2,IF('General Information'!M62,3,IF('General Information'!N62,4,0)))),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,"0 = No DES",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,"1 = ASHRAE 90.1 without Addenda (Path 1)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,"2 = Full DES Performance Accounting Method (Path 2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,"3 = Streamlined DES Accounting Method (Path3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,"DistrictHeating",{"$f":"'General Information'!L61","v":false},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,"DistrictCooling",{"$f":"'General Information'!K61","v":false},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,"ENERGY SOURCES 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#N/A"}]
[null,"",null,"",null,""]
[null,"Electricity","kWh","kW","Standard energy sources"]
[null,"Natural Gas","therm","Btuh"]
[null,"",null,"",null,""]
[null,{"$f":"IF(DESPath=3,IF(DistrictHeating,\"District Heating\",IF(DistrictCooling,\"District Cooling\",\"\")),\"\")","v":""},null,null,"District energy sources"]
[null,{"$f":"IF(DESPath=3,IF(AND(DistrictHeating,DistrictCooling),\"District Cooling\",\"\"),\"\")","v":""}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Building:",0]
[null,"Model Input Parameter",null,null,null,"Baseline Case",null,"Proposed Case"]
[null,"Shading Devices",null,null,null,null,"No shading projections, manual shading devices, or self-shading have been modeled for the Baseline building"]
[null,null,null,null,null,"\n","Any shading by adjacent structures and terrain has been modeled identically to the Proposed case (if applicable)"]
[null,"Building Shape & Orientation",null,null,null,null,"The Baseline building is modeled with the same shape and orientation as the Proposed building, and for new construction rotated 90°, 180°, and 270°"]
[null,"Above-Grade Wall & Vertical Glazing Area by Orientation",null,"Orientation",null,"Above-Grade Wall Area (ft2)",null,"Above-Grade Wall Area (ft2)","Vertical Glazing Area"]
[null,null,null,null,null,null,null,null,"(ft2)",null,"(%)"]
[null,null,null,"North",null,{"$f":"IF(H210=0,\"Identical to Proposed case\",H210)","v":"Identical to Proposed case"},null,null,null,null,{"$f":"IF(H210=0,\"\",I210/H210)","v":""}]
[null,null,null,"East",null,{"$f":"IF(H211=0,\"Identical to Proposed case\",H211)","v":"Identical to Proposed case"},null,null,null,null,{"$f":"IF(H211=0,\"\",I211/H211)","v":""}]
[null,null,null,"South",null,{"$f":"IF(H212=0,\"Identical to Proposed case\",H212)","v":"Identical to Proposed case"},null,null,null,null,{"$f":"IF(H212=0,\"\",I212/H212)","v":""}]
[null,null,null,"West",null,{"$f":"IF(H213=0,\"Identical to Proposed case\",H213)","v":"Identical to Proposed case"},null,null,null,null,{"$f":"IF(H213=0,\"\",I213/H213)","v":""}]
[null,null,null,"Total",null,{"$f":"IF(H214=0,\"Identical to Proposed case\",H214)","v":"Identical to Proposed case"},null,{"$f":"SUM(H210:H213)","v":0},{"$f":"SUM(I210:I213)","v":0},null,{"$f":"IF(H214=0,\"\",I214/H214)","v":""}]
[null,"Roof & Skylight Area",null,null,null,"Roof Area (ft2)",null,"Roof Area (ft2)","Skylight Area"]
[null,null,null,null,null,null,null,null,"(ft2)",null,"(%)"]
[null,null,null,null,null,{"$f":"IF(H217=0,\"Identical to Proposed case\",H217)","v":"Identical to Proposed case"},null,null,null,null,{"$f":"IF(H217=0,\"\",I217/H217)","v":""}]
[null,{"$f":"IF(#REF!=\"\",\"\",IF(#REF!<=0.4,\"\",\"**Baseline vertical glazing areas limited to 40% of gross above-grade wall area per Table G3.1#5(c)\"))","v":{"$error":"#REF!"}}]

{"sheet":"Envelope Assumptions","index":11,"n_rows":38,"n_cols":88,"rows_kept":38,"cut":false,"hidden":true,"merged":[[0,38,0,40],[0,35,0,37],[0,16,0,18],[0,19,0,21],[0,1,0,3],[0,4,0,6],[0,7,0,9],[0,10,0,12],[0,13,0,15],[0,0,1,0],[0,23,0,25],[0,26,0,28],[0,29,0,31],[0,32,0,34],[0,69,0,74],[0,75,0,80],[0,41,0,43],[0,45,0,56],[0,57,0,68]]}
["Climate Zone","Roof Constructions",null,null,"Above-Grade Exterior Wall Constructions",null,null,"Below-Grade Exterior Wall Constructions",null,null,"Exposed Floor Constructions",null,null,"Slab-On-Grade Floors",null,null,"Opaque Doors - Swinging",null,null,"Opaque Doors - Nonwwinging",null,null,null,"Roof Constructions",null,null,"Above-Grade Exterior Wall Constructions",null,null,"Below-Grade Exterior Wall Constructions",null,null,"Exposed Floor Constructions",null,null,"Slab-On-Grade Floors",null,null,"Opaque Doors - Swinging",null,null,"Opaque Doors - Nonswinging",null,null,null,"Vertical Glazing - Ufactor",null,null,null,null,null,null,null,null,null,null,null,"Vertical Glazing - SHGC",null,null,null,null,null,null,null,null,null,null,null,"Skylights - Ufactor",null,null,null,null,null,"Skylights - SHGC",null,null,null,null,null,null,null,null,null,null,"Table G3.1.1-1"]
[null,"Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated",null,"Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated",null,"Nonresidential 0%-10.0%","Residential 0%-10.0%","Semiheated 0%-10.0%","Nonresidential 10.1%-20.0%","Residential 10.1%-20.0%","Semiheated 10.1%-20.0%","Nonresidential 20.1%-30.0%","Residential 20.1%-30.0%","Semiheated 20.1%-30.0%","Nonresidential 30.1%-40.0%","Residential 30.1%-40.0%","Semiheated 30.1%-40.0%","Nonresidential 0%-10.0%","Residential 0%-10.0%","Semiheated 0%-10.0%","Nonresidential 10.1%-20.0%","Residential 10.1%-20.0%","Semiheated 10.1%-20.0%","Nonresidential 20.1%-30.0%","Residential 20.1%-30.0%","Semiheated 20.1%-30.0%","Nonresidential 30.1%-40.0%","Residential 30.1%-40.0%","Semiheated 30.1%-40.0%","Nonresidential 0%-2.0%","Nonresidential 2.1%+","Residential 0%-2.0%","Residential 2.1%+","Semiheated 0%-2.0%","Semiheated 2.1%+","Nonresidential 0%-2.0%","Nonresidential 2.1%+","Residential 0%-2.0%","Residential 2.1%+","Semiheated 0%-2.0%","Semiheated 2.1%+",null,null,null,null,null,"Building Area Type","Baseline Building Gross Above-Grade-Wall Area"]
["1A (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 1.282","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.352","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.350","steel-joist with a U-factor of 0.350","steel-joist with a U-factor of 0.350","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.70","U-factor of 0.70","U-factor of 0.70","U-factor of 1.450","U-factor of 1.450","U-factor of 1.450",null,6.3E-2,6.3E-2,1.282,0.124,0.124,0.35199999999999998,1.1399999999999999,1.1399999999999999,1.1399999999999999,0.35,0.35,0.35,0.73,0.73,0.73,0.7,0.7,0.7,1.45,1.45,1.45,null,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,0.25,0.25,"NR",0.25,0.25,"NR",0.25,0.25,"NR",0.25,0.25,"NR",1.36,1.36,1.36,1.36,1.36,1.36,0.36,0.19,0.19,0.19,"NR","NR",null,null,null,null,null,"Grocery Store",7.0000000000000007E-2]
["1A (SI)","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 7.28","steel-framed with a U-factor of 0.704","steel-framed with a U-factor of 0.704","steel-framed with a U-factor of 1.999","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 1.987","steel-joist with a U-factor of 1.987","steel-joist with a U-factor of 1.987","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 8.233","U-factor of 8.233",null,0.35799999999999998,0.35799999999999998,7.28,0.70399999999999996,0.70399999999999996,1.9990000000000001,6.4729999999999999,6.4729999999999999,6.4729999999999999,1.9870000000000001,1.9870000000000001,1.9870000000000001,1.264,1.264,1.264,3.9750000000000001,3.9750000000000001,3.9750000000000001,8.2330000000000005,8.2330000000000005,8.2330000000000005,null,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,0.25,0.25,"NR",0.25,0.25,"NR",0.25,0.25,"NR",0.25,0.25,"NR",7.72,7.72,7.72,7.72,7.72,7.72,0.36,0.19,0.19,0.19,"NR","NR",null,null,null,null,null,"Healthcare (outpatient)",0.21]
["1B (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 1.282","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.352","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.350","steel-joist with a U-factor of 0.350","steel-joist with a U-factor of 0.350","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.70","U-factor of 0.70","U-factor of 0.70","U-factor of 1.450","U-factor of 1.450","U-factor of 1.450",null,6.3E-2,6.3E-2,1.282,0.124,0.124,0.35199999999999998,1.1399999999999999,1.1399999999999999,1.1399999999999999,0.35,0.35,0.35,0.73,0.73,0.73,0.7,0.7,0.7,1.45,1.45,1.45,null,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,0.25,0.25,"NR",0.25,0.25,"NR",0.25,0.25,"NR",0.25,0.25,"NR",1.36,1.36,1.36,1.36,1.36,1.36,0.36,0.19,0.19,0.19,"NR","NR",null,null,null,null,null,"Hospital",0.27]
["1B (SI)","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 7.28","steel-framed with a U-factor of 0.704","steel-framed with a U-factor of 0.704","steel-framed with a U-factor of 1.999","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 1.987","steel-joist with a U-factor of 1.987","steel-joist with a U-factor of 1.987","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 8.233","U-factor of 8.233",null,0.35799999999999998,0.35799999999999998,7.28,0.70399999999999996,0.70399999999999996,1.9990000000000001,6.4729999999999999,6.4729999999999999,6.4729999999999999,1.9870000000000001,1.9870000000000001,1.9870000000000001,1.264,1.264,1.264,3.9750000000000001,3.9750000000000001,3.9750000000000001,8.2330000000000005,8.2330000000000005,8.2330000000000005,null,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,0.25,0.25,"NR",0.25,0.25,"NR",0.25,0.25,"NR",0.25,0.25,"NR",7.72,7.72,7.72,7.72,7.72,7.72,0.36,0.19,0.19,0.19,"NR","NR",null,null,null,null,null,"Hotel/motel (≤ 75 rooms)",0.24]
["2A (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.218","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.352","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.350","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.70","U-factor of 0.70","U-factor of 0.70","U-factor of 1.450","U-factor of 1.450","U-factor of 1.450",null,6.3E-2,6.3E-2,0.218,0.124,0.124,0.35199999999999998,1.1399999999999999,1.1399999999999999,1.1399999999999999,5.1999999999999998E-2,5.1999999999999998E-2,0.35,0.73,0.73,0.73,0.7,0.7,0.7,1.45,1.45,1.45,null,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,0.25,0.39,"NR",0.25,0.25,"NR",0.25,0.25,"NR",0.25,0.25,"NR",1.36,1.36,1.36,1.36,1.36,1.36,0.36,0.19,0.19,0.19,"NR","NR",null,null,null,null,null,"Hotel/motel (> 75 rooms)",0.34]
["2A (SI)","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 1.238","steel-framed with a U-factor of 0.704","steel-framed with a U-factor of 0.704","steel-framed with a U-factor of 1.999","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.295","steel-joist with a U-factor of 0.295","steel-joist with a U-factor of 1.987","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 8.233","U-factor of 8.233",null,0.35799999999999998,0.35799999999999998,1.238,0.70399999999999996,0.70399999999999996,1.9990000000000001,6.4729999999999999,6.4729999999999999,6.4729999999999999,0.29499999999999998,0.29499999999999998,1.9870000000000001,1.264,1.264,1.264,3.9750000000000001,3.9750000000000001,3.9750000000000001,8.2330000000000005,8.2330000000000005,8.2330000000000005,null,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,0.25,0.39,"NR",0.25,0.25,"NR",0.25,0.25,"NR",0.25,0.25,"NR",7.72,7.72,7.72,7.72,7.72,7.72,0.36,0.19,0.19,0.19,"NR","NR",null,null,null,null,null,"Office (≤ 5,000 sf)",0.19]
["2B (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.218","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.352","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.350","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.70","U-factor of 0.70","U-factor of 0.70","U-factor of 1.450","U-factor of 1.450","U-factor of 1.450",null,6.3E-2,6.3E-2,0.218,0.124,0.124,0.35199999999999998,1.1399999999999999,1.1399999999999999,1.1399999999999999,5.1999999999999998E-2,5.1999999999999998E-2,0.35,0.73,0.73,0.73,0.7,0.7,0.7,1.45,1.45,1.45,null,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,0.25,0.39,"NR",0.25,0.25,"NR",0.25,0.25,"NR",0.25,0.25,"NR",1.36,1.36,1.36,1.36,1.36,1.36,0.36,0.19,0.19,0.19,"NR","NR",null,null,null,null,null,"Office (5,000 to 50,000 sf)",0.31]
["2B (SI)","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 1.238","steel-framed with a U-factor of 0.704","steel-framed with a U-factor of 0.704","steel-framed with a U-factor of 1.999","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.295","steel-joist with a U-factor of 0.295","steel-joist with a U-factor of 1.987","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 8.233","U-factor of 8.233",null,0.35799999999999998,0.35799999999999998,1.238,0.70399999999999996,0.70399999999999996,1.9990000000000001,6.4729999999999999,6.4729999999999999,6.4729999999999999,0.29499999999999998,0.29499999999999998,1.9870000000000001,1.264,1.264,1.264,3.9750000000000001,3.9750000000000001,3.9750000000000001,8.2330000000000005,8.2330000000000005,8.2330000000000005,null,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,0.25,0.39,"NR",0.25,0.25,"NR",0.25,0.25,"NR",0.25,0.25,"NR",7.72,7.72,7.72,7.72,7.72,7.72,0.36,0.19,0.19,0.19,"NR","NR",null,null,null,null,null,"Office (>50,000 sf)",0.4]
["3A (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.218","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.352","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.70","U-factor of 0.70","U-factor of 0.70","U-factor of 1.450","U-factor of 0.50","U-factor of 1.450",null,6.3E-2,6.3E-2,0.218,0.124,8.4000000000000005E-2,0.35199999999999998,1.1399999999999999,1.1399999999999999,1.1399999999999999,5.1999999999999998E-2,5.1999999999999998E-2,6.9000000000000006E-2,0.73,0.73,0.73,0.7,0.7,0.7,1.45,0.5,1.45,null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.39,0.39,"NR",0.25,0.39,"NR",0.25,0.25,"NR",0.25,0.25,"NR",0.69,0.69,0.69,0.69,1.36,1.36,0.39,0.19,0.36,0.19,"NR","NR",null,null,null,null,null,"Restaurant (quick service)",0.34]
["3A (SI)","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 1.238","steel-framed with a U-factor of 0.704","steel-framed with a U-factor of 0.477","steel-framed with a U-factor of 1.999","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.295","steel-joist with a U-factor of 0.295","steel-joist with a U-factor of 0.392","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.35799999999999998,0.35799999999999998,1.238,0.70399999999999996,0.47699999999999998,1.9990000000000001,6.4729999999999999,6.4729999999999999,6.4729999999999999,0.29499999999999998,0.29499999999999998,0.39200000000000002,1.264,1.264,1.264,3.9750000000000001,3.9750000000000001,3.9750000000000001,8.2330000000000005,2.839,8.2330000000000005,null,3.24,3.24,6.92,3.24,3.24,6.92,3.24,3.24,6.92,3.24,3.24,6.92,0.39,0.39,"NR",0.25,0.39,"NR",0.25,0.25,"NR",0.25,0.25,"NR",3.9180000000000001,3.9180000000000001,3.9180000000000001,3.9180000000000001,7.7220000000000004,7.7220000000000004,0.39,0.19,0.36,0.19,"NR","NR",null,null,null,null,null,"Restaurant (full service)",0.24]
["3B (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.218","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.352","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.70","U-factor of 0.70","U-factor of 0.70","U-factor of 1.450","U-factor of 0.50","U-factor of 1.450",null,6.3E-2,6.3E-2,0.218,0.124,8.4000000000000005E-2,0.35199999999999998,1.1399999999999999,1.1399999999999999,1.1399999999999999,5.1999999999999998E-2,5.1999999999999998E-2,6.9000000000000006E-2,0.73,0.73,0.73,0.7,0.7,0.7,1.45,0.5,1.45,null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.39,0.39,"NR",0.25,0.39,"NR",0.25,0.25,"NR",0.25,0.25,"NR",0.69,0.69,0.69,0.69,1.36,1.36,0.39,0.19,0.36,0.19,"NR","NR",null,null,null,null,null,"Retail (stand alone)",0.11]
["3B (SI)","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 1.238","steel-framed with a U-factor of 0.704","steel-framed with a U-factor of 0.477","steel-framed with a U-factor of 1.999","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.295","steel-joist with a U-factor of 0.295","steel-joist with a U-factor of 0.392","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.35799999999999998,0.35799999999999998,1.238,0.70399999999999996,0.47699999999999998,1.9990000000000001,6.4729999999999999,6.4729999999999999,6.4729999999999999,0.29499999999999998,0.29499999999999998,0.39200000000000002,1.264,1.264,1.264,3.9750000000000001,3.9750000000000001,3.9750000000000001,8.2330000000000005,2.839,8.2330000000000005,null,3.24,3.24,6.92,3.24,3.24,6.92,3.24,3.24,6.92,3.24,3.24,6.92,0.39,0.39,"NR",0.25,0.39,"NR",0.25,0.25,"NR",0.25,0.25,"NR",3.9180000000000001,3.9180000000000001,3.9180000000000001,3.9180000000000001,7.7220000000000004,7.7220000000000004,0.39,0.19,0.36,0.19,"NR","NR",null,null,null,null,null,"Retail (strip mall)",0.2]
["3C (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.218","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.352","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.70","U-factor of 0.70","U-factor of 0.70","U-factor of 1.450","U-factor of 0.50","U-factor of 1.450",null,6.3E-2,6.3E-2,0.218,0.124,8.4000000000000005E-2,0.35199999999999998,1.1399999999999999,1.1399999999999999,1.1399999999999999,5.1999999999999998E-2,5.1999999999999998E-2,6.9000000000000006E-2,0.73,0.73,0.73,0.7,0.7,0.7,1.45,0.5,1.45,null,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,1.22,0.61,0.61,"NR",0.39,0.61,"NR",0.39,0.39,"NR",0.34,0.34,"NR",1.36,1.36,1.36,1.36,1.36,1.36,0.61,0.39,0.39,0.19,"NR","NR",null,null,null,null,null,"School (primary)",0.22]
["3C (SI)","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 1.238","steel-framed with a U-factor of 0.704","steel-framed with a U-factor of 0.477","steel-framed with a U-factor of 1.999","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.295","steel-joist with a U-factor of 0.295","steel-joist with a U-factor of 0.392","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.35799999999999998,0.35799999999999998,1.238,0.70399999999999996,0.47699999999999998,1.9990000000000001,6.4729999999999999,6.4729999999999999,6.4729999999999999,0.29499999999999998,0.29499999999999998,0.39200000000000002,1.264,1.264,1.264,3.9750000000000001,3.9750000000000001,3.9750000000000001,8.2330000000000005,2.839,8.2330000000000005,null,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,6.92,0.61,0.61,"NR",0.39,0.61,"NR",0.39,0.39,"NR",0.34,0.34,"NR",7.7220000000000004,7.7220000000000004,7.7220000000000004,7.7220000000000004,7.7220000000000004,7.7220000000000004,0.61,0.39,0.39,0.19,"NR","NR",null,null,null,null,null,"School (secondary or university)",0.22]
["4A (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.218","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,6.3E-2,6.3E-2,0.218,0.124,6.4000000000000001E-2,0.124,1.1399999999999999,1.1399999999999999,1.1399999999999999,5.1999999999999998E-2,3.7999999999999999E-2,6.9000000000000006E-2,0.73,0.73,0.73,0.7,0.7,0.7,1.45,0.5,1.45,null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.69,0.69,0.57999999999999996,0.57999999999999996,1.36,1.36,0.49,0.39,0.36,0.19,"NR","NR",null,null,null,null,null,"Warehouse (nonrefrigeratied)",0.06]
["4A (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 1.240","steel-framed with a U-factor of 0.705","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.36,0.36,1.24,0.70499999999999996,0.36499999999999999,0.70499999999999996,6.4729999999999999,6.4729999999999999,6.4729999999999999,0.29599999999999999,0.214,0.39,1.264,1.264,1.264,3.9750000000000001,3.9750000000000001,3.9750000000000001,8.2330000000000005,2.839,8.2330000000000005,null,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",3.92,3.92,3.29,3.29,7.72,7.72,0.49,0.39,0.36,0.19,"NR","NR",null,null,null,null,null,"Other",{"$f":"IF('General Information'!F17=\"\",\"-\",IF('General Information'!F17=\"Apartment\",0.3,0.4))","v":"-"}]
["4B (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.218","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,6.3E-2,6.3E-2,0.218,0.124,6.4000000000000001E-2,0.124,1.1399999999999999,1.1399999999999999,1.1399999999999999,5.1999999999999998E-2,3.7999999999999999E-2,6.9000000000000006E-2,0.73,0.73,0.73,0.7,0.7,0.7,1.45,0.5,1.45,null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.69,0.69,0.57999999999999996,0.57999999999999996,1.36,1.36,0.49,0.39,0.36,0.19,"NR","NR"]
["4B (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 1.240","steel-framed with a U-factor of 0.705","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.36,0.36,1.24,0.70499999999999996,0.36499999999999999,0.70499999999999996,6.4729999999999999,6.4729999999999999,6.4729999999999999,0.29599999999999999,0.214,0.39,1.264,1.264,1.264,3.9750000000000001,3.9750000000000001,3.9750000000000001,8.2330000000000005,2.839,8.2330000000000005,null,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",3.92,3.92,3.29,3.29,7.72,7.72,0.49,0.39,0.36,0.19,"NR","NR"]
["4C (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.218","steel-framed with a U-factor of 0.124","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,6.3E-2,6.3E-2,0.218,0.124,6.4000000000000001E-2,0.124,1.1399999999999999,1.1399999999999999,1.1399999999999999,5.1999999999999998E-2,3.7999999999999999E-2,6.9000000000000006E-2,0.73,0.73,0.73,0.7,0.7,0.7,1.45,0.5,1.45,null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.69,0.69,0.57999999999999996,0.57999999999999996,1.36,1.36,0.49,0.39,0.36,0.19,"NR","NR"]
["4C (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 1.240","steel-framed with a U-factor of 0.705","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.36,0.36,1.24,0.70499999999999996,0.36499999999999999,0.70499999999999996,6.4729999999999999,6.4729999999999999,6.4729999999999999,0.29599999999999999,0.214,0.39,1.264,1.264,1.264,3.9750000000000001,3.9750000000000001,3.9750000000000001,8.2330000000000005,2.839,8.2330000000000005,null,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",3.92,3.92,3.29,3.29,7.72,7.72,0.49,0.39,0.36,0.19,"NR","NR"]
["5A (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,6.3E-2,6.3E-2,0.17299999999999999,8.4000000000000005E-2,6.4000000000000001E-2,0.124,1.1399999999999999,1.1399999999999999,1.1399999999999999,5.1999999999999998E-2,3.7999999999999999E-2,6.9000000000000006E-2,0.73,0.73,0.73,0.7,0.7,0.7,1.45,0.5,1.45,null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.69,0.69,0.69,0.69,1.36,1.36,0.49,0.39,0.49,0.39,"NR","NR"]
["5A (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.36,0.36,0.98199999999999998,0.47899999999999998,0.36499999999999999,0.70499999999999996,6.4729999999999999,6.4729999999999999,6.4729999999999999,0.29599999999999999,0.214,0.39,1.264,1.264,1.264,3.9750000000000001,3.9750000000000001,3.9750000000000001,8.2330000000000005,2.839,8.2330000000000005,null,3.24,3.24,"NR",3.24,3.24,"NR",3.24,3.24,"NR",3.24,3.24,"NR",0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",3.9180000000000001,3.9180000000000001,3.9180000000000001,3.9180000000000001,7.7220000000000004,7.7220000000000004,0.49,0.39,0.49,0.39,"NR","NR"]
["5B (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,6.3E-2,6.3E-2,0.17299999999999999,8.4000000000000005E-2,6.4000000000000001E-2,0.124,1.1399999999999999,1.1399999999999999,1.1399999999999999,5.1999999999999998E-2,3.7999999999999999E-2,6.9000000000000006E-2,0.73,0.73,0.73,0.7,0.7,0.7,1.45,0.5,1.45,null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.69,0.69,0.69,0.69,1.36,1.36,0.49,0.39,0.49,0.39,"NR","NR"]
["5B (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.36,0.36,0.98199999999999998,0.47899999999999998,0.36499999999999999,0.70499999999999996,6.4729999999999999,6.4729999999999999,6.4729999999999999,0.29599999999999999,0.214,0.39,1.264,1.264,1.264,3.9750000000000001,3.9750000000000001,3.9750000000000001,8.2330000000000005,2.839,8.2330000000000005,null,3.24,3.24,"NR",3.24,3.24,"NR",3.24,3.24,"NR",3.24,3.24,"NR",0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",3.9180000000000001,3.9180000000000001,3.9180000000000001,3.9180000000000001,7.7220000000000004,7.7220000000000004,0.49,0.39,0.49,0.39,"NR","NR"]
["5C (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,6.3E-2,6.3E-2,0.17299999999999999,8.4000000000000005E-2,6.4000000000000001E-2,0.124,1.1399999999999999,1.1399999999999999,1.1399999999999999,5.1999999999999998E-2,3.7999999999999999E-2,6.9000000000000006E-2,0.73,0.73,0.73,0.7,0.7,0.7,1.45,0.5,1.45,null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.69,0.69,0.69,0.69,1.36,1.36,0.49,0.39,0.49,0.39,"NR","NR"]
["5C (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.36,0.36,0.98199999999999998,0.47899999999999998,0.36499999999999999,0.70499999999999996,6.4729999999999999,6.4729999999999999,6.4729999999999999,0.29599999999999999,0.214,0.39,1.264,1.264,1.264,3.9750000000000001,3.9750000000000001,3.9750000000000001,8.2330000000000005,2.839,8.2330000000000005,null,3.24,3.24,"NR",3.24,3.24,"NR",3.24,3.24,"NR",3.24,3.24,"NR",0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",3.9180000000000001,3.9180000000000001,3.9180000000000001,3.9180000000000001,7.7220000000000004,7.7220000000000004,0.49,0.39,0.49,0.39,"NR","NR"]
["6A (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,6.3E-2,6.3E-2,0.17299999999999999,8.4000000000000005E-2,6.4000000000000001E-2,0.124,1.1399999999999999,0.11899999999999999,1.1399999999999999,3.7999999999999999E-2,3.7999999999999999E-2,6.9000000000000006E-2,0.73,0.73,0.73,0.7,0.5,0.7,0.5,0.5,1.45,null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.69,0.69,0.57999999999999996,0.57999999999999996,1.36,1.36,0.49,0.49,0.49,0.39,"NR","NR"]
["6A (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.260","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,0.36,0.36,0.98199999999999998,0.47899999999999998,0.36499999999999999,0.70499999999999996,6.4729999999999999,0.67800000000000005,6.4729999999999999,0.214,0.214,0.39,1.264,1.26,1.264,3.9750000000000001,2.839,3.9750000000000001,2.839,2.839,8.2330000000000005,null,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",3.9180000000000001,3.9180000000000001,3.2930000000000001,3.2930000000000001,7.7220000000000004,7.7220000000000004,0.49,0.49,0.49,0.39,"NR","NR"]
["6B (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,6.3E-2,6.3E-2,0.17299999999999999,8.4000000000000005E-2,6.4000000000000001E-2,0.124,1.1399999999999999,0.11899999999999999,1.1399999999999999,3.7999999999999999E-2,3.7999999999999999E-2,6.9000000000000006E-2,0.73,0.73,0.73,0.7,0.5,0.7,0.5,0.5,1.45,null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.69,0.69,0.57999999999999996,0.57999999999999996,1.36,1.36,0.49,0.49,0.49,0.39,"NR","NR"]
["6B (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.260","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,0.36,0.36,0.98199999999999998,0.47899999999999998,0.36499999999999999,0.70499999999999996,6.4729999999999999,0.67800000000000005,6.4729999999999999,0.214,0.214,0.39,1.264,1.26,1.264,3.9750000000000001,2.839,3.9750000000000001,2.839,2.839,8.2330000000000005,null,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",3.9180000000000001,3.9180000000000001,3.2930000000000001,3.2930000000000001,7.7220000000000004,7.7220000000000004,0.49,0.49,0.49,0.39,"NR","NR"]
["7A (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.052","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.540","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.70","U-factor of 0.50","U-factor of 0.70","U-factor of 0.50","U-factor of 0.50","U-factor of 1.450",null,6.3E-2,6.3E-2,0.17299999999999999,6.4000000000000001E-2,6.4000000000000001E-2,0.124,0.11899999999999999,0.11899999999999999,1.1399999999999999,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,0.73,0.54,0.73,0.7,0.5,0.7,0.5,0.5,1.45,null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.49,0.49,"NR",0.49,0.49,"NR",0.49,0.49,"NR",0.49,0.49,"NR",0.69,0.69,0.69,0.69,1.36,1.36,0.68,0.64,0.64,0.64,"NR","NR"]
["7A (SI)","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.363","steel-framed with a U-factor of 0.363","steel-framed with a U-factor of 0.704","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.676","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.676","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.295","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 0.935","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,0.35799999999999998,0.35799999999999998,0.98199999999999998,0.36299999999999999,0.36299999999999999,0.70399999999999996,0.67600000000000005,0.67600000000000005,6.4729999999999999,0.216,0.216,0.29499999999999998,1.264,0.93500000000000005,1.264,3.9750000000000001,2.839,3.9750000000000001,2.839,2.839,8.2330000000000005,null,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,0.49,0.49,"NR",0.49,0.49,"NR",0.49,0.49,"NR",0.49,0.49,"NR",3.9180000000000001,3.9180000000000001,3.9180000000000001,3.9180000000000001,7.7220000000000004,7.7220000000000004,0.68,0.64,0.64,0.64,"NR","NR"]
["7B (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.052","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.540","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.70","U-factor of 0.50","U-factor of 0.70","U-factor of 0.50","U-factor of 0.50","U-factor of 1.450",null,6.3E-2,6.3E-2,0.17299999999999999,6.4000000000000001E-2,6.4000000000000001E-2,0.124,0.11899999999999999,0.11899999999999999,1.1399999999999999,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,0.73,0.54,0.73,0.7,0.5,0.7,0.5,0.5,1.45,null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.49,0.49,"NR",0.49,0.49,"NR",0.49,0.49,"NR",0.49,0.49,"NR",0.69,0.69,0.69,0.69,1.36,1.36,0.68,0.64,0.64,0.64,"NR","NR"]
["7B (SI)","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 0.358","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.363","steel-framed with a U-factor of 0.363","steel-framed with a U-factor of 0.704","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.676","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.676","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.295","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 0.935","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,0.35799999999999998,0.35799999999999998,0.98199999999999998,0.36299999999999999,0.36299999999999999,0.70399999999999996,0.67600000000000005,0.67600000000000005,6.4729999999999999,0.216,0.216,0.29499999999999998,1.264,0.93500000000000005,1.264,3.9750000000000001,2.839,3.9750000000000001,2.839,2.839,8.2330000000000005,null,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,0.49,0.49,"NR",0.49,0.49,"NR",0.49,0.49,"NR",0.49,0.49,"NR",3.9180000000000001,3.9180000000000001,3.9180000000000001,3.9180000000000001,7.7220000000000004,7.7220000000000004,0.68,0.64,0.64,0.64,"NR","NR"]
["8 (IP)","Insulation entirely above deck with a U-factor of 0.048","Insulation entirely above deck with a U-factor of 0.048","Insulation entirely above deck with a U-factor of 0.093","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.055","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.032","steel-joist with a U-factor of 0.052","6\" concrete slabs with no insulation with an F-factor of 0.540","6\" concrete slabs with no insulation with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.50","U-factor of 0.50","U-factor of 0.70","U-factor of 0.50","U-factor of 0.50","U-factor of 1.450",null,4.8000000000000001E-2,4.8000000000000001E-2,9.2999999999999999E-2,6.4000000000000001E-2,5.5E-2,0.124,0.11899999999999999,0.11899999999999999,1.1399999999999999,3.7999999999999999E-2,3.2000000000000001E-2,5.1999999999999998E-2,0.54,0.52,0.73,0.5,0.5,0.7,0.5,0.5,1.45,null,0.46,0.46,1.22,0.46,0.46,1.22,0.46,0.46,1.22,0.46,0.46,1.22,"NR","NR","NR","NR","NR","NR","NR","NR","NR","NR","NR","NR",0.57999999999999996,0.57999999999999996,0.57999999999999996,0.57999999999999996,0.81,0.81,"NR","NR","NR","NR","NR","NR"]
["8 (SI)","Insulation entirely above deck with a U-factor of 0.273","Insulation entirely above deck with a U-factor of 0.273","Insulation entirely above deck with a U-factor of 0.528","steel-framed with a U-factor of 0.363","steel-framed with a U-factor of 0.312","steel-framed with a U-factor of 0.704","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.676","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.676","205mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.182","steel-joist with a U-factor of 0.295","150 mm concrete slabs with no insulation with an F-factor of 0.935","150 mm concrete slabs with no insulation with an F-factor of 0.9","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.839","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,0.27300000000000002,0.27300000000000002,0.52800000000000002,0.36299999999999999,0.312,0.70399999999999996,0.67600000000000005,0.67600000000000005,6.4729999999999999,0.216,0.182,0.29499999999999998,0.93500000000000005,0.90039999999999998,1.264,2.839,2.8391000000000002,3.9750000000000001,2.839,2.8391000000000002,8.2330000000000005,null,2.61,2.61,6.93,2.61,2.61,6.93,2.61,2.61,6.93,2.61,2.61,6.93,"NR","NR","NR","NR","NR","NR","NR","NR","NR","NR","NR","NR",3.2930000000000001,3.2930000000000001,3.2930000000000001,3.2930000000000001,4.5990000000000002,4.5990000000000002,"NR","NR","NR","NR","NR","NR"]

{"sheet":"Envelope Lookup 90.1-2007","index":12,"n_rows":38,"n_cols":92,"rows_kept":38,"cut":false,"hidden":true,"merged":[[0,75,0,80],[0,35,0,37],[0,38,0,40],[0,41,0,43],[0,45,0,56],[0,57,0,68],[0,69,0,74],[0,32,0,34],[0,1,0,3],[0,4,0,6],[0,7,0,9],[0,10,0,12],[0,13,0,15],[0,16,0,18],[0,19,0,21],[0,23,0,25],[0,26,0,28],[0,29,0,31]]}
["*** THESE ARE NOT 2007 VALUES. THESE TABLES ARE HERE AS A PLACEHOLDER.","Roof Constructions",null,null,"Above-Grade Exterior Wall Constructions",null,null,"Below-Grade Exterior Wall Constructions",null,null,"Exposed Floor Constructions",null,null,"Slab-On-Grade Floors",null,null,"Opaque Doors - Swinging",null,null,"Opaque Doors - Nonwwinging",null,null,null,"Roof Constructions",null,null,"Above-Grade Exterior Wall Constructions",null,null,"Below-Grade Exterior Wall Constructions",null,null,"Exposed Floor Constructions",null,null,"Slab-On-Grade Floors",null,null,"Opaque Doors - Swinging",null,null,"Opaque Doors - Nonswinging",null,null,null,"Vertical Glazing - Ufactor",null,null,null,null,null,null,null,null,null,null,null,"Vertical Glazing - SHGC",null,null,null,null,null,null,null,null,null,null,null,"Skylights - Ufactor",null,null,null,null,null,"Skylights - SHGC"]
["Climate Zone","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated",null,"Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated",null,"Nonresidential 0%-10.0%","Residential 0%-10.0%","Semiheated 0%-10.0%","Nonresidential 10.1%-20.0%","Residential 10.1%-20.0%","Semiheated 10.1%-20.0%","Nonresidential 20.1%-30.0%","Residential 20.1%-30.0%","Semiheated 20.1%-30.0%","Nonresidential 30.1%-40.0%","Residential 30.1%-40.0%","Semiheated 30.1%-40.0%","Nonresidential 0%-10.0%","Residential 0%-10.0%","Semiheated 0%-10.0%","Nonresidential 10.1%-20.0%","Residential 10.1%-20.0%","Semiheated 10.1%-20.0%","Nonresidential 20.1%-30.0%","Residential 20.1%-30.0%","Semiheated 20.1%-30.0%","Nonresidential 30.1%-40.0%","Residential 30.1%-40.0%","Semiheated 30.1%-40.0%","Nonresidential 0%-2.0%","Nonresidential 2.1%+","Residential 0%-2.0%","Residential 2.1%+","Seimiheated 0%-2.0%","Seimiheated 2.1%+","Nonresidential 0%-2.0%","Nonresidential 2.1%+","Residential 0%-2.0%","Residential 2.1%+","Seimiheated 0%-2.0%","Seimiheated 2.1%+",null,null,null,null,null,null,null,"Climate Zone","Nonresidential","Residential","Semiheated"]
["1A (IP)","R-15 insulation entirely above deck with a U-factor of 0.063","R-20 insulation entirely above deck with a U-factor of 0.048","R-3.8 insulation entirely above deck with a U-factor of 0.218","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with no insulation with a U-factor of 0.352","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with no insulation with a U-factor of 0.350","steel-joist with no insulation with a U-factor of 0.350","steel-joist with no insulation with a U-factor of 0.350","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 1.450","U-factor of 1.450",null,"U-0.063","U-0.048","U-0.218","U-0.124","U-0.124","U-0.352","C-1.140","C-1.140","C-1.140","U-0.350","U-0.350","U-0.350","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-1.450","U-1.450",null,1.2,1.2,1.2,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.98,1.98,1.98,1.98,1.98,1.98,0.36,0.19,0.34,0.27,0.36,0.19,null,null,null,null,null,null,"need to be updated, currently have CZ 4 values",1,"Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["1A (SI)","R-2.6 c.i. insulation entirely above deck with a U-factor of 0.360","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.7 c.i. insulation entirely above deck with a U-factor of 1.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with no insulation with a U-factor of 1.998","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with no insulation with a U-factor of 1.986","steel-joist with no insulation with a U-factor of 1.986","steel-joist with no insulation with a U-factor of 1.986","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 8.233","U-factor of 8.233",null,"U-0.360","U-0.273","U-1.240","U-0.705","U-0.705","U-1.998","C-6.473","C-6.473","C-6.473","U-1.986","U-1.986","U-1.986","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-8.233","U-8.233",null,6.81,6.81,6.81,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,11.24,11.24,11.24,11.24,11.24,11.24,0.36,0.19,0.34,0.27,0.36,0.19,null,null,null,null,null,null,"need to be updated, currently have CZ 4 values",2,"Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["1B (IP)","R-15 insulation entirely above deck with a U-factor of 0.063","R-20 insulation entirely above deck with a U-factor of 0.048","R-3.8 insulation entirely above deck with a U-factor of 0.218","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with no insulation with a U-factor of 0.352","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with no insulation with a U-factor of 0.350","steel-joist with no insulation with a U-factor of 0.350","steel-joist with no insulation with a U-factor of 0.350","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 1.450","U-factor of 1.450",null,"U-0.063","U-0.048","U-0.218","U-0.124","U-0.124","U-0.352","C-1.140","C-1.140","C-1.140","U-0.350","U-0.350","U-0.350","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-1.450","U-1.450",null,1.2,1.2,1.2,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.98,1.98,1.98,1.98,1.98,1.98,0.36,0.19,0.34,0.27,0.36,0.19,null,null,null,null,null,null,"need to be updated, currently have CZ 4 values",3,"Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["1B (SI)","R-2.6 c.i. insulation entirely above deck with a U-factor of 0.360","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.7 c.i. insulation entirely above deck with a U-factor of 1.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with no insulation with a U-factor of 1.998","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with no insulation with a U-factor of 1.986","steel-joist with no insulation with a U-factor of 1.986","steel-joist with no insulation with a U-factor of 1.986","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 8.233","U-factor of 8.233",null,"U-0.360","U-0.273","U-1.240","U-0.705","U-0.705","U-1.998","C-6.473","C-6.473","C-6.473","U-1.986","U-1.986","U-1.986","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-8.233","U-8.233",null,6.81,6.81,6.81,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,11.24,11.24,11.24,11.24,11.24,11.24,0.36,0.19,0.34,0.27,0.36,0.19,null,null,null,null,null,null,null,4,"Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["2A (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-3.8 insulation entirely above deck with a U-factor of 0.218","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.218","U-0.124","U-0.064","U-0.124","C-1.140","C-1.140","C-1.140","U-0.052","U-0.052","U-0.069","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-0.500","U-1.450",null,0.75,0.7,1.1000000000000001,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.98,1.98,1.98,1.98,1.98,1.98,0.36,0.19,0.39,0.34,0.36,0.19,null,null,null,null,null,null,null,5,"Nonmetal framing, all: U-0.32; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.32; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.45; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.62; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.70; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["2A (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.7 c.i. insulation entirely above deck with a U-factor of 1.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-1.240","U-0.705","U-0.365","U-0.705","C-6.473","C-6.473","C-6.473","U-0.296","U-0.296","U-0.390","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-2.839","U-8.233",null,4.26,3.97,6.25,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,11.24,11.24,11.24,11.24,11.24,11.24,0.36,0.19,0.39,0.34,0.36,0.19,null,null,null,null,null,null,"need to be updated, currently have CZ 4 values",6,"Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["2B (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-3.8 insulation entirely above deck with a U-factor of 0.218","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.218","U-0.124","U-0.064","U-0.124","C-1.140","C-1.140","C-1.140","U-0.052","U-0.052","U-0.069","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-0.500","U-1.450",null,0.75,0.7,1.1000000000000001,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.98,1.98,1.98,1.98,1.98,1.98,0.36,0.19,0.39,0.34,0.36,0.19,null,null,null,null,null,null,"need to be updated, currently have CZ 4 values",7,"Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["2B (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.7 c.i. insulation entirely above deck with a U-factor of 1.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-1.240","U-0.705","U-0.365","U-0.705","C-6.473","C-6.473","C-6.473","U-0.296","U-0.296","U-0.390","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-2.839","U-8.233",null,4.26,3.97,6.25,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,11.24,11.24,11.24,11.24,11.24,11.24,0.36,0.19,0.39,0.34,0.36,0.19,null,null,null,null,null,null,"need to be updated, currently have CZ 4 values",8,"Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["3A (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-5.0 insulation entirely above deck with a U-factor of 0.173","steel-framed with R-13 cavity and R-3.8 continuous insulation with a U-factor of 0.084","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.173","U-0.084","U-0.064","U-0.124","C-1.140","C-1.140","C-1.140","U-0.052","U-0.052","U-0.069","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-0.500","U-1.450",null,0.65,0.6,0.9,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.17,1.17,1.17,1.17,1.17,1.17,0.39,0.19,0.65,0.34,0.39,0.19]
["3A (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.9 c.i. insulation entirely above deck with a U-factor of 0.982","steel-framed with R-2.3 cavity and R-0.7 continuous insulation with a U-factor of 0.479","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-0.982","U-0.479","U-0.365","U-0.705","C-6.473","C-6.473","C-6.473","U-0.296","U-0.296","U-0.390","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-2.839","U-8.233",null,3.69,3.41,5.1100000000000003,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,6.64,6.64,6.64,6.64,6.64,6.64,0.39,0.19,0.65,0.34,0.39,0.19]
["3B (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-5.0 insulation entirely above deck with a U-factor of 0.173","steel-framed with R-13 cavity and R-3.8 continuous insulation with a U-factor of 0.084","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.173","U-0.084","U-0.064","U-0.124","C-1.140","C-1.140","C-1.140","U-0.052","U-0.052","U-0.069","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-0.500","U-1.450",null,0.65,0.6,0.9,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.17,1.17,1.17,1.17,1.17,1.17,0.39,0.19,0.65,0.34,0.39,0.19]
["3B (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.9 c.i. insulation entirely above deck with a U-factor of 0.982","steel-framed with R-2.3 cavity and R-0.7 continuous insulation with a U-factor of 0.479","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-0.982","U-0.479","U-0.365","U-0.705","C-6.473","C-6.473","C-6.473","U-0.296","U-0.296","U-0.390","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-2.839","U-8.233",null,3.69,3.41,5.1100000000000003,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,6.64,6.64,6.64,6.64,6.64,6.64,0.39,0.19,0.65,0.34,0.39,0.19]
["3C (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-5.0 insulation entirely above deck with a U-factor of 0.173","steel-framed with R-13 cavity and R-3.8 continuous insulation with a U-factor of 0.084","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.173","U-0.084","U-0.064","U-0.124","C-1.140","C-1.140","C-1.140","U-0.052","U-0.052","U-0.069","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-0.500","U-1.450",null,0.65,0.6,0.9,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.17,1.17,1.17,1.17,1.17,1.17,0.39,0.19,0.65,0.34,0.39,0.19]
["3C (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.9 c.i. insulation entirely above deck with a U-factor of 0.982","steel-framed with R-2.3 cavity and R-0.7 continuous insulation with a U-factor of 0.479","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-0.982","U-0.479","U-0.365","U-0.705","C-6.473","C-6.473","C-6.473","U-0.296","U-0.296","U-0.390","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-2.839","U-8.233",null,3.69,3.41,5.1100000000000003,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,6.64,6.64,6.64,6.64,6.64,6.64,0.39,0.19,0.65,0.34,0.39,0.19]
["4A (IP)","R-30 insulation entirely above deck with a U-factor of 0.032","R-30 insulation entirely above deck with a U-factor of 0.032","R-10 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with  R-15 insulation for 24 in.  with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,3.2000000000000001E-2,3.2000000000000001E-2,9.2999999999999999E-2,6.4000000000000001E-2,6.4000000000000001E-2,0.124,0.11899999999999999,9.1999999999999998E-2,1.1399999999999999,3.7999999999999999E-2,3.7999999999999999E-2,0.52,0.52,0.52,0.73,0.5,0.5,0.7,0.5,0.5,1.45,null,0.42,0.42,0.73,0.42,0.42,0.73,0.42,0.42,0.73,0.42,0.42,0.73,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.5,0.5,0.5,0.5,1.1499999999999999,1.1499999999999999,0.4,0.4,0.4,0.4,"NR","NR"]
["4A (SI)","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.529","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.677","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.523","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.84","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.296","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.844","U-factor of 2.844","U-factor of 3.981","U-factor of 2.844","U-factor of 2.844","U-factor of 8.247",null,0.182,0.182,0.52900000000000003,0.36399999999999999,0.36399999999999999,0.70499999999999996,0.66700000000000004,0.52300000000000002,6.484,0.216,0.216,0.29599999999999999,0.9,0.9,1.264,2.8439999999999999,2.8439999999999999,3.9809999999999999,2.8439999999999999,2.8439999999999999,8.2469999999999999,null,2.38,2.38,4.1399999999999997,2.38,2.38,4.1399999999999997,2.38,2.38,4.1399999999999997,2.38,2.38,4.1399999999999997,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",2.84,2.84,2.84,2.84,6.53,6.53,0.4,0.4,0.4,0.4,"NR","NR"]
["4B (IP)","R-30 insulation entirely above deck with a U-factor of 0.032","R-30 insulation entirely above deck with a U-factor of 0.032","R-10 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with  R-15 insulation for 24 in.  with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,3.2000000000000001E-2,3.2000000000000001E-2,9.2999999999999999E-2,6.4000000000000001E-2,6.4000000000000001E-2,0.124,0.11899999999999999,9.1999999999999998E-2,1.1399999999999999,3.7999999999999999E-2,3.7999999999999999E-2,0.52,0.52,0.52,0.73,0.5,0.5,0.7,0.5,0.5,1.45,null,0.42,0.42,0.73,0.42,0.42,0.73,0.42,0.42,0.73,0.42,0.42,0.73,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.5,0.5,0.5,0.5,1.1499999999999999,1.1499999999999999,0.4,0.4,0.4,0.4,"NR","NR"]
["4B (SI)","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.529","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.677","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.523","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.84","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.296","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.844","U-factor of 2.844","U-factor of 3.981","U-factor of 2.844","U-factor of 2.844","U-factor of 8.247",null,0.182,0.182,0.52900000000000003,0.36399999999999999,0.36399999999999999,0.70499999999999996,0.66700000000000004,0.52300000000000002,6.484,0.216,0.216,0.29599999999999999,0.9,0.9,1.264,2.8439999999999999,2.8439999999999999,3.9809999999999999,2.8439999999999999,2.8439999999999999,8.2469999999999999,null,2.38,2.38,4.1399999999999997,2.38,2.38,4.1399999999999997,2.38,2.38,4.1399999999999997,2.38,2.38,4.1399999999999997,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",2.84,2.84,2.84,2.84,6.53,6.53,0.4,0.4,0.4,0.4,"NR","NR"]
["4C (IP)","R-30 insulation entirely above deck with a U-factor of 0.032","R-30 insulation entirely above deck with a U-factor of 0.032","R-10 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with  R-15 insulation for 24 in.  with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,3.2000000000000001E-2,3.2000000000000001E-2,9.2999999999999999E-2,6.4000000000000001E-2,6.4000000000000001E-2,0.124,0.11899999999999999,9.1999999999999998E-2,1.1399999999999999,3.7999999999999999E-2,3.7999999999999999E-2,0.52,0.52,0.52,0.73,0.5,0.5,0.7,0.5,0.5,1.45,null,0.42,0.42,0.73,0.42,0.42,0.73,0.42,0.42,0.73,0.42,0.42,0.73,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.5,0.5,0.5,0.5,1.1499999999999999,1.1499999999999999,0.4,0.4,0.4,0.4,"NR","NR"]
["4C (SI)","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.529","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.677","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.523","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.84","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.296","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.844","U-factor of 2.844","U-factor of 3.981","U-factor of 2.844","U-factor of 2.844","U-factor of 8.247",null,0.182,0.182,0.52900000000000003,0.36399999999999999,0.36399999999999999,0.70499999999999996,0.66700000000000004,0.52300000000000002,6.484,0.216,0.216,0.29599999999999999,0.9,0.9,1.264,2.8439999999999999,2.8439999999999999,3.9809999999999999,2.8439999999999999,2.8439999999999999,8.2469999999999999,null,2.38,2.38,4.1399999999999997,2.38,2.38,4.1399999999999997,2.38,2.38,4.1399999999999997,2.38,2.38,4.1399999999999997,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",2.84,2.84,2.84,2.84,6.53,6.53,0.4,0.4,0.4,0.4,"NR","NR"]
["5A (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,"U-0.063","U-0.063","U-0.173","U-0.084","U-0.064","U-0.124","C-1.140","C-1.140","C-1.140","U-0.052","U-0.038","U-0.069","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-0.500","U-1.450",null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",1.17,1.17,1.17,1.17,1.17,1.17,0.49,0.39,0.77,0.62,0.49,0.39]
["5A (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,"U-0.360","U-0.360","U-0.982","U-0.479","U-0.365","U-0.705","C-6.473","C-6.473","C-6.473","U-0.296","U-0.214","U-0.390","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-2.839","U-8.233",null,3.24,3.24,"NR",3.24,3.24,"NR",3.24,3.24,"NR",3.24,3.24,"NR",0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",6.64,6.64,6.64,6.64,6.64,6.64,0.49,0.39,0.77,0.62,0.49,0.39]
["5B (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,"U-0.063","U-0.063","U-0.173","U-0.084","U-0.064","U-0.124","C-1.140","C-1.140","C-1.140","U-0.052","U-0.038","U-0.069","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-0.500","U-1.450",null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",1.17,1.17,1.17,1.17,1.17,1.17,0.49,0.39,0.77,0.62,0.49,0.39]
["5B (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,"U-0.360","U-0.360","U-0.982","U-0.479","U-0.365","U-0.705","C-6.473","C-6.473","C-6.473","U-0.296","U-0.214","U-0.390","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-2.839","U-8.233",null,3.24,3.24,"NR",3.24,3.24,"NR",3.24,3.24,"NR",3.24,3.24,"NR",0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",6.64,6.64,6.64,6.64,6.64,6.64,0.49,0.39,0.77,0.62,0.49,0.39]
["5C (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,"U-0.063","U-0.063","U-0.173","U-0.084","U-0.064","U-0.124","C-1.140","C-1.140","C-1.140","U-0.052","U-0.038","U-0.069","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-0.500","U-1.450",null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",1.17,1.17,1.17,1.17,1.17,1.17,0.49,0.39,0.77,0.62,0.49,0.39]
["5C (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,"U-0.360","U-0.360","U-0.982","U-0.479","U-0.365","U-0.705","C-6.473","C-6.473","C-6.473","U-0.296","U-0.214","U-0.390","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-2.839","U-8.233",null,3.24,3.24,"NR",3.24,3.24,"NR",3.24,3.24,"NR",3.24,3.24,"NR",0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",6.64,6.64,6.64,6.64,6.64,6.64,0.49,0.39,0.77,0.62,0.49,0.39]
["6A (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,"U-0.063","U-0.063","U-0.173","U-0.084","U-0.064","U-0.124","C-1.140","C-0.119","C-1.140","U-0.038","U-0.038","U-0.069","F-0.730","F-0.730","F-0.730","U-0.700","U-0.500","U-0.700","U-0.500","U-0.500","U-1.450",null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",1.17,1.17,1.17,1.17,1.17,1.17,0.49,0.49,0.71,0.57999999999999996,0.49,0.49]
["6A (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.260","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,"U-0.360","U-0.360","U-0.982","U-0.479","U-0.365","U-0.705","C-6.473","C-0.678","C-6.473","U-0.214","U-0.214","U-0.390","F-1.264","F-1.260","F-1.264","U-3.975","U-2.839","U-3.975","U-2.839","U-2.839","U-8.233",null,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",6.64,6.64,6.64,6.64,6.64,6.64,0.49,0.49,0.71,0.57999999999999996,0.49,0.49]
["6B (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,"U-0.063","U-0.063","U-0.173","U-0.084","U-0.064","U-0.124","C-1.140","C-0.119","C-1.140","U-0.038","U-0.038","U-0.069","F-0.730","F-0.730","F-0.730","U-0.700","U-0.500","U-0.700","U-0.500","U-0.500","U-1.450",null,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.56999999999999995,0.56999999999999995,1.22,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",1.17,1.17,1.17,1.17,1.17,1.17,0.49,0.49,0.71,0.57999999999999996,0.49,0.49]
["6B (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.260","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,"U-0.360","U-0.360","U-0.982","U-0.479","U-0.365","U-0.705","C-6.473","C-0.678","C-6.473","U-0.214","U-0.214","U-0.390","F-1.264","F-1.260","F-1.264","U-3.975","U-2.839","U-3.975","U-2.839","U-2.839","U-8.233",null,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,3.24,3.24,6.93,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",6.64,6.64,6.64,6.64,6.64,6.64,0.49,0.49,0.71,0.57999999999999996,0.49,0.49]
["7A (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-10.0 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-15.6 continuous insulation with a U-factor of 0.042","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10.0 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-38 insulation with a U-factor of 0.032","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.093","U-0.064","U-0.042","U-0.124","C-0.119","C-0.092","C-1.140","U-0.038","U-0.032","U- 0.052","F-0.520","F-0.520","F-0.730","U-0.500","U-0.500","U-0.700","U-0.500","U-0.500","U-1.450",null,0.35,0.4,0.8,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,1.17,1.17,1.17,1.17,1.17,1.17,0.68,0.64,0.77,0.71,0.68,0.64]
["7A (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-1.8 insulation entirely above deck with a U-factor of 0.527","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity and R-2.7 continuous insulation with a U-factor of 0.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and R-1.3 continuous insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and R-1.8 continuous insulation with a C-factor of 0.522","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-5.3 insulation with a U-factor of 0.214","steel-joist with R-6.7 insulation with a U-factor of 0.183","steel-joist with R-3.3 insulation with a U-factor of 0.296","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.839","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-0.527","U-0.365","U-0.240","U-0.705","C-0.678","C-0.522","C-6.473","U-0.214","U-0.183","U- 0.296","F-0.900","F-0.900","F-1.264","U-2.839","U-2.839","U-3.975","U-2.839","U-2.839","U-8.233",null,0.35,0.4,0.8,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,6.64,6.64,6.64,6.64,6.64,6.64,0.68,0.64,0.77,0.71,0.68,0.64]
["7B (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-10.0 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-15.6 continuous insulation with a U-factor of 0.042","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10.0 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-38 insulation with a U-factor of 0.032","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.093","U-0.064","U-0.042","U-0.124","C-0.119","C-0.092","C-1.140","U-0.038","U-0.032","U- 0.052","F-0.520","F-0.520","F-0.730","U-0.500","U-0.500","U-0.700","U-0.500","U-0.500","U-1.450",null,0.35,0.4,0.8,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,1.17,1.17,1.17,1.17,1.17,1.17,0.68,0.64,0.77,0.71,0.68,0.64]
["7B (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-1.8 insulation entirely above deck with a U-factor of 0.527","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity and R-2.7 continuous insulation with a U-factor of 0.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and R-1.3 continuous insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and R-1.8 continuous insulation with a C-factor of 0.522","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-5.3 insulation with a U-factor of 0.214","steel-joist with R-6.7 insulation with a U-factor of 0.183","steel-joist with R-3.3 insulation with a U-factor of 0.296","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.839","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-0.527","U-0.365","U-0.240","U-0.705","C-0.678","C-0.522","C-6.473","U-0.214","U-0.183","U- 0.296","F-0.900","F-0.900","F-1.264","U-2.839","U-2.839","U-3.975","U-2.839","U-2.839","U-8.233",null,1.99,2.27,4.54,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,6.64,6.64,6.64,6.64,6.64,6.64,0.68,0.64,0.77,0.71,0.68,0.64]
["8 (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-15.0 insulation entirely above deck with a U-factor of 0.063","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-18.8 continuous insulation with a U-factor of 0.037","steel-framed with R-13 cavity and R-3.8 continuous insulation with a U-factor of 0.084","8\" medium weight concrete block with solid grouted cores and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-12.5 insulation with a C-factor of 0.075","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-38 insulation with a U-factor of 0.032","steel-joist with R-38 insulation with a U-factor of 0.032","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with R-20 insulation for 24 in. with an F-factor of 0.510","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 0.500",null,"U-0.048","U-0.048","U-0.063","U-0.064","U-0.037","U-0.084","C-0.119","C-0.075","C-1.140","U-0.032","U-0.032","U- 0.052","F-0.520","F-0.510","F-0.730","U-0.500","U-0.500","U-0.700","U-0.500","U-0.500","U-0.500",null,0.35,0.4,0.8,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,0.98,0.98,0.98,0.98,0.98,0.98,0.68,0.64,0.77,0.71,0.68,0.64]
["8 (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-2.6 c.i. insulation entirely above deck with a U-factor of 0.360","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity and R-3.3 continuous insulation with a U-factor of 0.212","steel-framed with R-2.3 cavity and R-0.7 continuous insulation with a U-factor of 0.479","205 mm medium weight concrete block with solid grouted cores and R-1.3 continuous insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and R-2.2 continuous insulation with a C-factor of 0.425","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-6.7 insulation with a U-factor of 0.183","steel-joist with R-6.7 insulation with a U-factor of 0.183","steel-joist with R-3.3 insulation with a U-factor of 0.296","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with R-3.5 insulation for 600 mm with an F-factor of 0.883","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.839","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 2.839",null,"U-0.273","U-0.273","U-0.360","U-0.365","U-0.212","U-0.479","C-0.678","C-0.425","C-6.473","U-0.183","U-0.183","U- 0.296","F-0.900","F-0.883","F-1.264","U-2.839","U-2.839","U-3.975","U-2.839","U-2.839","U-2.839",null,1.99,2.27,4.54,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,5.56,5.56,5.56,5.56,5.56,5.56,"NR","NR","NR","NR","NR","NR"]

{"sheet":"Envelope Lookup 90.1-2013","index":13,"n_rows":38,"n_cols":116,"rows_kept":38,"cut":false,"hidden":true,"merged":[[0,13,0,15],[0,16,0,18],[0,19,0,21],[0,44,0,46],[0,23,0,31],[0,32,0,43],[0,0,1,0],[0,1,0,3],[0,4,0,6],[0,7,0,9],[0,10,0,12],[0,47,0,55],[0,99,0,104],[0,69,0,80],[0,81,0,92],[0,93,0,98],[0,56,0,61],[0,62,0,67]]}
["Climate Zone","Roof Constructions",null,null,"Above-Grade Exterior Wall Constructions",null,null,"Below-Grade Exterior Wall Constructions",null,null,"Exposed Floor Constructions",null,null,"Slab-On-Grade Floors",null,null,"Opaque Doors - Swinging",null,null,"Opaque Doors - Nonwwinging",null,null,null,"Roof Constructions",null,null,null,null,null,null,null,null,"Above-Grade Exterior Wall Constructions",null,null,null,null,null,null,null,null,null,null,null,"Below-Grade Exterior Wall Constructions",null,null,"Exposed Floor Constructions",null,null,null,null,null,null,null,null,"Slab-On-Grade Floors",null,null,null,null,null,"Opaque Doors",null,null,null,null,null,null,"Vertical Glazing - Ufactor",null,null,null,null,null,null,null,null,null,null,null,"Vertical Glazing - SHGC",null,null,null,null,null,null,null,null,null,null,null,"Skylights - Ufactor",null,null,null,null,null,"Skylights - SHGC"]
[null,"Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated",null,"Nonresidential Insulation Entirely above Deck","Residential Insulation Entirely above Deck","Semiheated Insulation Entirely above Deck","Nonresidential Metal Building","Residential Metal Building","Semiheated Metal Building","Nonresidential Attic and Other","Residential Attic and Other","Semiheated Attic and Other","Nonresidential Mass","Residential Mass","Semiheated Mass","Nonresidential Metal Building","Residential Metal Building","Semiheated Metal Building","Nonresidential Steel Framed","Residential Steel Framed","Semiheated Steel Framed","Nonresidential Wood Framed and Other","Residential Wood Framed and Other","Semiheated Wood Framed and Other","Nonresidential","Residential","Semiheated","Nonresidential Mass","Residential Mass","Semiheated Mass","Nonresidential Steel Joist","Residential Steel Joist","Semiheated Steel Joist","Nonresidential Wood Framed and Other","Residential Wood Framed and Other","Semiheated Wood Framed and Other","Nonresidential Unheated","Residential Unheated","Semiheated Unheated","Nonresidential Heated","Residential Heated","Semiheated Heated","Nonresidential Swinging","Residential Swinging","Semiheated Swinging","Nonresidential Nonswinging","Residential Nonswinging","Semiheated Nonswinging",null,"Nonresidential Nonmetal framing all","Residential Nonmetal framing all","Semiheated Nonmetal framing all","Residential Metal framing fixed","Residential Metal framing fixed","Semiheated Metal framing fixed","Nonresidential Metal framing operable","Residential Metal framing operable","Semiheated Metal framing operable","Nonresidential Metal framing entrance door","Residential Metal framing entrance door","Semiheated Metal framing entrance door","Nonresidential 0%-10.0%","Residential 0%-10.0%","Semiheated 0%-10.0%","Nonresidential 10.1%-20.0%","Residential 10.1%-20.0%","Semiheated 10.1%-20.0%","Nonresidential 20.1%-30.0%","Residential 20.1%-30.0%","Semiheated 20.1%-30.0%","Nonresidential 30.1%-40.0%","Residential 30.1%-40.0%","Semiheated 30.1%-40.0%","Nonresidential 0%-2.0%","Nonresidential 2.1%+","Residential 0%-2.0%","Residential 2.1%+","Semiheated 0%-2.0%","Semiheated 2.1%+","Nonresidential 0%-2.0%","Nonresidential 2.1%+","Residential 0%-2.0%","Residential 2.1%+","Semiheated 0%-2.0%","Semiheated 2.1%+",null,null,null,null,null,null,null,"Climate Zone","Nonresidential","Residential","Semiheated"]
["1A (IP)","R-15 insulation entirely above deck with a U-factor of 0.063","R-20 insulation entirely above deck with a U-factor of 0.048","R-3.8 insulation entirely above deck with a U-factor of 0.218","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with no insulation with a U-factor of 0.352","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with no insulation with a U-factor of 0.350","steel-joist with no insulation with a U-factor of 0.350","steel-joist with no insulation with a U-factor of 0.350","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 1.450","U-factor of 1.450",null,4.8000000000000001E-2,3.9E-2,0.218,4.1000000000000002E-2,4.1000000000000002E-2,0.115,2.7E-2,2.7E-2,8.1000000000000003E-2,0.57999999999999996,0.151,0.57999999999999996,9.4E-2,9.4E-2,0.35199999999999998,0.124,0.124,0.35199999999999998,8.8999999999999996E-2,8.8999999999999996E-2,0.29199999999999998,1.1399999999999999,1.1399999999999999,1.1399999999999999,0.32200000000000001,0.32200000000000001,0.32200000000000001,0.35,0.35,0.35,0.28199999999999997,0.28199999999999997,0.28000000000000003,0.73,0.73,0.73,1.02,1.02,1.02,0.7,0.5,0.7,1.45,0.5,1.45,null,1.2,1.2,1.2,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,0.75,0.75,0.75,0.75,1.8,1.8,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"1-Nonmetal framing all","Nonmetal framing, all: U-0.50; SHGC-0.25; VT/SHGC-1.10","Nonmetal framing, all: U-0.50; SHGC-0.25; VT/SHGC-1.10","Nonmetal framing, all: U-0.93; SHGC-NR; VT/SHGC-NR"]
["1A (SI)","R-2.6 c.i. insulation entirely above deck with a U-factor of 0.360","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.7 c.i. insulation entirely above deck with a U-factor of 1.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with no insulation with a U-factor of 1.998","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with no insulation with a U-factor of 1.986","steel-joist with no insulation with a U-factor of 1.986","steel-joist with no insulation with a U-factor of 1.986","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 8.233","U-factor of 8.233",null,0.27,0.22,1.24,0.23,0.23,0.65,0.15,0.15,0.46,3.29,0.86,3.29,0.53,0.53,2,0.7,0.7,2,0.51,0.51,1.66,6.47,6.47,6.47,1.83,1.83,1.83,1.99,1.99,1.99,1.6,1.6,1.59,1.26,1.26,1.26,1.77,1.77,1.77,3.97,2.84,3.97,8.23,2.84,8.23,null,6.81,6.81,6.81,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,4.26,4.26,4.26,4.26,10.220000000000001,10.220000000000001,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"1-Metal framing fixed","Metal framing, fixed: U-0.57; SHGC-0.25; VT/SHGC-1.10","Metal framing, fixed: U-0.57; SHGC-0.25; VT/SHGC-1.10","Metal framing, fixed: U-1.20; SHGC-NR; VT/SHGC-NR"]
["1B (IP)","R-15 insulation entirely above deck with a U-factor of 0.063","R-20 insulation entirely above deck with a U-factor of 0.048","R-3.8 insulation entirely above deck with a U-factor of 0.218","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with no insulation with a U-factor of 0.352","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with no insulation with a U-factor of 0.350","steel-joist with no insulation with a U-factor of 0.350","steel-joist with no insulation with a U-factor of 0.350","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 1.450","U-factor of 1.450",null,4.8000000000000001E-2,3.9E-2,0.218,4.1000000000000002E-2,4.1000000000000002E-2,0.115,2.7E-2,2.7E-2,8.1000000000000003E-2,0.57999999999999996,0.151,0.57999999999999996,9.4E-2,9.4E-2,0.35199999999999998,0.124,0.124,0.35199999999999998,8.8999999999999996E-2,8.8999999999999996E-2,0.29199999999999998,1.1399999999999999,1.1399999999999999,1.1399999999999999,0.32200000000000001,0.32200000000000001,0.32200000000000001,0.35,0.35,0.35,0.28199999999999997,0.28199999999999997,0.28000000000000003,0.73,0.73,0.73,1.02,1.02,1.02,0.7,0.5,0.7,1.45,0.5,1.45,null,1.2,1.2,1.2,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,0.75,0.75,0.75,0.75,1.8,1.8,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"1-Metal framing operable","Metal framing, operable: U-0.65; SHGC-0.25; VT/SHGC-1.10","Metal framing, operable: U-0.65; SHGC-0.25; VT/SHGC-1.10","Metal framing, operable: U-1.20; SHGC-NR; VT/SHGC-NR"]
["1B (SI)","R-2.6 c.i. insulation entirely above deck with a U-factor of 0.360","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.7 c.i. insulation entirely above deck with a U-factor of 1.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with no insulation with a U-factor of 1.998","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with no insulation with a U-factor of 1.986","steel-joist with no insulation with a U-factor of 1.986","steel-joist with no insulation with a U-factor of 1.986","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 8.233","U-factor of 8.233",null,0.27,0.22,1.24,0.23,0.23,0.65,0.15,0.15,0.46,3.29,0.86,3.29,0.53,0.53,2,0.7,0.7,2,0.51,0.51,1.66,6.47,6.47,6.47,1.83,1.83,1.83,1.99,1.99,1.99,1.6,1.6,1.59,1.26,1.26,1.26,1.77,1.77,1.77,3.97,2.84,3.97,8.23,2.84,8.23,null,6.81,6.81,6.81,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,4.26,4.26,4.26,4.26,10.220000000000001,10.220000000000001,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"1-Metal framing entrance door","Metal framing, entrance door: U-1.10; SHGC-0.25; VT/SHGC-1.10","Metal framing, entrance door: U-1.10; SHGC-0.25; VT/SHGC-1.10","Metal framing, entrance door: U-1.10; SHGC-NR; VT/SHGC-NR"]
["2A (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-3.8 insulation entirely above deck with a U-factor of 0.218","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,3.9E-2,3.9E-2,0.17299999999999999,4.1000000000000002E-2,4.1000000000000002E-2,9.6000000000000002E-2,2.7E-2,2.7E-2,5.2999999999999999E-2,0.151,0.123,0.57999999999999996,9.4E-2,9.4E-2,0.16200000000000001,8.4000000000000005E-2,6.4000000000000001E-2,0.124,8.8999999999999996E-2,8.8999999999999996E-2,8.8999999999999996E-2,1.1399999999999999,1.1399999999999999,1.1399999999999999,0.107,8.6999999999999994E-2,0.32200000000000001,3.7999999999999999E-2,3.7999999999999999E-2,6.9000000000000006E-2,3.3000000000000002E-2,3.3000000000000002E-2,6.6000000000000003E-2,0.73,0.73,0.73,0.9,0.86,1.02,0.7,0.5,0.7,0.5,0.5,1.45,null,0.75,0.7,1.1000000000000001,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,0.65,0.65,0.65,0.65,1.8,1.8,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"2-Nonmetal framing all","Nonmetal framing, all: U-0.40; SHGC-0.25; VT/SHGC-1.10","Nonmetal framing, all: U-0.40; SHGC-0.25; VT/SHGC-1.10","Nonmetal framing, all: U-0.93; SHGC-NR; VT/SHGC-NR"]
["2A (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.7 c.i. insulation entirely above deck with a U-factor of 1.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.22,0.22,0.98,0.23,0.23,0.55000000000000004,0.15,0.15,0.3,0.86,0.7,3.29,0.53,0.53,0.92,0.48,0.36,0.7,0.51,0.51,0.51,6.47,6.47,6.47,0.61,0.49,1.83,0.22,0.22,0.39,0.19,0.19,0.37,1.26,1.26,1.26,1.56,1.49,1.77,3.97,2.84,3.97,2.84,2.84,8.23,null,4.26,3.97,6.25,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,3.69,3.69,3.69,3.69,10.220000000000001,10.220000000000001,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"2-Metal framing fixed","Metal framing, fixed: U-0.57; SHGC-0.25; VT/SHGC-1.10","Metal framing, fixed: U-0.57; SHGC-0.25; VT/SHGC-1.10","Metal framing, fixed: U-1.20; SHGC-NR; VT/SHGC-NR"]
["2B (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-3.8 insulation entirely above deck with a U-factor of 0.218","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,3.9E-2,3.9E-2,0.17299999999999999,4.1000000000000002E-2,4.1000000000000002E-2,9.6000000000000002E-2,2.7E-2,2.7E-2,5.2999999999999999E-2,0.151,0.123,0.57999999999999996,9.4E-2,9.4E-2,0.16200000000000001,8.4000000000000005E-2,6.4000000000000001E-2,0.124,8.8999999999999996E-2,8.8999999999999996E-2,8.8999999999999996E-2,1.1399999999999999,1.1399999999999999,1.1399999999999999,0.107,8.6999999999999994E-2,0.32200000000000001,3.7999999999999999E-2,3.7999999999999999E-2,6.9000000000000006E-2,3.3000000000000002E-2,3.3000000000000002E-2,6.6000000000000003E-2,0.73,0.73,0.73,0.9,0.86,1.02,0.7,0.5,0.7,0.5,0.5,1.45,null,0.75,0.7,1.1000000000000001,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,0.65,0.65,0.65,0.65,1.8,1.8,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"2-Metal framing operable","Metal framing, operable: U-0.65; SHGC-0.25; VT/SHGC-1.10","Metal framing, operable: U-0.65; SHGC-0.25; VT/SHGC-1.10","Metal framing, operable: U-1.20; SHGC-NR; VT/SHGC-NR"]
["2B (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.7 c.i. insulation entirely above deck with a U-factor of 1.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.22,0.22,0.98,0.23,0.23,0.55000000000000004,0.15,0.15,0.3,0.86,0.7,3.29,0.53,0.53,0.92,0.48,0.36,0.7,0.51,0.51,0.51,6.47,6.47,6.47,0.61,0.49,1.83,0.22,0.22,0.39,0.19,0.19,0.37,1.26,1.26,1.26,1.56,1.49,1.77,3.97,2.84,3.97,2.84,2.84,8.23,null,4.26,3.97,6.25,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,3.69,3.69,3.69,3.69,10.220000000000001,10.220000000000001,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"2-Metal framing entrance door","Metal framing, entrance door: U-0.83; SHGC-0.25; VT/SHGC-1.10","Metal framing, entrance door: U-0.77; SHGC-0.25; VT/SHGC-1.10","Metal framing, entrance door: U-0.83; SHGC-NR; VT/SHGC-NR"]
["3A (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-5.0 insulation entirely above deck with a U-factor of 0.173","steel-framed with R-13 cavity and R-3.8 continuous insulation with a U-factor of 0.084","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,3.9E-2,3.9E-2,0.11899999999999999,4.1000000000000002E-2,4.1000000000000002E-2,9.6000000000000002E-2,2.7E-2,2.7E-2,5.2999999999999999E-2,0.123,0.104,0.57999999999999996,9.4E-2,7.1999999999999995E-2,0.16200000000000001,7.6999999999999999E-2,6.4000000000000001E-2,0.124,8.8999999999999996E-2,6.4000000000000001E-2,8.8999999999999996E-2,1.1399999999999999,1.1399999999999999,1.1399999999999999,7.3999999999999996E-2,7.3999999999999996E-2,0.13700000000000001,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,0.01,0.73,0.54,0.73,0.86,0.86,1.02,0.7,0.5,0.7,0.5,0.5,1.45,null,0.65,0.6,0.9,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,1.7,1.7,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"3-Nonmetal framing all","Nonmetal framing, all: U-0.35; SHGC-0.25; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.25; VT/SHGC-1.10","Nonmetal framing, all: U-0.87; SHGC-NR; VT/SHGC-NR"]
["3A (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.9 c.i. insulation entirely above deck with a U-factor of 0.982","steel-framed with R-2.3 cavity and R-0.7 continuous insulation with a U-factor of 0.479","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.22,0.22,0.68,0.23,0.23,0.55000000000000004,0.15,0.15,0.3,0.7,0.59,3.29,0.53,0.41,0.92,0.44,0.36,0.7,0.51,0.36,0.51,6.47,6.47,6.47,0.42,0.42,0.78,0.22,0.22,0.3,0.19,0.19,0.06,1.26,0.94,1.26,1.49,1.49,1.77,3.97,2.84,3.97,2.84,2.84,8.23,null,3.69,3.41,5.1100000000000003,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,3.12,3.12,3.12,3.12,9.65,9.65,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"3-Metal framing fixed","Metal framing, fixed: U-0.50; SHGC-0.25; VT/SHGC-1.10","Metal framing, fixed: U-0.50; SHGC-0.25; VT/SHGC-1.10","Metal framing, fixed: U-1.20; SHGC-NR; VT/SHGC-NR"]
["3B (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-5.0 insulation entirely above deck with a U-factor of 0.173","steel-framed with R-13 cavity and R-3.8 continuous insulation with a U-factor of 0.084","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,3.9E-2,3.9E-2,0.11899999999999999,4.1000000000000002E-2,4.1000000000000002E-2,9.6000000000000002E-2,2.7E-2,2.7E-2,5.2999999999999999E-2,0.123,0.104,0.57999999999999996,9.4E-2,7.1999999999999995E-2,0.16200000000000001,7.6999999999999999E-2,6.4000000000000001E-2,0.124,8.8999999999999996E-2,6.4000000000000001E-2,8.8999999999999996E-2,1.1399999999999999,1.1399999999999999,1.1399999999999999,7.3999999999999996E-2,7.3999999999999996E-2,0.13700000000000001,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,0.01,0.73,0.54,0.73,0.86,0.86,1.02,0.7,0.5,0.7,0.5,0.5,1.45,null,0.65,0.6,0.9,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,1.7,1.7,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"3-Metal framing operable","Metal framing, operable: U-0.60; SHGC-0.25; VT/SHGC-1.10","Metal framing, operable: U-0.60; SHGC-0.25; VT/SHGC-1.10","Metal framing, operable: U-1.20; SHGC-NR; VT/SHGC-NR"]
["3B (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.9 c.i. insulation entirely above deck with a U-factor of 0.982","steel-framed with R-2.3 cavity and R-0.7 continuous insulation with a U-factor of 0.479","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.22,0.22,0.68,0.23,0.23,0.55000000000000004,0.15,0.15,0.3,0.7,0.59,3.29,0.53,0.41,0.92,0.44,0.36,0.7,0.51,0.36,0.51,6.47,6.47,6.47,0.42,0.42,0.78,0.22,0.22,0.3,0.19,0.19,0.06,1.26,0.94,1.26,1.49,1.49,1.77,3.97,2.84,3.97,2.84,2.84,8.23,null,3.69,3.41,5.1100000000000003,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,3.12,3.12,3.12,3.12,9.65,9.65,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"3-Metal framing entrance door","Metal framing, entrance door: U-0.77; SHGC-0.25; VT/SHGC-1.10","Metal framing, entrance door: U-0.68; SHGC-0.25; VT/SHGC-1.10","Metal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["3C (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-5.0 insulation entirely above deck with a U-factor of 0.173","steel-framed with R-13 cavity and R-3.8 continuous insulation with a U-factor of 0.084","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,3.9E-2,3.9E-2,0.11899999999999999,4.1000000000000002E-2,4.1000000000000002E-2,9.6000000000000002E-2,2.7E-2,2.7E-2,5.2999999999999999E-2,0.123,0.104,0.57999999999999996,9.4E-2,7.1999999999999995E-2,0.16200000000000001,7.6999999999999999E-2,6.4000000000000001E-2,0.124,8.8999999999999996E-2,6.4000000000000001E-2,8.8999999999999996E-2,1.1399999999999999,1.1399999999999999,1.1399999999999999,7.3999999999999996E-2,7.3999999999999996E-2,0.13700000000000001,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,0.01,0.73,0.54,0.73,0.86,0.86,1.02,0.7,0.5,0.7,0.5,0.5,1.45,null,0.65,0.6,0.9,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.55000000000000004,1.7,1.7,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"4-Nonmetal framing all","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR"]
["3C (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.9 c.i. insulation entirely above deck with a U-factor of 0.982","steel-framed with R-2.3 cavity and R-0.7 continuous insulation with a U-factor of 0.479","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.22,0.22,0.68,0.23,0.23,0.55000000000000004,0.15,0.15,0.3,0.7,0.59,3.29,0.53,0.41,0.92,0.44,0.36,0.7,0.51,0.36,0.51,6.47,6.47,6.47,0.42,0.42,0.78,0.22,0.22,0.3,0.19,0.19,0.06,1.26,0.94,1.26,1.49,1.49,1.77,3.97,2.84,3.97,2.84,2.84,8.23,null,3.69,3.41,5.1100000000000003,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,3.12,3.12,3.12,3.12,9.65,9.65,0.35,0.35,0.35,0.35,"NR","NR",null,null,null,null,null,null,null,"4-Metal framing fixed","Metal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10","Metal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10","Metal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR"]
["4A (IP)","R-30 insulation entirely above deck with a U-factor of 0.032","R-30 insulation entirely above deck with a U-factor of 0.032","R-10 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with  R-15 insulation for 24 in.  with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,3.2000000000000001E-2,3.2000000000000001E-2,9.2999999999999999E-2,3.6999999999999998E-2,3.6999999999999998E-2,8.2000000000000003E-2,2.1000000000000001E-2,2.1000000000000001E-2,3.4000000000000002E-2,0.104,0.09,0.57999999999999996,0.06,0.05,0.16200000000000001,6.4000000000000001E-2,6.4000000000000001E-2,0.124,6.4000000000000001E-2,6.4000000000000001E-2,8.8999999999999996E-2,0.11899999999999999,9.1999999999999998E-2,1.1399999999999999,5.7000000000000002E-2,5.0999999999999997E-2,0.107,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,5.0999999999999997E-2,0.52,0.52,0.73,0.84299999999999997,0.68799999999999994,0.9,0.5,0.5,0.7,0.5,0.5,1.45,null,0.35,0.35,0.51,0.42,0.42,0.73,0.5,0.5,0.81,0.77,0.68,0.77,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.5,0.5,0.5,0.5,1.1499999999999999,1.1499999999999999,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"4-Metal framing operable","Metal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10","Metal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10","Metal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR"]
["4A (SI)","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.529","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.677","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.523","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.84","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.296","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.844","U-factor of 2.844","U-factor of 3.981","U-factor of 2.844","U-factor of 2.844","U-factor of 8.247",null,0.18170441600000001,0.18170441600000001,0.52807845900000006,0.21009573100000001,0.21009573100000001,0.46561756600000004,0.11924352300000002,0.11924352300000002,0.19306094200000001,0.59053935199999996,0.51104367000000006,3.2933925400000001,0.34069578,0.28391315,0.91987860600000004,0.36340883200000001,0.36340883200000001,0.70410461200000007,0.36340883200000001,0.36340883200000001,0.50536540699999999,0.66700000000000004,0.52300000000000002,6.484,0.32366099100000001,0.28959141300000002,0.60757414100000007,0.215773994,0.215773994,0.29526967599999998,0.66700000000000004,0.52300000000000002,6.484,0.90038000000000007,0.90038000000000007,1.263995,1.4596545000000001,1.1912719999999999,1.5583500000000001,2.8391315000000001,2.8391315000000001,3.9747840999999999,2.8391315000000001,2.8391315000000001,8.2334813499999999,null,{"$f":"BR17*5.678263","v":1.98739205},{"$f":"BS17*5.678263","v":1.98739205},2.89591413,2.3848704600000001,2.3848704600000001,4.1451319900000003,2.8391315000000001,2.8391315000000001,4.5993930300000008,4.3722625100000005,3.8612188400000003,4.3722625100000005,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",2.84,2.84,2.84,2.84,6.53,6.53,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"4-Metal framing entrance door","Metal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Metal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Metal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["4B (IP)","R-30 insulation entirely above deck with a U-factor of 0.032","R-30 insulation entirely above deck with a U-factor of 0.032","R-10 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with  R-15 insulation for 24 in.  with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,3.2000000000000001E-2,3.2000000000000001E-2,9.2999999999999999E-2,3.6999999999999998E-2,3.6999999999999998E-2,8.2000000000000003E-2,2.1000000000000001E-2,2.1000000000000001E-2,3.4000000000000002E-2,0.104,0.09,0.57999999999999996,0.06,0.05,0.16200000000000001,6.4000000000000001E-2,6.4000000000000001E-2,0.124,6.4000000000000001E-2,6.4000000000000001E-2,8.8999999999999996E-2,0.11899999999999999,9.1999999999999998E-2,1.1399999999999999,5.7000000000000002E-2,5.0999999999999997E-2,0.107,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,5.0999999999999997E-2,0.52,0.52,0.73,0.84299999999999997,0.68799999999999994,0.9,0.5,0.5,0.7,0.5,0.5,1.45,null,0.35,0.35,0.51,0.42,0.42,0.73,0.5,0.5,0.81,0.77,0.68,0.77,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.5,0.5,0.5,0.5,1.1499999999999999,1.1499999999999999,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"5-Nonmetal framing all","Nonmetal framing, all: U-0.32; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.32; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.45; SHGC-NR; VT/SHGC-NR"]
["4B (SI)","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.529","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.677","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.523","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.84","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.296","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.844","U-factor of 2.844","U-factor of 3.981","U-factor of 2.844","U-factor of 2.844","U-factor of 8.247",null,0.18170441600000001,0.18170441600000001,0.52807845900000006,0.21009573100000001,0.21009573100000001,0.46561756600000004,0.11924352300000002,0.11924352300000002,0.19306094200000001,0.59053935199999996,0.51104367000000006,3.2933925400000001,0.34069578,0.28391315,0.91987860600000004,0.36340883200000001,0.36340883200000001,0.70410461200000007,0.36340883200000001,0.36340883200000001,0.50536540699999999,0.66700000000000004,0.52300000000000002,6.484,0.32366099100000001,0.28959141300000002,0.60757414100000007,0.215773994,0.215773994,0.29526967599999998,0.66700000000000004,0.52300000000000002,6.484,0.90038000000000007,0.90038000000000007,1.263995,1.4596545000000001,1.1912719999999999,1.5583500000000001,2.8391315000000001,2.8391315000000001,3.9747840999999999,2.8391315000000001,2.8391315000000001,8.2334813499999999,null,{"$f":"BR19*5.678263","v":1.98739205},{"$f":"BS19*5.678263","v":1.98739205},{"$f":"BT19*5.678263","v":2.89591413},{"$f":"BU19*5.678263","v":2.3848704600000001},{"$f":"BV19*5.678263","v":2.3848704600000001},{"$f":"BW19*5.678263","v":4.1451319900000003},{"$f":"BX19*5.678263","v":2.8391315000000001},{"$f":"BY19*5.678263","v":2.8391315000000001},{"$f":"BZ19*5.678263","v":4.5993930300000008},{"$f":"CA19*5.678263","v":4.3722625100000005},{"$f":"CB19*5.678263","v":3.8612188400000003},{"$f":"CC19*5.678263","v":4.3722625100000005},0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",2.84,2.84,2.84,2.84,6.53,6.53,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"5-Metal framing fixed","Metal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10","Metal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10","Metal framing, fixed: U-0.62; SHGC-NR; VT/SHGC-NR"]
["4C (IP)","R-30 insulation entirely above deck with a U-factor of 0.032","R-30 insulation entirely above deck with a U-factor of 0.032","R-10 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with  R-15 insulation for 24 in.  with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,3.2000000000000001E-2,3.2000000000000001E-2,9.2999999999999999E-2,3.6999999999999998E-2,3.6999999999999998E-2,8.2000000000000003E-2,2.1000000000000001E-2,2.1000000000000001E-2,3.4000000000000002E-2,0.104,0.09,0.57999999999999996,0.06,0.05,0.16200000000000001,6.4000000000000001E-2,6.4000000000000001E-2,0.124,6.4000000000000001E-2,6.4000000000000001E-2,8.8999999999999996E-2,0.11899999999999999,9.1999999999999998E-2,1.1399999999999999,5.7000000000000002E-2,5.0999999999999997E-2,0.107,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,5.0999999999999997E-2,0.52,0.52,0.73,0.84299999999999997,0.68799999999999994,0.9,0.5,0.5,0.7,0.5,0.5,1.45,null,0.35,0.35,0.51,0.42,0.42,0.73,0.5,0.5,0.81,0.77,0.68,0.77,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.5,0.5,0.5,0.5,1.1499999999999999,1.1499999999999999,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"5-Metal framing operable","Metal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10","Metal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10","Metal framing, operable: U-0.70; SHGC-NR; VT/SHGC-NR"]
["4C (SI)","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.529","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.677","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.523","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.84","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.296","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.844","U-factor of 2.844","U-factor of 3.981","U-factor of 2.844","U-factor of 2.844","U-factor of 8.247",null,0.18170441600000001,0.18170441600000001,0.52807845900000006,0.21009573100000001,0.21009573100000001,0.46561756600000004,0.11924352300000002,0.11924352300000002,0.19306094200000001,0.59053935199999996,0.51104367000000006,3.2933925400000001,0.34069578,0.28391315,0.91987860600000004,0.36340883200000001,0.36340883200000001,0.70410461200000007,0.36340883200000001,0.36340883200000001,0.50536540699999999,0.66700000000000004,0.52300000000000002,6.484,0.32366099100000001,0.28959141300000002,0.60757414100000007,0.215773994,0.215773994,0.29526967599999998,0.66700000000000004,0.52300000000000002,6.484,0.90038000000000007,0.90038000000000007,1.263995,1.4596545000000001,1.1912719999999999,1.5583500000000001,2.8391315000000001,2.8391315000000001,3.9747840999999999,2.8391315000000001,2.8391315000000001,8.2334813499999999,null,{"$f":"BR21*5.678263","v":1.98739205},{"$f":"BS21*5.678263","v":1.98739205},{"$f":"BT21*5.678263","v":2.89591413},{"$f":"BU21*5.678263","v":2.3848704600000001},{"$f":"BV21*5.678263","v":2.3848704600000001},{"$f":"BW21*5.678263","v":4.1451319900000003},{"$f":"BX21*5.678263","v":2.8391315000000001},{"$f":"BY21*5.678263","v":2.8391315000000001},{"$f":"BZ21*5.678263","v":4.5993930300000008},{"$f":"CA21*5.678263","v":4.3722625100000005},{"$f":"CB21*5.678263","v":3.8612188400000003},{"$f":"CC21*5.678263","v":4.3722625100000005},0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",2.84,2.84,2.84,2.84,6.53,6.53,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"5-Metal framing entrance door","Metal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Metal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Metal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["5A (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,3.2000000000000001E-2,3.2000000000000001E-2,6.3E-2,3.6999999999999998E-2,3.6999999999999998E-2,8.2000000000000003E-2,2.1000000000000001E-2,2.1000000000000001E-2,3.4000000000000002E-2,0.09,0.08,0.151,0.05,0.05,9.4E-2,5.5E-2,5.5E-2,8.4000000000000005E-2,5.0999999999999997E-2,5.0999999999999997E-2,8.8999999999999996E-2,0.11899999999999999,9.1999999999999998E-2,1.1399999999999999,5.7000000000000002E-2,5.0999999999999997E-2,0.107,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,5.0999999999999997E-2,0.52,0.51,0.73,0.68799999999999994,0.68799999999999994,0.9,0.5,0.5,0.7,0.5,0.5,1.45,null,0.32,0.32,0.45,0.42,0.42,0.62,0.5,0.5,0.7,0.77,0.68,0.77,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.5,0.5,0.5,0.5,0.98,0.98,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"6-Nonmetal framing all","Nonmetal framing, all: U-0.32; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.32; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.45; SHGC-NR; VT/SHGC-NR"]
["5A (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.18170441600000001,0.18170441600000001,0.357730569,0.21009573100000001,0.21009573100000001,0.46561756600000004,0.11924352300000002,0.11924352300000002,0.19306094200000001,0.51104367000000006,0.45426104,0.85741771300000003,0.28391315,0.28391315,0.53375672200000002,0.31230446500000003,0.31230446500000003,0.47697409200000007,0.28959141300000002,0.28959141300000002,0.50536540699999999,0.67571329700000005,0.52240019599999998,6.4732198199999997,0.32366099100000001,0.28959141300000002,0.60757414100000007,0.215773994,0.215773994,0.29526967599999998,0.66700000000000004,0.52300000000000002,6.484,0.90038000000000007,0.88306499999999999,1.263995,1.1912719999999999,1.1912719999999999,1.5583500000000001,2.8391315000000001,2.8391315000000001,3.9747840999999999,2.8391315000000001,2.8391315000000001,8.2334813499999999,null,{"$f":"BR23*5.678263","v":1.81704416},{"$f":"BS23*5.678263","v":1.81704416},{"$f":"BT23*5.678263","v":2.5552183500000001},{"$f":"BU23*5.678263","v":2.3848704600000001},{"$f":"BV23*5.678263","v":2.3848704600000001},{"$f":"BW23*5.678263","v":3.5205230600000004},{"$f":"BX23*5.678263","v":2.8391315000000001},{"$f":"BY23*5.678263","v":2.8391315000000001},{"$f":"BZ23*5.678263","v":3.9747840999999999},{"$f":"CA23*5.678263","v":4.3722625100000005},{"$f":"CB23*5.678263","v":3.8612188400000003},{"$f":"CC23*5.678263","v":4.3722625100000005},0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",2.84,2.84,2.84,2.84,5.56,5.56,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"6-Metal framing fixed","Metal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10","Metal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10","Metal framing, fixed: U-0.51; SHGC-NR; VT/SHGC-NR"]
["5B (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,3.2000000000000001E-2,3.2000000000000001E-2,6.3E-2,3.6999999999999998E-2,3.6999999999999998E-2,8.2000000000000003E-2,2.1000000000000001E-2,2.1000000000000001E-2,3.4000000000000002E-2,0.09,0.08,0.151,0.05,0.05,9.4E-2,5.5E-2,5.5E-2,8.4000000000000005E-2,5.0999999999999997E-2,5.0999999999999997E-2,8.8999999999999996E-2,0.11899999999999999,9.1999999999999998E-2,1.1399999999999999,5.7000000000000002E-2,5.0999999999999997E-2,0.107,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,5.0999999999999997E-2,0.52,0.51,0.73,0.68799999999999994,0.68799999999999994,0.9,0.5,0.5,0.7,0.5,0.5,1.45,null,0.32,0.32,0.45,0.42,0.42,0.62,0.5,0.5,0.7,0.77,0.68,0.77,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.5,0.5,0.5,0.5,0.98,0.98,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"6-Metal framing operable","Metal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10","Metal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10","Metal framing, operable: U-0.59; SHGC-NR; VT/SHGC-NR"]
["5B (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.18170441600000001,0.18170441600000001,0.357730569,0.21009573100000001,0.21009573100000001,0.46561756600000004,0.11924352300000002,0.11924352300000002,0.19306094200000001,0.51104367000000006,0.45426104,0.85741771300000003,0.28391315,0.28391315,0.53375672200000002,0.31230446500000003,0.31230446500000003,0.47697409200000007,0.28959141300000002,0.28959141300000002,0.50536540699999999,0.67571329700000005,0.52240019599999998,6.4732198199999997,0.32366099100000001,0.28959141300000002,0.60757414100000007,0.215773994,0.215773994,0.29526967599999998,0.66700000000000004,0.52300000000000002,6.484,0.90038000000000007,0.88306499999999999,1.263995,1.1912719999999999,1.1912719999999999,1.5583500000000001,2.8391315000000001,2.8391315000000001,3.9747840999999999,2.8391315000000001,2.8391315000000001,8.2334813499999999,null,{"$f":"BR25*5.678263","v":1.81704416},{"$f":"BS25*5.678263","v":1.81704416},{"$f":"BT25*5.678263","v":2.5552183500000001},{"$f":"BU25*5.678263","v":2.3848704600000001},{"$f":"BV25*5.678263","v":2.3848704600000001},{"$f":"BW25*5.678263","v":3.5205230600000004},{"$f":"BX25*5.678263","v":2.8391315000000001},{"$f":"BY25*5.678263","v":2.8391315000000001},{"$f":"BZ25*5.678263","v":3.9747840999999999},{"$f":"CA25*5.678263","v":4.3722625100000005},{"$f":"CB25*5.678263","v":3.8612188400000003},{"$f":"CC25*5.678263","v":4.3722625100000005},0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",2.84,2.84,2.84,2.84,5.56,5.56,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"6-Metal framing entrance door","Metal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Metal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Metal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["5C (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,3.2000000000000001E-2,3.2000000000000001E-2,6.3E-2,3.6999999999999998E-2,3.6999999999999998E-2,8.2000000000000003E-2,2.1000000000000001E-2,2.1000000000000001E-2,3.4000000000000002E-2,0.09,0.08,0.151,0.05,0.05,9.4E-2,5.5E-2,5.5E-2,8.4000000000000005E-2,5.0999999999999997E-2,5.0999999999999997E-2,8.8999999999999996E-2,0.11899999999999999,9.1999999999999998E-2,1.1399999999999999,5.7000000000000002E-2,5.0999999999999997E-2,0.107,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,5.0999999999999997E-2,0.52,0.51,0.73,0.68799999999999994,0.68799999999999994,0.9,0.5,0.5,0.7,0.5,0.5,1.45,null,0.32,0.32,0.45,0.42,0.42,0.62,0.5,0.5,0.7,0.77,0.68,0.77,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.5,0.5,0.5,0.5,0.98,0.98,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"7-Nonmetal framing all","Nonmetal framing, all: U-0.32; SHGC-0.45; VT/SHGC-1.10","Nonmetal framing, all: U-0.32; SHGC-0.45; VT/SHGC-1.10","Nonmetal framing, all: U-0.45; SHGC-NR; VT/SHGC-NR"]
["5C (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,0.18170441600000001,0.18170441600000001,0.357730569,0.21009573100000001,0.21009573100000001,0.46561756600000004,0.11924352300000002,0.11924352300000002,0.19306094200000001,0.51104367000000006,0.45426104,0.85741771300000003,0.28391315,0.28391315,0.53375672200000002,0.31230446500000003,0.31230446500000003,0.47697409200000007,0.28959141300000002,0.28959141300000002,0.50536540699999999,0.67571329700000005,0.52240019599999998,6.4732198199999997,0.32366099100000001,0.28959141300000002,0.60757414100000007,0.215773994,0.215773994,0.29526967599999998,0.66700000000000004,0.52300000000000002,6.484,0.90038000000000007,0.88306499999999999,1.263995,1.1912719999999999,1.1912719999999999,1.5583500000000001,2.8391315000000001,2.8391315000000001,3.9747840999999999,2.8391315000000001,2.8391315000000001,8.2334813499999999,null,{"$f":"BR27*5.678263","v":1.81704416},{"$f":"BS27*5.678263","v":1.81704416},{"$f":"BT27*5.678263","v":2.5552183500000001},{"$f":"BU27*5.678263","v":2.3848704600000001},{"$f":"BV27*5.678263","v":2.3848704600000001},{"$f":"BW27*5.678263","v":3.5205230600000004},{"$f":"BX27*5.678263","v":2.8391315000000001},{"$f":"BY27*5.678263","v":2.8391315000000001},{"$f":"BZ27*5.678263","v":3.9747840999999999},{"$f":"CA27*5.678263","v":4.3722625100000005},{"$f":"CB27*5.678263","v":3.8612188400000003},{"$f":"CC27*5.678263","v":4.3722625100000005},0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",2.84,2.84,2.84,2.84,5.56,5.56,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"7-Metal framing fixed","Metal framing, fixed: U-0.38; SHGC-0.45; VT/SHGC-1.10","Metal framing, fixed: U-0.38; SHGC-0.45; VT/SHGC-1.10","Metal framing, fixed: U-0.38; SHGC-NR; VT/SHGC-NR"]
["6A (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,3.2000000000000001E-2,3.2000000000000001E-2,6.3E-2,3.1E-2,2.9000000000000001E-2,0.06,2.1000000000000001E-2,2.1000000000000001E-2,3.4000000000000002E-2,0.08,8.1000000000000003E-2,0.151,0.05,0.05,9.4E-2,4.9000000000000002E-2,4.9000000000000002E-2,8.4000000000000005E-2,5.0999999999999997E-2,5.0999999999999997E-2,8.8999999999999996E-2,9.1999999999999998E-2,6.3E-2,0.11899999999999999,5.0999999999999997E-2,5.0999999999999997E-2,8.6999999999999994E-2,3.2000000000000001E-2,3.2000000000000001E-2,5.1999999999999998E-2,2.7E-2,2.7E-2,5.0999999999999997E-2,0.51,0.434,0.73,0.68799999999999994,0.67100000000000004,0.86,0.5,0.5,0.7,0.5,0.5,0.5,null,0.32,0.32,0.45,0.42,0.42,0.51,0.5,0.5,0.59,0.77,0.68,0.77,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.5,0.5,0.5,0.5,0.85,0.85,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"7-Metal framing operable","Metal framing, operable: U-0.40; SHGC-0.45; VT/SHGC-1.10","Metal framing, operable: U-0.40; SHGC-0.45; VT/SHGC-1.10","Metal framing, operable: U-0.44; SHGC-NR; VT/SHGC-NR"]
["6A (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.260","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,0.18170441600000001,0.18170441600000001,0.357730569,0.17602615300000002,0.16466962700000001,0.34069578,0.11924352300000002,0.11924352300000002,0.19306094200000001,0.45426104,0.45993930300000002,0.85741771300000003,0.28391315,0.28391315,0.53375672200000002,0.27823488700000004,0.27823488700000004,0.47697409200000007,0.28959141300000002,0.28959141300000002,0.50536540699999999,0.52240019599999998,0.357730569,0.67571329700000005,0.28959141300000002,0.28959141300000002,0.49400888100000001,0.18170441600000001,0.18170441600000001,0.29526967599999998,0.66700000000000004,0.52300000000000002,6.484,0.88306499999999999,0.751471,1.263995,1.1912719999999999,1.1618365000000002,1.48909,2.8391315000000001,2.8391315000000001,3.9747840999999999,2.8391315000000001,2.8391315000000001,2.8391315000000001,null,{"$f":"BR29*5.678263","v":1.81704416},{"$f":"BS29*5.678263","v":1.81704416},{"$f":"BT29*5.678263","v":2.5552183500000001},{"$f":"BU29*5.678263","v":2.3848704600000001},{"$f":"BV29*5.678263","v":2.3848704600000001},{"$f":"BW29*5.678263","v":2.89591413},{"$f":"BX29*5.678263","v":2.8391315000000001},{"$f":"BY29*5.678263","v":2.8391315000000001},{"$f":"BZ29*5.678263","v":3.35017517},{"$f":"CA29*5.678263","v":4.3722625100000005},{"$f":"CB29*5.678263","v":3.8612188400000003},{"$f":"CC29*5.678263","v":4.3722625100000005},0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",2.84,2.84,2.84,2.84,4.83,4.83,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"7-Metal framing entrance door","Metal framing, entrance door: U-0.77; SHGC-0.45; VT/SHGC-1.10","Metal framing, entrance door: U-0.68; SHGC-0.45; VT/SHGC-1.10","Metal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["6B (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,3.2000000000000001E-2,3.2000000000000001E-2,6.3E-2,3.1E-2,2.9000000000000001E-2,0.06,2.1000000000000001E-2,2.1000000000000001E-2,3.4000000000000002E-2,0.08,8.1000000000000003E-2,0.151,0.05,0.05,9.4E-2,4.9000000000000002E-2,4.9000000000000002E-2,8.4000000000000005E-2,5.0999999999999997E-2,5.0999999999999997E-2,8.8999999999999996E-2,9.1999999999999998E-2,6.3E-2,0.11899999999999999,5.0999999999999997E-2,5.0999999999999997E-2,8.6999999999999994E-2,3.2000000000000001E-2,3.2000000000000001E-2,5.1999999999999998E-2,2.7E-2,2.7E-2,5.0999999999999997E-2,0.51,0.434,0.73,0.68799999999999994,0.67100000000000004,0.86,0.5,0.5,0.7,0.5,0.5,0.5,null,0.32,0.32,0.45,0.42,0.42,0.51,0.5,0.5,0.59,0.77,0.68,0.77,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.5,0.5,0.5,0.5,0.85,0.85,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"8-Nonmetal framing all","Nonmetal framing, all: U-0.32; SHGC-0.45; VT/SHGC-1.10","Nonmetal framing, all: U-0.32; SHGC-0.45; VT/SHGC-1.10","Nonmetal framing, all: U-0.32; SHGC-NR; VT/SHGC-NR"]
["6B (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.260","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,0.18170441600000001,0.18170441600000001,0.357730569,0.17602615300000002,0.16466962700000001,0.34069578,0.11924352300000002,0.11924352300000002,0.19306094200000001,0.45426104,0.45993930300000002,0.85741771300000003,0.28391315,0.28391315,0.53375672200000002,0.27823488700000004,0.27823488700000004,0.47697409200000007,0.28959141300000002,0.28959141300000002,0.50536540699999999,0.52240019599999998,0.357730569,0.67571329700000005,0.28959141300000002,0.28959141300000002,0.49400888100000001,0.18170441600000001,0.18170441600000001,0.29526967599999998,0.66700000000000004,0.52300000000000002,6.484,0.88306499999999999,0.751471,1.263995,1.1912719999999999,1.1618365000000002,1.48909,2.8391315000000001,2.8391315000000001,3.9747840999999999,2.8391315000000001,2.8391315000000001,2.8391315000000001,null,{"$f":"BR31*5.678263","v":1.81704416},{"$f":"BS31*5.678263","v":1.81704416},{"$f":"BT31*5.678263","v":2.5552183500000001},{"$f":"BU31*5.678263","v":2.3848704600000001},{"$f":"BV31*5.678263","v":2.3848704600000001},{"$f":"BW31*5.678263","v":2.89591413},{"$f":"BX31*5.678263","v":2.8391315000000001},{"$f":"BY31*5.678263","v":2.8391315000000001},{"$f":"BZ31*5.678263","v":3.35017517},{"$f":"CA31*5.678263","v":4.3722625100000005},{"$f":"CB31*5.678263","v":3.8612188400000003},{"$f":"CC31*5.678263","v":4.3722625100000005},0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",2.84,2.84,2.84,2.84,4.83,4.83,0.4,0.4,0.4,0.4,"NR","NR",null,null,null,null,null,null,null,"8-Metal framing fixed","Metal framing, fixed: U-0.38; SHGC-0.45; VT/SHGC-1.10","Metal framing, fixed: U-0.38; SHGC-0.45; VT/SHGC-1.10","Metal framing, fixed: U-0.38; SHGC-NR; VT/SHGC-NR"]
["7A (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-10.0 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-15.6 continuous insulation with a U-factor of 0.042","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10.0 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-38 insulation with a U-factor of 0.032","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,2.8000000000000001E-2,2.8000000000000001E-2,3.9E-2,2.9000000000000001E-2,2.9000000000000001E-2,3.6999999999999998E-2,1.7000000000000001E-2,1.7000000000000001E-2,2.7E-2,7.0999999999999994E-2,7.0999999999999994E-2,0.123,4.3999999999999997E-2,4.3999999999999997E-2,7.1999999999999995E-2,4.9000000000000002E-2,4.2000000000000003E-2,6.4000000000000001E-2,5.0999999999999997E-2,5.0999999999999997E-2,6.4000000000000001E-2,6.3E-2,6.3E-2,0.11899999999999999,4.2000000000000003E-2,4.2000000000000003E-2,7.3999999999999996E-2,3.2000000000000001E-2,3.2000000000000001E-2,5.1999999999999998E-2,2.7E-2,2.7E-2,5.0999999999999997E-2,0.51,0.434,0.73,0.67100000000000004,0.67100000000000004,0.86,0.5,0.5,0.7,0.5,0.5,0.5,null,0.35,0.4,0.8,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,0.5,0.5,0.5,0.5,0.85,0.85,"NR","NR","NR","NR","NR","NR",null,null,null,null,null,null,null,"8-Metal framing operable","Metal framing, operable: U-0.40; SHGC-0.45; VT/SHGC-1.10","Metal framing, operable: U-0.40; SHGC-0.45; VT/SHGC-1.10","Metal framing, operable: U-0.44; SHGC-NR; VT/SHGC-NR"]
["7A (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-1.8 insulation entirely above deck with a U-factor of 0.527","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity and R-2.7 continuous insulation with a U-factor of 0.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and R-1.3 continuous insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and R-1.8 continuous insulation with a C-factor of 0.522","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-5.3 insulation with a U-factor of 0.214","steel-joist with R-6.7 insulation with a U-factor of 0.183","steel-joist with R-3.3 insulation with a U-factor of 0.296","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.839","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,0.16,0.16,0.22,0.16,0.16,0.21,0.1,0.1,0.15,0.4,0.4,0.7,0.25,0.25,0.41,0.28000000000000003,0.24,0.36,0.28999999999999998,0.28999999999999998,0.36,0.36,0.36,0.68,0.24,0.24,0.42,0.18,0.18,0.3,0.15,0.15,0.28999999999999998,0.88,0.75,1.26,1.1599999999999999,1.1599999999999999,1.49,2.84,2.84,3.97,2.84,2.84,2.84,null,0.35,0.4,0.8,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,2.84,2.84,2.84,2.84,4.83,4.83,"NR","NR","NR","NR","NR","NR",null,null,null,null,null,null,null,"8-Metal framing entrance door","Metal framing, entrance door: U-0.77; SHGC-0.45; VT/SHGC-1.10","Metal framing, entrance door: U-0.68; SHGC-0.45; VT/SHGC-1.10","Metal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["7B (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-10.0 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-15.6 continuous insulation with a U-factor of 0.042","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10.0 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-38 insulation with a U-factor of 0.032","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,2.8000000000000001E-2,2.8000000000000001E-2,3.9E-2,2.9000000000000001E-2,2.9000000000000001E-2,3.6999999999999998E-2,1.7000000000000001E-2,1.7000000000000001E-2,2.7E-2,7.0999999999999994E-2,7.0999999999999994E-2,0.123,4.3999999999999997E-2,4.3999999999999997E-2,7.1999999999999995E-2,4.9000000000000002E-2,4.2000000000000003E-2,6.4000000000000001E-2,5.0999999999999997E-2,5.0999999999999997E-2,6.4000000000000001E-2,6.3E-2,6.3E-2,0.11899999999999999,4.2000000000000003E-2,4.2000000000000003E-2,7.3999999999999996E-2,3.2000000000000001E-2,3.2000000000000001E-2,5.1999999999999998E-2,2.7E-2,2.7E-2,5.0999999999999997E-2,0.51,0.434,0.73,0.67100000000000004,0.67100000000000004,0.86,0.5,0.5,0.7,0.5,0.5,0.5,null,0.35,0.4,0.8,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,0.5,0.5,0.5,0.5,0.85,0.85,"NR","NR","NR","NR","NR","NR"]
["7B (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-1.8 insulation entirely above deck with a U-factor of 0.527","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity and R-2.7 continuous insulation with a U-factor of 0.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and R-1.3 continuous insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and R-1.8 continuous insulation with a C-factor of 0.522","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-5.3 insulation with a U-factor of 0.214","steel-joist with R-6.7 insulation with a U-factor of 0.183","steel-joist with R-3.3 insulation with a U-factor of 0.296","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.839","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,0.16,0.16,0.22,0.16,0.16,0.21,0.1,0.1,0.15,0.4,0.4,0.7,0.25,0.25,0.41,0.28000000000000003,0.24,0.36,0.28999999999999998,0.28999999999999998,0.36,0.36,0.36,0.68,0.24,0.24,0.42,0.18,0.18,0.3,0.15,0.15,0.28999999999999998,0.88,0.75,1.26,1.1599999999999999,1.1599999999999999,1.49,2.84,2.84,3.97,2.84,2.84,2.84,null,1.99,2.27,4.54,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,2.84,2.84,2.84,2.84,4.83,4.83,"NR","NR","NR","NR","NR","NR"]
["8 (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-15.0 insulation entirely above deck with a U-factor of 0.063","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-18.8 continuous insulation with a U-factor of 0.037","steel-framed with R-13 cavity and R-3.8 continuous insulation with a U-factor of 0.084","8\" medium weight concrete block with solid grouted cores and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-12.5 insulation with a C-factor of 0.075","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-38 insulation with a U-factor of 0.032","steel-joist with R-38 insulation with a U-factor of 0.032","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with R-20 insulation for 24 in. with an F-factor of 0.510","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 0.500",null,2.8000000000000001E-2,2.8000000000000001E-2,3.9E-2,2.5999999999999999E-2,2.5999999999999999E-2,3.6999999999999998E-2,1.7000000000000001E-2,1.7000000000000001E-2,2.7E-2,4.8000000000000001E-2,4.8000000000000001E-2,0.104,3.9E-2,3.9E-2,0.06,3.6999999999999998E-2,3.6999999999999998E-2,6.4000000000000001E-2,3.2000000000000001E-2,3.2000000000000001E-2,5.0999999999999997E-2,6.3E-2,6.3E-2,0.11899999999999999,3.7999999999999999E-2,3.7999999999999999E-2,6.4000000000000001E-2,3.2000000000000001E-2,3.2000000000000001E-2,5.1999999999999998E-2,2.7E-2,2.7E-2,3.3000000000000002E-2,0.434,0.42399999999999999,0.54,0.67100000000000004,0.373,0.86,0.5,0.5,0.5,0.5,0.5,0.5,null,0.35,0.4,0.8,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,0.5,0.5,0.5,0.5,0.85,0.85,"NR","NR","NR","NR","NR","NR"]
["8 (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-2.6 c.i. insulation entirely above deck with a U-factor of 0.360","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity and R-3.3 continuous insulation with a U-factor of 0.212","steel-framed with R-2.3 cavity and R-0.7 continuous insulation with a U-factor of 0.479","205 mm medium weight concrete block with solid grouted cores and R-1.3 continuous insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and R-2.2 continuous insulation with a C-factor of 0.425","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-6.7 insulation with a U-factor of 0.183","steel-joist with R-6.7 insulation with a U-factor of 0.183","steel-joist with R-3.3 insulation with a U-factor of 0.296","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with R-3.5 insulation for 600 mm with an F-factor of 0.883","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.839","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 2.839",null,0.16,0.16,0.22,0.15,0.15,0.21,0.1,0.1,0.15,0.27,0.27,0.59,0.22,0.22,0.34,0.21,0.21,0.36,0.18,0.18,0.28999999999999998,0.36,0.36,0.68,0.22,0.22,0.36,0.18,0.18,0.3,0.15,0.15,0.19,0.75,0.73,0.94,1.1599999999999999,0.65,1.49,2.84,2.84,2.84,2.84,2.84,2.84,null,1.99,2.27,4.54,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,2.84,2.84,2.84,2.84,4.83,4.83,"NR","NR","NR","NR","NR","NR"]

{"sheet":"Envelope Lookup 90.1-2010","index":14,"n_rows":38,"n_cols":116,"rows_kept":38,"cut":false,"hidden":true,"merged":[[0,13,0,15],[0,16,0,18],[0,19,0,21],[0,44,0,46],[0,23,0,31],[0,32,0,43],[0,0,1,0],[0,1,0,3],[0,4,0,6],[0,7,0,9],[0,10,0,12],[0,47,0,55],[0,56,0,61],[0,99,0,104],[0,69,0,80],[0,81,0,92],[0,93,0,98],[0,62,0,67]]}
["Climate Zone","Roof Constructions",null,null,"Above-Grade Exterior Wall Constructions",null,null,"Below-Grade Exterior Wall Constructions",null,null,"Exposed Floor Constructions",null,null,"Slab-On-Grade Floors",null,null,"Opaque Doors - Swinging",null,null,"Opaque Doors - Nonwwinging",null,null,null,"Roof Constructions",null,null,null,null,null,null,null,null,"Above-Grade Exterior Wall Constructions",null,null,null,null,null,null,null,null,null,null,null,"Below-Grade Exterior Wall Constructions",null,null,"Exposed Floor Constructions",null,null,null,null,null,null,null,null,"Slab-On-Grade Floors",null,null,null,null,null,"Opaque Doors",null,null,null,null,null,null,"Vertical Glazing - Ufactor",null,null,null,null,null,null,null,null,null,null,null,"Vertical Glazing - SHGC",null,null,null,null,null,null,null,null,null,null,null,"Skylights - Ufactor",null,null,null,null,null,"Skylights - SHGC"]
[null,"Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated","Nonresidential","Residential","Semiheated",null,"Nonresidential Insulation Entirely above Deck","Residential Insulation Entirely above Deck","Semiheated Insulation Entirely above Deck","Nonresidential Metal Building","Residential Metal Building","Semiheated Metal Building","Nonresidential Attic and Other","Residential Attic and Other","Semiheated Attic and Other","Nonresidential Mass","Residential Mass","Semiheated Mass","Nonresidential Metal Building","Residential Metal Building","Semiheated Metal Building","Nonresidential Steel Framed","Residential Steel Framed","Semiheated Steel Framed","Nonresidential Wood Framed and Other","Residential Wood Framed and Other","Semiheated Wood Framed and Other","Nonresidential","Residential","Semiheated","Nonresidential Mass","Residential Mass","Semiheated Mass","Nonresidential Steel Joist","Residential Steel Joist","Semiheated Steel Joist","Nonresidential Wood Framed and Other","Residential Wood Framed and Other","Semiheated Wood Framed and Other","Nonresidential Unheated","Residential Unheated","Semiheated Unheated","Nonresidential Heated","Residential Heated","Semiheated Heated","Nonresidential Swinging","Residential Swinging","Semiheated Swinging","Nonresidential Nonswinging","Residential Nonswinging","Semiheated Nonswinging",null,"Nonresidential Nonmetal framing all","Residential Nonmetal framing all","Semiheated Nonmetal framing all","Residential Metal framing fixed","Residential Metal framing fixed","Semiheated Metal framing fixed","Nonresidential Metal framing operable","Residential Metal framing operable","Semiheated Metal framing operable","Nonresidential Metal framing entrance door","Residential Metal framing entrance door","Semiheated Metal framing entrance door","Nonresidential 0%-10.0%","Residential 0%-10.0%","Semiheated 0%-10.0%","Nonresidential 10.1%-20.0%","Residential 10.1%-20.0%","Semiheated 10.1%-20.0%","Nonresidential 20.1%-30.0%","Residential 20.1%-30.0%","Semiheated 20.1%-30.0%","Nonresidential 30.1%-40.0%","Residential 30.1%-40.0%","Semiheated 30.1%-40.0%","Nonresidential 0%-2.0%","Nonresidential 2.1%+","Residential 0%-2.0%","Residential 2.1%+","Seimiheated 0%-2.0%","Seimiheated 2.1%+","Nonresidential 0%-2.0%","Nonresidential 2.1%+","Residential 0%-2.0%","Residential 2.1%+","Seimiheated 0%-2.0%","Seimiheated 2.1%+",null,null,null,null,null,null,null,"Climate Zone","Nonresidential","Residential","Semiheated"]
["1A (IP)","R-15 insulation entirely above deck with a U-factor of 0.063","R-20 insulation entirely above deck with a U-factor of 0.048","R-3.8 insulation entirely above deck with a U-factor of 0.218","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with no insulation with a U-factor of 0.352","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with no insulation with a U-factor of 0.350","steel-joist with no insulation with a U-factor of 0.350","steel-joist with no insulation with a U-factor of 0.350","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 1.450","U-factor of 1.450",null,"U-0.063","U-0.048","U-0.218","U-0.063","U-0.048","U-0.218","U-0.063","U-0.048","U-0.218","U-0.124","U-0.124","U-0.352","U-0.124","U-0.124","U-0.352","U-0.124","U-0.124","U-0.352","U-0.124","U-0.124","U-0.352","C-1.140","C-1.140","C-1.140","U-0.350","U-0.350","U-0.350","U-0.350","U-0.350","U-0.350","U-0.350","U-0.350","U-0.350","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-1.450","U-1.450",null,1.2,1.2,1.2,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.98,1.98,1.98,1.98,1.98,1.98,0.36,0.19,0.34,0.27,0.36,0.19,null,null,null,null,null,null,"need to be updated, currently have CZ 4 values",1,"Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["1A (SI)","R-2.6 c.i. insulation entirely above deck with a U-factor of 0.360","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.7 c.i. insulation entirely above deck with a U-factor of 1.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with no insulation with a U-factor of 1.998","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with no insulation with a U-factor of 1.986","steel-joist with no insulation with a U-factor of 1.986","steel-joist with no insulation with a U-factor of 1.986","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 8.233","U-factor of 8.233",null,"U-0.360","U-0.273","U-1.240","U-0.360","U-0.273","U-1.240","U-0.360","U-0.273","U-1.240","U-0.705","U-0.705","U-1.998","U-0.705","U-0.705","U-1.998","U-0.705","U-0.705","U-1.998","U-0.705","U-0.705","U-1.998","C-6.473","C-6.473","C-6.473","U-1.986","U-1.986","U-1.986","U-1.986","U-1.986","U-1.986","U-1.986","U-1.986","U-1.986","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-8.233","U-8.233",null,6.81,6.81,6.81,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,11.24,11.24,11.24,11.24,11.24,11.24,0.36,0.19,0.34,0.27,0.36,0.19,null,null,null,null,null,null,"need to be updated, currently have CZ 4 values",2,"Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["1B (IP)","R-15 insulation entirely above deck with a U-factor of 0.063","R-20 insulation entirely above deck with a U-factor of 0.048","R-3.8 insulation entirely above deck with a U-factor of 0.218","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with no insulation with a U-factor of 0.352","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with no insulation with a U-factor of 0.350","steel-joist with no insulation with a U-factor of 0.350","steel-joist with no insulation with a U-factor of 0.350","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 1.450","U-factor of 1.450",null,"U-0.063","U-0.048","U-0.218","U-0.063","U-0.048","U-0.218","U-0.063","U-0.048","U-0.218","U-0.124","U-0.124","U-0.352","U-0.124","U-0.124","U-0.352","U-0.124","U-0.124","U-0.352","U-0.124","U-0.124","U-0.352","C-1.140","C-1.140","C-1.140","U-0.350","U-0.350","U-0.350","U-0.350","U-0.350","U-0.350","U-0.350","U-0.350","U-0.350","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-1.450","U-1.450",null,1.2,1.2,1.2,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.98,1.98,1.98,1.98,1.98,1.98,0.36,0.19,0.34,0.27,0.36,0.19,null,null,null,null,null,null,"need to be updated, currently have CZ 4 values",3,"Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["1B (SI)","R-2.6 c.i. insulation entirely above deck with a U-factor of 0.360","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.7 c.i. insulation entirely above deck with a U-factor of 1.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with no insulation with a U-factor of 1.998","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with no insulation with a U-factor of 1.986","steel-joist with no insulation with a U-factor of 1.986","steel-joist with no insulation with a U-factor of 1.986","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 8.233","U-factor of 8.233",null,"U-0.360","U-0.273","U-1.240","U-0.360","U-0.273","U-1.240","U-0.360","U-0.273","U-1.240","U-0.705","U-0.705","U-1.998","U-0.705","U-0.705","U-1.998","U-0.705","U-0.705","U-1.998","U-0.705","U-0.705","U-1.998","C-6.473","C-6.473","C-6.473","U-1.986","U-1.986","U-1.986","U-1.986","U-1.986","U-1.986","U-1.986","U-1.986","U-1.986","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-8.233","U-8.233",null,6.81,6.81,6.81,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,11.24,11.24,11.24,11.24,11.24,11.24,0.36,0.19,0.34,0.27,0.36,0.19,null,null,null,null,null,null,null,"4-Nonmetal framing all","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR"]
["2A (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-3.8 insulation entirely above deck with a U-factor of 0.218","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.218","U-0.048","U-0.048","U-0.218","U-0.048","U-0.048","U-0.218","U-0.124","U-0.064","U-0.124","U-0.124","U-0.064","U-0.124","U-0.124","U-0.064","U-0.124","U-0.124","U-0.064","U-0.124","C-1.140","C-1.140","C-1.140","U-0.052","U-0.052","U-0.069","U-0.052","U-0.052","U-0.069","U-0.052","U-0.052","U-0.069","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-0.500","U-1.450",null,0.75,0.7,1.1000000000000001,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.98,1.98,1.98,1.98,1.98,1.98,0.36,0.19,0.39,0.34,0.36,0.19,null,null,null,null,null,null,null,"4-Metal framing fixed","Metal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10","Metal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10","Metal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR"]
["2A (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.7 c.i. insulation entirely above deck with a U-factor of 1.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-1.240","U-0.273","U-0.273","U-1.240","U-0.273","U-0.273","U-1.240","U-0.705","U-0.365","U-0.705","U-0.705","U-0.365","U-0.705","U-0.705","U-0.365","U-0.705","U-0.705","U-0.365","U-0.705","C-6.473","C-6.473","C-6.473","U-0.296","U-0.296","U-0.390","U-0.296","U-0.296","U-0.390","U-0.296","U-0.296","U-0.390","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-2.839","U-8.233",null,4.26,3.97,6.25,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,11.24,11.24,11.24,11.24,11.24,11.24,0.36,0.19,0.39,0.34,0.36,0.19,null,null,null,null,null,null,null,"4-Metal framing operable","Metal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10","Metal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10","Metal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR"]
["2B (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-3.8 insulation entirely above deck with a U-factor of 0.218","steel-framed with R-13 cavity insulation with a U-factor of 0.124","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.218","U-0.048","U-0.048","U-0.218","U-0.048","U-0.048","U-0.218","U-0.124","U-0.064","U-0.124","U-0.124","U-0.064","U-0.124","U-0.124","U-0.064","U-0.124","U-0.124","U-0.064","U-0.124","C-1.140","C-1.140","C-1.140","U-0.052","U-0.052","U-0.069","U-0.052","U-0.052","U-0.069","U-0.052","U-0.052","U-0.069","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-0.500","U-1.450",null,0.75,0.7,1.1000000000000001,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.98,1.98,1.98,1.98,1.98,1.98,0.36,0.19,0.39,0.34,0.36,0.19,null,null,null,null,null,null,null,"4-Metal framing entrance door","Metal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Metal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Metal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["2B (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.7 c.i. insulation entirely above deck with a U-factor of 1.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-1.240","U-0.273","U-0.273","U-1.240","U-0.273","U-0.273","U-1.240","U-0.705","U-0.365","U-0.705","U-0.705","U-0.365","U-0.705","U-0.705","U-0.365","U-0.705","U-0.705","U-0.365","U-0.705","C-6.473","C-6.473","C-6.473","U-0.296","U-0.296","U-0.390","U-0.296","U-0.296","U-0.390","U-0.296","U-0.296","U-0.390","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-2.839","U-8.233",null,4.26,3.97,6.25,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,11.24,11.24,11.24,11.24,11.24,11.24,0.36,0.19,0.39,0.34,0.36,0.19,null,null,null,null,null,null,null,"5-Nonmetal framing all","Nonmetal framing, all: U-0.32; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.32; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.45; SHGC-NR; VT/SHGC-NR"]
["3A (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-5.0 insulation entirely above deck with a U-factor of 0.173","steel-framed with R-13 cavity and R-3.8 continuous insulation with a U-factor of 0.084","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.173","U-0.048","U-0.048","U-0.173","U-0.048","U-0.048","U-0.173","U-0.084","U-0.064","U-0.124","U-0.084","U-0.064","U-0.124","U-0.084","U-0.064","U-0.124","U-0.084","U-0.064","U-0.124","C-1.140","C-1.140","C-1.140","U-0.052","U-0.052","U-0.069","U-0.052","U-0.052","U-0.069","U-0.052","U-0.052","U-0.069","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-0.500","U-1.450",null,0.65,0.6,0.9,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.17,1.17,1.17,1.17,1.17,1.17,0.39,0.19,0.65,0.34,0.39,0.19,null,null,null,null,null,null,null,"5-Metal framing fixed","Metal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10","Metal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10","Metal framing, fixed: U-0.62; SHGC-NR; VT/SHGC-NR"]
["3A (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.9 c.i. insulation entirely above deck with a U-factor of 0.982","steel-framed with R-2.3 cavity and R-0.7 continuous insulation with a U-factor of 0.479","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-0.982","U-0.273","U-0.273","U-0.982","U-0.273","U-0.273","U-0.982","U-0.479","U-0.365","U-0.705","U-0.479","U-0.365","U-0.705","U-0.479","U-0.365","U-0.705","U-0.479","U-0.365","U-0.705","C-6.473","C-6.473","C-6.473","U-0.296","U-0.296","U-0.390","U-0.296","U-0.296","U-0.390","U-0.296","U-0.296","U-0.390","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-2.839","U-8.233",null,3.69,3.41,5.1100000000000003,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,6.64,6.64,6.64,6.64,6.64,6.64,0.39,0.19,0.65,0.34,0.39,0.19,null,null,null,null,null,null,null,"5-Metal framing operable","Metal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10","Metal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10","Metal framing, operable: U-0.70; SHGC-NR; VT/SHGC-NR"]
["3B (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-5.0 insulation entirely above deck with a U-factor of 0.173","steel-framed with R-13 cavity and R-3.8 continuous insulation with a U-factor of 0.084","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.173","U-0.048","U-0.048","U-0.173","U-0.048","U-0.048","U-0.173","U-0.084","U-0.064","U-0.124","U-0.084","U-0.064","U-0.124","U-0.084","U-0.064","U-0.124","U-0.084","U-0.064","U-0.124","C-1.140","C-1.140","C-1.140","U-0.052","U-0.052","U-0.069","U-0.052","U-0.052","U-0.069","U-0.052","U-0.052","U-0.069","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-0.500","U-1.450",null,0.65,0.6,0.9,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.17,1.17,1.17,1.17,1.17,1.17,0.39,0.19,0.65,0.34,0.39,0.19,null,null,null,null,null,null,null,"5-Metal framing entrance door","Metal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Metal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Metal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["3B (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.9 c.i. insulation entirely above deck with a U-factor of 0.982","steel-framed with R-2.3 cavity and R-0.7 continuous insulation with a U-factor of 0.479","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-0.982","U-0.273","U-0.273","U-0.982","U-0.273","U-0.273","U-0.982","U-0.479","U-0.365","U-0.705","U-0.479","U-0.365","U-0.705","U-0.479","U-0.365","U-0.705","U-0.479","U-0.365","U-0.705","C-6.473","C-6.473","C-6.473","U-0.296","U-0.296","U-0.390","U-0.296","U-0.296","U-0.390","U-0.296","U-0.296","U-0.390","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-2.839","U-8.233",null,3.69,3.41,5.1100000000000003,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,6.64,6.64,6.64,6.64,6.64,6.64,0.39,0.19,0.65,0.34,0.39,0.19,null,null,null,null,null,null,"need to be updated, currently have CZ 4 values",6,"Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["3C (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-5.0 insulation entirely above deck with a U-factor of 0.173","steel-framed with R-13 cavity and R-3.8 continuous insulation with a U-factor of 0.084","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-19 insulation with a U-factor of 0.052","steel-joist with R-13 insulation with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.173","U-0.048","U-0.048","U-0.173","U-0.048","U-0.048","U-0.173","U-0.084","U-0.064","U-0.124","U-0.084","U-0.064","U-0.124","U-0.084","U-0.064","U-0.124","U-0.084","U-0.064","U-0.124","C-1.140","C-1.140","C-1.140","U-0.052","U-0.052","U-0.069","U-0.052","U-0.052","U-0.069","U-0.052","U-0.052","U-0.069","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","F-0.730","U-0.700","U-0.700","U-0.700","U-1.450","U-0.500","U-1.450",null,0.65,0.6,0.9,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,1.17,1.17,1.17,1.17,1.17,1.17,0.39,0.19,0.65,0.34,0.39,0.19,null,null,null,null,null,null,"need to be updated, currently have CZ 4 values",7,"Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["3C (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-0.9 c.i. insulation entirely above deck with a U-factor of 0.982","steel-framed with R-2.3 cavity and R-0.7 continuous insulation with a U-factor of 0.479","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-3.3 insulation with a U-factor of 0.296","steel-joist with R-2.3 insulation with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-0.982","U-0.273","U-0.273","U-0.982","U-0.273","U-0.273","U-0.982","U-0.479","U-0.365","U-0.705","U-0.479","U-0.365","U-0.705","U-0.479","U-0.365","U-0.705","U-0.479","U-0.365","U-0.705","C-6.473","C-6.473","C-6.473","U-0.296","U-0.296","U-0.390","U-0.296","U-0.296","U-0.390","U-0.296","U-0.296","U-0.390","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","F-1.264","U-3.975","U-3.975","U-3.975","U-8.233","U-2.839","U-8.233",null,3.69,3.41,5.1100000000000003,null,null,null,null,null,null,null,null,null,0.25,0.25,0.25,null,null,null,null,null,null,0.25,0.25,0.25,6.64,6.64,6.64,6.64,6.64,6.64,0.39,0.19,0.65,0.34,0.39,0.19,null,null,null,null,null,null,"need to be updated, currently have CZ 4 values",8,"Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.77; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.35; SHGC-0.40; VT/SHGC-1.10\nMetal framing, fixed: U-0.42; SHGC-0.40; VT/SHGC-1.10\nMetal framing, operable: U-0.50; SHGC-0.40; VT/SHGC-1.10\nMetal framing, entrance door: U-0.68; SHGC-0.40; VT/SHGC-1.10","Nonmetal framing, all: U-0.51; SHGC-NR; VT/SHGC-NR\nMetal framing, fixed: U-0.73; SHGC-NR; VT/SHGC-NR\nMetal framing, operable: U-0.81; SHGC-NR; VT/SHGC-NR\nMetal framing, entrance door: U-0.77; SHGC-NR; VT/SHGC-NR"]
["4A (IP)","R-30 insulation entirely above deck with a U-factor of 0.032","R-30 insulation entirely above deck with a U-factor of 0.032","R-10 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with  R-15 insulation for 24 in.  with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,4.8000000000000001E-2,4.8000000000000001E-2,0.17299999999999999,5.5E-2,5.5E-2,9.7000000000000003E-2,2.7E-2,2.7E-2,5.2999999999999999E-2,0.104,0.09,0.57999999999999996,8.4000000000000005E-2,8.4000000000000005E-2,0.113,6.4000000000000001E-2,6.4000000000000001E-2,0.124,8.8999999999999996E-2,6.4000000000000001E-2,8.8999999999999996E-2,0.11899999999999999,9.1999999999999998E-2,1.1399999999999999,8.6999999999999994E-2,7.3999999999999996E-2,0.13700000000000001,3.7999999999999999E-2,3.7999999999999999E-2,6.9000000000000006E-2,3.3000000000000002E-2,3.3000000000000002E-2,6.6000000000000003E-2,0.73,0.54,0.73,0.86,0.86,1.02,0.7,0.7,0.7,0.5,0.5,1.45,null,0.4,0.4,1.2,0.5,0.5,1.2,0.85,0.85,1.2,0.55000000000000004,0.55000000000000004,1.2,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.5,0.5,0.5,0.5,1.1499999999999999,1.1499999999999999,0.4,0.4,0.4,0.4,"NR","NR"]
["4A (SI)","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.529","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.677","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.523","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.84","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.296","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.844","U-factor of 2.844","U-factor of 3.981","U-factor of 2.844","U-factor of 2.844","U-factor of 8.247",null,{"$f":"X17*5.678263","v":0.27255662400000003},{"$f":"Y17*5.678263","v":0.27255662400000003},0.98233949899999995,0.31230446500000003,0.31230446500000003,0.55079151100000001,0.15331310100000001,0.15331310100000001,{"$f":"AF17*5.678263","v":0.300947939},{"$f":"AG17*5.678263","v":0.59053935199999996},{"$f":"AH17*5.678263","v":0.51104367000000006},3.2933925400000001,0.47697409200000007,0.47697409200000007,0.64164371900000006,0.36340883200000001,0.36340883200000001,{"$f":"AO17*5.678263","v":0.70410461200000007},{"$f":"AP17*5.678263","v":0.50536540699999999},0.36340883200000001,{"$f":"AR17*5.678263","v":0.50536540699999999},0.66700000000000004,0.52300000000000002,6.484,{"$f":"AV17*5.678263","v":0.49400888100000001},0.42019146200000002,{"$f":"AX17*5.678263","v":0.77792203100000012},{"$f":"AY17*5.678263","v":0.215773994},0.215773994,{"$f":"BA17*5.678263","v":0.39180014700000004},0.66700000000000004,0.52300000000000002,6.484,{"$f":"BE17*1.7315","v":1.263995},{"$f":"BF17*1.7315","v":0.93501000000000012},1.263995,1.48909,1.48909,1.76613,{"$f":"BK17*5.678263","v":3.9747840999999999},{"$f":"BL17*5.678263","v":3.9747840999999999},{"$f":"BM17*5.678263","v":3.9747840999999999},{"$f":"BN17*5.678263","v":2.8391315000000001},{"$f":"BO17*5.678263","v":2.8391315000000001},{"$f":"BP17*5.678263","v":8.2334813499999999},null,{"$f":"BR17*5.678263","v":2.2713052},{"$f":"BS17*5.678263","v":2.2713052},6.8139156000000005,2.8391315000000001,2.8391315000000001,6.8139156000000005,4.8265235500000001,4.8265235500000001,6.8139156000000005,3.1230446500000002,3.1230446500000002,6.8139156000000005,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",2.84,2.84,2.84,2.84,6.53,6.53,0.4,0.4,0.4,0.4,"NR","NR"]
["4B (IP)","R-30 insulation entirely above deck with a U-factor of 0.032","R-30 insulation entirely above deck with a U-factor of 0.032","R-10 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with  R-15 insulation for 24 in.  with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,4.8000000000000001E-2,4.8000000000000001E-2,0.17299999999999999,5.5E-2,5.5E-2,9.7000000000000003E-2,2.7E-2,2.7E-2,5.2999999999999999E-2,0.104,0.09,0.57999999999999996,8.4000000000000005E-2,8.4000000000000005E-2,0.113,6.4000000000000001E-2,6.4000000000000001E-2,0.124,8.8999999999999996E-2,6.4000000000000001E-2,8.8999999999999996E-2,0.11899999999999999,9.1999999999999998E-2,1.1399999999999999,8.6999999999999994E-2,7.3999999999999996E-2,0.13700000000000001,3.7999999999999999E-2,3.7999999999999999E-2,6.9000000000000006E-2,3.3000000000000002E-2,3.3000000000000002E-2,6.6000000000000003E-2,0.73,0.54,0.73,0.86,0.86,1.02,0.7,0.7,0.7,0.5,0.5,1.45,null,0.4,0.4,1.2,0.5,0.5,1.2,0.85,0.85,1.2,0.55000000000000004,0.55000000000000004,1.2,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.5,0.5,0.5,0.5,1.1499999999999999,1.1499999999999999,0.4,0.4,0.4,0.4,"NR","NR"]
["4B (SI)","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.529","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.677","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.523","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.84","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.296","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.844","U-factor of 2.844","U-factor of 3.981","U-factor of 2.844","U-factor of 2.844","U-factor of 8.247",null,{"$f":"X19*5.678263","v":0.27255662400000003},{"$f":"Y19*5.678263","v":0.27255662400000003},0.98233949899999995,0.31230446500000003,0.31230446500000003,0.55079151100000001,0.15331310100000001,0.15331310100000001,{"$f":"AF19*5.678263","v":0.300947939},{"$f":"AG19*5.678263","v":0.59053935199999996},{"$f":"AH19*5.678263","v":0.51104367000000006},3.2933925400000001,0.47697409200000007,0.47697409200000007,0.64164371900000006,0.36340883200000001,0.36340883200000001,{"$f":"AO19*5.678263","v":0.70410461200000007},{"$f":"AP19*5.678263","v":0.50536540699999999},0.36340883200000001,{"$f":"AR19*5.678263","v":0.50536540699999999},0.66700000000000004,0.52300000000000002,6.484,{"$f":"AV19*5.678263","v":0.49400888100000001},0.42019146200000002,{"$f":"AX19*5.678263","v":0.77792203100000012},{"$f":"AY19*5.678263","v":0.215773994},0.215773994,{"$f":"BA19*5.678263","v":0.39180014700000004},0.66700000000000004,0.52300000000000002,6.484,{"$f":"BE19*1.7315","v":1.263995},{"$f":"BF19*1.7315","v":0.93501000000000012},1.263995,1.48909,1.48909,1.76613,{"$f":"BK19*5.678263","v":3.9747840999999999},{"$f":"BL19*5.678263","v":3.9747840999999999},{"$f":"BM19*5.678263","v":3.9747840999999999},{"$f":"BN19*5.678263","v":2.8391315000000001},{"$f":"BO19*5.678263","v":2.8391315000000001},{"$f":"BP19*5.678263","v":8.2334813499999999},null,{"$f":"BR19*5.678263","v":2.2713052},{"$f":"BS19*5.678263","v":2.2713052},{"$f":"BT19*5.678263","v":6.8139156000000005},{"$f":"BU19*5.678263","v":2.8391315000000001},{"$f":"BV19*5.678263","v":2.8391315000000001},{"$f":"BW19*5.678263","v":6.8139156000000005},{"$f":"BX19*5.678263","v":4.8265235500000001},{"$f":"BY19*5.678263","v":4.8265235500000001},{"$f":"BZ19*5.678263","v":6.8139156000000005},{"$f":"CA19*5.678263","v":3.1230446500000002},{"$f":"CB19*5.678263","v":3.1230446500000002},{"$f":"CC19*5.678263","v":6.8139156000000005},0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",2.84,2.84,2.84,2.84,6.53,6.53,0.4,0.4,0.4,0.4,"NR","NR"]
["4C (IP)","R-30 insulation entirely above deck with a U-factor of 0.032","R-30 insulation entirely above deck with a U-factor of 0.032","R-10 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with  R-15 insulation for 24 in.  with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,4.8000000000000001E-2,4.8000000000000001E-2,0.17299999999999999,5.5E-2,5.5E-2,9.7000000000000003E-2,2.7E-2,2.7E-2,5.2999999999999999E-2,0.104,0.09,0.57999999999999996,8.4000000000000005E-2,8.4000000000000005E-2,0.113,6.4000000000000001E-2,6.4000000000000001E-2,0.124,8.8999999999999996E-2,6.4000000000000001E-2,8.8999999999999996E-2,0.11899999999999999,9.1999999999999998E-2,1.1399999999999999,8.6999999999999994E-2,7.3999999999999996E-2,0.13700000000000001,3.7999999999999999E-2,3.7999999999999999E-2,6.9000000000000006E-2,3.3000000000000002E-2,3.3000000000000002E-2,6.6000000000000003E-2,0.73,0.54,0.73,0.86,0.86,1.02,0.7,0.7,0.7,0.5,0.5,1.45,null,0.4,0.4,1.2,0.5,0.5,1.2,0.85,0.85,1.2,0.55000000000000004,0.55000000000000004,1.2,0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.5,0.5,0.5,0.5,1.1499999999999999,1.1499999999999999,0.4,0.4,0.4,0.4,"NR","NR"]
["4C (SI)","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.182","Insulation entirely above deck with a U-factor of 0.529","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.364","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.677","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.523","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.84","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.216","steel-joist with a U-factor of 0.296","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.844","U-factor of 2.844","U-factor of 3.981","U-factor of 2.844","U-factor of 2.844","U-factor of 8.247",null,{"$f":"X21*5.678263","v":0.27255662400000003},{"$f":"Y21*5.678263","v":0.27255662400000003},0.98233949899999995,0.31230446500000003,0.31230446500000003,0.55079151100000001,0.15331310100000001,0.15331310100000001,{"$f":"AF21*5.678263","v":0.300947939},{"$f":"AG21*5.678263","v":0.59053935199999996},{"$f":"AH21*5.678263","v":0.51104367000000006},3.2933925400000001,0.47697409200000007,0.47697409200000007,0.64164371900000006,0.36340883200000001,0.36340883200000001,{"$f":"AO21*5.678263","v":0.70410461200000007},{"$f":"AP21*5.678263","v":0.50536540699999999},0.36340883200000001,{"$f":"AR21*5.678263","v":0.50536540699999999},0.66700000000000004,0.52300000000000002,6.484,{"$f":"AV21*5.678263","v":0.49400888100000001},0.42019146200000002,{"$f":"AX21*5.678263","v":0.77792203100000012},{"$f":"AY21*5.678263","v":0.215773994},0.215773994,{"$f":"BA21*5.678263","v":0.39180014700000004},0.66700000000000004,0.52300000000000002,6.484,{"$f":"BE21*1.7315","v":1.263995},{"$f":"BF21*1.7315","v":0.93501000000000012},1.263995,1.48909,1.48909,1.76613,{"$f":"BK21*5.678263","v":3.9747840999999999},{"$f":"BL21*5.678263","v":3.9747840999999999},{"$f":"BM21*5.678263","v":3.9747840999999999},{"$f":"BN21*5.678263","v":2.8391315000000001},{"$f":"BO21*5.678263","v":2.8391315000000001},{"$f":"BP21*5.678263","v":8.2334813499999999},null,{"$f":"BR21*5.678263","v":2.2713052},{"$f":"BS21*5.678263","v":2.2713052},{"$f":"BT21*5.678263","v":6.8139156000000005},{"$f":"BU21*5.678263","v":2.8391315000000001},{"$f":"BV21*5.678263","v":2.8391315000000001},{"$f":"BW21*5.678263","v":6.8139156000000005},{"$f":"BX21*5.678263","v":4.8265235500000001},{"$f":"BY21*5.678263","v":4.8265235500000001},{"$f":"BZ21*5.678263","v":6.8139156000000005},{"$f":"CA21*5.678263","v":3.1230446500000002},{"$f":"CB21*5.678263","v":3.1230446500000002},{"$f":"CC21*5.678263","v":6.8139156000000005},0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",0.4,0.4,"NR",2.84,2.84,2.84,2.84,6.53,6.53,0.4,0.4,0.4,0.4,"NR","NR"]
["5A (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,4.8000000000000001E-2,4.8000000000000001E-2,0.11899999999999999,5.5E-2,5.5E-2,8.3000000000000004E-2,2.7E-2,2.7E-2,5.2999999999999999E-2,0.09,0.08,0.151,6.9000000000000006E-2,6.9000000000000006E-2,0.113,6.4000000000000001E-2,6.4000000000000001E-2,0.124,6.4000000000000001E-2,5.0999999999999997E-2,8.8999999999999996E-2,"C-1.140","C-1.140","C-1.140",7.3999999999999996E-2,6.4000000000000001E-2,0.13700000000000001,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,5.0999999999999997E-2,0.73,0.54,0.73,0.86,0.86,1.02,0.7,0.5,0.7,0.5,0.5,1.45,null,0.35,0.35,1.2,0.45,0.45,1.2,0.8,0.8,1.2,0.55000000000000004,0.55000000000000004,1.2,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",1.17,1.17,1.17,1.17,1.17,1.17,0.49,0.39,0.77,0.62,0.49,0.39]
["5A (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,{"$f":"X23*5.678263","v":0.27255662400000003},{"$f":"Y23*5.678263","v":0.27255662400000003},0.67571329700000005,0.31230446500000003,0.31230446500000003,0.47129582900000005,0.15331310100000001,0.15331310100000001,{"$f":"AF23*5.678263","v":0.300947939},{"$f":"AG23*5.678263","v":0.51104367000000006},{"$f":"AH23*5.678263","v":0.45426104},0.85741771300000003,0.39180014700000004,0.39180014700000004,0.64164371900000006,0.36340883200000001,0.36340883200000001,{"$f":"AO23*5.678263","v":0.70410461200000007},{"$f":"AP23*5.678263","v":0.36340883200000001},0.28959141300000002,{"$f":"AR23*5.678263","v":0.50536540699999999},"C-6.473","C-6.473","C-6.473",{"$f":"AV23*5.678263","v":0.42019146200000002},0.36340883200000001,{"$f":"AX23*5.678263","v":0.77792203100000012},{"$f":"AY23*5.678263","v":0.215773994},0.215773994,{"$f":"BA23*5.678263","v":0.29526967599999998},0.66700000000000004,0.52300000000000002,6.484,{"$f":"BE23*1.7315","v":1.263995},{"$f":"BF23*1.7315","v":0.93501000000000012},1.263995,1.48909,1.48909,1.76613,{"$f":"BK23*5.678263","v":3.9747840999999999},{"$f":"BL23*5.678263","v":2.8391315000000001},{"$f":"BM23*5.678263","v":3.9747840999999999},{"$f":"BN23*5.678263","v":2.8391315000000001},{"$f":"BO23*5.678263","v":2.8391315000000001},{"$f":"BP23*5.678263","v":8.2334813499999999},null,{"$f":"BR23*5.678263","v":1.98739205},{"$f":"BS23*5.678263","v":1.98739205},{"$f":"BT23*5.678263","v":6.8139156000000005},{"$f":"BU23*5.678263","v":2.5552183500000001},{"$f":"BV23*5.678263","v":2.5552183500000001},{"$f":"BW23*5.678263","v":6.8139156000000005},{"$f":"BX23*5.678263","v":4.5426104},{"$f":"BY23*5.678263","v":4.5426104},{"$f":"BZ23*5.678263","v":6.8139156000000005},{"$f":"CA23*5.678263","v":3.1230446500000002},{"$f":"CB23*5.678263","v":3.1230446500000002},{"$f":"CC23*5.678263","v":6.8139156000000005},0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",6.64,6.64,6.64,6.64,6.64,6.64,0.49,0.39,0.77,0.62,0.49,0.39]
["5B (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,4.8000000000000001E-2,4.8000000000000001E-2,0.11899999999999999,5.5E-2,5.5E-2,8.3000000000000004E-2,2.7E-2,2.7E-2,5.2999999999999999E-2,0.09,0.08,0.151,6.9000000000000006E-2,6.9000000000000006E-2,0.113,6.4000000000000001E-2,6.4000000000000001E-2,0.124,6.4000000000000001E-2,5.0999999999999997E-2,8.8999999999999996E-2,"C-1.140","C-1.140","C-1.140",7.3999999999999996E-2,6.4000000000000001E-2,0.13700000000000001,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,5.0999999999999997E-2,0.73,0.54,0.73,0.86,0.86,1.02,0.7,0.5,0.7,0.5,0.5,1.45,null,0.35,0.35,1.2,0.45,0.45,1.2,0.8,0.8,1.2,0.55000000000000004,0.55000000000000004,1.2,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",1.17,1.17,1.17,1.17,1.17,1.17,0.49,0.39,0.77,0.62,0.49,0.39]
["5B (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,{"$f":"X25*5.678263","v":0.27255662400000003},{"$f":"Y25*5.678263","v":0.27255662400000003},0.67571329700000005,0.31230446500000003,0.31230446500000003,0.47129582900000005,0.15331310100000001,0.15331310100000001,{"$f":"AF25*5.678263","v":0.300947939},{"$f":"AG25*5.678263","v":0.51104367000000006},{"$f":"AH25*5.678263","v":0.45426104},0.85741771300000003,0.39180014700000004,0.39180014700000004,0.64164371900000006,0.36340883200000001,0.36340883200000001,{"$f":"AO25*5.678263","v":0.70410461200000007},{"$f":"AP25*5.678263","v":0.36340883200000001},0.28959141300000002,{"$f":"AR25*5.678263","v":0.50536540699999999},"C-6.473","C-6.473","C-6.473",{"$f":"AV25*5.678263","v":0.42019146200000002},0.36340883200000001,{"$f":"AX25*5.678263","v":0.77792203100000012},{"$f":"AY25*5.678263","v":0.215773994},0.215773994,{"$f":"BA25*5.678263","v":0.29526967599999998},0.66700000000000004,0.52300000000000002,6.484,{"$f":"BE25*1.7315","v":1.263995},{"$f":"BF25*1.7315","v":0.93501000000000012},1.263995,1.48909,1.48909,1.76613,{"$f":"BK25*5.678263","v":3.9747840999999999},{"$f":"BL25*5.678263","v":2.8391315000000001},{"$f":"BM25*5.678263","v":3.9747840999999999},{"$f":"BN25*5.678263","v":2.8391315000000001},{"$f":"BO25*5.678263","v":2.8391315000000001},{"$f":"BP25*5.678263","v":8.2334813499999999},null,{"$f":"BR25*5.678263","v":1.98739205},{"$f":"BS25*5.678263","v":1.98739205},{"$f":"BT25*5.678263","v":6.8139156000000005},{"$f":"BU25*5.678263","v":2.5552183500000001},{"$f":"BV25*5.678263","v":2.5552183500000001},{"$f":"BW25*5.678263","v":6.8139156000000005},{"$f":"BX25*5.678263","v":4.5426104},{"$f":"BY25*5.678263","v":4.5426104},{"$f":"BZ25*5.678263","v":6.8139156000000005},{"$f":"CA25*5.678263","v":3.1230446500000002},{"$f":"CB25*5.678263","v":3.1230446500000002},{"$f":"CC25*5.678263","v":6.8139156000000005},0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",6.64,6.64,6.64,6.64,6.64,6.64,0.49,0.39,0.77,0.62,0.49,0.39]
["5C (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.052","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.700","U-factor of 0.700","U-factor of 1.450","U-factor of 0.500","U-factor of 1.450",null,4.8000000000000001E-2,4.8000000000000001E-2,0.11899999999999999,5.5E-2,5.5E-2,8.3000000000000004E-2,2.7E-2,2.7E-2,5.2999999999999999E-2,0.09,0.08,0.151,6.9000000000000006E-2,6.9000000000000006E-2,0.113,6.4000000000000001E-2,6.4000000000000001E-2,0.124,6.4000000000000001E-2,5.0999999999999997E-2,8.8999999999999996E-2,"C-1.140","C-1.140","C-1.140",7.3999999999999996E-2,6.4000000000000001E-2,0.13700000000000001,3.7999999999999999E-2,3.7999999999999999E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,5.0999999999999997E-2,0.73,0.54,0.73,0.86,0.86,1.02,0.7,0.5,0.7,0.5,0.5,1.45,null,0.35,0.35,1.2,0.45,0.45,1.2,0.8,0.8,1.2,0.55000000000000004,0.55000000000000004,1.2,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",1.17,1.17,1.17,1.17,1.17,1.17,0.49,0.39,0.77,0.62,0.49,0.39]
["5C (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.296","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 3.975","U-factor of 3.975","U-factor of 8.233","U-factor of 2.839","U-factor of 8.233",null,{"$f":"X27*5.678263","v":0.27255662400000003},{"$f":"Y27*5.678263","v":0.27255662400000003},0.67571329700000005,0.31230446500000003,0.31230446500000003,0.47129582900000005,0.15331310100000001,0.15331310100000001,{"$f":"AF27*5.678263","v":0.300947939},{"$f":"AG27*5.678263","v":0.51104367000000006},{"$f":"AH27*5.678263","v":0.45426104},0.85741771300000003,0.39180014700000004,0.39180014700000004,0.64164371900000006,0.36340883200000001,0.36340883200000001,{"$f":"AO27*5.678263","v":0.70410461200000007},{"$f":"AP27*5.678263","v":0.36340883200000001},0.28959141300000002,{"$f":"AR27*5.678263","v":0.50536540699999999},"C-6.473","C-6.473","C-6.473",{"$f":"AV27*5.678263","v":0.42019146200000002},0.36340883200000001,{"$f":"AX27*5.678263","v":0.77792203100000012},{"$f":"AY27*5.678263","v":0.215773994},0.215773994,{"$f":"BA27*5.678263","v":0.29526967599999998},0.66700000000000004,0.52300000000000002,6.484,{"$f":"BE27*1.7315","v":1.263995},{"$f":"BF27*1.7315","v":0.93501000000000012},1.263995,1.48909,1.48909,1.76613,{"$f":"BK27*5.678263","v":3.9747840999999999},{"$f":"BL27*5.678263","v":2.8391315000000001},{"$f":"BM27*5.678263","v":3.9747840999999999},{"$f":"BN27*5.678263","v":2.8391315000000001},{"$f":"BO27*5.678263","v":2.8391315000000001},{"$f":"BP27*5.678263","v":8.2334813499999999},null,{"$f":"BR27*5.678263","v":1.98739205},{"$f":"BS27*5.678263","v":1.98739205},{"$f":"BT27*5.678263","v":6.8139156000000005},{"$f":"BU27*5.678263","v":2.5552183500000001},{"$f":"BV27*5.678263","v":2.5552183500000001},{"$f":"BW27*5.678263","v":6.8139156000000005},{"$f":"BX27*5.678263","v":4.5426104},{"$f":"BY27*5.678263","v":4.5426104},{"$f":"BZ27*5.678263","v":6.8139156000000005},{"$f":"CA27*5.678263","v":3.1230446500000002},{"$f":"CB27*5.678263","v":3.1230446500000002},{"$f":"CC27*5.678263","v":6.8139156000000005},0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",6.64,6.64,6.64,6.64,6.64,6.64,0.49,0.39,0.77,0.62,0.49,0.39]
["6A (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,4.8000000000000001E-2,4.8000000000000001E-2,9.2999999999999999E-2,4.9000000000000002E-2,4.9000000000000002E-2,7.1999999999999995E-2,2.7E-2,2.7E-2,3.4000000000000002E-2,0.08,7.0999999999999994E-2,0.151,6.9000000000000006E-2,6.9000000000000006E-2,0.113,6.4000000000000001E-2,6.4000000000000001E-2,0.124,5.0999999999999997E-2,5.0999999999999997E-2,8.8999999999999996E-2,"C-1.140","C-0.119","C-1.140",6.4000000000000001E-2,5.7000000000000002E-2,0.13700000000000001,3.7999999999999999E-2,3.2000000000000001E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,5.0999999999999997E-2,0.54,0.52,0.73,0.86,0.68799999999999994,1.02,0.7,0.5,0.7,0.5,0.5,1.45,null,0.35,0.35,0.65,0.45,0.45,0.6,0.8,0.8,0.9,0.55000000000000004,0.55000000000000004,0.65,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",1.17,1.17,1.17,1.17,1.17,1.17,0.49,0.49,0.71,0.57999999999999996,0.49,0.49]
["6A (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.260","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,{"$f":"X29*5.678263","v":0.27255662400000003},{"$f":"Y29*5.678263","v":0.27255662400000003},0.52807845900000006,0.27823488700000004,0.27823488700000004,0.40883493599999998,0.15331310100000001,0.15331310100000001,{"$f":"AF29*5.678263","v":0.19306094200000001},{"$f":"AG29*5.678263","v":0.45426104},{"$f":"AH29*5.678263","v":0.40315667299999997},0.85741771300000003,0.39180014700000004,0.39180014700000004,0.64164371900000006,0.36340883200000001,0.36340883200000001,{"$f":"AO29*5.678263","v":0.70410461200000007},{"$f":"AP29*5.678263","v":0.28959141300000002},0.28959141300000002,{"$f":"AR29*5.678263","v":0.50536540699999999},"C-6.473","C-0.678","C-6.473",{"$f":"AV29*5.678263","v":0.36340883200000001},0.32366099100000001,{"$f":"AX29*5.678263","v":0.77792203100000012},{"$f":"AY29*5.678263","v":0.215773994},0.18170441600000001,{"$f":"BA29*5.678263","v":0.29526967599999998},0.66700000000000004,0.52300000000000002,6.484,{"$f":"BE29*1.7315","v":0.93501000000000012},{"$f":"BF29*1.7315","v":0.90038000000000007},1.263995,1.48909,1.1912719999999999,1.76613,{"$f":"BK29*5.678263","v":3.9747840999999999},{"$f":"BL29*5.678263","v":2.8391315000000001},{"$f":"BM29*5.678263","v":3.9747840999999999},{"$f":"BN29*5.678263","v":2.8391315000000001},{"$f":"BO29*5.678263","v":2.8391315000000001},{"$f":"BP29*5.678263","v":8.2334813499999999},null,{"$f":"BR29*5.678263","v":1.98739205},{"$f":"BS29*5.678263","v":1.98739205},{"$f":"BT29*5.678263","v":3.6908709500000003},{"$f":"BU29*5.678263","v":2.5552183500000001},{"$f":"BV29*5.678263","v":2.5552183500000001},{"$f":"BW29*5.678263","v":3.4069578000000003},{"$f":"BX29*5.678263","v":4.5426104},{"$f":"BY29*5.678263","v":4.5426104},{"$f":"BZ29*5.678263","v":5.1104367000000002},{"$f":"CA29*5.678263","v":3.1230446500000002},{"$f":"CB29*5.678263","v":3.1230446500000002},{"$f":"CC29*5.678263","v":3.6908709500000003},0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",6.64,6.64,6.64,6.64,6.64,6.64,0.49,0.49,0.71,0.57999999999999996,0.49,0.49]
["6B (IP)","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.063","Insulation entirely above deck with a U-factor of 0.173","steel-framed with a U-factor of 0.084","steel-framed with a U-factor of 0.064","steel-framed with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.038","steel-joist with a U-factor of 0.069","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.700","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,4.8000000000000001E-2,4.8000000000000001E-2,9.2999999999999999E-2,4.9000000000000002E-2,4.9000000000000002E-2,7.1999999999999995E-2,2.7E-2,2.7E-2,3.4000000000000002E-2,0.08,7.0999999999999994E-2,0.151,6.9000000000000006E-2,6.9000000000000006E-2,0.113,6.4000000000000001E-2,6.4000000000000001E-2,0.124,5.0999999999999997E-2,5.0999999999999997E-2,8.8999999999999996E-2,"C-1.140","C-0.119","C-1.140",6.4000000000000001E-2,5.7000000000000002E-2,0.13700000000000001,3.7999999999999999E-2,3.2000000000000001E-2,5.1999999999999998E-2,3.3000000000000002E-2,3.3000000000000002E-2,5.0999999999999997E-2,0.54,0.52,0.73,0.86,0.68799999999999994,1.02,0.7,0.5,0.7,0.5,0.5,1.45,null,0.35,0.35,0.65,0.45,0.45,0.6,0.8,0.8,0.9,0.55000000000000004,0.55000000000000004,0.65,0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",1.17,1.17,1.17,1.17,1.17,1.17,0.49,0.49,0.71,0.57999999999999996,0.49,0.49]
["6B (SI)","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.360","Insulation entirely above deck with a U-factor of 0.982","steel-framed with a U-factor of 0.479","steel-framed with a U-factor of 0.365","steel-framed with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.214","steel-joist with a U-factor of 0.390","150 mm concrete slabs with no insulation with an F-factor of 1.264","150 mm concrete slabs with no insulation with an F-factor of 1.260","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 3.975","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,{"$f":"X31*5.678263","v":0.27255662400000003},{"$f":"Y31*5.678263","v":0.27255662400000003},0.52807845900000006,0.27823488700000004,0.27823488700000004,0.40883493599999998,0.15331310100000001,0.15331310100000001,{"$f":"AF31*5.678263","v":0.19306094200000001},{"$f":"AG31*5.678263","v":0.45426104},{"$f":"AH31*5.678263","v":0.40315667299999997},0.85741771300000003,0.39180014700000004,0.39180014700000004,0.64164371900000006,0.36340883200000001,0.36340883200000001,{"$f":"AO31*5.678263","v":0.70410461200000007},{"$f":"AP31*5.678263","v":0.28959141300000002},0.28959141300000002,{"$f":"AR31*5.678263","v":0.50536540699999999},"C-6.473","C-0.678","C-6.473",{"$f":"AV31*5.678263","v":0.36340883200000001},0.32366099100000001,{"$f":"AX31*5.678263","v":0.77792203100000012},{"$f":"AY31*5.678263","v":0.215773994},0.18170441600000001,{"$f":"BA31*5.678263","v":0.29526967599999998},0.66700000000000004,0.52300000000000002,6.484,{"$f":"BE31*1.7315","v":0.93501000000000012},{"$f":"BF31*1.7315","v":0.90038000000000007},1.263995,1.48909,1.1912719999999999,1.76613,{"$f":"BK31*5.678263","v":3.9747840999999999},{"$f":"BL31*5.678263","v":2.8391315000000001},{"$f":"BM31*5.678263","v":3.9747840999999999},2.8391315000000001,2.8391315000000001,8.2334813499999999,null,{"$f":"BR31*5.678263","v":1.98739205},{"$f":"BS31*5.678263","v":1.98739205},{"$f":"BT31*5.678263","v":3.6908709500000003},{"$f":"BU31*5.678263","v":2.5552183500000001},{"$f":"BV31*5.678263","v":2.5552183500000001},{"$f":"BW31*5.678263","v":3.4069578000000003},{"$f":"BX31*5.678263","v":4.5426104},{"$f":"BY31*5.678263","v":4.5426104},{"$f":"BZ31*5.678263","v":5.1104367000000002},{"$f":"CA31*5.678263","v":3.1230446500000002},{"$f":"CB31*5.678263","v":3.1230446500000002},{"$f":"CC31*5.678263","v":3.6908709500000003},0.49,0.49,"NR",0.39,0.39,"NR",0.39,0.39,"NR",0.39,0.39,"NR",6.64,6.64,6.64,6.64,6.64,6.64,0.49,0.49,0.71,0.57999999999999996,0.49,0.49]
["7A (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-10.0 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-15.6 continuous insulation with a U-factor of 0.042","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10.0 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-38 insulation with a U-factor of 0.032","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.093","U-0.048","U-0.048","U-0.093","U-0.048","U-0.048","U-0.093","U-0.064","U-0.042","U-0.124","U-0.064","U-0.042","U-0.124","U-0.064","U-0.042","U-0.124","U-0.064","U-0.042","U-0.124","C-0.119","C-0.092","C-1.140","U-0.038","U-0.032","U- 0.052","U-0.038","U-0.032","U- 0.052","U-0.038","U-0.032","U- 0.052","F-0.520","F-0.520","F-0.730","F-0.520","F-0.520","F-0.730","U-0.500","U-0.500","U-0.700","U-0.500","U-0.500","U-1.450",null,0.35,0.4,0.8,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,1.17,1.17,1.17,1.17,1.17,1.17,0.68,0.64,0.77,0.71,0.68,0.64]
["7A (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-1.8 insulation entirely above deck with a U-factor of 0.527","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity and R-2.7 continuous insulation with a U-factor of 0.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and R-1.3 continuous insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and R-1.8 continuous insulation with a C-factor of 0.522","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-5.3 insulation with a U-factor of 0.214","steel-joist with R-6.7 insulation with a U-factor of 0.183","steel-joist with R-3.3 insulation with a U-factor of 0.296","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.839","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-0.527","U-0.273","U-0.273","U-0.527","U-0.273","U-0.273","U-0.527","U-0.365","U-0.240","U-0.705","U-0.365","U-0.240","U-0.705","U-0.365","U-0.240","U-0.705","U-0.365","U-0.240","U-0.705","C-0.678","C-0.522","C-6.473","U-0.214","U-0.183","U- 0.296","U-0.214","U-0.183","U- 0.296","U-0.214","U-0.183","U- 0.296","F-0.900","F-0.900","F-1.264","F-0.900","F-0.900","F-1.264","U-2.839","U-2.839","U-3.975","U-2.839","U-2.839","U-8.233",null,0.35,0.4,0.8,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,6.64,6.64,6.64,6.64,6.64,6.64,0.68,0.64,0.77,0.71,0.68,0.64]
["7B (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-10.0 insulation entirely above deck with a U-factor of 0.093","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-15.6 continuous insulation with a U-factor of 0.042","steel-framed with R-13 cavity insulation with a U-factor of 0.124","8\" medium weight concrete block with solid grouted cores and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-10.0 insulation with a C-factor of 0.092","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-30 insulation with a U-factor of 0.038","steel-joist with R-38 insulation with a U-factor of 0.032","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 1.450",null,"U-0.048","U-0.048","U-0.093","U-0.048","U-0.048","U-0.093","U-0.048","U-0.048","U-0.093","U-0.064","U-0.042","U-0.124","U-0.064","U-0.042","U-0.124","U-0.064","U-0.042","U-0.124","U-0.064","U-0.042","U-0.124","C-0.119","C-0.092","C-1.140","U-0.038","U-0.032","U- 0.052","U-0.038","U-0.032","U- 0.052","U-0.038","U-0.032","U- 0.052","F-0.520","F-0.520","F-0.730","F-0.520","F-0.520","F-0.730","U-0.500","U-0.500","U-0.700","U-0.500","U-0.500","U-1.450",null,0.35,0.4,0.8,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,1.17,1.17,1.17,1.17,1.17,1.17,0.68,0.64,0.77,0.71,0.68,0.64]
["7B (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-1.8 insulation entirely above deck with a U-factor of 0.527","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity and R-2.7 continuous insulation with a U-factor of 0.240","steel-framed with R-2.3 cavity insulation with a U-factor of 0.705","205 mm medium weight concrete block with solid grouted cores and R-1.3 continuous insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and R-1.8 continuous insulation with a C-factor of 0.522","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-5.3 insulation with a U-factor of 0.214","steel-joist with R-6.7 insulation with a U-factor of 0.183","steel-joist with R-3.3 insulation with a U-factor of 0.296","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.839","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 8.233",null,"U-0.273","U-0.273","U-0.527","U-0.273","U-0.273","U-0.527","U-0.273","U-0.273","U-0.527","U-0.365","U-0.240","U-0.705","U-0.365","U-0.240","U-0.705","U-0.365","U-0.240","U-0.705","U-0.365","U-0.240","U-0.705","C-0.678","C-0.522","C-6.473","U-0.214","U-0.183","U- 0.296","U-0.214","U-0.183","U- 0.296","U-0.214","U-0.183","U- 0.296","F-0.900","F-0.900","F-1.264","F-0.900","F-0.900","F-1.264","U-2.839","U-2.839","U-3.975","U-2.839","U-2.839","U-8.233",null,1.99,2.27,4.54,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,6.64,6.64,6.64,6.64,6.64,6.64,0.68,0.64,0.77,0.71,0.68,0.64]
["8 (IP)","R-20 insulation entirely above deck with a U-factor of 0.048","R-20 insulation entirely above deck with a U-factor of 0.048","R-15.0 insulation entirely above deck with a U-factor of 0.063","steel-framed with R-13 cavity and R-7.5 continuous insulation with a U-factor of 0.064","steel-framed with R-13 cavity and R-18.8 continuous insulation with a U-factor of 0.037","steel-framed with R-13 cavity and R-3.8 continuous insulation with a U-factor of 0.084","8\" medium weight concrete block with solid grouted cores and R-7.5 insulation with a C-factor of 0.119","8\" medium weight concrete block with solid grouted cores and R-12.5 insulation with a C-factor of 0.075","8\" medium weight concrete block with solid grouted cores and no insulation with a C-factor of 1.140","steel-joist with R-38 insulation with a U-factor of 0.032","steel-joist with R-38 insulation with a U-factor of 0.032","steel-joist with R-19 insulation with a U-factor of 0.052","6\" concrete slabs with R-15 insulation for 24 in. with an F-factor of 0.520","6\" concrete slabs with R-20 insulation for 24 in. with an F-factor of 0.510","6\" concrete slabs with no insulation with an F-factor of 0.730","U-factor of 0.500","U-factor of 0.500","U-factor of 0.700","U-factor of 0.500","U-factor of 0.500","U-factor of 0.500",null,"U-0.048","U-0.048","U-0.063","U-0.048","U-0.048","U-0.063","U-0.048","U-0.048","U-0.063","U-0.064","U-0.037","U-0.084","U-0.064","U-0.037","U-0.084","U-0.064","U-0.037","U-0.084","U-0.064","U-0.037","U-0.084","C-0.119","C-0.075","C-1.140","U-0.032","U-0.032","U- 0.052","U-0.032","U-0.032","U- 0.052","U-0.032","U-0.032","U- 0.052","F-0.520","F-0.510","F-0.730","F-0.520","F-0.510","F-0.730","U-0.500","U-0.500","U-0.700","U-0.500","U-0.500","U-0.500",null,0.35,0.4,0.8,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,0.98,0.98,0.98,0.98,0.98,0.98,0.68,0.64,0.77,0.71,0.68,0.64]
["8 (SI)","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-3.5 c.i. insulation entirely above deck with a U-factor of 0.273","R-2.6 c.i. insulation entirely above deck with a U-factor of 0.360","steel-framed with R-2.3 cavity and R-1.3 continuous insulation with a U-factor of 0.365","steel-framed with R-2.3 cavity and R-3.3 continuous insulation with a U-factor of 0.212","steel-framed with R-2.3 cavity and R-0.7 continuous insulation with a U-factor of 0.479","205 mm medium weight concrete block with solid grouted cores and R-1.3 continuous insulation with a C-factor of 0.678","205 mm medium weight concrete block with solid grouted cores and R-2.2 continuous insulation with a C-factor of 0.425","205 mm medium weight concrete block with solid grouted cores and no insulation with a C-factor of 6.473","steel-joist with R-6.7 insulation with a U-factor of 0.183","steel-joist with R-6.7 insulation with a U-factor of 0.183","steel-joist with R-3.3 insulation with a U-factor of 0.296","150 mm concrete slabs with R-2.6 insulation for 600 mm with an F-factor of 0.900","150 mm concrete slabs with R-3.5 insulation for 600 mm with an F-factor of 0.883","150 mm concrete slabs with no insulation with an F-factor of 1.264","U-factor of 2.839","U-factor of 2.839","U-factor of 3.975","U-factor of 2.839","U-factor of 2.839","U-factor of 2.839",null,"U-0.273","U-0.273","U-0.360","U-0.273","U-0.273","U-0.360","U-0.273","U-0.273","U-0.360","U-0.365","U-0.212","U-0.479","U-0.365","U-0.212","U-0.479","U-0.365","U-0.212","U-0.479","U-0.365","U-0.212","U-0.479","C-0.678","C-0.425","C-6.473","U-0.183","U-0.183","U- 0.296","U-0.183","U-0.183","U- 0.296","U-0.183","U-0.183","U- 0.296","F-0.900","F-0.883","F-1.264","F-0.900","F-0.883","F-1.264","U-2.839","U-2.839","U-3.975","U-2.839","U-2.839","U-2.839",null,1.99,2.27,4.54,null,null,null,null,null,null,null,null,null,0.45,0.45,0.45,null,null,null,null,null,null,0.45,0.45,0.45,5.56,5.56,5.56,5.56,5.56,5.56,"NR","NR","NR","NR","NR","NR"]

{"sheet":"6a - Lighting Counts","index":15,"n_rows":551,"n_cols":63,"rows_kept":551,"cut":false,"hidden":false,"merged":[[27,8,27,35],[25,3,25,6],[24,48,24,49],[20,3,20,7],[20,8,20,13],[21,3,21,7],[22,3,22,7],[23,3,23,7],[24,3,24,7],[24,45,24,47],[6,3,6,12],[13,3,13,13],[14,3,14,13],[19,3,19,7],[19,8,19,13],[15,3,15,13]]}
[]
[null,null,"Lighting Counts"]
[]
[null,null,"INSTRUCTIONS:"]
[null,null,1,{"$f":"\"Enter data as instructed in Steps 1-3, starting at row \"&ROW(C22)&\".\"","v":"Enter data as instructed in Steps 1-3, starting at row 22."}]
[null,null,2,"Many cells have additional instructions and tips displayed when the cell is selected."]
[null,null,3,"Review calculated proposed and baseline wattage and LPD's in the proposed and baseline lighting power columns. Proposed LPD's (w/o occupancy sensor credit) that exceed the baseline are shown in red for informational purposes."]
[null,null,4,"Review space type summary on LPD by Space Type tab generated based on inputs in the table below."]
[null,null,"PRODUCTIVITY TIPS:"]
[null,null,1,"CTRL+SHIFT+P adds a space/row immediately below the currently selected row, without disturbing any spreadsheet equations.   "]
[null,null,2,"CTRL+SHIFT+L marks the row as complete and highlights it in a different color, making it easier to input data quickly and accurately."]
[null,null,3,"Pressing CTRL+SHIFT+M enters data input mode by freezing panes. To exit data input mode, simply Unfreeze Panes through Excel's View menus."]
[null,null,"SPECIAL CASES"]
[null,null,1,"Dwelling Units\nIf you are not claiming performance credit for dwelling unit lighting: do not enter fixture counts in the table below; enter total thermal block area into the \"Area where prop. lighting is not specified\" column.\nIf you are claiming performance credit for dwelling unit lighting:\n  a) Enter fixture quantities into the table below\n  b) Complete the  \"Area where prop. lighting not specified\" column using the total area for spaces with no hard-wired fixtures and a proportional fraction of the area of spaces where specified fixtures are intended to be supplemented by plug-in lighting."]
[null,null,2,"Lighting exempt from 90.1 (Section 9.1.1, 9.2.2.3, or 9.4.2) must be modeled identically in the baseline and proposed models. This allowance can only be claimed if exempt lighting is specified in addition to the general lighting, and is separately controlled. Exempt lighting must be treated as unregulated load in PCIt calculations. Select \"Yes\" in Step 3 to indicate that the entered wattage is exempt. If the same type of fixtures provide are used for general and exempt lighting, enter the fixture in two columns in the table below. \n"]
[null,null,3,"Spaces with no permanent lighting specified (core & shell) must be modeled in the proposed design as meeting the minimum requirements established in Section 9 of ASHRAE Standard 90.1–2016 following the building area method. Area of these spaces must be entered into \"Area where propo. lighting not specified\" column."]
[]
[]
[]
[]
[]
[null,null,null,"Step 1: Enter Fixture Label (from lighting schedules and plans)"]
[null,null,null,"Step 2: Enter Rated Input Wattage or W/LnFt (for track lighting)"]
[null,null,null,null,null,null,null,null,{"$f":"IF(I25=\"Yes\",I23,0)","v":0},{"$f":"IF(J25=\"Yes\",J23,0)","v":0},0,0,0,{"$f":"IF(N25=\"Yes\",N23,0)","v":0},{"$f":"IF(O25=\"Yes\",O23,0)","v":0},{"$f":"IF(P25=\"Yes\",P23,0)","v":0},0,{"$f":"IF(R25=\"Yes\",R23,0)","v":0},{"$f":"IF(S25=\"Yes\",S23,0)","v":0},{"$f":"IF(T25=\"Yes\",T23,0)","v":0},0,{"$f":"IF(V25=\"Yes\",V23,0)","v":0},{"$f":"IF(W25=\"Yes\",W23,0)","v":0},{"$f":"IF(X25=\"Yes\",X23,0)","v":0},0,{"$f":"IF(Z25=\"Yes\",Z23,0)","v":0},{"$f":"IF(AA25=\"Yes\",AA23,0)","v":0},{"$f":"IF(AB25=\"Yes\",AB23,0)","v":0},0,{"$f":"IF(AD25=\"Yes\",AD23,0)","v":0},{"$f":"IF(AE25=\"Yes\",AE23,0)","v":0},{"$f":"IF(AF25=\"Yes\",AF23,0)","v":0},0,{"$f":"IF(AH25=\"Yes\",AH23,0)","v":0},{"$f":"IF(AI25=\"Yes\",AI23,0)","v":0},{"$f":"IF(AJ25=\"Yes\",AJ23,0)","v":0}]
[null,null,null,"Step 3: Does the fixture apply only toward exempt lighting (Section 9.1.1, 9.2.2.3, or 9.4.2)? ",null,null,null,null,"No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No","No",null,null,null,null,null,null,null,null,null,"Model Inputs",null,null,"Reference Values",null,null,null,null,null,null,null,"Hide","Hide","Hide","Hide","Hide"]
[null,null,null,"Calculated based on columns below, accounting for Multiplier. Totals for Area SF, Fixture Counts, and Watts; area-weighted average LPD.",null,null,null,{"$f":"SUMPRODUCT(H29:H551,F29:F551)","v":0},{"$f":"SUMPRODUCT(I29:I551,$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(J29:J551,$F$29:$F$551)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"SUMPRODUCT(AK29:AK551,F29:F551)","v":0},null,null,null,{"$f":"SUMPRODUCT(AO29:AO551,F29:F551)","v":0},null,{"$f":"SUMPRODUCT(AQ29:AQ551,F29:F551)","v":0},{"$f":"SUMPRODUCT(AR29:AR551,F29:F551)","v":0},{"$f":"SUMPRODUCT(AS29:AS551,F29:F551)","v":0},{"$f":"IFERROR(AQ26/H26,0)","v":0},{"$f":"IFERROR(AR26/H26,0)","v":0},{"$f":"IFERROR(AS26/H26,0)","v":0},{"$f":"IFERROR(AX26/H26,0)","v":0},{"$f":"SUMPRODUCT(AX29:AX551,F29:F551)","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"MOD(COLUMN(I27),2)","v":1},{"$f":"MOD(COLUMN(J27),2)","v":0},1,0,1,0,1,0,1,0,1,0,1,0,1,0,1,0,1,0,1,0,1,0,1,0,1,0]
[null,null,null,"Thermal Block Description (e.g. space name(s) from drawings, thermal block name from model, etc.)","Lighting Plans Dwg#","Multiplier","Space Type (90.1-2016 Table G3.7)\nSelect “Multiple” if there are several space types within a thermal block, and enter weighted average baseline LPD.","Area (SF)","FIXTURE COUNTS\nEnter fixture counts for each thermal block. If Rated Input Wattage in Step 4 is entered as W/LnFt, enter fixture length in linear feet (LnFt). \nDo not count fixtures meeting exceptions to 90.1-2016 Section 9.2.2.3.\n",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Connected Lighting Power Controlled by OS (W)","Occupancy Sensor Type","OS Credit (90.1 Table G3.7 note c)","OS Credit (90.1 Table G3.7)","Lighting Controlled by Daylighting (W)","Area where prop. lighting is not specified (SF)","Prop. Lighting Power (W)","Baseline Lighting Power (W)","Unregulated Lighting Power (Baseline and Proposed)\n(W)","Prop. LPD (W/SF)","Baseline LPD (W/SF)","Unregulated Lighting LPD (Baseline and Proposed)\n(W/SF)","Prop. LPD x OS Credit (W/SF)","Prop. Lighting Power x OS Credit (W)","Addtl. Lighting Allowance (decorative and/or retail; \"use it or lose it\" allowance)","Notes (Explain if: occupancy sensor performance credit is different than default; baseline LPD is custom/exempt or multiple; an additional lighting allowance is counted)","Done (Optional for productivity, select \"x\" to mark as complete)",null,null,null,"Default not Altered?","OS Credit Multiplier","OS Credit Adjusted","Was Proposed LPD Overwritten?","Was Baseline LPD Overwritten?","Baseline Lighting Power 2013 (W)","Baseline LPD 2013 (W/SF)"]
[null,null,null,null,null,{"$f":"IF(ISBLANK(D29)=FALSE,1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AL29=\"Manual-On Individual Workstation\",AL29=\"Partial-Auto-On Individual Workstation\",AL29=\"Other Individual Workstation\"),1.3,1)","v":1},{"$f":"IF(AL29=\"\",\"-\",BF29*AM29*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G29,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,{"$f":"SUMPRODUCT(I29:AJ29,$I$23:$AJ$23)+IF(H29>0,MIN(IF(ISBLANK(AP29)=TRUE,0,AP29),H29)*BJ29/H29,0)","v":0},{"$f":"IF(AU29=\"\",\"-\",IF(H29=\"\",0,AU29*H29))","v":"-"},{"$f":"SUMPRODUCT(I29:AJ29,$I$24:$AJ$24)","v":0},{"$f":"IF(ISBLANK(H29)=FALSE,AQ29/H29,\"-\")","v":"-"},{"$f":"IF(G29=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G29,'Lighting Assumptions'!$H$3:$H$112))","v":""},{"$f":"IF(ISBLANK(H29)=FALSE,AS29/H29,\"-\")","v":"-"},{"$f":"IF(ISBLANK(H29)=FALSE,(AQ29-IF(ISNUMBER(AN29)=TRUE,AN29,0)*AK29)/H29,\"-\")","v":"-"},{"$f":"IFERROR(AQ29-AK29*IF(ISNUMBER(AN29)=TRUE,AN29,0),\"\")","v":0},{"$f":"MIN(SUMPRODUCT(I29:AJ29,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H29)","v":0},null,null,null,null,null,{"$f":"IF(AK29=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G29,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},{"$f":"IF(AL29=\"\",\"-\",IF(AL29=\"Other\",1,1.25))","v":"-"},{"$f":"IF(BF29=\"-\",\"-\",BF29*AN29)","v":"-"},{"$f":"IF(LEFT(CELLformula(AW29),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU29),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(BK29=\"\",\"-\",IF(H29=\"\",0,BK29*H29))","v":"-"},{"$f":"IF(G29=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G29,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AL30=\"Manual-On Individual Workstation\",AL30=\"Partial-Auto-On Individual Workstation\",AL30=\"Other Individual Workstation\"),1.3,1)","v":1},{"$f":"IF(AL30=\"\",\"-\",BF30*AM30*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G30,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,{"$f":"SUMPRODUCT(I30:AJ30,$I$23:$AJ$23)+IF(H30>0,MIN(IF(ISBLANK(AP30)=TRUE,0,AP30),H30)*BJ30/H30,0)","v":0},"-",{"$f":"SUMPRODUCT(I30:AJ30,$I$24:$AJ$24)","v":0},"-",{"$f":"IF(G30=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G30,'Lighting Assumptions'!$H$3:$H$112))","v":""},{"$f":"IF(ISBLANK(H30)=FALSE,AS30/H30,\"-\")","v":"-"},"-",0,{"$f":"MIN(SUMPRODUCT(I30:AJ30,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H30)","v":0},null,null,null,null,null,{"$f":"IF(AK30=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G30,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW30),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU30),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(BK30=\"\",\"-\",IF(H30=\"\",0,BK30*H30))","v":"-"},{"$f":"IF(G30=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G30,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL31=\"\",\"-\",BF31*AM31*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G31,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,{"$f":"SUMPRODUCT(I31:AJ31,$I$23:$AJ$23)+IF(H31>0,MIN(IF(ISBLANK(AP31)=TRUE,0,AP31),H31)*BJ31/H31,0)","v":0},"-",0,"-",{"$f":"IF(G31=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G31,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I31:AJ31,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H31)","v":0},null,null,null,null,null,{"$f":"IF(AK31=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G31,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW31),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU31),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G31=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G31,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL32=\"\",\"-\",BF32*AM32*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G32,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G32=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G32,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I32:AJ32,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H32)","v":0},null,null,null,null,null,{"$f":"IF(AK32=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G32,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW32),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU32),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G32=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G32,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL33=\"\",\"-\",BF33*AM33*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G33,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G33=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G33,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I33:AJ33,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H33)","v":0},null,null,null,null,null,{"$f":"IF(AK33=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G33,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW33),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU33),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G33=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G33,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,{"$f":"IF(ISBLANK(D34)=FALSE,1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL34=\"\",\"-\",BF34*AM34*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G34,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G34=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G34,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I34:AJ34,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H34)","v":0},null,null,null,null,null,{"$f":"IF(AK34=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G34,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW34),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU34),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G34=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G34,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL35=\"\",\"-\",BF35*AM35*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G35,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G35=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G35,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I35:AJ35,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H35)","v":0},null,null,null,null,null,{"$f":"IF(AK35=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G35,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW35),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU35),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G35=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G35,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL36=\"\",\"-\",BF36*AM36*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G36,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G36=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G36,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I36:AJ36,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H36)","v":0},null,null,null,null,null,{"$f":"IF(AK36=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G36,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW36),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU36),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G36=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G36,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL37=\"\",\"-\",BF37*AM37*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G37,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G37=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G37,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I37:AJ37,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H37)","v":0},null,null,null,null,null,{"$f":"IF(AK37=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G37,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW37),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU37),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G37=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G37,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL38=\"\",\"-\",BF38*AM38*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G38,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G38=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G38,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I38:AJ38,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H38)","v":0},null,null,null,null,null,{"$f":"IF(AK38=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G38,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW38),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU38),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G38=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G38,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL39=\"\",\"-\",BF39*AM39*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G39,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G39=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G39,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I39:AJ39,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H39)","v":0},null,null,null,null,null,{"$f":"IF(AK39=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G39,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW39),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU39),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G39=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G39,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL40=\"\",\"-\",BF40*AM40*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G40,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G40=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G40,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I40:AJ40,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H40)","v":0},null,null,null,null,null,{"$f":"IF(AK40=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G40,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW40),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU40),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G40=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G40,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL41=\"\",\"-\",BF41*AM41*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G41,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G41=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G41,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I41:AJ41,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H41)","v":0},null,null,null,null,null,{"$f":"IF(AK41=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G41,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW41),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU41),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G41=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G41,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL42=\"\",\"-\",BF42*AM42*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G42,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G42=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G42,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I42:AJ42,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H42)","v":0},null,null,null,null,null,{"$f":"IF(AK42=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G42,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW42),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU42),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G42=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G42,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL43=\"\",\"-\",BF43*AM43*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G43,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G43=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G43,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I43:AJ43,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H43)","v":0},null,null,null,null,null,{"$f":"IF(AK43=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G43,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW43),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU43),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G43=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G43,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL44=\"\",\"-\",BF44*AM44*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G44,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G44=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G44,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I44:AJ44,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H44)","v":0},null,null,null,null,null,{"$f":"IF(AK44=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G44,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW44),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU44),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G44=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G44,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL45=\"\",\"-\",BF45*AM45*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G45,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G45=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G45,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I45:AJ45,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H45)","v":0},null,null,null,null,null,{"$f":"IF(AK45=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G45,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW45),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU45),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G45=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G45,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL46=\"\",\"-\",BF46*AM46*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G46,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G46=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G46,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I46:AJ46,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H46)","v":0},null,null,null,null,null,{"$f":"IF(AK46=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G46,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW46),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU46),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G46=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G46,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL47=\"\",\"-\",BF47*AM47*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G47,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G47=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G47,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I47:AJ47,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H47)","v":0},null,null,null,null,null,{"$f":"IF(AK47=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G47,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW47),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU47),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G47=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G47,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL48=\"\",\"-\",BF48*AM48*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G48,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G48=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G48,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I48:AJ48,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H48)","v":0},null,null,null,null,null,{"$f":"IF(AK48=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G48,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW48),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU48),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G48=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G48,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL49=\"\",\"-\",BF49*AM49*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G49,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G49=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G49,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I49:AJ49,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H49)","v":0},null,null,null,null,null,{"$f":"IF(AK49=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G49,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW49),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU49),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G49=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G49,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL50=\"\",\"-\",BF50*AM50*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G50,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G50=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G50,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I50:AJ50,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H50)","v":0},null,null,null,null,null,{"$f":"IF(AK50=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G50,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW50),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU50),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G50=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G50,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL51=\"\",\"-\",BF51*AM51*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G51,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G51=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G51,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I51:AJ51,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H51)","v":0},null,null,null,null,null,{"$f":"IF(AK51=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G51,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW51),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU51),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G51=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G51,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL52=\"\",\"-\",BF52*AM52*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G52,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G52=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G52,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I52:AJ52,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H52)","v":0},null,null,null,null,null,{"$f":"IF(AK52=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G52,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW52),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU52),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G52=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G52,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL53=\"\",\"-\",BF53*AM53*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G53,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G53=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G53,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I53:AJ53,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H53)","v":0},null,null,null,null,null,{"$f":"IF(AK53=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G53,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW53),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU53),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G53=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G53,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL54=\"\",\"-\",BF54*AM54*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G54,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G54=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G54,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I54:AJ54,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H54)","v":0},null,null,null,null,null,{"$f":"IF(AK54=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G54,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW54),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU54),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G54=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G54,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL55=\"\",\"-\",BF55*AM55*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G55,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G55=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G55,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I55:AJ55,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H55)","v":0},null,null,null,null,null,{"$f":"IF(AK55=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G55,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW55),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU55),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G55=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G55,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL56=\"\",\"-\",BF56*AM56*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G56,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G56=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G56,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I56:AJ56,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H56)","v":0},null,null,null,null,null,{"$f":"IF(AK56=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G56,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW56),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU56),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G56=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G56,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL57=\"\",\"-\",BF57*AM57*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G57,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G57=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G57,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I57:AJ57,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H57)","v":0},null,null,null,null,null,{"$f":"IF(AK57=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G57,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW57),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU57),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G57=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G57,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL58=\"\",\"-\",BF58*AM58*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G58,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G58=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G58,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I58:AJ58,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H58)","v":0},null,null,null,null,null,{"$f":"IF(AK58=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G58,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW58),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU58),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G58=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G58,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL59=\"\",\"-\",BF59*AM59*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G59,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G59=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G59,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I59:AJ59,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H59)","v":0},null,null,null,null,null,{"$f":"IF(AK59=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G59,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW59),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU59),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G59=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G59,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL60=\"\",\"-\",BF60*AM60*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G60,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G60=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G60,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I60:AJ60,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H60)","v":0},null,null,null,null,null,{"$f":"IF(AK60=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G60,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW60),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU60),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G60=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G60,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL61=\"\",\"-\",BF61*AM61*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G61,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G61=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G61,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I61:AJ61,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H61)","v":0},null,null,null,null,null,{"$f":"IF(AK61=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G61,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW61),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU61),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G61=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G61,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL62=\"\",\"-\",BF62*AM62*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G62,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G62=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G62,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I62:AJ62,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H62)","v":0},null,null,null,null,null,{"$f":"IF(AK62=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G62,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW62),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU62),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G62=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G62,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL63=\"\",\"-\",BF63*AM63*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G63,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G63=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G63,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I63:AJ63,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H63)","v":0},null,null,null,null,null,{"$f":"IF(AK63=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G63,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW63),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU63),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G63=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G63,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL64=\"\",\"-\",BF64*AM64*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G64,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G64=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G64,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I64:AJ64,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H64)","v":0},null,null,null,null,null,{"$f":"IF(AK64=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G64,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW64),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU64),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G64=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G64,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL65=\"\",\"-\",BF65*AM65*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G65,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G65=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G65,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I65:AJ65,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H65)","v":0},null,null,null,null,null,{"$f":"IF(AK65=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G65,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW65),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU65),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G65=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G65,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL66=\"\",\"-\",BF66*AM66*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G66,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G66=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G66,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I66:AJ66,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H66)","v":0},null,null,null,null,null,{"$f":"IF(AK66=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G66,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW66),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU66),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G66=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G66,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL67=\"\",\"-\",BF67*AM67*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G67,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G67=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G67,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I67:AJ67,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H67)","v":0},null,null,null,null,null,{"$f":"IF(AK67=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G67,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW67),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU67),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G67=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G67,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL68=\"\",\"-\",BF68*AM68*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G68,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G68=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G68,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I68:AJ68,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H68)","v":0},null,null,null,null,null,{"$f":"IF(AK68=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G68,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW68),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU68),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G68=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G68,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL69=\"\",\"-\",BF69*AM69*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G69,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G69=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G69,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I69:AJ69,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H69)","v":0},null,null,null,null,null,{"$f":"IF(AK69=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G69,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW69),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU69),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G69=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G69,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL70=\"\",\"-\",BF70*AM70*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G70,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G70=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G70,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I70:AJ70,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H70)","v":0},null,null,null,null,null,{"$f":"IF(AK70=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G70,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW70),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU70),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G70=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G70,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL71=\"\",\"-\",BF71*AM71*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G71,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G71=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G71,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I71:AJ71,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H71)","v":0},null,null,null,null,null,{"$f":"IF(AK71=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G71,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW71),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU71),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G71=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G71,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL72=\"\",\"-\",BF72*AM72*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G72,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G72=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G72,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I72:AJ72,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H72)","v":0},null,null,null,null,null,{"$f":"IF(AK72=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G72,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW72),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU72),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G72=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G72,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL73=\"\",\"-\",BF73*AM73*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G73,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G73=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G73,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I73:AJ73,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H73)","v":0},null,null,null,null,null,{"$f":"IF(AK73=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G73,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW73),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU73),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G73=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G73,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL74=\"\",\"-\",BF74*AM74*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G74,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G74=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G74,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I74:AJ74,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H74)","v":0},null,null,null,null,null,{"$f":"IF(AK74=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G74,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW74),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU74),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G74=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G74,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL75=\"\",\"-\",BF75*AM75*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G75,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G75=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G75,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I75:AJ75,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H75)","v":0},null,null,null,null,null,{"$f":"IF(AK75=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G75,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW75),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU75),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G75=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G75,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL76=\"\",\"-\",BF76*AM76*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G76,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G76=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G76,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I76:AJ76,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H76)","v":0},null,null,null,null,null,{"$f":"IF(AK76=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G76,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW76),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU76),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G76=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G76,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL77=\"\",\"-\",BF77*AM77*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G77,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G77=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G77,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I77:AJ77,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H77)","v":0},null,null,null,null,null,{"$f":"IF(AK77=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G77,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW77),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU77),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G77=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G77,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL78=\"\",\"-\",BF78*AM78*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G78,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G78=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G78,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I78:AJ78,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H78)","v":0},null,null,null,null,null,{"$f":"IF(AK78=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G78,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW78),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU78),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G78=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G78,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL79=\"\",\"-\",BF79*AM79*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G79,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G79=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G79,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I79:AJ79,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H79)","v":0},null,null,null,null,null,{"$f":"IF(AK79=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G79,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW79),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU79),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G79=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G79,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL80=\"\",\"-\",BF80*AM80*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G80,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G80=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G80,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I80:AJ80,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H80)","v":0},null,null,null,null,null,{"$f":"IF(AK80=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G80,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW80),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU80),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G80=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G80,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL81=\"\",\"-\",BF81*AM81*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G81,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G81=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G81,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I81:AJ81,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H81)","v":0},null,null,null,null,null,{"$f":"IF(AK81=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G81,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW81),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU81),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G81=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G81,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL82=\"\",\"-\",BF82*AM82*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G82,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G82=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G82,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I82:AJ82,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H82)","v":0},null,null,null,null,null,{"$f":"IF(AK82=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G82,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW82),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU82),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G82=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G82,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL83=\"\",\"-\",BF83*AM83*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G83,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G83=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G83,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I83:AJ83,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H83)","v":0},null,null,null,null,null,{"$f":"IF(AK83=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G83,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW83),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU83),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G83=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G83,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL84=\"\",\"-\",BF84*AM84*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G84,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G84=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G84,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I84:AJ84,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H84)","v":0},null,null,null,null,null,{"$f":"IF(AK84=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G84,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW84),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU84),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G84=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G84,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL85=\"\",\"-\",BF85*AM85*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G85,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G85=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G85,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I85:AJ85,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H85)","v":0},null,null,null,null,null,{"$f":"IF(AK85=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G85,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW85),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU85),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G85=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G85,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL86=\"\",\"-\",BF86*AM86*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G86,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G86=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G86,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I86:AJ86,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H86)","v":0},null,null,null,null,null,{"$f":"IF(AK86=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G86,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW86),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU86),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G86=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G86,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL87=\"\",\"-\",BF87*AM87*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G87,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G87=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G87,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I87:AJ87,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H87)","v":0},null,null,null,null,null,{"$f":"IF(AK87=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G87,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW87),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU87),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G87=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G87,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL88=\"\",\"-\",BF88*AM88*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G88,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G88=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G88,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I88:AJ88,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H88)","v":0},null,null,null,null,null,{"$f":"IF(AK88=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G88,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW88),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU88),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G88=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G88,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL89=\"\",\"-\",BF89*AM89*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G89,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G89=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G89,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I89:AJ89,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H89)","v":0},null,null,null,null,null,{"$f":"IF(AK89=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G89,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW89),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU89),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G89=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G89,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL90=\"\",\"-\",BF90*AM90*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G90,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G90=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G90,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I90:AJ90,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H90)","v":0},null,null,null,null,null,{"$f":"IF(AK90=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G90,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW90),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU90),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G90=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G90,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL91=\"\",\"-\",BF91*AM91*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G91,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G91=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G91,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I91:AJ91,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H91)","v":0},null,null,null,null,null,{"$f":"IF(AK91=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G91,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW91),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU91),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G91=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G91,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL92=\"\",\"-\",BF92*AM92*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G92,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G92=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G92,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I92:AJ92,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H92)","v":0},null,null,null,null,null,{"$f":"IF(AK92=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G92,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW92),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU92),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G92=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G92,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,{"$f":"IF(ISBLANK(D93)=FALSE,1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL93=\"\",\"-\",BF93*AM93*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G93,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,{"$f":"IF(AU93=\"\",\"-\",IF(H93=\"\",0,AU93*H93))","v":"-"},0,{"$f":"IF(ISBLANK(H93)=FALSE,AQ93/H93,\"-\")","v":"-"},{"$f":"IF(G93=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G93,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-",{"$f":"IF(ISBLANK(H93)=FALSE,(AQ93-IF(ISNUMBER(AN93)=TRUE,AN93,0)*AK93)/H93,\"-\")","v":"-"},{"$f":"IFERROR(AQ93-AK93*IF(ISNUMBER(AN93)=TRUE,AN93,0),\"\")","v":0},{"$f":"MIN(SUMPRODUCT(I93:AJ93,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H93)","v":0},null,null,null,null,null,{"$f":"IF(AK93=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G93,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},{"$f":"IF(AL93=\"\",\"-\",IF(AL93=\"Other\",1,1.25))","v":"-"},{"$f":"IF(BF93=\"-\",\"-\",BF93*AN93)","v":"-"},{"$f":"IF(LEFT(CELLformula(AW93),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU93),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G93=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G93,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AL94=\"Manual-On Individual Workstation\",AL94=\"Partial-Auto-On Individual Workstation\",AL94=\"Other Individual Workstation\"),1.3,1)","v":1},{"$f":"IF(AL94=\"\",\"-\",BF94*AM94*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G94,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,{"$f":"SUMPRODUCT(I94:AJ94,$I$23:$AJ$23)+IF(H94>0,MIN(IF(ISBLANK(AP94)=TRUE,0,AP94),H94)*BJ94/H94,0)","v":0},"-",{"$f":"SUMPRODUCT(I94:AJ94,$I$24:$AJ$24)","v":0},"-",{"$f":"IF(G94=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G94,'Lighting Assumptions'!$H$3:$H$112))","v":""},{"$f":"IF(ISBLANK(H94)=FALSE,AS94/H94,\"-\")","v":"-"},"-",0,{"$f":"MIN(SUMPRODUCT(I94:AJ94,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H94)","v":0},null,null,null,null,null,{"$f":"IF(AK94=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G94,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW94),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU94),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(BK94=\"\",\"-\",IF(H94=\"\",0,BK94*H94))","v":"-"},{"$f":"IF(G94=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G94,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL95=\"\",\"-\",BF95*AM95*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G95,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G95=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G95,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I95:AJ95,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H95)","v":0},null,null,null,null,null,{"$f":"IF(AK95=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G95,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW95),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU95),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G95=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G95,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL96=\"\",\"-\",BF96*AM96*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G96,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G96=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G96,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I96:AJ96,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H96)","v":0},null,null,null,null,null,{"$f":"IF(AK96=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G96,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW96),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU96),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G96=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G96,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL97=\"\",\"-\",BF97*AM97*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G97,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G97=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G97,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I97:AJ97,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H97)","v":0},null,null,null,null,null,{"$f":"IF(AK97=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G97,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW97),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU97),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G97=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G97,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL98=\"\",\"-\",BF98*AM98*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G98,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G98=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G98,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I98:AJ98,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H98)","v":0},null,null,null,null,null,{"$f":"IF(AK98=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G98,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW98),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU98),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G98=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G98,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL99=\"\",\"-\",BF99*AM99*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G99,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G99=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G99,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I99:AJ99,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H99)","v":0},null,null,null,null,null,{"$f":"IF(AK99=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G99,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW99),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU99),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G99=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G99,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL100=\"\",\"-\",BF100*AM100*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G100,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G100=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G100,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I100:AJ100,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H100)","v":0},null,null,null,null,null,{"$f":"IF(AK100=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G100,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW100),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU100),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G100=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G100,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL101=\"\",\"-\",BF101*AM101*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G101,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G101=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G101,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I101:AJ101,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H101)","v":0},null,null,null,null,null,{"$f":"IF(AK101=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G101,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW101),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU101),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G101=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G101,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL102=\"\",\"-\",BF102*AM102*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G102,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G102=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G102,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I102:AJ102,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H102)","v":0},null,null,null,null,null,{"$f":"IF(AK102=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G102,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW102),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU102),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G102=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G102,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL103=\"\",\"-\",BF103*AM103*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G103,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G103=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G103,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I103:AJ103,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H103)","v":0},null,null,null,null,null,{"$f":"IF(AK103=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G103,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW103),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU103),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G103=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G103,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL104=\"\",\"-\",BF104*AM104*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G104,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G104=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G104,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I104:AJ104,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H104)","v":0},null,null,null,null,null,{"$f":"IF(AK104=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G104,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW104),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU104),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G104=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G104,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL105=\"\",\"-\",BF105*AM105*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G105,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G105=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G105,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I105:AJ105,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H105)","v":0},null,null,null,null,null,{"$f":"IF(AK105=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G105,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW105),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU105),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G105=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G105,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL106=\"\",\"-\",BF106*AM106*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G106,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G106=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G106,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I106:AJ106,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H106)","v":0},null,null,null,null,null,{"$f":"IF(AK106=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G106,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW106),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU106),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G106=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G106,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL107=\"\",\"-\",BF107*AM107*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G107,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G107=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G107,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I107:AJ107,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H107)","v":0},null,null,null,null,null,{"$f":"IF(AK107=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G107,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW107),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU107),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G107=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G107,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL108=\"\",\"-\",BF108*AM108*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G108,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G108=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G108,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I108:AJ108,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H108)","v":0},null,null,null,null,null,{"$f":"IF(AK108=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G108,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW108),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU108),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G108=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G108,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL109=\"\",\"-\",BF109*AM109*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G109,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G109=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G109,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I109:AJ109,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H109)","v":0},null,null,null,null,null,{"$f":"IF(AK109=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G109,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW109),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU109),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G109=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G109,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL110=\"\",\"-\",BF110*AM110*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G110,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G110=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G110,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I110:AJ110,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H110)","v":0},null,null,null,null,null,{"$f":"IF(AK110=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G110,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW110),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU110),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G110=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G110,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL111=\"\",\"-\",BF111*AM111*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G111,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G111=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G111,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I111:AJ111,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H111)","v":0},null,null,null,null,null,{"$f":"IF(AK111=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G111,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW111),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU111),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G111=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G111,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL112=\"\",\"-\",BF112*AM112*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G112,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G112=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G112,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I112:AJ112,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H112)","v":0},null,null,null,null,null,{"$f":"IF(AK112=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G112,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW112),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU112),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G112=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G112,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL113=\"\",\"-\",BF113*AM113*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G113,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G113=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G113,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I113:AJ113,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H113)","v":0},null,null,null,null,null,{"$f":"IF(AK113=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G113,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW113),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU113),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G113=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G113,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL114=\"\",\"-\",BF114*AM114*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G114,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G114=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G114,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I114:AJ114,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H114)","v":0},null,null,null,null,null,{"$f":"IF(AK114=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G114,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW114),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU114),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G114=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G114,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL115=\"\",\"-\",BF115*AM115*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G115,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G115=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G115,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I115:AJ115,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H115)","v":0},null,null,null,null,null,{"$f":"IF(AK115=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G115,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW115),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU115),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G115=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G115,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL116=\"\",\"-\",BF116*AM116*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G116,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G116=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G116,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I116:AJ116,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H116)","v":0},null,null,null,null,null,{"$f":"IF(AK116=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G116,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW116),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU116),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G116=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G116,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL117=\"\",\"-\",BF117*AM117*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G117,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G117=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G117,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I117:AJ117,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H117)","v":0},null,null,null,null,null,{"$f":"IF(AK117=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G117,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW117),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU117),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G117=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G117,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL118=\"\",\"-\",BF118*AM118*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G118,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G118=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G118,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I118:AJ118,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H118)","v":0},null,null,null,null,null,{"$f":"IF(AK118=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G118,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW118),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU118),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G118=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G118,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL119=\"\",\"-\",BF119*AM119*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G119,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G119=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G119,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I119:AJ119,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H119)","v":0},null,null,null,null,null,{"$f":"IF(AK119=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G119,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW119),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU119),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G119=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G119,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL120=\"\",\"-\",BF120*AM120*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G120,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G120=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G120,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I120:AJ120,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H120)","v":0},null,null,null,null,null,{"$f":"IF(AK120=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G120,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW120),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU120),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G120=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G120,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL121=\"\",\"-\",BF121*AM121*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G121,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G121=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G121,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I121:AJ121,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H121)","v":0},null,null,null,null,null,{"$f":"IF(AK121=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G121,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW121),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU121),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G121=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G121,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL122=\"\",\"-\",BF122*AM122*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G122,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G122=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G122,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I122:AJ122,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H122)","v":0},null,null,null,null,null,{"$f":"IF(AK122=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G122,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW122),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU122),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G122=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G122,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL123=\"\",\"-\",BF123*AM123*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G123,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G123=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G123,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I123:AJ123,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H123)","v":0},null,null,null,null,null,{"$f":"IF(AK123=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G123,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW123),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU123),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G123=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G123,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL124=\"\",\"-\",BF124*AM124*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G124,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G124=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G124,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I124:AJ124,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H124)","v":0},null,null,null,null,null,{"$f":"IF(AK124=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G124,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW124),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU124),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G124=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G124,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL125=\"\",\"-\",BF125*AM125*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G125,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G125=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G125,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I125:AJ125,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H125)","v":0},null,null,null,null,null,{"$f":"IF(AK125=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G125,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW125),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU125),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G125=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G125,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL126=\"\",\"-\",BF126*AM126*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G126,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G126=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G126,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I126:AJ126,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H126)","v":0},null,null,null,null,null,{"$f":"IF(AK126=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G126,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW126),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU126),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G126=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G126,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL127=\"\",\"-\",BF127*AM127*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G127,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G127=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G127,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I127:AJ127,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H127)","v":0},null,null,null,null,null,{"$f":"IF(AK127=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G127,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW127),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU127),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G127=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G127,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL128=\"\",\"-\",BF128*AM128*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G128,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G128=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G128,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I128:AJ128,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H128)","v":0},null,null,null,null,null,{"$f":"IF(AK128=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G128,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW128),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU128),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G128=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G128,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL129=\"\",\"-\",BF129*AM129*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G129,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G129=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G129,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I129:AJ129,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H129)","v":0},null,null,null,null,null,{"$f":"IF(AK129=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G129,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW129),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU129),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G129=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G129,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL130=\"\",\"-\",BF130*AM130*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G130,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G130=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G130,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I130:AJ130,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H130)","v":0},null,null,null,null,null,{"$f":"IF(AK130=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G130,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW130),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU130),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G130=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G130,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL131=\"\",\"-\",BF131*AM131*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G131,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G131=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G131,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I131:AJ131,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H131)","v":0},null,null,null,null,null,{"$f":"IF(AK131=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G131,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW131),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU131),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G131=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G131,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL132=\"\",\"-\",BF132*AM132*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G132,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G132=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G132,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I132:AJ132,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H132)","v":0},null,null,null,null,null,{"$f":"IF(AK132=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G132,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW132),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU132),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G132=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G132,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL133=\"\",\"-\",BF133*AM133*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G133,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G133=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G133,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I133:AJ133,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H133)","v":0},null,null,null,null,null,{"$f":"IF(AK133=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G133,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW133),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU133),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G133=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G133,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL134=\"\",\"-\",BF134*AM134*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G134,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G134=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G134,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I134:AJ134,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H134)","v":0},null,null,null,null,null,{"$f":"IF(AK134=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G134,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW134),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU134),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G134=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G134,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL135=\"\",\"-\",BF135*AM135*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G135,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G135=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G135,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I135:AJ135,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H135)","v":0},null,null,null,null,null,{"$f":"IF(AK135=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G135,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW135),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU135),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G135=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G135,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL136=\"\",\"-\",BF136*AM136*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G136,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G136=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G136,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I136:AJ136,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H136)","v":0},null,null,null,null,null,{"$f":"IF(AK136=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G136,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW136),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU136),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G136=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G136,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL137=\"\",\"-\",BF137*AM137*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G137,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G137=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G137,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I137:AJ137,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H137)","v":0},null,null,null,null,null,{"$f":"IF(AK137=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G137,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW137),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU137),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G137=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G137,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL138=\"\",\"-\",BF138*AM138*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G138,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G138=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G138,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I138:AJ138,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H138)","v":0},null,null,null,null,null,{"$f":"IF(AK138=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G138,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW138),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU138),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G138=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G138,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL139=\"\",\"-\",BF139*AM139*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G139,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G139=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G139,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I139:AJ139,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H139)","v":0},null,null,null,null,null,{"$f":"IF(AK139=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G139,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW139),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU139),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G139=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G139,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL140=\"\",\"-\",BF140*AM140*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G140,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G140=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G140,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I140:AJ140,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H140)","v":0},null,null,null,null,null,{"$f":"IF(AK140=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G140,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW140),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU140),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G140=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G140,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL141=\"\",\"-\",BF141*AM141*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G141,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G141=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G141,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I141:AJ141,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H141)","v":0},null,null,null,null,null,{"$f":"IF(AK141=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G141,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW141),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU141),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G141=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G141,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL142=\"\",\"-\",BF142*AM142*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G142,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G142=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G142,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I142:AJ142,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H142)","v":0},null,null,null,null,null,{"$f":"IF(AK142=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G142,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW142),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU142),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G142=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G142,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL143=\"\",\"-\",BF143*AM143*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G143,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G143=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G143,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I143:AJ143,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H143)","v":0},null,null,null,null,null,{"$f":"IF(AK143=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G143,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW143),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU143),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G143=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G143,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL144=\"\",\"-\",BF144*AM144*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G144,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G144=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G144,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I144:AJ144,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H144)","v":0},null,null,null,null,null,{"$f":"IF(AK144=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G144,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW144),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU144),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G144=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G144,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL145=\"\",\"-\",BF145*AM145*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G145,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G145=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G145,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I145:AJ145,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H145)","v":0},null,null,null,null,null,{"$f":"IF(AK145=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G145,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW145),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU145),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G145=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G145,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL146=\"\",\"-\",BF146*AM146*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G146,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G146=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G146,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I146:AJ146,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H146)","v":0},null,null,null,null,null,{"$f":"IF(AK146=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G146,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW146),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU146),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G146=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G146,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL147=\"\",\"-\",BF147*AM147*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G147,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G147=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G147,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I147:AJ147,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H147)","v":0},null,null,null,null,null,{"$f":"IF(AK147=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G147,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW147),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU147),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G147=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G147,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL148=\"\",\"-\",BF148*AM148*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G148,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G148=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G148,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I148:AJ148,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H148)","v":0},null,null,null,null,null,{"$f":"IF(AK148=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G148,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW148),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU148),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G148=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G148,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL149=\"\",\"-\",BF149*AM149*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G149,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G149=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G149,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I149:AJ149,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H149)","v":0},null,null,null,null,null,{"$f":"IF(AK149=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G149,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW149),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU149),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G149=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G149,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL150=\"\",\"-\",BF150*AM150*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G150,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G150=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G150,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I150:AJ150,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H150)","v":0},null,null,null,null,null,{"$f":"IF(AK150=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G150,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW150),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU150),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G150=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G150,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL151=\"\",\"-\",BF151*AM151*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G151,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G151=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G151,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I151:AJ151,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H151)","v":0},null,null,null,null,null,{"$f":"IF(AK151=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G151,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW151),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU151),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G151=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G151,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL152=\"\",\"-\",BF152*AM152*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G152,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G152=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G152,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I152:AJ152,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H152)","v":0},null,null,null,null,null,{"$f":"IF(AK152=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G152,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW152),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU152),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G152=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G152,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL153=\"\",\"-\",BF153*AM153*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G153,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G153=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G153,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I153:AJ153,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H153)","v":0},null,null,null,null,null,{"$f":"IF(AK153=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G153,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW153),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU153),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G153=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G153,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL154=\"\",\"-\",BF154*AM154*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G154,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G154=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G154,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I154:AJ154,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H154)","v":0},null,null,null,null,null,{"$f":"IF(AK154=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G154,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW154),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU154),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G154=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G154,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL155=\"\",\"-\",BF155*AM155*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G155,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G155=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G155,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I155:AJ155,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H155)","v":0},null,null,null,null,null,{"$f":"IF(AK155=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G155,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW155),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU155),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G155=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G155,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL156=\"\",\"-\",BF156*AM156*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G156,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G156=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G156,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I156:AJ156,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H156)","v":0},null,null,null,null,null,{"$f":"IF(AK156=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G156,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW156),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU156),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G156=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G156,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,{"$f":"IF(ISBLANK(D157)=FALSE,1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL157=\"\",\"-\",BF157*AM157*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G157,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,{"$f":"IF(AU157=\"\",\"-\",IF(H157=\"\",0,AU157*H157))","v":"-"},0,{"$f":"IF(ISBLANK(H157)=FALSE,AQ157/H157,\"-\")","v":"-"},{"$f":"IF(G157=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G157,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-",{"$f":"IF(ISBLANK(H157)=FALSE,(AQ157-IF(ISNUMBER(AN157)=TRUE,AN157,0)*AK157)/H157,\"-\")","v":"-"},{"$f":"IFERROR(AQ157-AK157*IF(ISNUMBER(AN157)=TRUE,AN157,0),\"\")","v":0},{"$f":"MIN(SUMPRODUCT(I157:AJ157,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H157)","v":0},null,null,null,null,null,{"$f":"IF(AK157=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G157,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},{"$f":"IF(AL157=\"\",\"-\",IF(AL157=\"Other\",1,1.25))","v":"-"},{"$f":"IF(BF157=\"-\",\"-\",BF157*AN157)","v":"-"},{"$f":"IF(LEFT(CELLformula(AW157),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU157),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G157=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G157,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AL158=\"Manual-On Individual Workstation\",AL158=\"Partial-Auto-On Individual Workstation\",AL158=\"Other Individual Workstation\"),1.3,1)","v":1},{"$f":"IF(AL158=\"\",\"-\",BF158*AM158*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G158,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,{"$f":"SUMPRODUCT(I158:AJ158,$I$23:$AJ$23)+IF(H158>0,MIN(IF(ISBLANK(AP158)=TRUE,0,AP158),H158)*BJ158/H158,0)","v":0},"-",{"$f":"SUMPRODUCT(I158:AJ158,$I$24:$AJ$24)","v":0},"-",{"$f":"IF(G158=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G158,'Lighting Assumptions'!$H$3:$H$112))","v":""},{"$f":"IF(ISBLANK(H158)=FALSE,AS158/H158,\"-\")","v":"-"},"-",0,{"$f":"MIN(SUMPRODUCT(I158:AJ158,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H158)","v":0},null,null,null,null,null,{"$f":"IF(AK158=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G158,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW158),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU158),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(BK158=\"\",\"-\",IF(H158=\"\",0,BK158*H158))","v":"-"},{"$f":"IF(G158=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G158,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL159=\"\",\"-\",BF159*AM159*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G159,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G159=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G159,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I159:AJ159,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H159)","v":0},null,null,null,null,null,{"$f":"IF(AK159=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G159,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW159),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU159),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G159=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G159,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL160=\"\",\"-\",BF160*AM160*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G160,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G160=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G160,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I160:AJ160,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H160)","v":0},null,null,null,null,null,{"$f":"IF(AK160=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G160,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW160),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU160),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G160=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G160,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL161=\"\",\"-\",BF161*AM161*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G161,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G161=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G161,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I161:AJ161,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H161)","v":0},null,null,null,null,null,{"$f":"IF(AK161=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G161,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW161),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU161),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G161=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G161,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL162=\"\",\"-\",BF162*AM162*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G162,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G162=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G162,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I162:AJ162,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H162)","v":0},null,null,null,null,null,{"$f":"IF(AK162=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G162,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW162),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU162),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G162=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G162,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL163=\"\",\"-\",BF163*AM163*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G163,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G163=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G163,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I163:AJ163,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H163)","v":0},null,null,null,null,null,{"$f":"IF(AK163=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G163,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW163),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU163),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G163=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G163,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL164=\"\",\"-\",BF164*AM164*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G164,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G164=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G164,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I164:AJ164,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H164)","v":0},null,null,null,null,null,{"$f":"IF(AK164=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G164,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW164),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU164),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G164=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G164,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL165=\"\",\"-\",BF165*AM165*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G165,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G165=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G165,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I165:AJ165,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H165)","v":0},null,null,null,null,null,{"$f":"IF(AK165=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G165,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW165),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU165),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G165=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G165,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL166=\"\",\"-\",BF166*AM166*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G166,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G166=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G166,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I166:AJ166,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H166)","v":0},null,null,null,null,null,{"$f":"IF(AK166=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G166,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW166),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU166),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G166=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G166,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL167=\"\",\"-\",BF167*AM167*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G167,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G167=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G167,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I167:AJ167,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H167)","v":0},null,null,null,null,null,{"$f":"IF(AK167=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G167,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW167),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU167),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G167=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G167,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL168=\"\",\"-\",BF168*AM168*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G168,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G168=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G168,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I168:AJ168,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H168)","v":0},null,null,null,null,null,{"$f":"IF(AK168=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G168,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW168),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU168),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G168=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G168,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL169=\"\",\"-\",BF169*AM169*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G169,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G169=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G169,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I169:AJ169,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H169)","v":0},null,null,null,null,null,{"$f":"IF(AK169=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G169,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW169),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU169),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G169=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G169,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL170=\"\",\"-\",BF170*AM170*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G170,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G170=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G170,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I170:AJ170,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H170)","v":0},null,null,null,null,null,{"$f":"IF(AK170=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G170,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW170),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU170),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G170=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G170,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL171=\"\",\"-\",BF171*AM171*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G171,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G171=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G171,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I171:AJ171,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H171)","v":0},null,null,null,null,null,{"$f":"IF(AK171=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G171,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW171),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU171),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G171=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G171,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL172=\"\",\"-\",BF172*AM172*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G172,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G172=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G172,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I172:AJ172,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H172)","v":0},null,null,null,null,null,{"$f":"IF(AK172=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G172,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW172),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU172),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G172=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G172,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL173=\"\",\"-\",BF173*AM173*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G173,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G173=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G173,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I173:AJ173,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H173)","v":0},null,null,null,null,null,{"$f":"IF(AK173=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G173,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW173),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU173),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G173=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G173,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL174=\"\",\"-\",BF174*AM174*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G174,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G174=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G174,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I174:AJ174,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H174)","v":0},null,null,null,null,null,{"$f":"IF(AK174=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G174,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW174),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU174),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G174=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G174,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL175=\"\",\"-\",BF175*AM175*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G175,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G175=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G175,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I175:AJ175,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H175)","v":0},null,null,null,null,null,{"$f":"IF(AK175=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G175,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW175),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU175),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G175=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G175,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL176=\"\",\"-\",BF176*AM176*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G176,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G176=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G176,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I176:AJ176,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H176)","v":0},null,null,null,null,null,{"$f":"IF(AK176=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G176,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW176),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU176),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G176=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G176,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL177=\"\",\"-\",BF177*AM177*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G177,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G177=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G177,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I177:AJ177,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H177)","v":0},null,null,null,null,null,{"$f":"IF(AK177=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G177,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW177),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU177),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G177=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G177,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL178=\"\",\"-\",BF178*AM178*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G178,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G178=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G178,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I178:AJ178,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H178)","v":0},null,null,null,null,null,{"$f":"IF(AK178=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G178,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW178),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU178),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G178=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G178,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL179=\"\",\"-\",BF179*AM179*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G179,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G179=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G179,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I179:AJ179,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H179)","v":0},null,null,null,null,null,{"$f":"IF(AK179=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G179,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW179),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU179),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G179=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G179,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL180=\"\",\"-\",BF180*AM180*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G180,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G180=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G180,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I180:AJ180,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H180)","v":0},null,null,null,null,null,{"$f":"IF(AK180=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G180,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW180),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU180),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G180=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G180,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL181=\"\",\"-\",BF181*AM181*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G181,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G181=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G181,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I181:AJ181,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H181)","v":0},null,null,null,null,null,{"$f":"IF(AK181=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G181,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW181),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU181),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G181=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G181,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL182=\"\",\"-\",BF182*AM182*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G182,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G182=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G182,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I182:AJ182,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H182)","v":0},null,null,null,null,null,{"$f":"IF(AK182=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G182,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW182),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU182),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G182=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G182,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL183=\"\",\"-\",BF183*AM183*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G183,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G183=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G183,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I183:AJ183,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H183)","v":0},null,null,null,null,null,{"$f":"IF(AK183=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G183,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW183),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU183),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G183=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G183,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL184=\"\",\"-\",BF184*AM184*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G184,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G184=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G184,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I184:AJ184,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H184)","v":0},null,null,null,null,null,{"$f":"IF(AK184=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G184,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW184),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU184),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G184=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G184,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL185=\"\",\"-\",BF185*AM185*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G185,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G185=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G185,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I185:AJ185,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H185)","v":0},null,null,null,null,null,{"$f":"IF(AK185=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G185,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW185),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU185),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G185=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G185,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL186=\"\",\"-\",BF186*AM186*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G186,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G186=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G186,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I186:AJ186,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H186)","v":0},null,null,null,null,null,{"$f":"IF(AK186=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G186,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW186),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU186),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G186=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G186,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL187=\"\",\"-\",BF187*AM187*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G187,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G187=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G187,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I187:AJ187,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H187)","v":0},null,null,null,null,null,{"$f":"IF(AK187=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G187,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW187),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU187),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G187=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G187,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL188=\"\",\"-\",BF188*AM188*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G188,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G188=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G188,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I188:AJ188,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H188)","v":0},null,null,null,null,null,{"$f":"IF(AK188=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G188,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW188),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU188),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G188=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G188,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL189=\"\",\"-\",BF189*AM189*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G189,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G189=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G189,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I189:AJ189,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H189)","v":0},null,null,null,null,null,{"$f":"IF(AK189=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G189,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW189),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU189),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G189=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G189,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL190=\"\",\"-\",BF190*AM190*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G190,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G190=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G190,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I190:AJ190,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H190)","v":0},null,null,null,null,null,{"$f":"IF(AK190=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G190,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW190),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU190),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G190=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G190,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL191=\"\",\"-\",BF191*AM191*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G191,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G191=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G191,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I191:AJ191,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H191)","v":0},null,null,null,null,null,{"$f":"IF(AK191=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G191,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW191),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU191),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G191=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G191,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL192=\"\",\"-\",BF192*AM192*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G192,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G192=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G192,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I192:AJ192,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H192)","v":0},null,null,null,null,null,{"$f":"IF(AK192=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G192,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW192),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU192),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G192=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G192,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL193=\"\",\"-\",BF193*AM193*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G193,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G193=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G193,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I193:AJ193,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H193)","v":0},null,null,null,null,null,{"$f":"IF(AK193=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G193,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW193),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU193),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G193=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G193,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL194=\"\",\"-\",BF194*AM194*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G194,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G194=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G194,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I194:AJ194,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H194)","v":0},null,null,null,null,null,{"$f":"IF(AK194=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G194,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW194),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU194),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G194=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G194,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL195=\"\",\"-\",BF195*AM195*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G195,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G195=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G195,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I195:AJ195,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H195)","v":0},null,null,null,null,null,{"$f":"IF(AK195=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G195,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW195),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU195),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G195=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G195,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL196=\"\",\"-\",BF196*AM196*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G196,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G196=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G196,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I196:AJ196,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H196)","v":0},null,null,null,null,null,{"$f":"IF(AK196=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G196,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW196),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU196),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G196=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G196,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL197=\"\",\"-\",BF197*AM197*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G197,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G197=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G197,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I197:AJ197,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H197)","v":0},null,null,null,null,null,{"$f":"IF(AK197=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G197,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW197),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU197),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G197=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G197,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL198=\"\",\"-\",BF198*AM198*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G198,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G198=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G198,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I198:AJ198,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H198)","v":0},null,null,null,null,null,{"$f":"IF(AK198=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G198,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW198),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU198),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G198=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G198,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL199=\"\",\"-\",BF199*AM199*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G199,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G199=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G199,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I199:AJ199,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H199)","v":0},null,null,null,null,null,{"$f":"IF(AK199=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G199,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW199),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU199),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G199=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G199,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL200=\"\",\"-\",BF200*AM200*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G200,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G200=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G200,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I200:AJ200,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H200)","v":0},null,null,null,null,null,{"$f":"IF(AK200=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G200,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW200),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU200),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G200=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G200,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL201=\"\",\"-\",BF201*AM201*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G201,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G201=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G201,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I201:AJ201,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H201)","v":0},null,null,null,null,null,{"$f":"IF(AK201=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G201,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW201),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU201),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G201=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G201,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL202=\"\",\"-\",BF202*AM202*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G202,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G202=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G202,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I202:AJ202,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H202)","v":0},null,null,null,null,null,{"$f":"IF(AK202=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G202,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW202),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU202),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G202=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G202,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL203=\"\",\"-\",BF203*AM203*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G203,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G203=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G203,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I203:AJ203,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H203)","v":0},null,null,null,null,null,{"$f":"IF(AK203=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G203,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW203),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU203),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G203=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G203,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL204=\"\",\"-\",BF204*AM204*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G204,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G204=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G204,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I204:AJ204,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H204)","v":0},null,null,null,null,null,{"$f":"IF(AK204=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G204,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW204),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU204),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G204=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G204,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL205=\"\",\"-\",BF205*AM205*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G205,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G205=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G205,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I205:AJ205,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H205)","v":0},null,null,null,null,null,{"$f":"IF(AK205=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G205,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW205),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU205),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G205=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G205,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL206=\"\",\"-\",BF206*AM206*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G206,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G206=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G206,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I206:AJ206,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H206)","v":0},null,null,null,null,null,{"$f":"IF(AK206=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G206,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW206),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU206),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G206=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G206,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL207=\"\",\"-\",BF207*AM207*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G207,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G207=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G207,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I207:AJ207,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H207)","v":0},null,null,null,null,null,{"$f":"IF(AK207=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G207,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW207),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU207),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G207=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G207,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL208=\"\",\"-\",BF208*AM208*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G208,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G208=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G208,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I208:AJ208,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H208)","v":0},null,null,null,null,null,{"$f":"IF(AK208=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G208,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW208),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU208),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G208=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G208,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL209=\"\",\"-\",BF209*AM209*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G209,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G209=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G209,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I209:AJ209,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H209)","v":0},null,null,null,null,null,{"$f":"IF(AK209=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G209,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW209),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU209),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G209=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G209,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL210=\"\",\"-\",BF210*AM210*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G210,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G210=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G210,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I210:AJ210,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H210)","v":0},null,null,null,null,null,{"$f":"IF(AK210=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G210,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW210),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU210),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G210=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G210,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL211=\"\",\"-\",BF211*AM211*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G211,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G211=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G211,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I211:AJ211,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H211)","v":0},null,null,null,null,null,{"$f":"IF(AK211=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G211,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW211),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU211),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G211=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G211,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL212=\"\",\"-\",BF212*AM212*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G212,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G212=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G212,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I212:AJ212,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H212)","v":0},null,null,null,null,null,{"$f":"IF(AK212=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G212,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW212),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU212),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G212=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G212,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL213=\"\",\"-\",BF213*AM213*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G213,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G213=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G213,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I213:AJ213,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H213)","v":0},null,null,null,null,null,{"$f":"IF(AK213=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G213,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW213),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU213),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G213=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G213,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL214=\"\",\"-\",BF214*AM214*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G214,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G214=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G214,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I214:AJ214,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H214)","v":0},null,null,null,null,null,{"$f":"IF(AK214=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G214,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW214),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU214),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G214=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G214,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL215=\"\",\"-\",BF215*AM215*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G215,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G215=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G215,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I215:AJ215,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H215)","v":0},null,null,null,null,null,{"$f":"IF(AK215=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G215,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW215),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU215),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G215=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G215,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL216=\"\",\"-\",BF216*AM216*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G216,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G216=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G216,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I216:AJ216,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H216)","v":0},null,null,null,null,null,{"$f":"IF(AK216=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G216,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW216),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU216),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G216=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G216,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL217=\"\",\"-\",BF217*AM217*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G217,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G217=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G217,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I217:AJ217,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H217)","v":0},null,null,null,null,null,{"$f":"IF(AK217=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G217,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW217),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU217),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G217=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G217,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL218=\"\",\"-\",BF218*AM218*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G218,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G218=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G218,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I218:AJ218,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H218)","v":0},null,null,null,null,null,{"$f":"IF(AK218=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G218,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW218),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU218),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G218=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G218,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL219=\"\",\"-\",BF219*AM219*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G219,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G219=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G219,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I219:AJ219,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H219)","v":0},null,null,null,null,null,{"$f":"IF(AK219=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G219,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW219),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU219),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G219=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G219,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL220=\"\",\"-\",BF220*AM220*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G220,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G220=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G220,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I220:AJ220,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H220)","v":0},null,null,null,null,null,{"$f":"IF(AK220=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G220,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW220),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU220),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G220=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G220,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,{"$f":"IF(ISBLANK(D221)=FALSE,1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL221=\"\",\"-\",BF221*AM221*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G221,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,{"$f":"IF(AU221=\"\",\"-\",IF(H221=\"\",0,AU221*H221))","v":"-"},0,{"$f":"IF(ISBLANK(H221)=FALSE,AQ221/H221,\"-\")","v":"-"},{"$f":"IF(G221=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G221,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-",{"$f":"IF(ISBLANK(H221)=FALSE,(AQ221-IF(ISNUMBER(AN221)=TRUE,AN221,0)*AK221)/H221,\"-\")","v":"-"},{"$f":"IFERROR(AQ221-AK221*IF(ISNUMBER(AN221)=TRUE,AN221,0),\"\")","v":0},{"$f":"MIN(SUMPRODUCT(I221:AJ221,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H221)","v":0},null,null,null,null,null,{"$f":"IF(AK221=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G221,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},{"$f":"IF(AL221=\"\",\"-\",IF(AL221=\"Other\",1,1.25))","v":"-"},{"$f":"IF(BF221=\"-\",\"-\",BF221*AN221)","v":"-"},{"$f":"IF(LEFT(CELLformula(AW221),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU221),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G221=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G221,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AL222=\"Manual-On Individual Workstation\",AL222=\"Partial-Auto-On Individual Workstation\",AL222=\"Other Individual Workstation\"),1.3,1)","v":1},{"$f":"IF(AL222=\"\",\"-\",BF222*AM222*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G222,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,{"$f":"SUMPRODUCT(I222:AJ222,$I$23:$AJ$23)+IF(H222>0,MIN(IF(ISBLANK(AP222)=TRUE,0,AP222),H222)*BJ222/H222,0)","v":0},"-",{"$f":"SUMPRODUCT(I222:AJ222,$I$24:$AJ$24)","v":0},"-",{"$f":"IF(G222=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G222,'Lighting Assumptions'!$H$3:$H$112))","v":""},{"$f":"IF(ISBLANK(H222)=FALSE,AS222/H222,\"-\")","v":"-"},"-",0,{"$f":"MIN(SUMPRODUCT(I222:AJ222,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H222)","v":0},null,null,null,null,null,{"$f":"IF(AK222=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G222,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW222),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU222),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(BK222=\"\",\"-\",IF(H222=\"\",0,BK222*H222))","v":"-"},{"$f":"IF(G222=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G222,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL223=\"\",\"-\",BF223*AM223*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G223,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G223=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G223,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I223:AJ223,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H223)","v":0},null,null,null,null,null,{"$f":"IF(AK223=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G223,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW223),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU223),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G223=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G223,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL224=\"\",\"-\",BF224*AM224*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G224,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G224=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G224,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I224:AJ224,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H224)","v":0},null,null,null,null,null,{"$f":"IF(AK224=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G224,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW224),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU224),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G224=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G224,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL225=\"\",\"-\",BF225*AM225*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G225,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G225=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G225,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I225:AJ225,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H225)","v":0},null,null,null,null,null,{"$f":"IF(AK225=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G225,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW225),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU225),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G225=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G225,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL226=\"\",\"-\",BF226*AM226*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G226,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G226=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G226,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I226:AJ226,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H226)","v":0},null,null,null,null,null,{"$f":"IF(AK226=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G226,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW226),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU226),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G226=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G226,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL227=\"\",\"-\",BF227*AM227*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G227,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G227=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G227,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I227:AJ227,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H227)","v":0},null,null,null,null,null,{"$f":"IF(AK227=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G227,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW227),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU227),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G227=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G227,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL228=\"\",\"-\",BF228*AM228*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G228,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G228=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G228,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I228:AJ228,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H228)","v":0},null,null,null,null,null,{"$f":"IF(AK228=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G228,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW228),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU228),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G228=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G228,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL229=\"\",\"-\",BF229*AM229*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G229,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G229=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G229,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I229:AJ229,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H229)","v":0},null,null,null,null,null,{"$f":"IF(AK229=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G229,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW229),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU229),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G229=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G229,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL230=\"\",\"-\",BF230*AM230*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G230,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G230=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G230,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I230:AJ230,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H230)","v":0},null,null,null,null,null,{"$f":"IF(AK230=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G230,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW230),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU230),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G230=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G230,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL231=\"\",\"-\",BF231*AM231*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G231,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G231=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G231,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I231:AJ231,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H231)","v":0},null,null,null,null,null,{"$f":"IF(AK231=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G231,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW231),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU231),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G231=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G231,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL232=\"\",\"-\",BF232*AM232*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G232,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G232=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G232,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I232:AJ232,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H232)","v":0},null,null,null,null,null,{"$f":"IF(AK232=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G232,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW232),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU232),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G232=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G232,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL233=\"\",\"-\",BF233*AM233*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G233,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G233=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G233,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I233:AJ233,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H233)","v":0},null,null,null,null,null,{"$f":"IF(AK233=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G233,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW233),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU233),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G233=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G233,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL234=\"\",\"-\",BF234*AM234*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G234,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G234=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G234,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I234:AJ234,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H234)","v":0},null,null,null,null,null,{"$f":"IF(AK234=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G234,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW234),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU234),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G234=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G234,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL235=\"\",\"-\",BF235*AM235*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G235,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G235=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G235,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I235:AJ235,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H235)","v":0},null,null,null,null,null,{"$f":"IF(AK235=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G235,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW235),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU235),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G235=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G235,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL236=\"\",\"-\",BF236*AM236*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G236,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G236=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G236,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I236:AJ236,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H236)","v":0},null,null,null,null,null,{"$f":"IF(AK236=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G236,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW236),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU236),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G236=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G236,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL237=\"\",\"-\",BF237*AM237*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G237,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G237=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G237,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I237:AJ237,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H237)","v":0},null,null,null,null,null,{"$f":"IF(AK237=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G237,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW237),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU237),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G237=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G237,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL238=\"\",\"-\",BF238*AM238*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G238,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G238=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G238,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I238:AJ238,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H238)","v":0},null,null,null,null,null,{"$f":"IF(AK238=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G238,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW238),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU238),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G238=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G238,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL239=\"\",\"-\",BF239*AM239*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G239,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G239=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G239,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I239:AJ239,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H239)","v":0},null,null,null,null,null,{"$f":"IF(AK239=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G239,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW239),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU239),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G239=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G239,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL240=\"\",\"-\",BF240*AM240*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G240,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G240=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G240,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I240:AJ240,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H240)","v":0},null,null,null,null,null,{"$f":"IF(AK240=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G240,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW240),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU240),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G240=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G240,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL241=\"\",\"-\",BF241*AM241*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G241,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G241=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G241,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I241:AJ241,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H241)","v":0},null,null,null,null,null,{"$f":"IF(AK241=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G241,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW241),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU241),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G241=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G241,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL242=\"\",\"-\",BF242*AM242*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G242,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G242=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G242,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I242:AJ242,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H242)","v":0},null,null,null,null,null,{"$f":"IF(AK242=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G242,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW242),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU242),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G242=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G242,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL243=\"\",\"-\",BF243*AM243*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G243,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G243=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G243,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I243:AJ243,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H243)","v":0},null,null,null,null,null,{"$f":"IF(AK243=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G243,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW243),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU243),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G243=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G243,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL244=\"\",\"-\",BF244*AM244*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G244,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G244=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G244,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I244:AJ244,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H244)","v":0},null,null,null,null,null,{"$f":"IF(AK244=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G244,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW244),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU244),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G244=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G244,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL245=\"\",\"-\",BF245*AM245*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G245,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G245=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G245,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I245:AJ245,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H245)","v":0},null,null,null,null,null,{"$f":"IF(AK245=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G245,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW245),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU245),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G245=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G245,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL246=\"\",\"-\",BF246*AM246*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G246,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G246=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G246,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I246:AJ246,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H246)","v":0},null,null,null,null,null,{"$f":"IF(AK246=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G246,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW246),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU246),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G246=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G246,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL247=\"\",\"-\",BF247*AM247*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G247,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G247=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G247,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I247:AJ247,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H247)","v":0},null,null,null,null,null,{"$f":"IF(AK247=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G247,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW247),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU247),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G247=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G247,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL248=\"\",\"-\",BF248*AM248*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G248,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G248=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G248,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I248:AJ248,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H248)","v":0},null,null,null,null,null,{"$f":"IF(AK248=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G248,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW248),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU248),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G248=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G248,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL249=\"\",\"-\",BF249*AM249*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G249,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G249=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G249,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I249:AJ249,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H249)","v":0},null,null,null,null,null,{"$f":"IF(AK249=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G249,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW249),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU249),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G249=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G249,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL250=\"\",\"-\",BF250*AM250*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G250,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G250=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G250,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I250:AJ250,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H250)","v":0},null,null,null,null,null,{"$f":"IF(AK250=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G250,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW250),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU250),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G250=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G250,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL251=\"\",\"-\",BF251*AM251*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G251,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G251=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G251,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I251:AJ251,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H251)","v":0},null,null,null,null,null,{"$f":"IF(AK251=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G251,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW251),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU251),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G251=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G251,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL252=\"\",\"-\",BF252*AM252*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G252,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G252=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G252,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I252:AJ252,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H252)","v":0},null,null,null,null,null,{"$f":"IF(AK252=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G252,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW252),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU252),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G252=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G252,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL253=\"\",\"-\",BF253*AM253*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G253,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G253=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G253,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I253:AJ253,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H253)","v":0},null,null,null,null,null,{"$f":"IF(AK253=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G253,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW253),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU253),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G253=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G253,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL254=\"\",\"-\",BF254*AM254*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G254,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G254=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G254,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I254:AJ254,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H254)","v":0},null,null,null,null,null,{"$f":"IF(AK254=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G254,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW254),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU254),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G254=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G254,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL255=\"\",\"-\",BF255*AM255*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G255,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G255=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G255,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I255:AJ255,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H255)","v":0},null,null,null,null,null,{"$f":"IF(AK255=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G255,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW255),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU255),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G255=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G255,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL256=\"\",\"-\",BF256*AM256*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G256,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G256=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G256,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I256:AJ256,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H256)","v":0},null,null,null,null,null,{"$f":"IF(AK256=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G256,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW256),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU256),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G256=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G256,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL257=\"\",\"-\",BF257*AM257*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G257,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G257=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G257,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I257:AJ257,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H257)","v":0},null,null,null,null,null,{"$f":"IF(AK257=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G257,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW257),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU257),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G257=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G257,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL258=\"\",\"-\",BF258*AM258*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G258,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G258=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G258,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I258:AJ258,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H258)","v":0},null,null,null,null,null,{"$f":"IF(AK258=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G258,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW258),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU258),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G258=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G258,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL259=\"\",\"-\",BF259*AM259*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G259,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G259=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G259,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I259:AJ259,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H259)","v":0},null,null,null,null,null,{"$f":"IF(AK259=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G259,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW259),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU259),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G259=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G259,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL260=\"\",\"-\",BF260*AM260*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G260,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G260=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G260,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I260:AJ260,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H260)","v":0},null,null,null,null,null,{"$f":"IF(AK260=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G260,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW260),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU260),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G260=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G260,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL261=\"\",\"-\",BF261*AM261*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G261,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G261=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G261,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I261:AJ261,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H261)","v":0},null,null,null,null,null,{"$f":"IF(AK261=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G261,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW261),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU261),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G261=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G261,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL262=\"\",\"-\",BF262*AM262*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G262,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G262=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G262,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I262:AJ262,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H262)","v":0},null,null,null,null,null,{"$f":"IF(AK262=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G262,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW262),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU262),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G262=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G262,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL263=\"\",\"-\",BF263*AM263*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G263,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G263=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G263,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I263:AJ263,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H263)","v":0},null,null,null,null,null,{"$f":"IF(AK263=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G263,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW263),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU263),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G263=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G263,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL264=\"\",\"-\",BF264*AM264*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G264,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G264=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G264,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I264:AJ264,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H264)","v":0},null,null,null,null,null,{"$f":"IF(AK264=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G264,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW264),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU264),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G264=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G264,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL265=\"\",\"-\",BF265*AM265*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G265,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G265=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G265,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I265:AJ265,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H265)","v":0},null,null,null,null,null,{"$f":"IF(AK265=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G265,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW265),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU265),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G265=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G265,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL266=\"\",\"-\",BF266*AM266*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G266,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G266=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G266,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I266:AJ266,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H266)","v":0},null,null,null,null,null,{"$f":"IF(AK266=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G266,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW266),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU266),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G266=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G266,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL267=\"\",\"-\",BF267*AM267*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G267,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G267=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G267,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I267:AJ267,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H267)","v":0},null,null,null,null,null,{"$f":"IF(AK267=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G267,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW267),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU267),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G267=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G267,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL268=\"\",\"-\",BF268*AM268*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G268,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G268=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G268,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I268:AJ268,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H268)","v":0},null,null,null,null,null,{"$f":"IF(AK268=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G268,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW268),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU268),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G268=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G268,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL269=\"\",\"-\",BF269*AM269*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G269,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G269=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G269,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I269:AJ269,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H269)","v":0},null,null,null,null,null,{"$f":"IF(AK269=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G269,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW269),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU269),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G269=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G269,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL270=\"\",\"-\",BF270*AM270*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G270,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G270=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G270,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I270:AJ270,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H270)","v":0},null,null,null,null,null,{"$f":"IF(AK270=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G270,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW270),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU270),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G270=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G270,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL271=\"\",\"-\",BF271*AM271*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G271,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G271=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G271,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I271:AJ271,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H271)","v":0},null,null,null,null,null,{"$f":"IF(AK271=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G271,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW271),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU271),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G271=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G271,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL272=\"\",\"-\",BF272*AM272*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G272,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G272=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G272,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I272:AJ272,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H272)","v":0},null,null,null,null,null,{"$f":"IF(AK272=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G272,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW272),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU272),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G272=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G272,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL273=\"\",\"-\",BF273*AM273*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G273,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G273=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G273,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I273:AJ273,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H273)","v":0},null,null,null,null,null,{"$f":"IF(AK273=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G273,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW273),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU273),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G273=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G273,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL274=\"\",\"-\",BF274*AM274*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G274,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G274=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G274,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I274:AJ274,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H274)","v":0},null,null,null,null,null,{"$f":"IF(AK274=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G274,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW274),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU274),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G274=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G274,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL275=\"\",\"-\",BF275*AM275*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G275,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G275=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G275,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I275:AJ275,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H275)","v":0},null,null,null,null,null,{"$f":"IF(AK275=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G275,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW275),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU275),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G275=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G275,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL276=\"\",\"-\",BF276*AM276*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G276,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G276=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G276,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I276:AJ276,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H276)","v":0},null,null,null,null,null,{"$f":"IF(AK276=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G276,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW276),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU276),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G276=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G276,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL277=\"\",\"-\",BF277*AM277*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G277,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G277=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G277,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I277:AJ277,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H277)","v":0},null,null,null,null,null,{"$f":"IF(AK277=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G277,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW277),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU277),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G277=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G277,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL278=\"\",\"-\",BF278*AM278*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G278,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G278=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G278,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I278:AJ278,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H278)","v":0},null,null,null,null,null,{"$f":"IF(AK278=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G278,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW278),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU278),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G278=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G278,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL279=\"\",\"-\",BF279*AM279*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G279,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G279=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G279,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I279:AJ279,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H279)","v":0},null,null,null,null,null,{"$f":"IF(AK279=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G279,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW279),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU279),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G279=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G279,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL280=\"\",\"-\",BF280*AM280*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G280,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G280=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G280,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I280:AJ280,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H280)","v":0},null,null,null,null,null,{"$f":"IF(AK280=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G280,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW280),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU280),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G280=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G280,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL281=\"\",\"-\",BF281*AM281*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G281,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G281=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G281,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I281:AJ281,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H281)","v":0},null,null,null,null,null,{"$f":"IF(AK281=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G281,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW281),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU281),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G281=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G281,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL282=\"\",\"-\",BF282*AM282*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G282,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G282=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G282,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I282:AJ282,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H282)","v":0},null,null,null,null,null,{"$f":"IF(AK282=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G282,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW282),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU282),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G282=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G282,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL283=\"\",\"-\",BF283*AM283*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G283,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G283=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G283,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I283:AJ283,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H283)","v":0},null,null,null,null,null,{"$f":"IF(AK283=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G283,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW283),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU283),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G283=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G283,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL284=\"\",\"-\",BF284*AM284*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G284,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G284=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G284,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I284:AJ284,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H284)","v":0},null,null,null,null,null,{"$f":"IF(AK284=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G284,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW284),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU284),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G284=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G284,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,{"$f":"IF(ISBLANK(D285)=FALSE,1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL285=\"\",\"-\",BF285*AM285*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G285,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,{"$f":"IF(AU285=\"\",\"-\",IF(H285=\"\",0,AU285*H285))","v":"-"},0,{"$f":"IF(ISBLANK(H285)=FALSE,AQ285/H285,\"-\")","v":"-"},{"$f":"IF(G285=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G285,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-",{"$f":"IF(ISBLANK(H285)=FALSE,(AQ285-IF(ISNUMBER(AN285)=TRUE,AN285,0)*AK285)/H285,\"-\")","v":"-"},{"$f":"IFERROR(AQ285-AK285*IF(ISNUMBER(AN285)=TRUE,AN285,0),\"\")","v":0},{"$f":"MIN(SUMPRODUCT(I285:AJ285,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H285)","v":0},null,null,null,null,null,{"$f":"IF(AK285=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G285,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},{"$f":"IF(AL285=\"\",\"-\",IF(AL285=\"Other\",1,1.25))","v":"-"},{"$f":"IF(BF285=\"-\",\"-\",BF285*AN285)","v":"-"},{"$f":"IF(LEFT(CELLformula(AW285),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU285),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G285=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G285,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AL286=\"Manual-On Individual Workstation\",AL286=\"Partial-Auto-On Individual Workstation\",AL286=\"Other Individual Workstation\"),1.3,1)","v":1},{"$f":"IF(AL286=\"\",\"-\",BF286*AM286*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G286,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,{"$f":"SUMPRODUCT(I286:AJ286,$I$23:$AJ$23)+IF(H286>0,MIN(IF(ISBLANK(AP286)=TRUE,0,AP286),H286)*BJ286/H286,0)","v":0},"-",{"$f":"SUMPRODUCT(I286:AJ286,$I$24:$AJ$24)","v":0},"-",{"$f":"IF(G286=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G286,'Lighting Assumptions'!$H$3:$H$112))","v":""},{"$f":"IF(ISBLANK(H286)=FALSE,AS286/H286,\"-\")","v":"-"},"-",0,{"$f":"MIN(SUMPRODUCT(I286:AJ286,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H286)","v":0},null,null,null,null,null,{"$f":"IF(AK286=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G286,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW286),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU286),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(BK286=\"\",\"-\",IF(H286=\"\",0,BK286*H286))","v":"-"},{"$f":"IF(G286=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G286,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL287=\"\",\"-\",BF287*AM287*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G287,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G287=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G287,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I287:AJ287,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H287)","v":0},null,null,null,null,null,{"$f":"IF(AK287=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G287,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW287),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU287),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G287=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G287,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL288=\"\",\"-\",BF288*AM288*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G288,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G288=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G288,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I288:AJ288,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H288)","v":0},null,null,null,null,null,{"$f":"IF(AK288=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G288,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW288),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU288),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G288=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G288,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL289=\"\",\"-\",BF289*AM289*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G289,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G289=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G289,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I289:AJ289,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H289)","v":0},null,null,null,null,null,{"$f":"IF(AK289=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G289,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW289),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU289),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G289=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G289,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL290=\"\",\"-\",BF290*AM290*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G290,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G290=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G290,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I290:AJ290,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H290)","v":0},null,null,null,null,null,{"$f":"IF(AK290=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G290,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW290),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU290),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G290=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G290,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL291=\"\",\"-\",BF291*AM291*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G291,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G291=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G291,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I291:AJ291,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H291)","v":0},null,null,null,null,null,{"$f":"IF(AK291=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G291,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW291),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU291),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G291=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G291,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL292=\"\",\"-\",BF292*AM292*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G292,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G292=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G292,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I292:AJ292,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H292)","v":0},null,null,null,null,null,{"$f":"IF(AK292=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G292,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW292),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU292),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G292=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G292,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL293=\"\",\"-\",BF293*AM293*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G293,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G293=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G293,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I293:AJ293,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H293)","v":0},null,null,null,null,null,{"$f":"IF(AK293=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G293,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW293),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU293),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G293=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G293,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL294=\"\",\"-\",BF294*AM294*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G294,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G294=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G294,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I294:AJ294,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H294)","v":0},null,null,null,null,null,{"$f":"IF(AK294=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G294,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW294),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU294),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G294=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G294,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL295=\"\",\"-\",BF295*AM295*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G295,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G295=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G295,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I295:AJ295,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H295)","v":0},null,null,null,null,null,{"$f":"IF(AK295=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G295,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW295),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU295),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G295=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G295,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL296=\"\",\"-\",BF296*AM296*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G296,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G296=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G296,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I296:AJ296,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H296)","v":0},null,null,null,null,null,{"$f":"IF(AK296=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G296,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW296),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU296),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G296=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G296,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL297=\"\",\"-\",BF297*AM297*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G297,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G297=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G297,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I297:AJ297,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H297)","v":0},null,null,null,null,null,{"$f":"IF(AK297=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G297,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW297),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU297),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G297=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G297,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL298=\"\",\"-\",BF298*AM298*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G298,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G298=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G298,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I298:AJ298,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H298)","v":0},null,null,null,null,null,{"$f":"IF(AK298=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G298,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW298),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU298),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G298=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G298,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL299=\"\",\"-\",BF299*AM299*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G299,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G299=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G299,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I299:AJ299,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H299)","v":0},null,null,null,null,null,{"$f":"IF(AK299=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G299,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW299),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU299),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G299=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G299,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL300=\"\",\"-\",BF300*AM300*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G300,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G300=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G300,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I300:AJ300,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H300)","v":0},null,null,null,null,null,{"$f":"IF(AK300=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G300,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW300),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU300),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G300=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G300,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL301=\"\",\"-\",BF301*AM301*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G301,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G301=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G301,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I301:AJ301,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H301)","v":0},null,null,null,null,null,{"$f":"IF(AK301=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G301,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW301),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU301),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G301=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G301,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL302=\"\",\"-\",BF302*AM302*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G302,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G302=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G302,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I302:AJ302,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H302)","v":0},null,null,null,null,null,{"$f":"IF(AK302=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G302,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW302),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU302),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G302=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G302,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL303=\"\",\"-\",BF303*AM303*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G303,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G303=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G303,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I303:AJ303,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H303)","v":0},null,null,null,null,null,{"$f":"IF(AK303=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G303,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW303),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU303),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G303=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G303,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL304=\"\",\"-\",BF304*AM304*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G304,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G304=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G304,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I304:AJ304,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H304)","v":0},null,null,null,null,null,{"$f":"IF(AK304=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G304,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW304),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU304),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G304=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G304,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL305=\"\",\"-\",BF305*AM305*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G305,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G305=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G305,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I305:AJ305,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H305)","v":0},null,null,null,null,null,{"$f":"IF(AK305=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G305,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW305),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU305),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G305=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G305,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL306=\"\",\"-\",BF306*AM306*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G306,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G306=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G306,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I306:AJ306,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H306)","v":0},null,null,null,null,null,{"$f":"IF(AK306=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G306,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW306),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU306),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G306=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G306,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL307=\"\",\"-\",BF307*AM307*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G307,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G307=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G307,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I307:AJ307,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H307)","v":0},null,null,null,null,null,{"$f":"IF(AK307=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G307,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW307),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU307),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G307=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G307,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL308=\"\",\"-\",BF308*AM308*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G308,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G308=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G308,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I308:AJ308,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H308)","v":0},null,null,null,null,null,{"$f":"IF(AK308=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G308,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW308),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU308),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G308=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G308,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL309=\"\",\"-\",BF309*AM309*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G309,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G309=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G309,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I309:AJ309,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H309)","v":0},null,null,null,null,null,{"$f":"IF(AK309=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G309,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW309),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU309),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G309=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G309,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL310=\"\",\"-\",BF310*AM310*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G310,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G310=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G310,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I310:AJ310,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H310)","v":0},null,null,null,null,null,{"$f":"IF(AK310=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G310,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW310),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU310),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G310=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G310,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL311=\"\",\"-\",BF311*AM311*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G311,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G311=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G311,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I311:AJ311,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H311)","v":0},null,null,null,null,null,{"$f":"IF(AK311=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G311,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW311),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU311),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G311=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G311,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL312=\"\",\"-\",BF312*AM312*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G312,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G312=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G312,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I312:AJ312,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H312)","v":0},null,null,null,null,null,{"$f":"IF(AK312=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G312,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW312),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU312),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G312=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G312,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL313=\"\",\"-\",BF313*AM313*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G313,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G313=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G313,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I313:AJ313,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H313)","v":0},null,null,null,null,null,{"$f":"IF(AK313=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G313,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW313),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU313),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G313=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G313,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL314=\"\",\"-\",BF314*AM314*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G314,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G314=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G314,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I314:AJ314,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H314)","v":0},null,null,null,null,null,{"$f":"IF(AK314=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G314,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW314),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU314),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G314=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G314,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL315=\"\",\"-\",BF315*AM315*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G315,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G315=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G315,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I315:AJ315,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H315)","v":0},null,null,null,null,null,{"$f":"IF(AK315=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G315,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW315),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU315),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G315=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G315,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL316=\"\",\"-\",BF316*AM316*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G316,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G316=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G316,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I316:AJ316,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H316)","v":0},null,null,null,null,null,{"$f":"IF(AK316=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G316,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW316),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU316),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G316=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G316,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL317=\"\",\"-\",BF317*AM317*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G317,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G317=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G317,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I317:AJ317,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H317)","v":0},null,null,null,null,null,{"$f":"IF(AK317=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G317,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW317),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU317),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G317=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G317,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL318=\"\",\"-\",BF318*AM318*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G318,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G318=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G318,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I318:AJ318,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H318)","v":0},null,null,null,null,null,{"$f":"IF(AK318=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G318,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW318),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU318),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G318=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G318,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL319=\"\",\"-\",BF319*AM319*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G319,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G319=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G319,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I319:AJ319,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H319)","v":0},null,null,null,null,null,{"$f":"IF(AK319=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G319,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW319),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU319),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G319=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G319,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL320=\"\",\"-\",BF320*AM320*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G320,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G320=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G320,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I320:AJ320,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H320)","v":0},null,null,null,null,null,{"$f":"IF(AK320=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G320,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW320),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU320),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G320=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G320,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL321=\"\",\"-\",BF321*AM321*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G321,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G321=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G321,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I321:AJ321,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H321)","v":0},null,null,null,null,null,{"$f":"IF(AK321=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G321,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW321),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU321),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G321=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G321,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL322=\"\",\"-\",BF322*AM322*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G322,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G322=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G322,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I322:AJ322,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H322)","v":0},null,null,null,null,null,{"$f":"IF(AK322=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G322,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW322),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU322),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G322=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G322,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL323=\"\",\"-\",BF323*AM323*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G323,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G323=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G323,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I323:AJ323,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H323)","v":0},null,null,null,null,null,{"$f":"IF(AK323=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G323,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW323),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU323),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G323=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G323,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL324=\"\",\"-\",BF324*AM324*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G324,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G324=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G324,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I324:AJ324,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H324)","v":0},null,null,null,null,null,{"$f":"IF(AK324=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G324,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW324),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU324),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G324=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G324,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL325=\"\",\"-\",BF325*AM325*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G325,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G325=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G325,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I325:AJ325,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H325)","v":0},null,null,null,null,null,{"$f":"IF(AK325=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G325,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW325),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU325),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G325=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G325,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL326=\"\",\"-\",BF326*AM326*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G326,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G326=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G326,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I326:AJ326,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H326)","v":0},null,null,null,null,null,{"$f":"IF(AK326=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G326,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW326),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU326),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G326=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G326,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL327=\"\",\"-\",BF327*AM327*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G327,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G327=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G327,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I327:AJ327,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H327)","v":0},null,null,null,null,null,{"$f":"IF(AK327=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G327,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW327),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU327),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G327=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G327,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL328=\"\",\"-\",BF328*AM328*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G328,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G328=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G328,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I328:AJ328,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H328)","v":0},null,null,null,null,null,{"$f":"IF(AK328=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G328,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW328),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU328),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G328=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G328,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL329=\"\",\"-\",BF329*AM329*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G329,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G329=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G329,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I329:AJ329,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H329)","v":0},null,null,null,null,null,{"$f":"IF(AK329=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G329,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW329),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU329),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G329=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G329,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL330=\"\",\"-\",BF330*AM330*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G330,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G330=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G330,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I330:AJ330,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H330)","v":0},null,null,null,null,null,{"$f":"IF(AK330=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G330,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW330),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU330),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G330=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G330,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL331=\"\",\"-\",BF331*AM331*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G331,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G331=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G331,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I331:AJ331,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H331)","v":0},null,null,null,null,null,{"$f":"IF(AK331=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G331,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW331),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU331),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G331=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G331,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL332=\"\",\"-\",BF332*AM332*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G332,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G332=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G332,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I332:AJ332,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H332)","v":0},null,null,null,null,null,{"$f":"IF(AK332=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G332,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW332),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU332),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G332=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G332,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL333=\"\",\"-\",BF333*AM333*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G333,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G333=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G333,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I333:AJ333,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H333)","v":0},null,null,null,null,null,{"$f":"IF(AK333=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G333,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW333),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU333),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G333=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G333,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL334=\"\",\"-\",BF334*AM334*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G334,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G334=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G334,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I334:AJ334,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H334)","v":0},null,null,null,null,null,{"$f":"IF(AK334=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G334,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW334),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU334),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G334=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G334,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL335=\"\",\"-\",BF335*AM335*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G335,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G335=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G335,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I335:AJ335,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H335)","v":0},null,null,null,null,null,{"$f":"IF(AK335=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G335,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW335),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU335),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G335=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G335,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL336=\"\",\"-\",BF336*AM336*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G336,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G336=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G336,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I336:AJ336,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H336)","v":0},null,null,null,null,null,{"$f":"IF(AK336=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G336,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW336),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU336),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G336=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G336,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL337=\"\",\"-\",BF337*AM337*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G337,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G337=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G337,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I337:AJ337,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H337)","v":0},null,null,null,null,null,{"$f":"IF(AK337=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G337,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW337),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU337),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G337=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G337,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL338=\"\",\"-\",BF338*AM338*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G338,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G338=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G338,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I338:AJ338,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H338)","v":0},null,null,null,null,null,{"$f":"IF(AK338=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G338,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW338),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU338),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G338=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G338,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL339=\"\",\"-\",BF339*AM339*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G339,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G339=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G339,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I339:AJ339,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H339)","v":0},null,null,null,null,null,{"$f":"IF(AK339=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G339,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW339),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU339),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G339=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G339,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL340=\"\",\"-\",BF340*AM340*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G340,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G340=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G340,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I340:AJ340,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H340)","v":0},null,null,null,null,null,{"$f":"IF(AK340=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G340,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW340),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU340),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G340=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G340,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL341=\"\",\"-\",BF341*AM341*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G341,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G341=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G341,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I341:AJ341,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H341)","v":0},null,null,null,null,null,{"$f":"IF(AK341=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G341,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW341),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU341),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G341=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G341,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL342=\"\",\"-\",BF342*AM342*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G342,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G342=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G342,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I342:AJ342,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H342)","v":0},null,null,null,null,null,{"$f":"IF(AK342=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G342,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW342),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU342),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G342=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G342,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL343=\"\",\"-\",BF343*AM343*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G343,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G343=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G343,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I343:AJ343,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H343)","v":0},null,null,null,null,null,{"$f":"IF(AK343=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G343,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW343),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU343),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G343=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G343,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL344=\"\",\"-\",BF344*AM344*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G344,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G344=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G344,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I344:AJ344,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H344)","v":0},null,null,null,null,null,{"$f":"IF(AK344=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G344,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW344),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU344),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G344=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G344,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL345=\"\",\"-\",BF345*AM345*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G345,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G345=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G345,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I345:AJ345,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H345)","v":0},null,null,null,null,null,{"$f":"IF(AK345=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G345,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW345),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU345),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G345=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G345,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL346=\"\",\"-\",BF346*AM346*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G346,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G346=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G346,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I346:AJ346,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H346)","v":0},null,null,null,null,null,{"$f":"IF(AK346=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G346,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW346),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU346),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G346=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G346,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL347=\"\",\"-\",BF347*AM347*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G347,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G347=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G347,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I347:AJ347,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H347)","v":0},null,null,null,null,null,{"$f":"IF(AK347=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G347,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW347),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU347),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G347=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G347,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL348=\"\",\"-\",BF348*AM348*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G348,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G348=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G348,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I348:AJ348,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H348)","v":0},null,null,null,null,null,{"$f":"IF(AK348=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G348,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW348),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU348),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G348=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G348,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,{"$f":"IF(ISBLANK(D349)=FALSE,1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL349=\"\",\"-\",BF349*AM349*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G349,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,{"$f":"IF(AU349=\"\",\"-\",IF(H349=\"\",0,AU349*H349))","v":"-"},0,{"$f":"IF(ISBLANK(H349)=FALSE,AQ349/H349,\"-\")","v":"-"},{"$f":"IF(G349=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G349,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-",{"$f":"IF(ISBLANK(H349)=FALSE,(AQ349-IF(ISNUMBER(AN349)=TRUE,AN349,0)*AK349)/H349,\"-\")","v":"-"},{"$f":"IFERROR(AQ349-AK349*IF(ISNUMBER(AN349)=TRUE,AN349,0),\"\")","v":0},{"$f":"MIN(SUMPRODUCT(I349:AJ349,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H349)","v":0},null,null,null,null,null,{"$f":"IF(AK349=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G349,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},{"$f":"IF(AL349=\"\",\"-\",IF(AL349=\"Other\",1,1.25))","v":"-"},{"$f":"IF(BF349=\"-\",\"-\",BF349*AN349)","v":"-"},{"$f":"IF(LEFT(CELLformula(AW349),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU349),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G349=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G349,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AL350=\"Manual-On Individual Workstation\",AL350=\"Partial-Auto-On Individual Workstation\",AL350=\"Other Individual Workstation\"),1.3,1)","v":1},{"$f":"IF(AL350=\"\",\"-\",BF350*AM350*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G350,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,{"$f":"SUMPRODUCT(I350:AJ350,$I$23:$AJ$23)+IF(H350>0,MIN(IF(ISBLANK(AP350)=TRUE,0,AP350),H350)*BJ350/H350,0)","v":0},"-",{"$f":"SUMPRODUCT(I350:AJ350,$I$24:$AJ$24)","v":0},"-",{"$f":"IF(G350=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G350,'Lighting Assumptions'!$H$3:$H$112))","v":""},{"$f":"IF(ISBLANK(H350)=FALSE,AS350/H350,\"-\")","v":"-"},"-",0,{"$f":"MIN(SUMPRODUCT(I350:AJ350,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H350)","v":0},null,null,null,null,null,{"$f":"IF(AK350=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G350,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW350),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU350),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(BK350=\"\",\"-\",IF(H350=\"\",0,BK350*H350))","v":"-"},{"$f":"IF(G350=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G350,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL351=\"\",\"-\",BF351*AM351*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G351,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G351=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G351,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I351:AJ351,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H351)","v":0},null,null,null,null,null,{"$f":"IF(AK351=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G351,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW351),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU351),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G351=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G351,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL352=\"\",\"-\",BF352*AM352*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G352,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G352=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G352,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I352:AJ352,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H352)","v":0},null,null,null,null,null,{"$f":"IF(AK352=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G352,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW352),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU352),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G352=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G352,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL353=\"\",\"-\",BF353*AM353*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G353,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G353=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G353,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I353:AJ353,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H353)","v":0},null,null,null,null,null,{"$f":"IF(AK353=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G353,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW353),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU353),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G353=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G353,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL354=\"\",\"-\",BF354*AM354*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G354,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G354=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G354,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I354:AJ354,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H354)","v":0},null,null,null,null,null,{"$f":"IF(AK354=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G354,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW354),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU354),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G354=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G354,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL355=\"\",\"-\",BF355*AM355*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G355,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G355=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G355,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I355:AJ355,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H355)","v":0},null,null,null,null,null,{"$f":"IF(AK355=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G355,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW355),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU355),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G355=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G355,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL356=\"\",\"-\",BF356*AM356*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G356,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G356=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G356,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I356:AJ356,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H356)","v":0},null,null,null,null,null,{"$f":"IF(AK356=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G356,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW356),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU356),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G356=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G356,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL357=\"\",\"-\",BF357*AM357*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G357,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G357=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G357,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I357:AJ357,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H357)","v":0},null,null,null,null,null,{"$f":"IF(AK357=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G357,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW357),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU357),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G357=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G357,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL358=\"\",\"-\",BF358*AM358*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G358,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G358=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G358,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I358:AJ358,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H358)","v":0},null,null,null,null,null,{"$f":"IF(AK358=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G358,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW358),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU358),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G358=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G358,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL359=\"\",\"-\",BF359*AM359*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G359,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G359=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G359,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I359:AJ359,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H359)","v":0},null,null,null,null,null,{"$f":"IF(AK359=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G359,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW359),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU359),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G359=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G359,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL360=\"\",\"-\",BF360*AM360*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G360,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G360=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G360,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I360:AJ360,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H360)","v":0},null,null,null,null,null,{"$f":"IF(AK360=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G360,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW360),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU360),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G360=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G360,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL361=\"\",\"-\",BF361*AM361*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G361,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G361=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G361,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I361:AJ361,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H361)","v":0},null,null,null,null,null,{"$f":"IF(AK361=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G361,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW361),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU361),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G361=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G361,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL362=\"\",\"-\",BF362*AM362*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G362,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G362=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G362,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I362:AJ362,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H362)","v":0},null,null,null,null,null,{"$f":"IF(AK362=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G362,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW362),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU362),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G362=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G362,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL363=\"\",\"-\",BF363*AM363*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G363,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G363=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G363,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I363:AJ363,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H363)","v":0},null,null,null,null,null,{"$f":"IF(AK363=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G363,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW363),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU363),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G363=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G363,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL364=\"\",\"-\",BF364*AM364*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G364,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G364=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G364,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I364:AJ364,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H364)","v":0},null,null,null,null,null,{"$f":"IF(AK364=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G364,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW364),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU364),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G364=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G364,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL365=\"\",\"-\",BF365*AM365*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G365,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G365=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G365,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I365:AJ365,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H365)","v":0},null,null,null,null,null,{"$f":"IF(AK365=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G365,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW365),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU365),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G365=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G365,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL366=\"\",\"-\",BF366*AM366*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G366,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G366=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G366,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I366:AJ366,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H366)","v":0},null,null,null,null,null,{"$f":"IF(AK366=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G366,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW366),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU366),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G366=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G366,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL367=\"\",\"-\",BF367*AM367*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G367,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G367=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G367,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I367:AJ367,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H367)","v":0},null,null,null,null,null,{"$f":"IF(AK367=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G367,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW367),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU367),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G367=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G367,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL368=\"\",\"-\",BF368*AM368*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G368,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G368=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G368,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I368:AJ368,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H368)","v":0},null,null,null,null,null,{"$f":"IF(AK368=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G368,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW368),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU368),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G368=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G368,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL369=\"\",\"-\",BF369*AM369*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G369,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G369=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G369,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I369:AJ369,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H369)","v":0},null,null,null,null,null,{"$f":"IF(AK369=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G369,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW369),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU369),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G369=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G369,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL370=\"\",\"-\",BF370*AM370*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G370,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G370=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G370,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I370:AJ370,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H370)","v":0},null,null,null,null,null,{"$f":"IF(AK370=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G370,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW370),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU370),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G370=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G370,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL371=\"\",\"-\",BF371*AM371*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G371,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G371=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G371,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I371:AJ371,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H371)","v":0},null,null,null,null,null,{"$f":"IF(AK371=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G371,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW371),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU371),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G371=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G371,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL372=\"\",\"-\",BF372*AM372*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G372,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G372=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G372,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I372:AJ372,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H372)","v":0},null,null,null,null,null,{"$f":"IF(AK372=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G372,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW372),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU372),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G372=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G372,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL373=\"\",\"-\",BF373*AM373*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G373,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G373=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G373,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I373:AJ373,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H373)","v":0},null,null,null,null,null,{"$f":"IF(AK373=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G373,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW373),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU373),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G373=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G373,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL374=\"\",\"-\",BF374*AM374*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G374,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G374=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G374,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I374:AJ374,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H374)","v":0},null,null,null,null,null,{"$f":"IF(AK374=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G374,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW374),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU374),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G374=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G374,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL375=\"\",\"-\",BF375*AM375*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G375,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G375=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G375,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I375:AJ375,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H375)","v":0},null,null,null,null,null,{"$f":"IF(AK375=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G375,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW375),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU375),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G375=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G375,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL376=\"\",\"-\",BF376*AM376*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G376,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G376=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G376,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I376:AJ376,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H376)","v":0},null,null,null,null,null,{"$f":"IF(AK376=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G376,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW376),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU376),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G376=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G376,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL377=\"\",\"-\",BF377*AM377*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G377,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G377=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G377,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I377:AJ377,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H377)","v":0},null,null,null,null,null,{"$f":"IF(AK377=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G377,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW377),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU377),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G377=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G377,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL378=\"\",\"-\",BF378*AM378*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G378,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G378=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G378,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I378:AJ378,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H378)","v":0},null,null,null,null,null,{"$f":"IF(AK378=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G378,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW378),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU378),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G378=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G378,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL379=\"\",\"-\",BF379*AM379*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G379,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G379=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G379,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I379:AJ379,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H379)","v":0},null,null,null,null,null,{"$f":"IF(AK379=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G379,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW379),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU379),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G379=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G379,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL380=\"\",\"-\",BF380*AM380*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G380,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G380=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G380,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I380:AJ380,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H380)","v":0},null,null,null,null,null,{"$f":"IF(AK380=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G380,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW380),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU380),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G380=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G380,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL381=\"\",\"-\",BF381*AM381*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G381,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G381=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G381,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I381:AJ381,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H381)","v":0},null,null,null,null,null,{"$f":"IF(AK381=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G381,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW381),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU381),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G381=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G381,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL382=\"\",\"-\",BF382*AM382*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G382,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G382=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G382,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I382:AJ382,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H382)","v":0},null,null,null,null,null,{"$f":"IF(AK382=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G382,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW382),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU382),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G382=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G382,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL383=\"\",\"-\",BF383*AM383*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G383,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G383=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G383,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I383:AJ383,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H383)","v":0},null,null,null,null,null,{"$f":"IF(AK383=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G383,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW383),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU383),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G383=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G383,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL384=\"\",\"-\",BF384*AM384*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G384,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G384=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G384,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I384:AJ384,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H384)","v":0},null,null,null,null,null,{"$f":"IF(AK384=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G384,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW384),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU384),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G384=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G384,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL385=\"\",\"-\",BF385*AM385*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G385,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G385=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G385,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I385:AJ385,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H385)","v":0},null,null,null,null,null,{"$f":"IF(AK385=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G385,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW385),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU385),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G385=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G385,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL386=\"\",\"-\",BF386*AM386*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G386,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G386=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G386,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I386:AJ386,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H386)","v":0},null,null,null,null,null,{"$f":"IF(AK386=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G386,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW386),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU386),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G386=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G386,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL387=\"\",\"-\",BF387*AM387*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G387,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G387=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G387,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I387:AJ387,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H387)","v":0},null,null,null,null,null,{"$f":"IF(AK387=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G387,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW387),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU387),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G387=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G387,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL388=\"\",\"-\",BF388*AM388*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G388,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G388=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G388,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I388:AJ388,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H388)","v":0},null,null,null,null,null,{"$f":"IF(AK388=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G388,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW388),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU388),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G388=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G388,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL389=\"\",\"-\",BF389*AM389*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G389,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G389=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G389,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I389:AJ389,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H389)","v":0},null,null,null,null,null,{"$f":"IF(AK389=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G389,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW389),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU389),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G389=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G389,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL390=\"\",\"-\",BF390*AM390*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G390,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G390=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G390,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I390:AJ390,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H390)","v":0},null,null,null,null,null,{"$f":"IF(AK390=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G390,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW390),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU390),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G390=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G390,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL391=\"\",\"-\",BF391*AM391*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G391,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G391=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G391,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I391:AJ391,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H391)","v":0},null,null,null,null,null,{"$f":"IF(AK391=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G391,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW391),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU391),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G391=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G391,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL392=\"\",\"-\",BF392*AM392*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G392,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G392=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G392,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I392:AJ392,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H392)","v":0},null,null,null,null,null,{"$f":"IF(AK392=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G392,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW392),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU392),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G392=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G392,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL393=\"\",\"-\",BF393*AM393*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G393,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G393=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G393,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I393:AJ393,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H393)","v":0},null,null,null,null,null,{"$f":"IF(AK393=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G393,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW393),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU393),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G393=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G393,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL394=\"\",\"-\",BF394*AM394*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G394,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G394=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G394,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I394:AJ394,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H394)","v":0},null,null,null,null,null,{"$f":"IF(AK394=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G394,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW394),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU394),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G394=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G394,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL395=\"\",\"-\",BF395*AM395*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G395,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G395=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G395,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I395:AJ395,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H395)","v":0},null,null,null,null,null,{"$f":"IF(AK395=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G395,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW395),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU395),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G395=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G395,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL396=\"\",\"-\",BF396*AM396*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G396,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G396=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G396,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I396:AJ396,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H396)","v":0},null,null,null,null,null,{"$f":"IF(AK396=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G396,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW396),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU396),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G396=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G396,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL397=\"\",\"-\",BF397*AM397*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G397,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G397=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G397,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I397:AJ397,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H397)","v":0},null,null,null,null,null,{"$f":"IF(AK397=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G397,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW397),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU397),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G397=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G397,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL398=\"\",\"-\",BF398*AM398*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G398,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G398=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G398,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I398:AJ398,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H398)","v":0},null,null,null,null,null,{"$f":"IF(AK398=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G398,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW398),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU398),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G398=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G398,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL399=\"\",\"-\",BF399*AM399*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G399,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G399=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G399,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I399:AJ399,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H399)","v":0},null,null,null,null,null,{"$f":"IF(AK399=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G399,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW399),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU399),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G399=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G399,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL400=\"\",\"-\",BF400*AM400*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G400,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G400=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G400,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I400:AJ400,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H400)","v":0},null,null,null,null,null,{"$f":"IF(AK400=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G400,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW400),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU400),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G400=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G400,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL401=\"\",\"-\",BF401*AM401*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G401,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G401=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G401,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I401:AJ401,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H401)","v":0},null,null,null,null,null,{"$f":"IF(AK401=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G401,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW401),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU401),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G401=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G401,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL402=\"\",\"-\",BF402*AM402*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G402,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G402=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G402,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I402:AJ402,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H402)","v":0},null,null,null,null,null,{"$f":"IF(AK402=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G402,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW402),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU402),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G402=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G402,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL403=\"\",\"-\",BF403*AM403*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G403,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G403=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G403,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I403:AJ403,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H403)","v":0},null,null,null,null,null,{"$f":"IF(AK403=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G403,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW403),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU403),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G403=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G403,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL404=\"\",\"-\",BF404*AM404*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G404,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G404=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G404,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I404:AJ404,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H404)","v":0},null,null,null,null,null,{"$f":"IF(AK404=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G404,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW404),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU404),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G404=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G404,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL405=\"\",\"-\",BF405*AM405*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G405,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G405=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G405,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I405:AJ405,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H405)","v":0},null,null,null,null,null,{"$f":"IF(AK405=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G405,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW405),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU405),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G405=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G405,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL406=\"\",\"-\",BF406*AM406*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G406,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G406=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G406,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I406:AJ406,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H406)","v":0},null,null,null,null,null,{"$f":"IF(AK406=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G406,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW406),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU406),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G406=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G406,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL407=\"\",\"-\",BF407*AM407*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G407,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G407=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G407,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I407:AJ407,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H407)","v":0},null,null,null,null,null,{"$f":"IF(AK407=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G407,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW407),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU407),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G407=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G407,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL408=\"\",\"-\",BF408*AM408*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G408,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G408=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G408,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I408:AJ408,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H408)","v":0},null,null,null,null,null,{"$f":"IF(AK408=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G408,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW408),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU408),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G408=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G408,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL409=\"\",\"-\",BF409*AM409*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G409,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G409=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G409,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I409:AJ409,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H409)","v":0},null,null,null,null,null,{"$f":"IF(AK409=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G409,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW409),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU409),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G409=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G409,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL410=\"\",\"-\",BF410*AM410*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G410,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G410=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G410,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I410:AJ410,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H410)","v":0},null,null,null,null,null,{"$f":"IF(AK410=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G410,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW410),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU410),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G410=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G410,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL411=\"\",\"-\",BF411*AM411*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G411,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G411=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G411,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I411:AJ411,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H411)","v":0},null,null,null,null,null,{"$f":"IF(AK411=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G411,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW411),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU411),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G411=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G411,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL412=\"\",\"-\",BF412*AM412*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G412,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G412=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G412,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I412:AJ412,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H412)","v":0},null,null,null,null,null,{"$f":"IF(AK412=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G412,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW412),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU412),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G412=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G412,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,{"$f":"IF(ISBLANK(D413)=FALSE,1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL413=\"\",\"-\",BF413*AM413*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G413,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,{"$f":"IF(AU413=\"\",\"-\",IF(H413=\"\",0,AU413*H413))","v":"-"},0,{"$f":"IF(ISBLANK(H413)=FALSE,AQ413/H413,\"-\")","v":"-"},{"$f":"IF(G413=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G413,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-",{"$f":"IF(ISBLANK(H413)=FALSE,(AQ413-IF(ISNUMBER(AN413)=TRUE,AN413,0)*AK413)/H413,\"-\")","v":"-"},{"$f":"IFERROR(AQ413-AK413*IF(ISNUMBER(AN413)=TRUE,AN413,0),\"\")","v":0},{"$f":"MIN(SUMPRODUCT(I413:AJ413,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H413)","v":0},null,null,null,null,null,{"$f":"IF(AK413=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G413,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},{"$f":"IF(AL413=\"\",\"-\",IF(AL413=\"Other\",1,1.25))","v":"-"},{"$f":"IF(BF413=\"-\",\"-\",BF413*AN413)","v":"-"},{"$f":"IF(LEFT(CELLformula(AW413),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU413),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G413=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G413,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AL414=\"Manual-On Individual Workstation\",AL414=\"Partial-Auto-On Individual Workstation\",AL414=\"Other Individual Workstation\"),1.3,1)","v":1},{"$f":"IF(AL414=\"\",\"-\",BF414*AM414*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G414,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,{"$f":"SUMPRODUCT(I414:AJ414,$I$23:$AJ$23)+IF(H414>0,MIN(IF(ISBLANK(AP414)=TRUE,0,AP414),H414)*BJ414/H414,0)","v":0},"-",{"$f":"SUMPRODUCT(I414:AJ414,$I$24:$AJ$24)","v":0},"-",{"$f":"IF(G414=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G414,'Lighting Assumptions'!$H$3:$H$112))","v":""},{"$f":"IF(ISBLANK(H414)=FALSE,AS414/H414,\"-\")","v":"-"},"-",0,{"$f":"MIN(SUMPRODUCT(I414:AJ414,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H414)","v":0},null,null,null,null,null,{"$f":"IF(AK414=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G414,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW414),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU414),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(BK414=\"\",\"-\",IF(H414=\"\",0,BK414*H414))","v":"-"},{"$f":"IF(G414=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G414,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL415=\"\",\"-\",BF415*AM415*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G415,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G415=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G415,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I415:AJ415,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H415)","v":0},null,null,null,null,null,{"$f":"IF(AK415=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G415,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW415),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU415),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G415=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G415,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL416=\"\",\"-\",BF416*AM416*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G416,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G416=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G416,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I416:AJ416,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H416)","v":0},null,null,null,null,null,{"$f":"IF(AK416=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G416,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW416),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU416),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G416=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G416,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL417=\"\",\"-\",BF417*AM417*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G417,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G417=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G417,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I417:AJ417,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H417)","v":0},null,null,null,null,null,{"$f":"IF(AK417=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G417,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW417),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU417),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G417=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G417,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL418=\"\",\"-\",BF418*AM418*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G418,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G418=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G418,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I418:AJ418,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H418)","v":0},null,null,null,null,null,{"$f":"IF(AK418=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G418,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW418),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU418),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G418=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G418,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL419=\"\",\"-\",BF419*AM419*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G419,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G419=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G419,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I419:AJ419,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H419)","v":0},null,null,null,null,null,{"$f":"IF(AK419=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G419,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW419),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU419),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G419=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G419,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL420=\"\",\"-\",BF420*AM420*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G420,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G420=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G420,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I420:AJ420,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H420)","v":0},null,null,null,null,null,{"$f":"IF(AK420=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G420,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW420),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU420),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G420=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G420,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL421=\"\",\"-\",BF421*AM421*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G421,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G421=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G421,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I421:AJ421,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H421)","v":0},null,null,null,null,null,{"$f":"IF(AK421=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G421,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW421),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU421),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G421=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G421,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL422=\"\",\"-\",BF422*AM422*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G422,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G422=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G422,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I422:AJ422,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H422)","v":0},null,null,null,null,null,{"$f":"IF(AK422=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G422,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW422),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU422),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G422=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G422,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL423=\"\",\"-\",BF423*AM423*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G423,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G423=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G423,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I423:AJ423,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H423)","v":0},null,null,null,null,null,{"$f":"IF(AK423=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G423,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW423),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU423),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G423=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G423,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL424=\"\",\"-\",BF424*AM424*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G424,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G424=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G424,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I424:AJ424,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H424)","v":0},null,null,null,null,null,{"$f":"IF(AK424=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G424,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW424),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU424),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G424=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G424,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL425=\"\",\"-\",BF425*AM425*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G425,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G425=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G425,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I425:AJ425,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H425)","v":0},null,null,null,null,null,{"$f":"IF(AK425=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G425,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW425),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU425),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G425=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G425,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL426=\"\",\"-\",BF426*AM426*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G426,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G426=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G426,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I426:AJ426,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H426)","v":0},null,null,null,null,null,{"$f":"IF(AK426=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G426,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW426),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU426),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G426=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G426,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL427=\"\",\"-\",BF427*AM427*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G427,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G427=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G427,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I427:AJ427,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H427)","v":0},null,null,null,null,null,{"$f":"IF(AK427=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G427,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW427),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU427),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G427=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G427,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL428=\"\",\"-\",BF428*AM428*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G428,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G428=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G428,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I428:AJ428,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H428)","v":0},null,null,null,null,null,{"$f":"IF(AK428=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G428,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW428),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU428),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G428=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G428,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL429=\"\",\"-\",BF429*AM429*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G429,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G429=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G429,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I429:AJ429,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H429)","v":0},null,null,null,null,null,{"$f":"IF(AK429=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G429,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW429),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU429),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G429=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G429,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL430=\"\",\"-\",BF430*AM430*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G430,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G430=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G430,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I430:AJ430,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H430)","v":0},null,null,null,null,null,{"$f":"IF(AK430=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G430,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW430),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU430),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G430=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G430,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL431=\"\",\"-\",BF431*AM431*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G431,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G431=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G431,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I431:AJ431,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H431)","v":0},null,null,null,null,null,{"$f":"IF(AK431=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G431,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW431),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU431),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G431=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G431,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL432=\"\",\"-\",BF432*AM432*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G432,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G432=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G432,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I432:AJ432,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H432)","v":0},null,null,null,null,null,{"$f":"IF(AK432=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G432,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW432),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU432),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G432=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G432,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL433=\"\",\"-\",BF433*AM433*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G433,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G433=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G433,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I433:AJ433,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H433)","v":0},null,null,null,null,null,{"$f":"IF(AK433=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G433,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW433),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU433),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G433=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G433,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL434=\"\",\"-\",BF434*AM434*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G434,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G434=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G434,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I434:AJ434,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H434)","v":0},null,null,null,null,null,{"$f":"IF(AK434=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G434,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW434),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU434),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G434=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G434,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL435=\"\",\"-\",BF435*AM435*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G435,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G435=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G435,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I435:AJ435,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H435)","v":0},null,null,null,null,null,{"$f":"IF(AK435=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G435,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW435),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU435),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G435=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G435,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL436=\"\",\"-\",BF436*AM436*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G436,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G436=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G436,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I436:AJ436,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H436)","v":0},null,null,null,null,null,{"$f":"IF(AK436=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G436,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW436),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU436),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G436=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G436,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL437=\"\",\"-\",BF437*AM437*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G437,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G437=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G437,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I437:AJ437,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H437)","v":0},null,null,null,null,null,{"$f":"IF(AK437=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G437,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW437),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU437),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G437=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G437,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL438=\"\",\"-\",BF438*AM438*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G438,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G438=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G438,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I438:AJ438,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H438)","v":0},null,null,null,null,null,{"$f":"IF(AK438=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G438,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW438),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU438),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G438=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G438,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL439=\"\",\"-\",BF439*AM439*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G439,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G439=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G439,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I439:AJ439,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H439)","v":0},null,null,null,null,null,{"$f":"IF(AK439=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G439,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW439),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU439),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G439=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G439,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL440=\"\",\"-\",BF440*AM440*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G440,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G440=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G440,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I440:AJ440,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H440)","v":0},null,null,null,null,null,{"$f":"IF(AK440=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G440,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW440),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU440),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G440=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G440,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL441=\"\",\"-\",BF441*AM441*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G441,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G441=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G441,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I441:AJ441,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H441)","v":0},null,null,null,null,null,{"$f":"IF(AK441=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G441,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW441),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU441),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G441=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G441,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL442=\"\",\"-\",BF442*AM442*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G442,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G442=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G442,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I442:AJ442,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H442)","v":0},null,null,null,null,null,{"$f":"IF(AK442=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G442,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW442),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU442),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G442=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G442,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL443=\"\",\"-\",BF443*AM443*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G443,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G443=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G443,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I443:AJ443,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H443)","v":0},null,null,null,null,null,{"$f":"IF(AK443=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G443,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW443),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU443),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G443=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G443,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL444=\"\",\"-\",BF444*AM444*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G444,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G444=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G444,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I444:AJ444,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H444)","v":0},null,null,null,null,null,{"$f":"IF(AK444=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G444,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW444),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU444),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G444=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G444,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL445=\"\",\"-\",BF445*AM445*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G445,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G445=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G445,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I445:AJ445,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H445)","v":0},null,null,null,null,null,{"$f":"IF(AK445=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G445,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW445),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU445),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G445=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G445,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL446=\"\",\"-\",BF446*AM446*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G446,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G446=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G446,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I446:AJ446,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H446)","v":0},null,null,null,null,null,{"$f":"IF(AK446=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G446,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW446),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU446),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G446=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G446,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL447=\"\",\"-\",BF447*AM447*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G447,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G447=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G447,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I447:AJ447,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H447)","v":0},null,null,null,null,null,{"$f":"IF(AK447=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G447,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW447),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU447),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G447=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G447,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL448=\"\",\"-\",BF448*AM448*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G448,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G448=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G448,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I448:AJ448,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H448)","v":0},null,null,null,null,null,{"$f":"IF(AK448=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G448,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW448),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU448),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G448=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G448,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL449=\"\",\"-\",BF449*AM449*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G449,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G449=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G449,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I449:AJ449,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H449)","v":0},null,null,null,null,null,{"$f":"IF(AK449=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G449,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW449),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU449),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G449=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G449,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL450=\"\",\"-\",BF450*AM450*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G450,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G450=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G450,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I450:AJ450,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H450)","v":0},null,null,null,null,null,{"$f":"IF(AK450=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G450,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW450),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU450),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G450=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G450,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL451=\"\",\"-\",BF451*AM451*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G451,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G451=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G451,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I451:AJ451,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H451)","v":0},null,null,null,null,null,{"$f":"IF(AK451=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G451,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW451),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU451),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G451=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G451,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL452=\"\",\"-\",BF452*AM452*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G452,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G452=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G452,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I452:AJ452,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H452)","v":0},null,null,null,null,null,{"$f":"IF(AK452=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G452,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW452),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU452),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G452=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G452,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL453=\"\",\"-\",BF453*AM453*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G453,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G453=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G453,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I453:AJ453,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H453)","v":0},null,null,null,null,null,{"$f":"IF(AK453=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G453,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW453),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU453),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G453=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G453,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL454=\"\",\"-\",BF454*AM454*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G454,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G454=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G454,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I454:AJ454,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H454)","v":0},null,null,null,null,null,{"$f":"IF(AK454=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G454,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW454),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU454),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G454=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G454,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL455=\"\",\"-\",BF455*AM455*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G455,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G455=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G455,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I455:AJ455,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H455)","v":0},null,null,null,null,null,{"$f":"IF(AK455=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G455,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW455),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU455),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G455=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G455,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL456=\"\",\"-\",BF456*AM456*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G456,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G456=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G456,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I456:AJ456,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H456)","v":0},null,null,null,null,null,{"$f":"IF(AK456=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G456,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW456),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU456),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G456=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G456,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL457=\"\",\"-\",BF457*AM457*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G457,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G457=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G457,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I457:AJ457,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H457)","v":0},null,null,null,null,null,{"$f":"IF(AK457=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G457,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW457),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU457),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G457=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G457,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL458=\"\",\"-\",BF458*AM458*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G458,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G458=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G458,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I458:AJ458,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H458)","v":0},null,null,null,null,null,{"$f":"IF(AK458=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G458,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW458),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU458),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G458=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G458,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL459=\"\",\"-\",BF459*AM459*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G459,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G459=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G459,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I459:AJ459,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H459)","v":0},null,null,null,null,null,{"$f":"IF(AK459=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G459,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW459),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU459),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G459=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G459,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL460=\"\",\"-\",BF460*AM460*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G460,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G460=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G460,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I460:AJ460,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H460)","v":0},null,null,null,null,null,{"$f":"IF(AK460=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G460,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW460),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU460),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G460=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G460,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL461=\"\",\"-\",BF461*AM461*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G461,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G461=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G461,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I461:AJ461,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H461)","v":0},null,null,null,null,null,{"$f":"IF(AK461=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G461,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW461),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU461),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G461=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G461,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL462=\"\",\"-\",BF462*AM462*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G462,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G462=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G462,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I462:AJ462,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H462)","v":0},null,null,null,null,null,{"$f":"IF(AK462=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G462,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW462),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU462),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G462=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G462,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL463=\"\",\"-\",BF463*AM463*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G463,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G463=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G463,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I463:AJ463,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H463)","v":0},null,null,null,null,null,{"$f":"IF(AK463=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G463,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW463),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU463),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G463=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G463,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL464=\"\",\"-\",BF464*AM464*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G464,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G464=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G464,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I464:AJ464,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H464)","v":0},null,null,null,null,null,{"$f":"IF(AK464=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G464,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW464),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU464),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G464=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G464,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL465=\"\",\"-\",BF465*AM465*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G465,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G465=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G465,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I465:AJ465,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H465)","v":0},null,null,null,null,null,{"$f":"IF(AK465=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G465,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW465),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU465),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G465=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G465,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL466=\"\",\"-\",BF466*AM466*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G466,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G466=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G466,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I466:AJ466,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H466)","v":0},null,null,null,null,null,{"$f":"IF(AK466=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G466,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW466),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU466),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G466=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G466,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL467=\"\",\"-\",BF467*AM467*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G467,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G467=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G467,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I467:AJ467,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H467)","v":0},null,null,null,null,null,{"$f":"IF(AK467=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G467,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW467),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU467),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G467=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G467,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL468=\"\",\"-\",BF468*AM468*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G468,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G468=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G468,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I468:AJ468,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H468)","v":0},null,null,null,null,null,{"$f":"IF(AK468=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G468,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW468),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU468),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G468=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G468,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL469=\"\",\"-\",BF469*AM469*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G469,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G469=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G469,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I469:AJ469,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H469)","v":0},null,null,null,null,null,{"$f":"IF(AK469=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G469,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW469),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU469),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G469=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G469,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL470=\"\",\"-\",BF470*AM470*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G470,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G470=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G470,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I470:AJ470,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H470)","v":0},null,null,null,null,null,{"$f":"IF(AK470=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G470,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW470),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU470),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G470=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G470,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL471=\"\",\"-\",BF471*AM471*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G471,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G471=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G471,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I471:AJ471,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H471)","v":0},null,null,null,null,null,{"$f":"IF(AK471=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G471,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW471),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU471),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G471=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G471,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL472=\"\",\"-\",BF472*AM472*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G472,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G472=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G472,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I472:AJ472,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H472)","v":0},null,null,null,null,null,{"$f":"IF(AK472=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G472,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW472),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU472),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G472=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G472,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL473=\"\",\"-\",BF473*AM473*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G473,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G473=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G473,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I473:AJ473,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H473)","v":0},null,null,null,null,null,{"$f":"IF(AK473=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G473,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW473),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU473),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G473=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G473,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL474=\"\",\"-\",BF474*AM474*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G474,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G474=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G474,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I474:AJ474,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H474)","v":0},null,null,null,null,null,{"$f":"IF(AK474=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G474,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW474),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU474),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G474=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G474,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL475=\"\",\"-\",BF475*AM475*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G475,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G475=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G475,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I475:AJ475,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H475)","v":0},null,null,null,null,null,{"$f":"IF(AK475=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G475,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW475),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU475),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G475=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G475,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL476=\"\",\"-\",BF476*AM476*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G476,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G476=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G476,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I476:AJ476,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H476)","v":0},null,null,null,null,null,{"$f":"IF(AK476=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G476,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW476),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU476),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G476=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G476,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,{"$f":"IF(ISBLANK(D477)=FALSE,1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL477=\"\",\"-\",BF477*AM477*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G477,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,{"$f":"IF(AU477=\"\",\"-\",IF(H477=\"\",0,AU477*H477))","v":"-"},0,{"$f":"IF(ISBLANK(H477)=FALSE,AQ477/H477,\"-\")","v":"-"},{"$f":"IF(G477=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G477,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-",{"$f":"IF(ISBLANK(H477)=FALSE,(AQ477-IF(ISNUMBER(AN477)=TRUE,AN477,0)*AK477)/H477,\"-\")","v":"-"},{"$f":"IFERROR(AQ477-AK477*IF(ISNUMBER(AN477)=TRUE,AN477,0),\"\")","v":0},{"$f":"MIN(SUMPRODUCT(I477:AJ477,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H477)","v":0},null,null,null,null,null,{"$f":"IF(AK477=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G477,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},{"$f":"IF(AL477=\"\",\"-\",IF(AL477=\"Other\",1,1.25))","v":"-"},{"$f":"IF(BF477=\"-\",\"-\",BF477*AN477)","v":"-"},{"$f":"IF(LEFT(CELLformula(AW477),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU477),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G477=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G477,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AL478=\"Manual-On Individual Workstation\",AL478=\"Partial-Auto-On Individual Workstation\",AL478=\"Other Individual Workstation\"),1.3,1)","v":1},{"$f":"IF(AL478=\"\",\"-\",BF478*AM478*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G478,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,{"$f":"SUMPRODUCT(I478:AJ478,$I$23:$AJ$23)+IF(H478>0,MIN(IF(ISBLANK(AP478)=TRUE,0,AP478),H478)*BJ478/H478,0)","v":0},"-",{"$f":"SUMPRODUCT(I478:AJ478,$I$24:$AJ$24)","v":0},"-",{"$f":"IF(G478=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G478,'Lighting Assumptions'!$H$3:$H$112))","v":""},{"$f":"IF(ISBLANK(H478)=FALSE,AS478/H478,\"-\")","v":"-"},"-",0,{"$f":"MIN(SUMPRODUCT(I478:AJ478,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H478)","v":0},null,null,null,null,null,{"$f":"IF(AK478=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G478,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW478),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU478),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(BK478=\"\",\"-\",IF(H478=\"\",0,BK478*H478))","v":"-"},{"$f":"IF(G478=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G478,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL479=\"\",\"-\",BF479*AM479*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G479,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G479=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G479,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I479:AJ479,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H479)","v":0},null,null,null,null,null,{"$f":"IF(AK479=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G479,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW479),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU479),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G479=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G479,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL480=\"\",\"-\",BF480*AM480*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G480,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G480=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G480,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I480:AJ480,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H480)","v":0},null,null,null,null,null,{"$f":"IF(AK480=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G480,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW480),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU480),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G480=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G480,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL481=\"\",\"-\",BF481*AM481*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G481,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G481=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G481,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I481:AJ481,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H481)","v":0},null,null,null,null,null,{"$f":"IF(AK481=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G481,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW481),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU481),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G481=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G481,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL482=\"\",\"-\",BF482*AM482*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G482,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G482=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G482,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I482:AJ482,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H482)","v":0},null,null,null,null,null,{"$f":"IF(AK482=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G482,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW482),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU482),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G482=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G482,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL483=\"\",\"-\",BF483*AM483*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G483,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G483=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G483,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I483:AJ483,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H483)","v":0},null,null,null,null,null,{"$f":"IF(AK483=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G483,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW483),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU483),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G483=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G483,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL484=\"\",\"-\",BF484*AM484*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G484,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G484=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G484,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I484:AJ484,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H484)","v":0},null,null,null,null,null,{"$f":"IF(AK484=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G484,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW484),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU484),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G484=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G484,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL485=\"\",\"-\",BF485*AM485*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G485,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G485=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G485,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I485:AJ485,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H485)","v":0},null,null,null,null,null,{"$f":"IF(AK485=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G485,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW485),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU485),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G485=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G485,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL486=\"\",\"-\",BF486*AM486*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G486,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G486=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G486,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I486:AJ486,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H486)","v":0},null,null,null,null,null,{"$f":"IF(AK486=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G486,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW486),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU486),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G486=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G486,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL487=\"\",\"-\",BF487*AM487*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G487,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G487=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G487,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I487:AJ487,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H487)","v":0},null,null,null,null,null,{"$f":"IF(AK487=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G487,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW487),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU487),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G487=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G487,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL488=\"\",\"-\",BF488*AM488*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G488,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G488=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G488,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I488:AJ488,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H488)","v":0},null,null,null,null,null,{"$f":"IF(AK488=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G488,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW488),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU488),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G488=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G488,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL489=\"\",\"-\",BF489*AM489*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G489,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G489=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G489,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I489:AJ489,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H489)","v":0},null,null,null,null,null,{"$f":"IF(AK489=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G489,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW489),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU489),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G489=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G489,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL490=\"\",\"-\",BF490*AM490*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G490,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G490=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G490,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I490:AJ490,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H490)","v":0},null,null,null,null,null,{"$f":"IF(AK490=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G490,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW490),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU490),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G490=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G490,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL491=\"\",\"-\",BF491*AM491*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G491,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G491=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G491,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I491:AJ491,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H491)","v":0},null,null,null,null,null,{"$f":"IF(AK491=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G491,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW491),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU491),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G491=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G491,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL492=\"\",\"-\",BF492*AM492*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G492,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G492=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G492,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I492:AJ492,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H492)","v":0},null,null,null,null,null,{"$f":"IF(AK492=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G492,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW492),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU492),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G492=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G492,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL493=\"\",\"-\",BF493*AM493*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G493,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G493=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G493,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I493:AJ493,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H493)","v":0},null,null,null,null,null,{"$f":"IF(AK493=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G493,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW493),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU493),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G493=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G493,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL494=\"\",\"-\",BF494*AM494*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G494,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G494=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G494,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I494:AJ494,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H494)","v":0},null,null,null,null,null,{"$f":"IF(AK494=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G494,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW494),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU494),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G494=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G494,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL495=\"\",\"-\",BF495*AM495*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G495,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G495=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G495,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I495:AJ495,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H495)","v":0},null,null,null,null,null,{"$f":"IF(AK495=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G495,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW495),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU495),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G495=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G495,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL496=\"\",\"-\",BF496*AM496*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G496,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G496=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G496,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I496:AJ496,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H496)","v":0},null,null,null,null,null,{"$f":"IF(AK496=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G496,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW496),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU496),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G496=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G496,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL497=\"\",\"-\",BF497*AM497*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G497,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G497=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G497,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I497:AJ497,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H497)","v":0},null,null,null,null,null,{"$f":"IF(AK497=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G497,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW497),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU497),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G497=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G497,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL498=\"\",\"-\",BF498*AM498*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G498,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G498=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G498,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I498:AJ498,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H498)","v":0},null,null,null,null,null,{"$f":"IF(AK498=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G498,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW498),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU498),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G498=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G498,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL499=\"\",\"-\",BF499*AM499*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G499,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G499=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G499,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I499:AJ499,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H499)","v":0},null,null,null,null,null,{"$f":"IF(AK499=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G499,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW499),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU499),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G499=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G499,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL500=\"\",\"-\",BF500*AM500*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G500,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G500=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G500,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I500:AJ500,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H500)","v":0},null,null,null,null,null,{"$f":"IF(AK500=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G500,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW500),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU500),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G500=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G500,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL501=\"\",\"-\",BF501*AM501*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G501,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G501=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G501,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I501:AJ501,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H501)","v":0},null,null,null,null,null,{"$f":"IF(AK501=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G501,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW501),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU501),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G501=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G501,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL502=\"\",\"-\",BF502*AM502*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G502,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G502=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G502,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I502:AJ502,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H502)","v":0},null,null,null,null,null,{"$f":"IF(AK502=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G502,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW502),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU502),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G502=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G502,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL503=\"\",\"-\",BF503*AM503*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G503,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G503=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G503,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I503:AJ503,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H503)","v":0},null,null,null,null,null,{"$f":"IF(AK503=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G503,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW503),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU503),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G503=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G503,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL504=\"\",\"-\",BF504*AM504*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G504,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G504=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G504,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I504:AJ504,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H504)","v":0},null,null,null,null,null,{"$f":"IF(AK504=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G504,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW504),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU504),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G504=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G504,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL505=\"\",\"-\",BF505*AM505*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G505,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G505=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G505,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I505:AJ505,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H505)","v":0},null,null,null,null,null,{"$f":"IF(AK505=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G505,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW505),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU505),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G505=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G505,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL506=\"\",\"-\",BF506*AM506*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G506,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G506=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G506,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I506:AJ506,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H506)","v":0},null,null,null,null,null,{"$f":"IF(AK506=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G506,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW506),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU506),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G506=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G506,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL507=\"\",\"-\",BF507*AM507*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G507,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G507=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G507,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I507:AJ507,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H507)","v":0},null,null,null,null,null,{"$f":"IF(AK507=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G507,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW507),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU507),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G507=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G507,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL508=\"\",\"-\",BF508*AM508*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G508,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G508=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G508,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I508:AJ508,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H508)","v":0},null,null,null,null,null,{"$f":"IF(AK508=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G508,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW508),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU508),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G508=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G508,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL509=\"\",\"-\",BF509*AM509*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G509,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G509=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G509,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I509:AJ509,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H509)","v":0},null,null,null,null,null,{"$f":"IF(AK509=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G509,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW509),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU509),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G509=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G509,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL510=\"\",\"-\",BF510*AM510*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G510,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G510=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G510,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I510:AJ510,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H510)","v":0},null,null,null,null,null,{"$f":"IF(AK510=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G510,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW510),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU510),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G510=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G510,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL511=\"\",\"-\",BF511*AM511*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G511,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G511=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G511,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I511:AJ511,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H511)","v":0},null,null,null,null,null,{"$f":"IF(AK511=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G511,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW511),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU511),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G511=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G511,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL512=\"\",\"-\",BF512*AM512*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G512,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G512=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G512,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I512:AJ512,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H512)","v":0},null,null,null,null,null,{"$f":"IF(AK512=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G512,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW512),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU512),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G512=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G512,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL513=\"\",\"-\",BF513*AM513*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G513,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G513=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G513,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I513:AJ513,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H513)","v":0},null,null,null,null,null,{"$f":"IF(AK513=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G513,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW513),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU513),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G513=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G513,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL514=\"\",\"-\",BF514*AM514*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G514,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G514=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G514,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I514:AJ514,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H514)","v":0},null,null,null,null,null,{"$f":"IF(AK514=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G514,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW514),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU514),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G514=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G514,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL515=\"\",\"-\",BF515*AM515*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G515,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G515=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G515,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I515:AJ515,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H515)","v":0},null,null,null,null,null,{"$f":"IF(AK515=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G515,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW515),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU515),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G515=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G515,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL516=\"\",\"-\",BF516*AM516*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G516,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G516=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G516,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I516:AJ516,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H516)","v":0},null,null,null,null,null,{"$f":"IF(AK516=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G516,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW516),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU516),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G516=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G516,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL517=\"\",\"-\",BF517*AM517*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G517,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G517=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G517,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I517:AJ517,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H517)","v":0},null,null,null,null,null,{"$f":"IF(AK517=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G517,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW517),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU517),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G517=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G517,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL518=\"\",\"-\",BF518*AM518*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G518,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G518=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G518,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I518:AJ518,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H518)","v":0},null,null,null,null,null,{"$f":"IF(AK518=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G518,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW518),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU518),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G518=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G518,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL519=\"\",\"-\",BF519*AM519*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G519,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G519=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G519,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I519:AJ519,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H519)","v":0},null,null,null,null,null,{"$f":"IF(AK519=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G519,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW519),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU519),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G519=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G519,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL520=\"\",\"-\",BF520*AM520*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G520,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G520=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G520,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I520:AJ520,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H520)","v":0},null,null,null,null,null,{"$f":"IF(AK520=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G520,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW520),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU520),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G520=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G520,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL521=\"\",\"-\",BF521*AM521*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G521,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G521=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G521,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I521:AJ521,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H521)","v":0},null,null,null,null,null,{"$f":"IF(AK521=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G521,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW521),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU521),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G521=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G521,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL522=\"\",\"-\",BF522*AM522*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G522,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G522=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G522,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I522:AJ522,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H522)","v":0},null,null,null,null,null,{"$f":"IF(AK522=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G522,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW522),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU522),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G522=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G522,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL523=\"\",\"-\",BF523*AM523*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G523,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G523=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G523,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I523:AJ523,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H523)","v":0},null,null,null,null,null,{"$f":"IF(AK523=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G523,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW523),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU523),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G523=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G523,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL524=\"\",\"-\",BF524*AM524*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G524,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G524=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G524,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I524:AJ524,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H524)","v":0},null,null,null,null,null,{"$f":"IF(AK524=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G524,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW524),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU524),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G524=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G524,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL525=\"\",\"-\",BF525*AM525*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G525,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G525=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G525,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I525:AJ525,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H525)","v":0},null,null,null,null,null,{"$f":"IF(AK525=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G525,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW525),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU525),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G525=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G525,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL526=\"\",\"-\",BF526*AM526*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G526,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G526=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G526,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I526:AJ526,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H526)","v":0},null,null,null,null,null,{"$f":"IF(AK526=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G526,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW526),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU526),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G526=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G526,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL527=\"\",\"-\",BF527*AM527*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G527,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G527=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G527,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I527:AJ527,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H527)","v":0},null,null,null,null,null,{"$f":"IF(AK527=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G527,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW527),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU527),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G527=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G527,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL528=\"\",\"-\",BF528*AM528*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G528,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G528=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G528,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I528:AJ528,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H528)","v":0},null,null,null,null,null,{"$f":"IF(AK528=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G528,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW528),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU528),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G528=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G528,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL529=\"\",\"-\",BF529*AM529*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G529,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G529=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G529,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I529:AJ529,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H529)","v":0},null,null,null,null,null,{"$f":"IF(AK529=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G529,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW529),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU529),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G529=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G529,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL530=\"\",\"-\",BF530*AM530*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G530,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G530=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G530,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I530:AJ530,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H530)","v":0},null,null,null,null,null,{"$f":"IF(AK530=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G530,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW530),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU530),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G530=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G530,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL531=\"\",\"-\",BF531*AM531*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G531,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G531=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G531,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I531:AJ531,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H531)","v":0},null,null,null,null,null,{"$f":"IF(AK531=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G531,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW531),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU531),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G531=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G531,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL532=\"\",\"-\",BF532*AM532*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G532,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G532=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G532,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I532:AJ532,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H532)","v":0},null,null,null,null,null,{"$f":"IF(AK532=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G532,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW532),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU532),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G532=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G532,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL533=\"\",\"-\",BF533*AM533*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G533,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G533=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G533,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I533:AJ533,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H533)","v":0},null,null,null,null,null,{"$f":"IF(AK533=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G533,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW533),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU533),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G533=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G533,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL534=\"\",\"-\",BF534*AM534*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G534,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G534=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G534,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I534:AJ534,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H534)","v":0},null,null,null,null,null,{"$f":"IF(AK534=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G534,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW534),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU534),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G534=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G534,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL535=\"\",\"-\",BF535*AM535*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G535,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G535=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G535,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I535:AJ535,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H535)","v":0},null,null,null,null,null,{"$f":"IF(AK535=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G535,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW535),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU535),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G535=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G535,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL536=\"\",\"-\",BF536*AM536*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G536,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G536=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G536,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I536:AJ536,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H536)","v":0},null,null,null,null,null,{"$f":"IF(AK536=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G536,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW536),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU536),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G536=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G536,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL537=\"\",\"-\",BF537*AM537*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G537,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G537=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G537,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I537:AJ537,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H537)","v":0},null,null,null,null,null,{"$f":"IF(AK537=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G537,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW537),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU537),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G537=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G537,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL538=\"\",\"-\",BF538*AM538*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G538,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G538=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G538,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I538:AJ538,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H538)","v":0},null,null,null,null,null,{"$f":"IF(AK538=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G538,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW538),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU538),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G538=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G538,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL539=\"\",\"-\",BF539*AM539*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G539,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G539=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G539,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I539:AJ539,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H539)","v":0},null,null,null,null,null,{"$f":"IF(AK539=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G539,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW539),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU539),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G539=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G539,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL540=\"\",\"-\",BF540*AM540*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G540,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G540=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G540,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I540:AJ540,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H540)","v":0},null,null,null,null,null,{"$f":"IF(AK540=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G540,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW540),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU540),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G540=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G540,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,{"$f":"IF(ISBLANK(D541)=FALSE,1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL541=\"\",\"-\",BF541*AM541*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G541,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,{"$f":"IF(AU541=\"\",\"-\",IF(H541=\"\",0,AU541*H541))","v":"-"},0,{"$f":"IF(ISBLANK(H541)=FALSE,AQ541/H541,\"-\")","v":"-"},{"$f":"IF(G541=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G541,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-",{"$f":"IF(ISBLANK(H541)=FALSE,(AQ541-IF(ISNUMBER(AN541)=TRUE,AN541,0)*AK541)/H541,\"-\")","v":"-"},{"$f":"IFERROR(AQ541-AK541*IF(ISNUMBER(AN541)=TRUE,AN541,0),\"\")","v":0},{"$f":"MIN(SUMPRODUCT(I541:AJ541,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H541)","v":0},null,null,null,null,null,{"$f":"IF(AK541=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G541,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},{"$f":"IF(AL541=\"\",\"-\",IF(AL541=\"Other\",1,1.25))","v":"-"},{"$f":"IF(BF541=\"-\",\"-\",BF541*AN541)","v":"-"},{"$f":"IF(LEFT(CELLformula(AW541),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU541),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G541=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G541,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AL542=\"Manual-On Individual Workstation\",AL542=\"Partial-Auto-On Individual Workstation\",AL542=\"Other Individual Workstation\"),1.3,1)","v":1},{"$f":"IF(AL542=\"\",\"-\",BF542*AM542*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G542,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,{"$f":"SUMPRODUCT(I542:AJ542,$I$23:$AJ$23)+IF(H542>0,MIN(IF(ISBLANK(AP542)=TRUE,0,AP542),H542)*BJ542/H542,0)","v":0},"-",{"$f":"SUMPRODUCT(I542:AJ542,$I$24:$AJ$24)","v":0},"-",{"$f":"IF(G542=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G542,'Lighting Assumptions'!$H$3:$H$112))","v":""},{"$f":"IF(ISBLANK(H542)=FALSE,AS542/H542,\"-\")","v":"-"},"-",0,{"$f":"MIN(SUMPRODUCT(I542:AJ542,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H542)","v":0},null,null,null,null,null,{"$f":"IF(AK542=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G542,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW542),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU542),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(BK542=\"\",\"-\",IF(H542=\"\",0,BK542*H542))","v":"-"},{"$f":"IF(G542=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G542,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL543=\"\",\"-\",BF543*AM543*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G543,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G543=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G543,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I543:AJ543,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H543)","v":0},null,null,null,null,null,{"$f":"IF(AK543=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G543,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW543),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU543),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G543=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G543,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL544=\"\",\"-\",BF544*AM544*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G544,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G544=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G544,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I544:AJ544,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H544)","v":0},null,null,null,null,null,{"$f":"IF(AK544=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G544,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW544),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU544),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G544=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G544,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL545=\"\",\"-\",BF545*AM545*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G545,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G545=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G545,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I545:AJ545,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H545)","v":0},null,null,null,null,null,{"$f":"IF(AK545=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G545,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW545),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU545),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G545=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G545,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL546=\"\",\"-\",BF546*AM546*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G546,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G546=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G546,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I546:AJ546,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H546)","v":0},null,null,null,null,null,{"$f":"IF(AK546=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G546,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW546),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU546),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G546=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G546,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL547=\"\",\"-\",BF547*AM547*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G547,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G547=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G547,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I547:AJ547,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H547)","v":0},null,null,null,null,null,{"$f":"IF(AK547=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G547,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW547),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU547),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G547=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G547,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL548=\"\",\"-\",BF548*AM548*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G548,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G548=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G548,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I548:AJ548,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H548)","v":0},null,null,null,null,null,{"$f":"IF(AK548=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G548,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW548),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU548),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G548=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G548,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL549=\"\",\"-\",BF549*AM549*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G549,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G549=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G549,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I549:AJ549,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H549)","v":0},null,null,null,null,null,{"$f":"IF(AK549=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G549,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW549),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU549),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G549=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G549,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL550=\"\",\"-\",BF550*AM550*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G550,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G550=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G550,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I550:AJ550,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H550)","v":0},null,null,null,null,null,{"$f":"IF(AK550=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G550,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW550),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU550),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G550=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G550,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]
[null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(AL551=\"\",\"-\",BF551*AM551*SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G551,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},null,null,0,"-",0,"-",{"$f":"IF(G551=\"\",\"\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G551,'Lighting Assumptions'!$H$3:$H$112))","v":""},"-","-",0,{"$f":"MIN(SUMPRODUCT(I551:AJ551,IF($I$25:$AJ$25=\"yes\",1,0),$I$23:$AJ$23),H551)","v":0},null,null,null,null,null,{"$f":"IF(AK551=\"\",\"-\",SUMIF('Lighting Assumptions'!$G$3:$G$112,'6a - Lighting Counts'!G551,'Lighting Assumptions'!$J$3:$J$112))","v":"-"},"-","-",{"$f":"IF(LEFT(CELLformula(AW551),3)<>\"=IF\",1,\"\")","v":""},{"$f":"IF(LEFT(CELLformula(AU551),3)<>\"=IF\",1,\"\")","v":""},"-",{"$f":"IF(G551=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!$G$3:$G$112,'6a - Lighting Counts'!G551,'Lighting Assumptions 90.1-2013'!$H$3:$H$112))","v":""}]

{"sheet":"6b - General Lighting","index":16,"n_rows":175,"n_cols":37,"rows_kept":175,"cut":false,"hidden":false,"merged":[[25,1,25,2],[26,1,26,2],[73,11,73,13],[114,6,114,10],[73,9,73,10],[80,8,81,16],[99,2,99,5],[77,6,77,8],[77,9,77,10],[77,11,77,13],[77,14,77,16],[89,8,89,16],[88,2,88,3],[91,1,91,14],[84,2,84,3],[85,8,85,16],[84,8,84,16],[90,8,90,16],[87,8,87,16],[87,2,87,3],[91,15,91,16],[89,2,89,3],[92,15,92,16],[105,1,105,5],[116,11,116,13],[116,14,116,16],[116,1,116,10],[107,11,107,13],[107,14,107,16],[107,6,107,8],[110,11,110,13],[120,15,120,16],[120,1,120,14],[110,1,111,1],[110,6,110,10],[113,6,113,10],[111,6,111,10],[113,2,113,5],[113,11,113,13],[115,6,115,10],[115,2,115,5],[113,14,113,16],[110,14,110,16],[107,9,107,10],[114,14,114,16],[111,2,111,5],[111,14,111,16],[100,2,100,5],[100,6,100,10],[100,11,100,16],[93,15,93,16],[93,1,93,14],[96,6,96,10],[96,11,96,16],[96,2,96,5],[97,2,97,5],[97,6,97,10],[97,11,97,16],[174,1,174,16],[171,9,171,11],[159,5,159,6],[160,5,160,6],[161,5,161,6],[158,1,158,4],[159,1,159,4],[158,5,158,6],[160,1,160,4],[161,1,161,4],[164,9,164,11],[158,12,158,16],[159,12,159,16],[160,12,160,16],[161,12,161,16],[162,12,162,16],[173,1,173,11],[164,1,164,8],[162,9,162,11],[163,9,163,11],[162,5,162,6],[163,5,163,6],[167,1,169,8],[167,12,169,17],[5,1,5,16],[22,1,22,16],[21,1,21,16],[7,15,7,16],[9,15,9,16],[11,15,11,16],[13,15,13,16],[17,15,17,16],[7,1,7,14],[9,1,9,14],[11,1,11,14],[13,1,13,14],[17,1,17,14],[15,1,15,14],[15,15,15,16],[19,1,19,14],[19,15,19,16],[73,6,73,8],[58,1,58,2],[59,1,59,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[56,1,56,2],[57,1,57,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[72,6,72,10],[72,11,72,16],[68,6,68,7],[44,1,44,2],[45,1,45,2],[48,1,48,2],[61,6,61,7],[62,6,62,7],[63,6,63,7],[64,6,64,7],[27,1,27,2],[28,1,28,2],[29,1,29,2],[33,1,33,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[34,1,34,2],[46,1,46,2],[47,1,47,2],[132,2,132,11],[134,2,134,11],[158,9,158,11],[163,1,163,4],[164,12,164,16],[155,5,156,7],[141,9,142,11],[141,8,142,8],[141,7,142,7],[162,1,162,4],[141,5,142,6],[147,1,147,4],[143,9,143,11],[163,12,163,16],[160,9,160,11],[161,9,161,11],[159,9,159,11],[148,9,148,11],[154,12,154,16],[148,12,148,16],[139,25,140,26],[155,26,155,27],[141,25,141,26],[142,25,142,26],[154,26,154,27],[155,23,155,24],[147,9,147,11],[147,12,147,16],[141,23,141,24],[146,12,146,16],[144,12,144,16],[145,12,145,16],[139,12,139,16],[144,9,144,11],[139,9,139,11],[146,9,146,11],[143,12,143,16],[141,19,142,19],[138,20,142,20],[138,19,139,19],[155,19,156,19],[76,2,76,5],[76,6,76,8],[154,5,154,6],[154,9,154,11],[153,19,154,19],[153,18,164,18],[138,1,138,7],[153,8,153,11],[145,1,145,4],[144,5,144,6],[143,5,143,6],[141,1,142,1],[141,2,142,4],[146,1,146,4],[105,11,105,13],[98,2,98,5],[98,11,98,16],[110,2,110,5],[107,1,107,5],[105,14,105,16],[86,8,86,16],[90,1,90,3],[99,6,99,10],[88,8,88,16],[139,5,139,6],[139,1,139,4],[73,14,73,16],[66,6,66,7],[72,2,73,5],[69,1,69,2],[72,1,73,1],[65,6,65,7],[82,5,82,6],[75,9,75,10],[75,2,75,5],[75,6,75,8],[82,8,82,16],[75,11,75,13],[82,2,82,3],[76,9,76,10],[76,11,76,13],[76,14,76,16],[80,5,80,6],[75,14,75,16],[80,1,81,1],[77,2,77,5],[80,2,81,3],[67,6,67,7],[171,1,171,8],[145,5,145,6],[171,12,171,17],[138,12,138,17],[153,12,153,17],[141,12,142,17],[155,12,156,17],[86,2,86,3],[85,2,85,3],[98,6,98,10],[105,6,105,8],[111,11,111,13],[155,2,156,4],[143,1,143,4],[122,1,122,14],[122,15,122,16],[124,1,124,14],[124,15,124,16],[154,1,154,4],[146,5,146,6],[147,5,147,6],[118,1,118,16],[130,1,130,14],[130,15,130,16],[24,7,24,9],[24,10,24,11],[168,19,169,19],[153,1,153,7],[148,1,148,8],[99,11,99,16],[92,1,92,14],[132,12,132,16],[134,12,134,16],[115,14,115,16],[138,8,138,11],[114,2,114,5],[114,11,114,13],[115,11,115,13],[155,1,156,1],[145,9,145,11],[144,1,144,4],[155,8,156,11],[126,1,126,14],[126,15,126,16],[128,1,128,14],[128,15,128,16],[167,18,171,18],[167,9,169,11]]}
["G"]
["G","General Lighting"]
["G"]
["G"]
["G","Interior Lighting"]
["G","Instructions: Confirm that the energy model complies with the Interior lighting requirements listed, and provide a narrative explaining any discrepancies. Completing the Lighting Counts tab will populate the Interior Lighting by Space Type table. Please refer to the column header notes for information about Appendix G modeling protocol. Enter \"N/A\" for any information not applicable to the project. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Interior Lighting Requirements"]
["G","The baseline lighting schedules reflects the anticipated operating schedules, and include the occupancy sensors in employee lunch and break rooms, conference/meeting rooms, and classrooms (not including shop classrooms, laboratory classrooms, and preschool through 12th grade classrooms). "]
["G"]
["G","Baseline and proposed lighting schedules reflet the mandaotry shut-off lighting controls that turn off lighting during unoccupied hours."]
["G"]
["G","In spaces where proposed lighting is not specified or patially specified , or where the proposed lighting is specifically exempted in Section 9.1.1, 9.2.2.3, or 9.4.2, the same lighting power is modeled in the baseline and the proposed design?"]
["G"]
["G","The proposed lighting power includes all lighting system components shown or provided for on the plans (including lamps and ballasts and task and furniture-mounted fixtures), and is based on the manufacturers’ labeled maximum wattage of the luminaires."]
["G"]
["G","The proposed building design contains the mandatory automatic lighting controls specified in Section 9.4.1 (e.g., automatic daylight responsive controls, occupancy sensors, programmable controls, etc.). "]
[]
["G","Automatic daylighting controls are modeled directly in the proposed design or through schedule adjustments determined by a separate daylighting analysis approved by the rating authority. Modeling and schedule adjustments separately account for primary side lighted areas, secondary side lighted areas, and top lighted areas."]
["G"]
["G","The proposed lighting schedules are the same as the baseline, except as allowed in Table G3.7. The occupancy sensors included in the proposed design are modeled by reducing the lighting schedule each hour by the Occupancy Sensor Reduction factor in Table G3.7 for the applicable space type. This reduction is taken only for lighting controlled by the occupancy sensors. Credit for other programmable lighting control in buildings less than 5000 ft2 is taken by reducing the lighting schedule each hour by 10%."]
["G"]
["G","For each item entered as “No” above, describe the applicable ASHRAE 90.1 Appendix G exception(s) that apply, or the circumstances preventing the lighting parameters from being modeled as required. If the energy simulation software is not capable of modeling the required parameters, describe the adjustments that were made to provide a similar representation or provide a narrative justifying why the predicted energy performance results will not be influenced."]
["G"]
["G"]
["G","Table 6.1: Interior Lighting by Space Type",null,null,null,null,null,"Model Inputs",null,null,"Reference Values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2]
["G","Space Type",null,"Floor Area (SF)","Prop. Lighting Power (W)","Baseline Lighting Power (W)","Unregulated Lighting LPD (Baseline and Proposed)\n(W)","Prop. LPD (W/SF)","Baseline LPD (W/SF)","Unregulated Lighting LPD (Baseline and Proposed)\n(W/SF)","Prop. LPD x OS Credit (W/SF)","Prop. Lighting Power x OS Credit (W)",{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
["G",{"$f":"'Lighting Assumptions'!C3","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B27),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B27),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B27),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B27),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B27),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B27),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(D27>0, E27/D27, \"-\")","v":"-"},{"$f":"IF(ISERROR(IF(D27>0, F27/D27, \"-\"))=TRUE,\"\",IF(D27>0, F27/D27, \"-\"))","v":"-"},{"$f":"IF(D27>0, G27/D27, \"-\")","v":"-"},{"$f":"IF(D27>0, L27/D27, \"-\")","v":"-"},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B27),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B27,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B27,'Lighting Assumptions 90.1-2013'!I3:I106))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B27,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B27,'Lighting Assumptions 90.1-2010'!I3:I106))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W26,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W26,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},{"$f":"IF(B27=\"Dwelling Unit\",IF(H27<0.6,1,0),0)","v":0},{"$f":"IF(B27=\"Dwelling Unit\",0,IF(B27=\"\",\"\",IF(H27<(0.7*M27),1,0)))","v":""}]
["G",{"$f":"'Lighting Assumptions'!C4","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B28),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B28),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B28),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B28),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B28),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B28),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-",{"$f":"IF(D28>0, G28/D28, \"-\")","v":"-"},"-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B28),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B28,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B28,'Lighting Assumptions 90.1-2013'!I4:I107))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B28,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B28,'Lighting Assumptions 90.1-2010'!I4:I107))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W27,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W27,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C5","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B29),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B29),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B29),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B29),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B29),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B29),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B29),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B29,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B29,'Lighting Assumptions 90.1-2013'!I5:I108))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B29,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B29,'Lighting Assumptions 90.1-2010'!I5:I108))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W28,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W28,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C6","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B30),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B30),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B30),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B30),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B30),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B30),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B30),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B30,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B30,'Lighting Assumptions 90.1-2013'!I6:I109))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B30,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B30,'Lighting Assumptions 90.1-2010'!I6:I109))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W29,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W29,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C7","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B31),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B31),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B31),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B31),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B31),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B31),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B31),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B31,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B31,'Lighting Assumptions 90.1-2013'!I7:I110))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B31,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B31,'Lighting Assumptions 90.1-2010'!I7:I110))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W30,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W30,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C8","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B32),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B32),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B32),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B32),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B32),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B32),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B32),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B32,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B32,'Lighting Assumptions 90.1-2013'!I8:I111))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B32,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B32,'Lighting Assumptions 90.1-2010'!I8:I111))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W31,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W31,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
[null,{"$f":"'Lighting Assumptions'!C9","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B33),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B33),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B33),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B33),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B33),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B33),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B33),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B33,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B33,'Lighting Assumptions 90.1-2013'!I9:I112))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B33,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B33,'Lighting Assumptions 90.1-2010'!I9:I112))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W32,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W32,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
[null,{"$f":"'Lighting Assumptions'!C10","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B34),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B34),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B34),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B34),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B34),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B34),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B34),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B34,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B34,'Lighting Assumptions 90.1-2013'!I10:I113))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B34,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B34,'Lighting Assumptions 90.1-2010'!I10:I113))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W33,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W33,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
[null,{"$f":"'Lighting Assumptions'!C11","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B35),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B35),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B35),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B35),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B35),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B35),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B35),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B35,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B35,'Lighting Assumptions 90.1-2013'!I11:I114))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B35,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B35,'Lighting Assumptions 90.1-2010'!I11:I114))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W34,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W34,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["A",{"$f":"'Lighting Assumptions'!C12","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B36),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B36),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B36),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B36),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B36),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B36),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B36),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B36,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B36,'Lighting Assumptions 90.1-2013'!I12:I115))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B36,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B36,'Lighting Assumptions 90.1-2010'!I12:I115))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W33,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W33,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
[null,{"$f":"'Lighting Assumptions'!C13","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B37),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B37),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B37),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B37),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B37),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B37),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B37),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B37,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B37,'Lighting Assumptions 90.1-2013'!I13:I116))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B37,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B37,'Lighting Assumptions 90.1-2010'!I13:I116))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W36,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W36,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
[null,{"$f":"'Lighting Assumptions'!C14","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B38),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B38),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B38),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B38),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B38),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B38),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B38),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B38,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B38,'Lighting Assumptions 90.1-2013'!I14:I117))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B38,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B38,'Lighting Assumptions 90.1-2010'!I14:I117))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W37,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W37,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
[null,{"$f":"'Lighting Assumptions'!C15","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B39),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B39),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B39),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B39),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B39),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B39),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B39),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B39,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B39,'Lighting Assumptions 90.1-2013'!I15:I118))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B39,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B39,'Lighting Assumptions 90.1-2010'!I15:I118))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W38,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W38,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
[null,{"$f":"'Lighting Assumptions'!C16","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B40),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B40),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B40),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B40),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B40),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B40),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B40),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B40,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B40,'Lighting Assumptions 90.1-2013'!I16:I119))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B40,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B40,'Lighting Assumptions 90.1-2010'!I16:I119))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W39,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W39,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C17","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B41),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B41),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B41),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B41),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B41),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B41),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B41),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B41,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B41,'Lighting Assumptions 90.1-2013'!I17:I120))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B41,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B41,'Lighting Assumptions 90.1-2010'!I17:I120))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W40,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W40,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C18","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B42),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B42),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B42),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B42),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B42),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B42),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B42),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B42,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B42,'Lighting Assumptions 90.1-2013'!I18:I121))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B42,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B42,'Lighting Assumptions 90.1-2010'!I18:I121))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W41,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W41,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C19","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B43),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B43),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B43),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B43),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B43),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B43),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B43),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B43,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B43,'Lighting Assumptions 90.1-2013'!I19:I122))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B43,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B43,'Lighting Assumptions 90.1-2010'!I19:I122))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W42,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W42,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C20","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B44),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B44),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B44),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B44),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B44),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B44),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B44),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B44,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B44,'Lighting Assumptions 90.1-2013'!I20:I123))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B44,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B44,'Lighting Assumptions 90.1-2010'!I20:I123))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W43,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W43,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
[null,{"$f":"'Lighting Assumptions'!C21","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B45),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B45),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B45),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B45),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B45),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B45),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B45),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B45,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B45,'Lighting Assumptions 90.1-2013'!I21:I124))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B45,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B45,'Lighting Assumptions 90.1-2010'!I21:I124))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W44,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W44,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C22","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B46),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B46),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B46),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B46),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B46),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B46),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B46),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B46,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B46,'Lighting Assumptions 90.1-2013'!I22:I125))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B46,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B46,'Lighting Assumptions 90.1-2010'!I22:I125))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W45,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W45,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C23","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B47),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B47),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B47),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B47),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B47),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B47),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B47),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B47,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B47,'Lighting Assumptions 90.1-2013'!I23:I126))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B47,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B47,'Lighting Assumptions 90.1-2010'!I23:I126))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W46,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W46,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C24","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B48),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B48),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B48),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B48),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B48),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B48),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B48),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B48,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B48,'Lighting Assumptions 90.1-2013'!I24:I127))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B48,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B48,'Lighting Assumptions 90.1-2010'!I24:I127))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W47,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W47,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C25","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B49),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B49),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B49),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B49),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B49),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B49),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B49),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B49,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B49,'Lighting Assumptions 90.1-2013'!I25:I128))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B49,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B49,'Lighting Assumptions 90.1-2010'!I25:I128))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W46,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W46,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C26","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B50),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B50),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B50),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B50),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B50),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B50),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B50),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B50,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B50,'Lighting Assumptions 90.1-2013'!I26:I129))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B50,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B50,'Lighting Assumptions 90.1-2010'!I26:I129))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W49,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W49,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C27","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B51),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B51),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B51),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B51),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B51),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B51),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B51),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B51,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B51,'Lighting Assumptions 90.1-2013'!I27:I130))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B51,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B51,'Lighting Assumptions 90.1-2010'!I27:I130))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W50,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W50,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C28","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B52),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B52),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B52),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B52),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B52),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B52),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B52),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B52,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B52,'Lighting Assumptions 90.1-2013'!I28:I131))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B52,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B52,'Lighting Assumptions 90.1-2010'!I28:I131))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W51,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W51,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C29","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B53),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B53),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B53),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B53),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B53),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B53),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B53),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B53,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B53,'Lighting Assumptions 90.1-2013'!I29:I132))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B53,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B53,'Lighting Assumptions 90.1-2010'!I29:I132))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W52,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W52,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C30","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B54),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B54),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B54),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B54),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B54),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B54),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B54),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B54,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B54,'Lighting Assumptions 90.1-2013'!I30:I133))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B54,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B54,'Lighting Assumptions 90.1-2010'!I30:I133))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W53,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W53,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C31","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B55),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B55),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B55),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B55),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B55),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B55),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B55),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B55,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B55,'Lighting Assumptions 90.1-2013'!I31:I134))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B55,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B55,'Lighting Assumptions 90.1-2010'!I31:I134))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W54,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W54,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C32","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B56),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B56),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B56),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B56),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B56),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B56),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B56),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B56,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B56,'Lighting Assumptions 90.1-2013'!I32:I135))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B56,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B56,'Lighting Assumptions 90.1-2010'!I32:I135))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W55,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W55,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C33","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B57),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B57),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B57),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B57),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B57),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B57),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B57),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B57,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B57,'Lighting Assumptions 90.1-2013'!I33:I136))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B57,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B57,'Lighting Assumptions 90.1-2010'!I33:I136))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W56,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W56,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C34","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B58),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B58),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B58),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B58),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B58),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B58),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B58),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B58,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B58,'Lighting Assumptions 90.1-2013'!I34:I137))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B58,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B58,'Lighting Assumptions 90.1-2010'!I34:I137))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W57,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W57,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G",{"$f":"'Lighting Assumptions'!C35","v":""},null,{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B59),'6a - Lighting Counts'!H$29:$H$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B59),'6a - Lighting Counts'!$AQ$29:$AQ$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B59),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B59),'6a - Lighting Counts'!$AR$29:$AR$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},{"$f":"IF(ISERROR(SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B59),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551)=TRUE),\"\",SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= '6b - General Lighting'!B59),'6a - Lighting Counts'!$AS$29:$AS$551,'6a - Lighting Counts'!$F$29:$F$551))","v":0},"-","-","-","-",{"$f":"SUMPRODUCT(--('6a - Lighting Counts'!$G$29:$G$551= B59),'6a - Lighting Counts'!$AX$29:$AX$551,'6a - Lighting Counts'!$F$29:$F$551)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B59,'Lighting Assumptions 90.1-2013'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2013'!LPDSpacebySpace,'6b - General Lighting'!B59,'Lighting Assumptions 90.1-2013'!I35:I138))),\"\"),IFERROR(IF(SI_IP_Units=\"IP\",(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B59,'Lighting Assumptions 90.1-2010'!$H$3:$H$106)),(SUMIF('Lighting Assumptions 90.1-2010'!LPDSpacebySpace,'6b - General Lighting'!B59,'Lighting Assumptions 90.1-2010'!I35:I138))),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W58,'6a - Lighting Counts'!$G$33:$G$551), 0)))=TRUE,\"\",INDEX('6a - Lighting Counts'!$G$33:$G$551, MATCH(0, COUNTIF($W$26:W58,'6a - Lighting Counts'!$G$33:$G$551), 0)))","v":""},0,""]
["G","Total",null,{"$f":"SUM(D27:D59)","v":0},{"$f":"SUM(E27:E59)","v":0},{"$f":"SUM(F27:F59)","v":0},{"$f":"SUM(G27:G59)","v":0},"-",{"$f":"IF(D60>0, F60/D60, \"-\")","v":"-"},{"$f":"IF(D60>0, G60/D60, \"-\")","v":"-"},"-",{"$f":"SUM(L27:L59)","v":0},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IFERROR((SUMPRODUCT(D27:D59,M27:M59)/D60),\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(X27:X59)","v":0},{"$f":"SUM(Y27:Y59)","v":0}]
["G"]
["G"]
["G"]
["G"]
["B"]
[]
[]
[]
[]
["G"]
["G"]
["G"]
[]
["G"]
[]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["D"]
[]
[]
[]
[]
[]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
[]
["G"]
["G"]
["G"]
["G"]
["G","Table 6.2: Summary"]
[null,{"$f":"\"Total modeled interior lighting power, based on inputs above\"","v":"Total modeled interior lighting power, based on inputs above"}]
["G"]
["G","Building ID",null,null,null,null,{"$f":"CONCATENATE(\"Baseline\",CHAR(10),IF(SI_IP_Units=\"IP\",\"(W/sq ft)\",\"(W/sq m)\"))","v":"Baseline\n(W/sq ft)"},null,null,{"$f":"CONCATENATE(\"Proposed Design\",CHAR(10),IF(SI_IP_Units=\"IP\",\"(W/sq ft)\",\"(W/sq m)\"))","v":"Proposed Design\n(W/sq ft)"},null,{"$f":"CONCATENATE(\"Baseline\",CHAR(10),\"(kW)\")","v":"Baseline\n(kW)"},null,null,{"$f":"CONCATENATE(\"Proposed Design  \",CHAR(10),\"(kW)\")","v":"Proposed Design  \n(kW)"}]
[null,{"$f":"B105","v":0},null,null,null,null,"Base_LPD",null,null,"Design_LPD",null,"Base_Power",null,null,"Design_Power"]
[null,{"$f":"'1 - Multiple Buildings Details'!B24","v":0},null,null,null,null,{"$f":"I60","v":"-"},null,null,{"$f":"K60","v":"-"},null,{"$f":"IF(I60=\"-\",\"-\",I60*D60/1000)","v":"-"},null,null,{"$f":"IF(K60=\"-\",\"-\",K60*D60/1000)","v":"-"}]
["G"]
["G","Table 6.3: Interior Process Lighting (if applicable)"]
["G","Building ID","Description",null,null,null,"Section 9.2.2.3 Exemption",null,null,null,null,"Total Process Lighting Power (W)",null,null,"Modeled Identically In Baseline?"]
["G",null,"Helpful Hints\nDescribe any process lighting included in the design (example: 4 kW stage lighting and 20 3-Watt exit signs)",null,null,null,"Helpful Hints\nIndicate the specific exemption from Section 9.2.2.3 that excludes the lighting from the Section 9.5 or Section 9.6 lighting power density requirements [example: Stage lighting - 9.2.2.3(12); Exit signs - 9.2.2.3(10)]",null,null,null,null,"Helpful Hints\nProvide the total process lighting power for this line item description. ",null,null,"Helpful Hints\nAny lighting not regulated by ASHRAE 90.1 is considered process and must be modeled identically in the Proposed and Baseline case unless an Exceptional Calculation is submitted."]
["G",{"$f":"B111","v":"Building ID"},{"$f":"C111","v":"Description"},null,null,null,{"$f":"G111","v":"Section 9.2.2.3 Exemption"},null,null,null,null,{"$f":"L111","v":"Total Process Lighting Power (W)"},null,null,{"$f":"O111","v":"Modeled Identically In Baseline?"}]
["G",{"$f":"GI_Project_Name","v":0}]
["G",{"$f":"GI_Project_Name","v":0}]
["G",{"$f":"GI_Project_Name","v":0}]
["G",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L114=\"\",\"-\",SUM(L114:N116)&\" W\")","v":"-"}]
["G","Exterior Lighting"]
["G","Instructions: Complete the corresponding lighting table(s) if applicable. An example of the expected level of detail has been provided for each input. Please refer to the column header notes for information about Appendix G modeling protocol. For any information not applicable to the project, simply enter \"N/A\"."]
["G","Exterior Lighting Requirements"]
["G","The same schedules reflecting the mandatory exterior lighting controls were modeled in the baseline and proposed design. "]
[]
["G","The baseline lighting power allowance is based on the portions of the site that are illuminated. (The illuminated area is any area within a square pattern around each luminaire or pole that is six times the luminaire mounting height, with the luminaire in the middle of the pattern, less any area that is within a building, under a canopy, beyond property lines, or obstructed by a sign or structure.) "]
[]
["G","Any overlapping area of another lighting application were subtracted from the area of the other lighting application, to avoid double-counting. (The allowed area of roadway, driveway, sidewalk, walkway or bikeway was determined as either the actual paved area plus 5 feet on either side of the centerline path of travel, or a 25-foot-wide area running along the axis of the path of travel and including as much of the paved area of the site roadway, driveway, sidewalk, walkway or bikeway as possible.)"]
[]
["G","The proposed lighting power includes all lighting system components shown or provided for on the plans (including lamps and ballasts and task and furniture-mounted fixtures except where specifically exempted), manufacturers’ labeled maximum wattage of the luminaire."]
[]
["G","The proposed building design contains the mandatory automatic lighting controls specified in Section 9.4.1 (e.g., automatic daylight responsive controls, occupancy sensors, programmable controls, etc.). "]
[]
["G","Select the appropriate Exterior Lighting Zone from ASHRAE 90.1-2016 Table 9.4.2-1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P131=\"Zone 0\",0,IF(P131=\"Zone 1\",1,IF(P131=\"Zone 2\",2,IF(P131=\"Zone 3\",3,IF(P131=\"Zone 4\",4,\"\")))))","v":""}]
["G"]
["G"]
[]
["G"]
[]
[null,"Table 6.4: Tradable Surfaces"]
[null,"This table is only required to be completed if Tradable Exterior Lighting is applicable to the project."]
[null,"General Information",null,null,null,null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,null,"Proposed Design",null,null,null,null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
[null,"Table G3.6 Lighting Power Densities for Building Exteriors (Tradable)",null,null,null,"Required Input (Area or Length)",null,{"$f":"IF(SI_IP_Units=\"IP\",\"Total Area \n(sq ft) \nor Length \n(ft)\",\"Total Area \n(sq m) \nor Length \n(m)\")","v":"Total Area \n(sq ft) \nor Length \n(ft)"},"Allowed LPD","Lighting Power Allowance \n(W)",null,null,"Design Lighting Power \n(W)",null,null,null,null,"Plans / Specs",null,null,null,null,null,null,null,"***90.1-2010 LOOKUP TABLES ARE NOT SET UP…VALUES IN 2010 MUST BE UPDATED TO REFLECT 2010"]
[null,"Table G3.6 Tradable Exterior Lighting Application",null,null,null,"Required Input (Area or Length)",null,{"$f":"IF(SI_IP_Units=\"IP\",\"Total Area \n(sq ft) \nor Length \n(ft)\",\"Total Area \n(sq m) \nor Length \n(m)\")","v":"Total Area \n(sq ft) \nor Length \n(ft)"},"Allowed LPD","Lighting Power Allowance \n(W)",null,null,"Design Lighting Power \n(W)",null,null,null,null,null,null,"(W)"]
[null,null,"Helpful Hints\nFixtures cannot be double-counted for multiple exterior surface types",null,null,"Helpful Hints",null,"Helpful Hints\nOnly enter area or length of illuminated surface in the design","Helpful Hints\nAllowance calculated using the maximum lighting power density from Table G3.6.","Helpful Hints",null,null,"Helpful Hints\n• Lighting power should be modeled as designed (or installed)\n• Reference specific place in the submitted design documents (e.g. drawing & detail number) where relevant parameters are listed to support review.",null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2013,\"In accordance with Prescriptive Requirements of 90.1-2013 Table 9.4.2-2\",\"In accordance with Prescriptive Requirements of 90.1-2010 Table 9.4.2-2\")","v":"In accordance with Prescriptive Requirements of 90.1-2013 Table 9.4.2-2"},null,null,null,"Prescriptive Requirement 90.1-2013",null,"Prescriptive Requirement 90.1-2010"]
["G"]
["G","Parking lots and drives",null,null,null,{"$f":"IFERROR(VLOOKUP(B144,'Lighting Assumptions'!$L$4:$M$17,2,FALSE),\"\")","v":"Area"},null,null,{"$f":"IF(B144=\"\",\"\",SUMIF('Lighting Assumptions'!$L$16:$L$37,'6b - General Lighting'!W144,'Lighting Assumptions'!$N$16:$N$37))","v":0.15},{"$f":"IFERROR(H144*I144,\"\")","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF($P$131=\"\",\"-\",IF('General Information'!$K$48=2013,IF(AND(X144=\"\",Y144=\"\"),\"\",\"LPD-\"&X144&\", \"&Y144&\" Watts\"),IF(AND(Z144=\"\",AA144=\"\"),\"\",\"LPD-\"&Z144&\", \"&AA144&\" Watts\"))))","v":"-"},null,null,{"$f":"SI_IP_Units&'6b - General Lighting'!B144","v":"IPParking lots and drives"},{"$f":"IF(B144=\"\",\"\",INDEX('Lighting Assumptions 90.1-2013'!$N$16:$N$37,MATCH('6b - General Lighting'!W144,'Lighting Assumptions 90.1-2013'!$L$16:$L$37,0)))","v":""},{"$f":"IFERROR(H144*X144,\"No Allowance\")","v":"No Allowance"},{"$f":"IF(B144=\"\",\"\",INDEX('Lighting Assumptions 90.1-2010'!$N$16:$N$37,MATCH('6b - General Lighting'!W144,'Lighting Assumptions 90.1-2010'!$L$16:$L$37,0)))","v":""},{"$f":"IFERROR(H144*Z144,\"No Allowance\")","v":"No Allowance"}]
["G","Main entries",null,null,null,{"$f":"IFERROR(VLOOKUP(B145,'Lighting Assumptions'!$L$4:$M$17,2,FALSE),\"\")","v":"Length"},null,null,{"$f":"IF(B145=\"\",\"\",SUMIF('Lighting Assumptions'!$L$16:$L$37,'6b - General Lighting'!W145,'Lighting Assumptions'!$N$16:$N$37))","v":30},{"$f":"IFERROR(H145*I145,\"\")","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF($P$131=\"\",\"-\",IF('General Information'!$K$48=2013,IF(AND(X145=\"\",Y145=\"\"),\"\",\"LPD-\"&X145&\", \"&Y145&\" Watts\"),IF(AND(Z145=\"\",AA145=\"\"),\"\",\"LPD-\"&Z145&\", \"&AA145&\" Watts\"))))","v":"-"},null,null,{"$f":"SI_IP_Units&'6b - General Lighting'!B145","v":"IPMain entries"},{"$f":"IF(B145=\"\",\"\",INDEX('Lighting Assumptions 90.1-2013'!$N$16:$N$37,MATCH('6b - General Lighting'!W145,'Lighting Assumptions 90.1-2013'!$L$16:$L$37,0)))","v":""},{"$f":"IFERROR(H145*X145,\"No Allowance\")","v":"No Allowance"},{"$f":"IF(B145=\"\",\"\",INDEX('Lighting Assumptions 90.1-2010'!$N$16:$N$37,MATCH('6b - General Lighting'!W145,'Lighting Assumptions 90.1-2010'!$L$16:$L$37,0)))","v":""},{"$f":"IFERROR(H145*Z145,\"No Allowance\")","v":"No Allowance"}]
["G","Other doors",null,null,null,{"$f":"IFERROR(VLOOKUP(B146,'Lighting Assumptions'!$L$4:$M$17,2,FALSE),\"\")","v":"Length"},null,null,{"$f":"IF(B146=\"\",\"\",SUMIF('Lighting Assumptions'!$L$16:$L$37,'6b - General Lighting'!W146,'Lighting Assumptions'!$N$16:$N$37))","v":20},{"$f":"IFERROR(H146*I146,\"\")","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF($P$131=\"\",\"-\",IF('General Information'!$K$48=2013,IF(AND(X146=\"\",Y146=\"\"),\"\",\"LPD-\"&X146&\", \"&Y146&\" Watts\"),IF(AND(Z146=\"\",AA146=\"\"),\"\",\"LPD-\"&Z146&\", \"&AA146&\" Watts\"))))","v":"-"},null,null,{"$f":"SI_IP_Units&'6b - General Lighting'!B146","v":"IPOther doors"},{"$f":"IF(B146=\"\",\"\",INDEX('Lighting Assumptions 90.1-2013'!$N$16:$N$37,MATCH('6b - General Lighting'!W146,'Lighting Assumptions 90.1-2013'!$L$16:$L$37,0)))","v":""},"No Allowance",{"$f":"IF(B146=\"\",\"\",INDEX('Lighting Assumptions 90.1-2010'!$N$16:$N$37,MATCH('6b - General Lighting'!W146,'Lighting Assumptions 90.1-2010'!$L$16:$L$37,0)))","v":""},"No Allowance"]
[null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(B147,'Lighting Assumptions'!$L$4:$M$17,2,FALSE),\"\")","v":""},null,null,{"$f":"IF(B147=\"\",\"\",SUMIF('Lighting Assumptions'!$L$16:$L$37,'6b - General Lighting'!W147,'Lighting Assumptions'!$N$16:$N$37))","v":""},{"$f":"IFERROR(H147*I147,\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF($P$131=\"\",\"-\",IF('General Information'!$K$48=2013,IF(AND(X147=\"\",Y147=\"\"),\"\",\"LPD-\"&X147&\", \"&Y147&\" Watts\"),IF(AND(Z147=\"\",AA147=\"\"),\"\",\"LPD-\"&Z147&\", \"&AA147&\" Watts\"))))","v":"-"},null,null,{"$f":"SI_IP_Units&'6b - General Lighting'!B147","v":"IP"},{"$f":"IF(B147=\"\",\"\",INDEX('Lighting Assumptions 90.1-2013'!$N$16:$N$37,MATCH('6b - General Lighting'!W147,'Lighting Assumptions 90.1-2013'!$L$16:$L$37,0)))","v":""},"No Allowance",{"$f":"IF(B147=\"\",\"\",INDEX('Lighting Assumptions 90.1-2010'!$N$16:$N$37,MATCH('6b - General Lighting'!W147,'Lighting Assumptions 90.1-2010'!$L$16:$L$37,0)))","v":""},"No Allowance"]
["C",null,null,null,null,{"$f":"IFERROR(VLOOKUP(B148,'Lighting Assumptions'!$L$4:$M$17,2,FALSE),\"\")","v":""},null,null,{"$f":"IF(B148=\"\",\"\",SUMIF('Lighting Assumptions'!$L$16:$L$37,'6b - General Lighting'!W148,'Lighting Assumptions'!$N$16:$N$37))","v":""},{"$f":"IFERROR(H148*I148,\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF($P$131=\"\",\"-\",IF('General Information'!$K$48=2013,IF(AND(X148=\"\",Y148=\"\"),\"\",\"LPD-\"&X148&\", \"&Y148&\" Watts\"),IF(AND(Z148=\"\",AA148=\"\"),\"\",\"LPD-\"&Z148&\", \"&AA148&\" Watts\")))","v":"-"},null,null,{"$f":"SI_IP_Units&'6b - General Lighting'!B148","v":"IP"},{"$f":"IF(B148=\"\",\"\",INDEX('Lighting Assumptions 90.1-2013'!$N$16:$N$37,MATCH('6b - General Lighting'!W148,'Lighting Assumptions 90.1-2013'!$L$16:$L$37,0)))","v":""},{"$f":"IFERROR(H148*X148,\"No Allowance\")","v":"No Allowance"},{"$f":"IF(B148=\"\",\"\",INDEX('Lighting Assumptions 90.1-2010'!$N$16:$N$37,MATCH('6b - General Lighting'!W148,'Lighting Assumptions 90.1-2010'!$L$16:$L$37,0)))","v":""},{"$f":"IFERROR(H148*Z148,\"No Allowance\")","v":"No Allowance"}]
[null,"Total tradable surface lighting allowance",null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(J144:J147),\"\")","v":0},null,null,{"$f":"IFERROR(SUM(M144:M147),\"\")","v":0},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IFERROR(SUM(Y144:Y147),\"\"))","v":0}]
["G"]
["G"]
["G","Table 6.5: Nontradable Surfaces"]
["G","This table is only required to be completed if Nontradable Exterior Lighting is applicable to the project."]
["G","General Information",null,null,null,null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,null,"Proposed Design",null,null,null,null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"}]
["G","Table G3.6 Lighting Power Densities for Building Exteriors (Nontradable)",null,null,null,"Required Input",null,"Quantity of Required Input for Project","Allowed LPD","Lighting Power Allowance \n(W)",null,null,"Design Lighting Power \n(W)",null,null,null,null,"Plans / Specs",null,null,null,null,null,null,null,null,"***90.1-2010 LOOKUP TABLES ARE NOT SET UP…VALUES IN 2010 MUST BE UPDATED TO REFLECT 2010",null,null,"Adjusted Baseline (equal to lesser of proposed or baseline allowance)","Proposed"]
[null,null,"Helpful Hints\n•  Only enter area or length of illuminated surface in the design\n•  Fixtures cannot be double-counted for multiple exterior surface types",null,null,"Helpful Hints",null,null,"Helpful Hints\nTotal allowance calculated using the lesser of the design lighting power, or the lighting power allowance used, since no credit is permitted for nontradable surfaces.",null,null,null,"Helpful Hints\n• Lighting power should be modeled as designed (or installed)\n• Reference specific place in the submitted design documents (e.g. drawing & detail number) where relevant parameters are listed to support review.",null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2013,\"In accordance with Prescriptive Requirements of 90.1-2013 Table 9.4.2-2\",\"In accordance with Prescriptive Requirements of 90.1-2010 Table 9.4.2-2\")","v":"In accordance with Prescriptive Requirements of 90.1-2013 Table 9.4.2-2"},null,null,null,"Prescriptive Requirement 90.1-2013",null,null,"Prescriptive Requirement 90.1-2010"]
[]
[null,"Index",null,null,null,{"$f":"F155","v":"Required Input"},null,{"$f":"H155","v":"Quantity of Required Input for Project"},{"$f":"I155","v":"Allowed LPD"},{"$f":"J155","v":"Lighting Power Allowance \n(W)"},null,null,{"$f":"M155","v":"Design Lighting Power \n(W)"},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(B158=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!L27:L48,'6b - General Lighting'!W158,'Lighting Assumptions 90.1-2013'!N27:N48))","v":0},{"$f":"IFERROR(H158*X158,\"\")","v":""},null,{"$f":"IF(E158=\"\",\"\",SUMIF('Lighting Assumptions 90.1-2013'!O27:O48,'6b - General Lighting'!Z158,'Lighting Assumptions 90.1-2013'!Q27:Q48))","v":""},{"$f":"IFERROR(K158*AA158,\"\")","v":""}]
["G","Building facades",null,null,null,"Area",null,null,{"$f":"IF(AND(SI_IP_Units=\"IP\",F159=\"Area\"),'Lighting Assumptions'!N46,IF(AND(SI_IP_Units=\"IP\",F159=\"Length\"),'Lighting Assumptions'!N52,IF(AND(SI_IP_Units=\"SI\",F159=\"Area\"),'Lighting Assumptions'!O46,IF(AND(SI_IP_Units=\"SI\",F159=\"Length\"),'Lighting Assumptions'!O52,\"\"))))","v":0.2},{"$f":"IFERROR(IF(H159=\"\",\"\",H159*I159),\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IF(AND(X159=\"\",Y159=\"\"),\"\",\"LPD-\"&X159&\", \"&Y159&\" Watts\"),IF(AND(AA159=\"\",AB159=\"\"),\"\",\"LPD-\"&AA159&\", \"&AB159&\" Watts\")))","v":""},null,null,{"$f":"SI_IP_Units&'6b - General Lighting'!B159&F159","v":"IPBuilding facadesArea"},{"$f":"IF(H159=\"\",\"\",INDEX('Lighting Assumptions 90.1-2013'!$N$54:$N$67,MATCH('6b - General Lighting'!W159,'Lighting Assumptions 90.1-2013'!$L$54:$L$67,0)))","v":""},{"$f":"IFERROR(IF(H159=\"\",\"\",H159*X159),\"No Allowance\")","v":""},{"$f":"IFERROR(Y159+0,0)","v":0},{"$f":"IF(H159=\"\",\"\",INDEX('Lighting Assumptions 90.1-2010'!$N$54:$N$67,MATCH('6b - General Lighting'!W159,'Lighting Assumptions 90.1-2010'!$L$54:$L$67,0)))","v":""},{"$f":"IFERROR(IF(H159=\"\",\"\",H159*AA159),\"No Allowance\")","v":""},{"$f":"IFERROR(AB159+0,0)","v":0},{"$f":"IF(ISERROR(1/M159),0,MIN(J159,M159))","v":0},{"$f":"M159","v":0},{"$f":"IF(M159>J159,TRUE,FALSE)","v":false}]
["G","ATMs and night depositories",null,null,null,"Number of ATMs",null,null,{"$f":"IF(SI_IP_Units=\"IP\",'Lighting Assumptions'!N47,'Lighting Assumptions'!O47)","v":"270 W+90 per additional"},{"$f":"IFERROR(IF(H160>0,IF(H160=1,270,(270+(H160-1)*90)),\"\"),\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IF(AND(X160=\"\",Y160=\"\"),\"\",\"LPD-\"&X160),IF(AND(AA160=\"\",AB160=\"\"),\"\",\"LPD-\"&AA160)))","v":""},null,null,{"$f":"SI_IP_Units&'6b - General Lighting'!B160","v":"IPATMs and night depositories"},{"$f":"IF(H160=\"\",\"\",INDEX('Lighting Assumptions 90.1-2013'!$N$54:$N$67,MATCH('6b - General Lighting'!W160,'Lighting Assumptions 90.1-2013'!$L$54:$L$67,0)))","v":""},{"$f":"IFERROR(IF(H160=\"\",\"\",H160*X160),\"No Allowance\")","v":""},0,{"$f":"IF(H160=\"\",\"\",INDEX('Lighting Assumptions 90.1-2010'!$N$54:$N$67,MATCH('6b - General Lighting'!W160,'Lighting Assumptions 90.1-2010'!$L$54:$L$67,0)))","v":""},{"$f":"IFERROR(IF(H160=\"\",\"\",H160*AA160),\"No Allowance\")","v":""},{"$f":"IFERROR(AB160+0,0)","v":0},0,0,false]
["G","Entrances and gatehouse inspection stations at guarded facilities",null,null,null,"Uncovered Area",null,null,{"$f":"IF(SI_IP_Units=\"IP\",'Lighting Assumptions'!N48,'Lighting Assumptions'!O48)","v":1.25},{"$f":"IFERROR(IF(H161=\"\",\"\",H161*I161),\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IF(AND(X161=\"\",Y161=\"\"),\"\",\"LPD-\"&X161&\", \"&Y161&\" Watts\"),IF(AND(AA161=\"\",AB161=\"\"),\"\",\"LPD-\"&AA161&\", \"&AB161&\" Watts\")))","v":""},null,null,{"$f":"SI_IP_Units&'6b - General Lighting'!B161","v":"IPEntrances and gatehouse inspection stations at guarded facilities"},{"$f":"IF(H161=\"\",\"\",INDEX('Lighting Assumptions 90.1-2013'!$N$54:$N$67,MATCH('6b - General Lighting'!W161,'Lighting Assumptions 90.1-2013'!$L$54:$L$67,0)))","v":""},"",0,{"$f":"IF(H161=\"\",\"\",INDEX('Lighting Assumptions 90.1-2010'!$N$54:$N$67,MATCH('6b - General Lighting'!W161,'Lighting Assumptions 90.1-2010'!$L$54:$L$67,0)))","v":""},"",{"$f":"IFERROR(AB161+0,0)","v":0},0,0,false]
["G","Loading areas for law enforcement, fire, ambulance, and other emergency service vehicles",null,null,null,"Uncovered Area",null,null,{"$f":"IF(SI_IP_Units=\"IP\",'Lighting Assumptions'!N49,'Lighting Assumptions'!O49)","v":0.5},{"$f":"IFERROR(IF(H162=\"\",\"\",H162*I162),\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IF(AND(X162=\"\",Y162=\"\"),\"\",\"LPD-\"&X162&\", \"&Y162&\" Watts\"),IF(AND(AA162=\"\",AB162=\"\"),\"\",\"LPD-\"&AA162&\", \"&AB162&\" Watts\")))","v":""},null,null,{"$f":"SI_IP_Units&'6b - General Lighting'!B162","v":"IPLoading areas for law enforcement, fire, ambulance, and other emergency service vehicles"},{"$f":"IF(H162=\"\",\"\",INDEX('Lighting Assumptions 90.1-2013'!$N$54:$N$67,MATCH('6b - General Lighting'!W162,'Lighting Assumptions 90.1-2013'!$L$54:$L$67,0)))","v":""},"",0,{"$f":"IF(H162=\"\",\"\",INDEX('Lighting Assumptions 90.1-2010'!$N$54:$N$67,MATCH('6b - General Lighting'!W162,'Lighting Assumptions 90.1-2010'!$L$54:$L$67,0)))","v":""},"",{"$f":"IFERROR(AB162+0,0)","v":0},0,0,false]
["G","Drive-through windows at fast food restaurants",null,null,null,"Number of Drive-throughs",null,null,{"$f":"IF(SI_IP_Units=\"IP\",'Lighting Assumptions'!N50,'Lighting Assumptions'!O50)","v":400},{"$f":"IFERROR(IF(H163=\"\",\"\",H163*I163),\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IF(AND(X163=\"\",Y163=\"\"),\"\",\"LPD-\"&X163&\", \"&Y163&\" Watts\"),IF(AND(AA163=\"\",AB163=\"\"),\"\",\"LPD-\"&AA163&\", \"&AB163&\" Watts\")))","v":""},null,null,{"$f":"SI_IP_Units&'6b - General Lighting'!B163","v":"IPDrive-through windows at fast food restaurants"},{"$f":"IF(H163=\"\",\"\",INDEX('Lighting Assumptions 90.1-2013'!$N$54:$N$67,MATCH('6b - General Lighting'!W163,'Lighting Assumptions 90.1-2013'!$L$54:$L$67,0)))","v":""},"",0,{"$f":"IF(H163=\"\",\"\",INDEX('Lighting Assumptions 90.1-2010'!$N$54:$N$67,MATCH('6b - General Lighting'!W163,'Lighting Assumptions 90.1-2010'!$L$54:$L$67,0)))","v":""},"",{"$f":"IFERROR(IF(H163=\"\",\"\",AB163),\"\")","v":""},0,0,false]
["G","Parking near 24-hour retail entrances",null,null,null,"Main Entries",null,null,{"$f":"IF(SI_IP_Units=\"IP\",'Lighting Assumptions'!N51,'Lighting Assumptions'!O51)","v":800},{"$f":"IFERROR(IF(H164=\"\",\"\",H164*I164),\"\")","v":""},null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IF(AND(X164=\"\",Y164=\"\"),\"\",\"LPD-\"&X164&\", \"&Y164&\" Watts\"),IF(AND(AA164=\"\",AB164=\"\"),\"\",\"LPD-\"&AA164&\", \"&AB164&\" Watts\")))","v":""},null,null,{"$f":"SI_IP_Units&'6b - General Lighting'!B164","v":"IPParking near 24-hour retail entrances"},{"$f":"IF(H164=\"\",\"\",INDEX('Lighting Assumptions 90.1-2013'!$N$54:$N$67,MATCH('6b - General Lighting'!W164,'Lighting Assumptions 90.1-2013'!$L$54:$L$67,0)))","v":""},"",0,{"$f":"IF(H164=\"\",\"\",INDEX('Lighting Assumptions 90.1-2010'!$N$54:$N$67,MATCH('6b - General Lighting'!W164,'Lighting Assumptions 90.1-2010'!$L$54:$L$67,0)))","v":""},"",{"$f":"IFERROR(AB164+0,0)","v":0},0,0,false]
["G","Total nontradable surface lighting allowance",null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(AD159:AD164),\"\")","v":0},null,null,{"$f":"IFERROR(SUM(M159:M164),\"\")","v":0},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(SUM(Z159:Z164),\"\"),IFERROR(SUM(AC159:AC164),\"\")))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"SUM(AD159:AD164)+$M$135","v":0},{"$f":"SUM(AE159:AE164)","v":0},{"$f":"IF(AE165>AD165,TRUE,FALSE)","v":false},"value is True if the base allowance plus adjusted baseline is less than proposed"]
["G"]
["G","Table 6.6: Summary"]
["G","Input Parameter",null,null,null,null,null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,"Proposed Design",null,null,null,null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2013,\"In accordance with Prescriptive Requirements of 90.1-2013 Table 9.6.1\",\"In accordance with Prescriptive Requirements of 90.1-2010 Table 9.6.1\")","v":"In accordance with Prescriptive Requirements of 90.1-2013 Table 9.6.1"}]
[]
[null,"Index",null,null,null,null,null,null,null,"Base",null,null,"Design"]
["G","Total modeled exterior lighting power, including base allowance, based on inputs above (kW)",null,null,null,null,null,null,null,{"$f":"IFERROR(($J$149+$J$165+$M$135)/1000,0)","v":0},null,null,{"$f":"IFERROR(($M$149+$M$165)/1000,0)","v":0},null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IFERROR(($T$149+$T$165)/1000,0))","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M172>J172,TRUE,FALSE)","v":false}]
["G"]
["G","Additional notes:"]
["G"]

{"sheet":"Lighting Assumptions","index":17,"n_rows":550,"n_cols":15,"rows_kept":550,"cut":false,"hidden":true,"merged":[[42,11,43,11],[42,12,43,12],[0,3,1,3],[0,6,1,6],[0,7,0,8],[0,12,1,12],[0,11,1,11],[0,4,0,5]]}
[null,null,null,"Building Area Method Categories","Table G3.7 LPD",null,"Space by Space Categories","TableG3.7\nLPD ",null,"Table G3.7 per addendum bw",null,"Tradable Surfaces","Required Input","W/sf or W/linear foot","W/sm or W/linear meter"]
[null,null,null,null,"(W/sq ft)","(W/sq m)",null,"(W/sq ft)","(W/sq m)","occupancy sensor reduction",null,null,null,"IP","SI"]
[1,{"$f":"IF('6a - Lighting Counts'!G29=\"\",\"\",'6a - Lighting Counts'!G29)","v":""},{"$f":"IFERROR(VLOOKUP(ROW()-2,$A$3:$B$550,2,FALSE),\"\")","v":""},"Automotive facility",0.9,{"$f":"E3*10.7639","v":9.6875099999999996},"Audience Seating/Auditorium",0.9,{"$f":"H3*10.7639","v":9.6875099999999996},0.1,null,null,null,{"$f":"N1&\" \"&N2","v":"W/sf or W/linear foot IP"},{"$f":"O1&\" \"&O2","v":"W/sm or W/linear meter SI"}]
[{"$f":"IF(COUNTIF($B$3:B4,B4)=1,A3+1,A3)","v":1},{"$f":"IF('6a - Lighting Counts'!G30=\"\",\"\",'6a - Lighting Counts'!G30)","v":""},{"$f":"IFERROR(VLOOKUP(ROW()-2,$A$3:$B$550,2,FALSE),\"\")","v":""},"Convention center",1.2,{"$f":"E4*10.7639","v":12.916679999999999},"Audience Seating/Convention center",0.7,{"$f":"H4*10.7639","v":7.5347299999999988},0.1,null,"Parking lots and drives","Area",0.15,1.6]
[{"$f":"IF(COUNTIF($B$3:B5,B5)=1,A4+1,A4)","v":1},{"$f":"IF('6a - Lighting Counts'!G31=\"\",\"\",'6a - Lighting Counts'!G31)","v":""},"","Courthouse",1.2,12.916679999999999,"Audience Seating/Gymnasium",0.4,4.3055599999999998,0.1,null,"Walkways less than 10 ft wide","Length",1,3.3]
[{"$f":"IF(COUNTIF($B$3:B6,B6)=1,A5+1,A5)","v":1},{"$f":"IF('6a - Lighting Counts'!G32=\"\",\"\",'6a - Lighting Counts'!G32)","v":""},"","Dining: bar lounge/leisure",1.3,13.993069999999999,"Audience Seating/Motion Picture Theatre",1.2,12.916679999999999,0.1,null,"Walkways 10 ft wide or greater","Area",1,3.3]
[{"$f":"IF(COUNTIF($B$3:B7,B7)=1,A6+1,A6)","v":1},{"$f":"IF('6a - Lighting Counts'!G33=\"\",\"\",'6a - Lighting Counts'!G33)","v":""},"","Dining: cafeteria/fast food",1.4,15.069459999999998,"Audience Seating/Penitentiary",0.7,7.5347299999999988,0.1,null,"Plaza areas","Area",0.2,2.2000000000000002]
[{"$f":"IF(COUNTIF($B$3:B8,B8)=1,A7+1,A7)","v":1},{"$f":"IF('6a - Lighting Counts'!G34=\"\",\"\",'6a - Lighting Counts'!G34)","v":""},"","Dining: family",1.6,17.222239999999999,"Audience Seating/Performing Arts Theater",2.6,27.986139999999999,0.1,null,"Special feature areas","Area",0.2,2.2000000000000002]
[{"$f":"IF(COUNTIF($B$3:B9,B9)=1,A8+1,A8)","v":1},{"$f":"IF('6a - Lighting Counts'!G35=\"\",\"\",'6a - Lighting Counts'!G35)","v":""},"","Dormitory",1,10.7639,"Audience Seating/Religious Building",1.7,18.298629999999999,0.1,null,"Stairways","Area",1,10.8]
[{"$f":"IF(COUNTIF($B$3:B10,B10)=1,A9+1,A9)","v":1},{"$f":"IF('6a - Lighting Counts'!G36=\"\",\"\",'6a - Lighting Counts'!G36)","v":""},"","Exercise center",1,10.7639,"Audience Seating/Sports Arena",0.4,4.3055599999999998,0.1,null,"Main entries","Length",30,98]
[{"$f":"IF(COUNTIF($B$3:B11,B11)=1,A10+1,A10)","v":1},{"$f":"IF('6a - Lighting Counts'!G37=\"\",\"\",'6a - Lighting Counts'!G37)","v":""},"","Fire Station",1,10.7639,"Audience Seating/Transportation facility",0.5,5.3819499999999998,0.1,null,"Other doors","Length",20,66]
[{"$f":"IF(COUNTIF($B$3:B12,B12)=1,A11+1,A11)","v":1},{"$f":"IF('6a - Lighting Counts'!G38=\"\",\"\",'6a - Lighting Counts'!G38)","v":""},"","Gymnasium",1.1000000000000001,11.840290000000001,"Audience Seating/All Other",0.9,9.6875099999999996,0.1,null,"Canopies (free standing and attached and overhangs)","Area",1.25,13.5]
[{"$f":"IF(COUNTIF($B$3:B13,B13)=1,A12+1,A12)","v":1},{"$f":"IF('6a - Lighting Counts'!G39=\"\",\"\",'6a - Lighting Counts'!G39)","v":""},"","Health-care clinic",1,10.7639,"Atrium ≤40 ft high","<enter value>","<enter value>",0.1,null,"Outdoor Sales Open areas (including vehicle sales lots)","Area",0.5,5.4]
[{"$f":"IF(COUNTIF($B$3:B14,B14)=1,A13+1,A13)","v":1},{"$f":"IF('6a - Lighting Counts'!G40=\"\",\"\",'6a - Lighting Counts'!G40)","v":""},"","Hospital",1.2,12.916679999999999,"Atrium >40 ft high","<enter value>","<enter value>",0.1,null,"Outdoor Sales Street frontage for vehicle sales lots in addition to open-area allowance)","Length",20,66]
[{"$f":"IF(COUNTIF($B$3:B15,B15)=1,A14+1,A14)","v":1},{"$f":"IF('6a - Lighting Counts'!G41=\"\",\"\",'6a - Lighting Counts'!G41)","v":""},"","Hotel/motel",1.0900000000000001,11.732651000000001,"Banking Activity Area",1.5,16.145849999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B16,B16)=1,A15+1,A15)","v":1},{"$f":"IF('6a - Lighting Counts'!G42=\"\",\"\",'6a - Lighting Counts'!G42)","v":""},"","Library",1.3,13.993069999999999,"Classroom/Lecture Hall/Training Room in Penitentiary",1.3,13.993069999999999,0,null,"IPParking lots and drives",null,{"$f":"N4","v":0.15}]
[{"$f":"IF(COUNTIF($B$3:B17,B17)=1,A16+1,A16)","v":1},{"$f":"IF('6a - Lighting Counts'!G43=\"\",\"\",'6a - Lighting Counts'!G43)","v":""},"","Manufacturing facility",1.17,12.593762999999999,"Classroom/Lecture Hall/Training Room in All Other",1.4,15.069459999999998,0.3,null,"IPWalkways less than 10 ft wide",null,{"$f":"N5","v":1}]
[{"$f":"IF(COUNTIF($B$3:B18,B18)=1,A17+1,A17)","v":1},{"$f":"IF('6a - Lighting Counts'!G44=\"\",\"\",'6a - Lighting Counts'!G44)","v":""},"","Motion picture theater",1.2,12.916679999999999,"Conference/Meeting/Multipurpose Room",1.3,13.993069999999999,0,null,"IPWalkways 10 ft wide or greater",null,1]
[{"$f":"IF(COUNTIF($B$3:B19,B19)=1,A18+1,A18)","v":1},{"$f":"IF('6a - Lighting Counts'!G45=\"\",\"\",'6a - Lighting Counts'!G45)","v":""},"","Multifamily",0.7,7.5347299999999988,"Confinement Cells",0.9,9.6875099999999996,0,null,"IPPlaza areas",null,0.2]
[{"$f":"IF(COUNTIF($B$3:B20,B20)=1,A19+1,A19)","v":1},{"$f":"IF('6a - Lighting Counts'!G46=\"\",\"\",'6a - Lighting Counts'!G46)","v":""},"","Museum",1.1000000000000001,11.840290000000001,"Copy/Print Room",0.9,9.6875099999999996,0.1,null,"IPSpecial feature areas",null,0.2]
[{"$f":"IF(COUNTIF($B$3:B21,B21)=1,A20+1,A20)","v":1},{"$f":"IF('6a - Lighting Counts'!G47=\"\",\"\",'6a - Lighting Counts'!G47)","v":""},"","Office",1,10.7639,"Corridor/Facility for Visually Impaired",1.1499999999999999,12.378484999999998,0.25,null,"IPStairways",null,1]
[{"$f":"IF(COUNTIF($B$3:B22,B22)=1,A21+1,A21)","v":1},{"$f":"IF('6a - Lighting Counts'!G48=\"\",\"\",'6a - Lighting Counts'!G48)","v":""},"","Parking garage",0.3,3.2291699999999999,"Corridor/Hospital",1,10.7639,0.25,null,"IPMain entries",null,30]
[{"$f":"IF(COUNTIF($B$3:B23,B23)=1,A22+1,A22)","v":1},{"$f":"IF('6a - Lighting Counts'!G49=\"\",\"\",'6a - Lighting Counts'!G49)","v":""},"","Penitentiary",1,10.7639,"Corridor/Manufacturing Facility",0.5,5.3819499999999998,0.25,null,"IPOther doors",null,20]
[{"$f":"IF(COUNTIF($B$3:B24,B24)=1,A23+1,A23)","v":1},{"$f":"IF('6a - Lighting Counts'!G50=\"\",\"\",'6a - Lighting Counts'!G50)","v":""},"","Performing arts theater",1.6,17.222239999999999,"Corridor/All Other",{"$f":"IF(RatingSystemSelection=\"ENERGY STAR MFHR\",0.83,0.5)","v":0.83},8.934037,0.25,null,"IPCanopies (free standing and attached and overhangs)",null,1.25]
[{"$f":"IF(COUNTIF($B$3:B25,B25)=1,A24+1,A24)","v":1},{"$f":"IF('6a - Lighting Counts'!G51=\"\",\"\",'6a - Lighting Counts'!G51)","v":""},"","Police station",1,10.7639,"Courtroom",1.9,20.451409999999999,0.1,null,"IPOutdoor Sales Open areas (including vehicle sales lots)",null,0.5]
[{"$f":"IF(COUNTIF($B$3:B26,B26)=1,A25+1,A25)","v":1},{"$f":"IF('6a - Lighting Counts'!G52=\"\",\"\",'6a - Lighting Counts'!G52)","v":""},"","Post office",1.1000000000000001,11.840290000000001,"Computer Room",2.14,23.034746000000002,0.35,null,"IPOutdoor Sales Street frontage for vehicle sales lots in addition to open-area allowance)",null,20]
[{"$f":"IF(COUNTIF($B$3:B27,B27)=1,A26+1,A26)","v":1},{"$f":"IF('6a - Lighting Counts'!G53=\"\",\"\",'6a - Lighting Counts'!G53)","v":""},"","Religious building",1.3,13.993069999999999,"Dining Area/Penitentiary",1.3,13.993069999999999,0.35,null,"SIParking lots and drives",null,{"$f":"O4","v":1.6}]
[{"$f":"IF(COUNTIF($B$3:B28,B28)=1,A27+1,A27)","v":1},{"$f":"IF('6a - Lighting Counts'!G54=\"\",\"\",'6a - Lighting Counts'!G54)","v":""},"","Retail",1.5,16.145849999999999,"Dining Area/Facility for Visually Impaired",3.32,35.736148,0.35,null,"SIWalkways less than 10 ft wide",null,3.3]
[{"$f":"IF(COUNTIF($B$3:B29,B29)=1,A28+1,A28)","v":1},{"$f":"IF('6a - Lighting Counts'!G55=\"\",\"\",'6a - Lighting Counts'!G55)","v":""},"","School/university",1.2,12.916679999999999,"Dining Area/bar/Lounge or Leisure Dining",1.4,15.069459999999998,0.35,null,"SIWalkways 10 ft wide or greater",null,3.3]
[{"$f":"IF(COUNTIF($B$3:B30,B30)=1,A29+1,A29)","v":1},{"$f":"IF('6a - Lighting Counts'!G56=\"\",\"\",'6a - Lighting Counts'!G56)","v":""},"","Sports arena",1.1000000000000001,11.840290000000001,"Dining Area/Cafeteria/Fast Food",0.9,9.6875099999999996,0.35,null,"SIPlaza areas",null,3.3]
[{"$f":"IF(COUNTIF($B$3:B31,B31)=1,A30+1,A30)","v":1},{"$f":"IF('6a - Lighting Counts'!G57=\"\",\"\",'6a - Lighting Counts'!G57)","v":""},"","Town hall",1.1000000000000001,11.840290000000001,"Dining Area/Family Dining",2.1,22.604189999999999,0.35,null,"SISpecial feature areas",null,3.3]
[{"$f":"IF(COUNTIF($B$3:B32,B32)=1,A31+1,A31)","v":1},{"$f":"IF('6a - Lighting Counts'!G58=\"\",\"\",'6a - Lighting Counts'!G58)","v":""},"","Transportation",1,10.7639,"Dining Area/All Other",0.9,9.6875099999999996,0.35,null,"SIStairways",null,3.3]
[{"$f":"IF(COUNTIF($B$3:B33,B33)=1,A32+1,A32)","v":1},{"$f":"IF('6a - Lighting Counts'!G59=\"\",\"\",'6a - Lighting Counts'!G59)","v":""},"","Warehouse",0.8,8.6111199999999997,"Electrical/Mechanical Room",1.5,16.145849999999999,0.3,null,"SIMain entries",null,3.3]
[{"$f":"IF(COUNTIF($B$3:B34,B34)=1,A33+1,A33)","v":1},{"$f":"IF('6a - Lighting Counts'!G60=\"\",\"\",'6a - Lighting Counts'!G60)","v":""},"","Workshop",1.4,15.069459999999998,"Emergency Vehicle Garage",0.8,8.6111199999999997,0.1,null,"SIOther doors",null,3.3]
[{"$f":"IF(COUNTIF($B$3:B35,B35)=1,A34+1,A34)","v":1},{"$f":"IF('6a - Lighting Counts'!G61=\"\",\"\",'6a - Lighting Counts'!G61)","v":""},"",null,null,null,"Food Preparation Area",1.2,12.916679999999999,0.1,null,"SICanopies (free standing and attached and overhangs)",null,3.3]
[{"$f":"IF(COUNTIF($B$3:B36,B36)=1,A35+1,A35)","v":1},{"$f":"IF('6a - Lighting Counts'!G62=\"\",\"\",'6a - Lighting Counts'!G62)","v":""},"",null,null,null,"Guest Room",1.1000000000000001,11.840290000000001,0.45,null,"SIOutdoor Sales Open areas (including vehicle sales lots)",null,3.3]
[{"$f":"IF(COUNTIF($B$3:B37,B37)=1,A36+1,A36)","v":1},{"$f":"IF('6a - Lighting Counts'!G63=\"\",\"\",'6a - Lighting Counts'!G63)","v":""},"",null,null,null,"Judges Chambers",1.3,13.993069999999999,0.3,null,"SIOutdoor Sales Street frontage for vehicle sales lots in addition to open-area allowance)",null,3.3]
[{"$f":"IF(COUNTIF($B$3:B38,B38)=1,A37+1,A37)","v":1},{"$f":"IF('6a - Lighting Counts'!G64=\"\",\"\",'6a - Lighting Counts'!G64)","v":""},"",null,null,null,"Laboratory/Classroom",1.4,15.069459999999998,0]
[{"$f":"IF(COUNTIF($B$3:B39,B39)=1,A38+1,A38)","v":1},{"$f":"IF('6a - Lighting Counts'!G65=\"\",\"\",'6a - Lighting Counts'!G65)","v":""},"",null,null,null,"Laboratory/All Other",1.4,15.069459999999998,0.1]
[{"$f":"IF(COUNTIF($B$3:B40,B40)=1,A39+1,A39)","v":1},{"$f":"IF('6a - Lighting Counts'!G66=\"\",\"\",'6a - Lighting Counts'!G66)","v":""},"",null,null,null,"Laundry/Washing Area",0.6,6.4583399999999997,0.1]
[{"$f":"IF(COUNTIF($B$3:B41,B41)=1,A40+1,A40)","v":1},{"$f":"IF('6a - Lighting Counts'!G67=\"\",\"\",'6a - Lighting Counts'!G67)","v":""},"",null,null,null,"Loading Dock, Interior",0.59,6.350700999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B42,B42)=1,A41+1,A41)","v":1},{"$f":"IF('6a - Lighting Counts'!G68=\"\",\"\",'6a - Lighting Counts'!G68)","v":""},"",null,null,null,"Lobby/Facility for Visually Impaired",2.2599999999999998,24.326413999999996,0.25]
[{"$f":"IF(COUNTIF($B$3:B43,B43)=1,A42+1,A42)","v":1},{"$f":"IF('6a - Lighting Counts'!G69=\"\",\"\",'6a - Lighting Counts'!G69)","v":""},"",null,null,null,"Lobby/Elevator",0.8,8.6111199999999997,0.25,null,"Nontradable Surfaces","Required Input","W/sf or W/linear foot","W/sm or W/linear meter"]
[{"$f":"IF(COUNTIF($B$3:B44,B44)=1,A43+1,A43)","v":1},{"$f":"IF('6a - Lighting Counts'!G70=\"\",\"\",'6a - Lighting Counts'!G70)","v":""},"",null,null,null,"Lobby/Hotel",1.1000000000000001,11.840290000000001,0.25,null,null,null,"IP","SI"]
[{"$f":"IF(COUNTIF($B$3:B45,B45)=1,A44+1,A44)","v":1},{"$f":"IF('6a - Lighting Counts'!G71=\"\",\"\",'6a - Lighting Counts'!G71)","v":""},"",null,null,null,"Lobby/Motion Picture Theater",1.1000000000000001,11.840290000000001,0.25,null,null,null,{"$f":"N43&\" \"&N44","v":"W/sf or W/linear foot IP"},{"$f":"O43&\" \"&O44","v":"W/sm or W/linear meter SI"}]
[{"$f":"IF(COUNTIF($B$3:B46,B46)=1,A45+1,A45)","v":1},{"$f":"IF('6a - Lighting Counts'!G72=\"\",\"\",'6a - Lighting Counts'!G72)","v":""},"",null,null,null,"Lobby/Performing Arts Theater",3.3,35.520869999999995,0.25,null,"Building Facades","Area",0.2,2.2000000000000002]
[{"$f":"IF(COUNTIF($B$3:B47,B47)=1,A46+1,A46)","v":1},{"$f":"IF('6a - Lighting Counts'!G73=\"\",\"\",'6a - Lighting Counts'!G73)","v":""},"",null,null,null,"Lobby/All Other",1.3,13.993069999999999,0.25,null,"Automated teller machines (ATMs) and night depositories","Length","270 W+90 per additional","270 W+90 per additional"]
[{"$f":"IF(COUNTIF($B$3:B48,B48)=1,A47+1,A47)","v":1},{"$f":"IF('6a - Lighting Counts'!G74=\"\",\"\",'6a - Lighting Counts'!G74)","v":""},"",null,null,null,"Locker Room",0.6,6.4583399999999997,0.25,null,"Entrance and gatehouse inspection stations at guarded facilities","Area",1.25,13.5]
[{"$f":"IF(COUNTIF($B$3:B49,B49)=1,A48+1,A48)","v":1},{"$f":"IF('6a - Lighting Counts'!G75=\"\",\"\",'6a - Lighting Counts'!G75)","v":""},"",null,null,null,"Lounge/Breakroom/in Healthcare Facility",0.8,8.6111199999999997,0,null,"Loading areas for law enforcement, fire, ambulance and other emergency service vehicles","Area",0.5,5.4]
[{"$f":"IF(COUNTIF($B$3:B50,B50)=1,A49+1,A49)","v":1},{"$f":"IF('6a - Lighting Counts'!G76=\"\",\"\",'6a - Lighting Counts'!G76)","v":""},"",null,null,null,"Lounge/Breakroom/All Other",1.2,12.916679999999999,0,null,"Drive-up windows at fast food restaurants","Length",400,400]
[{"$f":"IF(COUNTIF($B$3:B51,B51)=1,A50+1,A50)","v":1},{"$f":"IF('6a - Lighting Counts'!G77=\"\",\"\",'6a - Lighting Counts'!G77)","v":""},"",null,null,null,"Office/Enclosed",1.1000000000000001,11.840290000000001,0.3,null,"Parking near 24-hour retail entrances","Length",800,800]
[{"$f":"IF(COUNTIF($B$3:B52,B52)=1,A51+1,A51)","v":1},{"$f":"IF('6a - Lighting Counts'!G78=\"\",\"\",'6a - Lighting Counts'!G78)","v":""},"",null,null,null,"Office/Open Plan",1.1000000000000001,11.840290000000001,0.15,null,"Building Facades","Length",5,5]
[{"$f":"IF(COUNTIF($B$3:B53,B53)=1,A52+1,A52)","v":1},{"$f":"IF('6a - Lighting Counts'!G79=\"\",\"\",'6a - Lighting Counts'!G79)","v":""},"",null,null,null,"Parking Area, Interior",0.2,2.1527799999999999,0.15]
[{"$f":"IF(COUNTIF($B$3:B54,B54)=1,A53+1,A53)","v":1},{"$f":"IF('6a - Lighting Counts'!G80=\"\",\"\",'6a - Lighting Counts'!G80)","v":""},"",null,null,null,"Pharmacy Area",1.2,12.916679999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B55,B55)=1,A54+1,A54)","v":1},{"$f":"IF('6a - Lighting Counts'!G81=\"\",\"\",'6a - Lighting Counts'!G81)","v":""},"",null,null,null,"Restroom/Facility for the Visually Impaired",1.52,16.361128000000001,0.45]
[{"$f":"IF(COUNTIF($B$3:B56,B56)=1,A55+1,A55)","v":1},{"$f":"IF('6a - Lighting Counts'!G82=\"\",\"\",'6a - Lighting Counts'!G82)","v":""},"",null,null,null,"Restroom/ All Other",0.9,9.6875099999999996,0.45]
[{"$f":"IF(COUNTIF($B$3:B57,B57)=1,A56+1,A56)","v":1},{"$f":"IF('6a - Lighting Counts'!G83=\"\",\"\",'6a - Lighting Counts'!G83)","v":""},"",null,null,null,"Sales Area",1.7,18.298629999999999,0.15]
[{"$f":"IF(COUNTIF($B$3:B58,B58)=1,A57+1,A57)","v":1},{"$f":"IF('6a - Lighting Counts'!G84=\"\",\"\",'6a - Lighting Counts'!G84)","v":""},"",null,null,null,"Seating Area, General",0.68,7.3194520000000001,0.1]
[{"$f":"IF(COUNTIF($B$3:B59,B59)=1,A58+1,A58)","v":1},{"$f":"IF('6a - Lighting Counts'!G85=\"\",\"\",'6a - Lighting Counts'!G85)","v":""},"",null,null,null,"Stairwell",0.6,6.4583399999999997,0.75]
[{"$f":"IF(COUNTIF($B$3:B60,B60)=1,A59+1,A59)","v":1},{"$f":"IF('6a - Lighting Counts'!G86=\"\",\"\",'6a - Lighting Counts'!G86)","v":""},"",null,null,null,"Storage Room/Hospital",0.9,9.6875099999999996,0.45]
[{"$f":"IF(COUNTIF($B$3:B61,B61)=1,A60+1,A60)","v":1},{"$f":"IF('6a - Lighting Counts'!G87=\"\",\"\",'6a - Lighting Counts'!G87)","v":""},"",null,null,null,"Storage Room/≥50 sqft",0.8,8.6111199999999997,0.45]
[{"$f":"IF(COUNTIF($B$3:B62,B62)=1,A61+1,A61)","v":1},{"$f":"IF('6a - Lighting Counts'!G88=\"\",\"\",'6a - Lighting Counts'!G88)","v":""},"",null,null,null,"Storage Room/<50 sgft",0.8,8.6111199999999997,0.45]
[{"$f":"IF(COUNTIF($B$3:B63,B63)=1,A62+1,A62)","v":1},{"$f":"IF('6a - Lighting Counts'!G89=\"\",\"\",'6a - Lighting Counts'!G89)","v":""},"",null,null,null,"Vehicular Maintenance Area",0.7,7.5347299999999988,0.1]
[{"$f":"IF(COUNTIF($B$3:B64,B64)=1,A63+1,A63)","v":1},{"$f":"IF('6a - Lighting Counts'!G90=\"\",\"\",'6a - Lighting Counts'!G90)","v":""},"",null,null,null,"Workshop",1.9,20.451409999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B65,B65)=1,A64+1,A64)","v":1},{"$f":"IF('6a - Lighting Counts'!G91=\"\",\"\",'6a - Lighting Counts'!G91)","v":""},"",null,null,null,"Assisted Living Facility/Chapel",2.77,29.816002999999998,0.1]
[{"$f":"IF(COUNTIF($B$3:B66,B66)=1,A65+1,A65)","v":1},{"$f":"IF('6a - Lighting Counts'!G92=\"\",\"\",'6a - Lighting Counts'!G92)","v":""},"",null,null,null,"Assisted Living Facility/Recreation Room",3.02,32.506977999999997,0.1]
[{"$f":"IF(COUNTIF($B$3:B67,B67)=1,A66+1,A66)","v":1},{"$f":"IF('6a - Lighting Counts'!G93=\"\",\"\",'6a - Lighting Counts'!G93)","v":""},"",null,null,null,"Convention Center-Exhibit Space",1.3,13.993069999999999,0.35]
[{"$f":"IF(COUNTIF($B$3:B68,B68)=1,A67+1,A67)","v":1},{"$f":"IF('6a - Lighting Counts'!G94=\"\",\"\",'6a - Lighting Counts'!G94)","v":""},{"$f":"IFERROR(VLOOKUP(ROW()-2,$A$3:$B$550,2,FALSE),\"\")","v":""},null,null,null,"Dormitory-Living Quarters",1.1100000000000001,{"$f":"H68*10.7639","v":11.947929},0.1]
[{"$f":"IF(COUNTIF($B$3:B69,B69)=1,A68+1,A68)","v":1},{"$f":"IF('6a - Lighting Counts'!G95=\"\",\"\",'6a - Lighting Counts'!G95)","v":""},"",null,null,null,"Fire Station-Sleeping Quarters",0.3,3.2291699999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B70,B70)=1,A69+1,A69)","v":1},{"$f":"IF('6a - Lighting Counts'!G96=\"\",\"\",'6a - Lighting Counts'!G96)","v":""},"",null,null,null,"Gymnasium/Fitness Center/Exercise Area",0.9,9.6875099999999996,0.35]
[{"$f":"IF(COUNTIF($B$3:B71,B71)=1,A70+1,A70)","v":1},{"$f":"IF('6a - Lighting Counts'!G97=\"\",\"\",'6a - Lighting Counts'!G97)","v":""},"",null,null,null,"Gymnasium/Fitness Center/Playing Area",1.4,15.069459999999998,0.35]
[{"$f":"IF(COUNTIF($B$3:B72,B72)=1,A71+1,A71)","v":1},{"$f":"IF('6a - Lighting Counts'!G98=\"\",\"\",'6a - Lighting Counts'!G98)","v":""},"",null,null,null,"Healthcare Facility/Emergency Room",2.7,29.062530000000002,0.1]
[{"$f":"IF(COUNTIF($B$3:B73,B73)=1,A72+1,A72)","v":1},{"$f":"IF('6a - Lighting Counts'!G99=\"\",\"\",'6a - Lighting Counts'!G99)","v":""},"",null,null,null,"Healthcare Facility/Exam/Treatment Room",1.5,16.145849999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B74,B74)=1,A73+1,A73)","v":1},{"$f":"IF('6a - Lighting Counts'!G100=\"\",\"\",'6a - Lighting Counts'!G100)","v":""},"",null,null,null,"Healthcare Facility/Imaging Room",0.4,4.3055599999999998,0.22]
[{"$f":"IF(COUNTIF($B$3:B75,B75)=1,A74+1,A74)","v":1},{"$f":"IF('6a - Lighting Counts'!G101=\"\",\"\",'6a - Lighting Counts'!G101)","v":""},"",null,null,null,"Healthcare Facility/Medical Supply Room",1.4,15.069459999999998,0.45]
[{"$f":"IF(COUNTIF($B$3:B76,B76)=1,A75+1,A75)","v":1},{"$f":"IF('6a - Lighting Counts'!G102=\"\",\"\",'6a - Lighting Counts'!G102)","v":""},"",null,null,null,"Healthcare Facility/Nursery",0.6,6.4583399999999997,0.1]
[{"$f":"IF(COUNTIF($B$3:B77,B77)=1,A76+1,A76)","v":1},{"$f":"IF('6a - Lighting Counts'!G103=\"\",\"\",'6a - Lighting Counts'!G103)","v":""},"",null,null,null,"Healthcare Facility/Nurses Station",1,10.7639,0.1]
[{"$f":"IF(COUNTIF($B$3:B78,B78)=1,A77+1,A77)","v":1},{"$f":"IF('6a - Lighting Counts'!G104=\"\",\"\",'6a - Lighting Counts'!G104)","v":""},"",null,null,null,"Healthcare Facility/Operating Room",2.2000000000000002,23.680580000000003,0.1]
[{"$f":"IF(COUNTIF($B$3:B79,B79)=1,A78+1,A78)","v":1},{"$f":"IF('6a - Lighting Counts'!G105=\"\",\"\",'6a - Lighting Counts'!G105)","v":""},"",null,null,null,"Healthcare Facility/Patient Room",0.7,7.5347299999999988,0.1]
[{"$f":"IF(COUNTIF($B$3:B80,B80)=1,A79+1,A79)","v":1},{"$f":"IF('6a - Lighting Counts'!G106=\"\",\"\",'6a - Lighting Counts'!G106)","v":""},"",null,null,null,"Healthcare Facility/Physical Therapy Room",0.9,9.6875099999999996,0.1]
[{"$f":"IF(COUNTIF($B$3:B81,B81)=1,A80+1,A80)","v":1},{"$f":"IF('6a - Lighting Counts'!G107=\"\",\"\",'6a - Lighting Counts'!G107)","v":""},"",null,null,null,"Healthcare Facility/Recovery Room",0.8,8.6111199999999997,0.1]
[{"$f":"IF(COUNTIF($B$3:B82,B82)=1,A81+1,A81)","v":1},{"$f":"IF('6a - Lighting Counts'!G108=\"\",\"\",'6a - Lighting Counts'!G108)","v":""},"",null,null,null,"Library/Reading Area",1.2,12.916679999999999,0.15]
[{"$f":"IF(COUNTIF($B$3:B83,B83)=1,A82+1,A82)","v":1},{"$f":"IF('6a - Lighting Counts'!G109=\"\",\"\",'6a - Lighting Counts'!G109)","v":""},"",null,null,null,"Library/Stacks",1.7,18.298629999999999,0.15]
[{"$f":"IF(COUNTIF($B$3:B84,B84)=1,A83+1,A83)","v":1},{"$f":"IF('6a - Lighting Counts'!G110=\"\",\"\",'6a - Lighting Counts'!G110)","v":""},"",null,null,null,"Manufacturing Facility/Detailed Manufacturing Area",2.1,22.604189999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B85,B85)=1,A84+1,A84)","v":1},{"$f":"IF('6a - Lighting Counts'!G111=\"\",\"\",'6a - Lighting Counts'!G111)","v":""},"",null,null,null,"Manufacturing Facility/Equipment Room",1.2,12.916679999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B86,B86)=1,A85+1,A85)","v":1},{"$f":"IF('6a - Lighting Counts'!G112=\"\",\"\",'6a - Lighting Counts'!G112)","v":""},"",null,null,null,"Manufacturing Facility/Extra High Bay Area (>50 ft floor-to-ceiling height)",1.32,14.208348000000001,0.1]
[{"$f":"IF(COUNTIF($B$3:B87,B87)=1,A86+1,A86)","v":1},{"$f":"IF('6a - Lighting Counts'!G113=\"\",\"\",'6a - Lighting Counts'!G113)","v":""},"",null,null,null,"Manufacturing Facility/High Bay Area (25-50 ft floor-to-ceiling height)",1.7,18.298629999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B88,B88)=1,A87+1,A87)","v":1},{"$f":"IF('6a - Lighting Counts'!G114=\"\",\"\",'6a - Lighting Counts'!G114)","v":""},"",null,null,null,"Manufacturing Facility/Low Bay Area (<25 ft floor-to-ceiling height)",1.2,12.916679999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B89,B89)=1,A88+1,A88)","v":1},{"$f":"IF('6a - Lighting Counts'!G115=\"\",\"\",'6a - Lighting Counts'!G115)","v":""},"",null,null,null,"Museum/General Exhibition Area",1,10.7639,0.1]
[{"$f":"IF(COUNTIF($B$3:B90,B90)=1,A89+1,A89)","v":1},{"$f":"IF('6a - Lighting Counts'!G116=\"\",\"\",'6a - Lighting Counts'!G116)","v":""},"",null,null,null,"Museum/Restoration Room",1.7,18.298629999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B91,B91)=1,A90+1,A90)","v":1},{"$f":"IF('6a - Lighting Counts'!G117=\"\",\"\",'6a - Lighting Counts'!G117)","v":""},"",null,null,null,"Post Office/Sorting Area",1.2,12.916679999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B92,B92)=1,A91+1,A91)","v":1},{"$f":"IF('6a - Lighting Counts'!G118=\"\",\"\",'6a - Lighting Counts'!G118)","v":""},"",null,null,null,"Religious Building/Fellowship Hall",0.9,9.6875099999999996,0.1]
[{"$f":"IF(COUNTIF($B$3:B93,B93)=1,A92+1,A92)","v":1},{"$f":"IF('6a - Lighting Counts'!G119=\"\",\"\",'6a - Lighting Counts'!G119)","v":""},"",null,null,null,"Religious building/Worship/Choir area",2.4,25.833359999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B94,B94)=1,A93+1,A93)","v":1},{"$f":"IF('6a - Lighting Counts'!G120=\"\",\"\",'6a - Lighting Counts'!G120)","v":""},"",null,null,null,"Retail Facilities/Dressing/Fitting Room",0.89,9.5798709999999989,0.1]
[{"$f":"IF(COUNTIF($B$3:B95,B95)=1,A94+1,A94)","v":1},{"$f":"IF('6a - Lighting Counts'!G121=\"\",\"\",'6a - Lighting Counts'!G121)","v":""},"",null,null,null,"Retail Facilities/Mall Concourse",1.7,18.298629999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B96,B96)=1,A95+1,A95)","v":1},{"$f":"IF('6a - Lighting Counts'!G122=\"\",\"\",'6a - Lighting Counts'!G122)","v":""},"",null,null,null,"Sporting Arena-Playing Area/Class I Facility",4.6100000000000003,49.621579000000004,0.1]
[{"$f":"IF(COUNTIF($B$3:B97,B97)=1,A96+1,A96)","v":1},{"$f":"IF('6a - Lighting Counts'!G123=\"\",\"\",'6a - Lighting Counts'!G123)","v":""},"",null,null,null,"Sporting Arena-Playing Area/Class II Facility",3.01,32.399338999999998,0.1]
[{"$f":"IF(COUNTIF($B$3:B98,B98)=1,A97+1,A97)","v":1},{"$f":"IF('6a - Lighting Counts'!G124=\"\",\"\",'6a - Lighting Counts'!G124)","v":""},"",null,null,null,"Sporting Arena-Playing Area/Class III Facility",2.2599999999999998,24.326413999999996,0.1]
[{"$f":"IF(COUNTIF($B$3:B99,B99)=1,A98+1,A98)","v":1},{"$f":"IF('6a - Lighting Counts'!G125=\"\",\"\",'6a - Lighting Counts'!G125)","v":""},"",null,null,null,"Sporting Arena-Playing Area/Class IV Facility",1.5,16.145849999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B100,B100)=1,A99+1,A99)","v":1},{"$f":"IF('6a - Lighting Counts'!G126=\"\",\"\",'6a - Lighting Counts'!G126)","v":""},"",null,null,null,"Transportation Facility/Baggage/Carousel Area",1,10.7639,0.1]
[{"$f":"IF(COUNTIF($B$3:B101,B101)=1,A100+1,A100)","v":1},{"$f":"IF('6a - Lighting Counts'!G127=\"\",\"\",'6a - Lighting Counts'!G127)","v":""},"",null,null,null,"Transportation Facility/Airport Concourse",0.6,6.4583399999999997,0.1]
[{"$f":"IF(COUNTIF($B$3:B102,B102)=1,A101+1,A101)","v":1},{"$f":"IF('6a - Lighting Counts'!G128=\"\",\"\",'6a - Lighting Counts'!G128)","v":""},"",null,null,null,"Transportation Facility/Terminal Ticket Counter",1.5,16.145849999999999,0.1]
[{"$f":"IF(COUNTIF($B$3:B103,B103)=1,A102+1,A102)","v":1},{"$f":"IF('6a - Lighting Counts'!G129=\"\",\"\",'6a - Lighting Counts'!G129)","v":""},"",null,null,null,"Warehouse-Storage Area/Medium to Bulky, Palletized Items",0.9,9.6875099999999996,0.45]
[{"$f":"IF(COUNTIF($B$3:B104,B104)=1,A103+1,A103)","v":1},{"$f":"IF('6a - Lighting Counts'!G130=\"\",\"\",'6a - Lighting Counts'!G130)","v":""},"",null,null,null,"Warehouse-Storage Area/Smaller, Hand Carried Items",1.4,15.069459999999998,0.45]
[{"$f":"IF(COUNTIF($B$3:B105,B105)=1,A104+1,A104)","v":1},{"$f":"IF('6a - Lighting Counts'!G131=\"\",\"\",'6a - Lighting Counts'!G131)","v":""},"",null,null,null,"Dwelling Unit",1.1000000000000001,11.840290000000001,0]
[{"$f":"IF(COUNTIF($B$3:B106,B106)=1,A105+1,A105)","v":1},{"$f":"IF('6a - Lighting Counts'!G132=\"\",\"\",'6a - Lighting Counts'!G132)","v":""},"",null,null,"ENERGY STAR","Elevator (interior)",0.8,{"$f":"H106*10.7639","v":8.6111199999999997},0.25]
[{"$f":"IF(COUNTIF($B$3:B107,B107)=1,A106+1,A106)","v":1},{"$f":"IF('6a - Lighting Counts'!G133=\"\",\"\",'6a - Lighting Counts'!G133)","v":""},"",null,null,null,"Multiple","<enter value>","<enter value>","<enter value>"]
[{"$f":"IF(COUNTIF($B$3:B108,B108)=1,A107+1,A107)","v":1},{"$f":"IF('6a - Lighting Counts'!G134=\"\",\"\",'6a - Lighting Counts'!G134)","v":""},"",null,null,"ENERGY STAR","Exercise Room",0.9,{"$f":"H108*10.7639","v":9.6875099999999996},0.35]
[{"$f":"IF(COUNTIF($B$3:B109,B109)=1,A108+1,A108)","v":1},{"$f":"IF('6a - Lighting Counts'!G135=\"\",\"\",'6a - Lighting Counts'!G135)","v":""},"",null,null,"ENERGY STAR","Trash Chute/Room",0.8,{"$f":"H109*10.7639","v":8.6111199999999997},0.45]
[{"$f":"IF(COUNTIF($B$3:B110,B110)=1,A109+1,A109)","v":1},{"$f":"IF('6a - Lighting Counts'!G136=\"\",\"\",'6a - Lighting Counts'!G136)","v":""},"",null,null,"ENERGY STAR","Janitor Closet",0.8,{"$f":"H110*10.7639","v":8.6111199999999997},0.45]
[{"$f":"IF(COUNTIF($B$3:B111,B111)=1,A110+1,A110)","v":1},{"$f":"IF('6a - Lighting Counts'!G137=\"\",\"\",'6a - Lighting Counts'!G137)","v":""},"",null,null,"ENERGY STAR","Community Room",1.2,{"$f":"H111*10.7639","v":12.916679999999999},0]
[{"$f":"IF(COUNTIF($B$3:B112,B112)=1,A111+1,A111)","v":1},{"$f":"IF('6a - Lighting Counts'!G138=\"\",\"\",'6a - Lighting Counts'!G138)","v":""},"",null,null,"ENERGY STAR","Tenant Storage",0.8,{"$f":"H112*10.7639","v":8.6111199999999997},0.45]
[{"$f":"IF(COUNTIF($B$3:B113,B113)=1,A112+1,A112)","v":1},{"$f":"IF('6a - Lighting Counts'!G139=\"\",\"\",'6a - Lighting Counts'!G139)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B114,B114)=1,A113+1,A113)","v":1},{"$f":"IF('6a - Lighting Counts'!G140=\"\",\"\",'6a - Lighting Counts'!G140)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B115,B115)=1,A114+1,A114)","v":1},{"$f":"IF('6a - Lighting Counts'!G141=\"\",\"\",'6a - Lighting Counts'!G141)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B116,B116)=1,A115+1,A115)","v":1},{"$f":"IF('6a - Lighting Counts'!G142=\"\",\"\",'6a - Lighting Counts'!G142)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B117,B117)=1,A116+1,A116)","v":1},{"$f":"IF('6a - Lighting Counts'!G143=\"\",\"\",'6a - Lighting Counts'!G143)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B118,B118)=1,A117+1,A117)","v":1},{"$f":"IF('6a - Lighting Counts'!G144=\"\",\"\",'6a - Lighting Counts'!G144)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B119,B119)=1,A118+1,A118)","v":1},{"$f":"IF('6a - Lighting Counts'!G145=\"\",\"\",'6a - Lighting Counts'!G145)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B120,B120)=1,A119+1,A119)","v":1},{"$f":"IF('6a - Lighting Counts'!G146=\"\",\"\",'6a - Lighting Counts'!G146)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B121,B121)=1,A120+1,A120)","v":1},{"$f":"IF('6a - Lighting Counts'!G147=\"\",\"\",'6a - Lighting Counts'!G147)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B122,B122)=1,A121+1,A121)","v":1},{"$f":"IF('6a - Lighting Counts'!G148=\"\",\"\",'6a - Lighting Counts'!G148)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B123,B123)=1,A122+1,A122)","v":1},{"$f":"IF('6a - Lighting Counts'!G149=\"\",\"\",'6a - Lighting Counts'!G149)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B124,B124)=1,A123+1,A123)","v":1},{"$f":"IF('6a - Lighting Counts'!G150=\"\",\"\",'6a - Lighting Counts'!G150)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B125,B125)=1,A124+1,A124)","v":1},{"$f":"IF('6a - Lighting Counts'!G151=\"\",\"\",'6a - Lighting Counts'!G151)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B126,B126)=1,A125+1,A125)","v":1},{"$f":"IF('6a - Lighting Counts'!G152=\"\",\"\",'6a - Lighting Counts'!G152)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B127,B127)=1,A126+1,A126)","v":1},{"$f":"IF('6a - Lighting Counts'!G153=\"\",\"\",'6a - Lighting Counts'!G153)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B128,B128)=1,A127+1,A127)","v":1},{"$f":"IF('6a - Lighting Counts'!G154=\"\",\"\",'6a - Lighting Counts'!G154)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B129,B129)=1,A128+1,A128)","v":1},{"$f":"IF('6a - Lighting Counts'!G155=\"\",\"\",'6a - Lighting Counts'!G155)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B130,B130)=1,A129+1,A129)","v":1},{"$f":"IF('6a - Lighting Counts'!G156=\"\",\"\",'6a - Lighting Counts'!G156)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B131,B131)=1,A130+1,A130)","v":1},{"$f":"IF('6a - Lighting Counts'!G157=\"\",\"\",'6a - Lighting Counts'!G157)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B132,B132)=1,A131+1,A131)","v":1},{"$f":"IF('6a - Lighting Counts'!G158=\"\",\"\",'6a - Lighting Counts'!G158)","v":""},{"$f":"IFERROR(VLOOKUP(ROW()-2,$A$3:$B$550,2,FALSE),\"\")","v":""}]
[{"$f":"IF(COUNTIF($B$3:B133,B133)=1,A132+1,A132)","v":1},{"$f":"IF('6a - Lighting Counts'!G159=\"\",\"\",'6a - Lighting Counts'!G159)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B134,B134)=1,A133+1,A133)","v":1},{"$f":"IF('6a - Lighting Counts'!G160=\"\",\"\",'6a - Lighting Counts'!G160)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B135,B135)=1,A134+1,A134)","v":1},{"$f":"IF('6a - Lighting Counts'!G161=\"\",\"\",'6a - Lighting Counts'!G161)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B136,B136)=1,A135+1,A135)","v":1},{"$f":"IF('6a - Lighting Counts'!G162=\"\",\"\",'6a - Lighting Counts'!G162)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B137,B137)=1,A136+1,A136)","v":1},{"$f":"IF('6a - Lighting Counts'!G163=\"\",\"\",'6a - Lighting Counts'!G163)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B138,B138)=1,A137+1,A137)","v":1},{"$f":"IF('6a - Lighting Counts'!G164=\"\",\"\",'6a - Lighting Counts'!G164)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B139,B139)=1,A138+1,A138)","v":1},{"$f":"IF('6a - Lighting Counts'!G165=\"\",\"\",'6a - Lighting Counts'!G165)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B140,B140)=1,A139+1,A139)","v":1},{"$f":"IF('6a - Lighting Counts'!G166=\"\",\"\",'6a - Lighting Counts'!G166)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B141,B141)=1,A140+1,A140)","v":1},{"$f":"IF('6a - Lighting Counts'!G167=\"\",\"\",'6a - Lighting Counts'!G167)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B142,B142)=1,A141+1,A141)","v":1},{"$f":"IF('6a - Lighting Counts'!G168=\"\",\"\",'6a - Lighting Counts'!G168)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B143,B143)=1,A142+1,A142)","v":1},{"$f":"IF('6a - Lighting Counts'!G169=\"\",\"\",'6a - Lighting Counts'!G169)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B144,B144)=1,A143+1,A143)","v":1},{"$f":"IF('6a - Lighting Counts'!G170=\"\",\"\",'6a - Lighting Counts'!G170)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B145,B145)=1,A144+1,A144)","v":1},{"$f":"IF('6a - Lighting Counts'!G171=\"\",\"\",'6a - Lighting Counts'!G171)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B146,B146)=1,A145+1,A145)","v":1},{"$f":"IF('6a - Lighting Counts'!G172=\"\",\"\",'6a - Lighting Counts'!G172)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B147,B147)=1,A146+1,A146)","v":1},{"$f":"IF('6a - Lighting Counts'!G173=\"\",\"\",'6a - Lighting Counts'!G173)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B148,B148)=1,A147+1,A147)","v":1},{"$f":"IF('6a - Lighting Counts'!G174=\"\",\"\",'6a - Lighting Counts'!G174)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B149,B149)=1,A148+1,A148)","v":1},{"$f":"IF('6a - Lighting Counts'!G175=\"\",\"\",'6a - Lighting Counts'!G175)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B150,B150)=1,A149+1,A149)","v":1},{"$f":"IF('6a - Lighting Counts'!G176=\"\",\"\",'6a - Lighting Counts'!G176)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B151,B151)=1,A150+1,A150)","v":1},{"$f":"IF('6a - Lighting Counts'!G177=\"\",\"\",'6a - Lighting Counts'!G177)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B152,B152)=1,A151+1,A151)","v":1},{"$f":"IF('6a - Lighting Counts'!G178=\"\",\"\",'6a - Lighting Counts'!G178)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B153,B153)=1,A152+1,A152)","v":1},{"$f":"IF('6a - Lighting Counts'!G179=\"\",\"\",'6a - Lighting Counts'!G179)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B154,B154)=1,A153+1,A153)","v":1},{"$f":"IF('6a - Lighting Counts'!G180=\"\",\"\",'6a - Lighting Counts'!G180)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B155,B155)=1,A154+1,A154)","v":1},{"$f":"IF('6a - Lighting Counts'!G181=\"\",\"\",'6a - Lighting Counts'!G181)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B156,B156)=1,A155+1,A155)","v":1},{"$f":"IF('6a - Lighting Counts'!G182=\"\",\"\",'6a - Lighting Counts'!G182)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B157,B157)=1,A156+1,A156)","v":1},{"$f":"IF('6a - Lighting Counts'!G183=\"\",\"\",'6a - Lighting Counts'!G183)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B158,B158)=1,A157+1,A157)","v":1},{"$f":"IF('6a - Lighting Counts'!G184=\"\",\"\",'6a - Lighting Counts'!G184)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B159,B159)=1,A158+1,A158)","v":1},{"$f":"IF('6a - Lighting Counts'!G185=\"\",\"\",'6a - Lighting Counts'!G185)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B160,B160)=1,A159+1,A159)","v":1},{"$f":"IF('6a - Lighting Counts'!G186=\"\",\"\",'6a - Lighting Counts'!G186)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B161,B161)=1,A160+1,A160)","v":1},{"$f":"IF('6a - Lighting Counts'!G187=\"\",\"\",'6a - Lighting Counts'!G187)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B162,B162)=1,A161+1,A161)","v":1},{"$f":"IF('6a - Lighting Counts'!G188=\"\",\"\",'6a - Lighting Counts'!G188)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B163,B163)=1,A162+1,A162)","v":1},{"$f":"IF('6a - Lighting Counts'!G189=\"\",\"\",'6a - Lighting Counts'!G189)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B164,B164)=1,A163+1,A163)","v":1},{"$f":"IF('6a - Lighting Counts'!G190=\"\",\"\",'6a - Lighting Counts'!G190)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B165,B165)=1,A164+1,A164)","v":1},{"$f":"IF('6a - Lighting Counts'!G191=\"\",\"\",'6a - Lighting Counts'!G191)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B166,B166)=1,A165+1,A165)","v":1},{"$f":"IF('6a - Lighting Counts'!G192=\"\",\"\",'6a - Lighting Counts'!G192)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B167,B167)=1,A166+1,A166)","v":1},{"$f":"IF('6a - Lighting Counts'!G193=\"\",\"\",'6a - Lighting Counts'!G193)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B168,B168)=1,A167+1,A167)","v":1},{"$f":"IF('6a - Lighting Counts'!G194=\"\",\"\",'6a - Lighting Counts'!G194)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B169,B169)=1,A168+1,A168)","v":1},{"$f":"IF('6a - Lighting Counts'!G195=\"\",\"\",'6a - Lighting Counts'!G195)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B170,B170)=1,A169+1,A169)","v":1},{"$f":"IF('6a - Lighting Counts'!G196=\"\",\"\",'6a - Lighting Counts'!G196)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B171,B171)=1,A170+1,A170)","v":1},{"$f":"IF('6a - Lighting Counts'!G197=\"\",\"\",'6a - Lighting Counts'!G197)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B172,B172)=1,A171+1,A171)","v":1},{"$f":"IF('6a - Lighting Counts'!G198=\"\",\"\",'6a - Lighting Counts'!G198)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B173,B173)=1,A172+1,A172)","v":1},{"$f":"IF('6a - Lighting Counts'!G199=\"\",\"\",'6a - Lighting Counts'!G199)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B174,B174)=1,A173+1,A173)","v":1},{"$f":"IF('6a - Lighting Counts'!G200=\"\",\"\",'6a - Lighting Counts'!G200)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B175,B175)=1,A174+1,A174)","v":1},{"$f":"IF('6a - Lighting Counts'!G201=\"\",\"\",'6a - Lighting Counts'!G201)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B176,B176)=1,A175+1,A175)","v":1},{"$f":"IF('6a - Lighting Counts'!G202=\"\",\"\",'6a - Lighting Counts'!G202)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B177,B177)=1,A176+1,A176)","v":1},{"$f":"IF('6a - Lighting Counts'!G203=\"\",\"\",'6a - Lighting Counts'!G203)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B178,B178)=1,A177+1,A177)","v":1},{"$f":"IF('6a - Lighting Counts'!G204=\"\",\"\",'6a - Lighting Counts'!G204)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B179,B179)=1,A178+1,A178)","v":1},{"$f":"IF('6a - Lighting Counts'!G205=\"\",\"\",'6a - Lighting Counts'!G205)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B180,B180)=1,A179+1,A179)","v":1},{"$f":"IF('6a - Lighting Counts'!G206=\"\",\"\",'6a - Lighting Counts'!G206)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B181,B181)=1,A180+1,A180)","v":1},{"$f":"IF('6a - Lighting Counts'!G207=\"\",\"\",'6a - Lighting Counts'!G207)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B182,B182)=1,A181+1,A181)","v":1},{"$f":"IF('6a - Lighting Counts'!G208=\"\",\"\",'6a - Lighting Counts'!G208)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B183,B183)=1,A182+1,A182)","v":1},{"$f":"IF('6a - Lighting Counts'!G209=\"\",\"\",'6a - Lighting Counts'!G209)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B184,B184)=1,A183+1,A183)","v":1},{"$f":"IF('6a - Lighting Counts'!G210=\"\",\"\",'6a - Lighting Counts'!G210)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B185,B185)=1,A184+1,A184)","v":1},{"$f":"IF('6a - Lighting Counts'!G211=\"\",\"\",'6a - Lighting Counts'!G211)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B186,B186)=1,A185+1,A185)","v":1},{"$f":"IF('6a - Lighting Counts'!G212=\"\",\"\",'6a - Lighting Counts'!G212)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B187,B187)=1,A186+1,A186)","v":1},{"$f":"IF('6a - Lighting Counts'!G213=\"\",\"\",'6a - Lighting Counts'!G213)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B188,B188)=1,A187+1,A187)","v":1},{"$f":"IF('6a - Lighting Counts'!G214=\"\",\"\",'6a - Lighting Counts'!G214)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B189,B189)=1,A188+1,A188)","v":1},{"$f":"IF('6a - Lighting Counts'!G215=\"\",\"\",'6a - Lighting Counts'!G215)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B190,B190)=1,A189+1,A189)","v":1},{"$f":"IF('6a - Lighting Counts'!G216=\"\",\"\",'6a - Lighting Counts'!G216)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B191,B191)=1,A190+1,A190)","v":1},{"$f":"IF('6a - Lighting Counts'!G217=\"\",\"\",'6a - Lighting Counts'!G217)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B192,B192)=1,A191+1,A191)","v":1},{"$f":"IF('6a - Lighting Counts'!G218=\"\",\"\",'6a - Lighting Counts'!G218)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B193,B193)=1,A192+1,A192)","v":1},{"$f":"IF('6a - Lighting Counts'!G219=\"\",\"\",'6a - Lighting Counts'!G219)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B194,B194)=1,A193+1,A193)","v":1},{"$f":"IF('6a - Lighting Counts'!G220=\"\",\"\",'6a - Lighting Counts'!G220)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B195,B195)=1,A194+1,A194)","v":1},{"$f":"IF('6a - Lighting Counts'!G221=\"\",\"\",'6a - Lighting Counts'!G221)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B196,B196)=1,A195+1,A195)","v":1},{"$f":"IF('6a - Lighting Counts'!G222=\"\",\"\",'6a - Lighting Counts'!G222)","v":""},{"$f":"IFERROR(VLOOKUP(ROW()-2,$A$3:$B$550,2,FALSE),\"\")","v":""}]
[{"$f":"IF(COUNTIF($B$3:B197,B197)=1,A196+1,A196)","v":1},{"$f":"IF('6a - Lighting Counts'!G223=\"\",\"\",'6a - Lighting Counts'!G223)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B198,B198)=1,A197+1,A197)","v":1},{"$f":"IF('6a - Lighting Counts'!G224=\"\",\"\",'6a - Lighting Counts'!G224)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B199,B199)=1,A198+1,A198)","v":1},{"$f":"IF('6a - Lighting Counts'!G225=\"\",\"\",'6a - Lighting Counts'!G225)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B200,B200)=1,A199+1,A199)","v":1},{"$f":"IF('6a - Lighting Counts'!G226=\"\",\"\",'6a - Lighting Counts'!G226)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B201,B201)=1,A200+1,A200)","v":1},{"$f":"IF('6a - Lighting Counts'!G227=\"\",\"\",'6a - Lighting Counts'!G227)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B202,B202)=1,A201+1,A201)","v":1},{"$f":"IF('6a - Lighting Counts'!G228=\"\",\"\",'6a - Lighting Counts'!G228)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B203,B203)=1,A202+1,A202)","v":1},{"$f":"IF('6a - Lighting Counts'!G229=\"\",\"\",'6a - Lighting Counts'!G229)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B204,B204)=1,A203+1,A203)","v":1},{"$f":"IF('6a - Lighting Counts'!G230=\"\",\"\",'6a - Lighting Counts'!G230)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B205,B205)=1,A204+1,A204)","v":1},{"$f":"IF('6a - Lighting Counts'!G231=\"\",\"\",'6a - Lighting Counts'!G231)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B206,B206)=1,A205+1,A205)","v":1},{"$f":"IF('6a - Lighting Counts'!G232=\"\",\"\",'6a - Lighting Counts'!G232)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B207,B207)=1,A206+1,A206)","v":1},{"$f":"IF('6a - Lighting Counts'!G233=\"\",\"\",'6a - Lighting Counts'!G233)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B208,B208)=1,A207+1,A207)","v":1},{"$f":"IF('6a - Lighting Counts'!G234=\"\",\"\",'6a - Lighting Counts'!G234)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B209,B209)=1,A208+1,A208)","v":1},{"$f":"IF('6a - Lighting Counts'!G235=\"\",\"\",'6a - Lighting Counts'!G235)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B210,B210)=1,A209+1,A209)","v":1},{"$f":"IF('6a - Lighting Counts'!G236=\"\",\"\",'6a - Lighting Counts'!G236)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B211,B211)=1,A210+1,A210)","v":1},{"$f":"IF('6a - Lighting Counts'!G237=\"\",\"\",'6a - Lighting Counts'!G237)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B212,B212)=1,A211+1,A211)","v":1},{"$f":"IF('6a - Lighting Counts'!G238=\"\",\"\",'6a - Lighting Counts'!G238)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B213,B213)=1,A212+1,A212)","v":1},{"$f":"IF('6a - Lighting Counts'!G239=\"\",\"\",'6a - Lighting Counts'!G239)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B214,B214)=1,A213+1,A213)","v":1},{"$f":"IF('6a - Lighting Counts'!G240=\"\",\"\",'6a - Lighting Counts'!G240)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B215,B215)=1,A214+1,A214)","v":1},{"$f":"IF('6a - Lighting Counts'!G241=\"\",\"\",'6a - Lighting Counts'!G241)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B216,B216)=1,A215+1,A215)","v":1},{"$f":"IF('6a - Lighting Counts'!G242=\"\",\"\",'6a - Lighting Counts'!G242)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B217,B217)=1,A216+1,A216)","v":1},{"$f":"IF('6a - Lighting Counts'!G243=\"\",\"\",'6a - Lighting Counts'!G243)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B218,B218)=1,A217+1,A217)","v":1},{"$f":"IF('6a - Lighting Counts'!G244=\"\",\"\",'6a - Lighting Counts'!G244)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B219,B219)=1,A218+1,A218)","v":1},{"$f":"IF('6a - Lighting Counts'!G245=\"\",\"\",'6a - Lighting Counts'!G245)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B220,B220)=1,A219+1,A219)","v":1},{"$f":"IF('6a - Lighting Counts'!G246=\"\",\"\",'6a - Lighting Counts'!G246)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B221,B221)=1,A220+1,A220)","v":1},{"$f":"IF('6a - Lighting Counts'!G247=\"\",\"\",'6a - Lighting Counts'!G247)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B222,B222)=1,A221+1,A221)","v":1},{"$f":"IF('6a - Lighting Counts'!G248=\"\",\"\",'6a - Lighting Counts'!G248)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B223,B223)=1,A222+1,A222)","v":1},{"$f":"IF('6a - Lighting Counts'!G249=\"\",\"\",'6a - Lighting Counts'!G249)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B224,B224)=1,A223+1,A223)","v":1},{"$f":"IF('6a - Lighting Counts'!G250=\"\",\"\",'6a - Lighting Counts'!G250)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B225,B225)=1,A224+1,A224)","v":1},{"$f":"IF('6a - Lighting Counts'!G251=\"\",\"\",'6a - Lighting Counts'!G251)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B226,B226)=1,A225+1,A225)","v":1},{"$f":"IF('6a - Lighting Counts'!G252=\"\",\"\",'6a - Lighting Counts'!G252)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B227,B227)=1,A226+1,A226)","v":1},{"$f":"IF('6a - Lighting Counts'!G253=\"\",\"\",'6a - Lighting Counts'!G253)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B228,B228)=1,A227+1,A227)","v":1},{"$f":"IF('6a - Lighting Counts'!G254=\"\",\"\",'6a - Lighting Counts'!G254)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B229,B229)=1,A228+1,A228)","v":1},{"$f":"IF('6a - Lighting Counts'!G255=\"\",\"\",'6a - Lighting Counts'!G255)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B230,B230)=1,A229+1,A229)","v":1},{"$f":"IF('6a - Lighting Counts'!G256=\"\",\"\",'6a - Lighting Counts'!G256)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B231,B231)=1,A230+1,A230)","v":1},{"$f":"IF('6a - Lighting Counts'!G257=\"\",\"\",'6a - Lighting Counts'!G257)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B232,B232)=1,A231+1,A231)","v":1},{"$f":"IF('6a - Lighting Counts'!G258=\"\",\"\",'6a - Lighting Counts'!G258)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B233,B233)=1,A232+1,A232)","v":1},{"$f":"IF('6a - Lighting Counts'!G259=\"\",\"\",'6a - Lighting Counts'!G259)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B234,B234)=1,A233+1,A233)","v":1},{"$f":"IF('6a - Lighting Counts'!G260=\"\",\"\",'6a - Lighting Counts'!G260)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B235,B235)=1,A234+1,A234)","v":1},{"$f":"IF('6a - Lighting Counts'!G261=\"\",\"\",'6a - Lighting Counts'!G261)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B236,B236)=1,A235+1,A235)","v":1},{"$f":"IF('6a - Lighting Counts'!G262=\"\",\"\",'6a - Lighting Counts'!G262)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B237,B237)=1,A236+1,A236)","v":1},{"$f":"IF('6a - Lighting Counts'!G263=\"\",\"\",'6a - Lighting Counts'!G263)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B238,B238)=1,A237+1,A237)","v":1},{"$f":"IF('6a - Lighting Counts'!G264=\"\",\"\",'6a - Lighting Counts'!G264)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B239,B239)=1,A238+1,A238)","v":1},{"$f":"IF('6a - Lighting Counts'!G265=\"\",\"\",'6a - Lighting Counts'!G265)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B240,B240)=1,A239+1,A239)","v":1},{"$f":"IF('6a - Lighting Counts'!G266=\"\",\"\",'6a - Lighting Counts'!G266)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B241,B241)=1,A240+1,A240)","v":1},{"$f":"IF('6a - Lighting Counts'!G267=\"\",\"\",'6a - Lighting Counts'!G267)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B242,B242)=1,A241+1,A241)","v":1},{"$f":"IF('6a - Lighting Counts'!G268=\"\",\"\",'6a - Lighting Counts'!G268)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B243,B243)=1,A242+1,A242)","v":1},{"$f":"IF('6a - Lighting Counts'!G269=\"\",\"\",'6a - Lighting Counts'!G269)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B244,B244)=1,A243+1,A243)","v":1},{"$f":"IF('6a - Lighting Counts'!G270=\"\",\"\",'6a - Lighting Counts'!G270)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B245,B245)=1,A244+1,A244)","v":1},{"$f":"IF('6a - Lighting Counts'!G271=\"\",\"\",'6a - Lighting Counts'!G271)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B246,B246)=1,A245+1,A245)","v":1},{"$f":"IF('6a - Lighting Counts'!G272=\"\",\"\",'6a - Lighting Counts'!G272)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B247,B247)=1,A246+1,A246)","v":1},{"$f":"IF('6a - Lighting Counts'!G273=\"\",\"\",'6a - Lighting Counts'!G273)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B248,B248)=1,A247+1,A247)","v":1},{"$f":"IF('6a - Lighting Counts'!G274=\"\",\"\",'6a - Lighting Counts'!G274)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B249,B249)=1,A248+1,A248)","v":1},{"$f":"IF('6a - Lighting Counts'!G275=\"\",\"\",'6a - Lighting Counts'!G275)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B250,B250)=1,A249+1,A249)","v":1},{"$f":"IF('6a - Lighting Counts'!G276=\"\",\"\",'6a - Lighting Counts'!G276)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B251,B251)=1,A250+1,A250)","v":1},{"$f":"IF('6a - Lighting Counts'!G277=\"\",\"\",'6a - Lighting Counts'!G277)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B252,B252)=1,A251+1,A251)","v":1},{"$f":"IF('6a - Lighting Counts'!G278=\"\",\"\",'6a - Lighting Counts'!G278)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B253,B253)=1,A252+1,A252)","v":1},{"$f":"IF('6a - Lighting Counts'!G279=\"\",\"\",'6a - Lighting Counts'!G279)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B254,B254)=1,A253+1,A253)","v":1},{"$f":"IF('6a - Lighting Counts'!G280=\"\",\"\",'6a - Lighting Counts'!G280)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B255,B255)=1,A254+1,A254)","v":1},{"$f":"IF('6a - Lighting Counts'!G281=\"\",\"\",'6a - Lighting Counts'!G281)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B256,B256)=1,A255+1,A255)","v":1},{"$f":"IF('6a - Lighting Counts'!G282=\"\",\"\",'6a - Lighting Counts'!G282)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B257,B257)=1,A256+1,A256)","v":1},{"$f":"IF('6a - Lighting Counts'!G283=\"\",\"\",'6a - Lighting Counts'!G283)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B258,B258)=1,A257+1,A257)","v":1},{"$f":"IF('6a - Lighting Counts'!G284=\"\",\"\",'6a - Lighting Counts'!G284)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B259,B259)=1,A258+1,A258)","v":1},{"$f":"IF('6a - Lighting Counts'!G285=\"\",\"\",'6a - Lighting Counts'!G285)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B260,B260)=1,A259+1,A259)","v":1},{"$f":"IF('6a - Lighting Counts'!G286=\"\",\"\",'6a - Lighting Counts'!G286)","v":""},{"$f":"IFERROR(VLOOKUP(ROW()-2,$A$3:$B$550,2,FALSE),\"\")","v":""}]
[{"$f":"IF(COUNTIF($B$3:B261,B261)=1,A260+1,A260)","v":1},{"$f":"IF('6a - Lighting Counts'!G287=\"\",\"\",'6a - Lighting Counts'!G287)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B262,B262)=1,A261+1,A261)","v":1},{"$f":"IF('6a - Lighting Counts'!G288=\"\",\"\",'6a - Lighting Counts'!G288)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B263,B263)=1,A262+1,A262)","v":1},{"$f":"IF('6a - Lighting Counts'!G289=\"\",\"\",'6a - Lighting Counts'!G289)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B264,B264)=1,A263+1,A263)","v":1},{"$f":"IF('6a - Lighting Counts'!G290=\"\",\"\",'6a - Lighting Counts'!G290)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B265,B265)=1,A264+1,A264)","v":1},{"$f":"IF('6a - Lighting Counts'!G291=\"\",\"\",'6a - Lighting Counts'!G291)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B266,B266)=1,A265+1,A265)","v":1},{"$f":"IF('6a - Lighting Counts'!G292=\"\",\"\",'6a - Lighting Counts'!G292)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B267,B267)=1,A266+1,A266)","v":1},{"$f":"IF('6a - Lighting Counts'!G293=\"\",\"\",'6a - Lighting Counts'!G293)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B268,B268)=1,A267+1,A267)","v":1},{"$f":"IF('6a - Lighting Counts'!G294=\"\",\"\",'6a - Lighting Counts'!G294)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B269,B269)=1,A268+1,A268)","v":1},{"$f":"IF('6a - Lighting Counts'!G295=\"\",\"\",'6a - Lighting Counts'!G295)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B270,B270)=1,A269+1,A269)","v":1},{"$f":"IF('6a - Lighting Counts'!G296=\"\",\"\",'6a - Lighting Counts'!G296)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B271,B271)=1,A270+1,A270)","v":1},{"$f":"IF('6a - Lighting Counts'!G297=\"\",\"\",'6a - Lighting Counts'!G297)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B272,B272)=1,A271+1,A271)","v":1},{"$f":"IF('6a - Lighting Counts'!G298=\"\",\"\",'6a - Lighting Counts'!G298)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B273,B273)=1,A272+1,A272)","v":1},{"$f":"IF('6a - Lighting Counts'!G299=\"\",\"\",'6a - Lighting Counts'!G299)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B274,B274)=1,A273+1,A273)","v":1},{"$f":"IF('6a - Lighting Counts'!G300=\"\",\"\",'6a - Lighting Counts'!G300)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B275,B275)=1,A274+1,A274)","v":1},{"$f":"IF('6a - Lighting Counts'!G301=\"\",\"\",'6a - Lighting Counts'!G301)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B276,B276)=1,A275+1,A275)","v":1},{"$f":"IF('6a - Lighting Counts'!G302=\"\",\"\",'6a - Lighting Counts'!G302)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B277,B277)=1,A276+1,A276)","v":1},{"$f":"IF('6a - Lighting Counts'!G303=\"\",\"\",'6a - Lighting Counts'!G303)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B278,B278)=1,A277+1,A277)","v":1},{"$f":"IF('6a - Lighting Counts'!G304=\"\",\"\",'6a - Lighting Counts'!G304)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B279,B279)=1,A278+1,A278)","v":1},{"$f":"IF('6a - Lighting Counts'!G305=\"\",\"\",'6a - Lighting Counts'!G305)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B280,B280)=1,A279+1,A279)","v":1},{"$f":"IF('6a - Lighting Counts'!G306=\"\",\"\",'6a - Lighting Counts'!G306)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B281,B281)=1,A280+1,A280)","v":1},{"$f":"IF('6a - Lighting Counts'!G307=\"\",\"\",'6a - Lighting Counts'!G307)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B282,B282)=1,A281+1,A281)","v":1},{"$f":"IF('6a - Lighting Counts'!G308=\"\",\"\",'6a - Lighting Counts'!G308)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B283,B283)=1,A282+1,A282)","v":1},{"$f":"IF('6a - Lighting Counts'!G309=\"\",\"\",'6a - Lighting Counts'!G309)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B284,B284)=1,A283+1,A283)","v":1},{"$f":"IF('6a - Lighting Counts'!G310=\"\",\"\",'6a - Lighting Counts'!G310)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B285,B285)=1,A284+1,A284)","v":1},{"$f":"IF('6a - Lighting Counts'!G311=\"\",\"\",'6a - Lighting Counts'!G311)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B286,B286)=1,A285+1,A285)","v":1},{"$f":"IF('6a - Lighting Counts'!G312=\"\",\"\",'6a - Lighting Counts'!G312)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B287,B287)=1,A286+1,A286)","v":1},{"$f":"IF('6a - Lighting Counts'!G313=\"\",\"\",'6a - Lighting Counts'!G313)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B288,B288)=1,A287+1,A287)","v":1},{"$f":"IF('6a - Lighting Counts'!G314=\"\",\"\",'6a - Lighting Counts'!G314)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B289,B289)=1,A288+1,A288)","v":1},{"$f":"IF('6a - Lighting Counts'!G315=\"\",\"\",'6a - Lighting Counts'!G315)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B290,B290)=1,A289+1,A289)","v":1},{"$f":"IF('6a - Lighting Counts'!G316=\"\",\"\",'6a - Lighting Counts'!G316)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B291,B291)=1,A290+1,A290)","v":1},{"$f":"IF('6a - Lighting Counts'!G317=\"\",\"\",'6a - Lighting Counts'!G317)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B292,B292)=1,A291+1,A291)","v":1},{"$f":"IF('6a - Lighting Counts'!G318=\"\",\"\",'6a - Lighting Counts'!G318)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B293,B293)=1,A292+1,A292)","v":1},{"$f":"IF('6a - Lighting Counts'!G319=\"\",\"\",'6a - Lighting Counts'!G319)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B294,B294)=1,A293+1,A293)","v":1},{"$f":"IF('6a - Lighting Counts'!G320=\"\",\"\",'6a - Lighting Counts'!G320)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B295,B295)=1,A294+1,A294)","v":1},{"$f":"IF('6a - Lighting Counts'!G321=\"\",\"\",'6a - Lighting Counts'!G321)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B296,B296)=1,A295+1,A295)","v":1},{"$f":"IF('6a - Lighting Counts'!G322=\"\",\"\",'6a - Lighting Counts'!G322)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B297,B297)=1,A296+1,A296)","v":1},{"$f":"IF('6a - Lighting Counts'!G323=\"\",\"\",'6a - Lighting Counts'!G323)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B298,B298)=1,A297+1,A297)","v":1},{"$f":"IF('6a - Lighting Counts'!G324=\"\",\"\",'6a - Lighting Counts'!G324)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B299,B299)=1,A298+1,A298)","v":1},{"$f":"IF('6a - Lighting Counts'!G325=\"\",\"\",'6a - Lighting Counts'!G325)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B300,B300)=1,A299+1,A299)","v":1},{"$f":"IF('6a - Lighting Counts'!G326=\"\",\"\",'6a - Lighting Counts'!G326)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B301,B301)=1,A300+1,A300)","v":1},{"$f":"IF('6a - Lighting Counts'!G327=\"\",\"\",'6a - Lighting Counts'!G327)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B302,B302)=1,A301+1,A301)","v":1},{"$f":"IF('6a - Lighting Counts'!G328=\"\",\"\",'6a - Lighting Counts'!G328)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B303,B303)=1,A302+1,A302)","v":1},{"$f":"IF('6a - Lighting Counts'!G329=\"\",\"\",'6a - Lighting Counts'!G329)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B304,B304)=1,A303+1,A303)","v":1},{"$f":"IF('6a - Lighting Counts'!G330=\"\",\"\",'6a - Lighting Counts'!G330)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B305,B305)=1,A304+1,A304)","v":1},{"$f":"IF('6a - Lighting Counts'!G331=\"\",\"\",'6a - Lighting Counts'!G331)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B306,B306)=1,A305+1,A305)","v":1},{"$f":"IF('6a - Lighting Counts'!G332=\"\",\"\",'6a - Lighting Counts'!G332)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B307,B307)=1,A306+1,A306)","v":1},{"$f":"IF('6a - Lighting Counts'!G333=\"\",\"\",'6a - Lighting Counts'!G333)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B308,B308)=1,A307+1,A307)","v":1},{"$f":"IF('6a - Lighting Counts'!G334=\"\",\"\",'6a - Lighting Counts'!G334)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B309,B309)=1,A308+1,A308)","v":1},{"$f":"IF('6a - Lighting Counts'!G335=\"\",\"\",'6a - Lighting Counts'!G335)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B310,B310)=1,A309+1,A309)","v":1},{"$f":"IF('6a - Lighting Counts'!G336=\"\",\"\",'6a - Lighting Counts'!G336)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B311,B311)=1,A310+1,A310)","v":1},{"$f":"IF('6a - Lighting Counts'!G337=\"\",\"\",'6a - Lighting Counts'!G337)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B312,B312)=1,A311+1,A311)","v":1},{"$f":"IF('6a - Lighting Counts'!G338=\"\",\"\",'6a - Lighting Counts'!G338)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B313,B313)=1,A312+1,A312)","v":1},{"$f":"IF('6a - Lighting Counts'!G339=\"\",\"\",'6a - Lighting Counts'!G339)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B314,B314)=1,A313+1,A313)","v":1},{"$f":"IF('6a - Lighting Counts'!G340=\"\",\"\",'6a - Lighting Counts'!G340)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B315,B315)=1,A314+1,A314)","v":1},{"$f":"IF('6a - Lighting Counts'!G341=\"\",\"\",'6a - Lighting Counts'!G341)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B316,B316)=1,A315+1,A315)","v":1},{"$f":"IF('6a - Lighting Counts'!G342=\"\",\"\",'6a - Lighting Counts'!G342)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B317,B317)=1,A316+1,A316)","v":1},{"$f":"IF('6a - Lighting Counts'!G343=\"\",\"\",'6a - Lighting Counts'!G343)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B318,B318)=1,A317+1,A317)","v":1},{"$f":"IF('6a - Lighting Counts'!G344=\"\",\"\",'6a - Lighting Counts'!G344)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B319,B319)=1,A318+1,A318)","v":1},{"$f":"IF('6a - Lighting Counts'!G345=\"\",\"\",'6a - Lighting Counts'!G345)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B320,B320)=1,A319+1,A319)","v":1},{"$f":"IF('6a - Lighting Counts'!G346=\"\",\"\",'6a - Lighting Counts'!G346)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B321,B321)=1,A320+1,A320)","v":1},{"$f":"IF('6a - Lighting Counts'!G347=\"\",\"\",'6a - Lighting Counts'!G347)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B322,B322)=1,A321+1,A321)","v":1},{"$f":"IF('6a - Lighting Counts'!G348=\"\",\"\",'6a - Lighting Counts'!G348)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B323,B323)=1,A322+1,A322)","v":1},{"$f":"IF('6a - Lighting Counts'!G349=\"\",\"\",'6a - Lighting Counts'!G349)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B324,B324)=1,A323+1,A323)","v":1},{"$f":"IF('6a - Lighting Counts'!G350=\"\",\"\",'6a - Lighting Counts'!G350)","v":""},{"$f":"IFERROR(VLOOKUP(ROW()-2,$A$3:$B$550,2,FALSE),\"\")","v":""}]
[{"$f":"IF(COUNTIF($B$3:B325,B325)=1,A324+1,A324)","v":1},{"$f":"IF('6a - Lighting Counts'!G351=\"\",\"\",'6a - Lighting Counts'!G351)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B326,B326)=1,A325+1,A325)","v":1},{"$f":"IF('6a - Lighting Counts'!G352=\"\",\"\",'6a - Lighting Counts'!G352)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B327,B327)=1,A326+1,A326)","v":1},{"$f":"IF('6a - Lighting Counts'!G353=\"\",\"\",'6a - Lighting Counts'!G353)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B328,B328)=1,A327+1,A327)","v":1},{"$f":"IF('6a - Lighting Counts'!G354=\"\",\"\",'6a - Lighting Counts'!G354)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B329,B329)=1,A328+1,A328)","v":1},{"$f":"IF('6a - Lighting Counts'!G355=\"\",\"\",'6a - Lighting Counts'!G355)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B330,B330)=1,A329+1,A329)","v":1},{"$f":"IF('6a - Lighting Counts'!G356=\"\",\"\",'6a - Lighting Counts'!G356)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B331,B331)=1,A330+1,A330)","v":1},{"$f":"IF('6a - Lighting Counts'!G357=\"\",\"\",'6a - Lighting Counts'!G357)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B332,B332)=1,A331+1,A331)","v":1},{"$f":"IF('6a - Lighting Counts'!G358=\"\",\"\",'6a - Lighting Counts'!G358)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B333,B333)=1,A332+1,A332)","v":1},{"$f":"IF('6a - Lighting Counts'!G359=\"\",\"\",'6a - Lighting Counts'!G359)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B334,B334)=1,A333+1,A333)","v":1},{"$f":"IF('6a - Lighting Counts'!G360=\"\",\"\",'6a - Lighting Counts'!G360)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B335,B335)=1,A334+1,A334)","v":1},{"$f":"IF('6a - Lighting Counts'!G361=\"\",\"\",'6a - Lighting Counts'!G361)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B336,B336)=1,A335+1,A335)","v":1},{"$f":"IF('6a - Lighting Counts'!G362=\"\",\"\",'6a - Lighting Counts'!G362)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B337,B337)=1,A336+1,A336)","v":1},{"$f":"IF('6a - Lighting Counts'!G363=\"\",\"\",'6a - Lighting Counts'!G363)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B338,B338)=1,A337+1,A337)","v":1},{"$f":"IF('6a - Lighting Counts'!G364=\"\",\"\",'6a - Lighting Counts'!G364)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B339,B339)=1,A338+1,A338)","v":1},{"$f":"IF('6a - Lighting Counts'!G365=\"\",\"\",'6a - Lighting Counts'!G365)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B340,B340)=1,A339+1,A339)","v":1},{"$f":"IF('6a - Lighting Counts'!G366=\"\",\"\",'6a - Lighting Counts'!G366)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B341,B341)=1,A340+1,A340)","v":1},{"$f":"IF('6a - Lighting Counts'!G367=\"\",\"\",'6a - Lighting Counts'!G367)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B342,B342)=1,A341+1,A341)","v":1},{"$f":"IF('6a - Lighting Counts'!G368=\"\",\"\",'6a - Lighting Counts'!G368)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B343,B343)=1,A342+1,A342)","v":1},{"$f":"IF('6a - Lighting Counts'!G369=\"\",\"\",'6a - Lighting Counts'!G369)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B344,B344)=1,A343+1,A343)","v":1},{"$f":"IF('6a - Lighting Counts'!G370=\"\",\"\",'6a - Lighting Counts'!G370)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B345,B345)=1,A344+1,A344)","v":1},{"$f":"IF('6a - Lighting Counts'!G371=\"\",\"\",'6a - Lighting Counts'!G371)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B346,B346)=1,A345+1,A345)","v":1},{"$f":"IF('6a - Lighting Counts'!G372=\"\",\"\",'6a - Lighting Counts'!G372)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B347,B347)=1,A346+1,A346)","v":1},{"$f":"IF('6a - Lighting Counts'!G373=\"\",\"\",'6a - Lighting Counts'!G373)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B348,B348)=1,A347+1,A347)","v":1},{"$f":"IF('6a - Lighting Counts'!G374=\"\",\"\",'6a - Lighting Counts'!G374)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B349,B349)=1,A348+1,A348)","v":1},{"$f":"IF('6a - Lighting Counts'!G375=\"\",\"\",'6a - Lighting Counts'!G375)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B350,B350)=1,A349+1,A349)","v":1},{"$f":"IF('6a - Lighting Counts'!G376=\"\",\"\",'6a - Lighting Counts'!G376)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B351,B351)=1,A350+1,A350)","v":1},{"$f":"IF('6a - Lighting Counts'!G377=\"\",\"\",'6a - Lighting Counts'!G377)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B352,B352)=1,A351+1,A351)","v":1},{"$f":"IF('6a - Lighting Counts'!G378=\"\",\"\",'6a - Lighting Counts'!G378)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B353,B353)=1,A352+1,A352)","v":1},{"$f":"IF('6a - Lighting Counts'!G379=\"\",\"\",'6a - Lighting Counts'!G379)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B354,B354)=1,A353+1,A353)","v":1},{"$f":"IF('6a - Lighting Counts'!G380=\"\",\"\",'6a - Lighting Counts'!G380)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B355,B355)=1,A354+1,A354)","v":1},{"$f":"IF('6a - Lighting Counts'!G381=\"\",\"\",'6a - Lighting Counts'!G381)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B356,B356)=1,A355+1,A355)","v":1},{"$f":"IF('6a - Lighting Counts'!G382=\"\",\"\",'6a - Lighting Counts'!G382)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B357,B357)=1,A356+1,A356)","v":1},{"$f":"IF('6a - Lighting Counts'!G383=\"\",\"\",'6a - Lighting Counts'!G383)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B358,B358)=1,A357+1,A357)","v":1},{"$f":"IF('6a - Lighting Counts'!G384=\"\",\"\",'6a - Lighting Counts'!G384)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B359,B359)=1,A358+1,A358)","v":1},{"$f":"IF('6a - Lighting Counts'!G385=\"\",\"\",'6a - Lighting Counts'!G385)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B360,B360)=1,A359+1,A359)","v":1},{"$f":"IF('6a - Lighting Counts'!G386=\"\",\"\",'6a - Lighting Counts'!G386)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B361,B361)=1,A360+1,A360)","v":1},{"$f":"IF('6a - Lighting Counts'!G387=\"\",\"\",'6a - Lighting Counts'!G387)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B362,B362)=1,A361+1,A361)","v":1},{"$f":"IF('6a - Lighting Counts'!G388=\"\",\"\",'6a - Lighting Counts'!G388)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B363,B363)=1,A362+1,A362)","v":1},{"$f":"IF('6a - Lighting Counts'!G389=\"\",\"\",'6a - Lighting Counts'!G389)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B364,B364)=1,A363+1,A363)","v":1},{"$f":"IF('6a - Lighting Counts'!G390=\"\",\"\",'6a - Lighting Counts'!G390)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B365,B365)=1,A364+1,A364)","v":1},{"$f":"IF('6a - Lighting Counts'!G391=\"\",\"\",'6a - Lighting Counts'!G391)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B366,B366)=1,A365+1,A365)","v":1},{"$f":"IF('6a - Lighting Counts'!G392=\"\",\"\",'6a - Lighting Counts'!G392)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B367,B367)=1,A366+1,A366)","v":1},{"$f":"IF('6a - Lighting Counts'!G393=\"\",\"\",'6a - Lighting Counts'!G393)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B368,B368)=1,A367+1,A367)","v":1},{"$f":"IF('6a - Lighting Counts'!G394=\"\",\"\",'6a - Lighting Counts'!G394)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B369,B369)=1,A368+1,A368)","v":1},{"$f":"IF('6a - Lighting Counts'!G395=\"\",\"\",'6a - Lighting Counts'!G395)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B370,B370)=1,A369+1,A369)","v":1},{"$f":"IF('6a - Lighting Counts'!G396=\"\",\"\",'6a - Lighting Counts'!G396)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B371,B371)=1,A370+1,A370)","v":1},{"$f":"IF('6a - Lighting Counts'!G397=\"\",\"\",'6a - Lighting Counts'!G397)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B372,B372)=1,A371+1,A371)","v":1},{"$f":"IF('6a - Lighting Counts'!G398=\"\",\"\",'6a - Lighting Counts'!G398)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B373,B373)=1,A372+1,A372)","v":1},{"$f":"IF('6a - Lighting Counts'!G399=\"\",\"\",'6a - Lighting Counts'!G399)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B374,B374)=1,A373+1,A373)","v":1},{"$f":"IF('6a - Lighting Counts'!G400=\"\",\"\",'6a - Lighting Counts'!G400)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B375,B375)=1,A374+1,A374)","v":1},{"$f":"IF('6a - Lighting Counts'!G401=\"\",\"\",'6a - Lighting Counts'!G401)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B376,B376)=1,A375+1,A375)","v":1},{"$f":"IF('6a - Lighting Counts'!G402=\"\",\"\",'6a - Lighting Counts'!G402)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B377,B377)=1,A376+1,A376)","v":1},{"$f":"IF('6a - Lighting Counts'!G403=\"\",\"\",'6a - Lighting Counts'!G403)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B378,B378)=1,A377+1,A377)","v":1},{"$f":"IF('6a - Lighting Counts'!G404=\"\",\"\",'6a - Lighting Counts'!G404)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B379,B379)=1,A378+1,A378)","v":1},{"$f":"IF('6a - Lighting Counts'!G405=\"\",\"\",'6a - Lighting Counts'!G405)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B380,B380)=1,A379+1,A379)","v":1},{"$f":"IF('6a - Lighting Counts'!G406=\"\",\"\",'6a - Lighting Counts'!G406)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B381,B381)=1,A380+1,A380)","v":1},{"$f":"IF('6a - Lighting Counts'!G407=\"\",\"\",'6a - Lighting Counts'!G407)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B382,B382)=1,A381+1,A381)","v":1},{"$f":"IF('6a - Lighting Counts'!G408=\"\",\"\",'6a - Lighting Counts'!G408)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B383,B383)=1,A382+1,A382)","v":1},{"$f":"IF('6a - Lighting Counts'!G409=\"\",\"\",'6a - Lighting Counts'!G409)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B384,B384)=1,A383+1,A383)","v":1},{"$f":"IF('6a - Lighting Counts'!G410=\"\",\"\",'6a - Lighting Counts'!G410)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B385,B385)=1,A384+1,A384)","v":1},{"$f":"IF('6a - Lighting Counts'!G411=\"\",\"\",'6a - Lighting Counts'!G411)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B386,B386)=1,A385+1,A385)","v":1},{"$f":"IF('6a - Lighting Counts'!G412=\"\",\"\",'6a - Lighting Counts'!G412)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B387,B387)=1,A386+1,A386)","v":1},{"$f":"IF('6a - Lighting Counts'!G413=\"\",\"\",'6a - Lighting Counts'!G413)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B388,B388)=1,A387+1,A387)","v":1},{"$f":"IF('6a - Lighting Counts'!G414=\"\",\"\",'6a - Lighting Counts'!G414)","v":""},{"$f":"IFERROR(VLOOKUP(ROW()-2,$A$3:$B$550,2,FALSE),\"\")","v":""}]
[{"$f":"IF(COUNTIF($B$3:B389,B389)=1,A388+1,A388)","v":1},{"$f":"IF('6a - Lighting Counts'!G415=\"\",\"\",'6a - Lighting Counts'!G415)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B390,B390)=1,A389+1,A389)","v":1},{"$f":"IF('6a - Lighting Counts'!G416=\"\",\"\",'6a - Lighting Counts'!G416)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B391,B391)=1,A390+1,A390)","v":1},{"$f":"IF('6a - Lighting Counts'!G417=\"\",\"\",'6a - Lighting Counts'!G417)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B392,B392)=1,A391+1,A391)","v":1},{"$f":"IF('6a - Lighting Counts'!G418=\"\",\"\",'6a - Lighting Counts'!G418)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B393,B393)=1,A392+1,A392)","v":1},{"$f":"IF('6a - Lighting Counts'!G419=\"\",\"\",'6a - Lighting Counts'!G419)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B394,B394)=1,A393+1,A393)","v":1},{"$f":"IF('6a - Lighting Counts'!G420=\"\",\"\",'6a - Lighting Counts'!G420)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B395,B395)=1,A394+1,A394)","v":1},{"$f":"IF('6a - Lighting Counts'!G421=\"\",\"\",'6a - Lighting Counts'!G421)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B396,B396)=1,A395+1,A395)","v":1},{"$f":"IF('6a - Lighting Counts'!G422=\"\",\"\",'6a - Lighting Counts'!G422)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B397,B397)=1,A396+1,A396)","v":1},{"$f":"IF('6a - Lighting Counts'!G423=\"\",\"\",'6a - Lighting Counts'!G423)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B398,B398)=1,A397+1,A397)","v":1},{"$f":"IF('6a - Lighting Counts'!G424=\"\",\"\",'6a - Lighting Counts'!G424)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B399,B399)=1,A398+1,A398)","v":1},{"$f":"IF('6a - Lighting Counts'!G425=\"\",\"\",'6a - Lighting Counts'!G425)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B400,B400)=1,A399+1,A399)","v":1},{"$f":"IF('6a - Lighting Counts'!G426=\"\",\"\",'6a - Lighting Counts'!G426)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B401,B401)=1,A400+1,A400)","v":1},{"$f":"IF('6a - Lighting Counts'!G427=\"\",\"\",'6a - Lighting Counts'!G427)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B402,B402)=1,A401+1,A401)","v":1},{"$f":"IF('6a - Lighting Counts'!G428=\"\",\"\",'6a - Lighting Counts'!G428)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B403,B403)=1,A402+1,A402)","v":1},{"$f":"IF('6a - Lighting Counts'!G429=\"\",\"\",'6a - Lighting Counts'!G429)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B404,B404)=1,A403+1,A403)","v":1},{"$f":"IF('6a - Lighting Counts'!G430=\"\",\"\",'6a - Lighting Counts'!G430)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B405,B405)=1,A404+1,A404)","v":1},{"$f":"IF('6a - Lighting Counts'!G431=\"\",\"\",'6a - Lighting Counts'!G431)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B406,B406)=1,A405+1,A405)","v":1},{"$f":"IF('6a - Lighting Counts'!G432=\"\",\"\",'6a - Lighting Counts'!G432)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B407,B407)=1,A406+1,A406)","v":1},{"$f":"IF('6a - Lighting Counts'!G433=\"\",\"\",'6a - Lighting Counts'!G433)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B408,B408)=1,A407+1,A407)","v":1},{"$f":"IF('6a - Lighting Counts'!G434=\"\",\"\",'6a - Lighting Counts'!G434)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B409,B409)=1,A408+1,A408)","v":1},{"$f":"IF('6a - Lighting Counts'!G435=\"\",\"\",'6a - Lighting Counts'!G435)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B410,B410)=1,A409+1,A409)","v":1},{"$f":"IF('6a - Lighting Counts'!G436=\"\",\"\",'6a - Lighting Counts'!G436)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B411,B411)=1,A410+1,A410)","v":1},{"$f":"IF('6a - Lighting Counts'!G437=\"\",\"\",'6a - Lighting Counts'!G437)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B412,B412)=1,A411+1,A411)","v":1},{"$f":"IF('6a - Lighting Counts'!G438=\"\",\"\",'6a - Lighting Counts'!G438)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B413,B413)=1,A412+1,A412)","v":1},{"$f":"IF('6a - Lighting Counts'!G439=\"\",\"\",'6a - Lighting Counts'!G439)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B414,B414)=1,A413+1,A413)","v":1},{"$f":"IF('6a - Lighting Counts'!G440=\"\",\"\",'6a - Lighting Counts'!G440)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B415,B415)=1,A414+1,A414)","v":1},{"$f":"IF('6a - Lighting Counts'!G441=\"\",\"\",'6a - Lighting Counts'!G441)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B416,B416)=1,A415+1,A415)","v":1},{"$f":"IF('6a - Lighting Counts'!G442=\"\",\"\",'6a - Lighting Counts'!G442)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B417,B417)=1,A416+1,A416)","v":1},{"$f":"IF('6a - Lighting Counts'!G443=\"\",\"\",'6a - Lighting Counts'!G443)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B418,B418)=1,A417+1,A417)","v":1},{"$f":"IF('6a - Lighting Counts'!G444=\"\",\"\",'6a - Lighting Counts'!G444)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B419,B419)=1,A418+1,A418)","v":1},{"$f":"IF('6a - Lighting Counts'!G445=\"\",\"\",'6a - Lighting Counts'!G445)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B420,B420)=1,A419+1,A419)","v":1},{"$f":"IF('6a - Lighting Counts'!G446=\"\",\"\",'6a - Lighting Counts'!G446)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B421,B421)=1,A420+1,A420)","v":1},{"$f":"IF('6a - Lighting Counts'!G447=\"\",\"\",'6a - Lighting Counts'!G447)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B422,B422)=1,A421+1,A421)","v":1},{"$f":"IF('6a - Lighting Counts'!G448=\"\",\"\",'6a - Lighting Counts'!G448)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B423,B423)=1,A422+1,A422)","v":1},{"$f":"IF('6a - Lighting Counts'!G449=\"\",\"\",'6a - Lighting Counts'!G449)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B424,B424)=1,A423+1,A423)","v":1},{"$f":"IF('6a - Lighting Counts'!G450=\"\",\"\",'6a - Lighting Counts'!G450)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B425,B425)=1,A424+1,A424)","v":1},{"$f":"IF('6a - Lighting Counts'!G451=\"\",\"\",'6a - Lighting Counts'!G451)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B426,B426)=1,A425+1,A425)","v":1},{"$f":"IF('6a - Lighting Counts'!G452=\"\",\"\",'6a - Lighting Counts'!G452)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B427,B427)=1,A426+1,A426)","v":1},{"$f":"IF('6a - Lighting Counts'!G453=\"\",\"\",'6a - Lighting Counts'!G453)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B428,B428)=1,A427+1,A427)","v":1},{"$f":"IF('6a - Lighting Counts'!G454=\"\",\"\",'6a - Lighting Counts'!G454)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B429,B429)=1,A428+1,A428)","v":1},{"$f":"IF('6a - Lighting Counts'!G455=\"\",\"\",'6a - Lighting Counts'!G455)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B430,B430)=1,A429+1,A429)","v":1},{"$f":"IF('6a - Lighting Counts'!G456=\"\",\"\",'6a - Lighting Counts'!G456)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B431,B431)=1,A430+1,A430)","v":1},{"$f":"IF('6a - Lighting Counts'!G457=\"\",\"\",'6a - Lighting Counts'!G457)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B432,B432)=1,A431+1,A431)","v":1},{"$f":"IF('6a - Lighting Counts'!G458=\"\",\"\",'6a - Lighting Counts'!G458)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B433,B433)=1,A432+1,A432)","v":1},{"$f":"IF('6a - Lighting Counts'!G459=\"\",\"\",'6a - Lighting Counts'!G459)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B434,B434)=1,A433+1,A433)","v":1},{"$f":"IF('6a - Lighting Counts'!G460=\"\",\"\",'6a - Lighting Counts'!G460)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B435,B435)=1,A434+1,A434)","v":1},{"$f":"IF('6a - Lighting Counts'!G461=\"\",\"\",'6a - Lighting Counts'!G461)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B436,B436)=1,A435+1,A435)","v":1},{"$f":"IF('6a - Lighting Counts'!G462=\"\",\"\",'6a - Lighting Counts'!G462)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B437,B437)=1,A436+1,A436)","v":1},{"$f":"IF('6a - Lighting Counts'!G463=\"\",\"\",'6a - Lighting Counts'!G463)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B438,B438)=1,A437+1,A437)","v":1},{"$f":"IF('6a - Lighting Counts'!G464=\"\",\"\",'6a - Lighting Counts'!G464)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B439,B439)=1,A438+1,A438)","v":1},{"$f":"IF('6a - Lighting Counts'!G465=\"\",\"\",'6a - Lighting Counts'!G465)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B440,B440)=1,A439+1,A439)","v":1},{"$f":"IF('6a - Lighting Counts'!G466=\"\",\"\",'6a - Lighting Counts'!G466)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B441,B441)=1,A440+1,A440)","v":1},{"$f":"IF('6a - Lighting Counts'!G467=\"\",\"\",'6a - Lighting Counts'!G467)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B442,B442)=1,A441+1,A441)","v":1},{"$f":"IF('6a - Lighting Counts'!G468=\"\",\"\",'6a - Lighting Counts'!G468)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B443,B443)=1,A442+1,A442)","v":1},{"$f":"IF('6a - Lighting Counts'!G469=\"\",\"\",'6a - Lighting Counts'!G469)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B444,B444)=1,A443+1,A443)","v":1},{"$f":"IF('6a - Lighting Counts'!G470=\"\",\"\",'6a - Lighting Counts'!G470)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B445,B445)=1,A444+1,A444)","v":1},{"$f":"IF('6a - Lighting Counts'!G471=\"\",\"\",'6a - Lighting Counts'!G471)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B446,B446)=1,A445+1,A445)","v":1},{"$f":"IF('6a - Lighting Counts'!G472=\"\",\"\",'6a - Lighting Counts'!G472)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B447,B447)=1,A446+1,A446)","v":1},{"$f":"IF('6a - Lighting Counts'!G473=\"\",\"\",'6a - Lighting Counts'!G473)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B448,B448)=1,A447+1,A447)","v":1},{"$f":"IF('6a - Lighting Counts'!G474=\"\",\"\",'6a - Lighting Counts'!G474)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B449,B449)=1,A448+1,A448)","v":1},{"$f":"IF('6a - Lighting Counts'!G475=\"\",\"\",'6a - Lighting Counts'!G475)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B450,B450)=1,A449+1,A449)","v":1},{"$f":"IF('6a - Lighting Counts'!G476=\"\",\"\",'6a - Lighting Counts'!G476)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B451,B451)=1,A450+1,A450)","v":1},{"$f":"IF('6a - Lighting Counts'!G477=\"\",\"\",'6a - Lighting Counts'!G477)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B452,B452)=1,A451+1,A451)","v":1},{"$f":"IF('6a - Lighting Counts'!G478=\"\",\"\",'6a - Lighting Counts'!G478)","v":""},{"$f":"IFERROR(VLOOKUP(ROW()-2,$A$3:$B$550,2,FALSE),\"\")","v":""}]
[{"$f":"IF(COUNTIF($B$3:B453,B453)=1,A452+1,A452)","v":1},{"$f":"IF('6a - Lighting Counts'!G479=\"\",\"\",'6a - Lighting Counts'!G479)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B454,B454)=1,A453+1,A453)","v":1},{"$f":"IF('6a - Lighting Counts'!G480=\"\",\"\",'6a - Lighting Counts'!G480)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B455,B455)=1,A454+1,A454)","v":1},{"$f":"IF('6a - Lighting Counts'!G481=\"\",\"\",'6a - Lighting Counts'!G481)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B456,B456)=1,A455+1,A455)","v":1},{"$f":"IF('6a - Lighting Counts'!G482=\"\",\"\",'6a - Lighting Counts'!G482)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B457,B457)=1,A456+1,A456)","v":1},{"$f":"IF('6a - Lighting Counts'!G483=\"\",\"\",'6a - Lighting Counts'!G483)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B458,B458)=1,A457+1,A457)","v":1},{"$f":"IF('6a - Lighting Counts'!G484=\"\",\"\",'6a - Lighting Counts'!G484)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B459,B459)=1,A458+1,A458)","v":1},{"$f":"IF('6a - Lighting Counts'!G485=\"\",\"\",'6a - Lighting Counts'!G485)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B460,B460)=1,A459+1,A459)","v":1},{"$f":"IF('6a - Lighting Counts'!G486=\"\",\"\",'6a - Lighting Counts'!G486)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B461,B461)=1,A460+1,A460)","v":1},{"$f":"IF('6a - Lighting Counts'!G487=\"\",\"\",'6a - Lighting Counts'!G487)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B462,B462)=1,A461+1,A461)","v":1},{"$f":"IF('6a - Lighting Counts'!G488=\"\",\"\",'6a - Lighting Counts'!G488)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B463,B463)=1,A462+1,A462)","v":1},{"$f":"IF('6a - Lighting Counts'!G489=\"\",\"\",'6a - Lighting Counts'!G489)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B464,B464)=1,A463+1,A463)","v":1},{"$f":"IF('6a - Lighting Counts'!G490=\"\",\"\",'6a - Lighting Counts'!G490)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B465,B465)=1,A464+1,A464)","v":1},{"$f":"IF('6a - Lighting Counts'!G491=\"\",\"\",'6a - Lighting Counts'!G491)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B466,B466)=1,A465+1,A465)","v":1},{"$f":"IF('6a - Lighting Counts'!G492=\"\",\"\",'6a - Lighting Counts'!G492)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B467,B467)=1,A466+1,A466)","v":1},{"$f":"IF('6a - Lighting Counts'!G493=\"\",\"\",'6a - Lighting Counts'!G493)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B468,B468)=1,A467+1,A467)","v":1},{"$f":"IF('6a - Lighting Counts'!G494=\"\",\"\",'6a - Lighting Counts'!G494)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B469,B469)=1,A468+1,A468)","v":1},{"$f":"IF('6a - Lighting Counts'!G495=\"\",\"\",'6a - Lighting Counts'!G495)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B470,B470)=1,A469+1,A469)","v":1},{"$f":"IF('6a - Lighting Counts'!G496=\"\",\"\",'6a - Lighting Counts'!G496)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B471,B471)=1,A470+1,A470)","v":1},{"$f":"IF('6a - Lighting Counts'!G497=\"\",\"\",'6a - Lighting Counts'!G497)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B472,B472)=1,A471+1,A471)","v":1},{"$f":"IF('6a - Lighting Counts'!G498=\"\",\"\",'6a - Lighting Counts'!G498)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B473,B473)=1,A472+1,A472)","v":1},{"$f":"IF('6a - Lighting Counts'!G499=\"\",\"\",'6a - Lighting Counts'!G499)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B474,B474)=1,A473+1,A473)","v":1},{"$f":"IF('6a - Lighting Counts'!G500=\"\",\"\",'6a - Lighting Counts'!G500)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B475,B475)=1,A474+1,A474)","v":1},{"$f":"IF('6a - Lighting Counts'!G501=\"\",\"\",'6a - Lighting Counts'!G501)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B476,B476)=1,A475+1,A475)","v":1},{"$f":"IF('6a - Lighting Counts'!G502=\"\",\"\",'6a - Lighting Counts'!G502)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B477,B477)=1,A476+1,A476)","v":1},{"$f":"IF('6a - Lighting Counts'!G503=\"\",\"\",'6a - Lighting Counts'!G503)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B478,B478)=1,A477+1,A477)","v":1},{"$f":"IF('6a - Lighting Counts'!G504=\"\",\"\",'6a - Lighting Counts'!G504)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B479,B479)=1,A478+1,A478)","v":1},{"$f":"IF('6a - Lighting Counts'!G505=\"\",\"\",'6a - Lighting Counts'!G505)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B480,B480)=1,A479+1,A479)","v":1},{"$f":"IF('6a - Lighting Counts'!G506=\"\",\"\",'6a - Lighting Counts'!G506)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B481,B481)=1,A480+1,A480)","v":1},{"$f":"IF('6a - Lighting Counts'!G507=\"\",\"\",'6a - Lighting Counts'!G507)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B482,B482)=1,A481+1,A481)","v":1},{"$f":"IF('6a - Lighting Counts'!G508=\"\",\"\",'6a - Lighting Counts'!G508)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B483,B483)=1,A482+1,A482)","v":1},{"$f":"IF('6a - Lighting Counts'!G509=\"\",\"\",'6a - Lighting Counts'!G509)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B484,B484)=1,A483+1,A483)","v":1},{"$f":"IF('6a - Lighting Counts'!G510=\"\",\"\",'6a - Lighting Counts'!G510)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B485,B485)=1,A484+1,A484)","v":1},{"$f":"IF('6a - Lighting Counts'!G511=\"\",\"\",'6a - Lighting Counts'!G511)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B486,B486)=1,A485+1,A485)","v":1},{"$f":"IF('6a - Lighting Counts'!G512=\"\",\"\",'6a - Lighting Counts'!G512)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B487,B487)=1,A486+1,A486)","v":1},{"$f":"IF('6a - Lighting Counts'!G513=\"\",\"\",'6a - Lighting Counts'!G513)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B488,B488)=1,A487+1,A487)","v":1},{"$f":"IF('6a - Lighting Counts'!G514=\"\",\"\",'6a - Lighting Counts'!G514)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B489,B489)=1,A488+1,A488)","v":1},{"$f":"IF('6a - Lighting Counts'!G515=\"\",\"\",'6a - Lighting Counts'!G515)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B490,B490)=1,A489+1,A489)","v":1},{"$f":"IF('6a - Lighting Counts'!G516=\"\",\"\",'6a - Lighting Counts'!G516)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B491,B491)=1,A490+1,A490)","v":1},{"$f":"IF('6a - Lighting Counts'!G517=\"\",\"\",'6a - Lighting Counts'!G517)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B492,B492)=1,A491+1,A491)","v":1},{"$f":"IF('6a - Lighting Counts'!G518=\"\",\"\",'6a - Lighting Counts'!G518)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B493,B493)=1,A492+1,A492)","v":1},{"$f":"IF('6a - Lighting Counts'!G519=\"\",\"\",'6a - Lighting Counts'!G519)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B494,B494)=1,A493+1,A493)","v":1},{"$f":"IF('6a - Lighting Counts'!G520=\"\",\"\",'6a - Lighting Counts'!G520)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B495,B495)=1,A494+1,A494)","v":1},{"$f":"IF('6a - Lighting Counts'!G521=\"\",\"\",'6a - Lighting Counts'!G521)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B496,B496)=1,A495+1,A495)","v":1},{"$f":"IF('6a - Lighting Counts'!G522=\"\",\"\",'6a - Lighting Counts'!G522)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B497,B497)=1,A496+1,A496)","v":1},{"$f":"IF('6a - Lighting Counts'!G523=\"\",\"\",'6a - Lighting Counts'!G523)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B498,B498)=1,A497+1,A497)","v":1},{"$f":"IF('6a - Lighting Counts'!G524=\"\",\"\",'6a - Lighting Counts'!G524)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B499,B499)=1,A498+1,A498)","v":1},{"$f":"IF('6a - Lighting Counts'!G525=\"\",\"\",'6a - Lighting Counts'!G525)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B500,B500)=1,A499+1,A499)","v":1},{"$f":"IF('6a - Lighting Counts'!G526=\"\",\"\",'6a - Lighting Counts'!G526)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B501,B501)=1,A500+1,A500)","v":1},{"$f":"IF('6a - Lighting Counts'!G527=\"\",\"\",'6a - Lighting Counts'!G527)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B502,B502)=1,A501+1,A501)","v":1},{"$f":"IF('6a - Lighting Counts'!G528=\"\",\"\",'6a - Lighting Counts'!G528)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B503,B503)=1,A502+1,A502)","v":1},{"$f":"IF('6a - Lighting Counts'!G529=\"\",\"\",'6a - Lighting Counts'!G529)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B504,B504)=1,A503+1,A503)","v":1},{"$f":"IF('6a - Lighting Counts'!G530=\"\",\"\",'6a - Lighting Counts'!G530)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B505,B505)=1,A504+1,A504)","v":1},{"$f":"IF('6a - Lighting Counts'!G531=\"\",\"\",'6a - Lighting Counts'!G531)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B506,B506)=1,A505+1,A505)","v":1},{"$f":"IF('6a - Lighting Counts'!G532=\"\",\"\",'6a - Lighting Counts'!G532)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B507,B507)=1,A506+1,A506)","v":1},{"$f":"IF('6a - Lighting Counts'!G533=\"\",\"\",'6a - Lighting Counts'!G533)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B508,B508)=1,A507+1,A507)","v":1},{"$f":"IF('6a - Lighting Counts'!G534=\"\",\"\",'6a - Lighting Counts'!G534)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B509,B509)=1,A508+1,A508)","v":1},{"$f":"IF('6a - Lighting Counts'!G535=\"\",\"\",'6a - Lighting Counts'!G535)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B510,B510)=1,A509+1,A509)","v":1},{"$f":"IF('6a - Lighting Counts'!G536=\"\",\"\",'6a - Lighting Counts'!G536)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B511,B511)=1,A510+1,A510)","v":1},{"$f":"IF('6a - Lighting Counts'!G537=\"\",\"\",'6a - Lighting Counts'!G537)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B512,B512)=1,A511+1,A511)","v":1},{"$f":"IF('6a - Lighting Counts'!G538=\"\",\"\",'6a - Lighting Counts'!G538)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B513,B513)=1,A512+1,A512)","v":1},{"$f":"IF('6a - Lighting Counts'!G539=\"\",\"\",'6a - Lighting Counts'!G539)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B514,B514)=1,A513+1,A513)","v":1},{"$f":"IF('6a - Lighting Counts'!G540=\"\",\"\",'6a - Lighting Counts'!G540)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B515,B515)=1,A514+1,A514)","v":1},{"$f":"IF('6a - Lighting Counts'!G541=\"\",\"\",'6a - Lighting Counts'!G541)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B516,B516)=1,A515+1,A515)","v":1},{"$f":"IF('6a - Lighting Counts'!G542=\"\",\"\",'6a - Lighting Counts'!G542)","v":""},{"$f":"IFERROR(VLOOKUP(ROW()-2,$A$3:$B$550,2,FALSE),\"\")","v":""}]
[{"$f":"IF(COUNTIF($B$3:B517,B517)=1,A516+1,A516)","v":1},{"$f":"IF('6a - Lighting Counts'!G543=\"\",\"\",'6a - Lighting Counts'!G543)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B518,B518)=1,A517+1,A517)","v":1},{"$f":"IF('6a - Lighting Counts'!G544=\"\",\"\",'6a - Lighting Counts'!G544)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B519,B519)=1,A518+1,A518)","v":1},{"$f":"IF('6a - Lighting Counts'!G545=\"\",\"\",'6a - Lighting Counts'!G545)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B520,B520)=1,A519+1,A519)","v":1},{"$f":"IF('6a - Lighting Counts'!G546=\"\",\"\",'6a - Lighting Counts'!G546)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B521,B521)=1,A520+1,A520)","v":1},{"$f":"IF('6a - Lighting Counts'!G547=\"\",\"\",'6a - Lighting Counts'!G547)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B522,B522)=1,A521+1,A521)","v":1},{"$f":"IF('6a - Lighting Counts'!G548=\"\",\"\",'6a - Lighting Counts'!G548)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B523,B523)=1,A522+1,A522)","v":1},{"$f":"IF('6a - Lighting Counts'!G549=\"\",\"\",'6a - Lighting Counts'!G549)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B524,B524)=1,A523+1,A523)","v":1},{"$f":"IF('6a - Lighting Counts'!G550=\"\",\"\",'6a - Lighting Counts'!G550)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B525,B525)=1,A524+1,A524)","v":1},{"$f":"IF('6a - Lighting Counts'!G551=\"\",\"\",'6a - Lighting Counts'!G551)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B526,B526)=1,A525+1,A525)","v":1},{"$f":"IF('6a - Lighting Counts'!G552=\"\",\"\",'6a - Lighting Counts'!G552)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B527,B527)=1,A526+1,A526)","v":1},{"$f":"IF('6a - Lighting Counts'!G553=\"\",\"\",'6a - Lighting Counts'!G553)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B528,B528)=1,A527+1,A527)","v":1},{"$f":"IF('6a - Lighting Counts'!G554=\"\",\"\",'6a - Lighting Counts'!G554)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B529,B529)=1,A528+1,A528)","v":1},{"$f":"IF('6a - Lighting Counts'!G555=\"\",\"\",'6a - Lighting Counts'!G555)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B530,B530)=1,A529+1,A529)","v":1},{"$f":"IF('6a - Lighting Counts'!G556=\"\",\"\",'6a - Lighting Counts'!G556)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B531,B531)=1,A530+1,A530)","v":1},{"$f":"IF('6a - Lighting Counts'!G557=\"\",\"\",'6a - Lighting Counts'!G557)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B532,B532)=1,A531+1,A531)","v":1},{"$f":"IF('6a - Lighting Counts'!G558=\"\",\"\",'6a - Lighting Counts'!G558)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B533,B533)=1,A532+1,A532)","v":1},{"$f":"IF('6a - Lighting Counts'!G559=\"\",\"\",'6a - Lighting Counts'!G559)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B534,B534)=1,A533+1,A533)","v":1},{"$f":"IF('6a - Lighting Counts'!G560=\"\",\"\",'6a - Lighting Counts'!G560)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B535,B535)=1,A534+1,A534)","v":1},{"$f":"IF('6a - Lighting Counts'!G561=\"\",\"\",'6a - Lighting Counts'!G561)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B536,B536)=1,A535+1,A535)","v":1},{"$f":"IF('6a - Lighting Counts'!G562=\"\",\"\",'6a - Lighting Counts'!G562)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B537,B537)=1,A536+1,A536)","v":1},{"$f":"IF('6a - Lighting Counts'!G563=\"\",\"\",'6a - Lighting Counts'!G563)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B538,B538)=1,A537+1,A537)","v":1},{"$f":"IF('6a - Lighting Counts'!G564=\"\",\"\",'6a - Lighting Counts'!G564)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B539,B539)=1,A538+1,A538)","v":1},{"$f":"IF('6a - Lighting Counts'!G565=\"\",\"\",'6a - Lighting Counts'!G565)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B540,B540)=1,A539+1,A539)","v":1},{"$f":"IF('6a - Lighting Counts'!G566=\"\",\"\",'6a - Lighting Counts'!G566)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B541,B541)=1,A540+1,A540)","v":1},{"$f":"IF('6a - Lighting Counts'!G567=\"\",\"\",'6a - Lighting Counts'!G567)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B542,B542)=1,A541+1,A541)","v":1},{"$f":"IF('6a - Lighting Counts'!G568=\"\",\"\",'6a - Lighting Counts'!G568)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B543,B543)=1,A542+1,A542)","v":1},{"$f":"IF('6a - Lighting Counts'!G569=\"\",\"\",'6a - Lighting Counts'!G569)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B544,B544)=1,A543+1,A543)","v":1},{"$f":"IF('6a - Lighting Counts'!G570=\"\",\"\",'6a - Lighting Counts'!G570)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B545,B545)=1,A544+1,A544)","v":1},{"$f":"IF('6a - Lighting Counts'!G571=\"\",\"\",'6a - Lighting Counts'!G571)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B546,B546)=1,A545+1,A545)","v":1},{"$f":"IF('6a - Lighting Counts'!G572=\"\",\"\",'6a - Lighting Counts'!G572)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B547,B547)=1,A546+1,A546)","v":1},{"$f":"IF('6a - Lighting Counts'!G573=\"\",\"\",'6a - Lighting Counts'!G573)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B548,B548)=1,A547+1,A547)","v":1},{"$f":"IF('6a - Lighting Counts'!G574=\"\",\"\",'6a - Lighting Counts'!G574)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B549,B549)=1,A548+1,A548)","v":1},{"$f":"IF('6a - Lighting Counts'!G575=\"\",\"\",'6a - Lighting Counts'!G575)","v":""},""]
[{"$f":"IF(COUNTIF($B$3:B550,B550)=1,A549+1,A549)","v":1},{"$f":"IF('6a - Lighting Counts'!G576=\"\",\"\",'6a - Lighting Counts'!G576)","v":""},""]

{"sheet":"Lighting Assumptions 90.1-2007","index":18,"n_rows":111,"n_cols":23,"rows_kept":111,"cut":false,"hidden":true,"merged":[[42,11,43,11],[42,12,43,12],[14,13,14,14],[14,15,14,16],[14,17,14,18],[14,19,14,20],[14,21,14,22],[41,13,41,14],[41,15,41,16],[41,17,41,18],[41,19,41,20],[41,21,41,22],[0,12,1,12],[0,3,1,3],[0,4,0,5],[0,6,1,6],[0,7,0,8],[0,11,1,11]]}
[null,null,"*** THESE ARE NOT 2007 VALUES. THESE TABLES ARE HERE AS A PLACEHOLDER.","Building Area Method Categories","Table 9.5.1 LPD",null,"Space by Space Categories","Table 9.6.1 LPD ",null,"Table 9.6.1 LPD ","Table 9.6.1 LPD ","Tradable Surfaces","Required Input","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter"]
[null,null,null,null,"(W/sq ft)","(W/sq m)",null,"(W/sq ft)","(W/sq m)","occupancy sensor required?","Dayighting required?",null,null,"IP","SI","IP","SI","IP","SI","IP","SI","IP","SI"]
[null,null,null,"Automotive facility",0.8,{"$f":"E3*10.7639","v":8.6111199999999997},"Audience Seating/Auditorium",0.63,{"$f":"H3*10.7639","v":6.7812570000000001},"No","Yes",null,null,{"$f":"N1&\" \"&N2","v":"W/sf or W/linear foot IP"},"W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI"]
[null,null,null,"Convention center",1.01,{"$f":"E4*10.7639","v":10.871539},"Audience Seating/Convention center",0.82,{"$f":"H4*10.7639","v":8.8263979999999993},"No","Yes","Parking lots and drives","Area","No Allowance","No Allowance",0.04,{"$f":"P4*10.7639","v":0.43055599999999999},0.06,{"$f":"R4*10.7639","v":0.64583399999999991},0.1,{"$f":"T4*10.7639","v":1.07639},0.13,{"$f":"V4*10.7639","v":1.3993070000000001}]
[null,null,null,"Courthouse",1.01,10.871539,"Audience Seating/Gymnasium",0.65,6.9965349999999997,"No","Yes","Walkways less than 10 ft wide","Length","No Allowance","No Allowance",0.7,{"$f":"P5*3.28","v":2.2959999999999998},0.7,{"$f":"R5*3.28","v":2.2959999999999998},0.8,{"$f":"T5*3.28","v":2.6240000000000001},1,{"$f":"V5*3.28","v":3.28}]
[null,null,null,"Dining: bar lounge/leisure",1.01,10.871539,"Audience Seating/Motion Picture Theatre",1.1399999999999999,12.270845999999999,"No","Yes","Walkways 10 ft wide or greater","Area","No Allowance","No Allowance",0.14000000000000001,{"$f":"P6*10.7639","v":1.5069460000000001},0.14000000000000001,{"$f":"R6*10.7639","v":1.5069460000000001},0.16,{"$f":"T6*10.7639","v":1.722224},0.2,{"$f":"V6*10.7639","v":2.1527799999999999}]
[null,null,null,"Dining: cafeteria/fast food",0.9,9.6875099999999996,"Audience Seating/Penitentiary",0.28000000000000003,3.0138920000000002,"No","Yes","Plaza areas","Area","No Allowance","No Allowance",0.14000000000000001,1.5069460000000001,0.14000000000000001,1.5069460000000001,0.16,1.722224,0.2,2.1527799999999999]
[null,null,null,"Dining: family",0.95,10.225705,"Audience Seating/Performing Arts Theater",2.4300000000000002,26.156276999999999,"No","Yes","Special feature areas","Area","No Allowance","No Allowance",0.14000000000000001,1.5069460000000001,0.14000000000000001,1.5069460000000001,0.16,1.722224,0.2,2.1527799999999999]
[null,null,null,"Dormitory",0.56999999999999995,6.1354229999999994,"Audience Seating/Religious Building",1.53,16.468767,"No","Yes","Stairways","Area","No Allowance","No Allowance",0.75,8.0729249999999997,1,10.7639,1,10.7639,1,10.7639]
[null,null,null,"Exercise center",0.84,9.0416759999999989,"Audience Seating/Sports Arena",0.43,4.6284770000000002,"No","Yes","Main entries","Length","No Allowance","No Allowance",20,{"$f":"P10*3.28","v":65.599999999999994},20,{"$f":"R10*3.28","v":65.599999999999994},30,{"$f":"T10*3.28","v":98.399999999999991},30,{"$f":"V10*3.28","v":98.399999999999991}]
[null,null,null,"Fire Station",0.67100000000000004,7.2225769,"Audience Seating/Transportation facility",0.43,4.6284770000000002,"No","Yes","Other doors","Length","No Allowance","No Allowance",20,{"$f":"P11*3.28","v":65.599999999999994},20,{"$f":"R11*3.28","v":65.599999999999994},20,{"$f":"T11*3.28","v":65.599999999999994},20,{"$f":"V11*3.28","v":65.599999999999994}]
[null,null,null,"Gymnasium",0.94,10.118065999999999,"Audience Seating/All Other",0.43,4.6284770000000002,"No","Yes","Canopies (free standing and attached and overhangs)","Area","No Allowance","No Allowance",0.25,2.6909749999999999,0.25,2.6909749999999999,0.4,4.3055599999999998,0.4,4.3055599999999998]
[null,null,null,"Health-care clinic",0.9,9.6875099999999996,"Atrium ≤40 ft high","0.03/ft total height","0.03/ft total height","Yes","Yes","Outdoor Sales Open areas (including vehicle sales lots)","Area","No Allowance","No Allowance",0.25,2.6909749999999999,0.25,2.6909749999999999,0.5,5.3819499999999998,0.75,8.0729249999999997]
[null,null,null,"Hospital",1.05,11.302095,"Atrium >40 ft high","0.40 + 0.02/ft\ntotal height","0.40 + 0.02/ft\ntotal height","Yes","Yes","Outdoor Sales Street frontage for vehicle sales lots in addition to open-area allowance)","Length","No Allowance","No Allowance","No Allowance","No Allowance",10,{"$f":"R14*3.28","v":32.799999999999997},10,{"$f":"T14*3.28","v":32.799999999999997},30,{"$f":"V14*3.28","v":98.399999999999991}]
[null,null,null,"Hotel/motel",0.87,9.3645929999999993,"Banking Activity Area",1.01,10.871539,"No","Yes",null,null,"Zone 0",null,"Zone 1",null,"Zone 2",null,"Zone 3",null,"Zone 4"]
[null,null,null,"Library",1.19,12.809040999999999,"Classroom/Lecture Hall/Training Room in Penitentiary",1.34,14.423626000000001,"Yes","Yes","IPParking lots and drives",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N4,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P4,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R4,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T4,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V4,\"\")))))","v":""}]
[null,null,null,"Manufacturing facility",1.17,12.593762999999999,"Classroom/Lecture Hall/Training Room in All Other",1.24,13.347235999999999,"Yes","Yes","IPWalkways less than 10 ft wide",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N5,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P5,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R5,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T5,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V5,\"\")))))","v":""}]
[null,null,null,"Motion picture theater",0.76,8.1805640000000004,"Conference/Meeting/Multipurpose Room",1.23,13.239597,"Yes","Yes","IPWalkways 10 ft wide or greater",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N6,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P6,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R6,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T6,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V6,\"\")))))","v":""}]
[null,null,null,"Multifamily",0.51,5.4895889999999996,"Confinement Cells",0.81,8.7187590000000004,"No","Yes","IPPlaza areas",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N7,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P7,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R7,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T7,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V7,\"\")))))","v":""}]
[null,null,null,"Museum",1.02,10.979177999999999,"Copy/Print Room",0.72,7.7500079999999993,"Yes","Yes","IPSpecial feature areas",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N8,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P8,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R8,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T8,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V8,\"\")))))","v":""}]
[null,null,null,"Office",0.82,8.8263979999999993,"Corridor/Facility for Visually Impaired",0.92,9.9027879999999993,"Yes","Yes","IPStairways",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N9,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P9,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R9,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T9,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V9,\"\")))))","v":""}]
[null,null,null,"Parking garage",0.21,2.2604189999999997,"Corridor/Hospital",0.99,10.656260999999999,"No","Yes","IPMain entries",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N10,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P10,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R10,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T10,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V10,\"\")))))","v":""}]
[null,null,null,"Penitentiary",0.81,8.7187590000000004,"Corridor/Manufacturing Facility",0.41,4.4131989999999996,"No","Yes","IPOther doors",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N11,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P11,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R11,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T11,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V11,\"\")))))","v":""}]
[null,null,null,"Performing arts theater",1.39,14.961820999999999,"Corridor/All Other",0.66,7.1041740000000004,"Yes","Yes","IPCanopies (free standing and attached and overhangs)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N12,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P12,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R12,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T12,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V12,\"\")))))","v":""}]
[null,null,null,"Police station",0.87,9.3645929999999993,"Courtroom",1.72,18.513908000000001,"No","Yes","IPOutdoor Sales Open areas (including vehicle sales lots)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N13,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P13,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R13,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T13,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V13,\"\")))))","v":""}]
[null,null,null,"Post office",0.87,9.3645929999999993,"Computer Room",1.71,18.406268999999998,"No","Yes","IPOutdoor Sales Street frontage for vehicle sales lots in addition to open-area allowance)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N14,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P14,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R14,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T14,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V14,\"\")))))","v":""}]
[null,null,null,"Religious building",1,10.7639,"Dining Area/Penitentiary",0.96,10.333343999999999,"No","Yes","SIParking lots and drives",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O4,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q4,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S4,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U4,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W4,\"\")))))","v":""}]
[null,null,null,"Retail",1.26,13.562514,"Dining Area/Facility for Visually Impaired",2.65,28.524334999999997,"No","Yes","SIWalkways less than 10 ft wide",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O5,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q5,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S5,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U5,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W5,\"\")))))","v":""}]
[null,null,null,"School/university",0.87,9.3645929999999993,"Dining Area/bar/Lounge or Leisure Dining",1.07,11.517373000000001,"No","Yes","SIWalkways 10 ft wide or greater",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O6,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q6,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S6,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U6,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W6,\"\")))))","v":""}]
[null,null,null,"Sports arena",0.91,9.7951490000000003,"Dining Area/Cafeteria/Fast Food",0.65,6.9965349999999997,"No","Yes","SIPlaza areas",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O7,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q7,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S7,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U7,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W7,\"\")))))","v":""}]
[null,null,null,"Town hall",0.89,9.5798709999999989,"Dining Area/Family Dining",0.89,9.5798709999999989,"No","Yes","SISpecial feature areas",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O8,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q8,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S8,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U8,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W8,\"\")))))","v":""}]
[null,null,null,"Transportation",0.7,7.5347299999999988,"Dining Area/All Other",0.65,6.9965349999999997,"No","Yes","SIStairways",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O9,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q9,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S9,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U9,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W9,\"\")))))","v":""}]
[null,null,null,"Warehouse",0.66,7.1041740000000004,"Electrical/Mechanical Room",0.42,4.5208379999999995,"No","Yes","SIMain entries",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O10,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q10,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S10,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U10,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W10,\"\")))))","v":""}]
[null,null,null,"Workshop",1.119,12.0448041,"Emergency Vehicle Garage",0.56000000000000005,6.0277840000000005,"No","Yes","SIOther doors",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O11,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q11,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S11,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U11,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W11,\"\")))))","v":""}]
[null,null,null,null,null,null,"Food Preparation Area",1.21,13.024318999999998,"No","Yes","SICanopies (free standing and attached and overhangs)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O12,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q12,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S12,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U12,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W12,\"\")))))","v":""}]
[null,null,null,null,null,null,"Guest Room",0.91,9.7951490000000003,"No","Yes","SIOutdoor Sales Open areas (including vehicle sales lots)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O13,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q13,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S13,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U13,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W13,\"\")))))","v":""}]
[null,null,null,null,null,null,"Judges Chambers",0.93,10.010427,"Yes","Yes","SIOutdoor Sales Street frontage for vehicle sales lots in addition to open-area allowance)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O14,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q14,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S14,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U14,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W14,\"\")))))","v":""}]
[null,null,null,null,null,null,"Laboratory/Classroom",1.43,15.392376999999998,"Yes","Yes"]
[null,null,null,null,null,null,"Laboratory/All Other",1.81,19.482658999999998,"No","Yes"]
[null,null,null,null,null,null,"Laundry/Washing Area",0.6,6.4583399999999997,"No","Yes"]
[null,null,null,null,null,null,"Loading Dock, Interior",0.47,5.0590329999999994,"No","Yes"]
[null,null,null,null,null,null,"Lobby/Facility for Visually Impaired",1.8,19.375019999999999,"Yes","Yes",null,null,"Zone 0",null,"Zone 1",null,"Zone 2",null,"Zone 3",null,"Zone 4"]
[null,null,null,null,null,null,"Lobby/Elevator",0.64,6.8888959999999999,"No","Yes","Nontradable Surfaces","Required Input","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter"]
[null,null,null,null,null,null,"Lobby/Hotel",1.06,11.409734,"No","Yes",null,null,"IP","SI","IP","SI","IP","SI","IP","SI","IP","SI"]
[null,null,null,null,null,null,"Lobby/Motion Picture Theater",0.59,6.350700999999999,"No","Yes",null,null,{"$f":"N43&\" \"&N44","v":"W/sf or W/linear foot IP"},"W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI"]
[null,null,null,null,null,null,"Lobby/Performing Arts Theater",2,21.527799999999999,"Yes","Yes","Building facades","Area","No Allowance","No Allowance","No Allowance","No Allowance",0.1,{"$f":"R46*10.7639","v":1.07639},0.15,{"$f":"T46*10.7639","v":1.6145849999999999},0.2,{"$f":"V46*10.7639","v":2.1527799999999999}]
[null,null,null,null,null,null,"Lobby/All Other",0.9,9.6875099999999996,"Yes","Yes","ATMs and night depositories","Length","No Allowance","No Allowance","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional"]
[null,null,null,null,null,null,"Locker Room",0.75,8.0729249999999997,"Yes","Yes","Entrances and gatehouse inspection stations at guarded facilities","Area","No Allowance","No Allowance",0.75,{"$f":"P48*10.7639","v":8.0729249999999997},0.75,{"$f":"R48*10.7639","v":8.0729249999999997},0.75,{"$f":"T48*10.7639","v":8.0729249999999997},0.75,{"$f":"V48*10.7639","v":8.0729249999999997}]
[null,null,null,null,null,null,"Lounge/Breakroom/in Healthcare Facility",0.92,9.9027879999999993,"Yes","Yes","Loading areas for law enforcement, fire, ambulance, and other emergency service vehicles","Area","No Allowance","No Allowance",0.5,{"$f":"P49*10.7639","v":5.3819499999999998},0.5,{"$f":"R49*10.7639","v":5.3819499999999998},0.5,{"$f":"T49*10.7639","v":5.3819499999999998},0.5,{"$f":"V49*10.7639","v":5.3819499999999998}]
[null,null,null,null,null,null,"Lounge/Breakroom/All Other",0.73,7.8576469999999992,"Yes","Yes","Drive-through windows at fast food restaurants","Length","No Allowance","No Allowance",400,400,400,400,400,400,400,400]
[null,null,null,null,null,null,"Office/Enclosed",1.1100000000000001,11.947929,"Yes","Yes","Parking near 24-hour retail entrances","Length","No Allowance","No Allowance",800,800,800,800,800,800,800,800]
[null,null,null,null,null,null,"Office/Open Plan",0.8,8.6111199999999997,"No","Yes","Building facades","Length","No Allowance","No Allowance","No Allowance","No Allowance",2.5,{"$f":"R52*3.28","v":8.1999999999999993},3.75,{"$f":"T52*3.28","v":12.299999999999999},5,{"$f":"V52*3.28","v":16.399999999999999}]
[null,null,null,null,null,null,"Parking Area, Interior",0.19,2.0451410000000001,"No","Yes"]
[null,null,null,null,null,null,"Pharmacy Area",0.19,2.0451410000000001,"No","Yes",{"$f":"\"IP\"&L46&M46","v":"IPBuilding facadesArea"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N46,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P46,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R46,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T46,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V46,\"\")))))","v":""}]
[null,null,null,null,null,null,"Restroom/Facility for the Visually Impaired",1.21,13.024318999999998,"Yes","Yes",{"$f":"\"IP\"&L47","v":"IPATMs and night depositories"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N47,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P47,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R47,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T47,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V47,\"\")))))","v":""}]
[null,null,null,null,null,null,"Restroom/ All Other",0.98,10.548622,"Yes","Yes",{"$f":"\"IP\"&L48","v":"IPEntrances and gatehouse inspection stations at guarded facilities"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N48,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P48,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R48,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T48,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V48,\"\")))))","v":""}]
[null,null,null,null,null,null,"Sales Area",1.44,15.500015999999999,"No","Yes",{"$f":"\"IP\"&L49","v":"IPLoading areas for law enforcement, fire, ambulance, and other emergency service vehicles"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N49,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P49,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R49,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T49,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V49,\"\")))))","v":""}]
[null,null,null,null,null,null,"Seating Area, General",0.54,5.812506,"No","Yes",{"$f":"\"IP\"&L50","v":"IPDrive-through windows at fast food restaurants"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N50,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P50,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R50,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T50,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V50,\"\")))))","v":""}]
[null,null,null,null,null,null,"Stairwell",0.69,7.427090999999999,"Yes","Yes",{"$f":"\"IP\"&L51","v":"IPParking near 24-hour retail entrances"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N51,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P51,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R51,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T51,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V51,\"\")))))","v":""}]
[null,null,null,null,null,null,"Storage Room/Hospital",0.63,6.7812570000000001,"No","Yes",{"$f":"\"IP\"&L52&M52","v":"IPBuilding facadesLength"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N52,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P52,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R52,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T52,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V52,\"\")))))","v":""}]
[null,null,null,null,null,null,"Storage Room/≥50 sqft",0.63,6.7812570000000001,"Yes","Yes",{"$f":"\"SI\"&L46&M46","v":"SIBuilding facadesArea"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O46,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q46,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S46,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U46,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W46,\"\")))))","v":""}]
[null,null,null,null,null,null,"Storage Room/<50 sgft",1.24,13.347235999999999,"No","Yes",{"$f":"\"SI\"&L47","v":"SIATMs and night depositories"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O47,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q47,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S47,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U47,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W47,\"\")))))","v":""}]
[null,null,null,null,null,null,"Vehicular Maintenance Area",0.67,7.2118130000000003,"No","Yes",{"$f":"\"SI\"&L48","v":"SIEntrances and gatehouse inspection stations at guarded facilities"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O48,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q48,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S48,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U48,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W48,\"\")))))","v":""}]
[null,null,null,null,null,null,"Workshop",1.59,17.114601,"No","Yes",{"$f":"\"SI\"&L49","v":"SILoading areas for law enforcement, fire, ambulance, and other emergency service vehicles"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O49,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q49,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S49,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U49,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W49,\"\")))))","v":""}]
[null,null,null,null,null,null,"Assisted Living Facility/Chapel",2.21,23.788218999999998,"No","Yes",{"$f":"\"SI\"&L50","v":"SIDrive-through windows at fast food restaurants"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O50,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q50,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S50,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U50,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W50,\"\")))))","v":""}]
[null,null,null,null,null,null,"Assisted Living Facility/Recreation Room",2.41,25.940999000000001,"No","No",{"$f":"\"SI\"&L51","v":"SIParking near 24-hour retail entrances"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O51,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q51,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S51,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U51,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W51,\"\")))))","v":""}]
[null,null,null,null,null,null,"Convention Center-Exhibit Space",1.45,15.607654999999999,"No","Yes",{"$f":"\"SI\"&L52&M52","v":"SIBuilding facadesLength"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O52,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q52,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S52,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U52,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W52,\"\")))))","v":""}]
[null,null,null,null,null,null,"Dormitory-Living Quarters",0.38,{"$f":"H68*10.7639","v":4.0902820000000002},"No","No"]
[null,null,null,null,null,null,"Fire Station-Sleeping Quarters",0.22,2.368058,"No","No"]
[null,null,null,null,null,null,"Gymnasium/Fitness Center/Exercise Area",0.72,7.7500079999999993,"No","Yes"]
[null,null,null,null,null,null,"Gymnasium/Fitness Center/Playing Area",1.2,12.916679999999999,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Emergency Room",1.68,18.083351999999998,"Yes","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Exam/Treatment Room",1.66,17.868074,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Imaging Room",1.51,16.253488999999998,"No","No"]
[null,null,null,null,null,null,"Healthcare Facility/Medical Supply Room",0.74,7.9652859999999999,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Nursery",0.88,9.472232,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Nurses Station",0.71,7.6423689999999995,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Operating Room",2.48,26.694471999999998,"No","No"]
[null,null,null,null,null,null,"Healthcare Facility/Patient Room",0.62,6.6736179999999994,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Physical Therapy Room",0.91,9.7951490000000003,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Recovery Room",1.1499999999999999,12.378484999999998,"No","Yes"]
[null,null,null,null,null,null,"Library/Reading Area",1.06,11.409734,"No","Yes"]
[null,null,null,null,null,null,"Library/Stacks",1.71,18.406268999999998,"Yes","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/Detailed Manufacturing Area",1.29,13.885431000000001,"No","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/Equipment Room",0.74,7.9652859999999999,"No","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/Extra High Bay Area (>50 ft floor-to-ceiling height)",1.05,11.302095,"No","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/High Bay Area (25-50 ft floor-to-ceiling height)",1.23,13.239597,"No","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/Low Bay Area (<25 ft floor-to-ceiling height)",1.19,12.809040999999999,"No","Yes"]
[null,null,null,null,null,null,"Museum/General Exhibition Area",1.05,11.302095,"No","Yes"]
[null,null,null,null,null,null,"Museum/Restoration Room",1.02,10.979177999999999,"No","Yes"]
[null,null,null,null,null,null,"Post Office/Sorting Area",0.94,10.118065999999999,"Yes","Yes"]
[null,null,null,null,null,null,"Religious Building/Fellowship Hall",0.64,6.8888959999999999,"No","Yes"]
[null,null,null,null,null,null,"Religious building/Worship/Choir area",1.53,16.468767,"No","Yes"]
[null,null,null,null,null,null,"Retail Facilities/Dressing/Fitting Room",0.71,7.6423689999999995,"Yes","Yes"]
[null,null,null,null,null,null,"Retail Facilities/Mall Concourse",1.1000000000000001,11.840290000000001,"No","Yes"]
[null,null,null,null,null,null,"Sporting Arena-Playing Area/Class I Facility",3.68,39.611151999999997,"No","Yes"]
[null,null,null,null,null,null,"Sporting Arena-Playing Area/Class II Facility",2.4,25.833359999999999,"No","Yes"]
[null,null,null,null,null,null,"Sporting Arena-Playing Area/Class III Facility",1.8,19.375019999999999,"No","Yes"]
[null,null,null,null,null,null,"Sporting Arena-Playing Area/Class IV Facility",1.2,12.916679999999999,"No","Yes"]
[null,null,null,null,null,null,"Transportation Facility/Baggage/Carousel Area",0.53,5.7048670000000001,"No","Yes"]
[null,null,null,null,null,null,"Transportation Facility/Airport Concourse",0.36,3.8750039999999997,"No","Yes"]
[null,null,null,null,null,null,"Transportation Facility/Terminal Ticket Counter",0.8,8.6111199999999997,"No","Yes"]
[null,null,null,null,null,null,"Warehouse-Storage Area/Medium to Bulky, Palletized Items",0.57999999999999996,6.2430619999999992,"Yes","Yes"]
[null,null,null,null,null,null,"Warehouse-Storage Area/Smaller, Hand Carried Items",0.95,10.225705,"Yes","Yes"]
[null,null,null,null,null,null,"Dwelling Unit",0.7,7.5347299999999988,"No","No"]
[null,null,null,null,null,null,"Multiple","See 9.6.1 (a)","See 9.6.1 (a)","See 9.6.1 (a)","See 9.6.1 (a)"]
[]
[null,null,null,null,null,null,"\"Similar\" space types used to map from Table G3.7 (BM baseline) to 90.1 2013 Table 9.6.1"]
[null,null,null,null,null,null,"Judges Chamber = Office"]
[null,null,null,null,null,null,"Dwelling Unit Controls = Dormitory - living quarters"]
[null,null,null,null,null,null,"Health Care Facility / Emergency Room = Exam / Treatment room"]

{"sheet":"Lighting Assumptions 90.1-2013","index":19,"n_rows":111,"n_cols":23,"rows_kept":111,"cut":false,"hidden":true,"merged":[[0,12,1,12],[0,3,1,3],[0,4,0,5],[0,6,1,6],[0,7,0,8],[0,11,1,11],[42,11,43,11],[42,12,43,12],[14,13,14,14],[14,15,14,16],[14,17,14,18],[14,21,14,22],[41,13,41,14],[41,15,41,16],[41,17,41,18],[41,19,41,20],[41,21,41,22],[14,19,14,20]]}
[null,null,null,"Building Area Method Categories","Table 9.5.1 LPD",null,"Space by Space Categories","Table 9.6.1 LPD ",null,"Table 9.6.1 LPD ","Table 9.6.1 LPD ","Tradable Surfaces","Required Input","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter"]
[null,null,null,null,"(W/sq ft)","(W/sq m)",null,"(W/sq ft)","(W/sq m)","occupancy sensor required?","Dayighting required?",null,null,"IP","SI","IP","SI","IP","SI","IP","SI","IP","SI"]
[null,null,null,"Automotive facility",0.8,{"$f":"E3*10.7639","v":8.6111199999999997},"Audience Seating/Auditorium",0.63,{"$f":"H3*10.7639","v":6.7812570000000001},"No","Yes",null,null,{"$f":"N1&\" \"&N2","v":"W/sf or W/linear foot IP"},"W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI"]
[null,null,null,"Convention center",1.01,{"$f":"E4*10.7639","v":10.871539},"Audience Seating/Convention center",0.82,{"$f":"H4*10.7639","v":8.8263979999999993},"No","Yes","Parking lots and drives","Area","No Allowance","No Allowance",0.04,{"$f":"P4*10.7639","v":0.43055599999999999},0.06,{"$f":"R4*10.7639","v":0.64583399999999991},0.1,{"$f":"T4*10.7639","v":1.07639},0.13,{"$f":"V4*10.7639","v":1.3993070000000001}]
[null,null,null,"Courthouse",1.01,10.871539,"Audience Seating/Gymnasium",0.65,6.9965349999999997,"No","Yes","Walkways less than 10 ft wide","Length","No Allowance","No Allowance",0.7,{"$f":"P5*3.28","v":2.2959999999999998},0.7,{"$f":"R5*3.28","v":2.2959999999999998},0.8,{"$f":"T5*3.28","v":2.6240000000000001},1,{"$f":"V5*3.28","v":3.28}]
[null,null,null,"Dining: bar lounge/leisure",1.01,10.871539,"Audience Seating/Motion Picture Theatre",1.1399999999999999,12.270845999999999,"No","Yes","Walkways 10 ft wide or greater","Area","No Allowance","No Allowance",0.14000000000000001,{"$f":"P6*10.7639","v":1.5069460000000001},0.14000000000000001,{"$f":"R6*10.7639","v":1.5069460000000001},0.16,{"$f":"T6*10.7639","v":1.722224},0.2,{"$f":"V6*10.7639","v":2.1527799999999999}]
[null,null,null,"Dining: cafeteria/fast food",0.9,9.6875099999999996,"Audience Seating/Penitentiary",0.28000000000000003,3.0138920000000002,"No","Yes","Plaza areas","Area","No Allowance","No Allowance",0.14000000000000001,1.5069460000000001,0.14000000000000001,1.5069460000000001,0.16,1.722224,0.2,2.1527799999999999]
[null,null,null,"Dining: family",0.95,10.225705,"Audience Seating/Performing Arts Theater",2.4300000000000002,26.156276999999999,"No","Yes","Special feature areas","Area","No Allowance","No Allowance",0.14000000000000001,1.5069460000000001,0.14000000000000001,1.5069460000000001,0.16,1.722224,0.2,2.1527799999999999]
[null,null,null,"Dormitory",0.56999999999999995,6.1354229999999994,"Audience Seating/Religious Building",1.53,16.468767,"No","Yes","Stairways","Area","No Allowance","No Allowance",0.75,8.0729249999999997,1,10.7639,1,10.7639,1,10.7639]
[null,null,null,"Exercise center",0.84,9.0416759999999989,"Audience Seating/Sports Arena",0.43,4.6284770000000002,"No","Yes","Main entries","Length","No Allowance","No Allowance",20,{"$f":"P10*3.28","v":65.599999999999994},20,{"$f":"R10*3.28","v":65.599999999999994},30,{"$f":"T10*3.28","v":98.399999999999991},30,{"$f":"V10*3.28","v":98.399999999999991}]
[null,null,null,"Fire Station",0.67100000000000004,7.2225769,"Audience Seating/Transportation facility",0.43,{"$f":"H11*10.7639","v":4.6284770000000002},"No","Yes","Other doors","Length","No Allowance","No Allowance",20,{"$f":"P11*3.28","v":65.599999999999994},20,{"$f":"R11*3.28","v":65.599999999999994},20,{"$f":"T11*3.28","v":65.599999999999994},20,{"$f":"V11*3.28","v":65.599999999999994}]
[null,null,null,"Gymnasium",0.94,10.118065999999999,"Audience Seating/All Other",0.43,4.6284770000000002,"No","Yes","Canopies (free standing and attached and overhangs)","Area","No Allowance","No Allowance",0.25,2.6909749999999999,0.25,2.6909749999999999,0.4,4.3055599999999998,0.4,4.3055599999999998]
[null,null,null,"Health-care clinic",0.9,9.6875099999999996,"Atrium ≤40 ft high","0.03/ft total height","0.03/ft total height","Yes","Yes","Outdoor Sales Open areas (including vehicle sales lots)","Area","No Allowance","No Allowance",0.25,2.6909749999999999,0.25,2.6909749999999999,0.5,5.3819499999999998,0.75,8.0729249999999997]
[null,null,null,"Hospital",1.05,11.302095,"Atrium >40 ft high","0.40 + 0.02/ft\ntotal height","0.40 + 0.02/ft\ntotal height","Yes","Yes","Outdoor Sales Street frontage for vehicle sales lots in addition to open-area allowance)","Length","No Allowance","No Allowance","No Allowance","No Allowance",10,{"$f":"R14*3.28","v":32.799999999999997},10,{"$f":"T14*3.28","v":32.799999999999997},30,{"$f":"V14*3.28","v":98.399999999999991}]
[null,null,null,"Hotel/motel",0.87,9.3645929999999993,"Banking Activity Area",1.01,10.871539,"No","Yes",null,null,"Zone 0",null,"Zone 1",null,"Zone 2",null,"Zone 3",null,"Zone 4"]
[null,null,null,"Library",1.19,12.809040999999999,"Classroom/Lecture Hall/Training Room in Penitentiary",1.34,14.423626000000001,"Yes","Yes","IPParking lots and drives",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N4,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P4,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R4,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T4,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V4,\"\")))))","v":""}]
[null,null,null,"Manufacturing facility",1.17,12.593762999999999,"Classroom/Lecture Hall/Training Room in All Other",1.24,13.347235999999999,"Yes","Yes","IPWalkways less than 10 ft wide",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N5,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P5,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R5,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T5,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V5,\"\")))))","v":""}]
[null,null,null,"Motion picture theater",0.76,8.1805640000000004,"Conference/Meeting/Multipurpose Room",1.23,13.239597,"Yes","Yes","IPWalkways 10 ft wide or greater",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N6,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P6,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R6,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T6,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V6,\"\")))))","v":""}]
[null,null,null,"Multifamily",0.51,5.4895889999999996,"Confinement Cells",0.81,8.7187590000000004,"No","Yes","IPPlaza areas",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N7,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P7,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R7,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T7,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V7,\"\")))))","v":""}]
[null,null,null,"Museum",1.02,10.979177999999999,"Copy/Print Room",0.72,7.7500079999999993,"Yes","Yes","IPSpecial feature areas",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N8,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P8,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R8,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T8,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V8,\"\")))))","v":""}]
[null,null,null,"Office",0.82,8.8263979999999993,"Corridor/Facility for Visually Impaired",0.92,9.9027879999999993,"Yes","Yes","IPStairways",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N9,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P9,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R9,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T9,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V9,\"\")))))","v":""}]
[null,null,null,"Parking garage",0.21,2.2604189999999997,"Corridor/Hospital",0.99,10.656260999999999,"No","Yes","IPMain entries",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N10,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P10,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R10,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T10,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V10,\"\")))))","v":""}]
[null,null,null,"Penitentiary",0.81,8.7187590000000004,"Corridor/Manufacturing Facility",0.41,4.4131989999999996,"No","Yes","IPOther doors",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N11,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P11,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R11,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T11,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V11,\"\")))))","v":""}]
[null,null,null,"Performing arts theater",1.39,14.961820999999999,"Corridor/All Other",0.66,7.1041740000000004,"Yes","Yes","IPCanopies (free standing and attached and overhangs)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N12,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P12,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R12,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T12,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V12,\"\")))))","v":""}]
[null,null,null,"Police station",0.87,9.3645929999999993,"Courtroom",1.72,18.513908000000001,"No","Yes","IPOutdoor Sales Open areas (including vehicle sales lots)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N13,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P13,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R13,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T13,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V13,\"\")))))","v":""}]
[null,null,null,"Post office",0.87,9.3645929999999993,"Computer Room",1.71,18.406268999999998,"No","Yes","IPOutdoor Sales Street frontage for vehicle sales lots in addition to open-area allowance)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N14,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P14,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R14,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T14,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V14,\"\")))))","v":""}]
[null,null,null,"Religious building",1,10.7639,"Dining Area/Penitentiary",0.96,10.333343999999999,"No","Yes","SIParking lots and drives",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O4,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q4,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S4,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U4,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W4,\"\")))))","v":""}]
[null,null,null,"Retail",1.26,13.562514,"Dining Area/Facility for Visually Impaired",2.65,28.524334999999997,"No","Yes","SIWalkways less than 10 ft wide",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O5,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q5,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S5,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U5,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W5,\"\")))))","v":""}]
[null,null,null,"School/university",0.87,9.3645929999999993,"Dining Area/bar/Lounge or Leisure Dining",1.07,11.517373000000001,"No","Yes","SIWalkways 10 ft wide or greater",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O6,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q6,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S6,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U6,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W6,\"\")))))","v":""}]
[null,null,null,"Sports arena",0.91,9.7951490000000003,"Dining Area/Cafeteria/Fast Food",0.65,6.9965349999999997,"No","Yes","SIPlaza areas",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O7,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q7,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S7,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U7,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W7,\"\")))))","v":""}]
[null,null,null,"Town hall",0.89,9.5798709999999989,"Dining Area/Family Dining",0.89,9.5798709999999989,"No","Yes","SISpecial feature areas",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O8,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q8,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S8,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U8,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W8,\"\")))))","v":""}]
[null,null,null,"Transportation",0.7,7.5347299999999988,"Dining Area/All Other",0.65,6.9965349999999997,"No","Yes","SIStairways",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O9,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q9,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S9,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U9,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W9,\"\")))))","v":""}]
[null,null,null,"Warehouse",0.66,7.1041740000000004,"Electrical/Mechanical Room",0.42,4.5208379999999995,"No","Yes","SIMain entries",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O10,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q10,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S10,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U10,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W10,\"\")))))","v":""}]
[null,null,null,"Workshop",1.119,12.0448041,"Emergency Vehicle Garage",0.56000000000000005,6.0277840000000005,"No","Yes","SIOther doors",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O11,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q11,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S11,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U11,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W11,\"\")))))","v":""}]
[null,null,null,null,null,null,"Food Preparation Area",1.21,13.024318999999998,"No","Yes","SICanopies (free standing and attached and overhangs)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O12,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q12,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S12,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U12,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W12,\"\")))))","v":""}]
[null,null,null,null,null,null,"Guest Room",0.91,9.7951490000000003,"No","Yes","SIOutdoor Sales Open areas (including vehicle sales lots)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O13,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q13,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S13,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U13,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W13,\"\")))))","v":""}]
[null,null,null,null,null,null,"Judges Chambers",0.93,10.010427,"Yes","Yes","SIOutdoor Sales Street frontage for vehicle sales lots in addition to open-area allowance)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O14,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q14,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S14,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U14,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W14,\"\")))))","v":""}]
[null,null,null,null,null,null,"Laboratory/Classroom",1.43,15.392376999999998,"Yes","Yes"]
[null,null,null,null,null,null,"Laboratory/All Other",1.81,19.482658999999998,"No","Yes"]
[null,null,null,null,null,null,"Laundry/Washing Area",0.6,6.4583399999999997,"No","Yes"]
[null,null,null,null,null,null,"Loading Dock, Interior",0.47,5.0590329999999994,"No","Yes"]
[null,null,null,null,null,null,"Lobby/Facility for Visually Impaired",1.8,19.375019999999999,"Yes","Yes",null,null,"Zone 0",null,"Zone 1",null,"Zone 2",null,"Zone 3",null,"Zone 4"]
[null,null,null,null,null,null,"Lobby/Elevator",0.64,6.8888959999999999,"No","Yes","Nontradable Surfaces","Required Input","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter"]
[null,null,null,null,null,null,"Lobby/Hotel",1.06,11.409734,"No","Yes",null,null,"IP","SI","IP","SI","IP","SI","IP","SI","IP","SI"]
[null,null,null,null,null,null,"Lobby/Motion Picture Theater",0.59,6.350700999999999,"No","Yes",null,null,{"$f":"N43&\" \"&N44","v":"W/sf or W/linear foot IP"},"W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI"]
[null,null,null,null,null,null,"Lobby/Performing Arts Theater",2,21.527799999999999,"Yes","Yes","Building facades","Area","No Allowance","No Allowance","No Allowance","No Allowance",0.1,{"$f":"R46*10.7639","v":1.07639},0.15,{"$f":"T46*10.7639","v":1.6145849999999999},0.2,{"$f":"V46*10.7639","v":2.1527799999999999}]
[null,null,null,null,null,null,"Lobby/All Other",0.9,9.6875099999999996,"Yes","Yes","ATMs and night depositories","Length","No Allowance","No Allowance","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional"]
[null,null,null,null,null,null,"Locker Room",0.75,8.0729249999999997,"Yes","Yes","Entrances and gatehouse inspection stations at guarded facilities","Area","No Allowance","No Allowance",0.75,{"$f":"P48*10.7639","v":8.0729249999999997},0.75,{"$f":"R48*10.7639","v":8.0729249999999997},0.75,{"$f":"T48*10.7639","v":8.0729249999999997},0.75,{"$f":"V48*10.7639","v":8.0729249999999997}]
[null,null,null,null,null,null,"Lounge/Breakroom/in Healthcare Facility",0.92,9.9027879999999993,"Yes","Yes","Loading areas for law enforcement, fire, ambulance, and other emergency service vehicles","Area","No Allowance","No Allowance",0.5,{"$f":"P49*10.7639","v":5.3819499999999998},0.5,{"$f":"R49*10.7639","v":5.3819499999999998},0.5,{"$f":"T49*10.7639","v":5.3819499999999998},0.5,{"$f":"V49*10.7639","v":5.3819499999999998}]
[null,null,null,null,null,null,"Lounge/Breakroom/All Other",0.73,7.8576469999999992,"Yes","Yes","Drive-through windows at fast food restaurants","Length","No Allowance","No Allowance",400,400,400,400,400,400,400,400]
[null,null,null,null,null,null,"Office/Enclosed",1.1100000000000001,11.947929,"Yes","Yes","Parking near 24-hour retail entrances","Length","No Allowance","No Allowance",800,800,800,800,800,800,800,800]
[null,null,null,null,null,null,"Office/Open Plan",0.8,8.6111199999999997,"No","Yes","Building facades","Length","No Allowance","No Allowance","No Allowance","No Allowance",2.5,{"$f":"R52*3.28","v":8.1999999999999993},3.75,{"$f":"T52*3.28","v":12.299999999999999},5,{"$f":"V52*3.28","v":16.399999999999999}]
[null,null,null,null,null,null,"Parking Area, Interior",0.19,2.0451410000000001,"No","Yes"]
[null,null,null,null,null,null,"Pharmacy Area",0.19,2.0451410000000001,"No","Yes",{"$f":"\"IP\"&L46&M46","v":"IPBuilding facadesArea"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N46,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P46,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R46,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T46,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V46,\"\")))))","v":""}]
[null,null,null,null,null,null,"Restroom/Facility for the Visually Impaired",1.21,13.024318999999998,"Yes","Yes",{"$f":"\"IP\"&L47","v":"IPATMs and night depositories"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N47,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P47,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R47,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T47,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V47,\"\")))))","v":""}]
[null,null,null,null,null,null,"Restroom/ All Other",0.98,10.548622,"Yes","Yes",{"$f":"\"IP\"&L48","v":"IPEntrances and gatehouse inspection stations at guarded facilities"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N48,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P48,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R48,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T48,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V48,\"\")))))","v":""}]
[null,null,null,null,null,null,"Sales Area",1.44,15.500015999999999,"No","Yes",{"$f":"\"IP\"&L49","v":"IPLoading areas for law enforcement, fire, ambulance, and other emergency service vehicles"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N49,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P49,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R49,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T49,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V49,\"\")))))","v":""}]
[null,null,null,null,null,null,"Seating Area, General",0.54,5.812506,"No","Yes",{"$f":"\"IP\"&L50","v":"IPDrive-through windows at fast food restaurants"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N50,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P50,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R50,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T50,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V50,\"\")))))","v":""}]
[null,null,null,null,null,null,"Stairwell",0.69,7.427090999999999,"Yes","Yes",{"$f":"\"IP\"&L51","v":"IPParking near 24-hour retail entrances"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N51,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P51,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R51,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T51,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V51,\"\")))))","v":""}]
[null,null,null,null,null,null,"Storage Room/Hospital",0.63,6.7812570000000001,"No","Yes",{"$f":"\"IP\"&L52&M52","v":"IPBuilding facadesLength"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!N52,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!P52,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!R52,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!T52,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!V52,\"\")))))","v":""}]
[null,null,null,null,null,null,"Storage Room/≥50 sqft",0.63,6.7812570000000001,"Yes","Yes",{"$f":"\"SI\"&L46&M46","v":"SIBuilding facadesArea"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O46,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q46,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S46,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U46,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W46,\"\")))))","v":""}]
[null,null,null,null,null,null,"Storage Room/<50 sgft",1.24,13.347235999999999,"No","Yes",{"$f":"\"SI\"&L47","v":"SIATMs and night depositories"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O47,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q47,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S47,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U47,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W47,\"\")))))","v":""}]
[null,null,null,null,null,null,"Vehicular Maintenance Area",0.67,7.2118130000000003,"No","Yes",{"$f":"\"SI\"&L48","v":"SIEntrances and gatehouse inspection stations at guarded facilities"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O48,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q48,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S48,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U48,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W48,\"\")))))","v":""}]
[null,null,null,null,null,null,"Workshop",1.59,17.114601,"No","Yes",{"$f":"\"SI\"&L49","v":"SILoading areas for law enforcement, fire, ambulance, and other emergency service vehicles"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O49,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q49,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S49,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U49,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W49,\"\")))))","v":""}]
[null,null,null,null,null,null,"Assisted Living Facility/Chapel",2.21,23.788218999999998,"No","Yes",{"$f":"\"SI\"&L50","v":"SIDrive-through windows at fast food restaurants"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O50,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q50,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S50,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U50,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W50,\"\")))))","v":""}]
[null,null,null,null,null,null,"Assisted Living Facility/Recreation Room",2.41,25.940999000000001,"No","No",{"$f":"\"SI\"&L51","v":"SIParking near 24-hour retail entrances"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O51,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q51,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S51,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U51,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W51,\"\")))))","v":""}]
[null,null,null,null,null,null,"Convention Center-Exhibit Space",1.45,15.607654999999999,"No","Yes",{"$f":"\"SI\"&L52&M52","v":"SIBuilding facadesLength"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2013'!O52,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2013'!Q52,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2013'!S52,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2013'!U52,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2013'!W52,\"\")))))","v":""}]
[null,null,null,null,null,null,"Dormitory-Living Quarters",0.38,{"$f":"H68*10.7639","v":4.0902820000000002},"No","No"]
[null,null,null,null,null,null,"Fire Station-Sleeping Quarters",0.22,2.368058,"No","No"]
[null,null,null,null,null,null,"Gymnasium/Fitness Center/Exercise Area",0.72,7.7500079999999993,"No","Yes"]
[null,null,null,null,null,null,"Gymnasium/Fitness Center/Playing Area",1.2,12.916679999999999,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Emergency Room",1.68,18.083351999999998,"Yes","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Exam/Treatment Room",1.66,17.868074,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Imaging Room",1.51,16.253488999999998,"No","No"]
[null,null,null,null,null,null,"Healthcare Facility/Medical Supply Room",0.74,7.9652859999999999,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Nursery",0.88,9.472232,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Nurses Station",0.71,7.6423689999999995,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Operating Room",2.48,26.694471999999998,"No","No"]
[null,null,null,null,null,null,"Healthcare Facility/Patient Room",0.62,6.6736179999999994,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Physical Therapy Room",0.91,9.7951490000000003,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Recovery Room",1.1499999999999999,12.378484999999998,"No","Yes"]
[null,null,null,null,null,null,"Library/Reading Area",1.06,11.409734,"No","Yes"]
[null,null,null,null,null,null,"Library/Stacks",1.71,18.406268999999998,"Yes","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/Detailed Manufacturing Area",1.29,13.885431000000001,"No","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/Equipment Room",0.74,7.9652859999999999,"No","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/Extra High Bay Area (>50 ft floor-to-ceiling height)",1.05,11.302095,"No","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/High Bay Area (25-50 ft floor-to-ceiling height)",1.23,13.239597,"No","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/Low Bay Area (<25 ft floor-to-ceiling height)",1.19,12.809040999999999,"No","Yes"]
[null,null,null,null,null,null,"Museum/General Exhibition Area",1.05,11.302095,"No","Yes"]
[null,null,null,null,null,null,"Museum/Restoration Room",1.02,10.979177999999999,"No","Yes"]
[null,null,null,null,null,null,"Post Office/Sorting Area",0.94,10.118065999999999,"Yes","Yes"]
[null,null,null,null,null,null,"Religious Building/Fellowship Hall",0.64,6.8888959999999999,"No","Yes"]
[null,null,null,null,null,null,"Religious building/Worship/Choir area",1.53,16.468767,"No","Yes"]
[null,null,null,null,null,null,"Retail Facilities/Dressing/Fitting Room",0.71,7.6423689999999995,"Yes","Yes"]
[null,null,null,null,null,null,"Retail Facilities/Mall Concourse",1.1000000000000001,11.840290000000001,"No","Yes"]
[null,null,null,null,null,null,"Sporting Arena-Playing Area/Class I Facility",3.68,39.611151999999997,"No","Yes"]
[null,null,null,null,null,null,"Sporting Arena-Playing Area/Class II Facility",2.4,25.833359999999999,"No","Yes"]
[null,null,null,null,null,null,"Sporting Arena-Playing Area/Class III Facility",1.8,19.375019999999999,"No","Yes"]
[null,null,null,null,null,null,"Sporting Arena-Playing Area/Class IV Facility",1.2,12.916679999999999,"No","Yes"]
[null,null,null,null,null,null,"Transportation Facility/Baggage/Carousel Area",0.53,5.7048670000000001,"No","Yes"]
[null,null,null,null,null,null,"Transportation Facility/Airport Concourse",0.36,3.8750039999999997,"No","Yes"]
[null,null,null,null,null,null,"Transportation Facility/Terminal Ticket Counter",0.8,8.6111199999999997,"No","Yes"]
[null,null,null,null,null,null,"Warehouse-Storage Area/Medium to Bulky, Palletized Items",0.57999999999999996,6.2430619999999992,"Yes","Yes"]
[null,null,null,null,null,null,"Warehouse-Storage Area/Smaller, Hand Carried Items",0.95,10.225705,"Yes","Yes"]
[null,null,null,null,null,null,"Dwelling Unit",0.7,7.5347299999999988,"No","No"]
[null,null,null,null,null,null,"Multiple","See 9.6.1 (a)","See 9.6.1 (a)","See 9.6.1 (a)","See 9.6.1 (a)"]
[]
[null,null,null,null,null,null,"\"Similar\" space types used to map from Table G3.7 (BM baseline) to 90.1 2013 Table 9.6.1"]
[null,null,null,null,null,null,"Judges Chamber = Office"]
[null,null,null,null,null,null,"Dwelling Unit Controls = Dormitory - living quarters"]
[null,null,null,null,null,null,"Health Care Facility / Emergency Room = Exam / Treatment room"]

{"sheet":"Lighting Assumptions 90.1-2010","index":20,"n_rows":106,"n_cols":23,"rows_kept":106,"cut":false,"hidden":true,"merged":[[0,12,1,12],[0,3,1,3],[0,4,0,5],[0,6,1,6],[0,7,0,8],[0,11,1,11],[14,19,14,20],[14,21,14,22],[41,13,41,14],[41,15,41,16],[41,17,41,18],[41,19,41,20],[41,21,41,22],[42,11,43,11],[42,12,43,12],[14,13,14,14],[14,15,14,16],[14,17,14,18]]}
[null,null,null,"Building Area Method Categories","Table 9.5.1 LPD",null,"Space by Space Categories","Table 9.6.1 LPD ",null,"Table 9.6.1 LPD ","Table 9.6.1 LPD ","Tradable Surfaces","Required Input","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter"]
[null,null,null,null,"(W/sq ft)","(W/sq m)",null,"(W/sq ft)","(W/sq m)","occupancy sensor required?","Dayighting required?",null,null,"IP","SI","IP","SI","IP","SI","IP","SI","IP","SI"]
[null,null,null,"Automotive facility",0.8,{"$f":"E3*10.7639","v":8.6111199999999997},"Audience Seating/Auditorium",0.63,{"$f":"H3*10.7639","v":6.7812570000000001},"No","Yes",null,null,{"$f":"N1&\" \"&N2","v":"W/sf or W/linear foot IP"},"W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI"]
[null,null,null,"Convention center",1.01,{"$f":"E4*10.7639","v":10.871539},"Audience Seating/Convention center",0.82,{"$f":"H4*10.7639","v":8.8263979999999993},"No","Yes","Parking lots and drives","Area",0,0,0.04,{"$f":"P4*10.7639","v":0.43055599999999999},0.06,{"$f":"R4*10.7639","v":0.64583399999999991},0.1,{"$f":"T4*10.7639","v":1.07639},0.13,{"$f":"V4*10.7639","v":1.3993070000000001}]
[null,null,null,"Courthouse",1.01,10.871539,"Audience Seating/Gymnasium",0.65,6.9965349999999997,"No","Yes","Walkways less than 10 ft wide","Length",0,0,0.7,{"$f":"P5*3.28","v":2.2959999999999998},0.7,{"$f":"R5*3.28","v":2.2959999999999998},0.8,{"$f":"T5*3.28","v":2.6240000000000001},1,{"$f":"V5*3.28","v":3.28}]
[null,null,null,"Dining: bar lounge/leisure",1.01,10.871539,"Audience Seating/Motion Picture Theatre",1.1399999999999999,12.270845999999999,"No","Yes","Walkways 10 ft wide or greater","Area",0,0,0.14000000000000001,{"$f":"P6*10.7639","v":1.5069460000000001},0.14000000000000001,{"$f":"R6*10.7639","v":1.5069460000000001},0.16,{"$f":"T6*10.7639","v":1.722224},0.2,{"$f":"V6*10.7639","v":2.1527799999999999}]
[null,null,null,"Dining: cafeteria/fast food",0.9,9.6875099999999996,"Audience Seating/Penitentiary",0.28000000000000003,3.0138920000000002,"No","Yes","Plaza areas","Area",0,0,0.14000000000000001,1.5069460000000001,0.14000000000000001,1.5069460000000001,0.16,1.722224,0.2,2.1527799999999999]
[null,null,null,"Dining: family",0.95,10.225705,"Audience Seating/Performing Arts Theater",2.4300000000000002,26.156276999999999,"No","Yes","Special feature areas","Area",0,0,0.14000000000000001,1.5069460000000001,0.14000000000000001,1.5069460000000001,0.16,1.722224,0.2,2.1527799999999999]
[null,null,null,"Dormitory",0.56999999999999995,6.1354229999999994,"Audience Seating/Religious Building",1.53,16.468767,"No","Yes","Stairways","Area",0,0,0.75,8.0729249999999997,1,10.7639,1,10.7639,1,10.7639]
[null,null,null,"Exercise center",0.84,9.0416759999999989,"Audience Seating/Sports Arena",0.43,4.6284770000000002,"No","Yes","Main entries","Length",0,0,20,{"$f":"P10*3.28","v":65.599999999999994},20,{"$f":"R10*3.28","v":65.599999999999994},30,{"$f":"T10*3.28","v":98.399999999999991},30,{"$f":"V10*3.28","v":98.399999999999991}]
[null,null,null,"Fire Station",0.67100000000000004,7.2225769,"Audience Seating/Transportation facility","NR","NR","NR","NR","Other doors","Length",0,0,20,{"$f":"P11*3.28","v":65.599999999999994},20,{"$f":"R11*3.28","v":65.599999999999994},20,{"$f":"T11*3.28","v":65.599999999999994},20,{"$f":"V11*3.28","v":65.599999999999994}]
[null,null,null,"Gymnasium",0.94,10.118065999999999,"Audience Seating/All Other",0.43,4.6284770000000002,"No","Yes","Canopies (free standing and attached and overhangs)","Area",0,0,0.25,2.6909749999999999,0.25,2.6909749999999999,0.4,4.3055599999999998,0.4,4.3055599999999998]
[null,null,null,"Health-care clinic",0.9,9.6875099999999996,"Atrium ≤40 ft high","NR","NR","NR","NR","Outdoor Sales Open areas (including vehicle sales lots)","Area",0,0,0.25,2.6909749999999999,0.25,2.6909749999999999,0.5,5.3819499999999998,0.75,8.0729249999999997]
[null,null,null,"Hospital",1.05,11.302095,"Atrium >40 ft high","NR","NR","NR","NR","Outdoor Sales Street frontage for vehicle sales lots in addition to open-area allowance)","Length",0,0,0,{"$f":"P14*3.28","v":0},10,{"$f":"R14*3.28","v":32.799999999999997},10,{"$f":"T14*3.28","v":32.799999999999997},30,{"$f":"V14*3.28","v":98.399999999999991}]
[null,null,null,"Hotel/motel",0.87,9.3645929999999993,"Banking Activity Area",1.01,10.871539,"No","Yes",null,null,"Zone 0",null,"Zone 1",null,"Zone 2",null,"Zone 3",null,"Zone 4"]
[null,null,null,"Library",1.19,12.809040999999999,"Classroom/Lecture Hall/Training Room in Penitentiary",1.34,14.423626000000001,"Yes","Yes","IPParking lots and drives",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N4,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P4,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R4,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T4,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V4,\"\")))))","v":""}]
[null,null,null,"Manufacturing facility",1.17,12.593762999999999,"Classroom/Lecture Hall/Training Room in All Other",1.24,13.347235999999999,"Yes","Yes","IPWalkways less than 10 ft wide",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N5,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P5,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R5,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T5,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V5,\"\")))))","v":""}]
[null,null,null,"Motion picture theater",0.76,8.1805640000000004,"Conference/Meeting/Multipurpose Room",1.23,13.239597,"Yes","Yes","IPWalkways 10 ft wide or greater",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N6,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P6,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R6,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T6,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V6,\"\")))))","v":""}]
[null,null,null,"Multifamily",0.51,5.4895889999999996,"Confinement Cells",0.81,8.7187590000000004,"No","Yes","IPPlaza areas",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N7,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P7,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R7,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T7,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V7,\"\")))))","v":""}]
[null,null,null,"Museum",1.02,10.979177999999999,"Copy/Print Room",0.72,7.7500079999999993,"Yes","Yes","IPSpecial feature areas",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N8,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P8,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R8,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T8,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V8,\"\")))))","v":""}]
[null,null,null,"Office",0.82,8.8263979999999993,"Corridor/Facility for Visually Impaired",0.92,9.9027879999999993,"Yes","Yes","IPStairways",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N9,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P9,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R9,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T9,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V9,\"\")))))","v":""}]
[null,null,null,"Parking garage",0.21,2.2604189999999997,"Corridor/Hospital",0.99,10.656260999999999,"No","Yes","IPMain entries",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N10,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P10,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R10,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T10,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V10,\"\")))))","v":""}]
[null,null,null,"Penitentiary",0.81,8.7187590000000004,"Corridor/Manufacturing Facility",0.41,4.4131989999999996,"No","Yes","IPOther doors",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N11,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P11,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R11,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T11,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V11,\"\")))))","v":""}]
[null,null,null,"Performing arts theater",1.39,14.961820999999999,"Corridor/All Other",0.66,7.1041740000000004,"Yes","Yes","IPCanopies (free standing and attached and overhangs)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N12,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P12,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R12,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T12,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V12,\"\")))))","v":""}]
[null,null,null,"Police station",0.87,9.3645929999999993,"Courtroom",1.72,18.513908000000001,"No","Yes","IPOutdoor Sales Open areas (including vehicle sales lots)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N13,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P13,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R13,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T13,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V13,\"\")))))","v":""}]
[null,null,null,"Post office",0.87,9.3645929999999993,"Computer Room",1.71,18.406268999999998,"No","Yes","IPOutdoor Sales Street frontage for vehicle sales lots in addition to open-area allowance)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N14,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P14,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R14,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T14,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V14,\"\")))))","v":""}]
[null,null,null,"Religious building",1,10.7639,"Dining Area/Penitentiary",0.96,10.333343999999999,"No","Yes","SIParking lots and drives",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O4,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q4,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S4,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U4,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W4,\"\")))))","v":""}]
[null,null,null,"Retail",1.26,13.562514,"Dining Area/Facility for Visually Impaired",2.65,28.524334999999997,"No","Yes","SIWalkways less than 10 ft wide",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O5,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q5,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S5,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U5,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W5,\"\")))))","v":""}]
[null,null,null,"School/university",0.87,9.3645929999999993,"Dining Area/bar/Lounge or Leisure Dining",1.07,11.517373000000001,"No","Yes","SIWalkways 10 ft wide or greater",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O6,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q6,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S6,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U6,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W6,\"\")))))","v":""}]
[null,null,null,"Sports arena",0.91,9.7951490000000003,"Dining Area/Cafeteria/Fast Food",0.65,6.9965349999999997,"No","Yes","SIPlaza areas",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O7,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q7,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S7,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U7,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W7,\"\")))))","v":""}]
[null,null,null,"Town hall",0.89,9.5798709999999989,"Dining Area/Family Dining",0.89,9.5798709999999989,"No","Yes","SISpecial feature areas",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O8,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q8,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S8,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U8,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W8,\"\")))))","v":""}]
[null,null,null,"Transportation",0.7,7.5347299999999988,"Dining Area/All Other",0.65,6.9965349999999997,"No","Yes","SIStairways",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O9,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q9,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S9,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U9,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W9,\"\")))))","v":""}]
[null,null,null,"Warehouse",0.66,7.1041740000000004,"Electrical/Mechanical Room",0.42,4.5208379999999995,"No","Yes","SIMain entries",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O10,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q10,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S10,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U10,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W10,\"\")))))","v":""}]
[null,null,null,"Workshop",1.119,12.0448041,"Emergency Vehicle Garage",0.56000000000000005,6.0277840000000005,"No","Yes","SIOther doors",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O11,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q11,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S11,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U11,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W11,\"\")))))","v":""}]
[null,null,null,null,null,null,"Food Preparation Area",1.21,13.024318999999998,"No","Yes","SICanopies (free standing and attached and overhangs)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O12,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q12,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S12,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U12,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W12,\"\")))))","v":""}]
[null,null,null,null,null,null,"Guest Room",0.91,9.7951490000000003,"No","Yes","SIOutdoor Sales Open areas (including vehicle sales lots)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O13,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q13,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S13,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U13,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W13,\"\")))))","v":""}]
[null,null,null,null,null,null,"Judges Chambers","NR","NR","NR","NR","SIOutdoor Sales Street frontage for vehicle sales lots in addition to open-area allowance)",null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O14,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q14,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S14,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U14,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W14,\"\")))))","v":""}]
[null,null,null,null,null,null,"Laboratory/Classroom",1.43,15.392376999999998,"Yes","Yes"]
[null,null,null,null,null,null,"Laboratory/All Other",1.81,19.482658999999998,"No","Yes"]
[null,null,null,null,null,null,"Laundry/Washing Area",0.6,6.4583399999999997,"No","Yes"]
[null,null,null,null,null,null,"Loading Dock, Interior",0.47,5.0590329999999994,"No","Yes"]
[null,null,null,null,null,null,"Lobby/Facility for Visually Impaired",1.8,19.375019999999999,"Yes","Yes",null,null,"Zone 0",null,"Zone 1",null,"Zone 2",null,"Zone 3",null,"Zone 4"]
[null,null,null,null,null,null,"Lobby/Elevator",0.64,6.8888959999999999,"No","Yes","Nontradable Surfaces","Required Input","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter","W/sf or W/linear foot","W/sm or W/linear meter"]
[null,null,null,null,null,null,"Lobby/Hotel",1.06,11.409734,"No","Yes",null,null,"IP","SI","IP","SI","IP","SI","IP","SI","IP","SI"]
[null,null,null,null,null,null,"Lobby/Motion Picture Theater",0.59,6.350700999999999,"No","Yes",null,null,{"$f":"N43&\" \"&N44","v":"W/sf or W/linear foot IP"},"W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI","W/sf or W/linear foot IP","W/sm or W/linear meter SI"]
[null,null,null,null,null,null,"Lobby/Performing Arts Theater",2,21.527799999999999,"Yes","Yes","Building facades","Area",0,0,0,{"$f":"P46*10.7639","v":0},0.1,{"$f":"R46*10.7639","v":1.07639},0.15,{"$f":"T46*10.7639","v":1.6145849999999999},0.2,{"$f":"V46*10.7639","v":2.1527799999999999}]
[null,null,null,null,null,null,"Lobby/All Other",0.9,9.6875099999999996,"Yes","Yes","ATMs and night depositories","Length",0,0,"270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional","270 W+90 per additional"]
[null,null,null,null,null,null,"Locker Room",0.75,8.0729249999999997,"Yes","Yes","Entrances and gatehouse inspection stations at guarded facilities","Area","NR","NR","NR","NR","NR","NR","NR","NR","NR","NR"]
[null,null,null,null,null,null,"Lounge/Breakroom/in Healthcare Facility",0.92,9.9027879999999993,"Yes","Yes","Loading areas for law enforcement, fire, ambulance, and other emergency service vehicles","Area","NR","NR","NR","NR","NR","NR","NR","NR","NR","NR"]
[null,null,null,null,null,null,"Lounge/Breakroom/All Other",0.73,7.8576469999999992,"Yes","Yes","Drive-through windows at fast food restaurants","Length",0,0,400,400,400,400,400,400,400,400]
[null,null,null,null,null,null,"Office/Enclosed",1.1100000000000001,11.947929,"Yes","Yes","Parking near 24-hour retail entrances","Length","NR","NR","NR","NR","NR","NR","NR","NR","NR","NR"]
[null,null,null,null,null,null,"Office/Open Plan",0.8,8.6111199999999997,"No","Yes","Building facades","Length",0,0,0,0,2.5,{"$f":"R52*3.28","v":8.1999999999999993},3.75,{"$f":"T52*3.28","v":12.299999999999999},5,{"$f":"V52*3.28","v":16.399999999999999}]
[null,null,null,null,null,null,"Parking Area, Interior",0.19,2.0451410000000001,"No","Yes"]
[null,null,null,null,null,null,"Pharmacy Area",0.19,2.0451410000000001,"No","Yes",{"$f":"\"IP\"&L46&M46","v":"IPBuilding facadesArea"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N46,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P46,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R46,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T46,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V46,\"\")))))","v":""}]
[null,null,null,null,null,null,"Restroom/Facility for the Visually Impaired",1.21,13.024318999999998,"Yes","Yes",{"$f":"\"IP\"&L47","v":"IPATMs and night depositories"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N47,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P47,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R47,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T47,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V47,\"\")))))","v":""}]
[null,null,null,null,null,null,"Restroom/ All Other",0.98,10.548622,"Yes","Yes",{"$f":"\"IP\"&L48","v":"IPEntrances and gatehouse inspection stations at guarded facilities"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N48,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P48,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R48,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T48,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V48,\"\")))))","v":""}]
[null,null,null,null,null,null,"Sales Area",1.44,15.500015999999999,"No","Yes",{"$f":"\"IP\"&L49","v":"IPLoading areas for law enforcement, fire, ambulance, and other emergency service vehicles"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N49,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P49,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R49,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T49,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V49,\"\")))))","v":""}]
[null,null,null,null,null,null,"Seating Area, General",0.54,5.812506,"No","Yes",{"$f":"\"IP\"&L50","v":"IPDrive-through windows at fast food restaurants"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N50,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P50,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R50,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T50,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V50,\"\")))))","v":""}]
[null,null,null,null,null,null,"Stairwell",0.69,7.427090999999999,"Yes","Yes",{"$f":"\"IP\"&L51","v":"IPParking near 24-hour retail entrances"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N51,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P51,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R51,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T51,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V51,\"\")))))","v":""}]
[null,null,null,null,null,null,"Storage Room/Hospital",0.63,6.7812570000000001,"No","Yes",{"$f":"\"IP\"&L52&M52","v":"IPBuilding facadesLength"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!N52,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!P52,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!R52,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!T52,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!V52,\"\")))))","v":""}]
[null,null,null,null,null,null,"Storage Room/≥50 sqft",0.63,6.7812570000000001,"Yes","Yes",{"$f":"\"SI\"&L46&M46","v":"SIBuilding facadesArea"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O46,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q46,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S46,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U46,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W46,\"\")))))","v":""}]
[null,null,null,null,null,null,"Storage Room/<50 sgft",1.24,13.347235999999999,"No","Yes",{"$f":"\"SI\"&L47","v":"SIATMs and night depositories"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O47,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q47,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S47,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U47,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W47,\"\")))))","v":""}]
[null,null,null,null,null,null,"Vehicular Maintenance Area",0.67,7.2118130000000003,"No","Yes",{"$f":"\"SI\"&L48","v":"SIEntrances and gatehouse inspection stations at guarded facilities"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O48,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q48,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S48,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U48,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W48,\"\")))))","v":""}]
[null,null,null,null,null,null,"Workshop",1.59,17.114601,"No","Yes",{"$f":"\"SI\"&L49","v":"SILoading areas for law enforcement, fire, ambulance, and other emergency service vehicles"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O49,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q49,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S49,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U49,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W49,\"\")))))","v":""}]
[null,null,null,null,null,null,"Assisted Living Facility/Chapel",2.21,23.788218999999998,"No","Yes",{"$f":"\"SI\"&L50","v":"SIDrive-through windows at fast food restaurants"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O50,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q50,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S50,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U50,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W50,\"\")))))","v":""}]
[null,null,null,null,null,null,"Assisted Living Facility/Recreation Room",2.41,25.940999000000001,"No","No",{"$f":"\"SI\"&L51","v":"SIParking near 24-hour retail entrances"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O51,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q51,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S51,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U51,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W51,\"\")))))","v":""}]
[null,null,null,null,null,null,"Convention Center-Exhibit Space",1.45,15.607654999999999,"No","Yes",{"$f":"\"SI\"&L52&M52","v":"SIBuilding facadesLength"},null,{"$f":"IF('6b - General Lighting'!$X$131=0,'Lighting Assumptions 90.1-2010'!O52,IF('6b - General Lighting'!$X$131=1,'Lighting Assumptions 90.1-2010'!Q52,IF('6b - General Lighting'!$X$131=2,'Lighting Assumptions 90.1-2010'!S52,IF('6b - General Lighting'!$X$131=3,'Lighting Assumptions 90.1-2010'!U52,IF('6b - General Lighting'!$X$131=4,'Lighting Assumptions 90.1-2010'!W52,\"\")))))","v":""}]
[null,null,null,null,null,null,"Dormitory-Living Quarters",0.38,{"$f":"H68*10.7639","v":4.0902820000000002},"No","No"]
[null,null,null,null,null,null,"Fire Station-Sleeping Quarters",0.22,2.368058,"No","No"]
[null,null,null,null,null,null,"Gymnasium/Fitness Center/Exercise Area",0.72,7.7500079999999993,"No","Yes"]
[null,null,null,null,null,null,"Gymnasium/Fitness Center/Playing Area",1.2,12.916679999999999,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Emergency Room","NR","NR","NR","NR"]
[null,null,null,null,null,null,"Healthcare Facility/Exam/Treatment Room",1.66,17.868074,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Imaging Room",1.51,16.253488999999998,"No","No"]
[null,null,null,null,null,null,"Healthcare Facility/Medical Supply Room",0.74,7.9652859999999999,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Nursery",0.88,9.472232,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Nurses Station",0.71,7.6423689999999995,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Operating Room",2.48,26.694471999999998,"No","No"]
[null,null,null,null,null,null,"Healthcare Facility/Patient Room",0.62,6.6736179999999994,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Physical Therapy Room",0.91,9.7951490000000003,"No","Yes"]
[null,null,null,null,null,null,"Healthcare Facility/Recovery Room",1.1499999999999999,12.378484999999998,"No","Yes"]
[null,null,null,null,null,null,"Library/Reading Area",1.06,11.409734,"No","Yes"]
[null,null,null,null,null,null,"Library/Stacks",1.71,18.406268999999998,"Yes","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/Detailed Manufacturing Area",1.29,13.885431000000001,"No","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/Equipment Room",0.74,7.9652859999999999,"No","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/Extra High Bay Area (>50 ft floor-to-ceiling height)",1.05,11.302095,"No","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/High Bay Area (25-50 ft floor-to-ceiling height)",1.23,13.239597,"No","Yes"]
[null,null,null,null,null,null,"Manufacturing Facility/Low Bay Area (<25 ft floor-to-ceiling height)",1.19,12.809040999999999,"No","Yes"]
[null,null,null,null,null,null,"Museum/General Exhibition Area",1.05,11.302095,"No","Yes"]
[null,null,null,null,null,null,"Museum/Restoration Room",1.02,10.979177999999999,"No","Yes"]
[null,null,null,null,null,null,"Post Office/Sorting Area",0.94,10.118065999999999,"Yes","Yes"]
[null,null,null,null,null,null,"Religious Building/Fellowship Hall",0.64,6.8888959999999999,"No","Yes"]
[null,null,null,null,null,null,"Religious building/Worship/Choir area",1.53,16.468767,"No","Yes"]
[null,null,null,null,null,null,"Retail Facilities/Dressing/Fitting Room",0.71,7.6423689999999995,"Yes","Yes"]
[null,null,null,null,null,null,"Retail Facilities/Mall Concourse",1.1000000000000001,11.840290000000001,"No","Yes"]
[null,null,null,null,null,null,"Sporting Arena-Playing Area/Class I Facility",3.68,39.611151999999997,"No","Yes"]
[null,null,null,null,null,null,"Sporting Arena-Playing Area/Class II Facility",2.4,25.833359999999999,"No","Yes"]
[null,null,null,null,null,null,"Sporting Arena-Playing Area/Class III Facility",1.8,19.375019999999999,"No","Yes"]
[null,null,null,null,null,null,"Sporting Arena-Playing Area/Class IV Facility",1.2,12.916679999999999,"No","Yes"]
[null,null,null,null,null,null,"Transportation Facility/Baggage/Carousel Area",0.53,5.7048670000000001,"No","Yes"]
[null,null,null,null,null,null,"Transportation Facility/Airport Concourse",0.36,3.8750039999999997,"No","Yes"]
[null,null,null,null,null,null,"Transportation Facility/Terminal Ticket Counter",0.8,8.6111199999999997,"No","Yes"]
[null,null,null,null,null,null,"Warehouse-Storage Area/Medium to Bulky, Palletized Items",0.57999999999999996,6.2430619999999992,"Yes","Yes"]
[null,null,null,null,null,null,"Warehouse-Storage Area/Smaller, Hand Carried Items",0.95,10.225705,"Yes","Yes"]
[null,null,null,null,null,null,"Dwelling Unit",0.51,5.4895889999999996,"NR","NR"]
[null,null,null,null,null,null,"Multiple","NR","NR","NR","NR"]

{"sheet":"7 - Process Loads","index":21,"n_rows":75,"n_cols":26,"rows_kept":75,"cut":false,"hidden":false,"merged":[[23,7,23,8],[22,7,22,8],[21,2,21,3],[21,7,21,8],[20,7,20,8],[22,2,22,3],[23,2,23,3],[20,2,20,3],[58,7,58,8],[38,1,38,7],[58,2,58,3],[51,2,51,7],[52,2,52,7],[55,2,55,3],[57,2,57,3],[56,7,56,8],[56,2,56,3],[55,1,56,1],[25,1,25,7],[32,7,32,8],[33,2,33,3],[33,7,33,8],[24,1,24,3],[32,2,32,3],[24,6,24,9],[25,8,25,9],[4,1,4,6],[19,2,19,3],[7,1,7,7],[9,1,9,7],[12,1,12,8],[11,1,11,8],[15,6,15,8],[15,1,15,5],[19,7,19,8],[74,1,74,8],[59,2,59,3],[70,1,70,8],[59,7,59,8],[60,2,60,3],[60,7,60,8],[55,9,56,9],[57,7,57,8],[36,2,36,3],[37,1,37,3],[34,7,34,8],[35,7,35,8],[36,7,36,8],[35,2,35,3],[34,2,34,3],[55,7,55,8]]}
["G"]
["G","Process Loads"]
["G"]
["G"]
["G","Instructions: Select the method(s) used to model receptacle equipment, and then complete the corresponding receptacle equipment table(s). Non-receptacle process equipment should be reported in the last table. Please refer to the column header notes for information about Appendix G modeling protocol. For any information not applicable to the project, simply enter \"N/A\"."]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Process Load Requirements"]
["G","At least 50% of all 125 volt 15 and 20 Ampere receptacles installed in all private offices, conference rooms, rooms used primarily for printing and/or copying functions, break rooms, classrooms, and individual workstations, and at least 25% of branch circuit feeders installed for modular furniture not shown on the construction documents, shall be controlled by an automatic device which functions on a scheduled basis, an occupant sensor, or a signal from another control system that indicates the area is unoccupied, in accordance with Section 8.4.2."]
["G"]
["G","All receptacle equipment and other process equipment designed or anticipated for the building have been accounted for in the energy models."]
["G"]
["G","If not all the process equipment has been accounted for in the energy model, indicated as \"No\" above, the project does not likely comply with LEED modeling requirements. It is recommended that the project team pursue a \"Credit Interpretation Ruling\" to justify the modeling approach. Please also provide any further information below to justify the modeling approach used."]
["G"]
["G"]
["G","Receptacle Equipment Modeling Method"]
["G","Indicate whether the receptacle equipment was modeled using an average equipment power density for the building, equipment power densities by space type, or by entering the power associated with specific devices in each space.  (select all that apply)",null,null,null,null,"     Building average equipment power density\n\n     Space by space equipment power density",null,null,null,null,null,null,null,false,true]
["G"]
["G","Table 7.1: Building Average Equipment Power Density"]
["G","Please do not include any equipment power densities below of items that have already been noted on the Multifamily Details tab."]
["G","Building ID","Building Type",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"Total Building Type Area\n(sq ft)\",\"Total Building Type Area\n(sq m)\")","v":"Total Building Type Area\n(sq ft)"},{"$f":"IF('General Information'!$K$11=\"IP\",\"Equipment Power Density\n(W/sq ft)\",\"Equipment Power Density\n(W/sq m)\")","v":"Equipment Power Density\n(W/sq ft)"},"Equipment Included in Power Density","Baseline Modeled Identically",null,"Measure #"]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Building Average Equipment Power Density",{"$f":"IF(J21=\"\",\"0\",J21)","v":"0"},"<User Entry>",{"$f":"C21&\" Building Type with total building area of \"&E21&\" sqft, and EPD of \"&F21&\" w/sf. The equipment in this EPD includes \"&G21&\".\"","v":" Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Building Average Equipment Power Density",{"$f":"IF(J22=\"\",\"0\",J22)","v":"0"},"<User Entry>",{"$f":"C22&\" Building Type with total building area of \"&E22&\" sqft, and EPD of \"&F22&\" w/sf. The equipment in this EPD includes \"&G22&\".\"","v":" Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H23=\"No\",\"Submit savings using Exceptional Calculation\",\"\")","v":""},null,null,null,null,null,null,null,"Building Average Equipment Power Density","0","<User Entry>"," Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."]
["A",{"$f":"GI_Project_Name","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H24=\"No\",\"Submit savings using Exceptional Calculation\",\"\")","v":""},null,null,null,null,null,null,null,"Building Average Equipment Power Density","0","<User Entry>"," Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."]
["G","Totals",null,null,{"$f":"SUM($E$21:$E$23)","v":0},{"$f":"IFERROR(SUMPRODUCT($E$21:$E$23,$F$21:$F$23)/SUM($E$21:$E$23),0)","v":0}]
["G","Total power modeled using building average method (kW)",null,null,null,null,null,null,{"$f":"SUMPRODUCT($E$21:$E$23,$F$21:$F$23)/1000","v":0}]
["G","Note: Any credit for improved receptacle equipment must be submitted using the Exceptional Calculation Method."]
[null,{"$f":"IF(ResDwellingUnitsExist=\"Yes\",\"Note: The above table is for spaces other than dwelling units.  To enter dwelling unit values, use the Multifamily Details tab.\",\"\")","v":"Note: The above table is for spaces other than dwelling units.  To enter dwelling unit values, use the Multifamily Details tab."}]
["G"]
["G"]
["G","Table 7.2: Space by Space Equipment Power Densities"]
["G"]
["G","Building ID","Space Type",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"Total Space Type Area\n(sq ft)\",\"Total Space Type Area\n(sq m)\")","v":"Total Space Type Area\n(sq ft)"},{"$f":"IF('General Information'!$K$11=\"IP\",\"Equipment Power Density\n(W/sq ft)\",\"Equipment Power Density\n(W/sq m)\")","v":"Equipment Power Density\n(W/sq ft)"},"Equipment Included in Power Density","Baseline Modeled Identically",null,"Measure #"]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Space by Space Equipment Power Densities",{"$f":"IF(J34=\"\",\"0\",J34)","v":"0"},"<User Entry>",{"$f":"C34&\" Building Type with total building area of \"&E34&\" sqft, and EPD of \"&F34&\" w/sf. The equipment in this EPD includes \"&G34&\".\"","v":" Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."}]
[null,0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H35=\"No\",\"Submit savings using Exceptional Calculation\",\"\")","v":""},null,null,null,null,null,null,null,"Space by Space Equipment Power Densities",{"$f":"IF(J35=\"\",\"0\",J35)","v":"0"},"<User Entry>",{"$f":"C35&\" Building Type with total building area of \"&E35&\" sqft, and EPD of \"&F35&\" w/sf. The equipment in this EPD includes \"&G35&\".\"","v":" Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."}]
[null,0,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,"Space by Space Equipment Power Densities","0","<User Entry>"," Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."]
["B",0,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,"Space by Space Equipment Power Densities","0","<User Entry>"," Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."]
["G","Totals",null,null,{"$f":"SUM($E$34:$E$37)","v":0},{"$f":"IFERROR(SUMPRODUCT($E$34:$E$37,$F$34:$F$37)/SUM($E$34:$E$37),0)","v":0}]
["G","Total power modeled using space by space method (kW)",null,null,null,null,null,null,{"$f":"SUMPRODUCT($E$34:$E$37,$F$34:$F$37)/1000","v":0}]
[null,"Note: Any credit for improved receptacle equipment must be submitted using the Exceptional Calculation Method."]
["G",{"$f":"IF(ResDwellingUnitsExist=\"Yes\",\"Note: The above table is for spaces other than dwelling units.  To enter dwelling unit values, use the Multifamily Details tab.\",\"\")","v":"Note: The above table is for spaces other than dwelling units.  To enter dwelling unit values, use the Multifamily Details tab."}]
["G"]
["G"]
[null,"Residential Equipment Calculator"]
[]
[null,"Load Source","Energy Star",null,"EFLH"]
[]
[]
[]
[]
["G","Table 7.3: Summary (excludes Multifamily appliance and plug loads, which are shown on Multifamily Details tab)"]
["G","Building ID","Input Parameter",null,null,null,null,null,"kW"]
[null,{"$f":"'1 - Multiple Buildings Details'!B25","v":0},{"$f":"\"Total power for receptacle equipment\"","v":"Total power for receptacle equipment"},null,null,null,null,null,{"$f":"IF($P$16=TRUE,SUMPRODUCT(--($B$34:$B$37=$B53),$E$34:$E$37,$F$34:$F$37)/1000,0)+IF($O$16=TRUE,SUMPRODUCT(--($B$21:$B$23=$B53),$E$21:$E$23,$F$21:$F$23)/1000,0)","v":0}]
["G"]
["G","Table 7.4: Non-Receptacle Process Equipment"]
["G","Building ID","Equipment Type ",null,"Energy \nSource",{"$f":"IF('General Information'!$K$11=\"IP\",\"Energy Demand \n(kW for electricity) \n(Btuh for non-electricity)\",\"\nEnergy Demand (kW)\")","v":"Energy Demand \n(kW for electricity) \n(Btuh for non-electricity)"},"Modeling Parameters","Baseline Modeled Identically",null,"Measure #"]
[null,null,"Helpful Hints\nModify equipment types as necessary.\n\nNote: Complete the Data Center Calculator (found under the \"Resources\" tab of the Credit Library) in order to claim credit for data center equipment.",null,"Helpful Hints","Helpful Hints","Helpful Hints\nProvide a description of the equipment, the operating schedule, and any latent and sensible loads modeled in the associated space (example: 15 kW electric range with hood; operates 2 full load hours/day; 6.3 kBtu/h (1.8 kW) sensible heat gain).","Helpful Hints\nAll process loads must be modeled identically between the Proposed and Baseline case and included in the simulations per Table G3.1#12.\n\nExceptions: When quantifying performance that exceeds the\nrequirements of Standard 90.1 variations of the power requirements, schedules, or control sequences of the\nequipment modeled in the baseline building design from those in the proposed design shall be approved by the rating authority based on documentation that the equipment installed in the\nproposed design represents a significant verifiable departure\nfrom documented current conventional practice. ",null,null,null,null,null,null,null,null,null,null,"If Baseline is not modeled identically to Proposed Design and No is selected in \"Baseline Modeled Identically\" list box, please provide a description of the equipment, the operating schedule, and any latent and sensible loads modeled in the associated space "]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H58=\"No\",\"Submit savings using Exceptional Calculation\",\"\")","v":""},null,null,null,null,{"$f":"IF(H58=\"No\",\"Please explain why baseline was not modeled identically.\",\"\")","v":""},null,null,"Non-Receptacle Process Equipment",{"$f":"IF(J58=\"\",\"0\",J58)","v":"0"},"<User Entry>",{"$f":"\"Non-Receptacle process equipment includes the following: \"&C58&\" with an \"&E58&\" energy source of \"&F58&Z58&\". The modeling parameters include: \"&G58&\".\"","v":"Non-Receptacle process equipment includes the following:  with an  energy source of  Btuh. The modeling parameters include: ."},{"$f":"IF(E58=\"Electricity\",\" kW\",\" Btuh\")","v":" Btuh"}]
[null,0,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,"",null,null,"Non-Receptacle Process Equipment",{"$f":"IF(J59=\"\",\"0\",J59)","v":"0"},"<User Entry>",{"$f":"\"Non-Receptacle process equipment includes the following: \"&C59&\" with an \"&E59&\" energy source of \"&F59&Z59&\". The modeling parameters include: \"&G59&\".\"","v":"Non-Receptacle process equipment includes the following:  with an  energy source of  Btuh. The modeling parameters include: ."},{"$f":"IF(E59=\"Electricity\",\" kW\",\" Btuh\")","v":" Btuh"}]
[null,0,null,null,null,null,null,null,null,null,null,null,null,"",null,null,null,null,"",null,null,"Non-Receptacle Process Equipment","0","<User Entry>","Non-Receptacle process equipment includes the following:  with an  energy source of  Btuh. The modeling parameters include: ."," Btuh"]
["C",0,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H61=\"No\",\"Submit savings using Exceptional Calculation\",\"\")","v":""},null,null,null,null,{"$f":"IF(H61=\"No\",\"Please explain why baseline was not modeled identically.\",\"\")","v":""},null,null,"Non-Receptacle Process Equipment","0","<User Entry>","Non-Receptacle process equipment includes the following:  with an  energy source of  Btuh. The modeling parameters include: ."," Btuh"]
["G","Note: Any credit for improved process equipment must be submitted using the Exceptional Calculation Method."]
["G"]
["G"]
["G","Table 7.5: Garage Fan Power Calculation"]
[]
[]
["G","Building ID","Total Design Fan Power (kW)","Total Base Fan Power (kW)",{"$f":"CONCATENATE(\"Ventilated Parking Area \",IF(SI_IP_Units=\"IP\",\"(square feet)\",\"(square meter)\"))","v":"Ventilated Parking Area (square feet)"},{"$f":"CONCATENATE(\"Proposed Airflow \",IF(SI_IP_Units=\"IP\",\"CFM\",\"M/S\"))","v":"Proposed Airflow CFM"},{"$f":"CONCATENATE(\"Baseline Airflow \",IF(SI_IP_Units=\"IP\",\"CFM\",\"M/S\"))","v":"Baseline Airflow CFM"},"Design EFLH","Base EFLH"]
[null,{"$f":"GI_Project_Name","v":0},null,"Same as Design",null,null,"Same as Design",null,"Same as Design"]
["D",null,null,"Same as Design",null,null,"Same as Design",null,"Same as Design"]
["G",{"$f":"\"Note: \"&CHAR(10)&\n\"1.  The Baseline parking area is modeled with a constant volume fan\"&CHAR(10)&\n\"2.  Credit can be taken for garage demand control ventilation (DCV) in the Proposed design.\"&CHAR(10)&\n\"3.  Fan power for the Baseline case is limited to 0.3 W/CFM\"","v":"Note: \n1.  The Baseline parking area is modeled with a constant volume fan\n2.  Credit can be taken for garage demand control ventilation (DCV) in the Proposed design.\n3.  Fan power for the Baseline case is limited to 0.3 W/CFM"}]
["G"]
["G"]
["G"]
["G"]

{"sheet":"8 - Service Water Heating","index":22,"n_rows":86,"n_cols":59,"rows_kept":86,"cut":false,"hidden":false,"merged":[[7,1,10,4],[25,1,25,4],[26,1,26,4],[29,1,29,4],[85,1,85,11],[12,1,12,4],[12,6,12,8],[12,10,12,12],[13,1,13,4],[13,6,13,12],[15,1,15,4],[15,6,15,8],[15,10,15,12],[19,1,19,4],[21,1,21,4],[52,4,55,4],[58,1,58,12],[14,1,14,4],[17,10,17,12],[25,6,25,8],[25,10,25,12],[26,6,26,8],[26,10,26,12],[29,6,29,8],[29,10,29,12],[27,6,27,8],[21,10,21,11],[27,10,27,12],[18,6,18,8],[36,1,36,12],[43,2,44,2],[18,1,18,4],[4,1,4,12],[84,1,84,11],[20,1,20,4],[20,6,20,8],[20,10,20,12],[22,1,22,4],[22,6,22,8],[22,10,22,12],[23,1,23,4],[23,6,23,8],[23,10,23,12],[52,6,53,8],[52,10,53,12],[43,3,44,4],[9,6,10,8],[19,10,19,11],[52,15,54,15],[41,15,42,15],[24,1,24,4],[41,1,41,4],[30,6,30,8],[30,10,30,12],[41,6,41,8],[31,1,31,4],[42,1,44,1],[24,6,24,8],[30,1,30,4],[28,1,28,4],[52,13,52,14],[53,13,54,14],[52,9,55,9],[52,1,53,3],[14,6,14,12],[17,1,17,4],[19,6,19,7],[16,1,16,4],[16,6,16,8],[16,10,16,12],[17,6,17,8],[21,6,21,7],[18,10,18,12],[27,1,27,4],[59,1,59,12],[7,16,9,16],[7,10,7,13],[7,6,8,8],[8,10,8,12],[9,10,9,13],[7,15,8,15],[7,9,10,9],[56,13,56,14],[41,16,44,16],[41,10,41,13],[43,10,44,13],[28,6,28,8],[24,10,24,12],[28,10,28,12],[43,15,44,15],[43,6,44,8],[31,6,31,8],[31,10,31,12]]}
["G"]
["G","Service Water Heating"]
["G"]
["G"]
["G","Instructions: Complete the Service Water Heaters table for each unique type of system in the project. Use the Add System button for more than one type of system. If the project includes service hot water circulation pumps, complete the Service Hot Water Pumps table. Please refer to the column header notes for information about Appendix G modeling protocol. Complete the Service Hot Water Fixtures table if credit is modeled for low-flow fixtures in the proposed. For any information not applicable to the project, simply enter \"N/A\"."]
["G"]
["G","Table 8.1: Service Water Heaters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Model Input Parameter",null,null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,null,"Proposed Design",null,null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Plans / Specs"]
[null,null,null,null,null,null,"Helpful Hints\n•  New and existing systems: as specified in Table G3.1.1-2; minimum performance requirements from Table 7.8 per Table G3.1#11(b)\n•  Capacity: for existing systems, use actual component capacities; for new systems, system shall be sized following Section 7.4.1\n•  Condenser heat recovery as required by 6.5.6.2 per Table G3.1#11(f): Verify that condenser heat recovery has been modeled in the Baseline if required by 6.5.6.2, and describe any condenser heat recovery modeled (example: preheats service hot water to 85°F); otherwise enter \"Not required\"",null,null,null,"Helpful Hints\n•  Service water heaters modeled as designed (or installed) per Table G3.1#11(a&b)\n•  Where no service hot water system exists or has been specified but the building will have service hot water loads, a service hot water system should be modeled identical to the Baseline per Table G3.1#11(c)\n•  For buildings with no service hot water loads, no service hot water system should be modeled per Table G3.1#11(d)\n•  For buildings where a combined system has been specified to meet both space heating and service water heating loads, the proposed design shall reflect the actual system type using actual capacities and efficiencies per Table G3.1#11(e)",null,null,null,null,{"$f":"IF('General Information'!$K$48=2013,\"In accordance with 90.1-2013 Section 7.5\",\"In accordance with 90.1-2010 Section 7.5\")","v":"In accordance with 90.1-2013 Section 7.5"}]
[]
[null,"Modeled_Input_Param",null,null,null,null,"Baseline",null,null,null,"Proposed",null,null,null,null,{"$f":"IF(AND($W12<>0,$D12<>\"\"),$W12,\"\")","v":""}]
["G"]
["G","Building ID",null,null,null,null,"TEST",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Service Water Heaters",{"$f":"Q14","v":0},{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&K16&\" \"&K18&\" system with \"&K19&\" fuel. The input rating is \"&K20&M20&\" with an efficiency of \"&K22&\". The storage temperature is \"&K23&\" (F) with a peak hot water demand of \"&K24&\". Condenser heat recovery: \"&K25&\". There are \"&K29&\" \"&K28&\" pump(s) woth a total pump power of \"&ROUND(K31,3)&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,"Building Area Type based on ASHRAE 90.1 Table G3.1.1-2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gas <= 75",{"$f":"IF(G21<=55,(0.96-(0.0003*G21)),(2.057-(0.00113*G21)))","v":{"$error":"#VALUE!"}},"Service Water Heaters",0,{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"AA14","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Baseline kBtu/Hr",{"$f":"SUM(BA:BA)","v":{"$error":"#VALUE!"}},{"$f":"SUMPRODUCT(BA:BA,BF:BF)/SUM(BA:BA)","v":{"$error":"#VALUE!"}}]
["G","In-Unit or Central System?",null,null,null,null,{"$f":"IF(K16=\"\",\"\",\"Central\")","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(G16=\"\",\"\",G16)","v":""},null,null,null,null,null,"Gas>75",{"$f":"0.8","v":0.8},"Service Water Heaters",0,{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"AA15","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."},null,null,{"$f":"G19&\" \"&G18","v":" "},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Proposed kBtu/Hr",{"$f":"SUM(BB:BB)","v":{"$error":"#VALUE!"}},{"$f":"SUMPRODUCT(BB:BB,BG:BG)/SUM(BB:BB)","v":{"$error":"#VALUE!"}}]
[null,"Number of heaters",null,null,null,null,{"$f":"IF(K17=\"\",\"\",1)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(I20=\"kBtu/h\",G20,G20*'12 - Performance_Outputs_1'!$K$17*1000)","v":{"$error":"#VALUE!"}},{"$f":"K17*IF(M20=\"kBtu/h\",K20,K20*'12 - Performance_Outputs_1'!$K$17*1000)","v":{"$error":"#VALUE!"}},"Total kBtu/hr",null,null,{"$f":"G22","v":""},{"$f":"K22","v":0}]
[null,"System Type",null,null,null,null,{"$f":"IF(AND(K16=\"In-Unit\",'General Information'!E9=\"ENERGY STAR MFHR\"),\"Storage\",IF(G15=\"\",\"\",VLOOKUP(G15,'SWH Lookup'!E4:G37,3)))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(G18=\"\",\"\",G18)","v":""},null,null,null,null,null,"Elec <= 12",{"$f":"IF(G21<=55,(0.675-(0.0015*G21)),(0.8012-(0.00078*G21)))","v":{"$error":"#VALUE!"}},"Service Water Heaters",0,{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"AA16","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,"Fuel",null,null,null,null,{"$f":"IF(AND(K16=\"In-Unit\",'General Information'!E9=\"ENERGY STAR MFHR\"),\"Gas\",IF(G15=\"\",\"\",VLOOKUP(G15,'SWH Lookup'!E4:G37,2)))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(G19=\"\",\"\",G19)","v":""},null,null,null,null,null,"Elec >12",{"$f":"(0.3+27/G21)","v":{"$error":"#VALUE!"}},"Service Water Heaters",0,{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."]
["G","Total input rating",null,null,null,null,null,null,{"$f":"IF(G15=\"\",\"\",IF(G19=\"Gas\",\"kBtu/h\",\"kW\"))","v":""},null,null,null,{"$f":"IF(G15=\"\",\"\",IF(K19=\"Gas\",\"kBtu/h\",\"kW\"))","v":""},null,null,{"$f":"IF(G20=\"\",\"\",G20&\" \"&I20)","v":""},null,null,null,null,null,null,null,"Service Water Heaters",0,{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."]
["G",{"$f":"IF(SI_IP_Units=\"IP\",\"Storage volume (gal)\",\"Storage volume (L)\")","v":"Storage volume (gal)"},null,null,null,null,{"$f":"IF(K21=\"\",\"-\",K21)","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(G21=\"\",\"\",G21)","v":"-"},null,null,null,null,null,null,null,"Service Water Heaters",{"$f":"Q21","v":0},{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"AA22","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
["G","Efficiency (Et, EF, COP) ",null,null,null,null,{"$f":"IFERROR(IF(AND(G16=\"In-Unit\",'General Information'!E9=\"ENERGY STAR MFHR\"),0.544,IFERROR(IF(G15=\"\",\"\",IF(AD16=\"Gas Storage\",IF(G20<=75,W15,IF(G20>75,W16)),IF(AD16=\"Electric Resistance Storage\",IF(G20<=12,W18,IF(G20>12,W19))))),\"-\")),\"-\")","v":""},null,{"$f":"IFERROR(IF(G20=\"\",\"\",IF(AD16=\"Gas Storage\",IF(G20<=75,\"EF\",IF(G20>75,\"Et\")),IF(AD16=\"Electric Resistance Storage\",IF(G20<=12,\"EF\",IF(G20>12,\"%/h\"))))),\"N/A\")","v":""},null,null,null,{"$f":"I22","v":""},null,null,null,null,null,null,null,null,null,null,"Service Water Heaters",0,{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"AA20","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
["G",{"$f":"IF(SI_IP_Units=\"IP\",\"Storage temperature (°F)\",\"Storage temperature (°C)\")","v":"Storage temperature (°F)"},null,null,null,null,{"$f":"IF(K23=\"\",\"-\",K23)","v":"-"},null,null,null,null,null,null,null,null,"N/A",null,null,null,null,null,null,null,"Service Water Heaters",0,{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"AA21","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
["G",{"$f":"IF(SI_IP_Units=\"IP\",\"Peak hot water demand (gpm). Refer to the Multifamily Details tab if this is a Multifamily project.\",\"Peak hot water demand (L/s). Refer to the Multifamily Details tab if this is a Multifamily project.\")","v":"Peak hot water demand (gpm). Refer to the Multifamily Details tab if this is a Multifamily project."},null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A",null,null,null,null,null,null,null,"Service Water Heaters",0,{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."]
["G","Condenser heat recovery",null,null,null,null,{"$f":"IF(K25=\"\",\"-\",K25)","v":"-"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Service Water Heaters",0,{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."]
["G","Number of Recirculation pumps",null,null,null,null,{"$f":"IF(K26=\"\",\"-\",K26)","v":"-"},null,null,null,null,null,null,null,null,"NA",null,null,null,null,null,null,null,"Service Water Heaters",{"$f":"Q26","v":0},{"$f":"\"SWH building area type based on: \"&G14&\" with an \"&G15&\" \"&G16&\" system with \"&G18&\" fuel. The input rating is \"&G19&M19&\" with an efficiency of \"&G21&\". The storage temperature is \"&G22&\" (F) with a peak hot water demand of \"&G23&\". Condenser heat recovery: \"&G24&\". There are \"&G26&\" \"&G31&\" pump(s) woth a total pump power of \"&G29&\" kW.\"","v":"SWH building area type based on: TEST with an   system with  fuel. The input rating is  with an efficiency of -. The storage temperature is  (F) with a peak hot water demand of -. Condenser heat recovery: . There are - Yes pump(s) woth a total pump power of - kW."},{"$f":"AA24","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
["G","Total recirculation pump power (kW)",null,null,null,null,{"$f":"IF(K27=\"\",\"-\",K27)","v":"-"},null,null,null,null,null,null,null,null,"NA",null,null,null,null,null,null,null,"Service Water Heaters",{"$f":"Q27","v":0},{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G27&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"AA25","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
["G","Recirculation pump control",null,null,null,null,null,null,null,null,null,null,null,null,null,"NA",null,null,null,null,null,null,null,"Service Water Heaters",{"$f":"Q28","v":0},{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"AA31","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
["G","Number of booster pumps",null,null,null,null,{"$f":"IF(K29=\"\",\"-\",K29)","v":"-"},null,null,null,null,null,null,null,null,"NA",null,null,null,null,null,null,null,"Service Water Heaters",0,{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"AA25","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
["G","Total booster pump power (kW)",null,null,null,null,{"$f":"IF(K30=\"\",\"-\",K30)","v":"-"},null,null,null,null,null,null,null,null,{"$f":"IF(G30=\"\",\"\",G30)","v":"-"},null,null,null,null,null,null,null,"Service Water Heaters",{"$f":"Q30","v":0},{"$f":"\"SWH building area type based on: \"&G14&\" with an \"&G15&\" \"&G16&\" system with \"&G18&\" fuel. The input rating is \"&G19&M19&\" with an efficiency of \"&G21&\". The storage temperature is \"&G22&\" (F) with a peak hot water demand of \"&G23&\". Condenser heat recovery: \"&G24&\". There are \"&G28&\" \"&G27&\" pump(s) woth a total pump power of \"&G30&\" kW.\"","v":"SWH building area type based on: TEST with an   system with  fuel. The input rating is  with an efficiency of -. The storage temperature is  (F) with a peak hot water demand of -. Condenser heat recovery: . There are  - pump(s) woth a total pump power of - kW."},{"$f":"AA28","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
["G","Booster pump controls meet 90.1 Section 10.4.2",null,null,null,null,"Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Service Water Heaters",0,{"$f":"\"SWH building area type based on: \"&G15&\" with an \"&G16&\" \"&G18&\" system with \"&G19&\" fuel. The input rating is \"&G20&M20&\" with an efficiency of \"&G22&\". The storage temperature is \"&G23&\" (F) with a peak hot water demand of \"&G24&\". Condenser heat recovery: \"&G25&\". There are \"&G29&\" \"&G28&\" pump(s) woth a total pump power of \"&G31&\" kW.\"","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"AA29","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
["G"]
["G"]
["G","Note: Any credit for improved service hot water pumps must be submitted using the Exceptional Calculation Method."]
["G"]
["G",{"$f":"CONCATENATE(\"Service Hot Water Flow\",IF(ResDwellingUnitsExist=\"Yes\", \" (Except Residential Dwelling Units & Laundry)\", \"\"))","v":"Service Hot Water Flow (Except Residential Dwelling Units & Laundry)"}]
[null,{"$f":"CONCATENATE(IF(ResDwellingUnitsExist=\"Yes\",CONCATENATE(\"This section is only required to be completed if credit is modeled in the proposed model for low-flow fixtures serving the non-residential portions of the project.\",\" Complete the Multifamily Details tab to take credit for the fixtures in the dwelling units and laundry rooms serving resdential spaces. \",\"The project still must include the non-residential DHW flow in the baseline and proposed case for non-residential spaces even if no credit is taken.\"),CONCATENATE(\"This section is only required to be completed if credit is modeled in the proposed model for low-flow fixtures. \", \"Please note that DHW must be included in the model as designed even if no credit is modeled.\")),\" \n\nNote: The DHW Equivalent Full Load Hours of Operation is linked from the Main Building schedules section of the Schedules tab, which must be completed prior to completion of this tab. \",\"The Modeled DHW Flow rate will not calculate unless a value is entered for the service water heating Equivalent Full Load Hours in the Schedules Tab.\",\" Please ensure that the modeled schedules and flow rates are consistent with the values reported here\")","v":"This section is only required to be completed if credit is modeled in the proposed model for low-flow fixtures serving the non-residential portions of the project. Complete the Multifamily Details tab to take credit for the fixtures in the dwelling units and laundry rooms serving resdential spaces. The project still must include the non-residential DHW flow in the baseline and proposed case for non-residential spaces even if no credit is taken. \n\nNote: The DHW Equivalent Full Load Hours of Operation is linked from the Main Building schedules section of the Schedules tab, which must be completed prior to completion of this tab. The Modeled DHW Flow rate will not calculate unless a value is entered for the service water heating Equivalent Full Load Hours in the Schedules Tab. Please ensure that the modeled schedules and flow rates are consistent with the values reported here"}]
[]
[null,{"$f":"CONCATENATE(\"Average Cold Water Temperature \",IF(SI_IP_Units=\"IP\",\"(deg. F)\",\"(deg. C)\"))","v":"Average Cold Water Temperature (deg. F)"}]
[null,"Table 8.2: Low-Flow Fixtures"]
[]
[null,"General Information",null,null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,null,"Proposed Design",null,null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
[null,"Building ID","Fixture Type",{"$f":"IF(SI_IP_Units=\"IP\",\"Fixture Outlet Temperature\n (°F)\",\"Fixture Outlet Temperature\n (°C)\")","v":"Fixture Outlet Temperature\n (°F)"},"Percent\nHot Water\n(%)",null,{"$f":"IF(SI_IP_Units=\"IP\",\"Flow Rate \n(gpm or gpc)\",\"Flow Rate \n(L/s or L/c)\")","v":"Flow Rate \n(gpm or gpc)"},{"$f":"IF(SI_IP_Units=\"IP\",\"Annual Total Water Consumption of Fixture\n(gallons/year)\",\"Annual Total Water Consumption \n(Liters/year)\")","v":"Annual Total Water Consumption of Fixture\n(gallons/year)"},{"$f":"IF(SI_IP_Units=\"IP\",\"Annual Fixture Hot Water Consumption \n(gallons/year)\",\"Annual Fixture Hot Water Consumption \n(Liters/year)\")","v":"Annual Fixture Hot Water Consumption \n(gallons/year)"},null,{"$f":"IF(SI_IP_Units=\"IP\",\"Flow Rate \n(gpm or gpc)\",\"Flow Rate \n(L/s or L/c)\")","v":"Flow Rate \n(gpm or gpc)"},{"$f":"IF(SI_IP_Units=\"IP\",\"Annual Total Water Consumption \n(gallons/year)\",\"Annual Total Water Consumption \n(Liters/year)\")","v":"Annual Total Water Consumption \n(gallons/year)"},{"$f":"IF(SI_IP_Units=\"IP\",\"Annual Fixture Hot Water Consumption \n(gallons/year)\",\"Annual Fixture Hot Water Consumption \n(Liters/year)\")","v":"Annual Fixture Hot Water Consumption \n(gallons/year)"},"Plans / Specs"]
[null,null,"Helpful Hints\n•  Describe a type of hot water fixture included in the project (example: Lavatory Faucets)","Helpful Hints\n•  Percent hot water is the portion of water usage from the fixture that is hot water versus cold water (e.g. - lavatory cold water usage associated with brushing teeth versus hot water usage associated with washing hands)",null,null,"Helpful Hints\n•  Fixtures included in the WE Prerequisite Indoor Water Use Reduction calculations: values must be consistent with the WE Prerequisite form\n•  Additional fixtures not included in WE Prerequisite Indoor Water Use Reduction: Use Proposed values or provide supporting documentation for Baseline assumption (example: Energy Star documentation of average hot water usage for dishwasher or clothes washer)",null,null,null,"Helpful Hints\n•  Values should be consistent with the design (or installed) fixtures and WE Prerequisite Indoor Water Use Reduction (if applicable)",null,null,null,null,{"$f":"IF('General Information'!$K$48=2013,\"In accordance with Prescriptive Requirements of 90.1-2013 Section 7.5\",\"In accordance with Prescriptive Requirements of 90.1-2010 Section 7.5\")","v":"In accordance with Prescriptive Requirements of 90.1-2013 Section 7.5"}]
[]
[null,"Building ID","Fixture_Type","Fixture_Temp","Percent_HW",null,"Base_Fixture_Flow","Base_Total_Annual_Fixture_Consumption","Base_Annual_HW_Fixture_Consumption",null,"Design_Fixture_Flow","Design_Total_Annual_Fixture_Consumption","Design_Annual_HW_Fixture_Consumption","Design_Annual_HW_Fixture_Consumption",null,{"$f":"IF(AND($W46<>0,$D46<>\"\"),$W46,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"Fixture_DT"]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,null,null,null,{"$f":"IFERROR(IF(H47>0,H47*$E47*($D47-$M$39)/(INDEX(SWH_Flow_Table,MATCH($B47,SWH_Flow_Index,0),MATCH($D$56,SWH_Flow_Hdr,0))-$M$39),\"\"),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(L47>0,L47*$E47*($D47-$M$39)/(INDEX(SWH_Flow_Table,MATCH($B47,SWH_Flow_Index,0),MATCH($D$56,SWH_Flow_Hdr,0))-$M$39),\"\"),\"\")","v":""},null,null,"N/A",null,null,null,null,null,null,null,"Low-Flow Fixtures",{"$f":"Q47","v":0},{"$f":"\"Fixtrue type of \"&C47&\" with fixture outlet temperature of \"&D47&\" (F) and (\"&E47&\"/1) % hot water. The \"&C47&\" has a flow rate of \"&G47&\" gpm with annual total water consumption of \"&H47&\" gallons/year.\"","v":"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year."},{"$f":"\"Fixtrue type of \"&C47&\" with fixture outlet temperature of \"&D47&\" (F) and (\"&E47&\"/1) % hot water. The \"&C47&\" has a flow rate of \"&K47&\" gpm with annual total water consumption of \"&L47&\" gallons/year.\"","v":"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year."},null,null,{"$f":"IFERROR(IF(D47-$M$39<0,0,D47-$M$39),\"\")","v":0}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,null,null,null,{"$f":"IFERROR(IF(H48>0,H48*$E48*($D48-$M$39)/(INDEX(SWH_Flow_Table,MATCH($B48,SWH_Flow_Index,0),MATCH($D$56,SWH_Flow_Hdr,0))-$M$39),\"\"),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(L48>0,L48*$E48*($D48-$M$39)/(INDEX(SWH_Flow_Table,MATCH($B48,SWH_Flow_Index,0),MATCH($D$56,SWH_Flow_Hdr,0))-$M$39),\"\"),\"\")","v":""},null,null,"N/A",null,null,null,null,null,null,null,"Low-Flow Fixtures",{"$f":"Q48","v":0},{"$f":"\"Fixtrue type of \"&C48&\" with fixture outlet temperature of \"&D48&\" (F) and (\"&E48&\"/1) % hot water. The \"&C48&\" has a flow rate of \"&G48&\" gpm with annual total water consumption of \"&H48&\" gallons/year.\"","v":"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year."},{"$f":"\"Fixtrue type of \"&C48&\" with fixture outlet temperature of \"&D48&\" (F) and (\"&E48&\"/1) % hot water. The \"&C48&\" has a flow rate of \"&K48&\" gpm with annual total water consumption of \"&L48&\" gallons/year.\"","v":"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year."},null,null,{"$f":"IFERROR(IF(D48-$M$39<0,0,D48-$M$39),\"\")","v":0}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,null,null,null,{"$f":"IFERROR(IF(H49>0,H49*$E49*($D49-$M$39)/(INDEX(SWH_Flow_Table,MATCH($B49,SWH_Flow_Index,0),MATCH($D$56,SWH_Flow_Hdr,0))-$M$39),\"\"),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(L49>0,L49*$E49*($D49-$M$39)/(INDEX(SWH_Flow_Table,MATCH($B49,SWH_Flow_Index,0),MATCH($D$56,SWH_Flow_Hdr,0))-$M$39),\"\"),\"\")","v":""},null,null,"N/A",null,null,null,null,null,null,null,"Low-Flow Fixtures",{"$f":"Q49","v":0},"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year.","Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year.",null,null,0]
["F",{"$f":"GI_Project_Name","v":0},null,null,null,null,null,null,{"$f":"IFERROR(IF(H50>0,H50*$E50*($D50-$M$39)/(INDEX(SWH_Flow_Table,MATCH($B50,SWH_Flow_Index,0),MATCH($D$56,SWH_Flow_Hdr,0))-$M$39),\"\"),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(L50>0,L50*$E50*($D50-$M$39)/(INDEX(SWH_Flow_Table,MATCH($B50,SWH_Flow_Index,0),MATCH($D$56,SWH_Flow_Hdr,0))-$M$39),\"\"),\"\")","v":""},null,null,"N/A",null,null,null,null,null,null,null,"Low-Flow Fixtures",{"$f":"Q50","v":0},"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year.","Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year.",null,null,0]
["G"]
[null,"Table 8.3: Low-Flow Fixture Summary"]
["G","Summary",null,null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,null,"Proposed Design",null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},null,"Measure #"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2013,\"In accordance with Prescriptive Requirements of 90.1-2013 Section 7.5\",\"In accordance with Prescriptive Requirements of 90.1-2010 Section 7.5\")","v":"In accordance with Prescriptive Requirements of 90.1-2013 Section 7.5"}]
["G","Building ID","DHW Equivalent Full Load Hours of Operation",{"$f":"CONCATENATE(\"DHW Supply Temperature from Water Heater\",IF(SI_IP_Units=\"IP\",\" (deg. F)\",\" (deg. C)\"))","v":"DHW Supply Temperature from Water Heater (deg. F)"},null,null,{"$f":"CONCATENATE(\"Modeled DHW Flow Rate \",IF(SI_IP_Units=\"IP\",\"gallons/minute\",\"Liters/second\"))","v":"Modeled DHW Flow Rate gallons/minute"},{"$f":"CONCATENATE(\"Total Annual Hot Water Consumption at Fixtures\",IF(SI_IP_Units=\"IP\",\" (gallons/year)\",\" (Liters/year)\"))","v":"Total Annual Hot Water Consumption at Fixtures (gallons/year)"},{"$f":"CONCATENATE(\"Total Annual DHW Heater Consumption\",IF(SI_IP_Units=\"IP\",\" (gallons/year)\",\" (Liters/year)\"))","v":"Total Annual DHW Heater Consumption (gallons/year)"},null,{"$f":"CONCATENATE(\"Modeled DHW Flow Rate \",IF(SI_IP_Units=\"IP\",\"gallons/minute\",\"Liters/second\"))","v":"Modeled DHW Flow Rate gallons/minute"},{"$f":"CONCATENATE(\"Total Annual Hot Water Consumption at Fixtures\",IF(SI_IP_Units=\"IP\",\" (gallons/year)\",\" (Liters/year)\"))","v":"Total Annual Hot Water Consumption at Fixtures (gallons/year)"},{"$f":"CONCATENATE(\"Total Annual DHW Heater Consumption\",IF(SI_IP_Units=\"IP\",\" (gallons/year)\",\" (Liters/year)\"))","v":"Total Annual DHW Heater Consumption (gallons/year)"}]
[null,"Building ID","DHW_EFLH","DHW_Supply_Temp",null,null,"Base_Modeled_DHW_Flow","Base_Fixture_HW_Use","Base_DHW_Heater_Use",null,"Design_Modeled_DHW_Flow","Design_Fixture_HW_Use","Design_DHW_Heater_Use"]
[null,{"$f":"'1 - Multiple Buildings Details'!B25","v":0},{"$f":"'2a - Schedules'!$E$12","v":2628},null,null,null,{"$f":"IFERROR(IF(SI_IP_Units=\"IP\",I57/$C57/60,I57/$C57/60/60),\"\")","v":""},{"$f":"IFERROR(SUMIF(SWH_Fixture_Index,$B57,(OFFSET(SWH_Fixture_Index,0,MATCH($I$46,SWH_Fixture_Hdr,0)-1,ROWS(SWH_Fixture_Table),1))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(OFFSET(SWH_Fixture_Index,0,MATCH($I$46,SWH_Fixture_Hdr,0)-1,ROWS(SWH_Fixture_Index),1),OFFSET(SWH_Fixture_Index,0,MATCH($AD$46,SWH_Fixture_Hdr,0)-1,ROWS(SWH_Fixture_Index),1),--(SWH_Fixture_Index=$B57))/($D57*$M$39/$D57/$M$39*($D57-$M$39)),\"\")","v":""},null,{"$f":"IFERROR(IF(SI_IP_Units=\"IP\",M57/$C57/60,M57/$C57/60/60),\"\")","v":""},{"$f":"IFERROR(SUMIF(SWH_Fixture_Index,$B57,(OFFSET(SWH_Fixture_Index,0,MATCH($M$46,SWH_Fixture_Hdr,0)-1,ROWS(SWH_Fixture_Table),1))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(OFFSET(SWH_Fixture_Index,0,MATCH($M$46,SWH_Fixture_Hdr,0)-1,ROWS(SWH_Fixture_Index),1),OFFSET(SWH_Fixture_Index,0,MATCH($AD$46,SWH_Fixture_Hdr,0)-1,ROWS(SWH_Fixture_Index),1),--(SWH_Fixture_Index=$B57))/($D57*$M$39/$D57/$M$39*($D57-$M$39)),\"\")","v":""},"N/A",null,null,null,null,null,null,null,null,null,"Low-Flow Fixture Summary",{"$f":"P57","v":0},{"$f":"\"Low flow fixture total modeled DHW flow rate is \"&G57&\" gallons/minute with total annual hot water consumption st fixtures of \"&H57&\" gallons/year. The total annual DHW heater consumption is \"&I57&\" gallons/year.\"","v":"Low flow fixture total modeled DHW flow rate is  gallons/minute with total annual hot water consumption st fixtures of 0 gallons/year. The total annual DHW heater consumption is  gallons/year."},{"$f":"\"Low flow fixture total modeled DHW flow rate is \"&K57&\" gallons/minute with total annual hot water consumption st fixtures of \"&L57&\" gallons/year. The total annual DHW heater consumption is \"&M57&\" gallons/year.\"","v":"Low flow fixture total modeled DHW flow rate is  gallons/minute with total annual hot water consumption st fixtures of 0 gallons/year. The total annual DHW heater consumption is  gallons/year."}]
["G"]
["G","Additional notes:"]
["G"]
[]
[]
[]
[]
[]
[]
[]
["G"]
[]
["G"]
["G"]
["G"]
[]
[]
[]
[]
[]
[]
[]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]
["G"]

{"sheet":"SWH Lookup","index":23,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":true,"merged":[[1,1,1,2],[1,4,1,6]]}
[null,null,null,null,"*this table is used as a lookup"]
[null,"Table G3.1.1-2 Baseline Service Hot-Water System",null,null,"Table G3.1.1-2 Baseline Service Hot-Water System"]
[null,"Building Area Type","Baseline Heating Method",null,"Building Area Type","Fuel","System Type"]
[null,"Automotive facility","Gas storage water heater",null,"Automotive facility","Gas","Storage"]
[null,"Convention center","Electric resistance storage water heater",null,"Convention center","Electric Resistance","Storage"]
[null,"Courthouse","Electric resistance storage water heater",null,"Courthouse","Electric Resistance","Storage"]
[null,"Dining: Bar lounge/leisure","Gas storage water heater",null,"Dining: Bar lounge/leisure","Gas","Storage"]
[null,"Dining: Cafeteria/fast food","Gas storage water heater",null,"Dining: Cafeteria/fast food","Gas","Storage"]
[null,"Dining: Family","Gas storage water heater",null,"Dining: Family","Gas","Storage"]
[null,"Dormitory","Gas storage water heater",null,"Dormitory","Gas","Storage"]
[null,"Exercise center","Gas storage water heater",null,"Exercise center","Gas","Storage"]
[null,"Fire station","Gas storage water heater",null,"Fire station","Gas","Storage"]
[null,"Gymnasium","Gas storage water heater",null,"Gymnasium","Gas","Storage"]
[null,"Health-care clinic","Gas storage water heater",null,"Health-care clinic","Gas","Storage"]
[null,"Hospital","Gas storage water heater",null,"Hospital","Gas","Storage"]
[null,"Hotel","Gas storage water heater",null,"Hotel","Gas","Storage"]
[null,"Library","Electric resistance storage water heater",null,"Library","Electric Resistance","Storage"]
[null,"Manufacturing facility","Gas storage water heater",null,"Manufacturing facility","Gas","Storage"]
[null,"Motel","Gas storage water heater",null,"Motel","Gas","Storage"]
[null,"Motion picture theater","Electric resistance storage water heater",null,"Motion picture theater","Electric Resistance","Storage"]
[null,"Multifamily","Gas storage water heater",null,"Multifamily","Gas","Storage"]
[null,"Museum","Electric resistance storage water heater",null,"Museum","Electric Resistance","Storage"]
[null,"Office","Electric resistance storage water heater",null,"Office","Electric Resistance","Storage"]
[null,"Parking garage","Electric resistance storage water heater",null,"Parking garage","Electric Resistance","Storage"]
[null,"Penitentiary","Gas storage water heater",null,"Penitentiary","Gas","Storage"]
[null,"Performing arts theater","Gas storage water heater",null,"Performing arts theater","Gas","Storage"]
[null,"Police station","Electric resistance storage water heater",null,"Police station","Electric Resistance","Storage"]
[null,"Post office","Electric resistance storage water heater",null,"Post office","Electric Resistance","Storage"]
[null,"Religious building","Electric resistance storage water heater",null,"Religious building","Electric Resistance","Storage"]
[null,"Retail","Electric resistance storage water heater",null,"Retail","Electric Resistance","Storage"]
[null,"School/university","Gas storage water heater",null,"School/university","Gas","Storage"]
[null,"Sports arena","Gas storage water heater",null,"Sports arena","Gas","Storage"]
[null,"Town hall","Electric resistance storage water heater",null,"Town hall","Electric Resistance","Storage"]
[null,"Transportation","Electric resistance storage water heater",null,"Transportation","Electric Resistance","Storage"]
[null,"Warehouse","Electric resistance storage water heater",null,"Warehouse","Electric Resistance","Storage"]
[null,"Workshop","Gas storage water heater",null,"Workshop","Gas","Storage"]
[null,"All Others","Gas storage water heater",null,"All Others","Gas","Storage"]

{"sheet":"9 - General HVAC","index":24,"n_rows":88,"n_cols":21,"rows_kept":88,"cut":false,"hidden":false,"merged":[[37,1,37,6],[42,1,42,4],[33,5,33,6],[26,5,26,6],[32,5,32,6],[40,1,40,4],[29,5,29,6],[30,5,30,6],[41,1,41,4],[39,1,39,4],[31,5,31,6],[27,5,27,6],[21,2,21,3],[22,2,22,3],[13,1,14,1],[26,1,27,1],[27,2,27,3],[13,2,13,3],[14,2,14,3],[18,2,18,3],[19,2,19,3],[20,2,20,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[48,1,48,4],[54,1,54,4],[43,1,43,4],[53,1,53,4],[51,1,51,4],[52,1,52,4],[50,1,50,4],[49,1,49,4],[47,1,47,4],[46,1,46,4],[87,1,87,6],[86,1,86,6],[79,1,79,4],[55,1,55,4],[56,1,56,4],[57,1,57,4],[58,1,58,4],[59,1,59,4],[60,1,60,4],[62,1,62,4],[63,1,63,4],[81,1,81,4],[78,1,78,4],[84,1,84,4],[70,1,70,4],[77,1,77,4],[4,1,4,6],[10,1,10,6],[9,1,9,6],[7,1,7,5],[5,1,5,5],[82,1,82,4],[83,1,83,4],[61,1,61,4],[64,1,64,4],[65,1,65,4],[67,1,67,4],[66,1,66,4],[80,1,80,4],[75,1,75,4],[72,1,72,4],[71,1,71,4],[73,1,73,4],[74,1,74,4],[76,1,76,4]]}
["G"]
["G","General HVAC"]
["G"]
["G"]
["G","Instructions: Confirm that the energy model complies with the General HVAC requirements listed, and provide a narrative explaining any discrepancies. Select the types of water-side systems that are installed on the project site (proposed). Describe each type of HVAC system in the proposed. Select the applicable baseline HVAC system type(s). Confirm that each of the HVAC modeling requirements have been incorporated into the energy models. Please refer to the column header notes for information about Appendix G modeling protocol. For any information not applicable to the project, simply enter \"N/A\". ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Enclosed parking garage ventilation systems automatically detect contaminant levels and modulate fan airflows rates to 50% or less of design capacity per Section 6.4.3.4.5"]
["G"]
["G","Spaces larger than 500 square feet (50 square meters), with occupancy of greater than or equal to 25 people per 1,000 square feet (100 square meters), and are served by systems that have one of the following: an air-side economizer, automatic modulating control of the outdoor air damper, or a design outdoor airflow of greater than 3,000 cfm (1,400 L/s), have been designed with demand control ventilation per Section 6.4.3.8."]
["G"]
["G","For each item entered as “No” above, describe the applicable ASHRAE 90.1 Appendix G exception(s) that apply, or the circumstances preventing the HVAC parameters from being modeled as required. If the energy simulation software is not capable of modeling the required parameters, describe the adjustments that were made to provide a similar representation or provide a narrative justifying why the predicted energy performance results will not be influenced."]
["G"]
["G"]
["G","Table 9.1: Proposed HVAC System Type(s)"]
["G","Building ID","System Description",null,"Energy Source #1","Energy Source #2","Areas Modeled"]
[null,null,"Helpful Hints\n•  Describe each type of HVAC system included in the Proposed building (example: Constant volume single-zone ground source heat pumps with dedicated outdoor air units with energy recovery).",null,"Helpful Hints\n•  Select the Energy Source(s) associated with this system.","Helpful Hints\n•  Select the Energy Source(s) associated with this system.","Helpful Hints\n•  Described areas served by each system.\n•  The HVAC system type and all related parameters, such as equipment capacities and efficiencies, must be modeled as designed (or installed) per Table G3.1#10(a&b)\n•  Where no heating system exists or has been designed, the system type shall be the same as modeled in the baseline building design and shall comply with, but not exceed, the requirements of Section 6, per Table G3.1#10(c)\n•  Where no cooling system exists or has been designed, the cooling system is modeled identically to the Baseline case per Table G3.1#10(d), unless using baseline HVAC system types 9 or 10.",null,"Electricity Used? (1 = Yes)"]
[null,{"$f":"GI_Project_Name","v":0}]
[null,0]
[null,0]
[null,0,null,null,null,null,null,null,{"$f":"IF(OR(E19=\"Electricity\",F19=\"Electricity\"),1,0)","v":0}]
[null,0,null,null,null,null,null,null,{"$f":"IF(OR(E20=\"Electricity\",F20=\"Electricity\"),1,0)","v":0}]
[null,0,null,null,null,null,null,null,0]
["A",0,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,0]
["G",null,null,null,null," ",null,null,{"$f":"SUM(I19:I23)","v":0}]
["G"]
["G","Table 9.2: Baseline HVAC System Type(s)"]
["G","Building ID","Model Input Parameter","Table G3.1.1-3 System Type \n(or Semiconditioned System Description)","G3.1.1 Exception \n(or Semiconditioned Capacity and Area)","Spaces Modeled",null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(Q31:Q38)","v":0},{"$f":"SUM(R31:R38)","v":0}]
["G",null,"Helpful Hints\n•  Refer to Section G3.1.1 and Table G3.1.1-3 (including footnotes) for Primary HVAC System selection\n•  Systems 1-4, 9-13: each thermal block shall be modeled with its own system\n•  Systems 5-8: each floor shall be modeled with a separate system\n•  Additional system types for conditioned spaces only permitted using Exceptions to G3.1.1 (min 20,000 sq ft (1,860 sq m) required for exception (b))\n•  Systems serving semiconditioned spaces should be modeled identically to the system in the Proposed case (see definition of space in Section 3.2 of ASHRAE 90.1\n•  For California Title-24 projects, type in the appropriate system type",null,"Helpful Hints\n•  Conditioned: describe the exception from G3.1.1 used to model this additional Baseline system type (example: Exception (c) used since peak loads differ by more than 10 Btu/h-sq ft (0.03 kW/sq m))\n•  Semiconditioned: list the total system capacity and floor area it serves","Helpful Hints\n•  List the spaces modeled with the primary system type (example: all spaces except kitchen)",null,null,null,null,null,null,"ctrl+shift+enter",null,"ctrl+shift+enter",null,"QA Checks help cells (Systems 1,5,7 or 10?)","QA Checks help cells (Systems 7,8,11,12 or 13?)"]
["G",{"$f":"B27","v":"Building ID"},{"$f":"C27","v":"Model Input Parameter"},{"$f":"D27","v":"Table G3.1.1-3 System Type \n(or Semiconditioned System Description)"},{"$f":"E27","v":"G3.1.1 Exception \n(or Semiconditioned Capacity and Area)"},{"$f":"F27","v":"Spaces Modeled"}]
[null,{"$f":"GI_Project_Name","v":0},null,null,null,null,null,null,null,{"$f":"IFERROR(_xlfn.NUMBERVALUE(IF(ISNUMBER(SEARCH(\"California\",D30)),\"Cali\",SUBSTITUTE(MID(D30,8,2),\" \",\"\"))),\"\")","v":0}]
[null,0,null,null,null,null,null,null,null,0,null,{"$f":"IF(J31=0,TRUE,IF(OR(J31=2,J31=3,J31=4,J31=6,J31=9,J31=10),TRUE,FALSE))","v":true},{"$f":"AND(EXACT(L31:L35,TRUE))","v":false},{"$f":"IF(J31=0,TRUE,IF(OR(J31=7,J31=8,J31=11,J31=12,J31=13),TRUE,FALSE))","v":true},{"$f":"AND(EXACT(N31:N35,TRUE))","v":false},null,{"$f":"IF(OR(J31=1,J31=5,J31=7,J31=10),1,0)","v":0},{"$f":"IF(OR(J31=7,J31=8,J31=11,J31=12),1,0)","v":0}]
[null,0,null,null,null,null,null,null,null,{"$f":"IFERROR(_xlfn.NUMBERVALUE(IF(ISNUMBER(SEARCH(\"California\",D32)),\"Cali\",SUBSTITUTE(MID(D32,8,2),\" \",\"\"))),\"\")","v":0},null,{"$f":"IF(J32=0,TRUE,IF(OR(J32=2,J32=3,J32=4,J32=6,J32=9,J32=10),TRUE,FALSE))","v":true},null,{"$f":"IF(J32=0,TRUE,IF(OR(J32=7,J32=8,J32=11,J32=12,J32=13),TRUE,FALSE))","v":true},null,null,{"$f":"IF(OR(J32=1,J32=5,J32=7,J32=10),1,0)","v":0},{"$f":"IF(OR(J32=7,J32=8,J32=11,J32=12),1,0)","v":0}]
[null,0,null,null,null,null,null,null,null,{"$f":"IFERROR(_xlfn.NUMBERVALUE(IF(ISNUMBER(SEARCH(\"California\",D33)),\"Cali\",SUBSTITUTE(MID(D33,8,2),\" \",\"\"))),\"\")","v":0},null,true,null,true,null,null,0,0]
["B",0,null,null,null,null,null,null,null,{"$f":"IFERROR(_xlfn.NUMBERVALUE(IF(ISNUMBER(SEARCH(\"California\",D34)),\"Cali\",SUBSTITUTE(MID(D34,8,2),\" \",\"\"))),\"\")","v":0},null,true,null,true,null,null,0,0]
["G"]
["G"]
["G","HVAC Modeling Requirements"]
["G","All proposed and baseline HVAC system types must be entered above to generate the correct modeling requirements below. Identify each applicable item (indicated in gray) as \"Yes\" or \"No\", and provide a further description for any items marked as \"No\" or \"N/A\"."]
["G","Proposed HVAC Requirements"]
["G","All proposed HVAC systems and related parameters, such as equipment capacities, efficiencies, airflows, fans, etc. have been modeled as designed and are consistent with supporting documentation.",null,null,null,null,"Required for all systems"]
["G","Each proposed HVAC thermal zone has been modeled as a separate thermal block except as allowed by Table G3.1#7.",null,null,null,null,"Required for all systems"]
["G","All proposed HVAC systems serving conditioned spaces have been modeled with heating and cooling as required by Table G3.1#1(b), with heating and/or cooling added as necessary identically to the baseline per Table G3.1#10(c&d) except where System types (9) or (10) have been modeled.",null,null,null,null,"Required for all systems"]
["G","All proposed HVAC systems and related parameters can be modeled directly in the energy simulation program used.",null,null,null,null,"Required for all systems"]
["G","All proposed fan part-load efficiency curves for variable volume fans have been modeled identically to the baseline curves for variable volume fans (if not, provide a description of the fan curves used in the space at the bottom of this table, and confirm that the proposed curves are representative of the actual building design).",null,null,null,null,"Required for all systems"]
["G"]
["G","Baseline Air-Side HVAC Requirements",null,null,null,null,null,null,"conditional final t/f","number search 1","number search 2"]
[null,"Temperature and humidity control set points and schedules as well as temperature control throttling range are the same for proposed design and baseline building design. (Table G3.1 No 4).",null,null,null,null,"Required for all systems"]
["G","All baseline single zone systems have been modeled with a separate HVAC system for each thermal block per G3.1.1.",null,null,null,null,"Required for Systems 1-4, 9-13",null,{"$f":"IF(J48=TRUE,TRUE,FALSE)","v":false},{"$f":"isbasehvac(1,2,3,4,9,10,11,12,13)","v":false}]
["G","All baseline VAV systems have been modeled with an HVAC system per floor, or one system per group of thermodynamically similar floors per G3.1.1.",null,null,null,null,"Required for Systems 5-8",null,{"$f":"IF(J49=TRUE,TRUE,FALSE)","v":false},{"$f":"isbasehvac(5,6,7,8)","v":false}]
["G","All applicable baseline exceptions to G3.1.1 have been implemented. Note that these exceptions are required, not optional.",null,null,null,null,"Required for all systems",null,true]
["G","Where baseline or proposed efficiency ratings for DX cooling equipment, such as EER and COP, include fan energy, the descriptor is broken down into its components so that supply fan energy can be modeled separately per G3.1.2.1.",null,null,null,null,"Required for Systems 1-6\nRequired for Systems 1, 3, and 5 if District Heating has been selected on the General Information tab\nNot required if District Cooling has been selected",null,{"$f":"IF(J51=TRUE,TRUE,IF(AND(K51=TRUE,'General Information'!$L$61=TRUE),TRUE,FALSE))","v":false},{"$f":"isbasehvac(1,2,3,4,5,6)","v":false},{"$f":"isbasehvac(1,3,5)","v":false}]
["G","All baseline system cooling capacities auto-sized with 15% oversizing per G3.1.2.2 (at the system or plant level, but not both).",null,null,null,null,"Required for all systems",null,true]
["G","All baseline system heating capacities auto-sized with 25% oversizing per G3.1.2.2 (at the system or plant level, but not both).",null,null,null,null,"Required for all systems",null,true]
["G","All baseline supply and return fans operate continuously when spaces are occupied and cycle when unoccupied per G3.1.2.4.",null,null,null,null,"Required for all systems",null,true]
["G","Demand control ventilation is modeled in the baseline case for all spaces larger than 500 sq ft (50 sq m) that have a design occupancy for ventilation of greater than or equal to 25 people per 1,000 sq ft (100 sq m) of floor area (except for spaces served by baseline systems that do not have one of the following: an air-side economizer, automatic modulating control of the outdoor air damper, or a design outdoor airflow of greater than 3,000 cfm (1,400 L/s)) per G3.1.2.5 / 6.4.3.8.",null,null,null,null,"Required for Systems 3-13",null,{"$f":"IF(J55=TRUE,TRUE,FALSE)","v":false},{"$f":"isbasehvac(3,4,5,6,7,8,9,10,11,12,13)","v":false}]
["G",{"$f":"IF('General Information'!E9=\"ENERGY STAR MFHR\",DropdownData!DV3,DropdownData!DW3)","v":"Mechanical ventilation was modeled following ENERGY STAR MFHR Simulation Guidelines Section 6.5.12. In the common spaces, the baseline ventilation rate was modeled the same as in the proposed design without exceeding ASHRAE 62.1-2013 (Simulation Guidelines Section 6.5.12, 1(b). \nIn apartments, the baseline ventilation method (mechanical versus natural) and controls (continuous versus intermittent) was modeled as specified for each application. The baseline local mechanical exhaust from bathrooms and kitchens, and the baseline dwelling-unit ventilation rate was modeled using the same rates as in the Proposed Design, without exceeding the minimum required by ASHRAE 62.2-2013.\nIf the same mechanical ventilation system was used to provide both local mechanical exhaust and whole-unit ventilation, the baseline ventilation rate was based on the greater of the two rates. \n"},null,null,null,null,"Required for all systems",null,true]
["G","All baseline systems are modeled with zero outside airflow when fans are cycled to meet unoccupied setback temperatures.",null,null,null,null,"Required for all systems",null,true]
["G","All baseline supply airflows for Systems 1-8 and 11-13 have been auto-sized based on a 20°F (11.1°C) supply-air-to-room-air cooling temperature difference (or the airflow rate required to comply with applicable codes/standards, whichever is greater) per G3.1.2.8.1. Exception: Laboratory spaces have been modeled with a 17°F (9.4°C) supply-air-to-room-air temperature difference or the required ventilation air or makeup air, whichever is greater.",null,null,null,null,"Required for Systems 1-8, 11-13",null,{"$f":"IF(J58=TRUE,TRUE,FALSE)","v":false},{"$f":"isbasehvac(1,2,3,4,5,6,7,8,11,12,13)","v":false}]
["G","All baseline supply airflows for systems 9-10 have been auto sized based on the difference between a supply air temperature set point of 105°F (40.6°C) and the design space heating temperature set point (or the airflow rate required to comply with applicable codes/standards, whichever is greater) per G3.1.2.8.2.",null,null,null,null,"Required for Systems 9 and 10",null,false,{"$f":"isbasehvac(9,10)","v":false}]
["G","All baseline heat pumps modeled with electric auxiliary heat only energized below 40°F (4°C) and as the last thermostat stage per G3.1.3.1 (compressor still enabled below 40°F (4°C)). The compressor continues to operate in conjunction with the electric auxiliary heat as low as 17°F(-8.3°C), in accordance with the Baseline equipment efficiency ratings from ASHRAE 90.1 Section 6.8.  See ASHRAE Interpretation 90.1-2007-09 for more information.",null,null,null,null,"Required for Systems 2 and 4\nNot required if District Heating and/or Cooling has been selected on the General Information tab",null,false,{"$f":"isbasehvac(2,4)","v":false}]
["G","All baseline VAV systems modeled with supply air temperature reset of 5°F (2.3°C) under minimum cooling load conditions per G3.1.3.12.",null,null,null,null,"Required for Systems 5-8",null,false,{"$f":"isbasehvac(5,6,7,8)","v":false}]
["G","All baseline VAV systems modeled with preheat coils controlled to a fixed setpoint of 20F less than the design room heating temperature setpoint per G3.1.3.19.",null,null,null,null,"Required for Systems 5-8",null,false,{"$f":"isbasehvac(5,6,7,8)","v":false}]
["G","All baseline VAV reheat boxes modeled with a minimum flow setpoint of 30% of peak zone flow (or minimum outdoor airflow rate or code required rate) per G3.1.3.13.",null,null,null,null,"Required for Systems 5 and 7",null,false,{"$f":"isbasehvac(5,7)","v":false}]
["G","All baseline fans in parallel VAV fan-powered boxes sized for 50% of peak primary airflow and modeled with 0.35 W/cfm (0.74 W/L/s) fan power and a minimum flow setpoint of 30% of peak (or minimum ventilation rate) per G3.1.3.14.",null,null,null,null,"Required for Systems 6 and 8",null,false,{"$f":"isbasehvac(6,8)","v":false}]
[null,"All baseline VAV fans (Systems 5-8 and 11) are modeled with VAV part-load performance curves consistent with Table G3.1.3.15 Method 1 or Method 2.",null,null,null,null,"Required for Systems 5-8 and 11",null,{"$f":"IF(J65=TRUE,TRUE,FALSE)","v":false},{"$f":"isbasehvac(5,6,7,8,11)","v":false}]
[null,"Computer room single-zone VAV systems (System 11) shall be controlled to a minimum volume setpoint of 50% of the design airflow rate, the minimum ventilation outdoor airflow rate, or the airflow rate required to comply with the applicable codes or accreditation standards, whichever is larger. Fan volume shall be reset from 100% airflow at 100% load to minimum airflow at 50% cooling load. In heating mode, fan will operate at the minimum airflow, per G3.1.3.17.",null,null,null,null,"Required for System 11",null,{"$f":"IF(J66=TRUE,TRUE,FALSE)","v":false},{"$f":"isbasehvac(11)","v":false}]
[null,"Computer room single-zone VAV systems (System 11) supply air temperature shall be reset from the minimum supply air temperature at 50% cooling load to the space temperature at 0% cooling load, per G3.1.3.17.",null,null,null,null,"Required for System 11",null,{"$f":"IF(J67=TRUE,TRUE,FALSE)","v":false},{"$f":"isbasehvac(11)","v":false}]
[null,"If the proposed design HVAC system(s) have humidistat controls, then the baseline systems shall employ mechanical cooling for dehumidification and shall have reheat available to avoid overcooling. When a baseline system does not meet any of the exceptions to Section 6.5.2.3, then only 25% of the system reheat energy shall be included in the baseline building performance, per G3.1.3.18",null,null,null,null,"Required for all systems",null,true]
["G"]
["G","Baseline Water-Side HVAC Requirements"]
["G","The baseline boiler(s) have been modeled as natural draft per G3.1.3.2.",null,null,null,null,"Required for Systems 1, 5, 7, 11 (if the proposed design heating source is fossil fuel), and 12\nRequired for Systems 1-2, 5-8, and 11-12 if District Cooling has been selected on the General Information tab\nNot required if District Heating has been selected",null,{"$f":"IF('General Information'!$L$61=TRUE,FALSE,IF(J71=TRUE,TRUE,IF(AND(K71=TRUE,'General Information'!$K$61=TRUE),TRUE,FALSE)))","v":false},{"$f":"isbasehvac(1,5,7,11,12)","v":false},{"$f":"isbasehvac(1,2,5,6,7,8,11,12)","v":false}]
["G","The baseline hot water design supply temperature has been modeled as 180°F (82°C) with a return temperature of 130°F (54°C) per G3.1.3.3.",null,null,null,null,"Required for Systems 1, 5, 7, 11 and 12\nRequired for Systems 1-2 and 5-8 if District Cooling has been selected on the General Information tab\nNot required if District Heating has been selected",null,{"$f":"IF('General Information'!$L$61=TRUE,FALSE,IF(J72=TRUE,TRUE,IF(AND(K72=TRUE,'General Information'!$K$61=TRUE),TRUE,FALSE)))","v":false},{"$f":"isbasehvac(1,5,7,11,12)","v":false},{"$f":"isbasehvac(1,2,5,6,7,8)","v":false}]
["G","The baseline hot water supply temperature reset schedule has been modeled as 180°F (82°C) at outdoor temperatures 20°F (-7°C) and below, 150°F (66°C) at outdoor temperatures 50°F (10°C) and above, and ramped linearly between 180°F (82°C) and 150°F (66°C) at outdoor temperatures between 20°F (-7°C) and 50°F (10°C) per G3.1.3.4.",null,null,null,null,"Required for Systems 1, 5, 7, 11 and 12\nRequired for Systems 1-2 and 5-8 if District Cooling has been selected on the General Information tab\nNot required if District Heating has been selected",null,{"$f":"IF('General Information'!$L$61=TRUE,FALSE,IF(J73=TRUE,TRUE,IF(AND(K73=TRUE,'General Information'!$K$61=TRUE),TRUE,FALSE)))","v":false},{"$f":"isbasehvac(1,5,7,11,12)","v":false},{"$f":"isbasehvac(1,2,5,6,7,8)","v":false}]
["G","The baseline hot water pump power has been modeled as 19 W/gpm (301 kW/1,000 L/s) per G3.1.3.5.",null,null,null,null,"Required for Systems 1, 5, 7, 11 and 12\nRequired for Systems 1-2 and 5-8 if District Cooling has been selected on the General Information tab\nNot required if District Heating has been selected",null,{"$f":"IF('General Information'!$L$61=TRUE,FALSE,IF(J74=TRUE,TRUE,IF(AND(K74=TRUE,'General Information'!$K$61=TRUE),TRUE,FALSE)))","v":false},{"$f":"isbasehvac(1,5,7,11,12)","v":false},{"$f":"isbasehvac(1,2,5,6,7,8)","v":false}]
["G","Piping losses have not been modeled in the baseline for hot or chilled water per G3.1.3.6.",null,null,null,null,"Required for Systems 1, 5, 7, 8, 11, 12, and 13\nRequired for all Systems if District Heating and/or Cooling has been selected on the General Information tab",null,{"$f":"IF(OR('General Information'!$K$61=TRUE,'General Information'!$L$61=TRUE),TRUE,IF(J75=TRUE,TRUE,FALSE))","v":false},{"$f":"isbasehvac(1,5,7,8,11,12,13)","v":false}]
["G","The baseline chiller(s) quantity and type have been modeled as indicated in Table G3.1.3.7 per G3.1.3.7",null,null,null,null,"Required for Systems 7, 8, 11, 12 and 13\nNot required if District Cooling has been selected on the General Information tab",null,{"$f":"IF('General Information'!$K$61=TRUE,FALSE,IF(J76=TRUE,TRUE,FALSE))","v":false},{"$f":"isbasehvac(7,8,11,12,13)","v":false}]
["G","The baseline chilled water design supply temperature has been modeled as 44°F (6.7°C) with a return temperature of 56°F (13°C) per G3.1.3.8.",null,null,null,null,"Required for Systems 7, 8, 11, 12 and 13\nNot required if District Cooling has been selected on the General Information tab",null,{"$f":"IF('General Information'!$K$61=TRUE,FALSE,IF(J77=TRUE,TRUE,FALSE))","v":false},{"$f":"isbasehvac(7,8,11,12,13)","v":false}]
["G","The baseline chilled water supply temperature reset schedule has been modeled as 44°F (7°C) at outdoor temperatures 80°F (27°C) and above, 54°F (12°C) at outdoor temperatures 60°F (16°C) and below, and ramped linearly between 44°F (7°C) and 54°F (12°C) at outdoor temperatures between 80°F (27°C) and 60°F (16°C), except for System 11, which should be modeled with load reset, per G3.1.3.9.",null,null,null,null,"Required for Systems 7, 8, 11, 12 and 13\nNot required if District Cooling has been selected on the General Information tab",null,{"$f":"IF('General Information'!$K$61=TRUE,FALSE,IF(J78=TRUE,TRUE,FALSE))","v":false},{"$f":"isbasehvac(7,8,11,12,13)","v":false}]
["G","The baseline chilled water pump power has been modeled as 22 W/gpm (349 kW/1,000 L/s) per G3.1.3.10. Recommended that the pump power be split as one-third (primary) and two-thirds (secondary).",null,null,null,null,"Required for Systems 7, 8 and 11\nNot required if District Cooling has been selected on the General Information tab",null,{"$f":"IF('General Information'!$K$61=TRUE,FALSE,IF(J79=TRUE,TRUE,FALSE))","v":false},{"$f":"isbasehvac(7,8,11)","v":false}]
["G","The baseline cooling tower has been modeled with a variable-speed axial fan per G3.1.3.11 with fan power per Table 6.8.1G.",null,null,null,null,"Required for Systems 7, 8, 11, 12, and 13\nNot required if District Cooling has been selected on the General Information tab",null,{"$f":"IF('General Information'!$K$61=TRUE,FALSE,IF(J80=TRUE,TRUE,FALSE))","v":false},{"$f":"isbasehvac(7,8,11,12,13)","v":false}]
["G","The baseline condenser water design supply temperature shall be calculated using the cooling tower approach to the 0.4% evaporation design wet-bulb temperature as generated by the formula per G3.1.3.11, with a design temperature rise of 10°F. ",null,null,null,null,"Required for Systems 7, 8, 11, 12, and 13\nNot required if District Cooling has been selected on the General Information tab",null,{"$f":"IF('General Information'!$K$61=TRUE,FALSE,IF(J81=TRUE,TRUE,FALSE))","v":false},{"$f":"isbasehvac(7,8,11,12,13)","v":false}]
["G","The baseline condenser water temperature reset schedule has been modeled to maintain a 70°F (21°C) leaving water temperature where weather permits, floating up to a leaving water temperature at design conditions per G3.1.3.11.",null,null,null,null,"Required for Systems 7, 8, 11, 12, and 13\nNot required if District Cooling has been selected on the General Information tab",null,{"$f":"IF('General Information'!$K$61=TRUE,FALSE,IF(J82=TRUE,TRUE,FALSE))","v":false},{"$f":"isbasehvac(7,8,11,12,13)","v":false}]
["G","The baseline condenser water pump power has been modeled as 19 W/gpm (301 kW/1,000 L/s) per G3.1.3.11.",null,null,null,null,"Required for Systems 7, 8, 11, 12, and 13\nNot required if District Cooling has been selected on the General Information tab",null,{"$f":"IF('General Information'!$K$61=TRUE,FALSE,IF(J83=TRUE,TRUE,FALSE))","v":false},{"$f":"isbasehvac(7,8,11,12,13)","v":false}]
[null,"System 11 must be modeled with an integrated water-side economizer meeting the requirements of Section 6.5.1.2 in the baseline. If the simulation cannot model an integrated water-side economizer, then an air-side economizer shall be modeled.",null,null,null,null,"Required for System 11",null,{"$f":"IF('General Information'!$K$61=TRUE,FALSE,IF(J84=TRUE,TRUE,FALSE))","v":false},{"$f":"isbasehvac(11)","v":false}]
["G","The baseline condenser water pump power has been modeled as 19 W/gpm (301 kW/1,000 L/s) per G3.1.3.11.",null,null,null,null,"Required for Systems 7, 8, 11, 12, and 13\nNot required if District Cooling has been selected on the General Information tab",null,{"$f":"IF('General Information'!$K$61=TRUE,FALSE,IF(J85=TRUE,TRUE,FALSE))","v":false},{"$f":"isbasehvac(7,8,11,12,13)","v":false}]
["G"]
["G","For each item entered as “No” above, describe the applicable ASHRAE 90.1 Appendix G exception(s) that apply, or the circumstances preventing the HVAC parameters from being modeled as required, or for proposed parameters, details confirming that the proposed model appropriately represents the actual building design. If the energy simulation software is not capable of modeling the required parameters, describe the adjustments that were made to provide a thermodynamically similar representation of the system or provide a narrative justifying why the predicted energy performance results will not be influenced."]
["G"]

{"sheet":"10a - Baseline Air-Side HVAC","index":25,"n_rows":65,"n_cols":39,"rows_kept":65,"cut":false,"hidden":false,"merged":[[6,8,6,11],[34,6,62,6],[34,11,62,11],[34,38,62,38],[34,13,62,13],[34,12,62,12],[6,35,6,38],[9,8,9,10],[10,8,10,10],[11,8,11,10],[12,8,12,10],[9,35,9,37],[10,35,10,37],[11,35,11,37],[12,35,12,37],[8,36,8,37],[44,3,45,3],[36,3,37,3],[40,3,41,3],[42,3,43,3],[61,3,62,3],[56,3,57,3],[58,3,59,3],[46,3,47,3],[48,3,49,3],[50,3,51,3],[54,3,55,3],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[61,2,62,2],[36,2,37,2],[38,2,39,2],[56,2,57,2],[54,2,55,2],[50,2,51,2],[48,2,49,2],[34,2,35,2],[14,1,17,1],[13,1,13,2],[19,1,20,1],[18,1,18,2],[4,1,4,10],[8,9,8,10],[61,1,62,1],[58,2,59,2],[52,2,53,2],[29,3,33,3],[40,2,41,2],[42,2,43,2],[52,3,53,3],[38,3,39,3],[34,3,35,3],[27,1,28,1],[29,1,33,1],[34,1,60,1],[44,2,45,2],[46,2,47,2]]}
[]
[null,"Air-Side HVAC: Baseline"]
[]
[]
[null,"Instructions: Enter all applicable input parameters for the baseline air-side HVAC systems below. All systems included in the model should be entered. Each individual system may be entered separately, or multiple systems may be grouped together if all input parameters identified with an (*) are similar. The table is set up for two unique HVAC systems (or two groups of similar systems), and additional systems (or groups of similar systems) should be added as necessary using the Add Baseline button. For any information not applicable to the project, simply enter \"N/A\".  Note: All baseline systems must be identified in the General HVAC Tab in order to display the relevant baseline inputs below. If General HVAC system types are changed, system types must be reselected in this tab.\n\n"]
[]
[null,"Table 10.1: Air-Side HVAC System Schedule"]
[null,null,null,null,null,null,null,null,"Baseline",null,"units","BL_Units",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Baseline",null,"units","BL_Units"]
[null,"Model Input Parameter",null,{"$f":"'General Information'!C42&\" - Baseline System Helpful Notes\"","v":"ASHRAE 90.1 2016 Appendix G - Baseline System Helpful Notes"},null,null,"Total for Project",null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},null,null,null,null,null,null,null,"Additional Notes (Optional):",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"Baseline\"&\" - \"&'General Information'!$C$42","v":"Baseline - ASHRAE 90.1 2016 Appendix G"},{"$f":"\"Prescriptive Requirement of \"&'General Information'!$K$7&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Units"]
[null,"Building ID",null,"Applies to Projects wih multiple buildings, based on the General Information tab.",null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ10=\"\",\"\",AJ10&\" Prescriptive Requirement\")","v":""}]
[null,"* System type",null,"Select from baseline systems entered on the General HVAC tab.",null,null,"N/A",null,null,null,null,{"$f":"IF(I11=\"\",\"\",VLOOKUP(I11,'HVAC Lookup'!$H$10:$J$22,3,FALSE))","v":""},{"$f":"IF(J11=\"\",\"\",VLOOKUP(J11,'HVAC Lookup'!$H$10:$J$22,3,FALSE))","v":""},{"$f":"IF(#REF!=\"\",\"\",VLOOKUP(#REF!,'HVAC Lookup'!$H$10:$J$22,3,FALSE))","v":{"$error":"#REF!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ11=\"\",\"\",AJ11)","v":""},null,{"$f":"IF(AJ11=\"\",\"\",VLOOKUP(AJ11,'HVAC Lookup'!$H$10:$J$22,3,FALSE))","v":""}]
[null,"System designation(s)",null,"Enter designation for the system (or a group of systems) used in the model.",null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ12=\"\",\"\",AJ12)","v":""}]
[null,"Number of similar systems",null,"Systems that have the same parameters marked with (*) may be aggregated for reporting.",null,null,"N/A",null,null,null,null,{"$f":"IFERROR((IF(K14=\"kBtu/h\",I14,IF(K14=\"tons\",I14*DropdownData!$G$8,IF(K14=\"kW\",I14*DropdownData!$G$2,IF(K14=\"Btuh\",I14/1000))))),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ13=\"\",\"\",AJ13)","v":""},null,{"$f":"IFERROR((IF(AL14=\"kBtu/h\",AJ14,IF(AL14=\"tons\",AJ14*DropdownData!$G$8,IF(AL14=\"kW\",AJ14*DropdownData!$G$2,IF(AL14=\"Btuh\",AJ14/1000))))),\"\")","v":0}]
[null,"Total cooling capacity ",null,"Enter the modeled cooling capacity for the Baseline HVAC system (or the total cooling capacity for a group of similar systems) (example: 105 kBtu/h (30.7 kW))\n\nNote: Auto-sized with 15% oversizing per G3.1.2.2",{"$f":"SUMIF(H8:AI8,\"BL_Units\",H13:AI13)","v":0},null,{"$f":"TEXT(IFERROR((SUMIF($G$8:$JR$8,\"Baseline\", $G14:$JR14)),\"-\"),\"#,##0\")&\" kBtu/h\"","v":"0 kBtu/h"},null,null,{"$f":"IF(I14=\"\",\"\",I14)","v":""},"kBtu/h",{"$f":"IFERROR((IF(K14=\"kBtu/h\",I14*1000,IF(K14=\"tons\",I14*DropdownData!$G$8*1000,IF(K14=\"kW\",I14*DropdownData!$G$2*1000,IF(K14=\"Btuh\",I14)))))/I13,\"\")","v":""},{"$f":"IFERROR((IF(K14=\"kBtu/h\",I14*1000,IF(K14=\"tons\",I14*DropdownData!$G$8*1000,IF(K14=\"kW\",I14*DropdownData!$G$2*1000,IF(K14=\"Btuh\",I14)))))/I13,\"\")","v":""},{"$f":"IFERROR((IF(#REF!=\"kBtu/h\",#REF!*1000,IF(#REF!=\"tons\",#REF!*DropdownData!$G$8*1000,IF(#REF!=\"kW\",#REF!*DropdownData!$G$2*1000,IF(#REF!=\"Btuh\",#REF!)))))/#REF!,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ14=\"\",\"\",AJ14)","v":""},"kBtu/h",{"$f":"IFERROR((IF(AL14=\"kBtu/h\",AJ14*1000,IF(AL14=\"tons\",AJ14*DropdownData!$G$8*1000,IF(AL14=\"kW\",AJ14*DropdownData!$G$2*1000,IF(AL14=\"Btuh\",AJ14)))))/AJ13,\"\")","v":""}]
[null,"* Tables G3.5.1-G3.5.6 Unitary Cooling (Systems 1 through 6)","Tables G3.5.1-G3.5.6 unitary cooling capacity range","Enter the cooling capacity size category from the appropriate Tables G3.5.1-G3.5.6  for the Baseline HVAC system (or  group of similar systems) (example: 65-135 kBtu/h (19-39.5 kW))\n\nNote: \nSystems 1 & 2: Table G3.5.4\nSystems 3, 5, & 6: Table G3.5.1\nSystem 4: Table G3.5.2\nSystems 7-13: N/A",null,null,"N/A",null,null,{"$f":"IF(I15=\"\",\"\",I15)","v":""},"N/A",{"$f":"IF(L14<7000,7000,IF(L14>15000,15000,L14))","v":15000},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ15=\"\",\"\",AJ15)","v":""},"N/A",{"$f":"IF(AM14<7000,7000,IF(AM14>15000,15000,AM14))","v":15000}]
[null,null,"Unitary cooling efficiency ","Units should be consistent with the ASHRAE 90.1 minimum efficiency rating requirements for this system type",null,null,"N/A",null,{"$f":"IFERROR(IF(I11=\"System 1 - PTAC\",12.5-(0.213*(L15)/1000),IF(ISERROR(VLOOKUP(I11&I15,'HVAC Lookup'!$AC$9:$AD$30,2,FALSE))=TRUE,\"\",VLOOKUP(I11&I15,'HVAC Lookup'!$AC$9:$AD$30,2,FALSE))),\"-\")","v":""},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IFERROR(IF(AND('General Information'!$K$48=2013,J11=\"System 1 - PTAC\"),14-(0.3*(L15)/1000),IF(AND('General Information'!$K$48=2010,J11=\"System 1 - PTAC\"),13.8-(0.3*(L15)/1000),IF('General Information'!$K$48=2013,IF(ISERROR(VLOOKUP(J11&J15,'HVAC Lookup 90.1-2013'!$AC$9:$AD$30,2,FALSE))=TRUE,\"\",VLOOKUP(J11&J15,'HVAC Lookup 90.1-2013'!$AC$9:$AD$30,2,FALSE)),IF(ISERROR(VLOOKUP(J11&J15,'HVAC Lookup 90.1-2010'!$AC$9:$AD$30,2,FALSE))=TRUE,\"\",VLOOKUP(J11&J15,'HVAC Lookup 90.1-2010'!$AC$9:$AD$30,2,FALSE))))),\"-\"))","v":""},{"$f":"IF(I11=\"\",\"-\",IF(ISERROR(VLOOKUP(I11&I15,'HVAC Lookup'!$AC$8:$AG$30,3,FALSE))=TRUE,\"\",VLOOKUP(I11&I15,'HVAC Lookup'!$AC$8:$AG$30,3,FALSE)))","v":"-"},{"$f":"IFERROR(I17*L14*I13,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AJ11=\"System 1 - PTAC\",12.5-(0.213*(AM15)/1000),IF(ISERROR(VLOOKUP(AJ11&AJ15,'HVAC Lookup'!$AC$9:$AD$30,2,FALSE))=TRUE,\"\",VLOOKUP(AJ11&AJ15,'HVAC Lookup'!$AC$9:$AD$30,2,FALSE))),\"-\")","v":""},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IFERROR(IF(AND('General Information'!$K$48=2013,AK11=\"System 1 - PTAC\"),14-(0.3*(AM15)/1000),IF(AND('General Information'!$K$48=2010,AK11=\"System 1 - PTAC\"),13.8-(0.3*(AM15)/1000),IF('General Information'!$K$48=2013,IF(ISERROR(VLOOKUP(AK11&AK15,'HVAC Lookup 90.1-2013'!$AC$9:$AD$30,2,FALSE))=TRUE,\"\",VLOOKUP(AK11&AK15,'HVAC Lookup 90.1-2013'!$AC$9:$AD$30,2,FALSE)),IF(ISERROR(VLOOKUP(AK11&AK15,'HVAC Lookup 90.1-2010'!$AC$9:$AD$30,2,FALSE))=TRUE,\"\",VLOOKUP(AK11&AK15,'HVAC Lookup 90.1-2010'!$AC$9:$AD$30,2,FALSE))))),\"-\"))","v":""},{"$f":"IF(AJ11=\"\",\"-\",IF(ISERROR(VLOOKUP(AJ11&AJ15,'HVAC Lookup'!$AC$8:$AG$30,3,FALSE))=TRUE,\"\",VLOOKUP(AJ11&AJ15,'HVAC Lookup'!$AC$8:$AG$30,3,FALSE)))","v":"-"}]
[null,null,"COPnfcooling","Calculated COP",null,null,{"$f":"ROUND(SUMIF(I8:JR8,\"BL_Units\",I18:JR18),2)&\" COP\"","v":"0 COP"},null,{"$f":"IFERROR(IF(I16=\"\",\"\",IF(K16=\"COP\",I16,IF(K16=\"EER\",(0.0000000784)*I16*(I14/I13)+0.338*I16,(-0.0076*I16^2+0.3796*I16)))),\"-\")","v":""},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IFERROR(IF(J16=\"\",\"\",IF(K16=\"COP\",J16,IF(K16=\"EER\",(0.0000000784)*J16*(J14/J13)+0.338*J16,(-0.0076*J16^2+0.3796*J16)))),\"-\"))","v":""},"COP",{"$f":"IFERROR(I17,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AJ16=\"\",\"\",IF(AL16=\"COP\",AJ16,IF(AL16=\"EER\",(0.0000000784)*AJ16*(AJ14/AJ13)+0.338*AJ16,(-0.0076*AJ16^2+0.3796*AJ16)))),\"-\")","v":""},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IFERROR(IF(AK16=\"\",\"\",IF(AL16=\"COP\",AK16,IF(AL16=\"EER\",(0.0000000784)*AK16*(AK14/AK13)+0.338*AK16,(-0.0076*AK16^2+0.3796*AK16)))),\"-\"))","v":""},"COP"]
[null,null,"Unitary cooling part-load efficiency (if applicable) ","Enter the modeled unitary cooling efficiency for the Baseline HVAC system (or group of similar systems) in units consistent with the appropriate Table G3.5",{"$f":"INDEX($G18:$JR18,(MATCH(\"units\",$G$8:$JR$8,0)))","v":"-"},null,"N/A",null,{"$f":"IF(ISERROR(VLOOKUP(I11&I15,'HVAC Lookup'!$AC$8:$AF$30,4,FALSE))=TRUE,\"\",VLOOKUP(I11&I15,'HVAC Lookup'!$AC$8:$AF$30,4,FALSE))","v":""},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IF(ISERROR(VLOOKUP(J11&J15,'HVAC Lookup 90.1-2013'!$AC$8:$AG$30,4,FALSE))=TRUE,\"\",VLOOKUP(J11&J15,'HVAC Lookup 90.1-2013'!$AC$8:$AG$30,4,FALSE)),IF(ISERROR(VLOOKUP(J11&J15,'HVAC Lookup 90.1-2010'!$AC$8:$AG$30,4,FALSE))=TRUE,\"\",VLOOKUP(J11&J15,'HVAC Lookup 90.1-2010'!$AC$8:$AG$30,4,FALSE))))","v":""},{"$f":"IF(I11=\"\",\"-\",IF(ISERROR(VLOOKUP(I11&I15,'HVAC Lookup'!$AC$8:$AG$30,5,FALSE))=TRUE,\"\",VLOOKUP(I11&I15,'HVAC Lookup'!$AC$8:$AG$30,5,FALSE)))","v":"-"},{"$f":"IFERROR(I14*I17/$E$14,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(VLOOKUP(AJ11&AJ15,'HVAC Lookup'!$AC$8:$AF$30,4,FALSE))=TRUE,\"\",VLOOKUP(AJ11&AJ15,'HVAC Lookup'!$AC$8:$AF$30,4,FALSE))","v":""},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IF(ISERROR(VLOOKUP(AK11&AK15,'HVAC Lookup 90.1-2013'!$AC$8:$AG$30,4,FALSE))=TRUE,\"\",VLOOKUP(AK11&AK15,'HVAC Lookup 90.1-2013'!$AC$8:$AG$30,4,FALSE)),IF(ISERROR(VLOOKUP(AK11&AK15,'HVAC Lookup 90.1-2010'!$AC$8:$AG$30,4,FALSE))=TRUE,\"\",VLOOKUP(AK11&AK15,'HVAC Lookup 90.1-2010'!$AC$8:$AG$30,4,FALSE))))","v":""},{"$f":"IF(AJ11=\"\",\"-\",IF(ISERROR(VLOOKUP(AJ11&AJ15,'HVAC Lookup'!$AC$8:$AG$30,5,FALSE))=TRUE,\"\",VLOOKUP(AJ11&AJ15,'HVAC Lookup'!$AC$8:$AG$30,5,FALSE)))","v":"-"},{"$f":"IFERROR(AJ14*AJ17/$E$14,0)","v":0}]
[null,"Total heating capacity ",null,"Enter the modeled heating capacity for the Baseline HVAC system (or the total heating capacity for a group of similar systems) in units of kBtu/h (kW) \n\nNote: Auto-sized with 25% oversizing per G3.1.2.2",null,null,{"$f":"TEXT(IFERROR(SUMIF($G$8:$JR$8,\"BL_Units\", $G19:$JR19),\"-\"),\"#,##0\")&\" kBtu/h\"","v":"0 kBtu/h"},null,null,{"$f":"IF(I19=\"\",\"\",I19)","v":""},{"$f":"IF(SI_IP_Units=\"SI\",\"kW\",\"kBtu/h\")","v":"kBtu/h"},{"$f":"IFERROR(IF(K19=\"kBtu/h\",I19,IF(K19=\"tons\",I19*DropdownData!J13,IF(K19=\"kW\",I19*DropdownData!J7,IF(K19=\"Btuh\",I19/DropdownData!J11)))),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ19=\"\",\"\",AJ19)","v":""},{"$f":"IF(SI_IP_Units=\"SI\",\"kW\",\"kBtu/h\")","v":"kBtu/h"}]
[null,"* Tables G3.5.1-G3.5.6  Unitary Heating (Systems 2, 3, 4, and 9)","Tables G3.5.1-G3.5.6  unitary heating capacity range","•  System 2: Table G3.5.4\n•  Systems 3 & 9: Table G3.5.5\n•  System 4: Table  G3.5.2\n•  Systems 1, 5-8, 10-13: N/A  ",null,null,"N/A",null,null,{"$f":"IF(I20=\"\",\"\",I20)","v":""},"N/A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ20=\"\",\"\",AJ20)","v":""},"N/A"]
[null,null,"Unitary heating efficiency ","List all relevant efficiencies (e.g. 3.2 COP at 47°F db/43°F wb, 2.0 COP at 17°F db/15°F wb outdoor air) (e.g. 3.2 COP at 8.3°C db/6.1°C wb, 2.0 COP at -8.3°C db/-9.4°C wb outdoor air)",null,null,"N/A",null,{"$f":"IF(I20=\"N/A\",\"N/A\",IF(ISERROR(VLOOKUP(I11&I20,'HVAC Lookup'!$AC$33:$AD$58,2,FALSE))=TRUE,\"\",VLOOKUP(I11&I20,'HVAC Lookup'!$AC$33:$AD$58,2,FALSE)))","v":""},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(J20=\"N/A\",\"N/A\",IF('General Information'!$K$48=2013,IF(ISERROR(VLOOKUP(J11&J20,'HVAC Lookup 90.1-2013'!$AC$34:$AE$58,2,FALSE))=TRUE,\"\",VLOOKUP(J11&J20,'HVAC Lookup 90.1-2013'!$AC$34:$AE$58,2,FALSE)),IF(ISERROR(VLOOKUP(J11&J20,'HVAC Lookup 90.1-2010'!$AC$34:$AE$58,2,FALSE))=TRUE,\"\",VLOOKUP(J11&J20,'HVAC Lookup 90.1-2010'!$AC$34:$AE$58,2,FALSE)))))","v":""},{"$f":"IF(I11=\"\",\"-\",IF(I20=\"N/A\",\"N/A\",IF(ISERROR(VLOOKUP(I11&I20,'HVAC Lookup'!$AC$33:$AE$58,3,FALSE))=TRUE,\"\",VLOOKUP(I11&I20,'HVAC Lookup'!$AC$33:$AE$58,3,FALSE))))","v":"-"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ20=\"N/A\",\"N/A\",IF(ISERROR(VLOOKUP(AJ11&AJ20,'HVAC Lookup'!$AC$33:$AD$58,2,FALSE))=TRUE,\"\",VLOOKUP(AJ11&AJ20,'HVAC Lookup'!$AC$33:$AD$58,2,FALSE)))","v":""},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(AK20=\"N/A\",\"N/A\",IF('General Information'!$K$48=2013,IF(ISERROR(VLOOKUP(AK11&AK20,'HVAC Lookup 90.1-2013'!$AC$34:$AE$58,2,FALSE))=TRUE,\"\",VLOOKUP(AK11&AK20,'HVAC Lookup 90.1-2013'!$AC$34:$AE$58,2,FALSE)),IF(ISERROR(VLOOKUP(AK11&AK20,'HVAC Lookup 90.1-2010'!$AC$34:$AE$58,2,FALSE))=TRUE,\"\",VLOOKUP(AK11&AK20,'HVAC Lookup 90.1-2010'!$AC$34:$AE$58,2,FALSE)))))","v":""},{"$f":"IF(AJ11=\"\",\"-\",IF(AJ20=\"N/A\",\"N/A\",IF(ISERROR(VLOOKUP(AJ11&AJ20,'HVAC Lookup'!$AC$33:$AE$58,3,FALSE))=TRUE,\"\",VLOOKUP(AJ11&AJ20,'HVAC Lookup'!$AC$33:$AE$58,3,FALSE))))","v":"-"}]
[null,"* Fan control",null,"•  Systems 1-4, 9, 10, 12 & 13: Constant Volume\n•  Systems 5-8, 11: Variable Volume",null,null,"N/A",null,{"$f":"IF(L11=\"\",\"\",IF(OR(L11=1,L11=2,L11=3,L11=4,L11=9,L11=10,L11=12,L11=13),\"Constant Volume\",\"Variable Volume\"))","v":""},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",\"Based on 90.1 2013 Table 6.5.3.2.1\")","v":"Based on 90.1 2013 Table 6.5.3.2.1"},"N/A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AM11=\"\",\"\",IF(OR(AM11=1,AM11=2,AM11=3,AM11=4,AM11=9,AM11=10,AM11=12,AM11=13),\"Constant Volume\",\"Variable Volume\"))","v":""},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",\"Based on 90.1 2013 Table 6.5.3.2.1\")","v":"Based on 90.1 2013 Table 6.5.3.2.1"},"N/A"]
[null,"Supply airflow ",null,"•  Systems 1-8, 11-13: Auto-sized based on 20°F (11.1°C) ΔT\n•  Systems 9-10: Auto-sized based on 105°F (40.6°C) SAT",{"$f":"TEXT(SUMIF($G$8:$JR$8, \"Baseline\", $G23:$JR23),\"#,##0\")","v":"0"},null,{"$f":"TEXT(SUMIF($G$8:$JR$8, \"Baseline\", $G23:$JR23),\"#,##0\")&\" CFM\"","v":"0 CFM"},null,null,{"$f":"IF(I23=\"\",\"\",\"N/A\")","v":""},{"$f":"IF('General Information'!$K$11=\"IP\",\"CFM\",\"L/s\")","v":"CFM"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ23=\"\",\"\",\"N/A\")","v":""},{"$f":"IF('General Information'!$K$11=\"IP\",\"CFM\",\"L/s\")","v":"CFM"}]
[null,"Outdoor airflow",null,"•  If the minimum outdoor air in the proposed building is provided in excess of the amount required by the local code: code-minimum ventilation.\n•  All other cases: identical to Proposed",{"$f":"TEXT(SUMIF($G$8:$JR$8, \"Baseline\", $G24:$JR24),\"#,##0\")","v":"0"},null,{"$f":"TEXT(SUMIF($G$8:$JR$8, \"Baseline\", $G24:$JR24),\"#,##0\")&\" CFM\"","v":"0 CFM"},null,null,{"$f":"IF(I24=\"\",\"\",\"N/A\")","v":""},{"$f":"IF('General Information'!$K$11=\"IP\",\"CFM\",\"L/s\")","v":"CFM"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ24=\"\",\"\",\"N/A\")","v":""},{"$f":"IF('General Information'!$K$11=\"IP\",\"CFM\",\"L/s\")","v":"CFM"}]
[null,"Demand control ventilation",null,"If required by Section 6.4.3.8 (spaces >500 sq ft (50 m2) with ≥25 people/1,000 sq ft (100 m2)) ",null,null,"N/A",null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",\"Based on 90.1 2013 Section 6.4.3.8\")","v":"Based on 90.1 2013 Section 6.4.3.8"},"N/A",{"$f":"IF(I25=\"\",\"\",IF(I25=\"No\",0,1))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",\"Based on 90.1 2013 Section 6.4.3.8\")","v":"Based on 90.1 2013 Section 6.4.3.8"},"N/A"]
[null,"* Economizer high-limit shutoff ",null,"•  Systems 1, 2, 9 & 10: N/A\n•  Systems 3-8, 11, 12, 13: as required by Table G3.1.2.6 and G3.1.2.7 by Climate Zone:\n    • Not Required - 1a, 1b, 2a, 3a, 4a \n    • 75°F - 1b, 2b, 3b, 3c, 4b, 4c, 5b, 5c, 6b, 7b, 8\n    • 70°F - 5a, 6a, 7a",null,null,"N/A",null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",\"Based on 90.1 2013 Section 6.5.1\")","v":"Based on 90.1 2013 Section 6.5.1"},"°F",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",\"Based on 90.1 2013 Section 6.5.1\")","v":"Based on 90.1 2013 Section 6.5.1"}]
[null,"* Supply air temperature reset",null,"•  Systems 5-8: Supply air temperature reset of 5°F under minimum cooling load conditions per G3.1.3.12 (e.g. from 55 °F to 60 °F (12.7 °C to 15.6 °C))\n•  System 11: as required by G3.1.3.17\n•  All other systems: Not required",null,null,"N/A",null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",\"Based on 90.1 2013 Section 6.5.3.4\")","v":"Based on 90.1 2013 Section 6.5.3.4"},"N/A",{"$f":"IF(I27=\"Not Required\",0,1)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",\"Based on 90.1 2013 Section 6.5.3.4\")","v":"Based on 90.1 2013 Section 6.5.3.4"},"N/A"]
[null,"* Energy Recovery per G3.1.2.10","For Baseline, any individual systems where supply airflow rate exceeds value in Table 6.5.6.1 based on climate zone and percent outdoor air? For proposed, indicate if energy recovery is modeled.","•  Exhaust air energy recovery required for individual systems with a supply air capacity of 5000 CFM or greater and an outside air supply of 70% or greater, unless exceptions apply, per G3.1.2.10\n•  50% energy recovery effectiveness\n•  Bypass or control to permit economizer",null,null,"N/A",null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",\"Based on 90.1 2013 Section 6.5.6\")","v":"Based on 90.1 2013 Section 6.5.6"},"N/A",{"$f":"IF(I28=\"No\",0,1)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",\"Based on 90.1 2013 Section 6.5.6\")","v":"Based on 90.1 2013 Section 6.5.6"},"N/A"]
[null,null,"Exhaust air energy recovery effectiveness or G3.1.2.10 exception claimed","If energy recovery is modeled for the Baseline HVAC system, list the recovery effectiveness. If energy recovery is required but not modeled, list the exception from G3.1.2.10 used (example: not modeled per exception 2)",null,null,"N/A",null,{"$f":"IF(I28=\"Yes\",50%,\"N/A\")","v":"N/A"},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",\"Based on 90.1 2013 Section 6.5.6\")","v":"Based on 90.1 2013 Section 6.5.6"},"N/A",{"$f":"IF(I28=\"Yes\",0,1)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ28=\"Yes\",50%,\"N/A\")","v":"N/A"},{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",\"Based on 90.1 2013 Section 6.5.6\")","v":"Based on 90.1 2013 Section 6.5.6"},"N/A"]
[null,"Fan Power","Supply fan power","Report exhaust fans not interlocked with HVAC operation (such as parking garage ventilation fans, or unconditioned electrical room exhaust fans), and exhaust fans not required in the calculations (such as those applying Exception 6.5.3.1.1, or kitchen hoods operating independently of the building HVAC system) in \"Process Equipment\".\n\nThese values are calculated based on system type, any pressure adjustments listed below, the total supply volume, and the ASHRAE 90.1 fan motor efficiency associated with the fan motor power.\n\nNote: The sum of fan power for all supply, return, relief, and exhaust fans cannot exceed G3.1.2.9 system fan power allowance calculated using supply airflow.",{"$f":"F30/F33","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($G$8:$JR$8, \"Baseline\", $G30:$JR30)","v":0},{"$f":"SUMIF($G$8:$JR$8, \"Baseline\", $G30:$JR30)&\" kW\"","v":"0 kW"},null,null,{"$f":"IF(I30=\"\",\"\",I30)","v":""},"kW",{"$f":"I30/I33","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ30=\"\",\"\",AJ30)","v":""},"kW",{"$f":"AJ30/AJ33","v":{"$error":"#DIV/0!"}}]
[null,null,"Return or relief fan power ",null,{"$f":"F31/F33","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($G$8:$JR$8, \"Baseline\", $G31:$JR31)","v":0},{"$f":"SUMIF($G$8:$JR$8, \"Baseline\", $G31:$JR31)&\" kW\"","v":"0 kW"},null,null,"","kW",{"$f":"I31/I33","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","kW",{"$f":"AJ31/AJ33","v":{"$error":"#DIV/0!"}}]
[null,null,"Exhaust fan power",null,{"$f":"F32/F33","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($G$8:$JR$8, \"Baseline\", $G32:$JR32)","v":0},{"$f":"SUMIF($G$8:$JR$8, \"Baseline\", $G32:$JR32)&\" kW\"","v":"0 kW"},null,null,"","kW",{"$f":"I32/I33","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","kW",{"$f":"AJ32/AJ33","v":{"$error":"#DIV/0!"}}]
[null,null,"System fan power",null,null,{"$f":"SUMIF($G$8:$JR$8, \"Baseline\", $G33:$JR33)","v":0},{"$f":"SUMIF($G$8:$JR$8, \"Baseline\", $G33:$JR33)&\" kW\"","v":"0 kW"},null,{"$f":"SUM(I30:I32)","v":0},0,"kW",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AJ30:AJ32)","v":0},0,"kW"]
[null,null,"Allowed fan power",null,null,null,{"$f":"ROUND(SUMIF($G$8:$JR$8, \"Baseline\", $G34:$JR34),0)&\" kW\"","v":"0 kW"},null,{"$f":"IF(ISERROR(1/I$23),\"\",IF(VLOOKUP(I$11,Fanslookup,13,FALSE)=1,(IF(SI_IP_Units=\"SI\",VLOOKUP((VLOOKUP(I$11,Fanslookup,12,FALSE)*I$23+I$61),Motor_Horsepower_Nominal_Efficiency_SI,4,TRUE)*(VLOOKUP(I$11,Fanslookup,12,FALSE)*I$23+I$61),VLOOKUP((VLOOKUP(I$11,Fanslookup,11,FALSE)*I$23+I$61),Motor_Horsepower_Nominal_Efficiency_IP,5,TRUE)*(VLOOKUP(I$11,Fanslookup,11,FALSE)*I$23+I$61))),(IF(SI_IP_Units=\"IP\",VLOOKUP(I$11,Fanslookup,11,FALSE),VLOOKUP(I$11,Fanslookup,12,FALSE))*I$23+VLOOKUP(I$11,Fanslookup,15,FALSE)*I$62*I$63)))","v":""},"","kW",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISERROR(1/AJ$23),\"\",IF(VLOOKUP(AJ$11,Fanslookup,13,FALSE)=1,(IF(SI_IP_Units=\"SI\",VLOOKUP((VLOOKUP(AJ$11,Fanslookup,12,FALSE)*AJ$23+AJ$61),Motor_Horsepower_Nominal_Efficiency_SI,4,TRUE)*(VLOOKUP(AJ$11,Fanslookup,12,FALSE)*AJ$23+AJ$61),VLOOKUP((VLOOKUP(AJ$11,Fanslookup,11,FALSE)*AJ$23+AJ$61),Motor_Horsepower_Nominal_Efficiency_IP,5,TRUE)*(VLOOKUP(AJ$11,Fanslookup,11,FALSE)*AJ$23+AJ$61))),(IF(SI_IP_Units=\"IP\",VLOOKUP(AJ$11,Fanslookup,11,FALSE),VLOOKUP(AJ$11,Fanslookup,12,FALSE))*AJ$23+VLOOKUP(AJ$11,Fanslookup,15,FALSE)*AJ$62*AJ$63)))","v":""},"","kW"]
[null,"* Pressure Drop Adjustments (Systems 3 through 8); \n\n","Return or exhaust systems required by code or accreditation standards to be fully ducted, or systems required to maintain air pressure differentials between adjacent rooms.","Adjustment = 0.5 in. w.c. (125 Pa) (2.15  in. w.c. (535 Pa) for laboratory and vivarium systems)",null,null,"N/A",null,null,{"$f":"IF(I35=\"\",\"\",I35)","v":""},{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ35=\"\",\"\",AJ35)","v":""},{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(L$11=1,\"n/a\",IF(L$11=2,\"n/a\",\"\"))","v":""},{"$f":"IF(I36=\"\",\"\",I36)","v":""},{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."},null,null,null,{"$f":"IF('General Information'!$K$11=\"IP\",\"IP\",\"SI\")","v":"IP"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AM$11=1,\"n/a\",IF(AM$11=2,\"n/a\",\"\"))","v":""},{"$f":"IF(AJ36=\"\",\"\",AJ36)","v":""},{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."}]
[null,null,"Return and/or exhaust airflow control devices","Only where modulated to maintain relative negative or positive space pressure (e.g. lab, operating room)",null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"},null,null,null,{"$f":"IF($O$36=\"SI\",125,0.5)","v":0.5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(OR(L$11=1,L$11=2),\"n/a\",IF('General Information'!$K$11=\"IP\",\"0.5\",\"125\"))","v":"0.5"},"0.5",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."},null,null,null,{"$f":"IF($O$36=\"SI\",535,2.15)","v":2.15},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AM$11=1,AM$11=2),\"n/a\",IF('General Information'!$K$11=\"IP\",\"0.5\",\"125\"))","v":"0.5"},"0.5",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."}]
[null,null,"Exhaust filters, scrubbers, or other exhaust treatment","Adjustment = Pressure drop of device calculated at fan system design condition",null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(L$11=1,\"n/a\",IF(L$11=2,\"n/a\",\"\"))","v":""},"",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AM$11=1,\"n/a\",IF(AM$11=2,\"n/a\",\"\"))","v":""},"",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."}]
[null,null,"Particulate filtration credit: MERV 9 through 12","Adjustment = 0.5 in. w.c. (125 Pa)",null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(OR(L$11=1,L$11=2),\"n/a\",IF('General Information'!$K$11=\"IP\",\"0.5\",\"125\"))","v":"0.5"},"0.5",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AM$11=1,AM$11=2),\"n/a\",IF('General Information'!$K$11=\"IP\",\"0.5\",\"125\"))","v":"0.5"},"0.5",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."}]
[null,null,"Particulate filtration credit: MERV 13 through 15","Adjustment = 0.9 in. w.c. (225 Pa)",null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(OR(L$11=1,L$11=2),\"n/a\",IF('General Information'!$K$11=\"IP\",\"0.9\",\"225\"))","v":"0.9"},"0.9",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AM$11=1,AM$11=2),\"n/a\",IF('General Information'!$K$11=\"IP\",\"0.9\",\"225\"))","v":"0.9"},"0.9",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."}]
[null,null,"Particulate filtration credit: MERV 16 and greater and electronically enhanced filters","Adjustment = Pressure drop calculated at 2× clean filter pressure drop at fan system design condition",null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(L$11=1,\"n/a\",IF(L$11=2,\"n/a\",\"\"))","v":""},"",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AM$11=1,\"n/a\",IF(AM$11=2,\"n/a\",\"\"))","v":""},"",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."}]
[null,null,"Carbon and other gas-phase air cleaners","Adjustment = Clean filter pressure drop at fan system design condition",null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(L$11=1,\"n/a\",IF(L$11=2,\"n/a\",\"\"))","v":""},"",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AM$11=1,\"n/a\",IF(AM$11=2,\"n/a\",\"\"))","v":""},"",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."}]
[null,null,"Biosafety cabinet","Adjustment = Pressure drop of device at fan system design condition",null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(L$11=1,\"n/a\",IF(L$11=2,\"n/a\",\"\"))","v":""},"",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AM$11=1,\"n/a\",IF(AM$11=2,\"n/a\",\"\"))","v":""},"",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."}]
[null,null,"Energy recovery device","May only be claimed if required in the baseline per Table G3.1.2.9 footnote.\n\nAdjustment = For each airstream [(2.2 × 0.5)– 0.5] in. of water",null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(OR(L$11=1,L$11=2),\"n/a\",IF('General Information'!$K$11=\"IP\",\"1.2\",\"300\"))","v":"1.2"},"1.2",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AM$11=1,AM$11=2),\"n/a\",IF('General Information'!$K$11=\"IP\",\"1.2\",\"300\"))","v":"1.2"},"1.2",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."}]
[null,null,"Evaporative humidifier/cooler in series with another cooling coil","May only be claimed if required in the baseline.\n\nAdjustment = Clean filter pressure drop at fan system design condition",null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(L$11=1,\"n/a\",IF(L$11=2,\"n/a\",\"\"))","v":""},"",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AM$11=1,\"n/a\",IF(AM$11=2,\"n/a\",\"\"))","v":""},"",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."}]
[null,null,"Sound attenuation section","Adjustment = 0.15 in. w.c. (38 Pa)",null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(OR(L$11=1,L$11=2),\"n/a\",IF('General Information'!$K$11=\"IP\",\"0.15\",\"38\"))","v":"0.15"},"0.15",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AM$11=1,AM$11=2),\"n/a\",IF('General Information'!$K$11=\"IP\",\"0.15\",\"38\"))","v":"0.15"},"0.15",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."}]
[null,null,"Exhaust system serving fume hoods ","Adjustment = 0.35 in. w.c. (85 Pa)",null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(OR(L$11=1,L$11=2),\"n/a\",IF('General Information'!$K$11=\"IP\",\"0.35\",\"85\"))","v":"0.35"},"0.35",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(AM$11=1,AM$11=2),\"n/a\",IF('General Information'!$K$11=\"IP\",\"0.35\",\"85\"))","v":"0.35"},"0.35",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."}]
[null,null,"Laboratory and vivarium exhaust systems in high-rise buildings","Adjustment = 0.25 in. w.c./100 ft of vertical duct exceeding 75 ft (60 Pa/30 m of vertical duct exceeding 25 m)",null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"CFMD: cfm\",\"CFMD: L/s\")","v":"CFMD: cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF(L$11=1,\"n/a\",IF(L$11=2,\"n/a\",\"\"))","v":""},"",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AM$11=1,\"n/a\",IF(AM$11=2,\"n/a\",\"\"))","v":""},"",{"$f":"IF('General Information'!$K$11=\"IP\",\"Adjustment: in. w. c.\",\"Adjustment: Pa\")","v":"Adjustment: in. w. c."}]
[null,null,"Total Table 6.5.3.1-2 pressure drop adjustment (A)",null,null,null,null,null,{"$f":"IFERROR((IFERROR(I35*I36,\"0\")+IFERROR(I37*I38,\"0\")+IFERROR(I39*I40,\"0\")+IFERROR(I41*I42,\"0\")+IFERROR(I43*I44,\"0\")+IFERROR(I45*I46,\"0\")+IFERROR(I47*I48,\"0\")+IFERROR(I49*I50,\"0\")+IFERROR(I51*I52,\"0\")+IFERROR(I53*I54,\"0\")+IFERROR(I55*I56,\"0\")+IFERROR(I57*I58,\"0\")+IFERROR(I59*I60,\"0\"))/IF('General Information'!$K$11=\"IP\",4131,650000),\"-\")","v":0},0,{"$f":"IF('General Information'!$K$11=\"IP\",\"bhp\",\"kWi\")","v":"bhp"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR((IFERROR(AJ35*AJ36,\"0\")+IFERROR(AJ37*AJ38,\"0\")+IFERROR(AJ39*AJ40,\"0\")+IFERROR(AJ41*AJ42,\"0\")+IFERROR(AJ43*AJ44,\"0\")+IFERROR(AJ45*AJ46,\"0\")+IFERROR(AJ47*AJ48,\"0\")+IFERROR(AJ49*AJ50,\"0\")+IFERROR(AJ51*AJ52,\"0\")+IFERROR(AJ53*AJ54,\"0\")+IFERROR(AJ55*AJ56,\"0\")+IFERROR(AJ57*AJ58,\"0\")+IFERROR(AJ59*AJ60,\"0\"))/IF('General Information'!$K$11=\"IP\",4131,650000),\"-\")","v":0},0,{"$f":"IF('General Information'!$K$11=\"IP\",\"bhp\",\"kWi\")","v":"bhp"}]
[null,"Fan power adjustments (Systems 9 through 10)","Non-mechanical cooling fan - additional fan power allowance","For Systems 9 and 10, if present in the proposed design, increases the baseline fan power allowance by 0.054 Watts/cfm (0.025 Watts/L/s).",null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"cfm\",\"L/s\")","v":"cfm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"",{"$f":"IF('General Information'!$K$11=\"IP\",\"cfm\",\"L/s\")","v":"cfm"}]
[null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$11=\"IP\",\"0.000054\",\"0.000114\")","v":"0.000054"},null,{"$f":"\"fan power per \" & K62 & \" (kW)\"","v":"fan power per cfm (kW)"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$11=\"IP\",\"0.000054\",\"0.000114\")","v":"0.000054"},null,{"$f":"\"fan power per \" & AL62 & \" (kW)\"","v":"fan power per cfm (kW)"}]
[null,null,"Constant Volume System Fan Power (Total) kW",null,null,null,{"$f":"SUMIF($G$8:$KA$8, \"Baseline\", $G64:$KA64)","v":0},null,{"$f":"IF(I22=\"Constant Volume\",I33,0)","v":0},null,"kW",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ22=\"Constant Volume\",AJ33,0)","v":0}]
[null,null,"Variable Volume System Fan Power (Total) kW",null,null,null,{"$f":"SUMIF($G$8:$KA$8, \"Baseline\", $G65:$KA65)","v":0},null,{"$f":"IF(I22=\"Variable Volume\",I33,0)","v":0},null,"kW",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AJ22=\"Variable Volume\",AJ33,0)","v":0}]

{"sheet":"10b - Proposed Air-Side HVAC","index":26,"n_rows":35,"n_cols":45,"rows_kept":35,"cut":false,"hidden":false,"merged":[[27,40,27,41],[25,40,25,41],[26,40,26,41],[10,40,10,43],[11,40,11,43],[12,40,12,43],[20,40,20,41],[23,40,23,41],[29,2,31,2],[19,8,19,9],[20,8,20,9],[23,8,23,9],[24,8,24,9],[26,8,26,9],[27,8,27,9],[25,8,25,9],[6,40,6,44],[9,40,9,43],[8,40,8,41],[24,40,24,41],[19,40,19,41],[9,8,9,11],[10,8,10,11],[11,8,11,11],[12,8,12,11],[4,1,4,11],[8,8,8,9]]}
[]
[null,"Air-Side HVAC: Proposed"]
[]
[]
[null,"Instructions: Enter all applicable input parameters for the proposed air-side HVAC systems below. All systems included in the model should be entered. Each individual system may be entered separately, or multiple systems may be grouped together if all input parameters identified with an (*) are similar. The table is set up for two unique HVAC systems (or two groups of similar systems), and additional systems (or groups of similar systems) should be added as necessary using the Add Proposed button. For any information not applicable to the project, simply enter \"N/A\".  Note: All baseline systems must be identified in the General HVAC Tab in order to display the relevant baseline inputs below. If General HVAC system types are changed, system types must be reselected in this tab."]
[]
[null,"Table 10.1: Air-Side HVAC System Schedule"]
[null,null,null,null,null,null,null,null,"Proposed","units",null,null,"Prop_Units",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Proposed","units",null,null,"Prop_Units"]
[null,"Model Input Parameter",{"$f":"'General Information'!C42&\" - Proposed System Helpful Notes\"","v":"ASHRAE 90.1 2016 Appendix G - Proposed System Helpful Notes"},null,"Units","Total for Project",null,null,"Proposed System Description",null,"Plans / Specs","Measure #",null,null,null,null,null,"Additional Notes (Optional):",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Proposed System Description",null,"Plans / Specs","Measure #"]
[null,"Building ID","Applies to Projects wih multiple buildings, based on the General Information tab.",null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n/a"]
[null,"* System type","Select from proposed systems entered on the General HVAC tab.",null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n/a"]
[null,"System designation(s)","Enter designation for the system (or a group of systems) used in the model.",null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n/a"]
[null,"Number of similar systems","Systems that have the same parameters marked with (*) may be aggregated for reporting.",null,null,"N/A",null,null,null,null,null,null,{"$f":"IFERROR(IF(J14=\"kBtu/h\",I14,IF(J14=\"tons\",I14*DropdownData!$G$8,IF(J14=\"kW\",I14*DropdownData!$G$2,IF(J14=\"Btuh\",I14/1000)))),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n/a",null,null,{"$f":"IFERROR(IF(AP14=\"kBtu/h\",AO14,IF(AP14=\"tons\",AO14*DropdownData!$G$8,IF(AP14=\"kW\",AO14*DropdownData!$G$2,IF(AP14=\"Btuh\",AO14/1000)))),\"\")","v":0}]
[null,"Total cooling capacity ","Cooling capacity based on the design documents, or the total for a group of similar systems.",{"$f":"(IFERROR((SUMIF($F$8:$JS$8,\"Prop_Units\",$F13:$JS13)),\"-\"))","v":0},"kBtu/h",{"$f":"TEXT(ROUND(IFERROR((SUMIF($F$8:$JS$8,\"Proposed\", $F14:$JS14)),\"-\"),0),\"#,##0\")&\" kBtu/h\"","v":"0 kBtu/h"},{"$f":"D14","v":0},null,null,"kBtu/h",null,null,{"$f":"IFERROR(IF(J14=\"kBtu/h\",I14*1000,IF(J14=\"tons\",I14*DropdownData!$G$8*1000,IF(J14=\"kW\",I14*DropdownData!$G$2*1000,IF(J14=\"Btuh\",I14)))),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kBtu/h",null,null,{"$f":"IFERROR(IF(AP14=\"kBtu/h\",AO14*1000,IF(AP14=\"tons\",AO14*DropdownData!$G$8*1000,IF(AP14=\"kW\",AO14*DropdownData!$G$2*1000,IF(AP14=\"Btuh\",AO14)))),\"\")","v":0}]
[null,"Unitary cooling efficiency ","Should be consistent with efficiency units used in 90.1 Section 6 tables for this system type.",null,null,{"$f":"IFERROR(ROUND((SUMPRODUCT(--($G$8:S$8=\"Proposed\"),$G14:S14,$G15:S15))/(SUMIF($G$8:S$8, \"Proposed\", $G14:S14)),2)&\" EER\",\"N/A\")","v":"N/A"},null,null,null,"EER",null,null,{"$f":"IFERROR(I15*M14,\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EER",null,null,{"$f":"IFERROR(AO15*AS14,\"\")","v":0}]
[null,"COPnfcooling","Please remove the Supply Fan Energy form the COP using the below formulas:\n\nCOPnfcooling = [(Gross Cooling Btu/h)/((Total Input Power W - Indoor Fan Power W)*3.413 Btu/h*W)]\n\nIndoor Fan Power W = [(Gross Cooling Btu/h - Net Cooling Btu/h)/(3.413 Btu/h*W)]",null,null,{"$f":"IFERROR(ROUND((SUMPRODUCT(--($G$8:S$8=\"Proposed\"),$G14:S14,$G16:S16))/(SUMIF($G$8:S$8, \"Proposed\", $G14:S14)),2)&\" COP\",\"N/A\")","v":"N/A"},null,null,null,"COP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COP"]
[null,"Unitary cooling part-load efficiency (if applicable) ","Enter the spefied unitary cooling efficiency for the proposed HVAC system (or group of similar systems) at AHRI rating conditions.",null,null,"N/A",null,null,null,"IEER",null,null,{"$f":"I17","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IEER"]
[null,"Total heating capacity ","Enter the specified heating capacity for the proposed HVAC system, or the total heating capacity for a group of similar systems.",{"$f":"TEXT(ROUND(IFERROR(SUMIF($F$8:$JS$8,\"Prop_Units\", $F18:$JS18),\"-\"),0),\"#,##0\")","v":"0"},null,{"$f":"TEXT(ROUND(IFERROR(SUMIF($F$8:$JS$8,\"Prop_Units\", $F18:$JS18),\"-\"),0),\"#,##0\")&\" kBtu/h\"","v":"0 kBtu/h"},null,null,null,{"$f":"IF(SI_IP_Units=\"SI\",\"kW\",\"kBtu/h\")","v":"kBtu/h"},null,null,{"$f":"IFERROR(IF(J18=\"kBtu/h\",I18,IF(J18=\"tons\",I18*DropdownData!U13,IF(J18=\"kW\",I18*DropdownData!U7,IF(J18=\"Btuh\",I18/DropdownData!U11)))),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(SI_IP_Units=\"SI\",\"kW\",\"kBtu/h\")","v":"kBtu/h"},null,null,{"$f":"IFERROR(IF(AP18=\"kBtu/h\",AO18,IF(AP18=\"tons\",AO18*DropdownData!AU13,IF(AP18=\"kW\",AO18*DropdownData!AU7,IF(AP18=\"Btuh\",AO18/DropdownData!AU11)))),\"\")","v":0}]
[null,"Unitary heating efficiency ","List all relevant efficiencies (e.g. 3.2 COP at 47°F db/43°F wb, 2.0 COP at 17°F db/15°F wb outdoor air) (e.g. 3.2 COP at 8.3°C db/6.1°C wb, 2.0 COP at -8.3°C db/-9.4°C wb outdoor air).",null,null,"N/A",null,null,null,"COP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COP"]
[null,"* Fan control","Constant or Variable Volume",null,null,"N/A"]
[null,"* Fan operation during unoccupied hours","Systems that deliver ventilation air must run continuously when zones are occupied. ",null,null,"N/A"]
[null,"Supply airflow ","Design flow based on drawings.",{"$f":"TEXT(ROUND(SUMIF($F$8:$JS$8, \"Proposed\", $F22:$JS22),0),\"#,##0\")","v":"0"},null,{"$f":"TEXT(ROUND(SUMIF($F$8:$JS$8, \"Proposed\", $F22:$JS22),0),\"#,##0\")&\" \"&IF('General Information'!$K$11=\"IP\",\"CFM\",\"L/s\")","v":"0 CFM"},null,null,null,{"$f":"IF('General Information'!$K$11=\"IP\",\"CFM\",\"L/s\")","v":"CFM"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$11=\"IP\",\"CFM\",\"L/s\")","v":"CFM"}]
[null,"Outdoor airflow","Minimum outdoor flow rate, as specified.",{"$f":"TEXT(ROUND(SUMIF($F$8:$JS$8, \"Proposed\", $F23:$JS23),0),\"#,##0\")","v":"0"},null,{"$f":"TEXT(ROUND(SUMIF($F$8:$JS$8, \"Proposed\", $F23:$JS23),0),\"#,##0\")&\" \"&IF('General Information'!$K$11=\"IP\",\"CFM\",\"L/s\")","v":"0 CFM"},null,null,null,{"$f":"IF('General Information'!$K$11=\"IP\",\"CFM\",\"L/s\")","v":"CFM"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$11=\"IP\",\"CFM\",\"L/s\")","v":"CFM"}]
[null,"Demand control ventilation (DCV)","As specified. If DCV is required is Section 6.4.3.8, it must be specified because it is a mandatory requirement.",null,null,"N/A",null,null,null,null,null,null,{"$f":"IF(I24=\"\",\"\",IF(I24=\"No\",0,1))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AO24=\"\",\"\",IF(AO24=\"No\",0,1))","v":""}]
[null,"* Air-side Economizer type","Indicate the type of economizer specified.",null,null,"N/A"]
[null,"* Economizer high-limit shutoff ","Describe specified economizer controls.",null,null,"N/A"]
[null,"* Supply air temperature reset","Describe specified supply air temperature reset (if any). ",null,null,"N/A"]
[null,"Exhaust Air Energy Recovery ","Select specified system type.",null,null,"N/A",null,null,null,null,null,null,{"$f":"IF(I28=\"None\",0,1)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AO28=\"None\",0,1)","v":1}]
[null,"Recovery Effectiveness","Recovery effectiveness must be based on specified OA and exhaust flow through the recovery device, and the rated effectiveness of the specified device.",null,null,"N/A",null,null,null,"% energy recovery effectiveness",null,null,{"$f":"IF(I28=\"None\",1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"% energy recovery effectiveness",null,null,{"$f":"IF(AO28=\"None\",1,0)","v":0}]
[null,"Supply fan power","All fans that operate at design conditions to supply air from the heating or cooling\nsource to the conditioned spaces and return it to the source or exhaust it to the outdoors. In multifamily buildings this includes kitchen and bathroom exhaust fans.",{"$f":"E30/E33","v":{"$error":"#DIV/0!"}},{"$f":"ROUND(SUMIF($F$8:$JS$8, \"Proposed\", $F30:$JS30),0)","v":0},{"$f":"ROUND(SUMIF($F$8:$JS$8, \"Proposed\", $F30:$JS30),0)&\" kW\"","v":"0 kW"},null,null,null,"kW",null,null,{"$f":"I30/I33","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kW",null,null,{"$f":"AO30/AO33","v":{"$error":"#DIV/0!"}}]
[null,"Return or relief fan power ",null,{"$f":"E31/E33","v":{"$error":"#DIV/0!"}},{"$f":"ROUND(SUMIF($F$8:$JS$8, \"Proposed\", $F31:$JS31),1)","v":0},{"$f":"ROUND(SUMIF($F$8:$JS$8, \"Proposed\", $F31:$JS31),1)&\" kW\"","v":"0 kW"},null,null,null,"kW",null,null,{"$f":"I31/I33","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kW",null,null,{"$f":"AO31/AO33","v":{"$error":"#DIV/0!"}}]
[null,"Exhaust fan power",null,{"$f":"E32/E33","v":{"$error":"#DIV/0!"}},{"$f":"ROUND(SUMIF($F$8:$JS$8, \"Proposed\", $F32:$JS32),1)","v":0},{"$f":"ROUND(SUMIF($F$8:$JS$8, \"Proposed\", $F32:$JS32),1)&\" kW\"","v":"0 kW"},null,null,null,"kW",null,null,{"$f":"I32/I33","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kW",null,null,{"$f":"AO32/AO33","v":{"$error":"#DIV/0!"}}]
[null,"System fan power","Auto-calculated to include all fans",{"$f":"ROUND(SUMIF($F$8:$JS$8, \"Proposed\", $F33:$JS33),0)","v":0},{"$f":"ROUND(SUMIF($F$8:$JS$8, \"Proposed\", $F33:$JS33),0)","v":0},{"$f":"ROUND(SUMIF($F$8:$JS$8, \"Proposed\", $F33:$JS33),0)&\" kW\"","v":"0 kW"},null,null,{"$f":"SUM(I30:I32)","v":0},"kW",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AO30:AO32)","v":0},"kW"]
[null,null,null,null,"kW",{"$f":"SUMIF($F$8:$JS$8, \"Proposed\", $F34:$JS34)","v":0},null,null,{"$f":"IF(I20=\"Constant Volume\",I33,0)","v":0},"kW",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AO20=\"Constant Volume\",AO33,0)","v":0}]
[null,null,null,null,"kW",{"$f":"SUMIF($F$8:$JS$8, \"Proposed\", $F35:$JS35)","v":0},null,null,{"$f":"IF(I20=\"Variable Volume\",I33,0)","v":0},"kW",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AO20=\"Variable Volume\",AO33,0)","v":0}]

{"sheet":"11 - Water-Side HVAC","index":27,"n_rows":107,"n_cols":27,"rows_kept":107,"cut":false,"hidden":false,"merged":[[85,8,85,10],[8,12,9,12],[8,13,9,13],[99,12,100,12],[99,13,100,13],[67,12,68,12],[67,13,68,13],[99,8,99,10],[8,16,9,16],[100,1,100,2],[32,5,32,7],[32,12,33,12],[32,13,33,13],[46,5,46,7],[46,12,47,12],[46,13,47,13],[67,5,67,7],[85,5,85,7],[85,12,86,12],[85,13,86,13],[8,8,8,10],[32,8,32,10],[46,8,46,10],[67,8,67,10],[101,1,101,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[4,1,4,6],[8,5,8,7],[102,1,102,2],[103,1,103,2],[99,5,99,7]]}
[]
[null,"Water-Side HVAC"]
[]
[]
[null,"Instructions: Enter all applicable input parameters for the baseline and proposed water-side HVAC systems below. All systems included in the model should be entered. Please refer to the row header notes for information about Appendix G modeling protocol. For any information not applicable to the project, simply enter \"N/A\". If taking credit for a campus or district plant efficiency using the DES Path 2 or 3 Guidance, please include all relevant information regarding the District Plant equipment in the proposed Case."]
[]
[null,"Water-Side HVAC System Schedule"]
[]
[null,"Table 11.1: Chilled Water",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,"Proposed Design",null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #",null,null,"Additional Notes (Optional):"]
[null,"Model Input Parameter",{"$f":"CodeUsed&\" - Baseline Systems Helpful Notes\"","v":"ASHRAE 90.1 2016 Appendix G - Baseline Systems Helpful Notes"},null,"Units",null,{"$f":"'1 - Multiple Buildings Details'!B24","v":0},null,null,"MPP BM HW Heat CZ 4A MPP","Plans / Specs"]
[null,"Number and type of chillers (and capacity per chiller if more than one type or size of chiller)","•  ≤300 tons (≤1055 kW) building peak: 1 water-cooled screw chiller\n•  300-600 tons (1055 - 2110 kW) building peak: 2 equally-sized water-cooled  screw chillers\n•  ≥600 tons (>2110 kW) building peak: At least 2 water-cooled centrifugal chillers (800 tons max per chiller) \n\nNote: Overwrite entry if more than 2 water-cooled centrifugal chillers, or N/A if purchased chilled water is modeled.",null,"n/a",null,{"$f":"IF(G13=\"\",\"\",IF(G13<=300,1,IF(G13<600,2,MAX(2,TRUNC((G13-1)/800,0)+1))))&IF(G13=\"\",\"\",IF(G13<600,\" water-cooled screw\",\" water-cooled centrifugal\"))","v":""},null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(M13=\"\",\"\",IF(M13<=300,1,IF(M13<600,2,MAX(2,TRUNC((M13-1)/800,0)+1))))&IF(M13=\"\",\"\",IF(M13<600,\" water-cooled screw\",\" water-cooled centrifugal\")))","v":""},null,null,null,null,null,"Chilled Water",{"$f":"N11","v":0},{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},null,null,null,{"$f":"SUM(X:X)","v":0},"Total Pump kW Baseline"]
[null,"Purchased chilled water rate (cost per unit energy)","Describe how the purchased chilled water rate was determined. Local purchased energy rates must be used when available; when not available, the rates must account for the total costs associated with maintaining the district equipment, and generating and delivering the energy to the project site.",null,"$",null,null,null,null,null,null,null,{"$f":"IF(G12=\"\",\"\",G12)","v":""},null,null,null,null,null,"Chilled Water",{"$f":"N12","v":0},{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},null,null,null,{"$f":"SUM(Y:Y)","v":0},"Total Pump kW Proposed"]
[null,"Total chiller capacity","Auto-sized with 15% oversizing (unless oversized at the system coil) per G3.1.2.2",null,"tons",null,null,null,null,null,null,null,{"$f":"IF(G13=\"\",\"\",G13)","v":""},null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"Chiller efficiency - full load","Per Table G3.5.3 efficiencies",null,"FL kW/Ton",null,{"$f":"IFERROR(IF(G13=\"\",\"\",IF(G13<150,0.79,IF(G13<600,0.718,IF(G13/LEFT(G11,1)<600,0.634,0.576)))),\"\")","v":""},null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(M13=\"\",\"\",IF(M13<75,0.75,IF(M13<150,0.72,IF(M13<300,0.66,IF(OR(M13>600,M13=600),0.56,0.61))))),\"\"),IFERROR(IF(M13=\"\",\"\",IF(M13<75,0.78,IF(M13<150,0.775,IF(M13<300,0.68,IF(OR(M13>300,M13=300),0.57,0.576))))),\"\")))","v":""},null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"Chiller efficiency - part load","Per Table G3.5.3  efficiencies",null,"IPLV (kW/Ton)",null,{"$f":"IFERROR(IF(G13=\"\",\"\",IF(G13<150,0.676,IF(G13<600,0.629,IF(G13/LEFT(G11,1)<600,0.596,0.549)))),\"\")","v":""},null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(M13=\"\",\"\",IF(M13<75,0.6,IF(M13<150,0.56,IF(M13<300,0.54,IF(OR(M13>600,M13=600),0.5,0.52))))),\"\"),IFERROR(IF(M13=\"\",\"\",IF(M13<75,0.63,IF(M13<150,0.615,IF(M13<300,0.58,IF(OR(M13>300,M13=300),0.54,0.58))))),\"\")))","v":""},null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"Chilled water (CHW) supply temp","•  44°F (6.7°C) per G3.1.3.8\n•  ASHRAE 90.1 (DES Path 1): Baseline supply temperature based on actual chilled water loop conditions in Proposed Case.",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"°F\",\"°C\")","v":"°F"},null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"CHW ΔT","•  12°F (6.3°C) per  G3.1.3.8\n•  ASHRAE 90.1 (DES Path 1): CHW ΔT  based on actual chilled water loop conditions in Proposed Case.",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"°F\",\"°C\")","v":"°F"},null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"CHW supply temp reset parameters","•  44°F (7°C) at outdoor temps 80°F (27°C) and above, 54°F (12°C) at outdoor temps 60°F (16°C) and below, and ramped linearly between 44°F (7°C) and 54°F (12°C) at outdoor temps between 80°F (27°C) and 60°F (16°C) per G3.1.3.9\n•  For CHW loops serving System, 11, load reset up to 54°F per G3.1.3.9\n•  ASHRAE 90.1 (DES Path 1): CHW Temp Reset based on actual CHW loop conditions in Proposed Case.",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"CHW loop configuration","•  Primary/secondary per G3.1.3.10\n•  ASHRAE 90.1 (DES Path 1) or Streamlined DES (DES Path 3): only building distribution pumps shall be modeled, in which case pump controls shall match the Baseline secondary CHW pump control requirements.",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"Number of primary or DES plant CHW pumps","•  1 per chiller per G3.1.3.11\n•  ASHRAE 90.1 (DES Path 1) or Streamlined DES (DES Path 3): no primary  CHW pumps should be modeled (since these are considered part of the upstream source)",null,"#",null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"Primary or DES plant CHW total pump power","•  The sum of primary and secondary must be 22 W/gpm (349 kW/1000 L/s) per G3.1.3.10. Recommended that the pump power be split as one-third (primary) and two-thirds (secondary).\n•  ASHRAE 90.1 (DES Path 1) or Streamlined DES (DES Path 3): Not applicable",null,"kW",null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},null,{"$f":"IF(E21=\"kW\",G21,\"\")","v":0},{"$f":"IF(E21=\"kW\",J21,\"\")","v":0}]
[null,"Primary or DES plant CHW pump flow","Auto-sized with a capacity ratio of 1.0 based on CHW temperatures",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"gpm\",\"L/s\")","v":"gpm"},null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"Primary or DES plant CHW pump control","Constant Flow - each primary pump interlocked to operate with associated chiller - G3.1.3.10, G3.1.3.11",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"Number of secondary or building booster CHW pumps","•  1 per G3.1.3.10\n•  ASHRAE 90.1 (DES Path 1) or Streamlined DES (DES Path 3): one on-site CHW distribution pump shall only be modeled if CHW distribution pumps are present on site (these would otherwise be considered part of the upstream source) (per G3.1.1.3.4)",null,"#",null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"Secondary or building booster CHW total pump power","•  The sum of primary and secondary must be 22 W/gpm (349 kW/1000 L/s) per G3.1.3.10. Recommended that the pump power be split as one-third (primary) and two-thirds (secondary).\n•  ASHRAE 90.1 (DES Path 1): 16 W/gpm (254 kW/1000 L/s) per exception to G3.1.3.10\n•  California Title 24 (DES Path 4): Same W/gpm (kW/1000 L/s) as Proposed or 22 W/gpm (349 kW/1000 L/s)",null,"kW",null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},null,{"$f":"IF(E25=\"kW\",G25,\"\")","v":0},{"$f":"IF(E25=\"kW\",J25,\"\")","v":0}]
[null,"Secondary or building booster CHW pump flow","Auto-sized with a capacity ratio of 1.0 based on CHW temperatures",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"gpm\",\"L/s\")","v":"gpm"},null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"Secondary or building booster CHW pump control","•  <300 tons (1055kW): riding the pump curve\n•  ≥300 tons (1055 kW): variable speed",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"Water-side economizer ","Not required",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,"Water-side energy recovery","Not required",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water",0,{"$f":"G11&\" chiller(s) with capacity of \"&G13&\" \"&E13&\" and efficiency of \"&G14&\" \"&E14&\" and \"&G15&\" \"&E15&\". This is a \"&G19&\" CHW loop configuration with \"&G20&\" CHW pumps with pump power of \"&G21&\" \"&E21&\" and pump flow of \"&G22&\" gpm with \"&G23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"J11&\" chiller(s) with capacity of \"&J13&\" \"&E13&\" and efficiency of \"&J14&\" \"&E14&\" and \"&J15&\" \"&E15&\". This is a \"&J19&\" CHW loop configuration with \"&J20&\" CHW pumps with pump power of \"&J21&\" \"&E21&\" and pump flow of \"&J22&\" gpm with \"&J23&\", pump control.\"","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[]
[]
[]
[null,"Table 11.2: Cooling Tower and Condenser Water",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,"Proposed Design",null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
[null,"Model Input Parameter",{"$f":"$C$10","v":"ASHRAE 90.1 2016 Appendix G - Baseline Systems Helpful Notes"},null,"Units",null,{"$f":"G10","v":0},null,null,"Project","Plans / Specs"]
[null,"Number of cooling towers or fluid coolers","1 per G3.1.3.11",null,"#",null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling Tower and Condenser Water",{"$f":"N35","v":0},{"$f":"G35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&G36&\" \"&E36&\" and \"&G37&\" control. The CW leaving temperature is \"&G38&\" (F) with a CW dela T of \"&G39&\" (F) and reset parameters include: \"&G40&\". There are \"&G41&\" CW pump with pump power of \"&G42&\" \"&E42&\", pump flow of \"&G43&\" gpm and \"&G44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"J35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&J36&\" \"&E36&\" and \"&J37&\" control. The CW leaving temperature is \"&J38&\" (F) with a CW dela T of \"&J39&\" (F) and reset parameters include: \"&J40&\". There are \"&J41&\" CW pump with pump power of \"&J42&\" \"&E42&\", pump flow of \"&J43&\" gpm and \"&J44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,"Cooling tower fan power","Minimum 38.2 gpm/hp (3.23 L/s·kW) (maximum 0.0262 hp/gpm or 19.5 W/gpm) (0.301 kW/L/s)  per G3.1.3.11",null,"kW",null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling Tower and Condenser Water",{"$f":"N36","v":0},{"$f":"G35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&G36&\" \"&E36&\" and \"&G37&\" control. The CW leaving temperature is \"&G38&\" (F) with a CW dela T of \"&G39&\" (F) and reset parameters include: \"&G40&\". There are \"&G41&\" CW pump with pump power of \"&G42&\" \"&E42&\", pump flow of \"&G43&\" gpm and \"&G44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"J35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&J36&\" \"&E36&\" and \"&J37&\" control. The CW leaving temperature is \"&J38&\" (F) with a CW dela T of \"&J39&\" (F) and reset parameters include: \"&J40&\". There are \"&J41&\" CW pump with pump power of \"&J42&\" \"&E42&\", pump flow of \"&J43&\" gpm and \"&J44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,"Cooling tower fan control","Variable-speed axial fans per G3.1.3.11",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling Tower and Condenser Water",0,{"$f":"G35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&G36&\" \"&E36&\" and \"&G37&\" control. The CW leaving temperature is \"&G38&\" (F) with a CW dela T of \"&G39&\" (F) and reset parameters include: \"&G40&\". There are \"&G41&\" CW pump with pump power of \"&G42&\" \"&E42&\", pump flow of \"&G43&\" gpm and \"&G44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"J35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&J36&\" \"&E36&\" and \"&J37&\" control. The CW leaving temperature is \"&J38&\" (F) with a CW dela T of \"&J39&\" (F) and reset parameters include: \"&J40&\". There are \"&J41&\" CW pump with pump power of \"&J42&\" \"&E42&\", pump flow of \"&J43&\" gpm and \"&J44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,"Condenser water (CW) leaving temp","Calculated using the cooling tower approach to the 0.4% evaporation design wet-bulb temperature as generated by the formula per G3.1.3.11.",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"°F\",\"°C\")","v":"°F"},null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling Tower and Condenser Water",0,{"$f":"G35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&G36&\" \"&E36&\" and \"&G37&\" control. The CW leaving temperature is \"&G38&\" (F) with a CW dela T of \"&G39&\" (F) and reset parameters include: \"&G40&\". There are \"&G41&\" CW pump with pump power of \"&G42&\" \"&E42&\", pump flow of \"&G43&\" gpm and \"&G44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"J35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&J36&\" \"&E36&\" and \"&J37&\" control. The CW leaving temperature is \"&J38&\" (F) with a CW dela T of \"&J39&\" (F) and reset parameters include: \"&J40&\". There are \"&J41&\" CW pump with pump power of \"&J42&\" \"&E42&\", pump flow of \"&J43&\" gpm and \"&J44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,"CW ΔT","10°F (5.6°) per G3.1.3.11",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"°F\",\"°C\")","v":"°F"},null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling Tower and Condenser Water",0,{"$f":"G35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&G36&\" \"&E36&\" and \"&G37&\" control. The CW leaving temperature is \"&G38&\" (F) with a CW dela T of \"&G39&\" (F) and reset parameters include: \"&G40&\". There are \"&G41&\" CW pump with pump power of \"&G42&\" \"&E42&\", pump flow of \"&G43&\" gpm and \"&G44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"J35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&J36&\" \"&E36&\" and \"&J37&\" control. The CW leaving temperature is \"&J38&\" (F) with a CW dela T of \"&J39&\" (F) and reset parameters include: \"&J40&\". There are \"&J41&\" CW pump with pump power of \"&J42&\" \"&E42&\", pump flow of \"&J43&\" gpm and \"&J44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,"CW loop temp reset parameters","Maintain a 70°F (21°C) leaving water temperature where weather permits, floating up to leaving water temperature at design conditions per G3.1.3.11",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling Tower and Condenser Water",0,{"$f":"G35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&G36&\" \"&E36&\" and \"&G37&\" control. The CW leaving temperature is \"&G38&\" (F) with a CW dela T of \"&G39&\" (F) and reset parameters include: \"&G40&\". There are \"&G41&\" CW pump with pump power of \"&G42&\" \"&E42&\", pump flow of \"&G43&\" gpm and \"&G44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"J35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&J36&\" \"&E36&\" and \"&J37&\" control. The CW leaving temperature is \"&J38&\" (F) with a CW dela T of \"&J39&\" (F) and reset parameters include: \"&J40&\". There are \"&J41&\" CW pump with pump power of \"&J42&\" \"&E42&\", pump flow of \"&J43&\" gpm and \"&J44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,"Number of CW pumps","1 per chiller per G3.1.3.11",null,"#",null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling Tower and Condenser Water",0,{"$f":"G35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&G36&\" \"&E36&\" and \"&G37&\" control. The CW leaving temperature is \"&G38&\" (F) with a CW dela T of \"&G39&\" (F) and reset parameters include: \"&G40&\". There are \"&G41&\" CW pump with pump power of \"&G42&\" \"&E42&\", pump flow of \"&G43&\" gpm and \"&G44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"J35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&J36&\" \"&E36&\" and \"&J37&\" control. The CW leaving temperature is \"&J38&\" (F) with a CW dela T of \"&J39&\" (F) and reset parameters include: \"&J40&\". There are \"&J41&\" CW pump with pump power of \"&J42&\" \"&E42&\", pump flow of \"&J43&\" gpm and \"&J44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,"CW total pump power","19 W/gpm (310 kW/1000 L/s) per G3.1.3.11",null,"kW",null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling Tower and Condenser Water",0,{"$f":"G35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&G36&\" \"&E36&\" and \"&G37&\" control. The CW leaving temperature is \"&G38&\" (F) with a CW dela T of \"&G39&\" (F) and reset parameters include: \"&G40&\". There are \"&G41&\" CW pump with pump power of \"&G42&\" \"&E42&\", pump flow of \"&G43&\" gpm and \"&G44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"J35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&J36&\" \"&E36&\" and \"&J37&\" control. The CW leaving temperature is \"&J38&\" (F) with a CW dela T of \"&J39&\" (F) and reset parameters include: \"&J40&\". There are \"&J41&\" CW pump with pump power of \"&J42&\" \"&E42&\", pump flow of \"&J43&\" gpm and \"&J44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},null,{"$f":"IF(E42=\"kW\",G42,\"\")","v":0},{"$f":"IF(E42=\"kW\",J42,\"\")","v":0}]
[null,"CW pump flow","Auto-sized with a capacity ratio of 1.0 based on CW temperatures",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"gpm\",\"L/s\")","v":"gpm"},null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling Tower and Condenser Water",0,{"$f":"G35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&G36&\" \"&E36&\" and \"&G37&\" control. The CW leaving temperature is \"&G38&\" (F) with a CW dela T of \"&G39&\" (F) and reset parameters include: \"&G40&\". There are \"&G41&\" CW pump with pump power of \"&G42&\" \"&E42&\", pump flow of \"&G43&\" gpm and \"&G44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"J35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&J36&\" \"&E36&\" and \"&J37&\" control. The CW leaving temperature is \"&J38&\" (F) with a CW dela T of \"&J39&\" (F) and reset parameters include: \"&J40&\". There are \"&J41&\" CW pump with pump power of \"&J42&\" \"&E42&\", pump flow of \"&J43&\" gpm and \"&J44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,"CW pump control","Riding the pump curve per G3.1.3.11",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling Tower and Condenser Water",0,{"$f":"G35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&G36&\" \"&E36&\" and \"&G37&\" control. The CW leaving temperature is \"&G38&\" (F) with a CW dela T of \"&G39&\" (F) and reset parameters include: \"&G40&\". There are \"&G41&\" CW pump with pump power of \"&G42&\" \"&E42&\", pump flow of \"&G43&\" gpm and \"&G44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"J35&\" Cooling tower(s), or fluid cooler(s), with fan power of \"&J36&\" \"&E36&\" and \"&J37&\" control. The CW leaving temperature is \"&J38&\" (F) with a CW dela T of \"&J39&\" (F) and reset parameters include: \"&J40&\". There are \"&J41&\" CW pump with pump power of \"&J42&\" \"&E42&\", pump flow of \"&J43&\" gpm and \"&J44&\" control.\"","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[]
[]
[null,"Table 11.3: Hot Water or Steam",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,"Proposed Design",null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
[null,"Model Input Parameter",{"$f":"$C$10","v":"ASHRAE 90.1 2016 Appendix G - Baseline Systems Helpful Notes"},null,"Units",null,{"$f":"G10","v":0},null,null,"MPP BM HW Heat CZ 4A MPP","Plans / Specs"]
[null,"Number and type of boilers","•  ≤15,000 sq ft (1400 m2): 1 natural draft hot water boiler\n•  >15,000 sq ft (1400 m2): 2 equally-sized natural draft hot water boilers staged as required by the load",null,"n/a",null,null,null,null,null,null,null,{"$f":"IF(G49=\"\",\"\",G49)","v":""},null,null,null,null,null,"Hot Water or Steam",{"$f":"N49","v":0},{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"Purchased heating rate (cost per unit energy)","Describe how the purchased heating rate was determined. Local purchased energy rates must be used when available; when not available, the rates must account for the total costs associated with maintaining the district equipment, and generating and delivering the energy to the project site.",null,"$",null,null,null,null,null,null,null,{"$f":"IF(G50=\"\",\"\",G50)","v":""},null,null,null,null,null,"Hot Water or Steam",{"$f":"N50","v":0},{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"Total boiler capacity","Auto-sized with 25% oversizing (unless oversized at the system coil) per G3.1.2.2",null,"MBH",null,null,null,null,null,null,null,{"$f":"IF(G51=\"\",\"\",G51)","v":""},null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"Boiler efficiency","Per Table G3.5.6 minimum efficiencies",null,"%",null,{"$f":"IFERROR(IF(G51=\"\",\"\",IF(G51/LEFT(G49,1)<300,\"80% AFUE\",IF(G51/LEFT(G49,1)<=2500,\"75% Et\",\"80% Ec\"))),\"\")","v":""},null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF('General Information'!$K$48=2013,IFERROR(IF(M51=\"\",\"\",IF(M51/LEFT(M49,1)<300,\"82% AFUE\",IF(M51/LEFT(M49,1)<=2500,\"80% Et\",\"82% Ec\"))),\"\"),IFERROR(IF(M51=\"\",\"\",IF(M51/LEFT(M49,1)<300,\"80% AFUE\",IF(M51/LEFT(M49,1)<=2500,\"80% Et\",\"82% Ec\"))),\"\")))","v":""},null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"Hot water or steam (HHW) supply temp","•  180°F (82°C) per G3.1.3.3\n•  ASHRAE 90.1 (DES Path 1) or Full DES (DES Path 2): Purchased Energy - Baseline supply temperature based on actual HHW/Steam loop conditions in Proposed Case",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"°F\",\"°C\")","v":"°F"},null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(G53=\"\",\"\",IF('General Information'!$K$11=\"IP\",\"180°F\",\"82.2°C\")))","v":""},null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"HHW ΔT","•  50°F (28°C) per G3.1.3.3\n•  ASHRAE 90.1 (DES Path 1): Baseline ΔT based on actual HHW/Steam loop conditions in Proposed Case",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"°F\",\"°C\")","v":"°F"},null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(G54=\"\",\"\",IF('General Information'!$K$11=\"IP\",\"50°F\",\"27.8°C\")))","v":""},null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"HHW temp reset parameters","•  180°F (83°C) at outdoor temps 20°F (-7°C) and below, 150°F (66°C) at outdoor temps 50°F (10°C) and above, and ramped linearly between 180°F (83°C) and 150°F (66°C) at outdoor temps between 20°F(-7°C) and 50°F (10°C) per G3.1.3.4\n•  ASHRAE 90.1 (DES Path 1): Baseline Temp Reset based on actual HHW/Steam loop conditions in Proposed Case",null,"n/a",null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(G55=\"\",\"\",\"180°F at 20°F and below; 150°F at 50°F and above; and ramped linearly between 180°F and 150°F between 20°F and 50°F\"))","v":""},null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"HHW loop configuration","•  Primary-only per G3.1.3.5\n•  ASHRAE 90.1 (DES Path 1) or Streamlined DES (DES Path 3): Baseline pumps shall only be modeled if distribution pumps are present in the building, in which case buildings shall be modeled as primary-only per G3.1.3.5",null,"n/a",null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(G55=\"\",\"\",\"Primary-only\"))","v":""},null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"Number of primary or DES plant HHW pumps","•  One pump\n•  ASHRAE 90.1 (DES Path 1) or Streamlined DES (DES Path 3): equal to the number of distribution pumps present in the building",null,"#",null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(G55=\"\",\"\",\"1\"))","v":""},null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"Primary or DES plant HHW total pump power","•  19 W/gpm (301 kW/1000 L/s) per G3.1.3.5\n•  ASHRAE 90.1 (Path 1) or Streamlined DES (Path 3): 14 W/gpm (222 kW/1000 L/s) per exception to G3.1.3.5",null,"kW",null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(G55=\"\",\"\",\"19 W/gpm\"))","v":""},null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},null,{"$f":"IF(E58=\"kW\",G58,\"\")","v":0},{"$f":"IF(E58=\"kW\",J58,\"\")","v":0}]
[null,"Primary or DES plant HHW pump flow","Auto-sized with a capacity ratio of 1.0 based on HHW temperatures",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"gpm\",\"L/s\")","v":"gpm"},null,null,null,null,null,null,null,"n/a",null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"Primary or DES plant HHW pump control","•  <120,000 sq ft (11,160 m2): riding the pump curve\n•  ≥120,000 sq ft (11,160 m2): variable speed",null,"n/a",null,null,null,null,null,null,null,{"$f":"IF('General Information'!$K$48=2007,\"Not Supported\",IF(G60=\"\",\"\",IF(GI_BldgArea<120000,\"Riding the Pump Curve\",\"Variable-Speed Drives\")))","v":""},null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"Number of secondary or building booster HHW pumps","Baseline is primary-only",null,"#",null,null,null,null,null,null,null,null,null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"Secondary or building booster HHW pump power","Baseline is primary-only",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},null,{"$f":"IF(E62=\"kW\",G62,\"\")","v":""},{"$f":"IF(E62=\"kW\",J62,\"\")","v":""}]
[null,"Secondary or building booster HW pump efficiency","Baseline is primary-only",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"Secondary or building booster HHW pump flow","Baseline is primary-only",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,"Secondary or building booster HHW pump control","Baseline is primary-only",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Hot Water or Steam",0,{"$f":"G49&\" with capacity of \"&G51&\" \"&E51&\" and efficiency of \"&G52&\". The HHW supply temp is \"&G53&\" (F) with a HHW delta T of \"&G54&\" (F). The HHW temp reset parameters are as follows: \"&G55&\". The HHW loop configuration is \"&G56&\" with \"&G57&\" pump(s) with pump power of \"&G58&\" \"&E58&\" and pump flow of \"&G59&\" gpm. The pump conrol is \"&G60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"J49&\" with capacity of \"&J51&\" \"&E51&\" and efficiency of \"&J52&\". The HHW supply temp is \"&J53&\" (F) with a HHW delta T of \"&J54&\" (F). The HHW temp reset parameters are as follows: \"&J55&\". The HHW loop configuration is \"&J56&\" with \"&J57&\" pump(s) with pump power of \"&J58&\" \"&E58&\" and pump flow of \"&J59&\" gpm. The pump conrol is \"&J60&\".\"","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[]
[]
[null,"Table 11.4: Geothermal Loop",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,"Proposed Design",null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
[null,"Model Input Parameter",{"$f":"$C$10","v":"ASHRAE 90.1 2016 Appendix G - Baseline Systems Helpful Notes"},null,"Units",null,{"$f":"G10","v":0},null,null,"Project","Plans / Specs"]
[null,"Type of geothermal system","Proposed Case: Describe the geothermal or geoexchange system (e.g. closed loop vertical system, 4 inch (100 mm) diameter drilled 20 feet (6095 mm) apart, 250 feet (76.2 m) deep)",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",{"$f":"N70","v":0},"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,"Soil conductivity (if applicable)","Proposed Case: For ground source systems, enter the soil conductivity modeled for the system. This should be based on testing performed on the soil.",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",{"$f":"N71","v":0},"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,"Geothermal source design temperature - summer","Proposed Case: Enter the summer design temperature of the soil (for ground source heat pumps), or surface water (for lake, pond, ocean, or other water exchange heat pumps)",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"°F\",\"°C\")","v":"°F"},null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",0,"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,"Geothermal source design temperature - winter","Proposed Case: Enter the winter design temperature of the soil (for ground source heat pumps), or surface water (for lake, pond, ocean, or other water exchange heat pumps)",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"°F\",\"°C\")","v":"°F"},null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",0,"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,"Geoexchange loop design fluid supply temperature - cooling",null,null,{"$f":"IF('General Information'!$K$11=\"IP\",\"°F\",\"°C\")","v":"°F"},null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",0,"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,"Geoexchange loop design fluid supply temperature -heating",null,null,{"$f":"IF('General Information'!$K$11=\"IP\",\"°F\",\"°C\")","v":"°F"},null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",0,"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,"Geoexchange loop - operating temperature","Proposed Case: Describe how the operating temperature of the geothermal loop will be controlled, and how this was accounted for in the energy model.",null,{"$f":"IF('General Information'!$K$11=\"IP\",\"°F\",\"°C\")","v":"°F"},null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",0,"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,"Geothermal energy transfer effect","Proposed Case: Describe how the energy transfer effect from the building to the ground or surface water source has been accounted for in the energy model and the geothermal loop design.",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",0,"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,"Geothermal loop pumping configuration",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",0,"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,"Number of geothermal loop pumps","Proposed Case: Enter the number of Proposed geothermal loop pumps modeled (example: 1 (additional scheduled pump is stand-by))",null,"#",null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",0,"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,"Geothermal loop pump control",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",0,"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,"Geothermal pump power ",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",0,"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."},null,{"$f":"IF(E81=\"kW\",G81,\"\")","v":""},{"$f":"IF(E81=\"kW\",J81,\"\")","v":""}]
[null,"Geothermal loop flow",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",0,"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,"Geothermal air-side efficiency curves","Proposed Case: Provide a brief description of how the geothermal air-side equipment efficiency curves were modeled, and confirm that they take into account the expected operating temperatures of the geothermal loop.",null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Geothermal Loop",0,"<User Entry>",{"$f":"J70&\" geothermal system with the following parameters: \"&B71&\": \"&J71&\", \"&B72&\": \"&J72&\" (F), \"&B73&\": \"&J73&\" (F), \"&B74&\": \"&J74&\" (F), \"&B75&\": \"&J75&\" (F), \"&B76&\": \"&J76&\" (F), \"&B77&\": \"&J77&\", \"&B78&\": \"&J78&\", \"&B79&\": \"&J79&\", \"&B80&\": \"&J80&\", \"&B81&\": \"&J81&\", \"&B82&\": \"&J82&\", \"&B83&\": \"&J83&\".\"","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[]
[]
[null,"Table 11.5: Combined Heat and Power (CHP)",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,"Proposed Design",null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
[null,"Model Input Parameter",{"$f":"$C$10","v":"ASHRAE 90.1 2016 Appendix G - Baseline Systems Helpful Notes"},null,"Units",null,{"$f":"G10","v":0},null,null,"Project","Plans / Specs"]
[null,"Type of generator",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Combined Heat and Power (CHP)",{"$f":"N88","v":0},"<User Entry>",{"$f":"J88&\" generator with the following parameters: \"&B89&\": \"&J89&\", \"&B90&\": \"&J90&\", \"&B91&\": \"&J91&\", \"&B92&\": \"&J92&\", \"&B93&\": \"&J93&\", \"&B94&\": \"&J94&\", \"&B95&\": \"&J95&\", \"&B96&\": \"&J96&\", \"&B97&\": \"&J97&\".\"","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,"Quantity of CHP generators",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Combined Heat and Power (CHP)",{"$f":"N89","v":0},"<User Entry>",{"$f":"J88&\" generator with the following parameters: \"&B89&\": \"&J89&\", \"&B90&\": \"&J90&\", \"&B91&\": \"&J91&\", \"&B92&\": \"&J92&\", \"&B93&\": \"&J93&\", \"&B94&\": \"&J94&\", \"&B95&\": \"&J95&\", \"&B96&\": \"&J96&\", \"&B97&\": \"&J97&\".\"","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,"Total capacity of CHP generators (kW) at design conditions",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Combined Heat and Power (CHP)",0,"<User Entry>",{"$f":"J88&\" generator with the following parameters: \"&B89&\": \"&J89&\", \"&B90&\": \"&J90&\", \"&B91&\": \"&J91&\", \"&B92&\": \"&J92&\", \"&B93&\": \"&J93&\", \"&B94&\": \"&J94&\", \"&B95&\": \"&J95&\", \"&B96&\": \"&J96&\", \"&B97&\": \"&J97&\".\"","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,"Thermal efficiency (%) at design conditions",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Combined Heat and Power (CHP)",0,"<User Entry>",{"$f":"J88&\" generator with the following parameters: \"&B89&\": \"&J89&\", \"&B90&\": \"&J90&\", \"&B91&\": \"&J91&\", \"&B92&\": \"&J92&\", \"&B93&\": \"&J93&\", \"&B94&\": \"&J94&\", \"&B95&\": \"&J95&\", \"&B96&\": \"&J96&\", \"&B97&\": \"&J97&\".\"","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,"Electrical efficiency (%) at design conditions",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Combined Heat and Power (CHP)",0,"<User Entry>",{"$f":"J88&\" generator with the following parameters: \"&B89&\": \"&J89&\", \"&B90&\": \"&J90&\", \"&B91&\": \"&J91&\", \"&B92&\": \"&J92&\", \"&B93&\": \"&J93&\", \"&B94&\": \"&J94&\", \"&B95&\": \"&J95&\", \"&B96&\": \"&J96&\", \"&B97&\": \"&J97&\".\"","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,"Controls or schedule",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Combined Heat and Power (CHP)",0,"<User Entry>",{"$f":"J88&\" generator with the following parameters: \"&B89&\": \"&J89&\", \"&B90&\": \"&J90&\", \"&B91&\": \"&J91&\", \"&B92&\": \"&J92&\", \"&B93&\": \"&J93&\", \"&B94&\": \"&J94&\", \"&B95&\": \"&J95&\", \"&B96&\": \"&J96&\", \"&B97&\": \"&J97&\".\"","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,"Fuel Source",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Combined Heat and Power (CHP)",0,"<User Entry>",{"$f":"J88&\" generator with the following parameters: \"&B89&\": \"&J89&\", \"&B90&\": \"&J90&\", \"&B91&\": \"&J91&\", \"&B92&\": \"&J92&\", \"&B93&\": \"&J93&\", \"&B94&\": \"&J94&\", \"&B95&\": \"&J95&\", \"&B96&\": \"&J96&\", \"&B97&\": \"&J97&\".\"","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,"Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.)",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Combined Heat and Power (CHP)",0,"<User Entry>",{"$f":"J88&\" generator with the following parameters: \"&B89&\": \"&J89&\", \"&B90&\": \"&J90&\", \"&B91&\": \"&J91&\", \"&B92&\": \"&J92&\", \"&B93&\": \"&J93&\", \"&B94&\": \"&J94&\", \"&B95&\": \"&J95&\", \"&B96&\": \"&J96&\", \"&B97&\": \"&J97&\".\"","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,"Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers)",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Combined Heat and Power (CHP)",0,"<User Entry>",{"$f":"J88&\" generator with the following parameters: \"&B89&\": \"&J89&\", \"&B90&\": \"&J90&\", \"&B91&\": \"&J91&\", \"&B92&\": \"&J92&\", \"&B93&\": \"&J93&\", \"&B94&\": \"&J94&\", \"&B95&\": \"&J95&\", \"&B96&\": \"&J96&\", \"&B97&\": \"&J97&\".\"","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,"Parasitic losses (e.g. air handling unit to cool the intake air)",null,null,"n/a",null,null,null,null,null,null,null,null,null,null,null,null,null,"Combined Heat and Power (CHP)",0,"<User Entry>",{"$f":"J88&\" generator with the following parameters: \"&B89&\": \"&J89&\", \"&B90&\": \"&J90&\", \"&B91&\": \"&J91&\", \"&B92&\": \"&J92&\", \"&B93&\": \"&J93&\", \"&B94&\": \"&J94&\", \"&B95&\": \"&J95&\", \"&B96&\": \"&J96&\", \"&B97&\": \"&J97&\".\"","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[]
[]
[null,"Table 11.6: Other",null,null,null,{"$f":"\"Baseline\"&\"-\"&'General Information'!$C$42","v":"Baseline-ASHRAE 90.1 2016 Appendix G"},null,null,"Proposed Design",null,null,null,{"$f":"\"Prescriptive Requirement of \"&'General Information'!C48&\" Applicable to App. G Baseline\"","v":"Prescriptive Requirement of ASHRAE 90.1-2013 Applicable to App. G Baseline"},"Measure #"]
[null,"Model Input Parameter",null,null,"Units",null,{"$f":"G10","v":0},null,null,"Project","Plans / Specs"]
[null,"Other (describe)"]
[null,"Other (describe)"]
[null,"Other (describe)"]
[null,"Other (describe)"]
[null,"Other (describe)"]
[null,"Other (describe)"]

{"sheet":"P4P - LEED Inputs","index":28,"n_rows":20,"n_cols":7,"rows_kept":20,"cut":false,"hidden":true,"merged":[[0,2,0,5],[1,2,1,5],[2,2,2,5],[6,1,6,6]]}
[null,null,"New Jersey Office of Clean Energy"]
[null,null,"Pay for Performance New Construction Program"]
[null,null,"ERP Tables and Incentive Calculator"]
[]
[null,"LEED Inputs"]
[null,"Instructions"]
[null,"1) This tab is to be used only for the New Jersey Office of Clean Energy, Pay for Performance New Construction Program.\n2) Select row 13-20 below and copy into the Window's clipboard by pressing Ctrl-C. Paste the rows as values in the \"P4P - LEED Inputs\" tab of the P4P ERP Tables workbook following instructions on this tab."]
[]
[]
[]
[]
[]
[null,"Project Name",{"$f":"GI_Project_Name","v":0},"Area sf New Construction Conditioned","Area (sf) Renovation Conditioned","Area sf New Construction Unconditioned (sf)","Area (sf) Renovation Unconditioned (sf)"]
[null,"Building Type 1",{"$f":"'General Information'!$F$17","v":0},{"$f":"'General Information'!$G$17","v":0},{"$f":"'General Information'!$H$17","v":0},{"$f":"'General Information'!$I$17","v":0},{"$f":"'General Information'!$J$17","v":0}]
[null,"Building Type 2",{"$f":"'General Information'!$F$18","v":0},{"$f":"'General Information'!$G$18","v":0},{"$f":"'General Information'!$H$18","v":0},{"$f":"'General Information'!$I$18","v":0},{"$f":"'General Information'!$J$18","v":0}]
[null,"Building Type 3",{"$f":"'General Information'!$F$19","v":0},{"$f":"'General Information'!$G$19","v":0},{"$f":"'General Information'!$H$19","v":0},{"$f":"'General Information'!$I$19","v":0},{"$f":"'General Information'!$J$19","v":0}]
[null,"Total Building Area (sf)",{"$f":"BuildingArea","v":0}]
[null,"Number of Stories Above Grade",{"$f":"'General Information'!F29","v":0}]
[null,"Number of Stories Below Grade",{"$f":"'General Information'!G29","v":0}]
[null,"Number of Identical Buildings",{"$f":"IF(MultipleBuildingsExist=\"No\",1,'1 - Multiple Buildings Details'!F33)","v":1}]

{"sheet":"Results from eQuest","index":29,"n_rows":15,"n_cols":76,"rows_kept":15,"cut":false,"hidden":false,"merged":[[5,64,5,65],[5,66,5,69],[5,70,5,75],[3,0,3,10],[5,11,5,23],[5,24,5,35],[5,36,5,48],[5,49,5,61],[5,62,5,63]]}
[]
["(OPTIONAL) Results from eQUEST Parms.csv File(s)"]
[]
["Instructions: \n1) Open Parms.csv file(s) that include results for baseline and proposed models\n2) Copy baseline runs from the appropriate Parms.csv file and paste values into rows 8-11 below. For projects that were not rotated, paste the lone baseline run into row 8. \n3) Copy the proposed run from the appropriate Parms.csv file and paste values into row 13 below. \n4) Copy all parametric runs including the proposed run, but not including baseline run(s), and paste values in rows 16 and below. This step is optional.\n\nNote: Lighting exempt from 90.1 (Section 9.1.1, 9.2.2.3, or 9.4.2) must be modeled identically in the baseline and proposed models. Exempt lighting must be treated as unregulated load in PCIt calculations. Please do not model exempt lighting with the Ambient Lights, but rather model as a process load so that it may be reported separately (please also update the Software Links in column BF of the '12 - Performance_Outputs_1' tab, or manually enter the exempt lighting consumption and demand on the the '12 - Performance_Outputs_1' tab)."]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Electric Usage:",null,null,null,null,null,null,null,null,null,null,null,null,"Non-Coincident Peak Demand:",null,null,null,null,null,null,null,null,null,null,null,"Coincident Peak Demand:",null,null,null,null,null,null,null,null,null,null,null,null,"Fuel Usage:",null,null,null,null,null,null,null,null,null,null,null,null,"Source Energy:",null,"TDV Energy:",null,"Annual Utility Costs:",null,null,null,"Hours Outside Throttling Range:"]
["Run Type","Internal Loads","Case #s","Short Name","Carry Fwd","Incremental First Cost ($)","Incremental Annual Maint. ($)","Date & Time of Run","File Name","Case Description","SS-D\nPeak Cooling Coil Load\nkBtu","PS-E\nAmbient Lights\nkWh","PS-E\nTask Lights\nkWh","PS-E\nMisc Equip\nkWh","PS-E\nSpace Heating\nkWh","PS-E\nSpace Cooling\nkWh","PS-E\nHeat Reject\nkWh","PS-E\nPumps & Aux\nkWh","PS-E\nVentilation Fans\nkWh","PS-E\nRefrig Display\nkWh","PS-E\nHeat Pump Supplement\nkWh","PS-E\nDomestic Hot Water\nkWh","PS-E\nExterior Usage\nkWh","PS-E\nTotal\nkWh","PS-E\nAmbient Lights\nkW","PS-E\nTask Lights\nkW","PS-E\nMisc Equip\nkW","PS-E\nSpace Heating\nkW","PS-E\nSpace Cooling\nkW","PS-E\nHeat Reject\nkW","PS-E\nPumps & Aux\nkW","PS-E\nVentilation Fans\nkW","PS-E\nRefrig Display\nkW","PS-E\nHeat Pump Supplement\nkW","PS-E\nDomestic Hot Water\nkW","PS-E\nExterior Usage\nkW","PS-E\nAmbient Lights\nkW","PS-E\nTask Lights\nkW","PS-E\nMisc Equip\nkW","PS-E\nSpace Heating\nkW","PS-E\nSpace Cooling\nkW","PS-E\nHeat Reject\nkW","PS-E\nPumps & Aux\nkW","PS-E\nVentilation Fans\nkW","PS-E\nRefrig Display\nkW","PS-E\nHeat Pump Supplement\nkW","PS-E\nDomestic Hot Water\nkW","PS-E\nExterior Usage\nkW","PS-E\nBldg Total\nkW","PS-E\nAmbient Lights\nTherms","PS-E\nTask Lights\nTherms","PS-E\nMisc Equip\nTherms","PS-E\nSpace Heating\nTherms","PS-E\nSpace Cooling\nTherms","PS-E\nHeat Reject\nTherms","PS-E\nPumps & Aux\nTherms","PS-E\nVentilation Fans\nTherms","PS-E\nRefrig Display\nTherms","PS-E\nHeat Pump Supplement\nTherms","PS-E\nDomestic Hot Water\nTherms","PS-E\nExterior Usage\nTherms","PS-E\nTotal\nTherms","BEPS\nBldg Energy\nMbtu","BEPS\nBldg EUI\nkBtu/sf/yr","TDV1\nBldg Energy\nTDV-Mbtu","TDV1\nBldg EUI\nTDV-kBtu/sf/yr","ES-E\nTotal Electric\n$","ES-E\nTotal Fuel\n$","ES-E\nElectric kWh\n$","ES-E\nElectric kW\n$","BEPS\nZone Outsd Thrtlng Rng\n% hrs","BEPS\nPlant Ld Not Met\n% hrs","SS-E\nHours Fan On\n# hrs","\nZone Outsd Thrtlng Rng\n# hrs","BEPS\nCool Loads Not Met\n# hrs","BEPS\nHeat Loads Not Met\n# hrs"]
[]
[]
[]
[]
[{"$f":"IF('[3]P4P - General Info'!C23=\"ASHRAE bEQ\",\"Proposed Design\",\"Average Baseline\")","v":"Average Baseline"},null,null,null,null,null,null,null,null,null,{"$f":"IF(K8=\"\",\"\",AVERAGE(K8:K11))","v":""},"","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","",""]
[]
[]
["Step 4, and the rows below are optional inputs."]

{"sheet":"ECM","index":30,"n_rows":233,"n_cols":5,"rows_kept":233,"cut":false,"hidden":true,"merged":[]}
[]
[null,{"$f":"GI_Project_Name&\" ECM Building Components\"","v":" ECM Building Components"}]
[]
[]
[null,"Item","Energy Efficient Measure #","Baseline Description","Proposed Description"]
[]
[null,"Shading and Fenestration"]
[null,"Automatically controlled fenestration shades or blinds",{"$f":"'4 - Shading and Fenestration'!M8","v":0},"<User Entry>","<User Entry>"]
[null,"Permanent shading devices such as fins, overhangs, and light shelves",{"$f":"'4 - Shading and Fenestration'!M9","v":0},"<User Entry>","<User Entry>"]
[null,"North Vertical Glazing Area",{"$f":"'4 - Shading and Fenestration'!M34","v":0},{"$f":"'4 - Shading and Fenestration'!C34&\": Building Area Type with \"&'4 - Shading and Fenestration'!G34&\" sq ft of Vertical Glazing on the \"&'4 - Shading and Fenestration'!D34&\" façade.\"","v":": Building Area Type with - sq ft of Vertical Glazing on the North façade."},{"$f":"'4 - Shading and Fenestration'!C34&\": Building Area Type with \"&'4 - Shading and Fenestration'!J34&\" sq ft of Vertical Glazing on the \"&'4 - Shading and Fenestration'!D34&\" façade.\"","v":": Building Area Type with  sq ft of Vertical Glazing on the North façade."}]
[null,"East Vertical Glazing Area",{"$f":"'4 - Shading and Fenestration'!M35","v":0},{"$f":"'4 - Shading and Fenestration'!C35&\": Building Area Type with \"&'4 - Shading and Fenestration'!G35&\" sq ft of Vertical Glazing on the \"&'4 - Shading and Fenestration'!D35&\" façade.\"","v":": Building Area Type with - sq ft of Vertical Glazing on the East façade."},{"$f":"'4 - Shading and Fenestration'!C35&\": Building Area Type with \"&'4 - Shading and Fenestration'!J35&\" sq ft of Vertical Glazing on the \"&'4 - Shading and Fenestration'!D35&\" façade.\"","v":": Building Area Type with  sq ft of Vertical Glazing on the East façade."}]
[null,"South Vertical Glazing Area",{"$f":"'4 - Shading and Fenestration'!M36","v":0},{"$f":"'4 - Shading and Fenestration'!C36&\": Building Area Type with \"&'4 - Shading and Fenestration'!G36&\" sq ft of Vertical Glazing on the \"&'4 - Shading and Fenestration'!D36&\" façade.\"","v":": Building Area Type with - sq ft of Vertical Glazing on the South façade."},{"$f":"'4 - Shading and Fenestration'!C36&\": Building Area Type with \"&'4 - Shading and Fenestration'!J36&\" sq ft of Vertical Glazing on the \"&'4 - Shading and Fenestration'!D36&\" façade.\"","v":": Building Area Type with  sq ft of Vertical Glazing on the South façade."}]
[null,"West Vertical Glazing Area",{"$f":"'4 - Shading and Fenestration'!M37","v":0},{"$f":"'4 - Shading and Fenestration'!C37&\": Building Area Type with \"&'4 - Shading and Fenestration'!G37&\" sq ft of Vertical Glazing on the \"&'4 - Shading and Fenestration'!D37&\" façade.\"","v":": Building Area Type with - sq ft of Vertical Glazing on the West façade."},{"$f":"'4 - Shading and Fenestration'!C37&\": Building Area Type with \"&'4 - Shading and Fenestration'!J37&\" sq ft of Vertical Glazing on the \"&'4 - Shading and Fenestration'!D37&\" façade.\"","v":": Building Area Type with  sq ft of Vertical Glazing on the West façade."}]
[null,"Total Vertical Glazing Area",{"$f":"'4 - Shading and Fenestration'!M42","v":0},{"$f":"\"Total of \"&'4 - Shading and Fenestration'!G42&\" sq ft of Vertical Glazing on the \"&\"building façades.\"","v":"Total of 0 sq ft of Vertical Glazing on the building façades."},{"$f":"\"Total of \"&'4 - Shading and Fenestration'!J42&\" sq ft of Vertical Glazing on the \"&\"building façades.\"","v":"Total of 0 sq ft of Vertical Glazing on the building façades."}]
[null,"Vertical Glazing (1)",{"$f":"'4 - Shading and Fenestration'!R68","v":0},{"$f":"\"Vertical Glazing is\"&'4 - Shading and Fenestration'!F68&\", \nU-\"&'4 - Shading and Fenestration'!G68&\",  \nSHGC-\"&'4 - Shading and Fenestration'!H68","v":"Vertical Glazing is, \nU-,  \nSHGC-"},{"$f":"'4 - Shading and Fenestration'!J68&\", \nU-\"&'4 - Shading and Fenestration'!K68&\",\nSHGC-\"&'4 - Shading and Fenestration'!L68&\", \nVLT-\"&'4 - Shading and Fenestration'!M68","v":", \nU-,\nSHGC-, \nVLT-"}]
[null,"Skylights (1)",{"$f":"'4 - Shading and Fenestration'!R77","v":0},{"$f":"'4 - Shading and Fenestration'!F77&\" of the façade,\n U-\"&'4 - Shading and Fenestration'!G77&\",  \nSHGC-\"&'4 - Shading and Fenestration'!H77","v":" of the façade,\n U-,  \nSHGC-"},{"$f":"'4 - Shading and Fenestration'!J77&\", \nU-\"&'4 - Shading and Fenestration'!K77&\",\nSHGC-\"&'4 - Shading and Fenestration'!L77&\", \nVLT-\"&'4 - Shading and Fenestration'!M77","v":", \nU-,\nSHGC-, \nVLT-"}]
[null,"Opaque Assemblies"]
[null,"Infiltration",{"$f":"'5 - Opaque Assemblies'!J36","v":0},{"$f":"ROUND('5 - Opaque Assemblies'!F42,3)&\" \"&'5 - Opaque Assemblies'!B42&\",\n \"&ROUND('5 - Opaque Assemblies'!F43,3)&\" \"&'5 - Opaque Assemblies'!B43&\", \n\"&'5 - Opaque Assemblies'!F44&\" \"&'5 - Opaque Assemblies'!B44","v":{"$error":"#VALUE!"}},{"$f":"ROUND('5 - Opaque Assemblies'!H42,3)&\" \"&'5 - Opaque Assemblies'!B42&\", \n\"&ROUND('5 - Opaque Assemblies'!H43,3)&\" \"&'5 - Opaque Assemblies'!B43&\", \n\"&'5 - Opaque Assemblies'!H44&\" \"&'5 - Opaque Assemblies'!B44","v":{"$error":"#VALUE!"}}]
[null,"Roof (1)",{"$f":"'5 - Opaque Assemblies'!R52","v":0},{"$f":"'5 - Opaque Assemblies'!C52&\" construction, \"&'5 - Opaque Assemblies'!D52&\"; \"&'5 - Opaque Assemblies'!F52&\" and Solar Reflectance and Thermal Emittance of \"&'5 - Opaque Assemblies'!N52","v":" construction, ;  and Solar Reflectance and Thermal Emittance of "},{"$f":"'5 - Opaque Assemblies'!I52&\" with U-\"&'5 - Opaque Assemblies'!J52&\" and Solar Reflectance and Thermal Emmitance of \"&'5 - Opaque Assemblies'!O52","v":" with U- and Solar Reflectance and Thermal Emmitance of "}]
[null,"AGW (1)",{"$f":"'5 - Opaque Assemblies'!O62","v":0},{"$f":"'5 - Opaque Assemblies'!C62&\" construction, \"&'5 - Opaque Assemblies'!D62&\"; \"&'5 - Opaque Assemblies'!F62","v":" construction, ; "},{"$f":"'5 - Opaque Assemblies'!I62&\" with U-\"&'5 - Opaque Assemblies'!J62","v":" with U-"}]
[null,"BGW (1)",{"$f":"'5 - Opaque Assemblies'!O72","v":0},{"$f":"'5 - Opaque Assemblies'!C72&\" construction, \"&'5 - Opaque Assemblies'!D72&\"; \"&'5 - Opaque Assemblies'!F72","v":" construction, ; "},{"$f":"'5 - Opaque Assemblies'!I72&\" with C-\"&'5 - Opaque Assemblies'!J72","v":" with C-"}]
[null,"Exposed Floor (1)",{"$f":"'5 - Opaque Assemblies'!O82","v":0},{"$f":"'5 - Opaque Assemblies'!C82&\" construction, \"&'5 - Opaque Assemblies'!D82&\"; \"&'5 - Opaque Assemblies'!F82","v":" construction, ; "},{"$f":"'5 - Opaque Assemblies'!I82&\" with U-\"&'5 - Opaque Assemblies'!J82","v":" with U-"}]
[null,"Slab on Grade Floor (1)",{"$f":"'5 - Opaque Assemblies'!O92","v":0},{"$f":"'5 - Opaque Assemblies'!C92&\" construction, \"&'5 - Opaque Assemblies'!D92&\"; \"&'5 - Opaque Assemblies'!F92","v":" construction, ; "},{"$f":"'5 - Opaque Assemblies'!I92&\" with F-\"&'5 - Opaque Assemblies'!J92","v":" with F-"}]
[null,"Opaque Doors (1)",{"$f":"'5 - Opaque Assemblies'!O102","v":0},{"$f":"'5 - Opaque Assemblies'!C102&\" construction, \"&'5 - Opaque Assemblies'!D102&\"; \"&'5 - Opaque Assemblies'!F102","v":" construction, ; "},{"$f":"'5 - Opaque Assemblies'!I102&\" with U-\"&'5 - Opaque Assemblies'!J102","v":" with U-"}]
[null,"Lighting General"]
[null,"Interior Lighting by Space Type",{"$f":"'6b - General Lighting'!N27","v":0},{"$f":"\"Interior lighting power is calculated as \"&'6b - General Lighting'!F60&\" Watts and \"&'6b - General Lighting'!I60&\" w/sf, both without lighting controls. Including lighting controls, the lighting power is calculated as \"&'6b - General Lighting'!L60&\" Watts and \"&'6b - General Lighting'!K60&\" w/sf.\"","v":"Interior lighting power is calculated as 0 Watts and - w/sf, both without lighting controls. Including lighting controls, the lighting power is calculated as 0 Watts and - w/sf."},{"$f":"\"Interior lighting power is calculated as \"&'6b - General Lighting'!E60&\" Watts and \"&'6b - General Lighting'!H60&\" w/sf\"","v":"Interior lighting power is calculated as 0 Watts and - w/sf"}]
[null,"Exterior Lighting",{"$f":"'6b - General Lighting'!U149","v":0},{"$f":"\"Lighting Power Allowance of \"&'6b - General Lighting'!J149&\" W\"","v":"Lighting Power Allowance of 0 W"},{"$f":"\"Lighting Power Allowance of \"&'6b - General Lighting'!M149&\" W\"","v":"Lighting Power Allowance of 0 W"}]
[null,{"$f":"'6b - General Lighting'!B27&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N27","v":0},{"$f":"\"The \"&'6b - General Lighting'!B27&\" LPD is \"&'6b - General Lighting'!I27","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B27&\" LPD is \"&'6b - General Lighting'!H27&\" without OS and \"&'6b - General Lighting'!K27&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B28&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N28","v":0},{"$f":"\"The \"&'6b - General Lighting'!B28&\" LPD is \"&'6b - General Lighting'!I28","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B28&\" LPD is \"&'6b - General Lighting'!H28&\" without OS and \"&'6b - General Lighting'!K28&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B29&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N29","v":0},{"$f":"\"The \"&'6b - General Lighting'!B29&\" LPD is \"&'6b - General Lighting'!I29","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B29&\" LPD is \"&'6b - General Lighting'!H29&\" without OS and \"&'6b - General Lighting'!K29&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B30&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N30","v":0},{"$f":"\"The \"&'6b - General Lighting'!B30&\" LPD is \"&'6b - General Lighting'!I30","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B30&\" LPD is \"&'6b - General Lighting'!H30&\" without OS and \"&'6b - General Lighting'!K30&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B31&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N31","v":0},{"$f":"\"The \"&'6b - General Lighting'!B31&\" LPD is \"&'6b - General Lighting'!I31","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B31&\" LPD is \"&'6b - General Lighting'!H31&\" without OS and \"&'6b - General Lighting'!K31&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B32&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N32","v":0},{"$f":"\"The \"&'6b - General Lighting'!B32&\" LPD is \"&'6b - General Lighting'!I32","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B32&\" LPD is \"&'6b - General Lighting'!H32&\" without OS and \"&'6b - General Lighting'!K32&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B33&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N33","v":0},{"$f":"\"The \"&'6b - General Lighting'!B33&\" LPD is \"&'6b - General Lighting'!I33","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B33&\" LPD is \"&'6b - General Lighting'!H33&\" without OS and \"&'6b - General Lighting'!K33&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B34&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N34","v":0},{"$f":"\"The \"&'6b - General Lighting'!B34&\" LPD is \"&'6b - General Lighting'!I34","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B34&\" LPD is \"&'6b - General Lighting'!H34&\" without OS and \"&'6b - General Lighting'!K34&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B35&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N35","v":0},{"$f":"\"The \"&'6b - General Lighting'!B35&\" LPD is \"&'6b - General Lighting'!I35","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B35&\" LPD is \"&'6b - General Lighting'!H35&\" without OS and \"&'6b - General Lighting'!K35&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B36&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N36","v":0},{"$f":"\"The \"&'6b - General Lighting'!B36&\" LPD is \"&'6b - General Lighting'!I36","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B36&\" LPD is \"&'6b - General Lighting'!H36&\" without OS and \"&'6b - General Lighting'!K36&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B37&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N37","v":0},{"$f":"\"The \"&'6b - General Lighting'!B37&\" LPD is \"&'6b - General Lighting'!I37","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B37&\" LPD is \"&'6b - General Lighting'!H37&\" without OS and \"&'6b - General Lighting'!K37&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B38&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N38","v":0},{"$f":"\"The \"&'6b - General Lighting'!B38&\" LPD is \"&'6b - General Lighting'!I38","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B38&\" LPD is \"&'6b - General Lighting'!H38&\" without OS and \"&'6b - General Lighting'!K38&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B39&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N39","v":0},{"$f":"\"The \"&'6b - General Lighting'!B39&\" LPD is \"&'6b - General Lighting'!I39","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B39&\" LPD is \"&'6b - General Lighting'!H39&\" without OS and \"&'6b - General Lighting'!K39&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B40&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N40","v":0},{"$f":"\"The \"&'6b - General Lighting'!B40&\" LPD is \"&'6b - General Lighting'!I40","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B40&\" LPD is \"&'6b - General Lighting'!H40&\" without OS and \"&'6b - General Lighting'!K40&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B41&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N41","v":0},{"$f":"\"The \"&'6b - General Lighting'!B41&\" LPD is \"&'6b - General Lighting'!I41","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B41&\" LPD is \"&'6b - General Lighting'!H41&\" without OS and \"&'6b - General Lighting'!K41&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B42&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N42","v":0},{"$f":"\"The \"&'6b - General Lighting'!B42&\" LPD is \"&'6b - General Lighting'!I42","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B42&\" LPD is \"&'6b - General Lighting'!H42&\" without OS and \"&'6b - General Lighting'!K42&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B43&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N43","v":0},{"$f":"\"The \"&'6b - General Lighting'!B43&\" LPD is \"&'6b - General Lighting'!I43","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B43&\" LPD is \"&'6b - General Lighting'!H43&\" without OS and \"&'6b - General Lighting'!K43&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B44&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N44","v":0},{"$f":"\"The \"&'6b - General Lighting'!B44&\" LPD is \"&'6b - General Lighting'!I44","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B44&\" LPD is \"&'6b - General Lighting'!H44&\" without OS and \"&'6b - General Lighting'!K44&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B45&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N45","v":0},{"$f":"\"The \"&'6b - General Lighting'!B45&\" LPD is \"&'6b - General Lighting'!I45","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B45&\" LPD is \"&'6b - General Lighting'!H45&\" without OS and \"&'6b - General Lighting'!K45&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B46&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N46","v":0},{"$f":"\"The \"&'6b - General Lighting'!B46&\" LPD is \"&'6b - General Lighting'!I46","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B46&\" LPD is \"&'6b - General Lighting'!H46&\" without OS and \"&'6b - General Lighting'!K46&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B47&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N47","v":0},{"$f":"\"The \"&'6b - General Lighting'!B47&\" LPD is \"&'6b - General Lighting'!I47","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B47&\" LPD is \"&'6b - General Lighting'!H47&\" without OS and \"&'6b - General Lighting'!K47&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B48&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N48","v":0},{"$f":"\"The \"&'6b - General Lighting'!B48&\" LPD is \"&'6b - General Lighting'!I48","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B48&\" LPD is \"&'6b - General Lighting'!H48&\" without OS and \"&'6b - General Lighting'!K48&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B49&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N49","v":0},{"$f":"\"The \"&'6b - General Lighting'!B49&\" LPD is \"&'6b - General Lighting'!I49","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B49&\" LPD is \"&'6b - General Lighting'!H49&\" without OS and \"&'6b - General Lighting'!K49&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B50&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N50","v":0},{"$f":"\"The \"&'6b - General Lighting'!B50&\" LPD is \"&'6b - General Lighting'!I50","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B50&\" LPD is \"&'6b - General Lighting'!H50&\" without OS and \"&'6b - General Lighting'!K50&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B51&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N51","v":0},{"$f":"\"The \"&'6b - General Lighting'!B51&\" LPD is \"&'6b - General Lighting'!I51","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B51&\" LPD is \"&'6b - General Lighting'!H51&\" without OS and \"&'6b - General Lighting'!K51&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B52&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N52","v":0},{"$f":"\"The \"&'6b - General Lighting'!B52&\" LPD is \"&'6b - General Lighting'!I52","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B52&\" LPD is \"&'6b - General Lighting'!H52&\" without OS and \"&'6b - General Lighting'!K52&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B53&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N53","v":0},{"$f":"\"The \"&'6b - General Lighting'!B53&\" LPD is \"&'6b - General Lighting'!I53","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B53&\" LPD is \"&'6b - General Lighting'!H53&\" without OS and \"&'6b - General Lighting'!K53&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B54&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N54","v":0},{"$f":"\"The \"&'6b - General Lighting'!B54&\" LPD is \"&'6b - General Lighting'!I54","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B54&\" LPD is \"&'6b - General Lighting'!H54&\" without OS and \"&'6b - General Lighting'!K54&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B55&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N55","v":0},{"$f":"\"The \"&'6b - General Lighting'!B55&\" LPD is \"&'6b - General Lighting'!I55","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B55&\" LPD is \"&'6b - General Lighting'!H55&\" without OS and \"&'6b - General Lighting'!K55&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B56&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N56","v":0},{"$f":"\"The \"&'6b - General Lighting'!B56&\" LPD is \"&'6b - General Lighting'!I56","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B56&\" LPD is \"&'6b - General Lighting'!H56&\" without OS and \"&'6b - General Lighting'!K56&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B57&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N57","v":0},{"$f":"\"The \"&'6b - General Lighting'!B57&\" LPD is \"&'6b - General Lighting'!I57","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B57&\" LPD is \"&'6b - General Lighting'!H57&\" without OS and \"&'6b - General Lighting'!K57&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B58&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N58","v":0},{"$f":"\"The \"&'6b - General Lighting'!B58&\" LPD is \"&'6b - General Lighting'!I58","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B58&\" LPD is \"&'6b - General Lighting'!H58&\" without OS and \"&'6b - General Lighting'!K58&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B59&\" LPD and OS\"","v":" LPD and OS"},{"$f":"'6b - General Lighting'!N59","v":0},{"$f":"\"The \"&'6b - General Lighting'!B59&\" LPD is \"&'6b - General Lighting'!I59","v":"The  LPD is -"},{"$f":"\"The \"&'6b - General Lighting'!B59&\" LPD is \"&'6b - General Lighting'!H59&\" without OS and \"&'6b - General Lighting'!K59&\" with OS.\"","v":"The  LPD is - without OS and - with OS."}]
[null,{"$f":"'6b - General Lighting'!B60&\" LPD and OS\"","v":"Total LPD and OS"},{"$f":"'6b - General Lighting'!N60","v":0},{"$f":"\"The \"&'6b - General Lighting'!B60&\" LPD is \"&ROUND('6b - General Lighting'!I60,3)","v":{"$error":"#VALUE!"}},{"$f":"\"The \"&'6b - General Lighting'!B60&\" LPD is \"&ROUND('6b - General Lighting'!H60,3)&\" without OS and \"&ROUND('6b - General Lighting'!K60,3)&\" with OS.\"","v":{"$error":"#VALUE!"}}]
[null,{"$f":"'6b - General Lighting'!B61&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B62&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B63&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B64&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B65&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B66&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B67&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B68&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B69&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B70&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B71&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B72&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B73&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B74&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B75&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B76&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B77&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B78&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B79&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B80&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B81&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B82&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B83&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B84&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B85&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B86&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B87&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B88&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B89&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B90&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B91&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B92&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B93&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B94&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B95&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B96&\" LPD and OS\"","v":" LPD and OS"}]
[null,{"$f":"'6b - General Lighting'!B97&\" LPD and OS\"","v":" LPD and OS"}]
[null,"Process Loads"]
[null,{"$f":"'7 - Process Loads'!V21","v":"Building Average Equipment Power Density"},{"$f":"'7 - Process Loads'!W21","v":"0"},{"$f":"'7 - Process Loads'!X21","v":"<User Entry>"},{"$f":"'7 - Process Loads'!Y21","v":" Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."}]
[null,{"$f":"'7 - Process Loads'!V22","v":"Building Average Equipment Power Density"},{"$f":"'7 - Process Loads'!W22","v":"0"},{"$f":"'7 - Process Loads'!X22","v":"<User Entry>"},{"$f":"'7 - Process Loads'!Y22","v":" Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."}]
[null,{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}}]
[null,{"$f":"'7 - Process Loads'!V23","v":"Building Average Equipment Power Density"},{"$f":"'7 - Process Loads'!W23","v":"0"},{"$f":"'7 - Process Loads'!X23","v":"<User Entry>"},{"$f":"'7 - Process Loads'!Y23","v":" Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."}]
[null,{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}}]
[null,{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}}]
[null,{"$f":"'7 - Process Loads'!V24","v":"Building Average Equipment Power Density"},{"$f":"'7 - Process Loads'!W24","v":"0"},{"$f":"'7 - Process Loads'!X24","v":"<User Entry>"},{"$f":"'7 - Process Loads'!Y24","v":" Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."}]
[null,{"$f":"'7 - Process Loads'!V25","v":0},{"$f":"'7 - Process Loads'!W25","v":0},{"$f":"'7 - Process Loads'!X25","v":0},{"$f":"'7 - Process Loads'!Y25","v":0}]
[null,{"$f":"'7 - Process Loads'!V26","v":0},{"$f":"'7 - Process Loads'!W26","v":0},{"$f":"'7 - Process Loads'!X26","v":0},{"$f":"'7 - Process Loads'!Y26","v":0}]
[null,{"$f":"'7 - Process Loads'!V34","v":"Space by Space Equipment Power Densities"},{"$f":"'7 - Process Loads'!W34","v":"0"},{"$f":"'7 - Process Loads'!X34","v":"<User Entry>"},{"$f":"'7 - Process Loads'!Y34","v":" Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."}]
[null,{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}}]
[null,{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}}]
[null,{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}}]
[null,{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}}]
[null,{"$f":"'7 - Process Loads'!V35","v":"Space by Space Equipment Power Densities"},{"$f":"'7 - Process Loads'!W35","v":"0"},{"$f":"'7 - Process Loads'!X35","v":"<User Entry>"},{"$f":"'7 - Process Loads'!Y35","v":" Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."}]
[null,{"$f":"'7 - Process Loads'!V36","v":"Space by Space Equipment Power Densities"},{"$f":"'7 - Process Loads'!W36","v":"0"},{"$f":"'7 - Process Loads'!X36","v":"<User Entry>"},{"$f":"'7 - Process Loads'!Y36","v":" Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."}]
[null,{"$f":"'7 - Process Loads'!V37","v":"Space by Space Equipment Power Densities"},{"$f":"'7 - Process Loads'!W37","v":"0"},{"$f":"'7 - Process Loads'!X37","v":"<User Entry>"},{"$f":"'7 - Process Loads'!Y37","v":" Building Type with total building area of  sqft, and EPD of  w/sf. The equipment in this EPD includes ."}]
[null,{"$f":"'7 - Process Loads'!V58","v":"Non-Receptacle Process Equipment"},{"$f":"'7 - Process Loads'!W58","v":"0"},{"$f":"'7 - Process Loads'!X58","v":"<User Entry>"},{"$f":"'7 - Process Loads'!Y58","v":"Non-Receptacle process equipment includes the following:  with an  energy source of  Btuh. The modeling parameters include: ."}]
[null,{"$f":"'7 - Process Loads'!V59","v":"Non-Receptacle Process Equipment"},{"$f":"'7 - Process Loads'!W59","v":"0"},{"$f":"'7 - Process Loads'!X59","v":"<User Entry>"},{"$f":"'7 - Process Loads'!Y59","v":"Non-Receptacle process equipment includes the following:  with an  energy source of  Btuh. The modeling parameters include: ."}]
[null,{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}}]
[null,{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}}]
[null,{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}}]
[null,{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}},{"$f":"'7 - Process Loads'!#REF!","v":{"$error":"#REF!"}}]
[null,{"$f":"'7 - Process Loads'!V60","v":"Non-Receptacle Process Equipment"},{"$f":"'7 - Process Loads'!W60","v":"0"},{"$f":"'7 - Process Loads'!X60","v":"<User Entry>"},{"$f":"'7 - Process Loads'!Y60","v":"Non-Receptacle process equipment includes the following:  with an  energy source of  Btuh. The modeling parameters include: ."}]
[null,{"$f":"'7 - Process Loads'!V61","v":"Non-Receptacle Process Equipment"},{"$f":"'7 - Process Loads'!W61","v":"0"},{"$f":"'7 - Process Loads'!X61","v":"<User Entry>"},{"$f":"'7 - Process Loads'!Y61","v":"Non-Receptacle process equipment includes the following:  with an  energy source of  Btuh. The modeling parameters include: ."}]
[null,{"$f":"'7 - Process Loads'!V62","v":0},{"$f":"'7 - Process Loads'!W62","v":0},{"$f":"'7 - Process Loads'!X62","v":0},{"$f":"'7 - Process Loads'!Y62","v":0}]
[null,{"$f":"'7 - Process Loads'!V63","v":0},{"$f":"'7 - Process Loads'!W63","v":0},{"$f":"'7 - Process Loads'!X63","v":0},{"$f":"'7 - Process Loads'!Y63","v":0}]
[null,"Service Water Heating"]
[null,{"$f":"'8 - Service Water Heating'!X14","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y14","v":0},{"$f":"'8 - Service Water Heating'!Z14","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA14","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X15","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y15","v":0},{"$f":"'8 - Service Water Heating'!Z15","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA15","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X16","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y16","v":0},{"$f":"'8 - Service Water Heating'!Z16","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA16","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X18","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y18","v":0},{"$f":"'8 - Service Water Heating'!Z18","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA18","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X19","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y19","v":0},{"$f":"'8 - Service Water Heating'!Z19","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA19","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X20","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y20","v":0},{"$f":"'8 - Service Water Heating'!Z20","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA20","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X22","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y22","v":0},{"$f":"'8 - Service Water Heating'!Z22","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA22","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X21","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y21","v":0},{"$f":"'8 - Service Water Heating'!Z21","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA21","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X23","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y23","v":0},{"$f":"'8 - Service Water Heating'!Z23","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA23","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X24","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y24","v":0},{"$f":"'8 - Service Water Heating'!Z24","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA24","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X25","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y25","v":0},{"$f":"'8 - Service Water Heating'!Z25","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA25","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X29","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y29","v":0},{"$f":"'8 - Service Water Heating'!Z29","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA29","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X31","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y31","v":0},{"$f":"'8 - Service Water Heating'!Z31","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA31","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X28","v":"Service Water Heaters"},{"$f":"'8 - Service Water Heating'!Y28","v":0},{"$f":"'8 - Service Water Heating'!Z28","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is - (F) with a peak hot water demand of . Condenser heat recovery: -. There are -  pump(s) woth a total pump power of Yes kW."},{"$f":"'8 - Service Water Heating'!AA28","v":"SWH building area type based on:  with an   system with  fuel. The input rating is  with an efficiency of . The storage temperature is  (F) with a peak hot water demand of . Condenser heat recovery: . There are   pump(s) woth a total pump power of 0 kW."}]
[null,{"$f":"'8 - Service Water Heating'!X33","v":0},{"$f":"'8 - Service Water Heating'!Y33","v":0},{"$f":"'8 - Service Water Heating'!Z33","v":0},{"$f":"'8 - Service Water Heating'!AA33","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X34","v":0},{"$f":"'8 - Service Water Heating'!Y34","v":0},{"$f":"'8 - Service Water Heating'!Z34","v":0},{"$f":"'8 - Service Water Heating'!AA34","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X35","v":0},{"$f":"'8 - Service Water Heating'!Y35","v":0},{"$f":"'8 - Service Water Heating'!Z35","v":0},{"$f":"'8 - Service Water Heating'!AA35","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X36","v":0},{"$f":"'8 - Service Water Heating'!Y36","v":0},{"$f":"'8 - Service Water Heating'!Z36","v":0},{"$f":"'8 - Service Water Heating'!AA36","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X37","v":0},{"$f":"'8 - Service Water Heating'!Y37","v":0},{"$f":"'8 - Service Water Heating'!Z37","v":0},{"$f":"'8 - Service Water Heating'!AA37","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X38","v":0},{"$f":"'8 - Service Water Heating'!Y38","v":0},{"$f":"'8 - Service Water Heating'!Z38","v":0},{"$f":"'8 - Service Water Heating'!AA38","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X39","v":0},{"$f":"'8 - Service Water Heating'!Y39","v":0},{"$f":"'8 - Service Water Heating'!Z39","v":0},{"$f":"'8 - Service Water Heating'!AA39","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X40","v":0},{"$f":"'8 - Service Water Heating'!Y40","v":0},{"$f":"'8 - Service Water Heating'!Z40","v":0},{"$f":"'8 - Service Water Heating'!AA40","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X41","v":0},{"$f":"'8 - Service Water Heating'!Y41","v":0},{"$f":"'8 - Service Water Heating'!Z41","v":0},{"$f":"'8 - Service Water Heating'!AA41","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X42","v":0},{"$f":"'8 - Service Water Heating'!Y42","v":0},{"$f":"'8 - Service Water Heating'!Z42","v":0},{"$f":"'8 - Service Water Heating'!AA42","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X43","v":0},{"$f":"'8 - Service Water Heating'!Y43","v":0},{"$f":"'8 - Service Water Heating'!Z43","v":0},{"$f":"'8 - Service Water Heating'!AA43","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X44","v":0},{"$f":"'8 - Service Water Heating'!Y44","v":0},{"$f":"'8 - Service Water Heating'!Z44","v":0},{"$f":"'8 - Service Water Heating'!AA44","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X45","v":0},{"$f":"'8 - Service Water Heating'!Y45","v":0},{"$f":"'8 - Service Water Heating'!Z45","v":0},{"$f":"'8 - Service Water Heating'!AA45","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X46","v":0},{"$f":"'8 - Service Water Heating'!Y46","v":0},{"$f":"'8 - Service Water Heating'!Z46","v":0},{"$f":"'8 - Service Water Heating'!AA46","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X47","v":"Low-Flow Fixtures"},{"$f":"'8 - Service Water Heating'!Y47","v":0},{"$f":"'8 - Service Water Heating'!Z47","v":"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year."},{"$f":"'8 - Service Water Heating'!AA47","v":"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year."}]
[null,{"$f":"'8 - Service Water Heating'!X48","v":"Low-Flow Fixtures"},{"$f":"'8 - Service Water Heating'!Y48","v":0},{"$f":"'8 - Service Water Heating'!Z48","v":"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year."},{"$f":"'8 - Service Water Heating'!AA48","v":"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year."}]
[null,{"$f":"'8 - Service Water Heating'!X49","v":"Low-Flow Fixtures"},{"$f":"'8 - Service Water Heating'!Y49","v":0},{"$f":"'8 - Service Water Heating'!Z49","v":"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year."},{"$f":"'8 - Service Water Heating'!AA49","v":"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year."}]
[null,{"$f":"'8 - Service Water Heating'!X50","v":"Low-Flow Fixtures"},{"$f":"'8 - Service Water Heating'!Y50","v":0},{"$f":"'8 - Service Water Heating'!Z50","v":"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year."},{"$f":"'8 - Service Water Heating'!AA50","v":"Fixtrue type of  with fixture outlet temperature of  (F) and (/1) % hot water. The  has a flow rate of  gpm with annual total water consumption of  gallons/year."}]
[null,{"$f":"'8 - Service Water Heating'!X51","v":0},{"$f":"'8 - Service Water Heating'!Y51","v":0},{"$f":"'8 - Service Water Heating'!Z51","v":0},{"$f":"'8 - Service Water Heating'!AA51","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X52","v":0},{"$f":"'8 - Service Water Heating'!Y52","v":0},{"$f":"'8 - Service Water Heating'!Z52","v":0},{"$f":"'8 - Service Water Heating'!AA52","v":0}]
[null,{"$f":"'8 - Service Water Heating'!X57","v":"Low-Flow Fixture Summary"},{"$f":"'8 - Service Water Heating'!Y57","v":0},{"$f":"'8 - Service Water Heating'!Z57","v":"Low flow fixture total modeled DHW flow rate is  gallons/minute with total annual hot water consumption st fixtures of 0 gallons/year. The total annual DHW heater consumption is  gallons/year."},{"$f":"'8 - Service Water Heating'!AA57","v":"Low flow fixture total modeled DHW flow rate is  gallons/minute with total annual hot water consumption st fixtures of 0 gallons/year. The total annual DHW heater consumption is  gallons/year."}]
[null,"Water-Side HVAC"]
[null,{"$f":"'11 - Water-Side HVAC'!S11","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T11","v":0},{"$f":"'11 - Water-Side HVAC'!U11","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V11","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S12","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T12","v":0},{"$f":"'11 - Water-Side HVAC'!U12","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V12","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S13","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T13","v":0},{"$f":"'11 - Water-Side HVAC'!U13","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V13","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S14","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T14","v":0},{"$f":"'11 - Water-Side HVAC'!U14","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V14","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S15","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T15","v":0},{"$f":"'11 - Water-Side HVAC'!U15","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V15","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S16","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T16","v":0},{"$f":"'11 - Water-Side HVAC'!U16","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V16","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S17","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T17","v":0},{"$f":"'11 - Water-Side HVAC'!U17","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V17","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S18","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T18","v":0},{"$f":"'11 - Water-Side HVAC'!U18","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V18","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S19","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T19","v":0},{"$f":"'11 - Water-Side HVAC'!U19","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V19","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S20","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T20","v":0},{"$f":"'11 - Water-Side HVAC'!U20","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V20","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S21","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T21","v":0},{"$f":"'11 - Water-Side HVAC'!U21","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V21","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S22","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T22","v":0},{"$f":"'11 - Water-Side HVAC'!U22","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V22","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S23","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T23","v":0},{"$f":"'11 - Water-Side HVAC'!U23","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V23","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S24","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T24","v":0},{"$f":"'11 - Water-Side HVAC'!U24","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V24","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S25","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T25","v":0},{"$f":"'11 - Water-Side HVAC'!U25","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V25","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S26","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T26","v":0},{"$f":"'11 - Water-Side HVAC'!U26","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V26","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S27","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T27","v":0},{"$f":"'11 - Water-Side HVAC'!U27","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V27","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S28","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T28","v":0},{"$f":"'11 - Water-Side HVAC'!U28","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V28","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S29","v":"Chilled Water"},{"$f":"'11 - Water-Side HVAC'!T29","v":0},{"$f":"'11 - Water-Side HVAC'!U29","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."},{"$f":"'11 - Water-Side HVAC'!V29","v":" chiller(s) with capacity of  tons and efficiency of  FL kW/Ton and  IPLV (kW/Ton). This is a  CHW loop configuration with  CHW pumps with pump power of  kW and pump flow of  gpm with , pump control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S35","v":"Cooling Tower and Condenser Water"},{"$f":"'11 - Water-Side HVAC'!T35","v":0},{"$f":"'11 - Water-Side HVAC'!U35","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"'11 - Water-Side HVAC'!V35","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S36","v":"Cooling Tower and Condenser Water"},{"$f":"'11 - Water-Side HVAC'!T36","v":0},{"$f":"'11 - Water-Side HVAC'!U36","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"'11 - Water-Side HVAC'!V36","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S37","v":"Cooling Tower and Condenser Water"},{"$f":"'11 - Water-Side HVAC'!T37","v":0},{"$f":"'11 - Water-Side HVAC'!U37","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"'11 - Water-Side HVAC'!V37","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S38","v":"Cooling Tower and Condenser Water"},{"$f":"'11 - Water-Side HVAC'!T38","v":0},{"$f":"'11 - Water-Side HVAC'!U38","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"'11 - Water-Side HVAC'!V38","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S39","v":"Cooling Tower and Condenser Water"},{"$f":"'11 - Water-Side HVAC'!T39","v":0},{"$f":"'11 - Water-Side HVAC'!U39","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"'11 - Water-Side HVAC'!V39","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S40","v":"Cooling Tower and Condenser Water"},{"$f":"'11 - Water-Side HVAC'!T40","v":0},{"$f":"'11 - Water-Side HVAC'!U40","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"'11 - Water-Side HVAC'!V40","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S41","v":"Cooling Tower and Condenser Water"},{"$f":"'11 - Water-Side HVAC'!T41","v":0},{"$f":"'11 - Water-Side HVAC'!U41","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"'11 - Water-Side HVAC'!V41","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S42","v":"Cooling Tower and Condenser Water"},{"$f":"'11 - Water-Side HVAC'!T42","v":0},{"$f":"'11 - Water-Side HVAC'!U42","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"'11 - Water-Side HVAC'!V42","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S43","v":"Cooling Tower and Condenser Water"},{"$f":"'11 - Water-Side HVAC'!T43","v":0},{"$f":"'11 - Water-Side HVAC'!U43","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"'11 - Water-Side HVAC'!V43","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S44","v":"Cooling Tower and Condenser Water"},{"$f":"'11 - Water-Side HVAC'!T44","v":0},{"$f":"'11 - Water-Side HVAC'!U44","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."},{"$f":"'11 - Water-Side HVAC'!V44","v":" Cooling tower(s), or fluid cooler(s), with fan power of  kW and  control. The CW leaving temperature is  (F) with a CW dela T of  (F) and reset parameters include: . There are  CW pump with pump power of  kW, pump flow of  gpm and  control."}]
[null,{"$f":"'11 - Water-Side HVAC'!S49","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T49","v":0},{"$f":"'11 - Water-Side HVAC'!U49","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V49","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S50","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T50","v":0},{"$f":"'11 - Water-Side HVAC'!U50","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V50","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S51","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T51","v":0},{"$f":"'11 - Water-Side HVAC'!U51","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V51","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S52","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T52","v":0},{"$f":"'11 - Water-Side HVAC'!U52","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V52","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S53","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T53","v":0},{"$f":"'11 - Water-Side HVAC'!U53","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V53","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S54","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T54","v":0},{"$f":"'11 - Water-Side HVAC'!U54","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V54","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S55","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T55","v":0},{"$f":"'11 - Water-Side HVAC'!U55","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V55","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S56","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T56","v":0},{"$f":"'11 - Water-Side HVAC'!U56","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V56","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S57","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T57","v":0},{"$f":"'11 - Water-Side HVAC'!U57","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V57","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S58","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T58","v":0},{"$f":"'11 - Water-Side HVAC'!U58","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V58","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S59","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T59","v":0},{"$f":"'11 - Water-Side HVAC'!U59","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V59","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S60","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T60","v":0},{"$f":"'11 - Water-Side HVAC'!U60","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V60","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S61","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T61","v":0},{"$f":"'11 - Water-Side HVAC'!U61","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V61","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S62","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T62","v":0},{"$f":"'11 - Water-Side HVAC'!U62","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V62","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S63","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T63","v":0},{"$f":"'11 - Water-Side HVAC'!U63","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V63","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S64","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T64","v":0},{"$f":"'11 - Water-Side HVAC'!U64","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V64","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S65","v":"Hot Water or Steam"},{"$f":"'11 - Water-Side HVAC'!T65","v":0},{"$f":"'11 - Water-Side HVAC'!U65","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."},{"$f":"'11 - Water-Side HVAC'!V65","v":" with capacity of  MBH and efficiency of . The HHW supply temp is  (F) with a HHW delta T of  (F). The HHW temp reset parameters are as follows: . The HHW loop configuration is  with  pump(s) with pump power of  kW and pump flow of  gpm. The pump conrol is ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S70","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T70","v":0},{"$f":"'11 - Water-Side HVAC'!U70","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V70","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S71","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T71","v":0},{"$f":"'11 - Water-Side HVAC'!U71","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V71","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S72","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T72","v":0},{"$f":"'11 - Water-Side HVAC'!U72","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V72","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S73","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T73","v":0},{"$f":"'11 - Water-Side HVAC'!U73","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V73","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S74","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T74","v":0},{"$f":"'11 - Water-Side HVAC'!U74","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V74","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S75","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T75","v":0},{"$f":"'11 - Water-Side HVAC'!U75","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V75","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S76","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T76","v":0},{"$f":"'11 - Water-Side HVAC'!U76","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V76","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S77","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T77","v":0},{"$f":"'11 - Water-Side HVAC'!U77","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V77","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S78","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T78","v":0},{"$f":"'11 - Water-Side HVAC'!U78","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V78","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S79","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T79","v":0},{"$f":"'11 - Water-Side HVAC'!U79","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V79","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S80","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T80","v":0},{"$f":"'11 - Water-Side HVAC'!U80","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V80","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S81","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T81","v":0},{"$f":"'11 - Water-Side HVAC'!U81","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V81","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S82","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T82","v":0},{"$f":"'11 - Water-Side HVAC'!U82","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V82","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S83","v":"Geothermal Loop"},{"$f":"'11 - Water-Side HVAC'!T83","v":0},{"$f":"'11 - Water-Side HVAC'!U83","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V83","v":" geothermal system with the following parameters: Soil conductivity (if applicable): , Geothermal source design temperature - summer:  (F), Geothermal source design temperature - winter:  (F), Geoexchange loop design fluid supply temperature - cooling:  (F), Geoexchange loop design fluid supply temperature -heating:  (F), Geoexchange loop - operating temperature:  (F), Geothermal energy transfer effect: , Geothermal loop pumping configuration: , Number of geothermal loop pumps: , Geothermal loop pump control: , Geothermal pump power : , Geothermal loop flow: , Geothermal air-side efficiency curves: ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S88","v":"Combined Heat and Power (CHP)"},{"$f":"'11 - Water-Side HVAC'!T88","v":0},{"$f":"'11 - Water-Side HVAC'!U88","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V88","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S89","v":"Combined Heat and Power (CHP)"},{"$f":"'11 - Water-Side HVAC'!T89","v":0},{"$f":"'11 - Water-Side HVAC'!U89","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V89","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S90","v":"Combined Heat and Power (CHP)"},{"$f":"'11 - Water-Side HVAC'!T90","v":0},{"$f":"'11 - Water-Side HVAC'!U90","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V90","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S91","v":"Combined Heat and Power (CHP)"},{"$f":"'11 - Water-Side HVAC'!T91","v":0},{"$f":"'11 - Water-Side HVAC'!U91","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V91","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S92","v":"Combined Heat and Power (CHP)"},{"$f":"'11 - Water-Side HVAC'!T92","v":0},{"$f":"'11 - Water-Side HVAC'!U92","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V92","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S93","v":"Combined Heat and Power (CHP)"},{"$f":"'11 - Water-Side HVAC'!T93","v":0},{"$f":"'11 - Water-Side HVAC'!U93","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V93","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S94","v":"Combined Heat and Power (CHP)"},{"$f":"'11 - Water-Side HVAC'!T94","v":0},{"$f":"'11 - Water-Side HVAC'!U94","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V94","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S95","v":"Combined Heat and Power (CHP)"},{"$f":"'11 - Water-Side HVAC'!T95","v":0},{"$f":"'11 - Water-Side HVAC'!U95","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V95","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S96","v":"Combined Heat and Power (CHP)"},{"$f":"'11 - Water-Side HVAC'!T96","v":0},{"$f":"'11 - Water-Side HVAC'!U96","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V96","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]
[null,{"$f":"'11 - Water-Side HVAC'!S97","v":"Combined Heat and Power (CHP)"},{"$f":"'11 - Water-Side HVAC'!T97","v":0},{"$f":"'11 - Water-Side HVAC'!U97","v":"<User Entry>"},{"$f":"'11 - Water-Side HVAC'!V97","v":" generator with the following parameters: Quantity of CHP generators: , Total capacity of CHP generators (kW) at design conditions: , Thermal efficiency (%) at design conditions: , Electrical efficiency (%) at design conditions: , Controls or schedule: , Fuel Source: , Where is the recovered heat used? (e.g. gas absorption chillers, hot water distribution loop, etc.): , Backup heat source when waste heat from CHP is unavailable? (e.g. fossil fuel boilers): , Parasitic losses (e.g. air handling unit to cool the intake air): ."}]

{"sheet":"Detailed Measures","index":31,"n_rows":42,"n_cols":22,"rows_kept":42,"cut":false,"hidden":false,"merged":[[4,1,4,4],[9,7,9,10],[9,11,9,12],[5,1,5,3]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'General Information'!C40","v":"eQuest"},"Units"]
["(OPTIONAL) Detailed Measures",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1000 Btu/hr"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CFM"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"each"]
[null,"Instructions: This tab is optional. The Baseline and Proposed details of the modeled Measures are reported in this tab. All grey cells in columns C:E of this tab are initially filled out with automated descriptions based on the inputs in this template (for eQUEST users). These cells are able to be edited by the user. If additional information needs to be added to the automated description, please copy the cell and paste values in the same cell, before editing text. If a value is edited and you would like to go back to the automated description, click the \"Automate\" button. Some descriptions will need to be filled out manually by the user.\n\neQUEST USERS: Please fill out 'Results from eQUEST' tab prior to starting the 'Detailed Measures' tab to enable functionality. Be sure all measures #'s are noted in previous support tabs. Manually enter Parametric Run description in columns D:E where \"<Enter Description Here>\" is noted. \n\nNon-eQUEST Users: Enter all measures #'s in previous support tabs. Parametric Run descriptions will need to manually entered in columns D:E, as well as the Incremental Energy Savings in columns H:K.\n\nPlease delete any cells associated with penalty measures, and hide rows that are blank.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SqFt"]
[null,"Fuel Cost: Please enter the fuel costs below.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tons"]
[null,null,{"$f":"IFERROR(AVERAGEIF('12 - Performance_Outputs_1'!B282:B287,\"Electricity\",'12 - Performance_Outputs_1'!E282:J287),\"\")","v":""},"$/kWh Electricity"]
[null,null,{"$f":"IFERROR(AVERAGEIF('12 - Performance_Outputs_1'!B282:B287,\"Natural Gas\",'12 - Performance_Outputs_1'!E282:J287),\"\")","v":""},"$/Therm Natural Gas"]
[null,null,null,"$/ 1000 Gallons Water"]
[null,null,{"$f":"IF(C9=\"\",\"Please enter value.\",\"\")","v":"Please enter value."},null,null,null,null,"Incremental Energy savings",null,null,null,"Incremental Metrics"]
[null,"Measure #","Parametric Run","Baseline Description","Proposed Design Description","Quantity","Units","Total Electric kWh","Total Non-Electric MMBtu","Heating MMBtu (Non-Electric Only)","Cooling kWh (Electric Only)","Water Savings 1000 gal","Total Cost Savings (S)",null,null,"Baseline Description","Proposed Description",null,"Baseline Description","Proposed Description"]
[null,1,{"$f":"IF('Results from eQuest'!J16=\"\",\"\",'Results from eQuest'!J16)","v":""},{"$f":"P12","v":""},{"$f":"Q12","v":""},null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C12=\"\",\"\",IFERROR(IF(C12=\"\",\"-\",(('Results from eQuest'!X15)-('Results from eQuest'!X16))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C12=\"\",\"\",IFERROR(IF(C12=\"\",\"-\",(('Results from eQuest'!BJ12)-('Results from eQuest'!BJ16))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C12=\"\",\"\",IF(C12=\"\",\"-\",(('Results from eQuest'!BA12+'Results from eQuest'!BG12)/10-('Results from eQuest'!BA16+'Results from eQuest'!BG16)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C12=\"\",\"\",IFERROR(IF(C12=\"\",\"-\",(('Results from eQuest'!P12+'Results from eQuest'!Q12)-('Results from eQuest'!P16+'Results from eQuest'!Q16))),\"-\")),\"<Enter Value>\")","v":""},null,{"$f":"IF(C12=\"\",\"\",$C$7*H12+$C$8*I12*10+$C$9*L12)","v":""},null,null,{"$f":"IF(C12=\"\",\"\",S12)","v":""},{"$f":"IF(C12=\"\",\"\",T12)","v":""},null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B12,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B12,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,2,{"$f":"IF('Results from eQuest'!J17=\"\",\"\",'Results from eQuest'!J17)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C13=\"\",\"\",IFERROR(IF(C13=\"\",\"-\",(('Results from eQuest'!X16)-('Results from eQuest'!X17))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C13=\"\",\"\",IFERROR(IF(C13=\"\",\"-\",(('Results from eQuest'!BJ16)-('Results from eQuest'!BJ17))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C13=\"\",\"\",IF(C13=\"\",\"-\",(('Results from eQuest'!BA16+'Results from eQuest'!BG16)/10-('Results from eQuest'!BA17+'Results from eQuest'!BG17)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C13=\"\",\"\",IFERROR(IF(C13=\"\",\"-\",(('Results from eQuest'!P16+'Results from eQuest'!Q16)-('Results from eQuest'!P17+'Results from eQuest'!Q17))),\"-\")),\"<Enter Value>\")","v":""},null,{"$f":"IF(C13=\"\",\"\",$C$7*H13+$C$8*I13*10+$C$9*L13)","v":""},null,null,{"$f":"IF(C13=\"\",\"\",S13)","v":""},{"$f":"IF(C13=\"\",\"\",T13)","v":""},null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B13,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B13,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,3,{"$f":"IF('Results from eQuest'!J18=\"\",\"\",'Results from eQuest'!J18)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C14=\"\",\"\",IFERROR(IF(C14=\"\",\"-\",(('Results from eQuest'!X17)-('Results from eQuest'!X18))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C14=\"\",\"\",IFERROR(IF(C14=\"\",\"-\",(('Results from eQuest'!BJ17)-('Results from eQuest'!BJ18))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C14=\"\",\"\",IF(C14=\"\",\"-\",(('Results from eQuest'!BA17+'Results from eQuest'!BG17)/10-('Results from eQuest'!BA18+'Results from eQuest'!BG18)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C14=\"\",\"\",IFERROR(IF(C14=\"\",\"-\",(('Results from eQuest'!P17+'Results from eQuest'!Q17)-('Results from eQuest'!P18+'Results from eQuest'!Q18))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B14,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B14,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,4,{"$f":"IF('Results from eQuest'!J19=\"\",\"\",'Results from eQuest'!J19)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C15=\"\",\"\",IFERROR(IF(C15=\"\",\"-\",(('Results from eQuest'!X18)-('Results from eQuest'!X19))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C15=\"\",\"\",IFERROR(IF(C15=\"\",\"-\",(('Results from eQuest'!BJ18)-('Results from eQuest'!BJ19))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C15=\"\",\"\",IF(C15=\"\",\"-\",(('Results from eQuest'!BA18+'Results from eQuest'!BG18)/10-('Results from eQuest'!BA19+'Results from eQuest'!BG19)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C15=\"\",\"\",IFERROR(IF(C15=\"\",\"-\",(('Results from eQuest'!P18+'Results from eQuest'!Q18)-('Results from eQuest'!P19+'Results from eQuest'!Q19))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B15,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B15,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,5,{"$f":"IF('Results from eQuest'!J20=\"\",\"\",'Results from eQuest'!J20)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C16=\"\",\"\",IFERROR(IF(C16=\"\",\"-\",(('Results from eQuest'!X19)-('Results from eQuest'!X20))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C16=\"\",\"\",IFERROR(IF(C16=\"\",\"-\",(('Results from eQuest'!BJ19)-('Results from eQuest'!BJ20))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C16=\"\",\"\",IF(C16=\"\",\"-\",(('Results from eQuest'!BA19+'Results from eQuest'!BG19)/10-('Results from eQuest'!BA20+'Results from eQuest'!BG20)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C16=\"\",\"\",IFERROR(IF(C16=\"\",\"-\",(('Results from eQuest'!P19+'Results from eQuest'!Q19)-('Results from eQuest'!P20+'Results from eQuest'!Q20))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B16,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B16,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,6,{"$f":"IF('Results from eQuest'!J21=\"\",\"\",'Results from eQuest'!J21)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C17=\"\",\"\",IFERROR(IF(C17=\"\",\"-\",(('Results from eQuest'!X20)-('Results from eQuest'!X21))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C17=\"\",\"\",IFERROR(IF(C17=\"\",\"-\",(('Results from eQuest'!BJ20)-('Results from eQuest'!BJ21))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C17=\"\",\"\",IF(C17=\"\",\"-\",(('Results from eQuest'!BA20+'Results from eQuest'!BG20)/10-('Results from eQuest'!BA21+'Results from eQuest'!BG21)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C17=\"\",\"\",IFERROR(IF(C17=\"\",\"-\",(('Results from eQuest'!P20+'Results from eQuest'!Q20)-('Results from eQuest'!P21+'Results from eQuest'!Q21))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B17,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B17,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,7,{"$f":"IF('Results from eQuest'!J22=\"\",\"\",'Results from eQuest'!J22)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C18=\"\",\"\",IFERROR(IF(C18=\"\",\"-\",(('Results from eQuest'!X21)-('Results from eQuest'!X22))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C18=\"\",\"\",IFERROR(IF(C18=\"\",\"-\",(('Results from eQuest'!BJ21)-('Results from eQuest'!BJ22))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C18=\"\",\"\",IF(C18=\"\",\"-\",(('Results from eQuest'!BA21+'Results from eQuest'!BG21)/10-('Results from eQuest'!BA22+'Results from eQuest'!BG22)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C18=\"\",\"\",IFERROR(IF(C18=\"\",\"-\",(('Results from eQuest'!P21+'Results from eQuest'!Q21)-('Results from eQuest'!P22+'Results from eQuest'!Q22))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B18,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B18,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,8,{"$f":"IF('Results from eQuest'!J23=\"\",\"\",'Results from eQuest'!J23)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C19=\"\",\"\",IFERROR(IF(C19=\"\",\"-\",(('Results from eQuest'!X22)-('Results from eQuest'!X23))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C19=\"\",\"\",IFERROR(IF(C19=\"\",\"-\",(('Results from eQuest'!BJ22)-('Results from eQuest'!BJ23))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C19=\"\",\"\",IF(C19=\"\",\"-\",(('Results from eQuest'!BA22+'Results from eQuest'!BG22)/10-('Results from eQuest'!BA23+'Results from eQuest'!BG23)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C19=\"\",\"\",IFERROR(IF(C19=\"\",\"-\",(('Results from eQuest'!P22+'Results from eQuest'!Q22)-('Results from eQuest'!P23+'Results from eQuest'!Q23))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B19,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B19,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,9,{"$f":"IF('Results from eQuest'!J24=\"\",\"\",'Results from eQuest'!J24)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C20=\"\",\"\",IFERROR(IF(C20=\"\",\"-\",(('Results from eQuest'!X23)-('Results from eQuest'!X24))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C20=\"\",\"\",IFERROR(IF(C20=\"\",\"-\",(('Results from eQuest'!BJ23)-('Results from eQuest'!BJ24))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C20=\"\",\"\",IF(C20=\"\",\"-\",(('Results from eQuest'!BA23+'Results from eQuest'!BG23)/10-('Results from eQuest'!BA24+'Results from eQuest'!BG24)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C20=\"\",\"\",IFERROR(IF(C20=\"\",\"-\",(('Results from eQuest'!P23+'Results from eQuest'!Q23)-('Results from eQuest'!P24+'Results from eQuest'!Q24))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B20,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B20,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,10,{"$f":"IF('Results from eQuest'!J25=\"\",\"\",'Results from eQuest'!J25)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C21=\"\",\"\",IFERROR(IF(C21=\"\",\"-\",(('Results from eQuest'!X24)-('Results from eQuest'!X25))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C21=\"\",\"\",IFERROR(IF(C21=\"\",\"-\",(('Results from eQuest'!BJ24)-('Results from eQuest'!BJ25))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C21=\"\",\"\",IF(C21=\"\",\"-\",(('Results from eQuest'!BA24+'Results from eQuest'!BG24)/10-('Results from eQuest'!BA25+'Results from eQuest'!BG25)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C21=\"\",\"\",IFERROR(IF(C21=\"\",\"-\",(('Results from eQuest'!P24+'Results from eQuest'!Q24)-('Results from eQuest'!P25+'Results from eQuest'!Q25))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B21,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B21,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,11,{"$f":"IF('Results from eQuest'!J26=\"\",\"\",'Results from eQuest'!J26)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C22=\"\",\"\",IFERROR(IF(C22=\"\",\"-\",(('Results from eQuest'!X25)-('Results from eQuest'!X26))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C22=\"\",\"\",IFERROR(IF(C22=\"\",\"-\",(('Results from eQuest'!BJ25)-('Results from eQuest'!BJ26))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C22=\"\",\"\",IF(C22=\"\",\"-\",(('Results from eQuest'!BA25+'Results from eQuest'!BG25)/10-('Results from eQuest'!BA26+'Results from eQuest'!BG26)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C22=\"\",\"\",IFERROR(IF(C22=\"\",\"-\",(('Results from eQuest'!P25+'Results from eQuest'!Q25)-('Results from eQuest'!P26+'Results from eQuest'!Q26))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B22,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B22,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,12,{"$f":"IF('Results from eQuest'!J27=\"\",\"\",'Results from eQuest'!J27)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C23=\"\",\"\",IFERROR(IF(C23=\"\",\"-\",(('Results from eQuest'!X26)-('Results from eQuest'!X27))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C23=\"\",\"\",IFERROR(IF(C23=\"\",\"-\",(('Results from eQuest'!BJ26)-('Results from eQuest'!BJ27))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C23=\"\",\"\",IF(C23=\"\",\"-\",(('Results from eQuest'!BA26+'Results from eQuest'!BG26)/10-('Results from eQuest'!BA27+'Results from eQuest'!BG27)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C23=\"\",\"\",IFERROR(IF(C23=\"\",\"-\",(('Results from eQuest'!P26+'Results from eQuest'!Q26)-('Results from eQuest'!P27+'Results from eQuest'!Q27))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B23,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B23,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,13,{"$f":"IF('Results from eQuest'!J28=\"\",\"\",'Results from eQuest'!J28)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C24=\"\",\"\",IFERROR(IF(C24=\"\",\"-\",(('Results from eQuest'!X27)-('Results from eQuest'!X28))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C24=\"\",\"\",IFERROR(IF(C24=\"\",\"-\",(('Results from eQuest'!BJ27)-('Results from eQuest'!BJ28))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C24=\"\",\"\",IF(C24=\"\",\"-\",(('Results from eQuest'!BA27+'Results from eQuest'!BG27)/10-('Results from eQuest'!BA28+'Results from eQuest'!BG28)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C24=\"\",\"\",IFERROR(IF(C24=\"\",\"-\",(('Results from eQuest'!P27+'Results from eQuest'!Q27)-('Results from eQuest'!P28+'Results from eQuest'!Q28))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B24,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B24,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,14,{"$f":"IF('Results from eQuest'!J29=\"\",\"\",'Results from eQuest'!J29)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C25=\"\",\"\",IFERROR(IF(C25=\"\",\"-\",(('Results from eQuest'!X28)-('Results from eQuest'!X29))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C25=\"\",\"\",IFERROR(IF(C25=\"\",\"-\",(('Results from eQuest'!BJ28)-('Results from eQuest'!BJ29))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C25=\"\",\"\",IF(C25=\"\",\"-\",(('Results from eQuest'!BA28+'Results from eQuest'!BG28)/10-('Results from eQuest'!BA29+'Results from eQuest'!BG29)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C25=\"\",\"\",IFERROR(IF(C25=\"\",\"-\",(('Results from eQuest'!P28+'Results from eQuest'!Q28)-('Results from eQuest'!P29+'Results from eQuest'!Q29))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B25,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B25,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,15,{"$f":"IF('Results from eQuest'!J30=\"\",\"\",'Results from eQuest'!J30)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C26=\"\",\"\",IFERROR(IF(C26=\"\",\"-\",(('Results from eQuest'!X29)-('Results from eQuest'!X30))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C26=\"\",\"\",IFERROR(IF(C26=\"\",\"-\",(('Results from eQuest'!BJ29)-('Results from eQuest'!BJ30))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C26=\"\",\"\",IF(C26=\"\",\"-\",(('Results from eQuest'!BA29+'Results from eQuest'!BG29)/10-('Results from eQuest'!BA30+'Results from eQuest'!BG30)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C26=\"\",\"\",IFERROR(IF(C26=\"\",\"-\",(('Results from eQuest'!P29+'Results from eQuest'!Q29)-('Results from eQuest'!P30+'Results from eQuest'!Q30))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B26,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B26,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,16,{"$f":"IF('Results from eQuest'!J31=\"\",\"\",'Results from eQuest'!J31)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C27=\"\",\"\",IFERROR(IF(C27=\"\",\"-\",(('Results from eQuest'!X30)-('Results from eQuest'!X31))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C27=\"\",\"\",IFERROR(IF(C27=\"\",\"-\",(('Results from eQuest'!BJ30)-('Results from eQuest'!BJ31))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C27=\"\",\"\",IF(C27=\"\",\"-\",(('Results from eQuest'!BA30+'Results from eQuest'!BG30)/10-('Results from eQuest'!BA31+'Results from eQuest'!BG31)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C27=\"\",\"\",IFERROR(IF(C27=\"\",\"-\",(('Results from eQuest'!P30+'Results from eQuest'!Q30)-('Results from eQuest'!P31+'Results from eQuest'!Q31))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B27,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B27,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,17,{"$f":"IF('Results from eQuest'!J32=\"\",\"\",'Results from eQuest'!J32)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C28=\"\",\"\",IFERROR(IF(C28=\"\",\"-\",(('Results from eQuest'!X31)-('Results from eQuest'!X32))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C28=\"\",\"\",IFERROR(IF(C28=\"\",\"-\",(('Results from eQuest'!BJ31)-('Results from eQuest'!BJ32))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C28=\"\",\"\",IF(C28=\"\",\"-\",(('Results from eQuest'!BA31+'Results from eQuest'!BG31)/10-('Results from eQuest'!BA32+'Results from eQuest'!BG32)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C28=\"\",\"\",IFERROR(IF(C28=\"\",\"-\",(('Results from eQuest'!P31+'Results from eQuest'!Q31)-('Results from eQuest'!P32+'Results from eQuest'!Q32))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B28,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B28,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,18,{"$f":"IF('Results from eQuest'!J33=\"\",\"\",'Results from eQuest'!J33)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C29=\"\",\"\",IFERROR(IF(C29=\"\",\"-\",(('Results from eQuest'!X32)-('Results from eQuest'!X33))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C29=\"\",\"\",IFERROR(IF(C29=\"\",\"-\",(('Results from eQuest'!BJ32)-('Results from eQuest'!BJ33))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C29=\"\",\"\",IF(C29=\"\",\"-\",(('Results from eQuest'!BA32+'Results from eQuest'!BG32)/10-('Results from eQuest'!BA33+'Results from eQuest'!BG33)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C29=\"\",\"\",IFERROR(IF(C29=\"\",\"-\",(('Results from eQuest'!P32+'Results from eQuest'!Q32)-('Results from eQuest'!P33+'Results from eQuest'!Q33))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B29,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B29,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,19,{"$f":"IF('Results from eQuest'!J34=\"\",\"\",'Results from eQuest'!J34)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C30=\"\",\"\",IFERROR(IF(C30=\"\",\"-\",(('Results from eQuest'!X33)-('Results from eQuest'!X34))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C30=\"\",\"\",IFERROR(IF(C30=\"\",\"-\",(('Results from eQuest'!BJ33)-('Results from eQuest'!BJ34))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C30=\"\",\"\",IF(C30=\"\",\"-\",(('Results from eQuest'!BA33+'Results from eQuest'!BG33)/10-('Results from eQuest'!BA34+'Results from eQuest'!BG34)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C30=\"\",\"\",IFERROR(IF(C30=\"\",\"-\",(('Results from eQuest'!P33+'Results from eQuest'!Q33)-('Results from eQuest'!P34+'Results from eQuest'!Q34))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B30,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B30,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,20,{"$f":"IF('Results from eQuest'!J35=\"\",\"\",'Results from eQuest'!J35)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C31=\"\",\"\",IFERROR(IF(C31=\"\",\"-\",(('Results from eQuest'!X34)-('Results from eQuest'!X35))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C31=\"\",\"\",IFERROR(IF(C31=\"\",\"-\",(('Results from eQuest'!BJ34)-('Results from eQuest'!BJ35))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C31=\"\",\"\",IF(C31=\"\",\"-\",(('Results from eQuest'!BA34+'Results from eQuest'!BG34)/10-('Results from eQuest'!BA35+'Results from eQuest'!BG35)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C31=\"\",\"\",IFERROR(IF(C31=\"\",\"-\",(('Results from eQuest'!P34+'Results from eQuest'!Q34)-('Results from eQuest'!P35+'Results from eQuest'!Q35))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B31,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B31,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,21,{"$f":"IF('Results from eQuest'!J36=\"\",\"\",'Results from eQuest'!J36)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C32=\"\",\"\",IFERROR(IF(C32=\"\",\"-\",(('Results from eQuest'!X35)-('Results from eQuest'!X36))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C32=\"\",\"\",IFERROR(IF(C32=\"\",\"-\",(('Results from eQuest'!BJ35)-('Results from eQuest'!BJ36))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C32=\"\",\"\",IF(C32=\"\",\"-\",(('Results from eQuest'!BA35+'Results from eQuest'!BG35)/10-('Results from eQuest'!BA36+'Results from eQuest'!BG36)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C32=\"\",\"\",IFERROR(IF(C32=\"\",\"-\",(('Results from eQuest'!P35+'Results from eQuest'!Q35)-('Results from eQuest'!P36+'Results from eQuest'!Q36))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B32,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B32,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,22,{"$f":"IF('Results from eQuest'!J37=\"\",\"\",'Results from eQuest'!J37)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C33=\"\",\"\",IFERROR(IF(C33=\"\",\"-\",(('Results from eQuest'!X36)-('Results from eQuest'!X37))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C33=\"\",\"\",IFERROR(IF(C33=\"\",\"-\",(('Results from eQuest'!BJ36)-('Results from eQuest'!BJ37))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C33=\"\",\"\",IF(C33=\"\",\"-\",(('Results from eQuest'!BA36+'Results from eQuest'!BG36)/10-('Results from eQuest'!BA37+'Results from eQuest'!BG37)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C33=\"\",\"\",IFERROR(IF(C33=\"\",\"-\",(('Results from eQuest'!P36+'Results from eQuest'!Q36)-('Results from eQuest'!P37+'Results from eQuest'!Q37))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B33,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B33,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,23,{"$f":"IF('Results from eQuest'!J38=\"\",\"\",'Results from eQuest'!J38)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C34=\"\",\"\",IFERROR(IF(C34=\"\",\"-\",(('Results from eQuest'!X37)-('Results from eQuest'!X38))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C34=\"\",\"\",IFERROR(IF(C34=\"\",\"-\",(('Results from eQuest'!BJ37)-('Results from eQuest'!BJ38))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C34=\"\",\"\",IF(C34=\"\",\"-\",(('Results from eQuest'!BA37+'Results from eQuest'!BG37)/10-('Results from eQuest'!BA38+'Results from eQuest'!BG38)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C34=\"\",\"\",IFERROR(IF(C34=\"\",\"-\",(('Results from eQuest'!P37+'Results from eQuest'!Q37)-('Results from eQuest'!P38+'Results from eQuest'!Q38))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B34,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B34,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,24,{"$f":"IF('Results from eQuest'!J39=\"\",\"\",'Results from eQuest'!J39)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C35=\"\",\"\",IFERROR(IF(C35=\"\",\"-\",(('Results from eQuest'!X38)-('Results from eQuest'!X39))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C35=\"\",\"\",IFERROR(IF(C35=\"\",\"-\",(('Results from eQuest'!BJ38)-('Results from eQuest'!BJ39))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C35=\"\",\"\",IF(C35=\"\",\"-\",(('Results from eQuest'!BA38+'Results from eQuest'!BG38)/10-('Results from eQuest'!BA39+'Results from eQuest'!BG39)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C35=\"\",\"\",IFERROR(IF(C35=\"\",\"-\",(('Results from eQuest'!P38+'Results from eQuest'!Q38)-('Results from eQuest'!P39+'Results from eQuest'!Q39))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B35,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B35,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,25,{"$f":"IF('Results from eQuest'!J40=\"\",\"\",'Results from eQuest'!J40)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C36=\"\",\"\",IFERROR(IF(C36=\"\",\"-\",(('Results from eQuest'!X39)-('Results from eQuest'!X40))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C36=\"\",\"\",IFERROR(IF(C36=\"\",\"-\",(('Results from eQuest'!BJ39)-('Results from eQuest'!BJ40))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C36=\"\",\"\",IF(C36=\"\",\"-\",(('Results from eQuest'!BA39+'Results from eQuest'!BG39)/10-('Results from eQuest'!BA40+'Results from eQuest'!BG40)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C36=\"\",\"\",IFERROR(IF(C36=\"\",\"-\",(('Results from eQuest'!P39+'Results from eQuest'!Q39)-('Results from eQuest'!P40+'Results from eQuest'!Q40))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B36,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B36,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,26,{"$f":"IF('Results from eQuest'!J41=\"\",\"\",'Results from eQuest'!J41)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C37=\"\",\"\",IFERROR(IF(C37=\"\",\"-\",(('Results from eQuest'!X40)-('Results from eQuest'!X41))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C37=\"\",\"\",IFERROR(IF(C37=\"\",\"-\",(('Results from eQuest'!BJ40)-('Results from eQuest'!BJ41))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C37=\"\",\"\",IF(C37=\"\",\"-\",(('Results from eQuest'!BA40+'Results from eQuest'!BG40)/10-('Results from eQuest'!BA41+'Results from eQuest'!BG41)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C37=\"\",\"\",IFERROR(IF(C37=\"\",\"-\",(('Results from eQuest'!P40+'Results from eQuest'!Q40)-('Results from eQuest'!P41+'Results from eQuest'!Q41))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B37,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B37,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,27,{"$f":"IF('Results from eQuest'!J42=\"\",\"\",'Results from eQuest'!J42)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C38=\"\",\"\",IFERROR(IF(C38=\"\",\"-\",(('Results from eQuest'!X41)-('Results from eQuest'!X42))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C38=\"\",\"\",IFERROR(IF(C38=\"\",\"-\",(('Results from eQuest'!BJ41)-('Results from eQuest'!BJ42))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C38=\"\",\"\",IF(C38=\"\",\"-\",(('Results from eQuest'!BA41+'Results from eQuest'!BG41)/10-('Results from eQuest'!BA42+'Results from eQuest'!BG42)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C38=\"\",\"\",IFERROR(IF(C38=\"\",\"-\",(('Results from eQuest'!P41+'Results from eQuest'!Q41)-('Results from eQuest'!P42+'Results from eQuest'!Q42))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B38,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B38,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,28,{"$f":"IF('Results from eQuest'!J43=\"\",\"\",'Results from eQuest'!J43)","v":""},{"$f":"P39","v":""},"",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C39=\"\",\"\",IFERROR(IF(C39=\"\",\"-\",(('Results from eQuest'!X42)-('Results from eQuest'!X43))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C39=\"\",\"\",IFERROR(IF(C39=\"\",\"-\",(('Results from eQuest'!BJ42)-('Results from eQuest'!BJ43))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C39=\"\",\"\",IF(C39=\"\",\"-\",(('Results from eQuest'!BA42+'Results from eQuest'!BG42)/10-('Results from eQuest'!BA43+'Results from eQuest'!BG43)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C39=\"\",\"\",IFERROR(IF(C39=\"\",\"-\",(('Results from eQuest'!P42+'Results from eQuest'!Q42)-('Results from eQuest'!P43+'Results from eQuest'!Q43))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B39,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B39,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,29,{"$f":"IF('Results from eQuest'!J44=\"\",\"\",'Results from eQuest'!J44)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C40=\"\",\"\",IFERROR(IF(C40=\"\",\"-\",(('Results from eQuest'!X43)-('Results from eQuest'!X44))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C40=\"\",\"\",IFERROR(IF(C40=\"\",\"-\",(('Results from eQuest'!BJ43)-('Results from eQuest'!BJ44))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C40=\"\",\"\",IF(C40=\"\",\"-\",(('Results from eQuest'!BA43+'Results from eQuest'!BG43)/10-('Results from eQuest'!BA44+'Results from eQuest'!BG44)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C40=\"\",\"\",IFERROR(IF(C40=\"\",\"-\",(('Results from eQuest'!P43+'Results from eQuest'!Q43)-('Results from eQuest'!P44+'Results from eQuest'!Q44))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B40,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B40,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,30,{"$f":"IF('Results from eQuest'!J45=\"\",\"\",'Results from eQuest'!J45)","v":""},"","",null,null,{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C41=\"\",\"\",IFERROR(IF(C41=\"\",\"-\",(('Results from eQuest'!X44)-('Results from eQuest'!X45))),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C41=\"\",\"\",IFERROR(IF(C41=\"\",\"-\",(('Results from eQuest'!BJ44)-('Results from eQuest'!BJ45))*0.1),\"-\")),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C41=\"\",\"\",IF(C41=\"\",\"-\",(('Results from eQuest'!BA44+'Results from eQuest'!BG44)/10-('Results from eQuest'!BA45+'Results from eQuest'!BG45)/10))),\"<Enter Value>\")","v":""},{"$f":"IF('General Information'!$C$40=\"eQuest\",IF(C41=\"\",\"\",IFERROR(IF(C41=\"\",\"-\",(('Results from eQuest'!P44+'Results from eQuest'!Q44)-('Results from eQuest'!P45+'Results from eQuest'!Q45))),\"-\")),\"<Enter Value>\")","v":""},null,"",null,null,"","",null,{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B41,ECM!$C$5:$C$274,0),2),\"<Enter Description Here>\")","v":"<Enter Description Here>"},{"$f":"IFERROR(INDEX(ECM!$C$5:$E$274,MATCH('Detailed Measures'!B41,ECM!$C$5:$C$274,0),3),\"<Enter Description Here>\")","v":"<Enter Description Here>"}]
[null,null,null,null,null,null,"Totals:",{"$f":"SUM(H12:H41)","v":0},{"$f":"SUM(I12:I41)","v":0},0,0,null,{"$f":"SUM(M12:M41)","v":0}]

{"sheet":"Results from Trace","index":32,"n_rows":55,"n_cols":12,"rows_kept":55,"cut":false,"hidden":true,"merged":[[3,0,3,7]]}
[]
["(OPTIONAL) Results from Trace Energy Cost Budget File(s)"]
[]
["Instructions\n1) Open Trace Energy Cost Budget (ECB) file(s) that include results for baseline and proposed models\n2) Copy end uses and associated affected fuel types from an ECB file (columns A and B from row 4 to the \"Total Building Consumption\" line item) and paste into columns A and B below.  \n3) Copy baseline runs Energy 10˄6 Btu/yr column from the appropriate ECB file and paste into columns C-F below. If the baseline is not being rotated, copy the lone baseline run into column C and leave columsn D-F blank.\n4) Copy proposed run Energy 10˄6 Btu/yr column from the approrpriate ECB file and paste into column H below. \n\n       "]
[]
["END USES (COL A)","AFFECTED FUELS (COL B)",{"$f":"IF('[3]P4P - General Info'!C23=\"ASHRAE bEQ\",\"PROPOSED DESIGN\n(Energy 10˄6 Btu/yr)\",\"BASELINE \n(Energy 10˄6 Btu/yr)\")","v":"BASELINE \n(Energy 10˄6 Btu/yr)"},{"$f":"IF('[3]P4P - General Info'!C23=\"ASHRAE bEQ\",\"Do not complete\",\"BASELINE, 90° Rotation\n(Energy 10˄6 Btu/yr)\")","v":"BASELINE, 90° Rotation\n(Energy 10˄6 Btu/yr)"},{"$f":"IF('[3]P4P - General Info'!C23=\"ASHRAE bEQ\",\"Do not complete\",\"BASELINE, 180° Rotation\n(Energy 10˄6 Btu/yr)\")","v":"BASELINE, 180° Rotation\n(Energy 10˄6 Btu/yr)"},{"$f":"IF('[3]P4P - General Info'!C23=\"ASHRAE bEQ\",\"Do not Complete\",\"BASELINE, 270° Rotation\n(Energy 10˄6 Btu/yr)\")","v":"BASELINE, 270° Rotation\n(Energy 10˄6 Btu/yr)"},{"$f":"IF('[3]P4P - General Info'!C23=\"ASHRAE bEQ\",\"PROPOSED DESIGN\n(Energy 10˄6 Btu/yr)\",\"AVERAGE BASELINE\n(Energy 10˄6 Btu/yr)\")","v":"AVERAGE BASELINE\n(Energy 10˄6 Btu/yr)"},{"$f":"IF('[3]P4P - General Info'!C23=\"ASHRAE bEQ\",\"FINAL ALTERNATIVE\n(Energy 10˄6 Btu/yr)\",\"PROPOSED \n(Energy 10˄6 Btu/yr)\")","v":"PROPOSED \n(Energy 10˄6 Btu/yr)"},null,null,null,"Lookup Value"]
["Lighting - Conditioned","Electricity",null,null,null,null,{"$f":"IF(C7=\"\",\"\",AVERAGE(C7:F7))","v":""},null,null,null,null,{"$f":"A7&B7","v":"Lighting - ConditionedElectricity"}]
["Space Heating","Electricity",null,null,null,null,{"$f":"IF(C8=\"\",\"\",AVERAGE(C8:F8))","v":""},null,null,null,null,{"$f":"A8&B8","v":"Space HeatingElectricity"}]
["Space Heating","Gas",null,null,null,null,"",null,null,null,null,"Space HeatingGas"]
["Space Cooling","Electricity",null,null,null,null,"",null,null,null,null,"Space CoolingElectricity"]
["Pumps","Electricity",null,null,null,null,"",null,null,null,null,"PumpsElectricity"]
["Heat Rejection","Electricity",null,null,null,null,"",null,null,null,null,"Heat RejectionElectricity"]
["Fans - Conditioned","Electricity",null,null,null,null,"",null,null,null,null,"Fans - ConditionedElectricity"]
["Receptacles - Conditioned","Electricity",null,null,null,null,"",null,null,null,null,"Receptacles - ConditionedElectricity"]
["Stand-alone Base Utilities","Electricity",null,null,null,null,"",null,null,null,null,"Stand-alone Base UtilitiesElectricity"]
["Stand-alone Base Utilities","Gas",null,null,null,null,"",null,null,null,null,"Stand-alone Base UtilitiesGas"]
["Total Building Consumption",null,null,null,null,null,"",null,null,null,null,"Total Building Consumption"]
[null,null,null,null,null,null,"",null,null,null,null,""]
[null,null,null,null,null,null,"",null,null,null,null,""]
[null,null,null,null,null,null,"",null,null,null,null,""]
[null,null,null,null,null,null,"",null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]

{"sheet":"12 - Performance_Outputs_1","index":33,"n_rows":455,"n_cols":61,"rows_kept":455,"cut":false,"hidden":false,"merged":[[148,21,149,21],[148,23,149,23],[149,10,149,12],[89,1,89,5],[89,9,89,10],[89,11,89,12],[90,1,90,5],[90,9,90,10],[90,11,90,12],[91,1,91,5],[91,9,91,10],[91,11,91,12],[120,20,121,20],[120,21,121,21],[121,10,121,12],[130,21,131,21],[128,21,129,21],[122,20,123,20],[130,20,131,20],[118,20,119,20],[124,20,125,20],[94,1,94,12],[97,1,97,12],[111,1,111,12],[87,11,87,12],[88,1,88,5],[88,9,88,10],[88,11,88,12],[148,20,149,20],[98,1,98,12],[100,1,100,12],[102,1,102,12],[104,1,104,12],[114,1,114,12],[116,1,116,2],[116,10,116,12],[118,1,119,2],[118,3,119,3],[118,4,119,4],[118,10,118,12],[119,10,119,12],[105,1,105,12],[109,1,109,12],[110,1,110,12],[112,1,112,12],[113,1,113,12],[124,1,125,2],[124,3,125,3],[177,23,178,23],[179,23,180,23],[181,23,182,23],[177,20,178,20],[177,21,178,21],[179,20,180,20],[179,21,180,21],[181,20,182,20],[181,21,182,21],[210,1,211,2],[210,3,211,3],[210,4,211,4],[210,10,211,11],[210,12,211,12],[210,9,211,9],[170,21,171,21],[134,21,135,21],[158,21,159,21],[164,21,165,21],[168,21,169,21],[150,20,151,20],[154,20,155,20],[164,20,165,20],[134,20,135,20],[168,1,169,2],[168,3,169,3],[162,20,163,20],[168,4,169,4],[168,10,168,12],[169,10,169,12],[170,1,171,2],[170,3,171,3],[170,4,171,4],[40,54,41,54],[172,21,173,21],[174,21,175,21],[172,20,173,20],[174,20,175,20],[126,20,127,20],[132,20,133,20],[136,20,137,20],[138,20,139,20],[140,20,141,20],[142,20,143,20],[146,20,147,20],[162,21,163,21],[144,21,145,21],[156,21,157,21],[144,20,145,20],[156,20,157,20],[158,20,159,20],[128,20,129,20],[168,20,169,20],[170,20,171,20],[170,23,171,23],[134,23,135,23],[172,23,173,23],[56,1,56,12],[59,1,59,12],[150,21,151,21],[154,21,155,21],[122,21,123,21],[118,21,119,21],[124,21,125,21],[126,21,127,21],[132,21,133,21],[136,21,137,21],[138,21,139,21],[140,21,141,21],[142,21,143,21],[146,21,147,21],[61,11,62,12],[62,6,62,7],[62,9,62,10],[61,1,62,1],[61,5,62,5],[65,9,65,10],[120,1,121,2],[120,3,121,3],[120,4,121,4],[120,10,120,12],[170,10,170,12],[171,10,171,12],[451,1,454,1],[319,2,319,3],[333,2,333,3],[345,2,345,3],[357,2,357,3],[398,1,398,3],[398,6,398,7],[398,10,398,12],[433,1,433,4],[417,1,417,11],[418,1,418,11],[419,1,419,11],[361,1,361,3],[362,1,362,11],[374,1,375,1],[374,2,375,3],[413,1,413,11],[414,1,414,11],[450,3,450,4],[435,2,435,6],[416,1,416,11],[430,1,430,4],[431,1,431,4],[432,1,432,4],[4,7,4,12],[6,1,6,12],[7,1,7,12],[8,1,8,12],[9,1,9,12],[10,1,10,12],[434,5,434,12],[430,5,430,7],[430,8,430,12],[431,8,431,12],[432,8,432,12],[431,5,431,7],[432,5,432,7],[433,5,433,7],[433,8,433,12],[11,1,11,12],[12,1,12,12],[13,1,14,1],[294,2,294,3],[298,1,298,3],[310,2,310,3],[307,2,307,3],[13,2,14,3],[13,4,14,4],[13,7,14,8],[14,10,14,11],[22,1,22,10],[22,11,22,12],[23,1,23,10],[23,11,23,12],[21,7,21,8],[21,10,21,11],[13,5,14,6],[16,5,16,6],[17,5,17,6],[18,5,18,6],[19,5,19,6],[20,5,20,6],[21,5,21,6],[13,9,13,12],[15,2,15,3],[16,2,16,3],[16,7,16,8],[16,10,16,11],[17,2,17,3],[17,7,17,8],[17,10,17,11],[18,2,18,3],[18,7,18,8],[18,10,18,11],[19,2,19,3],[19,7,19,8],[19,10,19,11],[20,2,20,3],[20,7,20,8],[20,10,20,11],[21,2,21,3],[36,1,36,3],[36,9,36,12],[39,1,39,12],[40,1,41,3],[40,4,40,6],[40,7,41,8],[40,9,41,12],[41,4,41,5],[33,1,33,3],[33,5,33,6],[33,7,33,8],[33,9,33,12],[35,1,35,3],[35,9,35,12],[37,1,37,3],[37,9,37,12],[38,1,38,3],[38,9,38,12],[30,1,30,12],[31,1,31,12],[49,7,49,8],[49,9,49,12],[50,1,50,8],[50,9,50,12],[51,1,51,11],[43,1,43,3],[43,7,43,8],[43,9,43,12],[44,1,44,3],[44,7,44,8],[44,9,44,12],[45,1,45,3],[45,7,45,8],[45,9,45,12],[46,1,46,3],[46,7,46,8],[46,9,46,12],[47,1,47,3],[47,7,47,8],[47,9,47,12],[48,1,48,3],[48,7,48,8],[48,9,48,12],[49,1,49,5],[65,11,65,12],[61,4,62,4],[61,3,62,3],[61,2,62,2],[61,6,61,10],[71,1,71,5],[71,9,71,10],[71,11,71,12],[76,1,76,4],[64,9,64,10],[64,11,64,12],[66,9,66,10],[66,11,66,12],[78,1,78,5],[78,9,78,10],[78,11,78,12],[67,9,67,10],[67,11,67,12],[68,1,68,4],[70,1,70,5],[70,9,70,10],[70,11,70,12],[72,1,72,5],[72,9,72,10],[72,11,72,12],[73,1,73,5],[73,9,73,10],[73,11,73,12],[74,1,74,5],[74,9,74,10],[74,11,74,12],[75,1,75,5],[75,9,75,10],[75,11,75,12],[79,1,79,5],[79,9,79,10],[79,11,79,12],[92,1,92,5],[92,9,92,10],[92,11,92,12],[80,1,80,5],[80,9,80,10],[80,11,80,12],[81,1,81,5],[81,9,81,10],[81,11,81,12],[82,1,82,5],[82,9,82,10],[82,11,82,12],[83,1,83,5],[83,9,83,10],[83,11,83,12],[84,1,84,4],[86,1,86,5],[86,9,86,10],[86,11,86,12],[87,1,87,5],[87,9,87,10],[124,4,125,4],[124,10,124,12],[125,10,125,12],[126,1,127,2],[126,3,127,3],[126,4,127,4],[126,10,126,12],[127,10,127,12],[122,1,123,2],[122,3,123,3],[122,4,123,4],[122,10,122,12],[123,10,123,12],[132,1,133,2],[132,3,133,3],[132,4,133,4],[132,10,132,12],[133,10,133,12],[136,1,137,2],[136,3,137,3],[136,4,137,4],[136,10,136,12],[137,10,137,12],[143,10,143,12],[146,1,147,2],[146,3,147,3],[146,4,147,4],[146,10,146,12],[147,10,147,12],[138,1,139,2],[138,3,139,3],[138,4,139,4],[138,10,138,12],[139,10,139,12],[140,1,141,2],[140,3,141,3],[140,4,141,4],[140,10,140,12],[141,10,141,12],[142,1,143,2],[142,3,143,3],[142,4,143,4],[142,10,142,12],[150,1,151,2],[150,3,151,3],[150,4,151,4],[150,10,150,12],[151,10,151,12],[154,1,155,2],[154,3,155,3],[154,4,155,4],[154,10,154,12],[155,10,155,12],[164,1,165,2],[164,3,165,3],[164,4,165,4],[164,10,164,12],[165,10,165,12],[144,1,145,2],[144,3,145,3],[144,4,145,4],[144,10,144,12],[145,10,145,12],[156,1,157,2],[156,3,157,3],[156,4,157,4],[156,10,156,12],[157,10,157,12],[148,1,149,2],[148,3,149,3],[148,4,149,4],[148,10,148,12],[162,1,163,2],[162,3,163,3],[162,4,163,4],[162,10,162,12],[163,10,163,12],[130,1,131,2],[130,3,131,3],[130,4,131,4],[130,10,130,12],[131,10,131,12],[128,1,129,2],[128,3,129,3],[128,4,129,4],[128,10,128,12],[129,10,129,12],[174,10,174,12],[175,10,175,12],[177,10,177,12],[134,1,135,2],[134,3,135,3],[134,4,135,4],[134,10,134,12],[135,10,135,12],[172,1,173,2],[172,3,173,3],[172,4,173,4],[172,10,172,12],[173,10,173,12],[177,1,177,3],[174,1,175,2],[174,3,175,3],[174,4,175,4],[160,1,161,2],[160,3,161,3],[160,4,161,4],[160,10,160,12],[166,1,167,2],[166,3,167,3],[166,4,167,4],[208,1,209,2],[178,10,178,12],[183,1,183,5],[183,10,183,12],[184,1,184,5],[184,10,184,12],[187,1,187,5],[187,10,187,12],[178,1,178,3],[179,1,179,3],[179,10,179,12],[180,1,180,3],[180,10,180,12],[181,1,181,3],[181,10,181,12],[182,1,182,3],[182,10,182,12],[212,12,213,12],[201,1,201,12],[202,1,202,12],[203,1,203,12],[204,1,204,12],[208,12,209,12],[189,1,189,4],[189,10,189,12],[190,1,190,4],[190,10,190,12],[195,1,195,5],[195,10,195,12],[191,1,191,4],[191,10,191,12],[192,1,192,4],[192,10,192,12],[193,1,193,4],[193,10,193,12],[194,1,194,4],[194,10,194,12],[206,1,206,2],[206,10,206,11],[199,1,199,12],[200,1,200,12],[226,12,227,12],[208,3,209,3],[208,4,209,4],[208,9,209,9],[208,10,209,11],[218,1,219,2],[218,3,219,3],[218,4,219,4],[224,1,225,2],[224,3,225,3],[224,4,225,4],[224,9,225,9],[224,10,225,11],[214,1,215,2],[214,3,215,3],[214,4,215,4],[214,9,215,9],[214,10,215,11],[214,12,215,12],[212,1,213,2],[212,3,213,3],[212,4,213,4],[212,9,213,9],[212,10,213,11],[230,1,231,2],[230,3,231,3],[230,4,231,4],[230,9,231,9],[230,10,231,11],[230,12,231,12],[224,12,225,12],[222,1,223,2],[222,3,223,3],[222,4,223,4],[222,9,223,9],[222,10,223,11],[222,12,223,12],[228,1,229,2],[228,3,229,3],[228,4,229,4],[228,9,229,9],[228,10,229,11],[228,12,229,12],[226,1,227,2],[226,3,227,3],[226,4,227,4],[226,9,227,9],[226,10,227,11],[234,1,235,2],[234,3,235,3],[234,4,235,4],[234,9,235,9],[234,10,235,11],[234,12,235,12],[232,1,233,2],[232,3,233,3],[232,4,233,4],[232,9,233,9],[232,10,233,11],[232,12,233,12],[238,1,239,2],[238,3,239,3],[238,4,239,4],[238,9,239,9],[238,10,239,11],[238,12,239,12],[236,1,237,2],[236,3,237,3],[236,4,237,4],[236,9,237,9],[236,10,237,11],[236,12,237,12],[242,9,243,9],[242,10,243,11],[242,12,243,12],[240,1,241,2],[240,3,241,3],[240,4,241,4],[240,9,241,9],[240,10,241,11],[240,12,241,12],[250,9,251,9],[250,10,251,11],[250,12,251,12],[216,1,217,2],[216,3,217,3],[216,4,217,4],[216,9,217,9],[216,10,217,11],[216,12,217,12],[218,9,219,9],[218,10,219,11],[218,12,219,12],[248,1,249,2],[248,3,249,3],[248,4,249,4],[248,9,249,9],[248,10,249,11],[244,4,245,4],[244,9,245,9],[244,10,245,11],[244,12,245,12],[242,1,243,2],[242,3,243,3],[242,4,243,4],[252,1,253,2],[252,3,253,3],[252,4,253,4],[252,9,253,9],[252,10,253,11],[252,12,253,12],[220,1,221,2],[220,3,221,3],[220,4,221,4],[220,9,221,9],[220,10,221,11],[220,12,221,12],[248,12,249,12],[246,1,247,2],[246,3,247,3],[246,4,247,4],[246,9,247,9],[246,10,247,11],[246,12,247,12],[244,1,245,2],[244,3,245,3],[250,1,251,2],[250,3,251,3],[250,4,251,4],[271,2,271,3],[274,2,274,3],[272,2,272,3],[273,2,273,3],[269,2,269,3],[270,2,270,3],[262,1,263,2],[262,3,263,3],[262,4,263,4],[262,9,263,9],[262,10,263,11],[262,12,263,12],[254,1,255,2],[254,3,255,3],[254,4,255,4],[254,9,255,9],[254,10,255,11],[254,12,255,12],[289,13,289,15],[292,2,292,3],[293,2,293,3],[282,2,282,3],[282,4,282,6],[282,7,282,9],[282,10,282,12],[288,1,288,11],[289,1,290,1],[289,2,290,3],[289,4,289,6],[289,7,289,9],[289,10,289,12],[283,2,283,3],[283,4,283,6],[283,7,283,9],[283,10,283,12],[284,2,284,3],[284,4,284,6],[284,7,284,9],[284,10,284,12],[286,2,286,3],[286,4,286,6],[286,7,286,9],[314,13,314,15],[317,2,317,3],[318,2,318,3],[313,1,313,3],[314,1,315,1],[314,2,315,3],[314,4,314,6],[314,7,314,9],[314,10,314,12],[328,13,328,15],[331,2,331,3],[332,2,332,3],[323,1,323,3],[324,1,324,3],[326,1,326,12],[328,1,329,1],[328,2,329,3],[328,4,328,6],[328,7,328,9],[328,10,328,12],[340,13,340,15],[343,2,343,3],[344,2,344,3],[337,1,337,3],[338,1,338,11],[340,1,341,1],[340,2,341,3],[340,4,340,6],[340,7,340,9],[340,10,340,12],[441,1,442,1],[415,1,415,11],[420,1,420,11],[394,6,394,7],[394,10,394,12],[406,2,406,3],[352,13,352,15],[355,2,355,3],[356,2,356,3],[352,1,353,1],[352,2,353,3],[352,4,352,6],[352,7,352,9],[352,10,352,12],[420,14,426,15],[437,1,438,1],[439,1,440,1],[397,10,397,12],[407,2,407,3],[408,2,408,3],[409,2,409,3],[422,1,422,11],[380,2,380,3],[381,2,381,3],[449,1,450,1],[421,1,421,11],[425,1,425,11],[426,1,426,11],[423,1,423,11],[424,1,424,11],[374,13,374,15],[377,2,377,3],[378,2,378,3],[434,1,434,4],[443,1,448,1],[401,1,402,1],[401,2,402,3],[401,4,401,6],[442,3,442,4],[374,4,374,6],[374,7,374,9],[374,10,374,12],[391,10,391,12],[392,2,392,3],[392,6,392,7],[392,10,392,12],[397,2,397,3],[397,6,397,7],[115,57,115,60],[205,57,205,60],[311,2,311,3],[379,2,379,3],[383,1,383,3],[401,7,401,9],[401,10,401,12],[394,2,394,3],[386,1,386,12],[387,4,387,7],[387,8,387,12],[387,13,387,15],[388,6,388,7],[388,10,388,12],[390,2,390,3],[390,6,390,7],[390,10,390,12],[393,2,393,3],[393,6,393,7],[393,10,393,12],[391,1,391,3],[391,6,391,7],[118,23,119,23],[120,23,121,23],[174,23,175,23],[146,23,147,23],[150,23,151,23],[154,23,155,23],[122,23,123,23],[162,23,163,23],[144,23,145,23],[156,23,157,23],[158,23,159,23],[164,23,165,23],[124,23,125,23],[126,23,127,23],[132,23,133,23],[136,23,137,23],[138,23,139,23],[140,23,141,23],[142,23,143,23],[130,23,131,23],[128,23,129,23],[275,1,275,3],[266,1,267,1],[266,2,267,3],[266,4,266,6],[286,10,286,12],[295,2,295,3],[296,2,296,3],[297,2,297,3],[320,2,320,3],[285,2,285,3],[285,4,285,6],[285,7,285,9],[285,10,285,12],[278,1,278,11],[279,1,279,3],[279,4,279,6],[279,7,279,9],[279,10,279,12],[281,2,281,3],[281,4,281,6],[281,7,281,9],[281,10,281,12],[266,7,266,9],[266,10,266,12],[321,2,321,3],[322,2,322,3],[300,1,300,11],[301,1,301,12],[302,1,303,1],[302,2,303,3],[302,4,302,6],[302,7,302,9],[302,10,302,11],[305,1,305,3],[306,2,306,3],[309,1,309,3],[334,2,334,3],[335,2,335,3],[336,2,336,3],[346,2,346,3],[347,2,347,3],[348,2,348,3],[358,2,358,3],[359,2,359,3],[360,2,360,3],[349,1,349,3],[350,1,350,11],[410,1,410,3],[387,1,388,1],[387,2,388,3],[382,2,382,3],[395,2,395,3],[395,6,395,7],[395,10,395,12],[396,2,396,3],[396,6,396,7],[396,10,396,12],[404,2,404,3],[405,2,405,3],[160,20,161,20],[160,21,161,21],[160,23,161,23],[161,10,161,12],[152,1,153,2],[152,3,153,3],[152,4,153,4],[152,10,152,12],[152,20,153,20],[152,21,153,21],[152,23,153,23],[153,10,153,12],[158,1,159,2],[158,3,159,3],[158,4,159,4],[158,10,158,12],[159,10,159,12],[166,10,166,12],[166,20,167,20],[166,21,167,21],[166,23,167,23],[167,10,167,12],[260,1,261,2],[260,3,261,3],[260,4,261,4],[260,9,261,9],[260,10,261,11],[260,12,261,12],[258,1,259,2],[258,3,259,3],[258,4,259,4],[258,9,259,9],[258,10,259,11],[258,12,259,12],[256,1,257,2],[256,3,257,3],[256,4,257,4],[256,9,257,9],[256,10,257,11],[256,12,257,12],[168,23,169,23]]}
["G"]
["G","Performance Rating Method Outputs"]
["G"]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Multiplier"]
["G","Energy Model ID",null,null,null,null,null,{"$f":"INDEX(MBD_EMI_Table,2,1)","v":0},null,null,null,null,null,null,null,null,{"$f":"IFERROR(INDEX(MBD_EMI_Table,MATCH($H$5,MBD_EMI_Index,0),MATCH('1 - Multiple Buildings Details'!$J$16,MBD_EMI_Hdr,0)),\"ERROR\")","v":0}]
["G"]
["G","Table 12.1: Energy Sources"]
["G"]
["G","Enter each energy source serving the project, the units for the energy consumption and demand, and the associated utility rate name and tariff structure. Default EIA Rates may be used in lieu of local utility rates at the discretion of the energy modeler.  All project energy types and the demand and consumption units must be entered before entering energy simulation output data. Also enter the units used to report energy consumption totals (the sum of all energy types) for site energy consumption and source energy consumption (generally, the IP units are Btu x 10^6, the SI site energy units are kWh, and the SI source energy units are MJ).\n\n\n"]
["G","DES Path 1: If the project is using campus or district thermal energy using ASHRAE 90.1-2010 without Addenda (District Energy Modeling Path 1), select District Cooling, District Hot Water, or District Steam as applicable and all other energy sources serving the building "]
["G","DES Path 2: If the project is modeling campus or district thermal energy using the Full DES Performance Accounting method (District Energy Modeling Path 2) include each energy source serving the building except District Energy, AND include each energy source in the district or campus plant (e.g. electricity, natural gas, etc.) if different from the energy sources serving the building. Do not select District Cooling, District Hot Water, or District Steam. "]
["G","DES Path 3: If the project is modeling campus or district thermal energy using the Streamlined DES Accounting Method (District Energy Modeling Path 3), select District Cooling, District Hot Water, or District Steam as applicable, AND each energy source serving the building, AND each energy source in the district or campus plant if different from the energy sources serving the building (e.g. electricity, natural gas, etc.).\n"]
["G"]
["G","Energy Type","Energy Consumption Units",null,"Demand Units","Utility Rate Structure Type",null,"Utility Rate Description",null,"Unit Conversion Factors"]
["G",null,null,null,null,null,null,null,null,"Site to Source Conversion Factors",{"$f":"CONCATENATE(\"Energy Type Consumption Units to Site Energy Consumption (\",PO_SiteUnits,\")\")","v":"Energy Type Consumption Units to Site Energy Consumption (Btu x 10^6)"},null,{"$f":"CONCATENATE(\"Energy Type Consumption Units to Source Energy Consumption (\",PO_SourceUnits,\")\")","v":"Energy Type Consumption Units to Source Energy Consumption (Btu x 10^6)"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Energy_Type","Energy_Consumption_Units",null,"Demand_Units","Utility_Rate_Structure",null,"Utility_Rate_Name",null,null,"Site_Energy_Conversion_Factor",null,"Source_Energy_Conversion_Factor"]
["G",null,null,null,null,null,null,null,null,{"$f":"R17","v":""},{"$f":"IFERROR(VLOOKUP(\"kBtu\",EnergyUnitsTable,3,FALSE)/VLOOKUP(PO_SiteUnits,EnergyUnitsTable,3,FALSE)*VLOOKUP($C17,EnergyUnitsTable,3,FALSE),\"\")","v":""},null,{"$f":"IFERROR(VLOOKUP(\"kBtu\",EnergyUnitsTable,3,FALSE)/VLOOKUP(PO_SourceUnits,EnergyUnitsTable,3,FALSE)*VLOOKUP($C17,EnergyUnitsTable,3,FALSE)*J17,\"\")","v":""},null,null,null,null,{"$f":"IFERROR(VLOOKUP(B17,FuelTable,2,FALSE),\"\")","v":""}]
["G",null,null,null,null,null,null,null,null,"","",null,"",null,null,null,null,""]
["G",null,null,null,null,null,null,null,null,"","",null,"",null,null,null,null,""]
["G",null,null,null,null,null,null,null,null,"","",null,"",null,null,null,null,""]
["G",null,null,null,null,null,null,null,null,"","",null,"",null,null,null,null,""]
["G",null,null,null,null,null,null,null,null,"","",null,"",null,null,null,null,""]
["G","Site energy consumption units used to report energy consumption totals (sum of energy types)",null,null,null,null,null,null,null,null,null,"Btu x 10^6"]
["G","Source energy consumption units used to report energy consumption totals (sum of energy types)",null,null,null,null,null,null,null,null,null,{"$f":"IF(SI_IP_Units=\"SI\",\"MWh\",\"Btu x 10^6\")","v":"Btu x 10^6"}]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NOTE: these buttons are not working when template is locked"]
["G"]
["G","Table 12.2: On-Site Renewable Energy Production"]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Site-generated renewable energy?"]
["G","The project building uses on-site renewable energy systems. (Optional)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
["G"]
["G","Table: On-Site Renewable energy source summary"]
["G","Renewable energy production should be reported in the table below. Note: This calculator will automatically reduce the proposed energy consumption and cost to accurately reflect the revised results. Therefore, any site-generated renewable energy production should NOT be included in the Performance Rating Method tables below.\n\nSelect the site-generated renewable energy source. Enter the rated capacity of the site-generated renewable source including the units (e.g. for photovoltaics 10 kW). Include all relevant capacities (i.e for solar thermal, both the storage tank capacity and the solar thermal panel capacity).\n\nThe cost of the Site-generated renewable cost will be automatically determined using the virtual rate once the output data (consumption and cost) is entered below. The cost may be overridden by the user, however this may generate an issue on the Quality Checks and the user should be prepared to justify the entered cost value."]
["G"]
["G","On-Site Renewable Source",null,null,"Offset \nEnergy Type","Rated Capacity ",null,"Annual Site Energy Generated",null,"Annual Energy Cost Offset with \nSite-Generated Renewables \n($/year)",null,null,null,null,null,null,null,null,null,"Default_Cost","Rate_Variance",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Renewable_Source",null,null,"Offset_Energy_Type","Rated_Capacity",null,"Annual_Site_Energy",null,"Cost",null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion","EFLH","Default_Cost","Rate_Variance"]
["A","Photovoltaic system",null,null,"Electricity",null,{"$f":"IFERROR(IF(ISBLANK($E36),\"\",VLOOKUP($E36,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR(IF(ISBLANK($E36),\"\",VLOOKUP($E36,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($H36*VLOOKUP($E36,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},"","","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E36),\"\",VLOOKUP($E36,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E36),\"\",VLOOKUP($E36,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR((H36*VLOOKUP(I36,EnergyUnitsTable,3,FALSE))/(F36*VLOOKUP(G36,DemandTable,3,FALSE)),\"\")","v":""},{"$f":"IFERROR($H36*VLOOKUP($E36,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(1-$J36/$T36,0)","v":0}]
[null,"Solar thermal system",null,null,"Natural Gas",null,{"$f":"IFERROR(IF(ISBLANK($E37),\"\",VLOOKUP($E37,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR(IF(ISBLANK($E37),\"\",VLOOKUP($E37,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},"","","","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E37),\"\",VLOOKUP($E37,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E37),\"\",VLOOKUP($E37,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR((H37*VLOOKUP(I37,EnergyUnitsTable,3,FALSE))/(F37*VLOOKUP(G37,DemandTable,3,FALSE)),\"\")","v":""},{"$f":"IFERROR($H37*VLOOKUP($E37,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(1-$J37/$T37,0)","v":0}]
["A",null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E38),\"\",VLOOKUP($E38,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR(IF(ISBLANK($E38),\"\",VLOOKUP($E38,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},"","","","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E38),\"\",VLOOKUP($E38,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E38),\"\",VLOOKUP($E38,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR((H38*VLOOKUP(I38,EnergyUnitsTable,3,FALSE))/(F38*VLOOKUP(G38,DemandTable,3,FALSE)),\"\")","v":""},{"$f":"IFERROR($H38*VLOOKUP($E38,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(1-$J38/$T38,0)","v":0}]
[null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E39),\"\",VLOOKUP($E39,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR(IF(ISBLANK($E39),\"\",VLOOKUP($E39,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},"","","","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E39),\"\",VLOOKUP($E39,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E39),\"\",VLOOKUP($E39,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR((H39*VLOOKUP(I39,EnergyUnitsTable,3,FALSE))/(F39*VLOOKUP(G39,DemandTable,3,FALSE)),\"\")","v":""},{"$f":"IFERROR($H39*VLOOKUP($E39,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(1-$J39/$T39,0)","v":0}]
[null,"Renewable Summary"]
[null,"Offset Energy Type",null,null,"Annual Site Energy Generated",null,null,{"$f":"CONCATENATE(\"Annual Source Energy Offset with Site-Generated Renewables\n (\", PO_SourceUnits, \")\")","v":"Annual Source Energy Offset with Site-Generated Renewables\n (Btu x 10^6)"},null,"Annual Energy Cost Offset with \nSite-Generated Renewables \n($/year)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
[null,null,null,null,"Units per Energy Type",null,{"$f":"CONCATENATE(\"Units = \", PO_SiteUnits,\")\")","v":"Units = Btu x 10^6)"}]
[null,"Energy_Type",null,null,"Site_Energy_Ind_Units","Site_Ind_Units","Site_Energy_Same_Units","Source_Energy",null,"Cost",null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
[null,{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},null,null,{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,SUMIF(INDEX(PO_renewable_table,0,MATCH($E$35,PO_renewable_hdr,0)),$B44,INDEX(PO_renewable_table,0,MATCH($H$35,PO_renewable_hdr,0))),\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B44),\"\",VLOOKUP($B44,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($E44*$Q44,\"\")","v":""},{"$f":"IFERROR($E44*$R44,\"\")","v":""},null,{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,SUMIF($E$36:$E$37,$B44,$J$36:$J$37),0),\"\")","v":0},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B44),\"\",VLOOKUP($B44,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B44),\"\",VLOOKUP($B44,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
[null,{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},null,null,"","",{"$f":"IFERROR($E45*$Q45,\"\")","v":""},{"$f":"IFERROR($E45*$R45,\"\")","v":""},null,0,null,null,null,null,null,null,"",""]
[null,{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},null,null,"","",{"$f":"IFERROR($E46*$Q46,\"\")","v":""},{"$f":"IFERROR($E46*$R46,\"\")","v":""},null,0,null,null,null,null,null,null,"",""]
[null,{"$f":"IFERROR(IF(ISBLANK(B20),\"\",B20),\"\")","v":""},null,null,"","",{"$f":"IFERROR($E47*$Q47,\"\")","v":""},{"$f":"IFERROR($E47*$R47,\"\")","v":""},null,0,null,null,null,null,null,null,"",""]
[null,"",null,null,"","","","",null,0,null,null,null,null,null,null,"",""]
[null,"",null,null,"","","","",null,0,null,null,null,null,null,null,"",""]
[null,"Total",null,null,null,null,{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_2_Table,0,MATCH($G$43,PO_Enrgy_2_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_2_Table,0,MATCH($H$43,PO_Enrgy_2_Hdr,0))),\"\")","v":0},{"$f":"SUM(I43:I45)","v":0},{"$f":"IFERROR(SUM(J35:J37),\"\")","v":0}]
[null,"Percent renewable energy (by cost)",null,null,null,null,null,null,null,{"$f":"IF(Datacenter_Avg=TRUE,IFERROR($J50/$J$362,\"\"),IFERROR($J50/$J$324,\"\"))","v":""}]
["G"]
["G"]
["G","Table 12.3: Exceptional Calculation Methods",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Exceptional Calculations?"]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false]
["G","The building energy analysis includes exceptional calculation methods. (Optional)"]
["G","Data Centers:  If using the Data Center Calculator to document energy improvements in IT loads, the checkbox stating that the building energy analysis includes exceptional calculation methods must be checked.  In the table below, select the checkbox “Apply to Baseline?” for each end-use impacted, and provide:\n•  The completed Data Center Calculator (found under the prerequisite's \"Resources\" tab in the Credit Library), as well as copies of any other spreadsheets used to perform the calculations\n•  If energy efficiency credit is applied for any future IT equipment, electrical infrastructure, and/or for future server room cooling equipment that will serve unfinished spaces (meaning that the IT equipment, electrical infrastructure, and/or unfinished space cooling equipment will not be installed during Startup Occupancy), provide a binding Owner commitment letter and (for any tenants) sample lease agreements with binding tenant requirements that confirms that the future installed IT equipment will be at least as efficient as the equipment modeled in the Data Center Calculator. Note that the future equipment may not be modeled as being more efficient than the equipment installed for Startup occupancy.\n•  If taking credit for the impact of IT equipment load reductions on HVAC energy consumption, upload the simulation input summary and simulation output reports, and Performance Rating summary with the baseline model revised to include the baseline IT and electrical infrastructure from the Data Center Calculator.\n"]
["G"]
["G","Table: Exceptional calculation methods energy summary"]
["G","Report Exceptional calculation methods in the table below.\n\nSelect \"Add to Baseline\" if the exceptional calculation adjusts the Baseline building energy consumption and cost up, or \"Subtract from Proposed\" if the exceptional calculation adjusts the Proposed building energy consumption and cost down.\n\nThis calculator will automatically reduce the proposed energy consumption and cost, or increase the baseline energy consumption and cost to accurately reflect the revised results. Therefore, any exceptional calculation methods should NOT be included in the Performance Rating Method Compliance report below.  If any single Exceptional Calculation Method results in energy penalties for a given energy type (i.e. increased proposed case electricity energy usage, or decreased baseline case fossil fuel energy usage), that penalty should be entered as a negative number. If any single Exceptional Calculation Method affects more than one energy type, please add additional rows to capture the method's impact to that energy type. If taking credit for Data Center Equipment or Retail Process Loads, those savings must be recorded here and the supplemental spreadsheets associated with that equipment must be uploaded as part of the submittal documents.\n\nThe cost of the Exceptional Calculation Method will be automatically determined using the virtual rate once the output data (consumption and cost) is entered below. The cost may be overridden by the user, however this may generate an issue on the Quality Checks and the user should be prepared to justify the entered cost value."]
["G"]
["G","Exceptional \nCalculation \nNumber","Exceptional \nCalculation \nMethod ID","Unregulated?","Energy Type(s)","Add to Baseline?\nSubtract from Proposed?","Annual Energy Difference by Energy Type",null,null,null,null,"Annual Energy Cost Difference"]
["G",null,null,null,null,null,"Site Energy \n(Units per Energy Type)",null,{"$f":"CONCATENATE(\"Site Energy \n(Units = \", PO_SiteUnits,\")\")","v":"Site Energy \n(Units = Btu x 10^6)"},{"$f":"\"Source Energy Consumption \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Consumption \n(Btu x 10^6)"},null,null,null,null,null,null,null,null,null,null,null,null,"Unregulated Baseline",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Ex_Calc_Number","Ex_Calc_ID","Unregulated","Energy_Type","Add_Baseline_Subtract_Proposed","Site_Energy_Ind_Units","Site_Ind_Units","Site_Energy_Same_Units","Source_Energy",null,"Cost",null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",null,"Default_Cost","Rate_Variance"]
["B",null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E65),\"\",VLOOKUP($E65,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($E65,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)*$G65,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($E65,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)*$G65,\"\")","v":""},null,{"$f":"IFERROR($G65*IF($F65=\"Subtract from Proposed\",VLOOKUP($E65,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($E65,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},"",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E65),\"\",VLOOKUP($E65,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E65),\"\",VLOOKUP($E65,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR($G65*IF($F65=\"Subtract from Proposed\",VLOOKUP($E65,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($E65,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(1-$J65/$T65,0)","v":0},null,{"$f":"IF(AND(D65=\"x\",Y65=1),G65,0)","v":0},{"$f":"IF(E65=\"Electricity\",\"kWh\",IF(E65=\"Natural Gas\",\"THERM\",IF(E65=\"District Cooling\",\"MWh\",\"\")))","v":""},{"$f":"IF(F65=\"Add to Baseline\",1,2)","v":2},null,null,""]
[null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E66),\"\",VLOOKUP($E66,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($E66,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)*$G66,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($E66,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)*$G66,\"\")","v":""},null,"","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E66),\"\",VLOOKUP($E66,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E66),\"\",VLOOKUP($E66,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR($G66*IF($F66=\"Subtract from Proposed\",VLOOKUP($E66,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($E66,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(1-$J66/$T66,0)","v":0},null,{"$f":"IF(AND(D66=\"x\",Y66=1),G66,0)","v":0},{"$f":"IF(E66=\"Electricity\",\"kWh\",IF(E66=\"Natural Gas\",\"THERM\",IF(E66=\"District Cooling\",\"MWh\",\"\")))","v":""},{"$f":"IF(F66=\"Add to Baseline\",1,2)","v":2}]
[null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E67),\"\",VLOOKUP($E67,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($E67,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)*$G67,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($E67,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)*$G67,\"\")","v":""},null,"","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E67),\"\",VLOOKUP($E67,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E67),\"\",VLOOKUP($E67,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR($G67*IF($F67=\"Subtract from Proposed\",VLOOKUP($E67,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($E67,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(1-$J67/$T67,0)","v":0},null,{"$f":"IF(AND(D67=\"x\",Y67=1),G67,0)","v":0},{"$f":"IF(E67=\"Electricity\",\"kWh\",IF(E67=\"Natural Gas\",\"THERM\",IF(E67=\"District Cooling\",\"MWh\",\"\")))","v":""},{"$f":"IF(F67=\"Add to Baseline\",1,2)","v":2},null,null,""]
[null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E68),\"\",VLOOKUP($E68,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($E68,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)*$G68,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($E68,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)*$G68,\"\")","v":""},null,"","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E68),\"\",VLOOKUP($E68,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E68),\"\",VLOOKUP($E68,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR($G68*IF($F68=\"Subtract from Proposed\",VLOOKUP($E68,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($E68,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(1-$J68/$T68,0)","v":0},null,{"$f":"IF(AND(D68=\"x\",Y68=1),G68,0)","v":0},{"$f":"IF(E68=\"Electricity\",\"kWh\",IF(E68=\"Natural Gas\",\"THERM\",IF(E68=\"District Cooling\",\"MWh\",\"\")))","v":""},{"$f":"IF(F68=\"Add to Baseline\",1,2)","v":2},null,null,""]
[null,"Subtotals added to baseline"]
[null,"Energy_Type",null,null,null,null,"Site_Energy_Ind_Units","Site_Ind_Units","Site_Energy_Same_Units","Source_Energy",null,"Cost",null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
[null,{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($G$64,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($E$64,PO_ExCalc_Hdr,0)),$B71,INDEX(PO_ExCalc_Table,0,MATCH($F$64,PO_ExCalc_Hdr,0)),\"Add to Baseline\"),\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B71),\"\",VLOOKUP($B71,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($G71*$Q71,\"\")","v":""},{"$f":"IFERROR($G71*$R71,\"\")","v":""},{"$f":"IFERROR($G71*$Q71,\"\")","v":""},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($L$64,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($E$64,PO_ExCalc_Hdr,0)),$B71,INDEX(PO_ExCalc_Table,0,MATCH($F$64,PO_ExCalc_Hdr,0)),\"Add to Baseline\"),\"\"),\"\")","v":""},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(M$65:M$68,$E$65:$E$68,$B71,$F$65:$F$68,\"Add to Baseline\"),\"\"),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B71),\"\",VLOOKUP($B71,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B71),\"\",VLOOKUP($B71,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
[null,{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($G$64,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($E$64,PO_ExCalc_Hdr,0)),$B72,INDEX(PO_ExCalc_Table,0,MATCH($F$64,PO_ExCalc_Hdr,0)),\"Add to Baseline\"),\"\"),\"\")","v":""},"",{"$f":"IFERROR($G72*$Q72,\"\")","v":""},{"$f":"IFERROR($G72*$R72,\"\")","v":""},{"$f":"IFERROR($G72*$Q72,\"\")","v":""},"","",null,null,null,"",""]
[null,{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},null,null,null,null,"","",{"$f":"IFERROR($G73*$Q73,\"\")","v":""},{"$f":"IFERROR($G73*$R73,\"\")","v":""},{"$f":"IFERROR($G73*$Q73,\"\")","v":""},"","",null,null,null,"",""]
[null,{"$f":"IFERROR(IF(ISBLANK(B20),\"\",B20),\"\")","v":""},null,null,null,null,"","",{"$f":"IFERROR($G74*$Q74,\"\")","v":""},{"$f":"IFERROR($G74*$R74,\"\")","v":""},{"$f":"IFERROR($G74*$Q74,\"\")","v":""},"","",null,null,null,"",""]
[null,"",null,null,null,null,"","","","","","","",null,null,null,"",""]
[null,"",null,null,null,null,"","","","","","","",null,null,null,"",""]
[null,"Subtotals subtracted from proposed"]
[null,"Energy_Type",null,null,null,null,"Site_Energy_Ind_Units","Site_Ind_Units","Site_Energy_Same_Units","Source_Energy",null,"Cost",null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
[null,{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($G$64,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($E$64,PO_ExCalc_Hdr,0)),$B79,INDEX(PO_ExCalc_Table,0,MATCH($F$64,PO_ExCalc_Hdr,0)),\"Subtract from Proposed\"),\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B79),\"\",VLOOKUP($B79,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($G79*$Q79,\"\")","v":""},{"$f":"IFERROR($G79*$R79,\"\")","v":""},{"$f":"IFERROR($G79*$Q79,\"\")","v":""},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($L$64,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($E$64,PO_ExCalc_Hdr,0)),$B79,INDEX(PO_ExCalc_Table,0,MATCH($F$64,PO_ExCalc_Hdr,0)),\"Subtract from Proposed\"),\"\"),\"\")","v":""},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(M$65:M$68,$E$65:$E$68,$B79,$F$65:$F$68,\"Add to Baseline\"),\"\"),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B79),\"\",VLOOKUP($B79,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B79),\"\",VLOOKUP($B79,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
[null,{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},null,null,null,null,"","",{"$f":"IFERROR($G80*$Q80,\"\")","v":""},{"$f":"IFERROR($G80*$R80,\"\")","v":""},{"$f":"IFERROR($G80*$Q80,\"\")","v":""},"","",null,null,null,"",""]
[null,{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},null,null,null,null,"","",{"$f":"IFERROR($G81*$Q81,\"\")","v":""},{"$f":"IFERROR($G81*$R81,\"\")","v":""},{"$f":"IFERROR($G81*$Q81,\"\")","v":""},"","",null,null,null,"",""]
[null,{"$f":"IFERROR(IF(ISBLANK(B20),\"\",B20),\"\")","v":""},null,null,null,null,"","",{"$f":"IFERROR($G82*$Q82,\"\")","v":""},{"$f":"IFERROR($G82*$R82,\"\")","v":""},{"$f":"IFERROR($G82*$Q82,\"\")","v":""},"","",null,null,null,"",""]
[null,"",null,null,null,null,"","","","","","","",null,null,null,"",""]
[null,"",null,null,null,null,"","","","","","","",null,null,null,"",""]
[null,"Subtotals added to proposed"]
[null,"Energy_Type",null,null,null,null,"Site_Energy_Ind_Units","Site_Ind_Units","Site_Energy_Same_Units","Source_Energy",null,"Cost",null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
[null,{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($G$64,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($E$64,PO_ExCalc_Hdr,0)),$B87,INDEX(PO_ExCalc_Table,0,MATCH($F$64,PO_ExCalc_Hdr,0)),\"Add to Proposed\"),\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B87),\"\",VLOOKUP($B87,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($G87*$Q87,\"\")","v":""},{"$f":"IFERROR($G87*$R87,\"\")","v":""},{"$f":"IFERROR($G87*$Q87,\"\")","v":""},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($L$64,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($E$64,PO_ExCalc_Hdr,0)),$B87,INDEX(PO_ExCalc_Table,0,MATCH($F$64,PO_ExCalc_Hdr,0)),\"Add to Proposed\"),\"\"),\"\")","v":""},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(M$65:M$68,$E$65:$E$68,$B87,$F$65:$F$68,\"Add to Baseline\"),\"\"),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B87),\"\",VLOOKUP($B87,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B87),\"\",VLOOKUP($B87,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
[null,{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},null,null,null,null,"","",{"$f":"IFERROR($G88*$Q88,\"\")","v":""},{"$f":"IFERROR($G88*$R88,\"\")","v":""},{"$f":"IFERROR($G88*$Q88,\"\")","v":""},"","",null,null,null,"",""]
[null,{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},null,null,null,null,"","",{"$f":"IFERROR($G89*$Q89,\"\")","v":""},{"$f":"IFERROR($G89*$R89,\"\")","v":""},{"$f":"IFERROR($G89*$Q89,\"\")","v":""},"","",null,null,null,"",""]
[null,"",null,null,null,null,"","",{"$f":"IFERROR($G90*$Q90,\"\")","v":""},{"$f":"IFERROR($G90*$R90,\"\")","v":""},{"$f":"IFERROR($G90*$Q90,\"\")","v":""},"","",null,null,null,"",""]
[null,"",null,null,null,null,"","","","","","","",null,null,null,"",""]
[null,"",null,null,null,null,"","","","","","","",null,null,null,"",""]
[null,"Total Exceptional Calculation Method Adjustment",null,null,null,null,null,null,{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_3_Table,0,MATCH($I70,PO_Enrgy_3_Hdr,0)),INDEX(PO_Enrgy_4_Table,0,MATCH($I78,PO_Enrgy_4_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_3_Table,0,MATCH($J70,PO_Enrgy_3_Hdr,0)),INDEX(PO_Enrgy_4_Table,0,MATCH($J78,PO_Enrgy_4_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(K$40:K$80),0)","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_3_Table,0,MATCH($L70,PO_Enrgy_3_Hdr,0)),INDEX(PO_Enrgy_4_Table,0,MATCH($L78,PO_Enrgy_4_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(M$40:M$80),0)","v":0}]
["G"]
["G","Upload: Exceptional calculation \nProvide a detailed narrative explaining the exceptional calculation method(s) performed, including all end-uses affected by the exceptional calculation method. If more than one exceptional calculation method is used, the exceptional calculation ID in the narrative must match the values listed in the table above.  The exceptional calculation method must include:\n•  Step-by-step documentation of the exceptional calculation method(s) performed detailed enough to reproduce the results\n•  Copies of all spreadsheets used to perform the calculations, or simulation energy model input and output summaries documenting the calculations performed\n•  For methods that significantly impact HVAC or refrigeration energy, the calculations shall be performed on a time step basis consistent with the simulation program used\n•  The Performance Rating calculated with and without the exceptional calculation method\n•  Documentation of the baseline and proposed assumptions. Documentation of baseline assumptions verify that the efficiency measure is not conventional practice by including, but not limited to:\n    ○  a recently published study (published within five years of the project registration date) with researched tabulations or monitored data establishing standard practice for the given application in similar newly constructed facilities\n    ○  a new construction utility or government program that incentivizes the measure\n    ○  a document showing the systems used to perform the same function in other newly constructed facilities (for example, three similar facilities built within the past five years). These systems would be treated as the baseline system in the analysis, and evidence must be provided to demonstrate how the energy for the baseline and proposed buildings are determined \n    ○  use any of the prescriptive requirements from 90.1 as the baseline requirement without further justification to substantiate conventional practice, but only for the specific component addressed by the prescriptive requirement"]
["G"]
["G","Energy Modeling Output Reporting Method"]
["G","Select one of the following before entering any simulation output data:\nNote: If this is selected after data has been entered in the tables below, the energy types, baseline energy by end use, and baseline cost data will be cleared from these tables."]
["G","Complete the baseline results for each of the four building orientations, in addition to the proposed results.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
["G"]
["G","Report the averaged baseline results, in addition to the proposed results. In the EAp2 form uploads, provide simulation output summaries from the simulation output software that include the energy consumption by end-use, total energy consumption by energy type, and total energy cost by energy type, reported separately  for each of the four baseline rotations, and the average baseline energy consumption by end-use, energy consumption by energy type, and energy cost by energy type. (The simulation software must report this average as a standard report in order to use this option)."]
["G"]
["G","The project is not required to simulate four baseline orientations because (a) the vertical fenestration area on each orientation varies by less than 5%, (b) the energy code used does not require simulation of four baseline orientations, or (c) the building is more than 50% existing based on conditioned floor area. Report the non-rotated baseline results, in addition to the proposed results.\n"]
["G"]
["G","The project is not required to simulate four baseline orientations because the building orientation is dictated by site consideration, as allowed by Table G3.1.5 (a) (baseline) Exception 1. Report the non-rotated baseline results, in addition to the proposed results."]
["G"]
["G"]
["G","Performance Rating Method Compliance Report"]
["G","Table 12.4: Baseline energy summary by end use"]
["G","Complete the table below for the proposed, providing information on baseline energy consumption and peak demand by end-use. This data will be used to auto populate the Performance tables below. If an end-use has two energy types (e.g. proposed space heating includes both fossil fuel and electric), enter the end-use twice in the table, and list the two different energy types. When linking to the Results from eQUEST or Results from Trace tabs, scroll to the right to customize the linked rows/columns for each end-use. For those using the 'Results from Trace' tab, note that TRACE uses a unit conversion factor of 3.413 btu/W, whereas this worksheet uses a conversion factor of 3.412 btu/W. As a result, model results will differ by 0.03% versus those shown in Trace output reports."]
["G","ASHRAE 90.1-2010 without Addenda (District Energy Modeling Path 1): Report the district energy type (District Cooling, District Hot Water, or District Steam) for the cooling and heating end-uses as applicable for both the baseline and proposed.  "]
["G","Full DES Performance Accounting method (District Energy Modeling Path 2): Report the baseline energy as if the thermal energy is produced in the building.  Report the proposed energy used to generate and distribute the district thermal energy serving the building based on calculated average district thermal efficiencies (e.g. report the electricity used to generate and distribute chilled water to the building).\n"]
["G","Streamlined DES Accounting Method (District Energy Modeling Path 3): Report the energy type (District Cooling, District Hot Water, or District Steam for the cooling and heating end-uses as applicable for both the baseline and proposed. "]
["G","Data Centers: The energy consumption for IT equipment must be metered and reported separately from other end-uses in the energy model, and in the tables below to allow the proper determination of the PUE. Complete the table below for the baseline using the full build-out IT loads for the proposed design.\n"]
["G","Retail: The energy consumption for cooking, refrigeration, and kitchen ventilation fans must be metered and reported separately from other end-uses in the energy model and in the tables below. Energy savings or consumption attributable to unregulated equipment, other than Commercial Kitchen Equipment, Supermarket Refrigeration, Walk-in Coolers and Freezers, or Commercial Kitchen Ventilation listed in Tables 1 – 4 of the LEED v4 BD+C:Retail and ID+C: Retail Rating System Appendix 3 must be claimed via Exceptional Calculation Methodology."]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Software Links"]
["G","End Use",null,"Unregulated?","Energy Type","Units of \nAnnual Energy and Peak Demand","Baseline 0° rotation","Baseline 90° rotation","Baseline 180° rotation","Baseline 270° rotation","Baseline Design Total\n (Average of 4 rotations)",null,null,null,null,null,null,null,null,null,"Unregulated ",null,null,null,null,"Proposed Design CL G","Proposed Design CL H","Proposed Design CL I","Proposed Design CL J",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):",null,null,"\"Results from eQUEST\" End Use Column","\"Results from Trace\" End Use Label","\"Results from Trace\" End Use Fuel Label","\"Results from Trace\" End Use Row"]
["G","End_Use",null,"Unregulated","Energy_Type","Energy_Units","Baseline_0_Rotation","Baseline_90_Rotation","Baseline_180_Rotation","Baseline_270_Rotation","Base_Consumption_Demand",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion","EFLH"]
["G","Interior lighting",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E119),\"\",\"Consumption (\" & VLOOKUP($E119,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF119&\"8\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!C\"&$BI119)/$Q119,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF119&\"9\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!D\"&$BI119)/$Q119,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF119&\"10\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!E\"&$BI119)/$Q119,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF119&\"11\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!F\"&$BI119)/$Q119,\"\")),\"\")","v":0},{"$f":"IFERROR(AVERAGEIF(G119:J119,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E119),\"\",VLOOKUP($E119,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E119),\"\",VLOOKUP($E119,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F119),(K119*VLOOKUP(MID(F119,FIND(\"(\",F119)+1,LEN(F119)-FIND(\"(\",F119)-1),EnergyUnitsTable,3,FALSE))/(K120*VLOOKUP(MID(F120,FIND(\"(\",F120)+1,LEN(F120)-FIND(\"(\",F120)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D119=\"x\",K119,0)","v":0},{"$f":"IF(E119=\"Electricity\",\"kWh\",IF(E119=\"Natural Gas\",\"THERM\",IF(E119=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D119=\"x\",FALSE,TRUE)","v":true},null,{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF119&\"8\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!C\"&$BI119)/$Q119,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF119&\"9\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!D\"&$BI119)/$Q119,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF119&\"10\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!E\"&$BI119)/$Q119,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF119&\"11\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!F\"&$BI119)/$Q119,\"\")),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L","Lighting - Conditioned","Electricity",{"$f":"IF(BG119<>\"\",IFERROR(MATCH(BG119&BH119,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":7}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E119),\"\",\"Demand (\" & VLOOKUP($E119,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF120&\"8\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!C\"&$BI120)/$Q120,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF120&\"9\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!D\"&$BI120)/$Q120,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF120&\"10\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!E\"&$BI120)/$Q120,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF120&\"11\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!F\"&$BI120)/$Q120,\"\")),\"\")","v":0},"",null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E120),\"\",VLOOKUP($E120,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E120),\"\",VLOOKUP($E120,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F120),(K120*VLOOKUP(MID(F120,FIND(\"(\",F120)+1,LEN(F120)-FIND(\"(\",F120)-1),EnergyUnitsTable,3,FALSE))/(K125*VLOOKUP(MID(F125,FIND(\"(\",F125)+1,LEN(F125)-FIND(\"(\",F125)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y"]
["G","Lighting in Apartments",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E121),\"\",\"Consumption (\" & VLOOKUP($E121,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,{"$f":"IFERROR(AVERAGEIF(G121:J121,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E121),\"\",VLOOKUP($E121,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E121),\"\",VLOOKUP($E121,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F121),(K121*VLOOKUP(MID(F121,FIND(\"(\",F121)+1,LEN(F121)-FIND(\"(\",F121)-1),EnergyUnitsTable,3,FALSE))/(K122*VLOOKUP(MID(F122,FIND(\"(\",F122)+1,LEN(F122)-FIND(\"(\",F122)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D121=\"x\",K121,0)","v":0},{"$f":"IF(E121=\"Electricity\",\"kWh\",IF(E121=\"Natural Gas\",\"THERM\",IF(E121=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D121=\"x\",FALSE,TRUE)","v":true},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"M","Stand-alone Base Utilities","Electricity"]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E121),\"\",\"Demand (\" & VLOOKUP($E121,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,{"$f":"IFERROR(AVERAGEIF(G122:J122,\"<>0\"),\"\")","v":""},null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F122),(K122*VLOOKUP(MID(F122,FIND(\"(\",F122)+1,LEN(F122)-FIND(\"(\",F122)-1),EnergyUnitsTable,3,FALSE))/(K125*VLOOKUP(MID(F125,FIND(\"(\",F125)+1,LEN(F125)-FIND(\"(\",F125)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Z"]
["G","Interior lighting - process",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E123),\"\",\"Consumption (\" & VLOOKUP($E123,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","",{"$f":"IFERROR(AVERAGEIF(G123:J123,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E123),\"\",VLOOKUP($E123,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E123),\"\",VLOOKUP($E123,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F123),(K123*VLOOKUP(MID(F123,FIND(\"(\",F123)+1,LEN(F123)-FIND(\"(\",F123)-1),EnergyUnitsTable,3,FALSE))/(K124*VLOOKUP(MID(F124,FIND(\"(\",F124)+1,LEN(F124)-FIND(\"(\",F124)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D123=\"x\",K123,0)","v":""},{"$f":"IF(E123=\"Electricity\",\"kWh\",IF(E123=\"Natural Gas\",\"THERM\",IF(E123=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D123=\"x\",TRUE,FALSE)","v":true},null,"","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG123<>\"\",IFERROR(MATCH(BG123&BH123,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E123),\"\",\"Demand (\" & VLOOKUP($E123,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","",{"$f":"IFERROR(AVERAGEIF(G124:J124,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E124),\"\",VLOOKUP($E124,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E124),\"\",VLOOKUP($E124,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F124),(K124*VLOOKUP(MID(F124,FIND(\"(\",F124)+1,LEN(F124)-FIND(\"(\",F124)-1),EnergyUnitsTable,3,FALSE))/(K163*VLOOKUP(MID(F163,FIND(\"(\",F163)+1,LEN(F163)-FIND(\"(\",F163)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,"","","",""]
["G","Exterior lighting",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E125),\"\",\"Consumption (\" & VLOOKUP($E125,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,{"$f":"IFERROR(AVERAGEIF(G125:J125,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E125),\"\",VLOOKUP($E125,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E125),\"\",VLOOKUP($E125,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F125),(K125*VLOOKUP(MID(F125,FIND(\"(\",F125)+1,LEN(F125)-FIND(\"(\",F125)-1),EnergyUnitsTable,3,FALSE))/(K126*VLOOKUP(MID(F126,FIND(\"(\",F126)+1,LEN(F126)-FIND(\"(\",F126)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D125=\"x\",K125,0)","v":0},{"$f":"IF(E125=\"Electricity\",\"kWh\",IF(E125=\"Natural Gas\",\"THERM\",IF(E125=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D125=\"x\",FALSE,TRUE)","v":true},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W","Stand-alone Base Utilities","Electricity",{"$f":"IF(BG125<>\"\",IFERROR(MATCH(BG125&BH125,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":15}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E125),\"\",\"Demand (\" & VLOOKUP($E125,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,"",null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F126),(K126*VLOOKUP(MID(F126,FIND(\"(\",F126)+1,LEN(F126)-FIND(\"(\",F126)-1),EnergyUnitsTable,3,FALSE))/(K127*VLOOKUP(MID(F127,FIND(\"(\",F127)+1,LEN(F127)-FIND(\"(\",F127)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AJ"]
["G","Space heating",null,null,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E127),\"\",\"Consumption (\" & VLOOKUP($E127,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,"",null,null,null,null,null,"",{"$f":"IFERROR(IF(ISBLANK($E127),\"\",VLOOKUP($E127,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F127),(K127*VLOOKUP(MID(F127,FIND(\"(\",F127)+1,LEN(F127)-FIND(\"(\",F127)-1),EnergyUnitsTable,3,FALSE))/(K128*VLOOKUP(MID(F128,FIND(\"(\",F128)+1,LEN(F128)-FIND(\"(\",F128)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D127=\"x\",K127,0)","v":0},{"$f":"IF(E127=\"Electricity\",\"kWh\",IF(E127=\"Natural Gas\",\"THERM\",IF(E127=\"District Cooling\",\"MWh\",\"\")))","v":"THERM"},null,{"$f":"IF(D127=\"x\",FALSE,TRUE)","v":true},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BA","Space Heating","Gas",{"$f":"IF(BG127<>\"\",IFERROR(MATCH(BG127&BH127,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":9}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E127),\"\",\"Demand (\" & VLOOKUP($E127,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F128),(K128*VLOOKUP(MID(F128,FIND(\"(\",F128)+1,LEN(F128)-FIND(\"(\",F128)-1),EnergyUnitsTable,3,FALSE))/(K133*VLOOKUP(MID(F133,FIND(\"(\",F133)+1,LEN(F133)-FIND(\"(\",F133)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,"","","",""]
["G","Space heating",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E129),\"\",\"Consumption (\" & VLOOKUP($E129,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,{"$f":"IFERROR(AVERAGEIF(G129:J129,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E129),\"\",VLOOKUP($E129,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E129),\"\",VLOOKUP($E129,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F129),(K129*VLOOKUP(MID(F129,FIND(\"(\",F129)+1,LEN(F129)-FIND(\"(\",F129)-1),EnergyUnitsTable,3,FALSE))/(K130*VLOOKUP(MID(F130,FIND(\"(\",F130)+1,LEN(F130)-FIND(\"(\",F130)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D129=\"x\",K129,0)","v":0},{"$f":"IF(E129=\"Electricity\",\"kWh\",IF(E129=\"Natural Gas\",\"THERM\",IF(E129=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D129=\"x\",FALSE,TRUE)","v":true},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O",null,null,{"$f":"IF(BG129<>\"\",IFERROR(MATCH(BG129&BH129,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E129),\"\",\"Demand (\" & VLOOKUP($E129,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,{"$f":"IFERROR(AVERAGEIF(G130:J130,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E130),\"\",VLOOKUP($E130,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E130),\"\",VLOOKUP($E130,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F130),(K130*VLOOKUP(MID(F130,FIND(\"(\",F130)+1,LEN(F130)-FIND(\"(\",F130)-1),EnergyUnitsTable,3,FALSE))/(K169*VLOOKUP(MID(F169,FIND(\"(\",F169)+1,LEN(F169)-FIND(\"(\",F169)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AB"]
["G","Heat Pump Supplementary",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E131),\"\",\"Consumption (\" & VLOOKUP($E131,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,{"$f":"IFERROR(AVERAGEIF(G131:J131,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E131),\"\",VLOOKUP($E131,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E131),\"\",VLOOKUP($E131,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F131),(K131*VLOOKUP(MID(F131,FIND(\"(\",F131)+1,LEN(F131)-FIND(\"(\",F131)-1),EnergyUnitsTable,3,FALSE))/(K132*VLOOKUP(MID(F132,FIND(\"(\",F132)+1,LEN(F132)-FIND(\"(\",F132)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D131=\"x\",K131,0)","v":0},{"$f":"IF(E131=\"Electricity\",\"kWh\",IF(E131=\"Natural Gas\",\"THERM\",IF(E131=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D131=\"x\",FALSE,TRUE)","v":true},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"U",null,null,{"$f":"IF(BG131<>\"\",IFERROR(MATCH(BG131&BH131,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E131),\"\",\"Demand (\" & VLOOKUP($E131,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,{"$f":"IFERROR(AVERAGEIF(G132:J132,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E132),\"\",VLOOKUP($E132,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E132),\"\",VLOOKUP($E132,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F132),(K132*VLOOKUP(MID(F132,FIND(\"(\",F132)+1,LEN(F132)-FIND(\"(\",F132)-1),EnergyUnitsTable,3,FALSE))/(K129*VLOOKUP(MID(F129,FIND(\"(\",F129)+1,LEN(F129)-FIND(\"(\",F129)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AH"]
["G","Space cooling",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E133),\"\",\"Consumption (\" & VLOOKUP($E133,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,"",null,null,null,null,null,"","","",null,{"$f":"IF(D133=\"x\",K133,0)","v":0},{"$f":"IF(E133=\"Electricity\",\"kWh\",IF(E133=\"Natural Gas\",\"THERM\",IF(E133=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D133=\"x\",FALSE,TRUE)","v":true},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"P","Space Cooling","Electricity",{"$f":"IF(BG133<>\"\",IFERROR(MATCH(BG133&BH133,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":10}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E133),\"\",\"Demand (\" & VLOOKUP($E133,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,"",null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F134),(K134*VLOOKUP(MID(F134,FIND(\"(\",F134)+1,LEN(F134)-FIND(\"(\",F134)-1),EnergyUnitsTable,3,FALSE))/(K137*VLOOKUP(MID(F137,FIND(\"(\",F137)+1,LEN(F137)-FIND(\"(\",F137)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AC"]
["G","Space cooling",null,null,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E135),\"\",\"Consumption (\" & VLOOKUP($E135,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,{"$f":"IFERROR(AVERAGEIF(G135:J135,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E135),\"\",VLOOKUP($E135,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E135),\"\",VLOOKUP($E135,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F135),(K135*VLOOKUP(MID(F135,FIND(\"(\",F135)+1,LEN(F135)-FIND(\"(\",F135)-1),EnergyUnitsTable,3,FALSE))/(K136*VLOOKUP(MID(F136,FIND(\"(\",F136)+1,LEN(F136)-FIND(\"(\",F136)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D135=\"x\",K135,0)","v":0},{"$f":"IF(E135=\"Electricity\",\"kWh\",IF(E135=\"Natural Gas\",\"THERM\",IF(E135=\"District Cooling\",\"MWh\",\"\")))","v":"THERM"},null,{"$f":"IF(D135=\"x\",FALSE,TRUE)","v":true},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BB",null,null,{"$f":"IF(BG135<>\"\",IFERROR(MATCH(BG135&BH135,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E135),\"\",\"Demand (\" & VLOOKUP($E135,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","",{"$f":"IFERROR(AVERAGEIF(G136:J136,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E136),\"\",VLOOKUP($E136,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E136),\"\",VLOOKUP($E136,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F136),(K136*VLOOKUP(MID(F136,FIND(\"(\",F136)+1,LEN(F136)-FIND(\"(\",F136)-1),EnergyUnitsTable,3,FALSE))/(K173*VLOOKUP(MID(F173,FIND(\"(\",F173)+1,LEN(F173)-FIND(\"(\",F173)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,"","","",""]
["G","Pumps",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E137),\"\",\"Consumption (\" & VLOOKUP($E137,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,"",null,null,null,null,null,"","","",null,{"$f":"IF(D137=\"x\",K137,0)","v":0},{"$f":"IF(E137=\"Electricity\",\"kWh\",IF(E137=\"Natural Gas\",\"THERM\",IF(E137=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D137=\"x\",FALSE,TRUE)","v":true},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R","Pumps","Electricity",{"$f":"IF(BG137<>\"\",IFERROR(MATCH(BG137&BH137,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":11}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E137),\"\",\"Demand (\" & VLOOKUP($E137,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,"",null,null,null,null,null,"","","",null,null,null,null,null,null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AE"]
["G","Heat rejection",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E139),\"\",\"Consumption (\" & VLOOKUP($E139,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,"",null,null,null,null,null,"","","",null,{"$f":"IF(D139=\"x\",K139,0)","v":0},{"$f":"IF(E139=\"Electricity\",\"kWh\",IF(E139=\"Natural Gas\",\"THERM\",IF(E139=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D139=\"x\",FALSE,TRUE)","v":true},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Q","Heat Rejection","Electricity",{"$f":"IF(BG139<>\"\",IFERROR(MATCH(BG139&BH139,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":12}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E139),\"\",\"Demand (\" & VLOOKUP($E139,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,"",null,null,null,null,null,"","","",null,null,null,null,null,null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AD"]
["G","Fans - interior ventilation",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E141),\"\",\"Consumption (\" & VLOOKUP($E141,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,"",null,null,null,null,null,"","","",null,{"$f":"IF(D141=\"x\",K141,0)","v":0},{"$f":"IF(E141=\"Electricity\",\"kWh\",IF(E141=\"Natural Gas\",\"THERM\",IF(E141=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D141=\"x\",FALSE,TRUE)","v":true},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S","Fans - Conditioned","Electricity",{"$f":"IF(BG141<>\"\",IFERROR(MATCH(BG141&BH141,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":13}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E141),\"\",\"Demand (\" & VLOOKUP($E141,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,"",null,null,null,null,null,"","","",null,null,null,null,null,null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AF"]
["G","Fans - parking garage",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E143),\"\",\"Consumption (\" & VLOOKUP($E143,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,{"$f":"IF(D143=\"x\",K143,0)","v":0},{"$f":"IF(E143=\"Electricity\",\"kWh\",IF(E143=\"Natural Gas\",\"THERM\",IF(E143=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D143=\"x\",FALSE,TRUE)","v":true},null,"","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG143<>\"\",IFERROR(MATCH(BG143&BH143,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E143),\"\",\"Demand (\" & VLOOKUP($E143,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F144),(K144*VLOOKUP(MID(F144,FIND(\"(\",F144)+1,LEN(F144)-FIND(\"(\",F144)-1),EnergyUnitsTable,3,FALSE))/(K147*VLOOKUP(MID(F147,FIND(\"(\",F147)+1,LEN(F147)-FIND(\"(\",F147)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,"","","",""]
["G","Fans - Kitchen Ventilation",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E145),\"\",\"Consumption (\" & VLOOKUP($E145,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","",{"$f":"IFERROR(AVERAGEIF(G145:J145,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E145),\"\",VLOOKUP($E145,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E145),\"\",VLOOKUP($E145,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F145),(K145*VLOOKUP(MID(F145,FIND(\"(\",F145)+1,LEN(F145)-FIND(\"(\",F145)-1),EnergyUnitsTable,3,FALSE))/(K146*VLOOKUP(MID(F146,FIND(\"(\",F146)+1,LEN(F146)-FIND(\"(\",F146)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D145=\"x\",K145,0)","v":0},{"$f":"IF(E145=\"Electricity\",\"kWh\",IF(E145=\"Natural Gas\",\"THERM\",IF(E145=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D145=\"x\",FALSE,TRUE)","v":true},null,"","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG145<>\"\",IFERROR(MATCH(BG145&BH145,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E145),\"\",\"Demand (\" & VLOOKUP($E145,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","",{"$f":"IFERROR(AVERAGEIF(G146:J146,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E146),\"\",VLOOKUP($E146,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E146),\"\",VLOOKUP($E146,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F146),(K146*VLOOKUP(MID(F146,FIND(\"(\",F146)+1,LEN(F146)-FIND(\"(\",F146)-1),EnergyUnitsTable,3,FALSE))/(K157*VLOOKUP(MID(F157,FIND(\"(\",F157)+1,LEN(F157)-FIND(\"(\",F157)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,"","","",""]
["G","Service water heating",null,null,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E147),\"\",\"Consumption (\" & VLOOKUP($E147,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,"",null,null,null,null,null,"","","",null,{"$f":"IF(D147=\"x\",K147,0)","v":0},{"$f":"IF(E147=\"Electricity\",\"kWh\",IF(E147=\"Natural Gas\",\"THERM\",IF(E147=\"District Cooling\",\"MWh\",\"\")))","v":"THERM"},null,{"$f":"IF(D147=\"x\",FALSE,TRUE)","v":true},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BH","Stand-alone Base Utilities","Gas",{"$f":"IF(BG147<>\"\",IFERROR(MATCH(BG147&BH147,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":16}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E147),\"\",\"Demand (\" & VLOOKUP($E147,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F148),(K148*VLOOKUP(MID(F148,FIND(\"(\",F148)+1,LEN(F148)-FIND(\"(\",F148)-1),EnergyUnitsTable,3,FALSE))/(K151*VLOOKUP(MID(F151,FIND(\"(\",F151)+1,LEN(F151)-FIND(\"(\",F151)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,"","","",""]
["G","Service water heating",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E149),\"\",\"Consumption (\" & VLOOKUP($E149,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,{"$f":"IFERROR(AVERAGEIF(G149:J149,\"<>0\"),\"\")","v":""},null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F149),(K149*VLOOKUP(MID(F149,FIND(\"(\",F149)+1,LEN(F149)-FIND(\"(\",F149)-1),EnergyUnitsTable,3,FALSE))/(K150*VLOOKUP(MID(F150,FIND(\"(\",F150)+1,LEN(F150)-FIND(\"(\",F150)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D149=\"x\",K149,0)","v":0},{"$f":"IF(E149=\"Electricity\",\"kWh\",IF(E149=\"Natural Gas\",\"THERM\",IF(E149=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D149=\"x\",FALSE,TRUE)","v":true},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"V","Stand-alone Base Utilities","Gas",{"$f":"IF(BG149<>\"\",IFERROR(MATCH(BG149&BH149,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":16}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E149),\"\",\"Demand (\" & VLOOKUP($E149,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,"",null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F150),(K150*VLOOKUP(MID(F150,FIND(\"(\",F150)+1,LEN(F150)-FIND(\"(\",F150)-1),EnergyUnitsTable,3,FALSE))/(K153*VLOOKUP(MID(F153,FIND(\"(\",F153)+1,LEN(F153)-FIND(\"(\",F153)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AI"]
["G","Misc Equipment",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E151),\"\",\"Consumption (\" & VLOOKUP($E151,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF151&\"8\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!C\"&$BI151)/$Q151,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF151&\"9\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!D\"&$BI151)/$Q151,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF151&\"10\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!E\"&$BI151)/$Q151,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF151&\"11\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!F\"&$BI151)/$Q151,\"\")),\"\")","v":0},"",null,null,null,null,null,"","","",null,{"$f":"IF(D151=\"x\",K151,0)","v":""},{"$f":"IF(E151=\"Electricity\",\"kWh\",IF(E151=\"Natural Gas\",\"THERM\",IF(E151=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D151=\"x\",TRUE,FALSE)","v":true},null,{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF151&\"8\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!C\"&$BI151)/$Q151,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF151&\"9\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!D\"&$BI151)/$Q151,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF151&\"10\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!E\"&$BI151)/$Q151,\"\")),\"\")","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF151&\"11\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!F\"&$BI151)/$Q151,\"\")),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N","Receptacles - Conditioned","Electricity",{"$f":"IF(BG151<>\"\",IFERROR(MATCH(BG151&BH151,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":14}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E151),\"\",\"Demand (\" & VLOOKUP($E151,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,"",null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F152),(K152*VLOOKUP(MID(F152,FIND(\"(\",F152)+1,LEN(F152)-FIND(\"(\",F152)-1),EnergyUnitsTable,3,FALSE))/(K155*VLOOKUP(MID(F155,FIND(\"(\",F155)+1,LEN(F155)-FIND(\"(\",F155)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AA"]
["G","Misc Equipment",null,"x","Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E153),\"\",\"Consumption (\" & VLOOKUP($E153,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,{"$f":"IFERROR(AVERAGEIF(G153:J153,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E153),\"\",VLOOKUP($E153,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E153),\"\",VLOOKUP($E153,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F153),(K153*VLOOKUP(MID(F153,FIND(\"(\",F153)+1,LEN(F153)-FIND(\"(\",F153)-1),EnergyUnitsTable,3,FALSE))/(K154*VLOOKUP(MID(F154,FIND(\"(\",F154)+1,LEN(F154)-FIND(\"(\",F154)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D153=\"x\",K153,0)","v":""},{"$f":"IF(E153=\"Electricity\",\"kWh\",IF(E153=\"Natural Gas\",\"THERM\",IF(E153=\"District Cooling\",\"MWh\",\"\")))","v":"THERM"},null,{"$f":"IF(D153=\"x\",FALSE,TRUE)","v":false},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AZ",null,null,{"$f":"IF(BG153<>\"\",IFERROR(MATCH(BG153&BH153,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E153),\"\",\"Demand (\" & VLOOKUP($E153,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","",{"$f":"IFERROR(AVERAGEIF(G154:J154,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E154),\"\",VLOOKUP($E154,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E154),\"\",VLOOKUP($E154,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F154),(K154*VLOOKUP(MID(F154,FIND(\"(\",F154)+1,LEN(F154)-FIND(\"(\",F154)-1),EnergyUnitsTable,3,FALSE))/(K169*VLOOKUP(MID(F169,FIND(\"(\",F169)+1,LEN(F169)-FIND(\"(\",F169)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,"","","",""]
["G","IT equipment",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E155),\"\",\"Consumption (\" & VLOOKUP($E155,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,{"$f":"IF(D155=\"x\",K155,0)","v":""},{"$f":"IF(E155=\"Electricity\",\"kWh\",IF(E155=\"Natural Gas\",\"THERM\",IF(E155=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D155=\"x\",TRUE,FALSE)","v":true},null,"","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG155<>\"\",IFERROR(MATCH(BG155&BH155,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E155),\"\",\"Demand (\" & VLOOKUP($E155,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F156),(K156*VLOOKUP(MID(F156,FIND(\"(\",F156)+1,LEN(F156)-FIND(\"(\",F156)-1),EnergyUnitsTable,3,FALSE))/(K123*VLOOKUP(MID(F123,FIND(\"(\",F123)+1,LEN(F123)-FIND(\"(\",F123)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,"","","",""]
["G","Cooking",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E157),\"\",\"Consumption (\" & VLOOKUP($E157,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,{"$f":"IF(D157=\"x\",K157,0)","v":""},{"$f":"IF(E157=\"Electricity\",\"kWh\",IF(E157=\"Natural Gas\",\"THERM\",IF(E157=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D157=\"x\",TRUE,FALSE)","v":true},null,"","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG157<>\"\",IFERROR(MATCH(BG157&BH157,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E157),\"\",\"Demand (\" & VLOOKUP($E157,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,null,null,null,null,null,"","","",""]
["G","Industrial Process",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E159),\"\",\"Consumption (\" & VLOOKUP($E159,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,{"$f":"IF(D159=\"x\",K159,0)","v":""},{"$f":"IF(E159=\"Electricity\",\"kWh\",IF(E159=\"Natural Gas\",\"THERM\",IF(E159=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D159=\"x\",TRUE,FALSE)","v":true},null,"","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG159<>\"\",IFERROR(MATCH(BG159&BH159,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E159),\"\",\"Demand (\" & VLOOKUP($E159,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F160),(K160*VLOOKUP(MID(F160,FIND(\"(\",F160)+1,LEN(F160)-FIND(\"(\",F160)-1),EnergyUnitsTable,3,FALSE))/(K165*VLOOKUP(MID(F165,FIND(\"(\",F165)+1,LEN(F165)-FIND(\"(\",F165)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,"","","",""]
["G","Refrigeration Equipment (Regulated)",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E161),\"\",\"Consumption (\" & VLOOKUP($E161,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,{"$f":"IFERROR(AVERAGEIF(G161:J161,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E161),\"\",VLOOKUP($E161,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E161),\"\",VLOOKUP($E161,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F161),(K161*VLOOKUP(MID(F161,FIND(\"(\",F161)+1,LEN(F161)-FIND(\"(\",F161)-1),EnergyUnitsTable,3,FALSE))/(K162*VLOOKUP(MID(F162,FIND(\"(\",F162)+1,LEN(F162)-FIND(\"(\",F162)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D161=\"x\",K161,0)","v":0},{"$f":"IF(E161=\"Electricity\",\"kWh\",IF(E161=\"Natural Gas\",\"THERM\",IF(E161=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D161=\"x\",FALSE,TRUE)","v":true},null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T",null,null,{"$f":"IF(BG161<>\"\",IFERROR(MATCH(BG161&BH161,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E161),\"\",\"Demand (\" & VLOOKUP($E161,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,0,0,{"$f":"IFERROR(AVERAGEIF(G162:J162,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E162),\"\",VLOOKUP($E162,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E162),\"\",VLOOKUP($E162,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F162),(K162*VLOOKUP(MID(F162,FIND(\"(\",F162)+1,LEN(F162)-FIND(\"(\",F162)-1),EnergyUnitsTable,3,FALSE))/(K169*VLOOKUP(MID(F169,FIND(\"(\",F169)+1,LEN(F169)-FIND(\"(\",F169)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AG"]
["G","Refrigeration Equipment (Unregulated)",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E163),\"\",\"Consumption (\" & VLOOKUP($E163,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","",{"$f":"IFERROR(AVERAGEIF(G163:J163,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E163),\"\",VLOOKUP($E163,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E163),\"\",VLOOKUP($E163,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F163),(K163*VLOOKUP(MID(F163,FIND(\"(\",F163)+1,LEN(F163)-FIND(\"(\",F163)-1),EnergyUnitsTable,3,FALSE))/(K164*VLOOKUP(MID(F164,FIND(\"(\",F164)+1,LEN(F164)-FIND(\"(\",F164)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D163=\"x\",K163,0)","v":""},{"$f":"IF(E163=\"Electricity\",\"kWh\",IF(E163=\"Natural Gas\",\"THERM\",IF(E163=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D163=\"x\",TRUE,FALSE)","v":true},null,"","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG163<>\"\",IFERROR(MATCH(BG163&BH163,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E163),\"\",\"Demand (\" & VLOOKUP($E163,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","",{"$f":"IFERROR(AVERAGEIF(G164:J164,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E164),\"\",VLOOKUP($E164,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E164),\"\",VLOOKUP($E164,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F164),(K164*VLOOKUP(MID(F164,FIND(\"(\",F164)+1,LEN(F164)-FIND(\"(\",F164)-1),EnergyUnitsTable,3,FALSE))/(K145*VLOOKUP(MID(F145,FIND(\"(\",F145)+1,LEN(F145)-FIND(\"(\",F145)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,"","","",""]
["G","Elevators and escalators",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E165),\"\",\"Consumption (\" & VLOOKUP($E165,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F165),(K165*VLOOKUP(MID(F165,FIND(\"(\",F165)+1,LEN(F165)-FIND(\"(\",F165)-1),EnergyUnitsTable,3,FALSE))/(K166*VLOOKUP(MID(F166,FIND(\"(\",F166)+1,LEN(F166)-FIND(\"(\",F166)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D165=\"x\",K165,0)","v":0},{"$f":"IF(E165=\"Electricity\",\"kWh\",IF(E165=\"Natural Gas\",\"THERM\",IF(E165=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D165=\"x\",FALSE,TRUE)","v":true},null,"","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG165<>\"\",IFERROR(MATCH(BG165&BH165,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E165),\"\",\"Demand (\" & VLOOKUP($E165,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F166),(K166*VLOOKUP(MID(F166,FIND(\"(\",F166)+1,LEN(F166)-FIND(\"(\",F166)-1),EnergyUnitsTable,3,FALSE))/(K131*VLOOKUP(MID(F131,FIND(\"(\",F131)+1,LEN(F131)-FIND(\"(\",F131)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,"","","",""]
["G","Building Transformers",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E167),\"\",\"Consumption (\" & VLOOKUP($E167,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","",{"$f":"IFERROR(AVERAGEIF(G167:J167,\"<>0\"),\"\")","v":""},null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F167),(K167*VLOOKUP(MID(F167,FIND(\"(\",F167)+1,LEN(F167)-FIND(\"(\",F167)-1),EnergyUnitsTable,3,FALSE))/(K168*VLOOKUP(MID(F168,FIND(\"(\",F168)+1,LEN(F168)-FIND(\"(\",F168)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IF(D167=\"x\",K167,0)","v":0},{"$f":"IF(E167=\"Electricity\",\"kWh\",IF(E167=\"Natural Gas\",\"THERM\",IF(E167=\"District Cooling\",\"MWh\",\"\")))","v":"kWh"},null,{"$f":"IF(D167=\"x\",TRUE,FALSE)","v":false},null,"","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG167<>\"\",IFERROR(MATCH(BG167&BH167,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E167),\"\",\"Demand (\" & VLOOKUP($E167,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,null,null,null,null,null,"","","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E169),\"\",\"Consumption (\" & VLOOKUP($E169,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,{"$f":"IF(D169=\"x\",K169,0)","v":0},{"$f":"IF(E169=\"Electricity\",\"kWh\",IF(E169=\"Natural Gas\",\"THERM\",IF(E169=\"District Cooling\",\"MWh\",\"\")))","v":""},null,{"$f":"IF(D169=\"x\",FALSE,TRUE)","v":true},null,"","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG169<>\"\",IFERROR(MATCH(BG169&BH169,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E169),\"\",\"Demand (\" & VLOOKUP($E169,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,null,null,null,null,null,"","","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E171),\"\",\"Consumption (\" & VLOOKUP($E171,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,{"$f":"IF(D171=\"x\",K171,0)","v":0},{"$f":"IF(E171=\"Electricity\",\"kWh\",IF(E171=\"Natural Gas\",\"THERM\",IF(E171=\"District Cooling\",\"MWh\",\"\")))","v":""},null,{"$f":"IF(D171=\"x\",FALSE,TRUE)","v":true},null,"","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG171<>\"\",IFERROR(MATCH(BG171&BH171,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E171),\"\",\"Demand (\" & VLOOKUP($E171,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F172),(K172*VLOOKUP(MID(F172,FIND(\"(\",F172)+1,LEN(F172)-FIND(\"(\",F172)-1),EnergyUnitsTable,3,FALSE))/(K135*VLOOKUP(MID(F135,FIND(\"(\",F135)+1,LEN(F135)-FIND(\"(\",F135)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,null,null,null,null,"","","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E173),\"\",\"Consumption (\" & VLOOKUP($E173,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,{"$f":"IF(D173=\"x\",K173,0)","v":0},{"$f":"IF(E173=\"Electricity\",\"kWh\",IF(E173=\"Natural Gas\",\"THERM\",IF(E173=\"District Cooling\",\"MWh\",\"\")))","v":""},null,{"$f":"IF(D173=\"x\",FALSE,TRUE)","v":true},null,"","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG173<>\"\",IFERROR(MATCH(BG173&BH173,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E173),\"\",\"Demand (\" & VLOOKUP($E173,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,null,null,null,null,null,"","","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E175),\"\",\"Consumption (\" & VLOOKUP($E175,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,{"$f":"IF(D175=\"x\",K175,0)","v":0},{"$f":"IF(E175=\"Electricity\",\"kWh\",IF(E175=\"Natural Gas\",\"THERM\",IF(E175=\"District Cooling\",\"MWh\",\"\")))","v":""},null,{"$f":"IF(D175=\"x\",TRUE,FALSE)","v":false},null,"","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BG175<>\"\",IFERROR(MATCH(BG175&BH175,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E175),\"\",\"Demand (\" & VLOOKUP($E175,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},"","","","","",null,null,null,null,null,"","","",null,null,null,null,null,null,"","","",""]
["G",null,null,null,"Energy_Type","Energy_Units","Baseline_0_Rotation","Baseline_90_Rotation","Baseline_180_Rotation","Baseline_270_Rotation","Baseline_Total",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",""]
["G","Total energy consumption by energy type ",null,null,{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK(E178),\"\",VLOOKUP($E178,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IFERROR(SUMIFS(INDEX(PO_baseline_table,0,MATCH(G$118,PO_baseline_hdr,0)),INDEX(PO_baseline_table,0,MATCH($E$118,PO_baseline_hdr,0)),$E178,INDEX(PO_baseline_table,0,MATCH($F$118,PO_baseline_hdr,0)),\"=Con*\"),\"\")","v":0},0,0,0,0,"","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E178),\"\",VLOOKUP($E178,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E178),\"\",VLOOKUP($E178,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IF(D178=\"x\",K178,0)","v":0},{"$f":"IF(E178=\"Electricity\",\"kWh\",IF(E178=\"Natural Gas\",\"THERM\",IF(E178=\"District Cooling\",\"MWh\",\"\")))","v":""},null,{"$f":"IF(D178=\"x\",TRUE,FALSE)","v":false}]
["G",null,null,null,"","",0,0,0,0,0,"","",null,null,null,"",""]
["G",null,null,null,"","",0,0,0,0,0,"","",null,null,null,"","",null,null,{"$f":"IF(D180=\"x\",K180,0)","v":0},{"$f":"IF(E180=\"Electricity\",\"kWh\",IF(E180=\"Natural Gas\",\"THERM\",IF(E180=\"District Cooling\",\"MWh\",\"\")))","v":""},null,{"$f":"IF(D180=\"x\",TRUE,FALSE)","v":false}]
["G",null,null,null,"","",0,0,0,0,0,"","",null,null,null,"",""]
["G",null,null,null,"","",0,0,0,0,0,"","",null,null,null,"","",null,null,{"$f":"IF(D182=\"x\",K182,0)","v":0},{"$f":"IF(E182=\"Electricity\",\"kWh\",IF(E182=\"Natural Gas\",\"THERM\",IF(E182=\"District Cooling\",\"MWh\",\"\")))","v":""},null,{"$f":"IF(D182=\"x\",TRUE,FALSE)","v":false}]
["G",null,null,null,"","",0,0,0,0,0,"","",null,null,null,"",""]
["G",{"$f":"\"Total site energy (\" & PO_SiteUnits & \")\"","v":"Total site energy (Btu x 10^6)"},null,null,null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_5_Table,0,MATCH(G$177,PO_Enrgy_5_Hdr,0)),INDEX(PO_Enrgy_5_Table,0,MATCH($Q177,PO_Enrgy_5_Hdr,0))),\"\")","v":0},0,0,0,0,"",""]
["G",{"$f":"\"Total source energy (\" & PO_SourceUnits & \")\"","v":"Total source energy (Btu x 10^6)"},null,null,null,null,{"$f":"IFERROR(SUMPRODUCT(G$178:G$179,$R$178:$R$179),0)","v":0},{"$f":"IFERROR(SUMPRODUCT(H$178:H$179,$R$178:$R$179),0)","v":0},0,0,0,0,0]
["G"]
["G","Table 12.5: Baseline building annual energy cost by energy type "]
["G","Energy Type",null,null,null,null,"Baseline 0° rotation","Baseline 90° rotation","Baseline 180° rotation","Baseline 270° rotation","Baseline Design Total",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Energy_Type",null,null,null,null,"Baseline_0_Rotation","Baseline_90_Rotation","Baseline_180_Rotation","Baseline_270_Rotation","Base_Cost",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B190),\"\",VLOOKUP($B190,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(SimTool=\"eQuest\",'Results from eQuest'!BQ8+'Results from eQuest'!BR8,\"\")","v":0},{"$f":"IF(SimTool=\"eQuest\",'Results from eQuest'!BQ9+'Results from eQuest'!BR9,\"\")","v":0},{"$f":"IF(SimTool=\"eQuest\",'Results from eQuest'!BQ10+'Results from eQuest'!BR10,\"\")","v":0},{"$f":"IF(SimTool=\"eQuest\",'Results from eQuest'!BQ11+'Results from eQuest'!BR11,\"\")","v":0},{"$f":"IFERROR(AVERAGEIF(G190:J190,\"<>0\"),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B190),\"\",VLOOKUP($B190,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B190),\"\",VLOOKUP($B190,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","",null,null,null,"",{"$f":"IF(SimTool=\"eQuest\",'Results from eQuest'!BP8,\"\")","v":0},{"$f":"IF(SimTool=\"eQuest\",'Results from eQuest'!BP9,\"\")","v":0},{"$f":"IF(SimTool=\"eQuest\",'Results from eQuest'!BP10,\"\")","v":0},{"$f":"IF(SimTool=\"eQuest\",'Results from eQuest'!BP11,\"\")","v":0},{"$f":"IFERROR(AVERAGEIF(G191:J191,\"<>0\"),\"\")","v":""},null,null,null,null,null,"",""]
["G","",null,null,null,"",null,null,null,null,"",null,null,null,null,null,"",""]
["G","",null,null,null,"",null,null,null,null,"",null,null,null,null,null,"",""]
["G","",null,null,null,"",null,null,null,null,"",null,null,null,null,null,"",""]
["G","",null,null,null,"",null,null,null,null,"",null,null,null,null,null,"",""]
["G","Baseline annual energy cost",null,null,null,null,{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_6_Table,0,MATCH(G$189,PO_Enrgy_6_Hdr,0))),\"\")","v":0},0,0,0,0,"",""]
["G"]
["G"]
["G","Table 12.6: Proposed energy summary by end use"]
["G","Complete the table below, providing information on energy consumption and demand by end-use. If an end-use has two energy types (e.g. proposed case space heating includes both fossil fuel and electric), enter the end-use twice in the table, and list the two different energy types."]
["G","ASHRAE 90.1-2010 without Addenda (District Energy Modeling Path 1): Report the district energy type (District Cooling, District Hot Water, or District Steam) for the cooling and heating end-uses as applicable for both the baseline and proposed."]
["G","Full DES Performance Accounting method (District Energy Modeling Path 2): Report the baseline energy as if the thermal energy is produced in the building.  Report the proposed energy used to generate and distribute the district thermal energy serving the building based on calculated average district thermal efficiencies (e.g. report the electricity used to generate and distribute chilled water to the building).\n"]
["G","Streamlined DES Accounting Method (District Energy Modeling Path 3): Report the energy type (District Cooling, District Hot Water, or District Steam for the cooling and heating end-uses as applicable for both the baseline and proposed. "]
["G","Data Centers: The energy consumption for IT equipment must be metered and reported separately from other end-uses in the energy model, and in the tables below to allow the proper determination of the PUE. Complete the table below for the baseline using the full build-out IT loads for the proposed design.\n"]
["G","Retail: The energy consumption for cooking, refrigeration, and kitchen ventilation fans must be metered and reported separately from other end-uses in the energy model and in the tables below. Energy savings or consumption attributable to unregulated equipment, other than Commercial Kitchen Equipment, Supermarket Refrigeration, Walk-in Coolers and Freezers, or Commercial Kitchen Ventilation listed in Tables 1 – 4 of the LEED v4 BD+C: Retail and ID+C: Retail Rating System Appendix 3 must be claimed via Exceptional Calculation Methodology."]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Software Link References"]
["G","End Use",null,"Unregulated?","Energy Type","Units of \nAnnual Energy and Peak Demand","Baseline","Proposed Design","Energy / Demand Savings \nper End-Use","End Use \nPercent Contribution to Total Energy Savings","End Use \nPercent \nContribution to \nTotal Cost Savings",null,"Percent of Total Proposed  \nSite Energy Consumption",null,null,null,null,null,null,null,null,null,null,"contribution rank",null,"Rank with ties","rank no ties",null,null,null,null,null,null,"QC_EFLH",null,"1 notes if this is a regulated or unregulated \"Other\" load","if unregulated, this is the difference between baseline and proposed consumptions","Proposed Design CL H",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):",null,null,"eQUEST Outputs End Use Column","TRACE End Use Label","TRACE End Use Fuel Label","TRACE Output End Use Row"]
["G","End_Use",null,"Unregulated","Energy_Type","Energy_Units","Base_Consumption_Demand","Design_Consumption_Demand","End_Use_Savings","End_Use_Contribution_to_Energy_Savings","End_Use_Contribution_to_Cost_Savings",null,"Percent_Design_Site_Consumption",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion","Base_EFLH","Design_EFLH",null,null,null,"contribution rank",null,"Rank with ties","rank no ties"]
["G",{"$f":"INDEX(PO_baseline_table,1, 1)","v":"Interior lighting"},null,{"$f":"INDEX(PO_baseline_table,1, 3)","v":0},{"$f":"INDEX(PO_baseline_table,1, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E209),\"\",\"Consumption (\" & VLOOKUP($E209,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,1, 10)","v":""},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF209&\"13\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!H\"&$BI209)/$Q209,\"\")),\"\")","v":0},{"$f":"IFERROR(1-H209/G209,\"\")","v":""},{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G209-$H209)*VLOOKUP($E209,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G209*VLOOKUP($E209,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H209*VLOOKUP($E209,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H209*Q209)/$H$276,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($E209),\"\",VLOOKUP($E209,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E209),\"\",VLOOKUP($E209,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F209),(G209*VLOOKUP(MID(F209,FIND(\"(\",F209)+1,LEN(F209)-FIND(\"(\",F209)-1),EnergyUnitsTable,3,FALSE))/(G210*VLOOKUP(MID(F210,FIND(\"(\",F210)+1,LEN(F210)-FIND(\"(\",F210)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",$F209),(H209*VLOOKUP(MID($F209,FIND(\"(\",$F209)+1,LEN($F209)-FIND(\"(\",$F209)-1),EnergyUnitsTable,3,FALSE))/(H210*VLOOKUP(MID($F210,FIND(\"(\",$F210)+1,LEN($F210)-FIND(\"(\",$F210)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IF(G209=\"\",\"\",G209*Q209)","v":""},{"$f":"IF(H209=\"\",\"\",H209*Q209)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR($AN209*H209,0)","v":0},{"$f":"IFERROR(G209*VLOOKUP($AF209,PO_Enrgy_8_Table,4,FALSE),0)","v":0},{"$f":"IFERROR(H209*VLOOKUP($AF209,PO_Enrgy_8_Table,7,FALSE),0)","v":0},{"$f":"IFERROR(IF(D209=\"x\",IF(OR(G209/H209>1.03,G209/H209<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J209*100,)","v":0},null,{"$f":"RANK(AA209,$AA$209:$AA$264,0)","v":1},{"$f":"AC209","v":1},{"$f":"B209","v":"Interior lighting"},{"$f":"IF(D209=\"x\",1,0)","v":0},{"$f":"IFERROR(G209/'6b - General Lighting'!O108,\"\")","v":""},null,{"$f":"IF(AND(AF209=1,AJ209=1),1,0)","v":0},null,{"$f":"IFERROR(IF(D209=\"x\",(ABS(G209-H209))/(MIN(G209,H209)),\"\"),0)","v":""},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF209&\"13\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!H\"&$BI209)/$Q209,\"\")),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BF119","v":"L"},"Lighting - Conditioned","Electricity",{"$f":"IF(BG209<>\"\",IFERROR(MATCH(BG209&BH209,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":7}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E209),\"\",\"Demand (\" & VLOOKUP($E209,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,2, 10)","v":""},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF210&\"13\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!H\"&$BI210)/$Q210,\"\")),\"\")","v":0},{"$f":"IFERROR(1-H210/G210,\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E210),\"\",VLOOKUP($E210,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E210),\"\",VLOOKUP($E210,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F210),(G210*VLOOKUP(MID(F210,FIND(\"(\",F210)+1,LEN(F210)-FIND(\"(\",F210)-1),EnergyUnitsTable,3,FALSE))/(G211*VLOOKUP(MID(F211,FIND(\"(\",F211)+1,LEN(F211)-FIND(\"(\",F211)-1),DemandTable,3,FALSE)),1),\"\")","v":""},"",null,null,0,0,0,null,null,null,null,null,null,{"$f":"IF(D210=\"x\",1,0)","v":0},null,null,{"$f":"IF(AND(AF210=1,AJ210=1),1,0)","v":0},null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y",0,0]
["G",{"$f":"INDEX(PO_baseline_table,3, 1)","v":"Lighting in Apartments"},null,{"$f":"INDEX(PO_baseline_table,3, 3)","v":0},{"$f":"INDEX(PO_baseline_table,3, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E211),\"\",\"Consumption (\" & VLOOKUP($E211,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,3, 10)","v":""},0,{"$f":"IFERROR(1-H211/G211,\"\")","v":""},{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G211-$H211)*VLOOKUP($E211,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G211*VLOOKUP($E211,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H211*VLOOKUP($E211,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H211*Q211)/$H$276,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($E211),\"\",VLOOKUP($E211,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E211),\"\",VLOOKUP($E211,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},"","",{"$f":"IF(G211=\"\",\"\",G211*Q211)","v":""},{"$f":"IF(H211=\"\",\"\",H211*Q211)","v":{"$error":"#VALUE!"}},0,0,0,{"$f":"IFERROR(IF(D211=\"x\",IF(OR(G211/H211>1.03,G211/H211<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J211*100,)","v":0},null,{"$f":"RANK(AA211,$AA$209:$AA$264,0)","v":1},{"$f":"AC211+COUNTIF($AC209:$AC$210,AC211)","v":2},{"$f":"B211","v":"Lighting in Apartments"},{"$f":"IF(D211=\"x\",1,0)","v":0},null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BF121","v":"M"},"Stand-alone Base Utilities","Electricity"]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E211),\"\",\"Demand (\" & VLOOKUP($E211,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,4, 10)","v":""},0,{"$f":"IFERROR(1-H212/G212,\"\")","v":""},null,null,null,null,null,null,null,"",{"$f":"IFERROR(IF(ISBLANK($E212),\"\",VLOOKUP($E212,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},"","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Z"]
["G",{"$f":"INDEX(PO_baseline_table,5, 1)","v":"Interior lighting - process"},null,{"$f":"INDEX(PO_baseline_table,5, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,5, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E213),\"\",\"Consumption (\" & VLOOKUP($E213,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,5, 10)","v":""},"",{"$f":"IFERROR(1-H213/G213,\"\")","v":""},{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G213-$H213)*VLOOKUP($E213,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G213*VLOOKUP($E213,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H213*VLOOKUP($E213,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H213*Q213)/$H$276,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($E213),\"\",VLOOKUP($E213,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E213),\"\",VLOOKUP($E213,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},"","",{"$f":"IF(G213=\"\",\"\",G213*Q213)","v":""},{"$f":"IF(H213=\"\",\"\",H213*Q213)","v":""},0,0,0,{"$f":"IFERROR(IF(D213=\"x\",IF(OR(G213/H213>1.03,G213/H213<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J213*100,)","v":0},null,{"$f":"RANK(AA213,$AA$209:$AA$264,0)","v":1},{"$f":"AC213+COUNTIF($AC$209:$AC212,AC213)","v":3},{"$f":"B213","v":"Interior lighting - process"},1,null,null,1,1,0,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BG125","v":"Stand-alone Base Utilities"},"Electricity",{"$f":"IF(BG213<>\"\",IFERROR(MATCH(BG213&BH213,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":15}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E213),\"\",\"Demand (\" & VLOOKUP($E213,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,6, 10)","v":""},"",{"$f":"IFERROR(1-H214/G214,\"\")","v":""},null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_baseline_table,7, 1)","v":"Exterior lighting"},null,{"$f":"INDEX(PO_baseline_table,7, 3)","v":0},{"$f":"INDEX(PO_baseline_table,7, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E215),\"\",\"Consumption (\" & VLOOKUP($E215,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,7, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G215-$H215)*VLOOKUP($E215,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G215*VLOOKUP($E215,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H215*VLOOKUP($E215,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H215*Q215)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G215=\"\",\"\",G215*Q215)","v":""},{"$f":"IF(H215=\"\",\"\",H215*Q215)","v":{"$error":"#VALUE!"}},0,0,0,{"$f":"IFERROR(IF(D215=\"x\",IF(OR(G215/H215>1.03,G215/H215<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J215*100,)","v":0},null,{"$f":"RANK(AA215,$AA$209:$AA$264,0)","v":1},{"$f":"AC215+COUNTIF($AC$209:$AC214,AC215)","v":4},{"$f":"B215","v":"Exterior lighting"},0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W","Space Heating","Gas",{"$f":"IF(BG215<>\"\",IFERROR(MATCH(BG215&BH215,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":9}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E215),\"\",\"Demand (\" & VLOOKUP($E215,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,8, 10)","v":""},0,"",null,null,null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F216),(G216*VLOOKUP(MID(F216,FIND(\"(\",F216)+1,LEN(F216)-FIND(\"(\",F216)-1),EnergyUnitsTable,3,FALSE))/(G219*VLOOKUP(MID(F219,FIND(\"(\",F219)+1,LEN(F219)-FIND(\"(\",F219)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",$F216),(H216*VLOOKUP(MID($F216,FIND(\"(\",$F216)+1,LEN($F216)-FIND(\"(\",$F216)-1),EnergyUnitsTable,3,FALSE))/(H219*VLOOKUP(MID($F219,FIND(\"(\",$F219)+1,LEN($F219)-FIND(\"(\",$F219)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"",0,null,"Is Electric Space Heating Used in the propsoed?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AJ",0,0]
["G",{"$f":"INDEX(PO_baseline_table,9, 1)","v":"Space heating"},null,{"$f":"INDEX(PO_baseline_table,9, 3)","v":0},{"$f":"INDEX(PO_baseline_table,9, 4)","v":"Natural Gas"},{"$f":"IFERROR(IF(ISBLANK(E217),\"\",\"Consumption (\" & VLOOKUP($E217,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,9, 10)","v":""},0,{"$f":"IFERROR(1-H217/G217,\"\")","v":""},{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G217-$H217)*VLOOKUP($E217,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G217*VLOOKUP($E217,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H217*VLOOKUP($E217,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H217*Q217)/$H$276,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($E217),\"\",VLOOKUP($E217,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E217),\"\",VLOOKUP($E217,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F217),(G217*VLOOKUP(MID(F217,FIND(\"(\",F217)+1,LEN(F217)-FIND(\"(\",F217)-1),EnergyUnitsTable,3,FALSE))/(G218*VLOOKUP(MID(F218,FIND(\"(\",F218)+1,LEN(F218)-FIND(\"(\",F218)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",$F217),(H217*VLOOKUP(MID($F217,FIND(\"(\",$F217)+1,LEN($F217)-FIND(\"(\",$F217)-1),EnergyUnitsTable,3,FALSE))/(H218*VLOOKUP(MID($F218,FIND(\"(\",$F218)+1,LEN($F218)-FIND(\"(\",$F218)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IF(G217=\"\",\"\",G217*Q217)","v":""},{"$f":"IF(H217=\"\",\"\",H217*Q217)","v":{"$error":"#VALUE!"}},0,0,0,{"$f":"IFERROR(IF(D217=\"x\",IF(OR(G217/H217>1.03,G217/H217<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J217*100,)","v":0},null,{"$f":"RANK(AA217,$AA$209:$AA$264,0)","v":1},{"$f":"AC217+COUNTIF($AC$209:$AC216,AC217)","v":5},{"$f":"B217","v":"Space heating"},0,null,null,0,null,"",0,null,{"$f":"IF(AND(E217=\"Electricity\",H217>0),1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BA",0,0,{"$f":"IF(BG217<>\"\",IFERROR(MATCH(BG217&BH217,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E217),\"\",\"Demand (\" & VLOOKUP($E217,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,10, 10)","v":""},"",{"$f":"IFERROR(1-H218/G218,\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E218),\"\",VLOOKUP($E218,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E218),\"\",VLOOKUP($E218,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F218),(G218*VLOOKUP(MID(F218,FIND(\"(\",F218)+1,LEN(F218)-FIND(\"(\",F218)-1),EnergyUnitsTable,3,FALSE))/(G251*VLOOKUP(MID(F251,FIND(\"(\",F251)+1,LEN(F251)-FIND(\"(\",F251)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",$F218),(H218*VLOOKUP(MID($F218,FIND(\"(\",$F218)+1,LEN($F218)-FIND(\"(\",$F218)-1),EnergyUnitsTable,3,FALSE))/(H251*VLOOKUP(MID($F251,FIND(\"(\",$F251)+1,LEN($F251)-FIND(\"(\",$F251)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,{"$f":"IF(AND(E219=\"Electricity\",H219>0),1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_baseline_table,11, 1)","v":"Space heating"},null,{"$f":"INDEX(PO_baseline_table,11, 3)","v":0},{"$f":"INDEX(PO_baseline_table,11, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E219),\"\",\"Consumption (\" & VLOOKUP($E219,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,11, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G219-$H219)*VLOOKUP($E219,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G219*VLOOKUP($E219,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H219*VLOOKUP($E219,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H219*Q219)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G219=\"\",\"\",G219*Q219)","v":""},{"$f":"IF(H219=\"\",\"\",H219*Q219)","v":{"$error":"#VALUE!"}},0,0,0,{"$f":"IFERROR(IF(D219=\"x\",IF(OR(G219/H219>1.03,G219/H219<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J219*100,)","v":0},null,{"$f":"RANK(AA219,$AA$209:$AA$264,0)","v":1},{"$f":"AC219+COUNTIF($AC$209:$AC218,AC219)","v":6},{"$f":"B219","v":"Space heating"},0,null,null,0,null,"",0,null,{"$f":"SUM(AN217:AN218)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O",{"$f":"BG133","v":"Space Cooling"},{"$f":"BH133","v":"Electricity"},{"$f":"IF(BG219<>\"\",IFERROR(MATCH(BG219&BH219,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":10}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E219),\"\",\"Demand (\" & VLOOKUP($E219,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,12, 10)","v":""},0,"",null,null,null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F220),(G220*VLOOKUP(MID(F220,FIND(\"(\",F220)+1,LEN(F220)-FIND(\"(\",F220)-1),EnergyUnitsTable,3,FALSE))/(G223*VLOOKUP(MID(F223,FIND(\"(\",F223)+1,LEN(F223)-FIND(\"(\",F223)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",$F220),(H220*VLOOKUP(MID($F220,FIND(\"(\",$F220)+1,LEN($F220)-FIND(\"(\",$F220)-1),EnergyUnitsTable,3,FALSE))/(H223*VLOOKUP(MID($F223,FIND(\"(\",$F223)+1,LEN($F223)-FIND(\"(\",$F223)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AB",{"$f":"BG134","v":0},{"$f":"BH134","v":0}]
["G",{"$f":"INDEX(PO_baseline_table,13, 1)","v":"Heat Pump Supplementary"},null,{"$f":"INDEX(PO_baseline_table,13, 3)","v":0},{"$f":"INDEX(PO_baseline_table,13, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E221),\"\",\"Consumption (\" & VLOOKUP($E221,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,13, 10)","v":""},0,{"$f":"IFERROR(1-H221/G221,\"\")","v":""},{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G221-$H221)*VLOOKUP($E221,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G221*VLOOKUP($E221,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H221*VLOOKUP($E221,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H221*Q221)/$H$276,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($E221),\"\",VLOOKUP($E221,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E221),\"\",VLOOKUP($E221,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F221),(G221*VLOOKUP(MID(F221,FIND(\"(\",F221)+1,LEN(F221)-FIND(\"(\",F221)-1),EnergyUnitsTable,3,FALSE))/(G222*VLOOKUP(MID(F222,FIND(\"(\",F222)+1,LEN(F222)-FIND(\"(\",F222)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",$F221),(H221*VLOOKUP(MID($F221,FIND(\"(\",$F221)+1,LEN($F221)-FIND(\"(\",$F221)-1),EnergyUnitsTable,3,FALSE))/(H222*VLOOKUP(MID($F222,FIND(\"(\",$F222)+1,LEN($F222)-FIND(\"(\",$F222)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IF(G221=\"\",\"\",G221*Q221)","v":""},{"$f":"IF(H221=\"\",\"\",H221*Q221)","v":{"$error":"#VALUE!"}},0,0,0,{"$f":"IFERROR(IF(D221=\"x\",IF(OR(G221/H221>1.03,G221/H221<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J221*100,)","v":0},null,{"$f":"RANK(AA221,$AA$209:$AA$264,0)","v":1},{"$f":"AC221+COUNTIF($AC$209:$AC220,AC221)","v":7},{"$f":"B221","v":"Heat Pump Supplementary"},0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"U",{"$f":"BG171","v":0},0,{"$f":"IF(BG221<>\"\",IFERROR(MATCH(BG221&BH221,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E221),\"\",\"Demand (\" & VLOOKUP($E221,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,14, 10)","v":""},0,{"$f":"IFERROR(1-H222/G222,\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E222),\"\",VLOOKUP($E222,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E222),\"\",VLOOKUP($E222,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F222),(G222*VLOOKUP(MID(F222,FIND(\"(\",F222)+1,LEN(F222)-FIND(\"(\",F222)-1),EnergyUnitsTable,3,FALSE))/(G253*VLOOKUP(MID(F253,FIND(\"(\",F253)+1,LEN(F253)-FIND(\"(\",F253)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",$F222),(H222*VLOOKUP(MID($F222,FIND(\"(\",$F222)+1,LEN($F222)-FIND(\"(\",$F222)-1),EnergyUnitsTable,3,FALSE))/(H253*VLOOKUP(MID($F253,FIND(\"(\",$F253)+1,LEN($F253)-FIND(\"(\",$F253)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AH",0,0]
["G",{"$f":"INDEX(PO_baseline_table,15, 1)","v":"Space cooling"},null,{"$f":"INDEX(PO_baseline_table,15, 3)","v":0},{"$f":"INDEX(PO_baseline_table,15, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E223),\"\",\"Consumption (\" & VLOOKUP($E223,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,15, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G223-$H223)*VLOOKUP($E223,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G223*VLOOKUP($E223,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H223*VLOOKUP($E223,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H223*Q223)/$H$276,\"\")","v":""},null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F223),(G223*VLOOKUP(MID(F223,FIND(\"(\",F223)+1,LEN(F223)-FIND(\"(\",F223)-1),EnergyUnitsTable,3,FALSE))/(G224*VLOOKUP(MID(F224,FIND(\"(\",F224)+1,LEN(F224)-FIND(\"(\",F224)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",$F223),(H223*VLOOKUP(MID($F223,FIND(\"(\",$F223)+1,LEN($F223)-FIND(\"(\",$F223)-1),EnergyUnitsTable,3,FALSE))/(H224*VLOOKUP(MID($F224,FIND(\"(\",$F224)+1,LEN($F224)-FIND(\"(\",$F224)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IF(G223=\"\",\"\",G223*Q223)","v":""},{"$f":"IF(H223=\"\",\"\",H223*Q223)","v":{"$error":"#VALUE!"}},0,0,0,{"$f":"IFERROR(IF(D223=\"x\",IF(OR(G223/H223>1.03,G223/H223<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J223*100,)","v":0},null,{"$f":"RANK(AA223,$AA$209:$AA$264,0)","v":1},{"$f":"AC223+COUNTIF($AC$209:$AC222,AC223)","v":8},{"$f":"B223","v":"Space cooling"},0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"P",{"$f":"BG137","v":"Pumps"},"Electricity",{"$f":"IF(BG223<>\"\",IFERROR(MATCH(BG223&BH223,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":11}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E223),\"\",\"Demand (\" & VLOOKUP($E223,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,16, 10)","v":""},0,"",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AC",0,0]
["G",{"$f":"INDEX(PO_baseline_table,17, 1)","v":"Space cooling"},null,{"$f":"INDEX(PO_baseline_table,17, 3)","v":0},{"$f":"INDEX(PO_baseline_table,17, 4)","v":"Natural Gas"},{"$f":"IFERROR(IF(ISBLANK(E225),\"\",\"Consumption (\" & VLOOKUP($E225,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,17, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G225-$H225)*VLOOKUP($E225,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G225*VLOOKUP($E225,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H225*VLOOKUP($E225,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H225*Q225)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G225=\"\",\"\",G225*Q225)","v":""},{"$f":"IF(H225=\"\",\"\",H225*Q225)","v":{"$error":"#VALUE!"}},0,0,0,{"$f":"IFERROR(IF(D225=\"x\",IF(OR(G225/H225>1.03,G225/H225<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J225*100,)","v":0},null,{"$f":"RANK(AA225,$AA$209:$AA$264,0)","v":1},{"$f":"AC225+COUNTIF($AC$209:$AC224,AC225)","v":9},{"$f":"B225","v":"Space cooling"},0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BB","Heat Rejection","Electricity",{"$f":"IF(BG225<>\"\",IFERROR(MATCH(BG225&BH225,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":12}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E225),\"\",\"Demand (\" & VLOOKUP($E225,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,18, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_baseline_table,19, 1)","v":"Pumps"},null,{"$f":"INDEX(PO_baseline_table,19, 3)","v":0},{"$f":"INDEX(PO_baseline_table,19, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E227),\"\",\"Consumption (\" & VLOOKUP($E227,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,19, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G227-$H227)*VLOOKUP($E227,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G227*VLOOKUP($E227,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H227*VLOOKUP($E227,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H227*Q227)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G227=\"\",\"\",G227*Q227)","v":""},{"$f":"IF(H227=\"\",\"\",H227*Q227)","v":{"$error":"#VALUE!"}},0,0,0,{"$f":"IFERROR(IF(D227=\"x\",IF(OR(G227/H227>1.03,G227/H227<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J227*100,)","v":0},null,{"$f":"RANK(AA227,$AA$209:$AA$264,0)","v":1},{"$f":"AC227+COUNTIF($AC$209:$AC226,AC227)","v":10},{"$f":"B227","v":"Pumps"},0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R","Fans - Conditioned","Electricity",{"$f":"IF(BG227<>\"\",IFERROR(MATCH(BG227&BH227,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":13}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E227),\"\",\"Demand (\" & VLOOKUP($E227,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,20, 10)","v":""},0,"",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AE",0,0]
["G",{"$f":"INDEX(PO_baseline_table,21, 1)","v":"Heat rejection"},null,{"$f":"INDEX(PO_baseline_table,21, 3)","v":0},{"$f":"INDEX(PO_baseline_table,21, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E229),\"\",\"Consumption (\" & VLOOKUP($E229,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,21, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G229-$H229)*VLOOKUP($E229,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G229*VLOOKUP($E229,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H229*VLOOKUP($E229,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H229*Q229)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G229=\"\",\"\",G229*Q229)","v":""},{"$f":"IF(H229=\"\",\"\",H229*Q229)","v":{"$error":"#VALUE!"}},0,0,0,{"$f":"IFERROR(IF(D229=\"x\",IF(OR(G229/H229>1.03,G229/H229<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J229*100,)","v":0},null,{"$f":"RANK(AA229,$AA$209:$AA$264,0)","v":1},{"$f":"AC229+COUNTIF($AC$209:$AC228,AC229)","v":11},{"$f":"B229","v":"Heat rejection"},0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Q",0,0,{"$f":"IF(BG229<>\"\",IFERROR(MATCH(BG229&BH229,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E229),\"\",\"Demand (\" & VLOOKUP($E229,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,22, 10)","v":""},0,"",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AD",0,0]
["G",{"$f":"INDEX(PO_baseline_table,23, 1)","v":"Fans - interior ventilation"},null,{"$f":"INDEX(PO_baseline_table,23, 3)","v":0},{"$f":"INDEX(PO_baseline_table,23, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E231),\"\",\"Consumption (\" & VLOOKUP($E231,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,23, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G231-$H231)*VLOOKUP($E231,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G231*VLOOKUP($E231,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H231*VLOOKUP($E231,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H231*Q231)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G231=\"\",\"\",G231*Q231)","v":""},{"$f":"IF(H231=\"\",\"\",H231*Q231)","v":{"$error":"#VALUE!"}},0,0,0,{"$f":"IFERROR(IF(D231=\"x\",IF(OR(G231/H231>1.03,G231/H231<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J231*100,)","v":0},null,{"$f":"RANK(AA231,$AA$209:$AA$264,0)","v":1},{"$f":"AC231+COUNTIF($AC$209:$AC230,AC231)","v":12},{"$f":"B231","v":"Fans - interior ventilation"},0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S",{"$f":"BG147","v":"Stand-alone Base Utilities"},{"$f":"BH147","v":"Gas"},{"$f":"IF(BG231<>\"\",IFERROR(MATCH(BG231&BH231,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":16}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E231),\"\",\"Demand (\" & VLOOKUP($E231,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,24, 10)","v":""},0,"",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AF",{"$f":"BG148","v":0},{"$f":"BH148","v":0}]
["G",{"$f":"INDEX(PO_baseline_table,25, 1)","v":"Fans - parking garage"},null,{"$f":"INDEX(PO_baseline_table,25, 3)","v":0},{"$f":"INDEX(PO_baseline_table,25, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E233),\"\",\"Consumption (\" & VLOOKUP($E233,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,25, 10)","v":""},"","",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G233-$H233)*VLOOKUP($E233,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G233*VLOOKUP($E233,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H233*VLOOKUP($E233,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H233*Q233)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G233=\"\",\"\",G233*Q233)","v":""},{"$f":"IF(H233=\"\",\"\",H233*Q233)","v":""},0,0,0,{"$f":"IFERROR(IF(D233=\"x\",IF(OR(G233/H233>1.03,G233/H233<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J233*100,)","v":0},null,{"$f":"RANK(AA233,$AA$209:$AA$264,0)","v":1},{"$f":"AC233+COUNTIF($AC$209:$AC232,AC233)","v":13},{"$f":"B233","v":"Fans - parking garage"},0,null,null,0,1,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BG151","v":"Receptacles - Conditioned"},"Electricity",{"$f":"IF(BG233<>\"\",IFERROR(MATCH(BG233&BH233,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":14}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E233),\"\",\"Demand (\" & VLOOKUP($E233,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,26, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_baseline_table,27, 1)","v":"Fans - Kitchen Ventilation"},null,{"$f":"INDEX(PO_baseline_table,27, 3)","v":0},{"$f":"INDEX(PO_baseline_table,27, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E235),\"\",\"Consumption (\" & VLOOKUP($E235,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,27, 10)","v":""},"","",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G235-$H235)*VLOOKUP($E235,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G235*VLOOKUP($E235,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H235*VLOOKUP($E235,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H235*Q235)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G235=\"\",\"\",G235*Q235)","v":""},{"$f":"IF(H235=\"\",\"\",H235*Q235)","v":""},0,0,0,{"$f":"IFERROR(IF(D235=\"x\",IF(OR(G235/H235>1.03,G235/H235<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J235*100,)","v":0},null,{"$f":"RANK(AA235,$AA$209:$AA$264,0)","v":1},{"$f":"AC235+COUNTIF($AC$209:$AC234,AC235)","v":14},{"$f":"B235","v":"Fans - Kitchen Ventilation"},0,null,null,0,1,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BG155","v":0},{"$f":"BH155","v":0},{"$f":"IF(BG235<>\"\",IFERROR(MATCH(BG235&BH235,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E235),\"\",\"Demand (\" & VLOOKUP($E235,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,28, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BG156","v":0},{"$f":"BH156","v":0}]
["G",{"$f":"INDEX(PO_baseline_table,29, 1)","v":"Service water heating"},null,{"$f":"INDEX(PO_baseline_table,29, 3)","v":0},{"$f":"INDEX(PO_baseline_table,29, 4)","v":"Natural Gas"},{"$f":"IFERROR(IF(ISBLANK(E237),\"\",\"Consumption (\" & VLOOKUP($E237,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,29, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G237-$H237)*VLOOKUP($E237,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G237*VLOOKUP($E237,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H237*VLOOKUP($E237,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H237*Q237)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G237=\"\",\"\",G237*Q237)","v":""},{"$f":"IF(H237=\"\",\"\",H237*Q237)","v":{"$error":"#VALUE!"}},0,0,0,{"$f":"IFERROR(IF(D237=\"x\",IF(OR(G237/H237>1.03,G237/H237<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J237*100,)","v":0},null,{"$f":"RANK(AA237,$AA$209:$AA$264,0)","v":1},{"$f":"AC237+COUNTIF($AC$209:$AC236,AC237)","v":15},{"$f":"B237","v":"Service water heating"},0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BH",{"$f":"BG123","v":0},{"$f":"BH123","v":0},{"$f":"IF(BG237<>\"\",IFERROR(MATCH(BG237&BH237,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E237),\"\",\"Demand (\" & VLOOKUP($E237,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,30, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BG124","v":0},{"$f":"BH124","v":0}]
["G",{"$f":"INDEX(PO_baseline_table,31, 1)","v":"Service water heating"},null,{"$f":"INDEX(PO_baseline_table,31, 3)","v":0},{"$f":"INDEX(PO_baseline_table,31, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E239),\"\",\"Consumption (\" & VLOOKUP($E239,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,31, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G239-$H239)*VLOOKUP($E239,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G239*VLOOKUP($E239,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H239*VLOOKUP($E239,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H239*Q239)/$H$276,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($E239),\"\",VLOOKUP($E239,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},"","","",{"$f":"IF(G239=\"\",\"\",G239*Q239)","v":""},{"$f":"IF(H239=\"\",\"\",H239*Q239)","v":{"$error":"#VALUE!"}},0,0,0,{"$f":"IFERROR(IF(D239=\"x\",IF(OR(G239/H239>1.03,G239/H239<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J239*100,)","v":0},null,{"$f":"RANK(AA239,$AA$209:$AA$264,0)","v":1},{"$f":"AC239+COUNTIF($AC$209:$AC238,AC239)","v":16},{"$f":"B239","v":"Service water heating"},0,null,null,0,1,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"BF151","v":"N"},{"$f":"BG163","v":0},{"$f":"BH163","v":0},{"$f":"IF(BG239<>\"\",IFERROR(MATCH(BG239&BH239,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E239),\"\",\"Demand (\" & VLOOKUP($E239,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,32, 10)","v":""},0,"",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AA",{"$f":"BG164","v":0},{"$f":"BH164","v":0}]
["G",{"$f":"INDEX(PO_baseline_table,33, 1)","v":"Misc Equipment"},null,{"$f":"INDEX(PO_baseline_table,33, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,33, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E241),\"\",\"Consumption (\" & VLOOKUP($E241,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,33, 10)","v":""},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF241&\"13\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!H\"&$BI241)/$Q241,\"\")),\"\")","v":0},"",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G241-$H241)*VLOOKUP($E241,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G241*VLOOKUP($E241,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H241*VLOOKUP($E241,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H241*Q241)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G241=\"\",\"\",G241*Q241)","v":""},{"$f":"IF(H241=\"\",\"\",H241*Q241)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR($AN241*H241,0)","v":0},{"$f":"IFERROR(G241*VLOOKUP($AF241,PO_Enrgy_8_Table,4,FALSE),0)","v":0},{"$f":"IFERROR(H241*VLOOKUP($AF241,PO_Enrgy_8_Table,7,FALSE),0)","v":0},{"$f":"IFERROR(IF(D241=\"x\",IF(OR(G241/H241>1.03,G241/H241<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J241*100,)","v":0},null,{"$f":"RANK(AA241,$AA$209:$AA$264,0)","v":1},{"$f":"AC241+COUNTIF($AC$209:$AC240,AC241)","v":17},{"$f":"B241","v":"Misc Equipment"},1,null,null,1,1,{"$f":"IFERROR(IF(D241=\"x\",(ABS(G241-H241))/(MIN(G241,H241)),\"\"),0)","v":0},{"$f":"IFERROR(IF(SimTool=\"eQUEST\",INDIRECT(\"'Results from eQuest'!\"&$BF241&\"13\"),IF(SimTool=\"Trace\",INDIRECT(\"'Results from Trace'!H\"&$BI241)/$Q241,\"\")),\"\")","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AZ",{"$f":"BG145","v":0},{"$f":"BH145","v":0},{"$f":"IF(BG241<>\"\",IFERROR(MATCH(BG241&BH241,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E241),\"\",\"Demand (\" & VLOOKUP($E241,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,34, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BG146","v":0},{"$f":"BH146","v":0}]
["G",{"$f":"INDEX(PO_baseline_table,35, 1)","v":"Misc Equipment"},null,{"$f":"INDEX(PO_baseline_table,35, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,35, 4)","v":"Natural Gas"},{"$f":"IFERROR(IF(ISBLANK(E243),\"\",\"Consumption (\" & VLOOKUP($E243,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,35, 10)","v":""},"","",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G243-$H243)*VLOOKUP($E243,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G243*VLOOKUP($E243,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H243*VLOOKUP($E243,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H243*Q243)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G243=\"\",\"\",G243*Q243)","v":""},{"$f":"IF(H243=\"\",\"\",H243*Q243)","v":""},0,0,0,{"$f":"IFERROR(IF(D243=\"x\",IF(OR(G243/H243>1.03,G243/H243<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J243*100,)","v":0},null,{"$f":"RANK(AA243,$AA$209:$AA$264,0)","v":1},{"$f":"AC243+COUNTIF($AC$209:$AC242,AC243)","v":18},{"$f":"B243","v":"Misc Equipment"},1,null,null,1,1,0,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BG157","v":0},0,{"$f":"IF(BG243<>\"\",IFERROR(MATCH(BG243&BH243,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E243),\"\",\"Demand (\" & VLOOKUP($E243,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,36, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_baseline_table,37, 1)","v":"IT equipment"},null,{"$f":"INDEX(PO_baseline_table,37, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,37, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E245),\"\",\"Consumption (\" & VLOOKUP($E245,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,37, 10)","v":""},"","",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G245-$H245)*VLOOKUP($E245,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G245*VLOOKUP($E245,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H245*VLOOKUP($E245,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H245*Q245)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G245=\"\",\"\",G245*Q245)","v":""},{"$f":"IF(H245=\"\",\"\",H245*Q245)","v":""},0,0,0,{"$f":"IFERROR(IF(D245=\"x\",IF(OR(G245/H245>1.03,G245/H245<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J245*100,)","v":0},null,{"$f":"RANK(AA245,$AA$209:$AA$264,0)","v":1},{"$f":"AC245+COUNTIF($AC$209:$AC244,AC245)","v":19},{"$f":"B245","v":"IT equipment"},1,null,null,1,1,0,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,{"$f":"IF(BG245<>\"\",IFERROR(MATCH(BG245&BH245,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E245),\"\",\"Demand (\" & VLOOKUP($E245,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,38, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_baseline_table,39, 1)","v":"Cooking"},null,{"$f":"INDEX(PO_baseline_table,39, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,39, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E247),\"\",\"Consumption (\" & VLOOKUP($E247,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,39, 10)","v":""},"","",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G247-$H247)*VLOOKUP($E247,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G247*VLOOKUP($E247,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H247*VLOOKUP($E247,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H247*Q247)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G247=\"\",\"\",G247*Q247)","v":""},{"$f":"IF(H247=\"\",\"\",H247*Q247)","v":""},0,0,0,{"$f":"IFERROR(IF(D247=\"x\",IF(OR(G247/H247>1.03,G247/H247<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J247*100,)","v":0},null,{"$f":"RANK(AA247,$AA$209:$AA$264,0)","v":1},{"$f":"AC247+COUNTIF($AC$209:$AC246,AC247)","v":20},{"$f":"B247","v":"Cooking"},1,null,null,1,1,0,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BG165","v":0},{"$f":"BH165","v":0},{"$f":"IF(BG247<>\"\",IFERROR(MATCH(BG247&BH247,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E247),\"\",\"Demand (\" & VLOOKUP($E247,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,40, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BG166","v":0},{"$f":"BH166","v":0}]
["G",{"$f":"INDEX(PO_baseline_table,41, 1)","v":"Industrial Process"},null,{"$f":"INDEX(PO_baseline_table,41, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,41, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E249),\"\",\"Consumption (\" & VLOOKUP($E249,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,41, 10)","v":""},0,"",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G249-$H249)*VLOOKUP($E249,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G249*VLOOKUP($E249,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H249*VLOOKUP($E249,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H249*Q249)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G249=\"\",\"\",G249*Q249)","v":""},{"$f":"IF(H249=\"\",\"\",H249*Q249)","v":{"$error":"#VALUE!"}},0,0,0,{"$f":"IFERROR(IF(D249=\"x\",IF(OR(G249/H249>1.03,G249/H249<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J249*100,)","v":0},null,{"$f":"RANK(AA249,$AA$209:$AA$264,0)","v":1},{"$f":"AC249+COUNTIF($AC$209:$AC248,AC249)","v":21},{"$f":"B249","v":"Industrial Process"},1,null,null,1,1,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T",{"$f":"BG131","v":0},{"$f":"BH131","v":0},{"$f":"IF(BG249<>\"\",IFERROR(MATCH(BG249&BH249,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E249),\"\",\"Demand (\" & VLOOKUP($E249,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,42, 10)","v":""},0,"",null,null,null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F250),(G250*VLOOKUP(MID(F250,FIND(\"(\",F250)+1,LEN(F250)-FIND(\"(\",F250)-1),EnergyUnitsTable,3,FALSE))/(G217*VLOOKUP(MID(F217,FIND(\"(\",F217)+1,LEN(F217)-FIND(\"(\",F217)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",$F250),(H250*VLOOKUP(MID($F250,FIND(\"(\",$F250)+1,LEN($F250)-FIND(\"(\",$F250)-1),EnergyUnitsTable,3,FALSE))/(H217*VLOOKUP(MID($F217,FIND(\"(\",$F217)+1,LEN($F217)-FIND(\"(\",$F217)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AG",{"$f":"BG132","v":0},{"$f":"BH132","v":0}]
["G",{"$f":"INDEX(PO_baseline_table,43, 1)","v":"Refrigeration Equipment (Regulated)"},null,{"$f":"INDEX(PO_baseline_table,43, 3)","v":0},{"$f":"INDEX(PO_baseline_table,43, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E251),\"\",\"Consumption (\" & VLOOKUP($E251,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,43, 10)","v":""},"","",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G251-$H251)*VLOOKUP($E251,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G251*VLOOKUP($E251,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H251*VLOOKUP($E251,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H251*Q251)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G251=\"\",\"\",G251*Q251)","v":""},{"$f":"IF(H251=\"\",\"\",H251*Q251)","v":""},0,0,0,{"$f":"IFERROR(IF(D251=\"x\",IF(OR(G251/H251>1.03,G251/H251<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J251*100,)","v":0},null,{"$f":"RANK(AA251,$AA$209:$AA$264,0)","v":1},{"$f":"AC251+COUNTIF($AC$209:$AC250,AC251)","v":22},{"$f":"B251","v":"Refrigeration Equipment (Regulated)"},0,null,null,0,1,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BG169","v":0},0,{"$f":"IF(BG251<>\"\",IFERROR(MATCH(BG251&BH251,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E251),\"\",\"Demand (\" & VLOOKUP($E251,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,44, 10)","v":""},"","",null,null,null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F252),(G252*VLOOKUP(MID(F252,FIND(\"(\",F252)+1,LEN(F252)-FIND(\"(\",F252)-1),EnergyUnitsTable,3,FALSE))/(G221*VLOOKUP(MID(F221,FIND(\"(\",F221)+1,LEN(F221)-FIND(\"(\",F221)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",$F252),(H252*VLOOKUP(MID($F252,FIND(\"(\",$F252)+1,LEN($F252)-FIND(\"(\",$F252)-1),EnergyUnitsTable,3,FALSE))/(H221*VLOOKUP(MID($F221,FIND(\"(\",$F221)+1,LEN($F221)-FIND(\"(\",$F221)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_baseline_table,45, 1)","v":"Refrigeration Equipment (Unregulated)"},null,{"$f":"INDEX(PO_baseline_table,45, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,45, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E253),\"\",\"Consumption (\" & VLOOKUP($E253,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,45, 10)","v":""},"",{"$f":"IFERROR(1-H253/G253,\"\")","v":""},{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G253-$H253)*VLOOKUP($E253,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G253*VLOOKUP($E253,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H253*VLOOKUP($E253,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H253*Q253)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G253=\"\",\"\",G253*Q253)","v":""},{"$f":"IF(H253=\"\",\"\",H253*Q253)","v":""},0,0,0,{"$f":"IFERROR(IF(D253=\"x\",IF(OR(G253/H253>1.03,G253/H253<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J253*100,)","v":0},null,{"$f":"RANK(AA253,$AA$209:$AA$264,0)","v":1},{"$f":"AC253+COUNTIF($AC$209:$AC252,AC253)","v":23},{"$f":"B253","v":"Refrigeration Equipment (Unregulated)"},1,null,null,1,1,0,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BG135","v":0},{"$f":"BH135","v":0},{"$f":"IF(BG253<>\"\",IFERROR(MATCH(BG253&BH253,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E253),\"\",\"Demand (\" & VLOOKUP($E253,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,46, 10)","v":""},"",{"$f":"IFERROR(1-H254/G254,\"\")","v":""},null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BG136","v":0},{"$f":"BH136","v":0}]
["G",{"$f":"INDEX(PO_baseline_table,47, 1)","v":"Elevators and escalators"},null,{"$f":"INDEX(PO_baseline_table,47, 3)","v":0},{"$f":"INDEX(PO_baseline_table,47, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E255),\"\",\"Consumption (\" & VLOOKUP($E255,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,47, 10)","v":""},"",{"$f":"IFERROR(1-H255/G255,\"\")","v":""},{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G255-$H255)*VLOOKUP($E255,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G255*VLOOKUP($E255,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H255*VLOOKUP($E255,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H255*Q255)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G255=\"\",\"\",G255*Q255)","v":""},{"$f":"IF(H255=\"\",\"\",H255*Q255)","v":""},0,0,0,{"$f":"IFERROR(IF(D255=\"x\",IF(OR(G255/H255>1.03,G255/H255<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J255*100,)","v":0},null,{"$f":"RANK(AA255,$AA$209:$AA$264,0)","v":1},{"$f":"AC255+COUNTIF($AC$209:$AC254,AC255)","v":24},{"$f":"B255","v":"Elevators and escalators"},0,null,null,0,1,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"BG173","v":0},0,{"$f":"IF(BG255<>\"\",IFERROR(MATCH(BG255&BH255,'Results from Trace'!$L$1:$L$21,0),\"\"),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E255),\"\",\"Demand (\" & VLOOKUP($E255,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,48, 10)","v":""},"",{"$f":"IFERROR(1-H256/G256,\"\")","v":""},null,null,null,null,null,null,null,"","",{"$f":"IFERROR(IF(FIND(\"Consumption\",F256),(G256*VLOOKUP(MID(F256,FIND(\"(\",F256)+1,LEN(F256)-FIND(\"(\",F256)-1),EnergyUnitsTable,3,FALSE))/(G257*VLOOKUP(MID(F257,FIND(\"(\",F257)+1,LEN(F257)-FIND(\"(\",F257)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",$F256),(H256*VLOOKUP(MID($F256,FIND(\"(\",$F256)+1,LEN($F256)-FIND(\"(\",$F256)-1),EnergyUnitsTable,3,FALSE))/(H257*VLOOKUP(MID($F257,FIND(\"(\",$F257)+1,LEN($F257)-FIND(\"(\",$F257)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_baseline_table,49, 1)","v":"Building Transformers"},null,{"$f":"INDEX(PO_baseline_table,49, 3)","v":0},{"$f":"INDEX(PO_baseline_table,49, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E257),\"\",\"Consumption (\" & VLOOKUP($E257,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,49, 10)","v":""},"","",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G257-$H257)*VLOOKUP($E257,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G257*VLOOKUP($E257,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H257*VLOOKUP($E257,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,"",null,null,null,"","","","",{"$f":"IF(G257=\"\",\"\",G257*Q257)","v":""},{"$f":"IF(H257=\"\",\"\",H257*Q257)","v":""},0,0,0,{"$f":"IFERROR(IF(D257=\"x\",IF(OR(G257/H257>1.03,G257/H257<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J257*100,)","v":0},null,{"$f":"RANK(AA257,$AA$209:$AA$264,0)","v":1},{"$f":"AC257+COUNTIF($AC$209:$AC256,AC257)","v":25},{"$f":"B257","v":"Building Transformers"},0,null,null,0,1,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E257),\"\",\"Demand (\" & VLOOKUP($E257,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,50, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_baseline_table,51, 1)","v":0},null,{"$f":"INDEX(PO_baseline_table,51, 3)","v":0},{"$f":"INDEX(PO_baseline_table,51, 4)","v":0},{"$f":"IFERROR(IF(ISBLANK(E259),\"\",\"Consumption (\" & VLOOKUP($E259,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,51, 10)","v":""},"","",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G259-$H259)*VLOOKUP($E259,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G259*VLOOKUP($E259,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H259*VLOOKUP($E259,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,"",null,null,null,"","","","",{"$f":"IF(G259=\"\",\"\",G259*Q259)","v":""},{"$f":"IF(H259=\"\",\"\",H259*Q259)","v":""},0,0,0,{"$f":"IFERROR(IF(D259=\"x\",IF(OR(G259/H259>1.03,G259/H259<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J259*100,)","v":0},null,{"$f":"RANK(AA259,$AA$209:$AA$264,0)","v":1},{"$f":"AC259+COUNTIF($AC$209:$AC258,AC259)","v":26},{"$f":"B259","v":0},0,null,null,0,1,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E259),\"\",\"Demand (\" & VLOOKUP($E259,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,52, 10)","v":""},"",{"$f":"IFERROR(1-H260/G260,\"\")","v":""},null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_baseline_table,53, 1)","v":0},null,{"$f":"INDEX(PO_baseline_table,53, 3)","v":0},{"$f":"INDEX(PO_baseline_table,53, 4)","v":0},{"$f":"IFERROR(IF(ISBLANK(E261),\"\",\"Consumption (\" & VLOOKUP($E261,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,53, 10)","v":""},"","",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G261-$H261)*VLOOKUP($E261,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G261*VLOOKUP($E261,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H261*VLOOKUP($E261,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H261*Q261)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G261=\"\",\"\",G261*Q261)","v":""},{"$f":"IF(H261=\"\",\"\",H261*Q261)","v":""},0,0,0,{"$f":"IFERROR(IF(D261=\"x\",IF(OR(G261/H261>1.03,G261/H261<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J261*100,)","v":0},null,{"$f":"RANK(AA261,$AA$209:$AA$264,0)","v":1},{"$f":"AC261+COUNTIF($AC$209:$AC260,AC261)","v":27},{"$f":"B261","v":0},0,null,null,0,1,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E261),\"\",\"Demand (\" & VLOOKUP($E261,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,54, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G",{"$f":"INDEX(PO_baseline_table,55, 1)","v":0},null,{"$f":"INDEX(PO_baseline_table,55, 3)","v":0},{"$f":"INDEX(PO_baseline_table,55, 4)","v":0},{"$f":"IFERROR(IF(ISBLANK(E263),\"\",\"Consumption (\" & VLOOKUP($E263,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,55, 10)","v":""},"","",{"$f":"IFERROR(IF($E$411-$H$411<0,\"\",($G263-$H263)*VLOOKUP($E263,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$411-$H$411)),\"\")","v":""},{"$f":"IFERROR(IF($G$411-$J$411<0,\"\",($G263*VLOOKUP($E263,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)-($H263*VLOOKUP($E263,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)))/($G$411-$J$411)),\"\")","v":""},null,{"$f":"IFERROR((H263*Q263)/$H$276,\"\")","v":""},null,null,null,"","","","",{"$f":"IF(G263=\"\",\"\",G263*Q263)","v":""},{"$f":"IF(H263=\"\",\"\",H263*Q263)","v":""},0,0,0,{"$f":"IFERROR(IF(D263=\"x\",IF(OR(G263/H263>1.03,G263/H263<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J263*100,)","v":0},null,{"$f":"RANK(AA263,$AA$209:$AA$264,0)","v":1},{"$f":"AC263+COUNTIF($AC$209:$AC262,AC263)","v":28},{"$f":"B263","v":0},0,null,null,0,1,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E263),\"\",\"Demand (\" & VLOOKUP($E263,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,56, 10)","v":""},"","",null,null,null,null,null,null,null,"","","","",null,null,0,0,0,null,null,null,null,null,null,0,null,null,0,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
["G"]
["G","Table 12.7: Performance rating energy consumption and cost by fuel type"]
["G","Energy Type","Site Energy Units",null,"Baseline",null,null,"Proposed Design",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy","Source Energy","Cost",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site_Energy",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B270),\"\",VLOOKUP($B270,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C270=\"\",\"\",VLOOKUP(C270,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(SUMIFS(G$209:G$264,$F$209:$F$264,\"=Con*\",$E$209:$E$264,$B270), 0)","v":0},{"$f":"IFERROR(SUMIFS(G$209:G$264,$F$209:$F$264,\"=Con*\",$E$209:$E$264,$B270)*VLOOKUP($B270,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE), 0)","v":0},{"$f":"INDEX(PO_Enrgy_6_Table,1, 10)","v":""},{"$f":"IFERROR(SUMIFS(H$209:H$264,$F$209:$F$264,\"=Con*\",$E$209:$E$264,$B270), 0)","v":0},{"$f":"IFERROR(SUMIFS(H$209:H$264,$F$209:$F$264,\"=Con*\",$E$209:$E$264,$B270)*VLOOKUP($B270,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE), 0)","v":0},{"$f":"IF(SimTool=\"eQuest\",'Results from eQuest'!BQ13-'Results from eQuest'!BR13,\"\")","v":0},{"$f":"IFERROR(1-H270/E270,\"\")","v":""},{"$f":"IFERROR(1-I270/F270,\"\")","v":""},{"$f":"IFERROR(1-J270/G270,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B270),\"\",VLOOKUP($B270,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B270),\"\",VLOOKUP($B270,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C271=\"\",\"\",VLOOKUP(C271,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(SUMIFS(G$209:G$264,$F$209:$F$264,\"=Con*\",$E$209:$E$264,$B271), 0)","v":0},0,{"$f":"INDEX(PO_Enrgy_6_Table,2, 10)","v":""},0,0,{"$f":"IF(SimTool=\"eQuest\",'Results from eQuest'!BP13,\"\")","v":0},{"$f":"IFERROR(1-H271/E271,\"\")","v":""},{"$f":"IFERROR(1-I271/F271,\"\")","v":""},{"$f":"IFERROR(1-J271/G271,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C272=\"\",\"\",VLOOKUP(C272,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,{"$f":"INDEX(PO_Enrgy_6_Table,3, 10)","v":""},0,0,null,{"$f":"IFERROR(1-H272/E272,\"\")","v":""},"",{"$f":"IFERROR(1-J272/G272,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C273=\"\",\"\",VLOOKUP(C273,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,{"$f":"INDEX(PO_Enrgy_6_Table,4, 10)","v":""},0,0,null,{"$f":"IFERROR(1-H273/E273,\"\")","v":""},"",{"$f":"IFERROR(1-J273/G273,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C274=\"\",\"\",VLOOKUP(C274,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,{"$f":"INDEX(PO_Enrgy_6_Table,5, 10)","v":""},0,0,null,"","","",null,null,null,"",""]
["G","","",{"$f":"IF(C275=\"\",\"\",VLOOKUP(C275,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,{"$f":"INDEX(PO_Enrgy_6_Table,6, 10)","v":""},0,0,null,"","","",null,null,null,"",""]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_7_Table,0,MATCH(E$269,PO_Enrgy_7_Hdr,0)),INDEX(PO_Enrgy_7_Table,0,MATCH($Q$269,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(F$269,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(G$269,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_7_Table,0,MATCH(H$269,PO_Enrgy_7_Hdr,0)),INDEX(PO_Enrgy_7_Table,0,MATCH($Q$269,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(I$269,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(J$269,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H276/E276,\"\")","v":""},"",{"$f":"IFERROR(1-J276/G276,\"\")","v":""}]
["G"]
["G"]
["G","Table 12.8: Virtual rate (average energy cost per unit energy)"]
["G","Energy Type",null,null,"Baseline",null,null,"Proposed Design",null,null,"Percent Variance",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Energy_Type","Units",null,"Base_Virtual_Rate",null,null,"Design_Virtual_Rate",null,null,"Percent_Variance",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",null,"Default_Base","Default_Proposed"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(CONCATENATE(\"$ / \",VLOOKUP($B282,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IF(C282=\"\",\"\",VLOOKUP(C282,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B282=\"District Cooling\",$B282=\"District Steam\",$B282=\"District Hot Water\")),IF($B282=\"District Cooling\",$V$306,$W$306),VLOOKUP($B282,PO_Enrgy_7_Table,MATCH($G$269,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B282,PO_Enrgy_7_Table,MATCH($E$269,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},"","",{"$f":"IFERROR(IF(AND(DESPath=3,OR($B282=\"District Cooling\",$B282=\"District Steam\",$B282=\"District Hot Water\")),IF($B282=\"District Cooling\",$V$310,$W$310),VLOOKUP($B282,PO_Enrgy_7_Table,MATCH($J$269,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B282,PO_Enrgy_7_Table,MATCH($H$269,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},"","",{"$f":"IFERROR(ABS(1-H282/E282),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B282),\"\",VLOOKUP($B282,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B282),\"\",VLOOKUP($B282,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B282=\"District Cooling\",$B282=\"District Steam\",$B282=\"District Hot Water\")),IF($B282=\"District Cooling\",$V$306,$W$306),VLOOKUP($B282,PO_Enrgy_7_Table,MATCH($G$269,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B282,PO_Enrgy_7_Table,MATCH($E$269,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B282=\"District Cooling\",$B282=\"District Steam\",$B282=\"District Hot Water\")),IF($B282=\"District Cooling\",$V$310,$W$310),VLOOKUP($B282,PO_Enrgy_7_Table,MATCH($J$269,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B282,PO_Enrgy_7_Table,MATCH($H$269,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C283=\"\",\"\",VLOOKUP(C283,ProjectEnergyTypeTable,3,FALSE))","v":""},"","","","","","",{"$f":"IFERROR(ABS(1-H283/E283),\"\")","v":""},null,null,null,null,null,"","",null,"",""]
["G","","",{"$f":"IF(C284=\"\",\"\",VLOOKUP(C284,ProjectEnergyTypeTable,3,FALSE))","v":""},"","","","","","",{"$f":"IFERROR(ABS(1-H284/E284),\"\")","v":""},null,null,null,null,null,"","",null,"",""]
["G","","",{"$f":"IF(C285=\"\",\"\",VLOOKUP(C285,ProjectEnergyTypeTable,3,FALSE))","v":""},"","","","","","",{"$f":"IFERROR(ABS(1-H285/E285),\"\")","v":""},null,null,null,null,null,"","",null,"",""]
["G","","",{"$f":"IF(C286=\"\",\"\",VLOOKUP(C286,ProjectEnergyTypeTable,3,FALSE))","v":""},"","","","","","","",null,null,null,null,null,"","",null,"",""]
["G","","",{"$f":"IF(C287=\"\",\"\",VLOOKUP(C287,ProjectEnergyTypeTable,3,FALSE))","v":""},"","","","","","","",null,null,null,null,null,"","",null,"",""]
["G"]
["G","Table 12.9: Baseline and Proposed Results with Exceptional Calculation Method"]
["G","Energy Type","Site Energy Units",null,"Baseline Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy","Source Energy","Cost",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site_Energy",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B293),\"\",VLOOKUP($B293,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C293=\"\",\"\",VLOOKUP(C293,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(VLOOKUP($B293,PO_Enrgy_7_Table,MATCH($E$269,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B293,PO_Enrgy_3_Table,MATCH($G$70,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B293,PO_Enrgy_7_Table,MATCH($F$269,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B293,PO_Enrgy_3_Table,MATCH($J$70,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B293,PO_Enrgy_7_Table,MATCH($G$269,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B293,PO_Enrgy_3_Table,MATCH($L$70,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B293,PO_Enrgy_7_Table,MATCH($H$269,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B293,PO_Enrgy_4_Table,MATCH($G$70,PO_Enrgy_3_Hdr,0),FALSE),0)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B293,PO_Enrgy_4_Table_Add_P,MATCH($G$70,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B293,PO_Enrgy_7_Table,MATCH($I$269,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B293,PO_Enrgy_4_Table,MATCH($J$70,PO_Enrgy_3_Hdr,0),FALSE),0)-+IF(PO_ShowExCalc=TRUE,VLOOKUP($B293,PO_Enrgy_4_Table_Add_P,MATCH($J$70,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B293,PO_Enrgy_7_Table,MATCH($J$269,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B293,PO_Enrgy_4_Table,MATCH($L$70,PO_Enrgy_3_Hdr,0),FALSE),0)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B293,PO_Enrgy_4_Table_Add_P,MATCH($L$70,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(1-H293/E293,\"\")","v":""},{"$f":"IFERROR(1-I293/F293,\"\")","v":""},{"$f":"IFERROR(1-J293/G293,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B293),\"\",VLOOKUP($B293,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B293),\"\",VLOOKUP($B293,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C294=\"\",\"\",VLOOKUP(C294,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,{"$f":"IFERROR(VLOOKUP($B294,PO_Enrgy_7_Table,MATCH($I$269,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B294,PO_Enrgy_4_Table,MATCH($J$70,PO_Enrgy_3_Hdr,0),FALSE),0)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B294,PO_Enrgy_4_Table_Add_P,MATCH($J$70,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},0,{"$f":"IFERROR(1-H294/E294,\"\")","v":""},{"$f":"IFERROR(1-I294/F294,\"\")","v":""},{"$f":"IFERROR(1-J294/G294,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C295=\"\",\"\",VLOOKUP(C295,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,{"$f":"IFERROR(VLOOKUP($B295,PO_Enrgy_7_Table,MATCH($I$269,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B295,PO_Enrgy_4_Table,MATCH($J$70,PO_Enrgy_3_Hdr,0),FALSE),0)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B295,PO_Enrgy_4_Table_Add_P,MATCH($J$70,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},0,{"$f":"IFERROR(1-H295/E295,\"\")","v":""},"",{"$f":"IFERROR(1-J295/G295,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C296=\"\",\"\",VLOOKUP(C296,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,{"$f":"IFERROR(VLOOKUP($B296,PO_Enrgy_7_Table,MATCH($I$269,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B296,PO_Enrgy_4_Table,MATCH($J$70,PO_Enrgy_3_Hdr,0),FALSE),0)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B296,PO_Enrgy_4_Table_Add_P,MATCH($J$70,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},0,{"$f":"IFERROR(1-H296/E296,\"\")","v":""},"",{"$f":"IFERROR(1-J296/G296,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C297=\"\",\"\",VLOOKUP(C297,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,{"$f":"IFERROR(VLOOKUP($B297,PO_Enrgy_7_Table,MATCH($I$269,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B297,PO_Enrgy_4_Table,MATCH($J$70,PO_Enrgy_3_Hdr,0),FALSE),0)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B297,PO_Enrgy_4_Table_Add_P,MATCH($J$70,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},0,"","","",null,null,null,"",""]
["G","","",{"$f":"IF(C298=\"\",\"\",VLOOKUP(C298,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,{"$f":"IFERROR(VLOOKUP($B298,PO_Enrgy_7_Table,MATCH($I$269,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B298,PO_Enrgy_4_Table,MATCH($J$70,PO_Enrgy_3_Hdr,0),FALSE),0)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B298,PO_Enrgy_4_Table_Add_P,MATCH($J$70,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},0,"","","",null,null,null,"",""]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_9_Table,0,MATCH(E$292,PO_Enrgy_9_Hdr,0)),INDEX(PO_Enrgy_9_Table,0,MATCH($Q$292,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(F$292,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(G$292,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_9_Table,0,MATCH(H$292,PO_Enrgy_9_Hdr,0)),INDEX(PO_Enrgy_9_Table,0,MATCH($Q$292,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(I$292,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(J$292,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H299/E299,\"\")","v":""},"",{"$f":"IFERROR(1-J299/G299,\"\")","v":""}]
["G"]
["G","Table: Streamlined DES Accounting Method (DES Path 3) - District Energy Allocation to Project Based on Average Efficiencies"]
["G","Select the fossil fuel energy type used to generate any district heating or cooling.  Enter the proposed average District Cooling and District Heating efficiencies as applicable. For District Cooling, include chillers, cooling towers, chilled water and condenser water pumps, thermal distribution losses, and any other end-uses contributing towards the energy used to generate and distribute chilled water to the building. For District Heating, include boilers, pumps, thermal distribution losses, and any other end-uses contributing towards the energy used to generate and distribute heating to the building. In the Uploads section of the form, provide details regarding the calculations and or monitoring used to determine the proposed District Energy average efficiency, including any energy simulation outputs for the district plant if using the modeling method.\n\n* Average DES efficiency (COP) per energy source is equal to one unit of thermal energy divided by the input energy for the energy source associated with generating one unit of thermal energy and delivering it to the building. Baseline average efficiency is determined based on chilled water or hot water capacity and ASHRAE 90.1 Appendix G Baseline requirements for on-site CHW and HHW generation equipment (see District Energy Path 3 tab for details)."]
["G","Fuel Source for District Cooling and/or Heating","Site Energy Units",null,"District Cooling ",null,null,"District Heating"]
["G",null,null,null,"Average \nEfficiency \n(COP)*","Site Energy Use \n(Units shown per energy type)","Cost","Average \nEfficiency \n(COP)*","Site Energy Use (Units shown per energy type)","Cost"]
["G","Energy_Type","Energy_Units",null,"Cooling_Avg_Efficiency","Cooling_Site_Energy","Cooling_Cost","Heating_Avg_Effiicency","Heating_Site_Energy","Heating_Cost",null,null,null,null,null,null,null,null,null,null,"Total Baseline","Cost/Unit District Cooling","Cost/Unit District Heating"]
["G","Baseline",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",null,null,null,{"$f":"IFERROR(V308+V307,\"\")","v":""},{"$f":"IFERROR(W308+W307,\"\")","v":""}]
["G",{"$f":"IFERROR(IF(DESPath=3,\"Electricity\",\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B307),\"\",VLOOKUP($B307,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C307=\"\",\"\",VLOOKUP(C307,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(AND(DESPath=3,DistrictCooling,$B$307=\"Electricity\"),DESPath3_Cooling_COP,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(DESPath=3,VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($E$292,PO_Enrgy_9_Hdr,0),FALSE)/$E307*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C307,EnergyUnitsTable,3,FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(F307*VLOOKUP($B307,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(IF(AND(DESPath=3,DistrictHeating,$B$307=\"Electricity\"),DESPath3_Heating_eCOP,\"\"),\"\")","v":""},{"$f":"IF(DESPath = 3,IFERROR(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($E$292,PO_Enrgy_9_Hdr,0),FALSE)/$H307*VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C307,EnergyUnitsTable,3,FALSE),0)+IFERROR(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($E$292,PO_Enrgy_9_Hdr,0),FALSE)/$H307*VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($H307,EnergyUnitsTable,3,FALSE),0),0)","v":0},{"$f":"IFERROR(I307*VLOOKUP($B307,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B307),\"\",VLOOKUP($B307,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B307),\"\",VLOOKUP($B307,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,null,"Elec",{"$f":"IFERROR(VLOOKUP($B307,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)/$E$307*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C307,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B307,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)/$H$307*(IFERROR(VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1)+IFERROR(VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1))/VLOOKUP($C307,EnergyUnitsTable,3,FALSE),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(DESPath=3,IF(MATCH(\"Natural Gas\",PO_Enrgy_1_Index,0)>0,\"Natural Gas\",IF(MATCH(\"Fuel Oil / Diesel\",PO_Enrgy_1_Table,0)>1,\"Fuel Oil / Diesel\",\"\")),\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B308),\"\",VLOOKUP($B308,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C308=\"\",\"\",VLOOKUP(C308,ProjectEnergyTypeTable,3,FALSE))","v":""},null,null,null,{"$f":"IFERROR(IF(AND(DESPath=3,DistrictHeating,$B$307=\"Electricity\"),DESPath3_Heating_fCOP,\"\"),\"\")","v":""},{"$f":"IF(DESPath = 3,IFERROR(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($E$292,PO_Enrgy_9_Hdr,0),FALSE)/$H308*VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C308,EnergyUnitsTable,3,FALSE),0)+IFERROR(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($E$292,PO_Enrgy_9_Hdr,0),FALSE)/$H308*VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($H308,EnergyUnitsTable,3,FALSE),0),0)","v":0},{"$f":"IFERROR(I308*VLOOKUP($B308,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B308),\"\",VLOOKUP($B308,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B308),\"\",VLOOKUP($B308,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,null,"Fuel",{"$f":"IFERROR(VLOOKUP($B308,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)/$E$307*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C308,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B308,PO_Enrgy_8_Table,MATCH($E$281,PO_Enrgy_8_Hdr,0),FALSE)/$H$307*(IFERROR(VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1)+IFERROR(VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1))/VLOOKUP($C308,EnergyUnitsTable,3,FALSE),\"\")","v":""}]
["G","Energy_Type","Energy_Units",null,"Cooling_Avg_Efficiency","Cooling_Site_Energy","Cooling_Cost","Heating_Avg_Effiicency","Heating_Site_Energy","Heating_Cost",null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",null,null,null,"Cost/Unit District Cooling","Cost/Unit District Heating"]
["G","Proposed",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Total Proposed",{"$f":"IFERROR(V311+V312,\"\")","v":""},{"$f":"IFERROR(W311+W312,\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B311),\"\",VLOOKUP($B311,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C311=\"\",\"\",VLOOKUP(C311,ProjectEnergyTypeTable,3,FALSE))","v":""},null,{"$f":"IFERROR(VLOOKUP($B311,PO_Enrgy_9_Table,MATCH($E$292,PO_Enrgy_9_Hdr,0),FALSE)/$E$311*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C311,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(F311*VLOOKUP($B311,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,{"$f":"IF(DESPath = 3,IFERROR(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($H$292,PO_Enrgy_9_Hdr,0),FALSE)/$H311*VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C311,EnergyUnitsTable,3,FALSE),0)+IFERROR(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($H$292,PO_Enrgy_9_Hdr,0),FALSE)/$H311*VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($H311,EnergyUnitsTable,3,FALSE),0),0)","v":0},{"$f":"IFERROR(I311*VLOOKUP($B311,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B311),\"\",VLOOKUP($B311,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B311),\"\",VLOOKUP($B311,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,null,"Elec",{"$f":"IFERROR(VLOOKUP($B311,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)/$E$311*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C311,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B311,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)/$H$311*(IFERROR(VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1)+IFERROR(VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1))/VLOOKUP($C311,EnergyUnitsTable,3,FALSE),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK($B$308),\"\",$B$308),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B312),\"\",VLOOKUP($B312,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C312=\"\",\"\",VLOOKUP(C312,ProjectEnergyTypeTable,3,FALSE))","v":""},null,{"$f":"IFERROR(VLOOKUP($B312,PO_Enrgy_9_Table,MATCH($E$292,PO_Enrgy_9_Hdr,0),FALSE)/$E$311*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C312,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(F312*VLOOKUP($B312,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,{"$f":"IF(DESPath = 3,IFERROR(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($H$292,PO_Enrgy_9_Hdr,0),FALSE)/$H312*VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C312,EnergyUnitsTable,3,FALSE),0)+IFERROR(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($H$292,PO_Enrgy_9_Hdr,0),FALSE)/$H312*VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($H312,EnergyUnitsTable,3,FALSE),0),0)","v":0},{"$f":"IFERROR(I312*VLOOKUP($B312,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B312),\"\",VLOOKUP($B312,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B312),\"\",VLOOKUP($B312,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,null,"Fuel",{"$f":"IFERROR(VLOOKUP($B312,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)/$E$311*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C312,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B312,PO_Enrgy_8_Table,MATCH($H$281,PO_Enrgy_8_Hdr,0),FALSE)/$H$311*(IFERROR(VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1)+IFERROR(VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$292,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1))/VLOOKUP($C312,EnergyUnitsTable,3,FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(G312/E312,\"\")","v":""},{"$f":"IFERROR(J312/H312,\"\")","v":""}]
["G",null,null,null,null,null,null,null,"("]
["G"]
["G","Energy Type","Site Energy Units",null,"Baseline Energy Consumption \nwith District Energy Average Efficiencies \n(if DES Path 3 is used)",null,null,"Proposed Energy Consumption \nwith District Energy Average Efficiencies \n(if DES Path 3 is used)",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy","Source Energy","Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B318),\"\",VLOOKUP($B318,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C318=\"\",\"\",VLOOKUP(C318,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B318,PO_DESbase_Enrgy_Table,MATCH($F$305,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B318,PO_DESbase_Enrgy_Table,MATCH($I$305,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B318<>\"District Cooling\",B318<>\"District Hot Water\",B318<>\"District Steam\")),VLOOKUP($B318,PO_Enrgy_9_Table,MATCH($E$292,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E318*$R318,\"\")","v":""},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B318,PO_DESbase_Enrgy_Table,MATCH($G$305,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B318,PO_DESbase_Enrgy_Table,MATCH($J$305,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B318<>\"District Cooling\",B318<>\"District Hot Water\",B318<>\"District Steam\")),VLOOKUP($B318,PO_Enrgy_9_Table,MATCH($G$292,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B318,PO_DESdesign_Enrgy_Table,MATCH($F$309,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B318,PO_DESdesign_Enrgy_Table,MATCH($I$309,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B318<>\"District Cooling\",B318<>\"District Hot Water\",B318<>\"District Steam\")),VLOOKUP($B318,PO_Enrgy_9_Table,MATCH($H$292,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(H318*$R318,\"\")","v":""},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B318,PO_DESdesign_Enrgy_Table,MATCH($G$309,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B318,PO_DESdesign_Enrgy_Table,MATCH($J$309,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B318<>\"District Cooling\",B318<>\"District Hot Water\",B318<>\"District Steam\")),VLOOKUP($B318,PO_Enrgy_9_Table,MATCH($J$292,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(1-H318/E318,\"\")","v":""},{"$f":"IFERROR(1-I318/F318,\"\")","v":""},{"$f":"IFERROR(1-J318/G318,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B318),\"\",VLOOKUP($B318,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B318),\"\",VLOOKUP($B318,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C319=\"\",\"\",VLOOKUP(C319,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E319*$R319,\"\")","v":""},0,0,{"$f":"IFERROR(H319*$R319,\"\")","v":""},0,{"$f":"IFERROR(1-H319/E319,\"\")","v":""},{"$f":"IFERROR(1-I319/F319,\"\")","v":""},{"$f":"IFERROR(1-J319/G319,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C320=\"\",\"\",VLOOKUP(C320,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E320*$R320,\"\")","v":""},0,0,{"$f":"IFERROR(H320*$R320,\"\")","v":""},0,{"$f":"IFERROR(1-H320/E320,\"\")","v":""},"",{"$f":"IFERROR(1-J320/G320,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C321=\"\",\"\",VLOOKUP(C321,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E321*$R321,\"\")","v":""},0,0,{"$f":"IFERROR(H321*$R321,\"\")","v":""},0,{"$f":"IFERROR(1-H321/E321,\"\")","v":""},"",{"$f":"IFERROR(1-J321/G321,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C322=\"\",\"\",VLOOKUP(C322,ProjectEnergyTypeTable,3,FALSE))","v":""},0,"",0,0,"",0,"","","",null,null,null,"",""]
["G","","",{"$f":"IF(C323=\"\",\"\",VLOOKUP(C323,ProjectEnergyTypeTable,3,FALSE))","v":""},0,"",0,0,"",0,"","","",null,null,null,"",""]
["G",{"$f":"\"Energy Model Subtotal (\" & PO_SiteUnits & \")\"","v":"Energy Model Subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_10_Table,0,MATCH(E$317,PO_Enrgy_10_Hdr,0)),INDEX(PO_Enrgy_10_Table,0,MATCH($Q$317,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_10_Table,0,MATCH(F$317,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_10_Table,0,MATCH(G$317,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_10_Table,0,MATCH(H$317,PO_Enrgy_10_Hdr,0)),INDEX(PO_Enrgy_10_Table,0,MATCH($Q$317,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_10_Table,0,MATCH(I$317,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_10_Table,0,MATCH(J$317,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H324/E324,\"\")","v":""},"",{"$f":"IFERROR(1-J324/G324,\"\")","v":""}]
["G"]
["G","Data Center - Performance Rating Method Results"]
["G",{"$f":"CONCATENATE(\"Startup IT Loads: Enter the simulated energy consumption and cost for the Data Center based on Startup IT Loads as defined in the LEED Reference Guide.\",\" Report exceptional calculations and results from the Data Center calculator in the startup load results below,\",\" but do not include renewable energy in these reported results. Provide separate exceptional calculation method uploads as applicable for Startup Loads and for Full build-out.\", \" Also upload simulation outputs and performance rating method calculations with and without the exceptional calculation methods for both Startup IT Loads, and the full buildout IT loads.\",\"\n\n\",IF(DESPath=3,\" Note: The calculations using DES Path 3 must be performed manually for the Startup IT Load method, and supplemental documentation uploaded for the project must show these calculations.\",\"\"))","v":"Startup IT Loads: Enter the simulated energy consumption and cost for the Data Center based on Startup IT Loads as defined in the LEED Reference Guide. Report exceptional calculations and results from the Data Center calculator in the startup load results below, but do not include renewable energy in these reported results. Provide separate exceptional calculation method uploads as applicable for Startup Loads and for Full build-out. Also upload simulation outputs and performance rating method calculations with and without the exceptional calculation methods for both Startup IT Loads, and the full buildout IT loads.\n\n"}]
["G","Table: Performance rating data center - Startup IT loads"]
["G","Energy Type","Site Energy Units",null,"Baseline Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy","Source Energy","Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B332),\"\",VLOOKUP($B332,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C332=\"\",\"\",VLOOKUP(C332,ProjectEnergyTypeTable,3,FALSE))","v":""},null,{"$f":"IFERROR(E332*$Q332,\"\")","v":""},null,null,{"$f":"IFERROR(H332*$Q332,\"\")","v":""},null,{"$f":"IFERROR(1-H332/E332,\"\")","v":""},{"$f":"IFERROR(1-I332/F332,\"\")","v":""},{"$f":"IFERROR(1-J332/G332,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B332),\"\",VLOOKUP($B332,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B332),\"\",VLOOKUP($B332,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C333=\"\",\"\",VLOOKUP(C333,ProjectEnergyTypeTable,3,FALSE))","v":""},null,{"$f":"IFERROR(E333*$Q333,\"\")","v":""},null,null,{"$f":"IFERROR(H333*$Q333,\"\")","v":""},null,{"$f":"IFERROR(1-H333/E333,\"\")","v":""},{"$f":"IFERROR(1-I333/F333,\"\")","v":""},{"$f":"IFERROR(1-J333/G333,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C334=\"\",\"\",VLOOKUP(C334,ProjectEnergyTypeTable,3,FALSE))","v":""},null,{"$f":"IFERROR(E334*$Q334,\"\")","v":""},null,null,{"$f":"IFERROR(H334*$Q334,\"\")","v":""},null,{"$f":"IFERROR(1-H334/E334,\"\")","v":""},"",{"$f":"IFERROR(1-J334/G334,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C335=\"\",\"\",VLOOKUP(C335,ProjectEnergyTypeTable,3,FALSE))","v":""},null,{"$f":"IFERROR(E335*$Q335,\"\")","v":""},null,null,{"$f":"IFERROR(H335*$Q335,\"\")","v":""},null,{"$f":"IFERROR(1-H335/E335,\"\")","v":""},"",{"$f":"IFERROR(1-J335/G335,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C336=\"\",\"\",VLOOKUP(C336,ProjectEnergyTypeTable,3,FALSE))","v":""},null,"",null,null,"",null,"","","",null,null,null,"",""]
["G","","",{"$f":"IF(C337=\"\",\"\",VLOOKUP(C337,ProjectEnergyTypeTable,3,FALSE))","v":""},null,"",null,null,"",null,"","","",null,null,null,"",""]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_11_Table,0,MATCH(E$331,PO_Enrgy_11_Hdr,0)),INDEX(PO_Enrgy_11_Table,0,MATCH($Q$331,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_11_Table,0,MATCH(F$331,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_11_Table,0,MATCH(G$331,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_11_Table,0,MATCH(H$331,PO_Enrgy_11_Hdr,0)),INDEX(PO_Enrgy_11_Table,0,MATCH($Q$331,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_11_Table,0,MATCH(I$331,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_11_Table,0,MATCH(J$331,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H338/E338,\"\")","v":""},"",{"$f":"IFERROR(1-J338/G338,\"\")","v":""}]
["G"]
["G","Table: Performance rating data center - Full load IT loads (tabulated from spreadsheet data entered above)"]
["G","Energy Type","Site Energy Units",null,"Baseline Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy","Source Energy","Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B344),\"\",VLOOKUP($B344,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C344=\"\",\"\",VLOOKUP(C344,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(VLOOKUP($B344,PO_Enrgy_10_Table,MATCH($E$317,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(E344*$R344,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B344,PO_Enrgy_10_Table,MATCH($G$317,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B344,PO_Enrgy_10_Table,MATCH($H$317,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(H344*$R344,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B344,PO_Enrgy_10_Table,MATCH($J$317,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(1-H344/E344,\"\")","v":""},{"$f":"IFERROR(1-I344/F344,\"\")","v":""},{"$f":"IFERROR(1-J344/G344,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B344),\"\",VLOOKUP($B344,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B344),\"\",VLOOKUP($B344,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C345=\"\",\"\",VLOOKUP(C345,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E345*$R345,\"\")","v":""},0,0,{"$f":"IFERROR(H345*$R345,\"\")","v":""},0,{"$f":"IFERROR(1-H345/E345,\"\")","v":""},{"$f":"IFERROR(1-I345/F345,\"\")","v":""},{"$f":"IFERROR(1-J345/G345,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C346=\"\",\"\",VLOOKUP(C346,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E346*$R346,\"\")","v":""},0,0,{"$f":"IFERROR(H346*$R346,\"\")","v":""},0,{"$f":"IFERROR(1-H346/E346,\"\")","v":""},"",{"$f":"IFERROR(1-J346/G346,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C347=\"\",\"\",VLOOKUP(C347,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E347*$R347,\"\")","v":""},0,0,{"$f":"IFERROR(H347*$R347,\"\")","v":""},0,{"$f":"IFERROR(1-H347/E347,\"\")","v":""},"",{"$f":"IFERROR(1-J347/G347,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C348=\"\",\"\",VLOOKUP(C348,ProjectEnergyTypeTable,3,FALSE))","v":""},0,"",0,0,"",0,"","","",null,null,null,"",""]
["G","","",{"$f":"IF(C349=\"\",\"\",VLOOKUP(C349,ProjectEnergyTypeTable,3,FALSE))","v":""},0,"",0,0,"",0,"","","",null,null,null,"",""]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_12_Table,0,MATCH(E$343,PO_Enrgy_12_Hdr,0)),INDEX(PO_Enrgy_12_Table,0,MATCH($Q$343,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_12_Table,0,MATCH(F$343,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_12_Table,0,MATCH(G$343,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_12_Table,0,MATCH(H$343,PO_Enrgy_12_Hdr,0)),INDEX(PO_Enrgy_12_Table,0,MATCH($Q$343,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_12_Table,0,MATCH(I$343,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_12_Table,0,MATCH(J$343,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H350/E350,\"\")","v":""},"",{"$f":"IFERROR(1-J350/G350,\"\")","v":""}]
["G"]
["G","Table: Performance rating data center - Average between full Load IT loads and startup IT loads"]
["G","Energy Type","Site Energy Units",null,"Baseline Building Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Building Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy","Source Energy","Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B356),\"\",VLOOKUP($B356,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C356=\"\",\"\",VLOOKUP(C356,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B356,PO_Enrgy_11_Table,MATCH($E$331,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B356,PO_Enrgy_12_Table,MATCH($E$343,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B356,PO_Enrgy_12_Table,MATCH($E$343,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(E356*$R356,\"\")","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B356,PO_Enrgy_11_Table,MATCH($G$331,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B356,PO_Enrgy_12_Table,MATCH($G$343,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B356,PO_Enrgy_12_Table,MATCH($G$343,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B356,PO_Enrgy_11_Table,MATCH($H$331,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B356,PO_Enrgy_12_Table,MATCH($H$343,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B356,PO_Enrgy_12_Table,MATCH($H$343,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(H356*$R356,\"\")","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B356,PO_Enrgy_11_Table,MATCH($J$331,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B356,PO_Enrgy_12_Table,MATCH($J$343,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B356,PO_Enrgy_12_Table,MATCH($J$343,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(1-H356/E356,\"\")","v":""},{"$f":"IFERROR(1-I356/F356,\"\")","v":""},{"$f":"IFERROR(1-J356/G356,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B356),\"\",VLOOKUP($B356,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B356),\"\",VLOOKUP($B356,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C357=\"\",\"\",VLOOKUP(C357,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E357*$R357,\"\")","v":""},0,0,{"$f":"IFERROR(H357*$R357,\"\")","v":""},0,{"$f":"IFERROR(1-H357/E357,\"\")","v":""},{"$f":"IFERROR(1-I357/F357,\"\")","v":""},{"$f":"IFERROR(1-J357/G357,\"\")","v":""},null,null,null,"",{"$f":"IFERROR(IF(ISBLANK($B357),\"\",VLOOKUP($B357,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C358=\"\",\"\",VLOOKUP(C358,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E358*$R358,\"\")","v":""},0,0,{"$f":"IFERROR(H358*$R358,\"\")","v":""},0,{"$f":"IFERROR(1-H358/E358,\"\")","v":""},"",{"$f":"IFERROR(1-J358/G358,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C359=\"\",\"\",VLOOKUP(C359,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E359*$R359,\"\")","v":""},0,0,{"$f":"IFERROR(H359*$R359,\"\")","v":""},0,{"$f":"IFERROR(1-H359/E359,\"\")","v":""},"",{"$f":"IFERROR(1-J359/G359,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C360=\"\",\"\",VLOOKUP(C360,ProjectEnergyTypeTable,3,FALSE))","v":""},0,"",0,0,"",0,"","","",null,null,null,"",""]
["G","","",{"$f":"IF(C361=\"\",\"\",VLOOKUP(C361,ProjectEnergyTypeTable,3,FALSE))","v":""},0,"",0,0,"",0,"","","",null,null,null,"",""]
["G",{"$f":"\"Energy Model Subtotal (\" & PO_SiteUnits & \")\"","v":"Energy Model Subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_13_Table,0,MATCH(E$355,PO_Enrgy_13_Hdr,0)),INDEX(PO_Enrgy_13_Table,0,MATCH($Q$355,PO_Enrgy_13_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(F$355,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(G$355,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_13_Table,0,MATCH(H$355,PO_Enrgy_13_Hdr,0)),INDEX(PO_Enrgy_13_Table,0,MATCH($Q$355,PO_Enrgy_13_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(I$355,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(J$355,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H362/E362,\"\")","v":""},"",{"$f":"IFERROR(1-J362/G362,\"\")","v":""}]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Source"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Unregulated",null,"Unregulated",null,null,"Unregulated"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUMIF($V$119:$V$176,R365,$U$119:$U$176)+SUMIF($X$65:$X$68,R365,$W$65:$W$68)","v":0},"kWh",{"$f":"IFERROR(Q365*E282,\"-\")","v":"-"},"$",{"$f":"SUM(S365:S370)/U375","v":{"$error":"#DIV/0!"}},{"$f":"IFERROR(Q365*IFERROR(VLOOKUP(\"Electricity\",PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE),0),0)","v":0},{"$f":"$L$23","v":"Btu x 10^6"},{"$f":"SUM(V365:V370)/X375","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"$L$23","v":"Btu x 10^6"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Btu x 10^6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Btu x 10^6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUMIF($V$119:$V$176,R369,$U$119:$U$176)+SUMIF($X$65:$X$68,R369,$W$65:$W$68)","v":0},"THERM",{"$f":"IFERROR(Q369*E283,\"-\")","v":"-"},"$",null,{"$f":"IFERROR(Q369*IFERROR(VLOOKUP(\"Natural Gas\",PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE),0),0)","v":0},"Btu x 10^6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUMIF($V$119:$V$176,R370,$U$119:$U$176)+SUMIF($X$65:$X$68,R370,$W$65:$W$68)","v":0},"MWh",{"$f":"IFERROR(Q370*E284,\"-\")","v":"-"},"$",null,{"$f":"IFERROR(Q370*IFERROR(IF(DistrictCooling=FALSE,0,VLOOKUP(\"District Cooling\",PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),0),0)","v":0},"Btu x 10^6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Regulated",null,"Regulated",null,null,"Regulated"]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(E293)-Q365","v":0},"kWh",{"$f":"IFERROR(Q372*E282,\"\")","v":""},"$",{"$f":"SUM(S372:S375)/U375","v":{"$error":"#DIV/0!"}},{"$f":"Q372*IFERROR(VLOOKUP(\"Electricity\",PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE),0)","v":0},"Btu x 10^6",{"$f":"SUM(V372:V375)/X375","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Btu x 10^6"]
["G","Table 12.10: Proposed Results including Exceptional Calculation Method & Renewable Energy Production",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(E294)-Q369","v":0},"THERM",{"$f":"IFERROR(Q374*E283,\"-\")","v":"-"},"$",null,{"$f":"Q374*IFERROR(VLOOKUP(\"Natural Gas\",PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE),0)","v":0},"Btu x 10^6"]
["G","Energy Type","Site Energy Units",null,"On-Site Renewable Savings",null,null,"Proposed with On-Site Renewable Energy",null,null,"Percent Cost Savings",null,null,null,null,null,{"$f":"(E295)-Q370","v":0},"MWh",{"$f":"IFERROR(Q375*E284,\"-\")","v":"-"},"$",{"$f":"SUM(S365:S370,S372:S375)","v":0},{"$f":"Q375*IFERROR(IF(DistrictCooling=FALSE,0,VLOOKUP(\"District Cooling\",PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),0)","v":0},"Btu x 10^6",{"$f":"SUM(V365:V370,V372:V375)","v":0}]
["G",null,null,null,"Site Energy Use Savings ",{"$f":"\"Source Energy Use Savings \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use Savings \n(Btu x 10^6)"},"Cost Savings","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy","Source Energy","Cost",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Energy_Type","Energy_Units",null,"Renewable_Site_Savings","Renewable_Source_Savings","Renewable_Cost_Savings","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion","Virtual Rate"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B378),\"\",VLOOKUP($B378,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C378=\"\",\"\",VLOOKUP(C378,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,VLOOKUP($B378,PO_Enrgy_2_Table,MATCH($E$43,PO_Enrgy_2_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E378*$R378,\"\")","v":""},{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,VLOOKUP($B378,PO_Enrgy_2_Table,MATCH($J$43,PO_Enrgy_2_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B378,PO_Enrgy_13_Table,MATCH($H$355,PO_Enrgy_13_Hdr,0),FALSE)-IF(PO_SiteRenewable=TRUE,VLOOKUP($B378,PO_Enrgy_2_Table,MATCH($E$43,PO_Enrgy_2_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(H378*$R378,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B378,PO_Enrgy_13_Table,MATCH($J$355,PO_Enrgy_13_Hdr,0),FALSE)-IF(PO_SiteRenewable=TRUE,VLOOKUP($B378,PO_Enrgy_2_Table,MATCH($J$43,PO_Enrgy_2_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(1-$H378/VLOOKUP($B378,PO_Enrgy_13_Table,MATCH($E$355,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(1-$I378/VLOOKUP($B378,PO_Enrgy_13_Table,MATCH($F$355,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(1-$J378/VLOOKUP($B378,PO_Enrgy_13_Table,MATCH($G$355,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B378),\"\",VLOOKUP($B378,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B378),\"\",VLOOKUP($B378,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(G378/E378,\"\")","v":""}]
["G","","",{"$f":"IF(C379=\"\",\"\",VLOOKUP(C379,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E379*$R379,\"\")","v":""},0,0,{"$f":"IFERROR(H379*$R379,\"\")","v":""},0,{"$f":"IFERROR(1-$H379/VLOOKUP($B379,PO_Enrgy_13_Table,MATCH($E$355,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},"","",null,null,null,"","",{"$f":"IFERROR(G379/E379,\"\")","v":""}]
["G","","",{"$f":"IF(C380=\"\",\"\",VLOOKUP(C380,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E380*$R380,\"\")","v":""},0,0,{"$f":"IFERROR(H380*$R380,\"\")","v":""},0,"","","",null,null,null,"","",{"$f":"IFERROR(G380/E380,\"\")","v":""}]
["G","","",{"$f":"IF(C381=\"\",\"\",VLOOKUP(C381,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E381*$R381,\"\")","v":""},0,0,{"$f":"IFERROR(H381*$R381,\"\")","v":""},0,"","","",null,null,null,"","",{"$f":"IFERROR(G381/E381,\"\")","v":""}]
["G","","",{"$f":"IF(C382=\"\",\"\",VLOOKUP(C382,ProjectEnergyTypeTable,3,FALSE))","v":""},0,"",0,0,"",0,"","","",null,null,null,"","",""]
["G","","",{"$f":"IF(C383=\"\",\"\",VLOOKUP(C383,ProjectEnergyTypeTable,3,FALSE))","v":""},0,"",0,0,"",0,{"$f":"IFERROR(1-$H383/VLOOKUP($B383,PO_Enrgy_13_Table,MATCH($E$355,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},"","",null,null,null,"","",""]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_14_Table,0,MATCH(E$377,PO_Enrgy_14_Hdr,0)),INDEX(PO_Enrgy_14_Table,0,MATCH($Q$377,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(F$377,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(G$377,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_14_Table,0,MATCH(H$377,PO_Enrgy_14_Hdr,0)),INDEX(PO_Enrgy_14_Table,0,MATCH($Q$377,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(I$377,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(J$377,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-$H384/$E$362,\"\")","v":""},{"$f":"IFERROR(1-$I384/$F$362,\"\")","v":""},{"$f":"IFERROR(1-$J384/$G$362,\"\")","v":""}]
["G"]
["G","Table: Data center PUE3 of startup and full buildout IT loads "]
["G",{"$f":"\"Enter the IT equipment energy consumption \" & IF(Datacenter_Avg=FALSE, \" and total building consumption by end-use including renewable energy \",\"\") & \"for the Startup IT loads.  The information for the full buildout loads is tabulated from the data above.  PUE3 is calculated based on source energy.\"","v":"Enter the IT equipment energy consumption  and total building consumption by end-use including renewable energy for the Startup IT loads.  The information for the full buildout loads is tabulated from the data above.  PUE3 is calculated based on source energy."}]
["G","Energy Type","Site Energy Units",null,"Startup IT Loads\nBuilding energy consumption with Startup IT loads \nincluding Data Center Calculator and exceptional calculation measures",null,null,null,"Full Buildout IT Loads\nBuilding energy consumption with Full Buildout IT loads \nincluding Data Center Calculator and exceptional calculation measures"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"PUE3",null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"PUE3"]
["G","Energy_Type","Energy_Units",null,"Startup_Site_Energy","Startup_Source_Energy","Startup_PUE",null,"Buildout_Site_Energy","Buildout_Source_Energy","Buildoout_PUE",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"B235","v":"Fans - Kitchen Ventilation"},"kWh",{"$f":"IF(C391=\"\",\"\",VLOOKUP(C391,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,{"$f":"IFERROR(E391*$R391,\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP(B391,PO_design_table,MATCH($H$208,PO_design_hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(I391*$R391,\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(\"Electricity\",PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(\"electricity\",PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE),\"\")","v":""}]
["G","Total building consumption by end-use",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B393),\"\",VLOOKUP($B393,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C393=\"\",\"\",VLOOKUP(C393,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B393,PO_Enrgy_11_Table,MATCH($H$331,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B393,PO_Enrgy_14_Table,MATCH($E$377,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(E393*$R393,\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP($B393,PO_Enrgy_12_Table,MATCH($H$343,PO_Enrgy_12_Hdr,0),FALSE)-VLOOKUP($B393,PO_Enrgy_14_Table,MATCH($E$377,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(I393*$R393,\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B393),\"\",VLOOKUP($B393,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B393),\"\",VLOOKUP($B393,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C394=\"\",\"\",VLOOKUP(C394,ProjectEnergyTypeTable,3,FALSE))","v":""},"",{"$f":"IFERROR(E394*$R394,\"\")","v":""},null,null,0,{"$f":"IFERROR(I394*$R394,\"\")","v":""},null,null,null,null,null,null,"",""]
["G","","",{"$f":"IF(C395=\"\",\"\",VLOOKUP(C395,ProjectEnergyTypeTable,3,FALSE))","v":""},"",{"$f":"IFERROR(E395*$R395,\"\")","v":""},null,null,0,{"$f":"IFERROR(I395*$R395,\"\")","v":""},null,null,null,null,null,null,"",""]
["G","","",{"$f":"IF(C396=\"\",\"\",VLOOKUP(C396,ProjectEnergyTypeTable,3,FALSE))","v":""},"",{"$f":"IFERROR(E396*$R396,\"\")","v":""},null,null,0,{"$f":"IFERROR(I396*$R396,\"\")","v":""},null,null,null,null,null,null,"",""]
["G","","",{"$f":"IF(C397=\"\",\"\",VLOOKUP(C397,ProjectEnergyTypeTable,3,FALSE))","v":""},"","",null,null,0,"",null,null,null,null,null,null,"",""]
["G","","",{"$f":"IF(C398=\"\",\"\",VLOOKUP(C398,ProjectEnergyTypeTable,3,FALSE))","v":""},"","",null,null,0,"",null,null,null,null,null,null,"",""]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_15_Table,0,MATCH(E$390,PO_Enrgy_15_Hdr,0)),INDEX(PO_Enrgy_15_Table,0,MATCH($Q$390,PO_Enrgy_15_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_15_Table,0,MATCH(F$390,PO_Enrgy_15_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(F399/F391,\"\")","v":""},null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_15_Table,0,MATCH(I$390,PO_Enrgy_15_Hdr,0)),INDEX(PO_Enrgy_15_Table,0,MATCH($Q$390,PO_Enrgy_15_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_15_Table,0,MATCH(J$390,PO_Enrgy_15_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(J399/J391,\"\")","v":""}]
["G"]
["G","Table 12.11: Baseline and Proposed Total Energy Usage including Exceptional Calculation Methods and Renewable Energy Production"]
["G","Energy Type","Site Energy Units",null,"Baseline",null,null,"Proposed Design",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy","Source Energy","Cost",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B405),\"\",VLOOKUP($B405,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C405=\"\",\"\",VLOOKUP(C405,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(VLOOKUP($B405,PO_Enrgy_13_Table,MATCH($E$355,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(E405*$R405,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B405,PO_Enrgy_13_Table,MATCH($G$355,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B405,PO_Enrgy_14_Table,MATCH($H$355,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(H405*$R405,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B405,PO_Enrgy_14_Table,MATCH($J$355,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(1-H405/E405,\"\")","v":""},{"$f":"IFERROR(1-I405/F405,\"\")","v":""},{"$f":"IFERROR(1-J405/G405,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B405),\"\",VLOOKUP($B405,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B405),\"\",VLOOKUP($B405,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C406=\"\",\"\",VLOOKUP(C406,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E406*$R406,\"\")","v":""},0,0,{"$f":"IFERROR(H406*$R406,\"\")","v":""},0,{"$f":"IFERROR(1-H406/E406,\"\")","v":""},{"$f":"IFERROR(1-I406/F406,\"\")","v":""},{"$f":"IFERROR(1-J406/G406,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C407=\"\",\"\",VLOOKUP(C407,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E407*$R407,\"\")","v":""},0,0,{"$f":"IFERROR(H407*$R407,\"\")","v":""},0,{"$f":"IFERROR(1-H407/E407,\"\")","v":""},"",{"$f":"IFERROR(1-J407/G407,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C408=\"\",\"\",VLOOKUP(C408,ProjectEnergyTypeTable,3,FALSE))","v":""},0,{"$f":"IFERROR(E408*$R408,\"\")","v":""},0,0,{"$f":"IFERROR(H408*$R408,\"\")","v":""},0,{"$f":"IFERROR(1-H408/E408,\"\")","v":""},"",{"$f":"IFERROR(1-J408/G408,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C409=\"\",\"\",VLOOKUP(C409,ProjectEnergyTypeTable,3,FALSE))","v":""},0,"",0,0,"",0,"","","",null,null,null,"",""]
["G","","",{"$f":"IF(C410=\"\",\"\",VLOOKUP(C410,ProjectEnergyTypeTable,3,FALSE))","v":""},0,"",0,0,"",0,"","","",null,null,null,"",""]
["G","Totals",null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_16_Table,0,MATCH(E$404,PO_Enrgy_16_Hdr,0)),INDEX(PO_Enrgy_16_Table,0,MATCH($Q$404,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(F$404,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(G$404,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_16_Table,0,MATCH(H$404,PO_Enrgy_16_Hdr,0)),INDEX(PO_Enrgy_16_Table,0,MATCH($Q$404,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(I$404,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(J$404,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H411/E411,\"\")","v":""},"",{"$f":"IFERROR(1-J411/G411,\"\")","v":""}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Cost $",{"$f":"\"Source Energy \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy \n(Btu x 10^6)"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
[null,"Proposed Building Performance before site-generated renewable energy and exceptional calculations (PBP nre_nec, $/Source Energy)",null,null,null,null,null,null,null,null,null,null,{"$f":"J276","v":0},{"$f":"I276","v":0}]
[null,"Onsite Renewable Cost Savings, $/Source Energy",null,null,null,null,null,null,null,null,null,null,{"$f":"G384","v":0},{"$f":"F384","v":0}]
[null,"Exceptional Calculations Cost Savings, $/Source Energy",null,null,null,null,null,null,null,null,null,null,{"$f":"L93","v":0},{"$f":"J93","v":0}]
[null,"Proposed Building Performance including site-generated renewable energy and exceptional calculations (PBP, $/Source Energy)",null,null,null,null,null,null,null,null,null,null,{"$f":"J411","v":0},{"$f":"I411","v":0}]
[null,"Baseline Building Unregulated Energy Cost (BBUEC, $/Source Energy)",null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(G411-M419,\"\")","v":""},{"$f":"IFERROR(F411-N419,\"\")","v":""}]
[null,"Baseline Building Regulated Energy Cost (BBREC, $/Source Energy)",null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(G411*U372,\"\")","v":""},{"$f":"IFERROR(F411*X372,\"\")","v":""}]
[null,"Baseline Building Performance (BBP, $/Source Energy)",null,null,null,null,null,null,null,null,null,null,{"$f":"G411","v":0},{"$f":"F411","v":0}]
[null,"Building Performance Factor (BPF)",null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR((SUMPRODUCT('General Information'!K17:K21,'General Information'!M17:M21))/BuildingArea,\"\")","v":""},{"$f":"M421","v":""},{"$f":"IF('General Information'!L48=1,\"Update reference edition of 90.1 in row 48 of the General Information tab.\",\"\")","v":""}]
[null,"Target Performance Cost Index (PCIt) ",null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(((M418+(M421*M419))/M420),\"\")","v":""},{"$f":"IFERROR(((N418+(N421*N419))/N420),\"\")","v":""}]
[null,"Performance Cost Index without site-generated renewables and exceptional calculations (PCI nre_nec)",null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(M414/M420,\"\")","v":""},{"$f":"IFERROR(N414/N420,\"\")","v":""}]
[null,"Performance Cost Index including exceptional calculations (PCI ec)",null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR((M414-M416)/M420,\"\")","v":""},{"$f":"IFERROR((N414-N416)/N420,\"\")","v":""}]
[null,"Performance Cost Index including exceptional calculations and site-generated renewables (PCI ec+re)",null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(M417/M420,\"\")","v":""},{"$f":"IFERROR(N417/N420,\"\")","v":""}]
[null,{"$f":"\"% Improvement Beyond \"&'General Information'!C48&\", excluding site-generated renewable and exceptional calculations\"","v":"% Improvement Beyond ASHRAE 90.1-2013, excluding site-generated renewable and exceptional calculations"},null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(((M422-M423)/M422),\"-\")","v":"-"},{"$f":"IFERROR(((N422-N423)/N422),\"-\")","v":"-"}]
[null,{"$f":"\"% Improvement Beyond \"&'General Information'!C48&\", all included\"","v":"% Improvement Beyond ASHRAE 90.1-2013, all included"},null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(((M422-M425)/M422),\"-\")","v":"-"},{"$f":"IFERROR(((N422-N425)/N422),\"-\")","v":"-"}]
["G"]
["G","Table 12.12: Unmet Loads"]
[null,"Enter the non-coincident unmet load hours, consistent with the energy simulation output reports."]
["G","Unmet Loads",null,null,null,"Baseline",null,null,"Proposed Design",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Number of hours heating loads not met"]
["G","Number of hours cooling loads not met"]
["G","Totals",null,null,null,{"$f":"IF(ISERROR(F432+F433),0,F432+F433)","v":0},null,null,{"$f":"IF(ISERROR(I432+I433),0,I432+I433)","v":0}]
["G","Compliance",null,null,null,{"$f":"IF(ISERROR(OR(F432+F433,I432+I433)),\"Enter numbers only\",\n     IF(OR(F434>300,I434>300),\"No\",\"Yes\"))","v":"Yes"}]
[null,null,{"$f":"IF(ISERROR(F434+I434),\"\",IF(OR(I434>300,F434>300),\"Revise the model so that the unmet load hours for both the baseline and proposed case are 300 hours or less\",\"\"))","v":""}]
[null,"Quality Assurance Checks"]
[null,{"$f":"IF(MultipleBuildingsExist=\"No\",\"General information\",\"Multiple Building Details\")","v":"General information"},{"$f":"\"Total Area \"&IF(SI_IP_Units=\"IP\",\"(sq ft)\",\"(sq m)\")","v":"Total Area (sq ft)"}]
[null,null,{"$f":"IFERROR(IF(MultipleBuildingsExist=\"No\",\nGI_BldgArea,\nSUMIF(MBD_BS_Index,$H$5,OFFSET(MBD_BS_Index,0,MATCH('1 - Multiple Buildings Details'!$G$22,MBD_BS_Hdr,0)-1,1,1))+SUMIF(MBD_BS_Index,$H$5,OFFSET(MBD_BS_Index,0,MATCH('1 - Multiple Buildings Details'!$H$22,MBD_BS_Hdr,0)-1,1,1))),\"\")","v":0}]
[null,"Lighting",{"$f":"\"Total Area \"&IF(SI_IP_Units=\"IP\",\"(sq ft)\",\"(sq m)\")","v":"Total Area (sq ft)"},"Base Lighting Demand",null,"Design Lighting Demand","Base Exterior Lighting Demand","Design Exterior Lighting Demand","Base Non Tradeable Exterior Lighting Maximum","Design Non Tradeable Exterior Lighting Maximum"]
[null,null,{"$f":"IFERROR(TotalArea,\"\")","v":0},{"$f":"IFERROR(OFFSET(L_IL_SumTable,MATCH($H$5,L_IL_SumIndex,0)-1,MATCH('6b - General Lighting'!$L$107,L_IL_SumHdr,0)-1,1,1),\"\")","v":"Base_Power"},null,{"$f":"IFERROR(OFFSET(L_IL_SumTable,MATCH($H$5,L_IL_SumIndex,0)-1,MATCH('6b - General Lighting'!$O$107,L_IL_SumHdr,0)-1,1,1),\"\")","v":"Design_Power"},{"$f":"IFERROR(OFFSET(L_ExtSum_Table,1,MATCH('6b - General Lighting'!$J$171,L_ExtSum_Hdr,0)-1,1,1),\"\")","v":0},{"$f":"IFERROR(OFFSET(L_ExtSum_Table,1,MATCH('6b - General Lighting'!$M$171,L_ExtSum_Hdr,0)-1,1,1),\"\")","v":0},{"$f":"IFERROR(OFFSET(L_NTSurface_Table,MATCH('6b - General Lighting'!$B$165,L_NTSurface_Index,0)-1,MATCH('6b - General Lighting'!$J$158,L_NTSurface_Hdr,0)-1,1,1),\"\")","v":0},{"$f":"IFERROR(OFFSET(L_NTSurface_Table,MATCH('6b - General Lighting'!$B$165,L_NTSurface_Index,0)-1,MATCH('6b - General Lighting'!$M$158,L_NTSurface_Hdr,0)-1,1,1),\"\")","v":0}]
[null,"Shading and Fenestration","Zones Modeled","Baseline Above 40%",null,"App G. Baseline %","Entered Baseline %"]
[null,null,{"$f":"IFERROR('4 - Shading and Fenestration'!I49,\"\")","v":0},{"$f":"IF(IFERROR(COUNTIFS('4 - Shading and Fenestration'!S:S,$H$5,'4 - Shading and Fenestration'!U:U,TRUE),\"\")>0,TRUE,FALSE)","v":false},null,{"$f":"IFERROR(ROUND('4 - Shading and Fenestration'!D53,3),\"-\")","v":0},{"$f":"ROUND('4 - Shading and Fenestration'!B53,3)","v":{"$error":"#VALUE!"}}]
[null,"Performance Outputs","Baseline Lighting EFLHs","Design Lighting EFLHs",null,"Base Lighting Demand","Design Lighting Demand","Base Exterior Lighting Consumption","Design Exterior Lighting Consumption","Base Exterior EFLH","Design Ext EFLH"]
[null,null,{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$209,PO_design_index,0)-2,MATCH($S$208,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$209,PO_design_index,0)-2,MATCH($T$208,PO_design_hdr,0)-1,1,1)),\"\")","v":0},null,{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$209,PO_design_index,0)-1,MATCH($G$208,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$209,PO_design_index,0)-1,MATCH($H$208,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$213,PO_design_index,0)-2,MATCH($G$208,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$213,PO_design_index,0)-2,MATCH($H$208,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$213,PO_design_index,0)-2,MATCH($S$208,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$213,PO_design_index,0)-2,MATCH($T$208,PO_design_hdr,0)-1,1,1)),\"\")","v":0}]
[null,null,"Base Exterior Lighting Demand","Design Exterior Lighting Demand",null,"Base Miscellaneous % of Total","Design Miscellaneous % of Total","Unregulated Load Difference","Base Service Hot Waters % of Total","Design Service Hot Water % of Total","Base Pump Consumption",null,"Base Fan EFLH"]
[null,null,{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$213,PO_design_index,0)-1,MATCH($G$208,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$213,PO_design_index,0)-1,MATCH($H$208,PO_design_hdr,0)-1,1,1)),\"\")","v":0},null,{"$f":"IFERROR((OFFSET(PO_design_table,MATCH($B$233,PO_design_index,0)-2,MATCH($G$208,PO_design_hdr,0)-1,1,1)*OFFSET(PO_design_table,MATCH($B$233,PO_design_index,0)-2,MATCH($Q$208,PO_design_hdr,0)-1,1,1))/OFFSET(PO_ModelSubtotal,0,4,1,1),\"\")","v":""},{"$f":"IFERROR((OFFSET(PO_design_table,MATCH($B$233,PO_design_index,0)-2,MATCH($H$208,PO_design_hdr,0)-1,1,1)*OFFSET(PO_design_table,MATCH($B$233,PO_design_index,0)-2,MATCH($Q$208,PO_design_hdr,0)-1,1,1))/OFFSET(PO_ModelSubtotal,0,7,1,1),\"\")","v":""},null,{"$f":"IFERROR((OFFSET(PO_design_table,MATCH($B$231,PO_design_index,0)-2,MATCH($G$208,PO_design_hdr,0)-1,1,1)*OFFSET(PO_design_table,MATCH($B$231,PO_design_index,0)-2,MATCH($Q$208,PO_design_hdr,0)-1,1,1))/OFFSET(PO_ModelSubtotal,0,4,1,1),\"\")","v":""},{"$f":"IFERROR((OFFSET(PO_design_table,MATCH($B$231,PO_design_index,0)-2,MATCH($H$208,PO_design_hdr,0)-1,1,1)*OFFSET(PO_design_table,MATCH($B$231,PO_design_index,0)-2,MATCH($Q$208,PO_design_hdr,0)-1,1,1))/OFFSET(PO_ModelSubtotal,0,7,1,1),\"\")","v":""},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$223,PO_design_index,0)-2,MATCH($G$208,PO_design_hdr,0)-1,1,1)),\"\")","v":0},null,{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$227,PO_design_index,0)-2,MATCH($S$208,PO_design_hdr,0)-1,1,1)),\"\")","v":0}]
[null,null,"Design Fan EFLH","Base Fan Demand",null,"Design Fan Demand","PV EFLH","Renewable Rate Difference","Proposed Electric Rate","Proposed Gas Rate","Total Baseline Exterior Lighting Demand",null,"Total Design Exterior Lighting Demand"]
[null,null,{"$f":"IFERROR(IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$227,PO_design_index,0)-2,MATCH($T$208,PO_design_hdr,0)-1,1,1)),\"\"),\"\")","v":0},{"$f":"IFERROR(IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$227,PO_design_index,0)-1,MATCH($G$208,PO_design_hdr,0)-1,1,1)),\"\"),\"\")","v":0},null,{"$f":"IFERROR(IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$227,PO_design_index,0)-1,MATCH($H$208,PO_design_hdr,0)-1,1,1)),\"\"),\"\")","v":0},{"$f":"IFERROR(MAX(IFERROR(OFFSET(PO_renewable_table,MATCH(\"Photovoltaic system\",PO_renewable_Index,0)-2,MATCH($S$35,PO_renewable_hdr,0)-1,1,1),0),\nIFERROR(OFFSET(PO_renewable_table,MATCH(\"Solar thermal system\",PO_renewable_Index,0)-2,MATCH($S$35,PO_renewable_hdr,0)-1,1,1),0)),\"\")","v":""},null,{"$f":"IFERROR(OFFSET(PO_Enrgy_8_Table,MATCH(\"Electricity\",PO_Enrgy_8_Index,0)-2,MATCH($H$281,PO_Enrgy_8_Hdr,0)-1,1,1),\"\")","v":""},{"$f":"IFERROR(OFFSET(PO_Enrgy_8_Table,MATCH(\"Natural Gas\",PO_Enrgy_8_Index,0)-2,MATCH($H$281,PO_Enrgy_8_Hdr,0)-1,1,1),\"\")","v":""},{"$f":"IFERROR(GetPerformanceOutputRangeSums(\"PO_QA_BaseExtLtgDem\"),\"\")","v":"Error"},null,{"$f":"IFERROR(GetPerformanceOutputRangeSums(\"PO_QA_DesignExtLtgDem\"),\"\")","v":"Error"}]
[null,"General HVAC","Base non-water systems","Base water systems"]
[null,null,{"$f":"IFERROR(isbasehvac(2)+isbasehvac(3)+isbasehvac(4)+isbasehvac(6)+isbasehvac(9)+isbasehvac(10),\"\")","v":0},{"$f":"IFERROR(isbasehvac(1)+isbasehvac(5)+isbasehvac(7)+isbasehvac(8)+isbasehvac(11)+isbasehvac(12)+isbasehvac(13),\"\")","v":0}]
[null,"Air-Side HVAC","Base Fan Flow","Design Fan Flow",null,"Base Fan Power","Design Fan Power","Base Cooling Capacity","Design Cooling Capacity","Base Heating Capacity","Design Heating Capacity"]
[null,null,{"$f":"IFERROR(SUMIFS(AHVAC_Base_FanFlow,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_FanFlow,AHVAC_Design_ID,$H$5),\"\")","v":0},null,{"$f":"IFERROR(SUMIFS(AHVAC_Base_FanPower,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_FanPower,AHVAC_Design_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Base_CoolingCap,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_CoolingCap,AHVAC_Design_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Base_HeatingCap,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_HeatingCap,AHVAC_Design_ID,$H$5),\"\")","v":0}]
[null,null,"Base OA","Design OA"]
[null,null,{"$f":"IFERROR(SUMIFS(AHVAC_Base_OAFlow,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_OAFlow,AHVAC_Design_ID,$H$5),\"\")","v":0}]

{"sheet":"90.1-2004 Site EUI","index":34,"n_rows":79,"n_cols":23,"rows_kept":79,"cut":false,"hidden":true,"merged":[[78,1,78,2],[2,1,2,2],[2,3,2,22],[3,1,3,2],[26,1,26,2],[28,1,28,2],[28,3,28,22],[29,1,29,2],[52,1,52,2],[54,1,54,2],[54,3,54,22],[55,1,55,2]]}
[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23]
[]
[null,"Climate Zone 4A",null,"Site EUI (kBtu/SF/yr)"]
[null,"Building Type",null,"Lighting, Interior","Lighting, Exterior","DHW","Heating","Humidfy","Heat","Cooling","Heat Rejection","Fan","Heat Recovery","Fans","Pumps","Refrigeration","Elevator","Transformers","Cooking","Data Center","Equipment","Total","Weight"]
[null,"Apartments","Mid Rise",3.400673442,2.0497325260000001,11.07698497,9.7048652559999997,0,{"$f":"G5+H5","v":9.7048652559999997},5.1329011351175131,0,6.6386607806526179,0,{"$f":"L5+M5","v":6.6386607806526179},0,0,3.6409424406179123,0,0,0,10.903869648531787,52.548630198919838,0.23138567210488928]
[null,null,"High Rise",3.1704590850000001,2.3986648860000002,12.43616694,11.423244889999999,0,{"$f":"G6+H6","v":11.423244889999999},5.4521241511760241,0.25726473266786798,7.3243460463296666,0,{"$f":"L6+M6","v":7.3243460463296666},0.82619180861153263,0,1.8323394492391682,0.40659291729893776,0,0,10.950199897782836,56.47759480410604,0.27946667242036716]
["Multifamily",null,"Weighted Average",{"$f":"SUMPRODUCT(D5:D6,$V5:$V6)/SUM($V5:$V6)","v":3.2814181603246695},{"$f":"SUMPRODUCT(E5:E6,$V5:$V6)/SUM($V5:$V6)","v":2.2304859221812725},11.781066291393786,10.595017590321277,0,10.595017590321277,5.2982645433488527,0.13326787503281215,6.9938583911080787,0,6.9938583911080787,0.42798259038996028,0,2.7040527436138397,0.21062262802175796,0,0,10.927869571892442,54.583906307628752,0.25629251679769866]
[null,"Healthcare","Hospital",16.420497780000002,1.0263596239999999,4.8278698970000002,53.04110996,7.4638269399999997,60.504936899999997,16.008226649165014,2.4664036132355562,17.163190371882518,0,17.163190371882518,4.4795131117469493,1.0435172832042565,9.9723134562589788,0.68132064049424235,16.988614125821439,0,21.584459558713572,173.16722301152254,0.17848792406481528]
[null,null,"Clinic",14.15332733,5.2526237370000004,2.9571542289999999,42.443957959999999,5.0664688619999998,47.510426821999999,28.327955966394761,0,13.404308647975382,0,13.404308647975382,0.43713980486494408,0,15.096741643465389,0,0,0,32.18137152998257,159.32104971068304,0.18710373737855782]
["Healthcare/hospital",null,"Weighted Average",{"$f":"SUMPRODUCT(D8:D9,$V8:$V9)/SUM($V8:$V9)","v":15.334119686091013},{"$f":"SUMPRODUCT(E8:E9,$V8:$V9)/SUM($V8:$V9)","v":3.0514922078500155},{"$f":"SUMPRODUCT(F8:F9,$V8:$V9)/SUM($V8:$V9)","v":3.9314641937378036},{"$f":"SUMPRODUCT(G8:G9,$V8:$V9)/SUM($V8:$V9)","v":47.963188363666639},{"$f":"SUMPRODUCT(H8:H9,$V8:$V9)/SUM($V8:$V9)","v":6.3150658050818222},{"$f":"SUMPRODUCT(I8:I9,$V8:$V9)/SUM($V8:$V9)","v":54.278254168748447},{"$f":"SUMPRODUCT(J8:J9,$V8:$V9)/SUM($V8:$V9)","v":21.911569317170738},{"$f":"SUMPRODUCT(K8:K9,$V8:$V9)/SUM($V8:$V9)","v":1.2845573801227852},{"$f":"SUMPRODUCT(L8:L9,$V8:$V9)/SUM($V8:$V9)","v":15.362017124212688},{"$f":"SUMPRODUCT(M8:M9,$V8:$V9)/SUM($V8:$V9)","v":0},{"$f":"SUMPRODUCT(N8:N9,$V8:$V9)/SUM($V8:$V9)","v":15.362017124212688},{"$f":"SUMPRODUCT(O8:O9,$V8:$V9)/SUM($V8:$V9)","v":2.5424969478325656},{"$f":"SUMPRODUCT(P8:P9,$V8:$V9)/SUM($V8:$V9)","v":0.54348680817379447},{"$f":"SUMPRODUCT(Q8:Q9,$V8:$V9)/SUM($V8:$V9)","v":12.427826462081191},{"$f":"SUMPRODUCT(R8:R9,$V8:$V9)/SUM($V8:$V9)","v":0.35484681107352711},{"$f":"SUMPRODUCT(S8:S9,$V8:$V9)/SUM($V8:$V9)","v":8.8480447953746655},{"$f":"SUMPRODUCT(T8:T9,$V8:$V9)/SUM($V8:$V9)","v":0},{"$f":"SUMPRODUCT(U8:U9,$V8:$V9)/SUM($V8:$V9)","v":26.662266138571098},{"$f":"SUMPRODUCT(V8:V9,$V8:$V9)/SUM($V8:$V9)","v":166.53244204104035},{"$f":"SUMPRODUCT(W8:W9,$V8:$V9)/SUM($V8:$V9)","v":0.18261643184651263}]
[null,"Hotel","Large",11.27571893,2.375318751,16.986839939999999,23.287102919999999,0,23.287102919999999,17.189910940058958,0,7.8454534007533576,3.9195049549623322,11.76495835571569,1.8294852988863415,0.7994606177530299,7.5937691377333767,0.44441758131346221,19.803352735924612,0,7.4458244095061108,120.79615961789156,0.19357586285323519]
[null,null,"Small",10.92771031,2.090873422,13.13367994,9.9881969159999997,0,9.9881969159999997,7.9145089046803383,0,6.511596039535207,0,6.511596039535207,5.7055740012036471E-3,0,5.6869727610347303,0,0,0,16.769679724961289,73.028923592212763,0.18280635362367731]
["Hotel/motel",null,"Weighted Average",{"$f":"SUMPRODUCT(D11:D12,$V11:$V12)/SUM($V11:$V12)","v":11.144597124202233},{"$f":"SUMPRODUCT(E11:E12,$V11:$V12)/SUM($V11:$V12)","v":2.2681461608807667},{"$f":"SUMPRODUCT(F11:F12,$V11:$V12)/SUM($V11:$V12)","v":15.535056081233153},{"$f":"SUMPRODUCT(G11:G12,$V11:$V12)/SUM($V11:$V12)","v":18.276374822577438},{"$f":"SUMPRODUCT(H11:H12,$V11:$V12)/SUM($V11:$V12)","v":0},{"$f":"SUMPRODUCT(I11:I12,$V11:$V12)/SUM($V11:$V12)","v":18.276374822577438},{"$f":"SUMPRODUCT(J11:J12,$V11:$V12)/SUM($V11:$V12)","v":13.695148470154816},{"$f":"SUMPRODUCT(K11:K12,$V11:$V12)/SUM($V11:$V12)","v":0},{"$f":"SUMPRODUCT(L11:L12,$V11:$V12)/SUM($V11:$V12)","v":7.3428860049239999},{"$f":"SUMPRODUCT(M11:M12,$V11:$V12)/SUM($V11:$V12)","v":2.4427238122194943},{"$f":"SUMPRODUCT(N11:N12,$V11:$V12)/SUM($V11:$V12)","v":9.7856098171434933},{"$f":"SUMPRODUCT(O11:O12,$V11:$V12)/SUM($V11:$V12)","v":1.1423261966080858},{"$f":"SUMPRODUCT(P11:P12,$V11:$V12)/SUM($V11:$V12)","v":0.49824187247029539},{"$f":"SUMPRODUCT(Q11:Q12,$V11:$V12)/SUM($V11:$V12)","v":6.8753312317948216},{"$f":"SUMPRODUCT(R11:R12,$V11:$V12)/SUM($V11:$V12)","v":0.27697105142550343},{"$f":"SUMPRODUCT(S11:S12,$V11:$V12)/SUM($V11:$V12)","v":12.341895684703893},{"$f":"SUMPRODUCT(T11:T12,$V11:$V12)/SUM($V11:$V12)","v":0},{"$f":"SUMPRODUCT(U11:U12,$V11:$V12)/SUM($V11:$V12)","v":10.958842983470156},{"$f":"SUMPRODUCT(V11:V12,$V11:$V12)/SUM($V11:$V12)","v":102.79854149666465},{"$f":"SUMPRODUCT(W11:W12,$V11:$V12)/SUM($V11:$V12)","v":0.18951815446160009}]
[null,"Office","Large",9.7720209400000009,1.8762692439999999,1.0254198510000001,9.1966524570000008,5.4229742999999997E-2,9.2508822000000013,10.847526801687966,1.5393108729050839,4.6444580374978948,0,4.6444580374978948,2.6401252156088799,0,3.7199093720667165,0.27344264041653632,0,28.373422517411417,11.164870782868572,85.127658475463065,0.34018675031287815]
[null,null,"Medium",9.7719831740000007,3.9965125389999998,1.3674313899999999,9.5469629739999995,0,9.5469629739999995,7.8010397367047064,0,1.969175617214888,0,1.969175617214888,2.6517312411426866E-3,0,3.0930073842022847,0.59657588685015295,0,0,11.336653317296932,49.481993750510114,0.1967408890034183]
[null,null,"Small",12.22708319,4.4231852519999997,3.1084636520000002,2.469014059,0,2.469014059,5.4897811504907308,0,4.2956762104689208,0,4.2956762104689208,0,0,0,0,0,0,9.097942397310069,41.111145911269723,0.16685138805183178]
["Office",null,"Weighted Average",{"$f":"SUMPRODUCT(D14:D16,$V14:$V16)/SUM($V14:$V16)","v":10.346389795103857},{"$f":"SUMPRODUCT(E14:E16,$V14:$V16)/SUM($V14:$V16)","v":3.0691872327839342},1.609071482252979,7.7213184967989559,2.6271511911245445E-2,7.7475900087102012,8.7361699158480608,0.74571668046878892,3.8095134541658155,0,3.8095134541658155,1.2797511337267915,0,2.6730776983694775,0.30046128045466697,0,13.745458974957227,10.729671005935613,64.792058662777407,0.25924014220995706]
[null,"Dining","Restaurant",31.98926148,10.000844259999999,69.185966570000005,122.482365,0,122.482365,24.810847073791347,0,51.804855707015633,0,51.804855707015633,7.7539281715739733E-2,18.388938893331723,0,0,152.90540510521441,0,0,481.64602337106891,0.192721124592207]
[null,null,"Fast Food",28.46036192,10.37885868,70.811526939999993,177.26567689999999,0,177.26567689999999,28.111620135945621,0,47.155953938424631,0,47.155953938424631,0,40.912866293926882,0,0,269.48507596961235,0,0,672.58194077790949,0.15169200879179751]
["Restaurant",null,"Weighted Average",{"$f":"SUMPRODUCT(D18:D19,$V18:$V19)/SUM($V18:$V19)","v":29.932931024841526},{"$f":"SUMPRODUCT(E18:E19,$V18:$V19)/SUM($V18:$V19)","v":10.221117620326261},{"$f":"SUMPRODUCT(F18:F19,$V18:$V19)/SUM($V18:$V19)","v":70.133199337239688},{"$f":"SUMPRODUCT(G18:G19,$V18:$V19)/SUM($V18:$V19)","v":154.40523239224049},{"$f":"SUMPRODUCT(H18:H19,$V18:$V19)/SUM($V18:$V19)","v":0},{"$f":"SUMPRODUCT(I18:I19,$V18:$V19)/SUM($V18:$V19)","v":154.40523239224049},{"$f":"SUMPRODUCT(J18:J19,$V18:$V19)/SUM($V18:$V19)","v":26.734245588787488},{"$f":"SUMPRODUCT(K18:K19,$V18:$V19)/SUM($V18:$V19)","v":0},{"$f":"SUMPRODUCT(L18:L19,$V18:$V19)/SUM($V18:$V19)","v":49.095887053401192},{"$f":"SUMPRODUCT(M18:M19,$V18:$V19)/SUM($V18:$V19)","v":0},{"$f":"SUMPRODUCT(N18:N19,$V18:$V19)/SUM($V18:$V19)","v":49.095887053401192},{"$f":"SUMPRODUCT(O18:O19,$V18:$V19)/SUM($V18:$V19)","v":3.2356248378517624E-2},{"$f":"SUMPRODUCT(P18:P19,$V18:$V19)/SUM($V18:$V19)","v":31.513891047997841},{"$f":"SUMPRODUCT(Q18:Q19,$V18:$V19)/SUM($V18:$V19)","v":0},{"$f":"SUMPRODUCT(R18:R19,$V18:$V19)/SUM($V18:$V19)","v":0},{"$f":"SUMPRODUCT(S18:S19,$V18:$V19)/SUM($V18:$V19)","v":220.83772326130637},{"$f":"SUMPRODUCT(T18:T19,$V18:$V19)/SUM($V18:$V19)","v":0},{"$f":"SUMPRODUCT(U18:U19,$V18:$V19)/SUM($V18:$V19)","v":0},{"$f":"SUMPRODUCT(V18:V19,$V18:$V19)/SUM($V18:$V19)","v":592.90658357451935},{"$f":"SUMPRODUCT(W18:W19,$V18:$V19)/SUM($V18:$V19)","v":0.16881298582709978}]
[null,"Commercial","Retail Store",18.89221216,4.4161817760000002,3.6915427030000001,21.318591940000001,0,21.318591940000001,9.7384832698849841,0,14.508666053782603,0,14.508666053782603,0,0,0,0,0,0,7.4931493277174797,80.058827230385063,0.16686701421318281]
[null,null,"Strip Mall",26.631692269999999,6.0582307010000003,2.9279903420000002,25.303768340000001,0,25.303768340000001,10.021066959999999,0,11.101840484444445,0,11.101840484444445,0,0,0,0,0,0,5.4236712755555549,87.468260373000007,0.17783967651747074]
["Retail",null,"Weighted Average",{"$f":"SUMPRODUCT(D21:D22,$V21:$V22)/SUM($V21:$V22)","v":22.933104120205343},{"$f":"SUMPRODUCT(E21:E22,$V21:$V22)/SUM($V21:$V22)","v":5.2735187295148691},{"$f":"SUMPRODUCT(F21:F22,$V21:$V22)/SUM($V21:$V22)","v":3.2928812227832482},{"$f":"SUMPRODUCT(G21:G22,$V21:$V22)/SUM($V21:$V22)","v":23.399308867478489},{"$f":"SUMPRODUCT(H21:H22,$V21:$V22)/SUM($V21:$V22)","v":0},{"$f":"SUMPRODUCT(I21:I22,$V21:$V22)/SUM($V21:$V22)","v":23.399308867478489},{"$f":"SUMPRODUCT(J21:J22,$V21:$V22)/SUM($V21:$V22)","v":9.8860242087130992},{"$f":"SUMPRODUCT(K21:K22,$V21:$V22)/SUM($V21:$V22)","v":0},{"$f":"SUMPRODUCT(L21:L22,$V21:$V22)/SUM($V21:$V22)","v":12.729914269774136},{"$f":"SUMPRODUCT(M21:M22,$V21:$V22)/SUM($V21:$V22)","v":0},{"$f":"SUMPRODUCT(N21:N22,$V21:$V22)/SUM($V21:$V22)","v":12.729914269774136},{"$f":"SUMPRODUCT(O21:O22,$V21:$V22)/SUM($V21:$V22)","v":0},{"$f":"SUMPRODUCT(P21:P22,$V21:$V22)/SUM($V21:$V22)","v":0},{"$f":"SUMPRODUCT(Q21:Q22,$V21:$V22)/SUM($V21:$V22)","v":0},{"$f":"SUMPRODUCT(R21:R22,$V21:$V22)/SUM($V21:$V22)","v":0},{"$f":"SUMPRODUCT(S21:S22,$V21:$V22)/SUM($V21:$V22)","v":0},{"$f":"SUMPRODUCT(T21:T22,$V21:$V22)/SUM($V21:$V22)","v":0},{"$f":"SUMPRODUCT(U21:U22,$V21:$V22)/SUM($V21:$V22)","v":6.4126455853540234},{"$f":"SUMPRODUCT(V21:V22,$V21:$V22)/SUM($V21:$V22)","v":83.927397003823202},{"$f":"SUMPRODUCT(W21:W22,$V21:$V22)/SUM($V21:$V22)","v":0.17259599629689612}]
[null,"School","Secondary",14.812607059999999,0.99261105199999999,2.9372792360000002,13.98019802,0,13.98019802,14.022384366983264,0,7.9149492619270037,2.8967789124033252,10.811728174330328,0.95093757225433528,0.94437653482670836,0.34053881146459192,0.35674836827305617,4.0631337714826774,0,9.5406132051762249,73.753156172791194,0.19428622027148637]
[null,null,"Primary",15.51480074,1.088551051,1.8992069890000001,19.245586880000001,0,19.245586880000001,11.189822824808342,0,6.163926735082951,2.0444301356156789,8.2083568706986298,1.8330522870779756E-2,1.741150212144567,0,0.61562868805689641,6.5470043462519074,0,14.056271833793794,80.124710958624917,0.17919046104370323]
["School",null,"Weighted Average",{"$f":"SUMPRODUCT(D24:D25,$V24:$V25)/SUM($V24:$V25)","v":15.178241616130954},{"$f":"SUMPRODUCT(E24:E25,$V24:$V25)/SUM($V24:$V25)","v":1.0425673246761784},{"$f":"SUMPRODUCT(F24:F25,$V24:$V25)/SUM($V24:$V25)","v":2.3967516065520873},{"$f":"SUMPRODUCT(G24:G25,$V24:$V25)/SUM($V24:$V25)","v":16.721903298069389},{"$f":"SUMPRODUCT(H24:H25,$V24:$V25)/SUM($V24:$V25)","v":0},{"$f":"SUMPRODUCT(I24:I25,$V24:$V25)/SUM($V24:$V25)","v":16.721903298069389},{"$f":"SUMPRODUCT(J24:J25,$V24:$V25)/SUM($V24:$V25)","v":12.547460266004832},{"$f":"SUMPRODUCT(K24:K25,$V24:$V25)/SUM($V24:$V25)","v":0},{"$f":"SUMPRODUCT(L24:L25,$V24:$V25)/SUM($V24:$V25)","v":7.0031860794700984},{"$f":"SUMPRODUCT(M24:M25,$V24:$V25)/SUM($V24:$V25)","v":2.4529581040623669},{"$f":"SUMPRODUCT(N24:N25,$V24:$V25)/SUM($V24:$V25)","v":9.4561441835324658},{"$f":"SUMPRODUCT(O24:O25,$V24:$V25)/SUM($V24:$V25)","v":0.46532601769583437},{"$f":"SUMPRODUCT(P24:P25,$V24:$V25)/SUM($V24:$V25)","v":1.3592592062898619},{"$f":"SUMPRODUCT(Q24:Q25,$V24:$V25)/SUM($V24:$V25)","v":0.16321913354436554},{"$f":"SUMPRODUCT(R24:R25,$V24:$V25)/SUM($V24:$V25)","v":0.49154820129804683},{"$f":"SUMPRODUCT(S24:S25,$V24:$V25)/SUM($V24:$V25)","v":5.3564933401596315},{"$f":"SUMPRODUCT(T24:T25,$V24:$V25)/SUM($V24:$V25)","v":0},{"$f":"SUMPRODUCT(U24:U25,$V24:$V25)/SUM($V24:$V25)","v":11.891931488635418},{"$f":"SUMPRODUCT(V24:V25,$V24:$V25)/SUM($V24:$V25)","v":77.070845682589081},{"$f":"SUMPRODUCT(W24:W25,$V24:$V25)/SUM($V24:$V25)","v":0.18642580884666374}]
["Warehouse","Warehouse",null,8.7793392059999995,2.2493003680000001,0.47871407199999999,12.242857860000001,0,12.242857860000001,0.30620941992506484,0,0.83920689941396864,0,0.83920689941396864,0,0,0,0,0,0,2.5371117206263811,27.432739545965415,0.14631429773497143]
[]
[null,"Climate Zone 5A",null,"Site EUI (kBtu/SF/yr)"]
[null,"Building Type",null,"Lighting, Interior","Lighting, Exterior","DHW","Heating","Humidfy","Heat","Cooling","Heat Rejection","Fan","Heat Recovery","Fans","Pumps","Refrigeration","Elevator","Transformers","Cooking","Data Center","Equipment","Total","Weight"]
[null,"Apartments","Mid Rise",3.400673442,2.0474847039999999,11.71649028,17.481005119999999,0,{"$f":"G31+H31","v":17.481005119999999},4.0856971429418216,0,6.7198633413354667,0,{"$f":"L31+M31","v":6.7198633413354667},0,0,3.6409424406179123,0,0,0,10.903869648531787,59.996026119426986,0.15323697055373742]
[null,null,"High Rise",3.1704590850000001,2.3957427010000001,13.24653979,21.080318510000001,0,{"$f":"G32+H32","v":21.080318510000001},4.238068388419955,0.19870862706278455,7.4705677221642635,0,{"$f":"L32+M32","v":7.4705677221642635},0.84765863429438559,0,1.8323394492391682,0.40659291729893776,0,0,10.950199897782836,65.837195722262337,0.12973302267845771]
["Multifamily",null,"Weighted Average",{"$f":"SUMPRODUCT(D31:D32,$V31:$V32)/SUM($V31:$V32)","v":3.2802229960998517},{"$f":"SUMPRODUCT(E31:E32,$V31:$V32)/SUM($V31:$V32)","v":2.2296967587718166},{"$f":"SUMPRODUCT(F31:F32,$V31:$V32)/SUM($V31:$V32)","v":12.517027432115162},{"$f":"SUMPRODUCT(G31:G32,$V31:$V32)/SUM($V31:$V32)","v":19.364201756428173},{"$f":"SUMPRODUCT(H31:H32,$V31:$V32)/SUM($V31:$V32)","v":0},{"$f":"SUMPRODUCT(I31:I32,$V31:$V32)/SUM($V31:$V32)","v":19.364201756428173},{"$f":"SUMPRODUCT(J31:J32,$V31:$V32)/SUM($V31:$V32)","v":4.1654192971087847},{"$f":"SUMPRODUCT(K31:K32,$V31:$V32)/SUM($V31:$V32)","v":0.10396633401069204},{"$f":"SUMPRODUCT(L31:L32,$V31:$V32)/SUM($V31:$V32)","v":7.1126393549097351},{"$f":"SUMPRODUCT(M31:M32,$V31:$V32)/SUM($V31:$V32)","v":0},{"$f":"SUMPRODUCT(N31:N32,$V31:$V32)/SUM($V31:$V32)","v":7.1126393549097351},{"$f":"SUMPRODUCT(O31:O32,$V31:$V32)/SUM($V31:$V32)","v":0.44350344523417184},{"$f":"SUMPRODUCT(P31:P32,$V31:$V32)/SUM($V31:$V32)","v":0},{"$f":"SUMPRODUCT(Q31:Q32,$V31:$V32)/SUM($V31:$V32)","v":2.69466333097962},{"$f":"SUMPRODUCT(R31:R32,$V31:$V32)/SUM($V31:$V32)","v":0.21273346643840821},{"$f":"SUMPRODUCT(S31:S32,$V31:$V32)/SUM($V31:$V32)","v":0},{"$f":"SUMPRODUCT(T31:T32,$V31:$V32)/SUM($V31:$V32)","v":0},{"$f":"SUMPRODUCT(U31:U32,$V31:$V32)/SUM($V31:$V32)","v":10.928110096667496},{"$f":"SUMPRODUCT(V31:V32,$V31:$V32)/SUM($V31:$V32)","v":63.052184268763909},{"$f":"SUMPRODUCT(W31:W32,$V31:$V32)/SUM($V31:$V32)","v":0.14093947078489683}]
[null,"Healthcare","Hospital",16.420497780000002,1.025103418,5.0802276219999998,58.174775990000001,8.2533917179999996,66.428167708000004,12.599904012819824,2.0147975275464698,17.233537910816104,0,17.233537910816104,4.0207230992832326,1.0294242210637272,9.9723134562589788,0.68135989706046762,16.988614125821439,0,21.584459558713572,175.07913033738382,0.23550813259375961]
[null,null,"Clinic",14.15332733,5.253086809,3.124514113,48.397214470000002,6.066240938,54.463455408000002,20.016048200068383,0,13.403150969569678,0,13.403150969569678,0.55823308772529678,0,15.096741643465389,0,0,0,32.18137152998257,158.24992909081135,0.24213976109604499]
["Healthcare/hospital",null,"Weighted Average",{"$f":"SUMPRODUCT(D34:D35,$V34:$V35)/SUM($V34:$V35)","v":15.344145290466846},{"$f":"SUMPRODUCT(E34:E35,$V34:$V35)/SUM($V34:$V35)","v":3.0323633699845018},{"$f":"SUMPRODUCT(F34:F35,$V34:$V35)/SUM($V34:$V35)","v":4.1517411448470485},{"$f":"SUMPRODUCT(G34:G35,$V34:$V35)/SUM($V34:$V35)","v":53.532821220513839},{"$f":"SUMPRODUCT(H34:H35,$V34:$V35)/SUM($V34:$V35)","v":7.2150290368714671},{"$f":"SUMPRODUCT(I34:I35,$V34:$V35)/SUM($V34:$V35)","v":60.747850257385323},{"$f":"SUMPRODUCT(J34:J35,$V34:$V35)/SUM($V34:$V35)","v":16.120762031537307},{"$f":"SUMPRODUCT(K34:K35,$V34:$V35)/SUM($V34:$V35)","v":1.0582605655020465},{"$f":"SUMPRODUCT(L34:L35,$V34:$V35)/SUM($V34:$V35)","v":15.415039209015418},{"$f":"SUMPRODUCT(M34:M35,$V34:$V35)/SUM($V34:$V35)","v":0},{"$f":"SUMPRODUCT(N34:N35,$V34:$V35)/SUM($V34:$V35)","v":15.415039209015418},{"$f":"SUMPRODUCT(O34:O35,$V34:$V35)/SUM($V34:$V35)","v":2.3768856260469056},{"$f":"SUMPRODUCT(P34:P35,$V34:$V35)/SUM($V34:$V35)","v":0.54069902480524934},{"$f":"SUMPRODUCT(Q34:Q35,$V34:$V35)/SUM($V34:$V35)","v":12.405165841369016},{"$f":"SUMPRODUCT(R34:R35,$V34:$V35)/SUM($V34:$V35)","v":0.35788028331149319},{"$f":"SUMPRODUCT(S34:S35,$V34:$V35)/SUM($V34:$V35)","v":8.9231697707020299},{"$f":"SUMPRODUCT(T34:T35,$V34:$V35)/SUM($V34:$V35)","v":0},{"$f":"SUMPRODUCT(U34:U35,$V34:$V35)/SUM($V34:$V35)","v":26.615405768178807},{"$f":"SUMPRODUCT(V34:V35,$V34:$V35)/SUM($V34:$V35)","v":167.089368183152},{"$f":"SUMPRODUCT(W34:W35,$V34:$V35)/SUM($V34:$V35)","v":0.23865653718243707}]
[null,"Hotel","Large",11.27571893,2.3755516490000002,17.51903634,37.08408215,0,37.08408215,13.592347576154602,0,10.591699795283327,3.7721586472322306,14.363858442515557,1.67049412954471,0.79503557058630858,7.5937691377333767,0.44433994898460527,19.803352735924612,0,7.4458244095061108,133.96341101994989,0.18565490755171163]
[null,null,"Small",10.92771031,2.0884595259999998,13.986456459999999,16.305540529999998,0,16.305540529999998,6.4402763645201606,0,6.5076460256469595,0,6.5076460256469595,5.7055740012036471E-3,0,5.6869727610347303,0,0,0,16.769679724961289,78.718447276164341,0.21185128964646066]
["Hotel/motel",null,"Weighted Average",{"$f":"SUMPRODUCT(D37:D38,$V37:$V38)/SUM($V37:$V38)","v":11.146912935804767},{"$f":"SUMPRODUCT(E37:E38,$V37:$V38)/SUM($V37:$V38)","v":2.2692922513775069},{"$f":"SUMPRODUCT(F37:F38,$V37:$V38)/SUM($V37:$V38)","v":16.211547279765004},{"$f":"SUMPRODUCT(G37:G38,$V37:$V38)/SUM($V37:$V38)","v":29.393466005804683},{"$f":"SUMPRODUCT(H37:H38,$V37:$V38)/SUM($V37:$V38)","v":0},{"$f":"SUMPRODUCT(I37:I38,$V37:$V38)/SUM($V37:$V38)","v":29.393466005804683},{"$f":"SUMPRODUCT(J37:J38,$V37:$V38)/SUM($V37:$V38)","v":10.945201528537503},{"$f":"SUMPRODUCT(K37:K38,$V37:$V38)/SUM($V37:$V38)","v":0},{"$f":"SUMPRODUCT(L37:L38,$V37:$V38)/SUM($V37:$V38)","v":9.0800975650144267},{"$f":"SUMPRODUCT(M37:M38,$V37:$V38)/SUM($V37:$V38)","v":2.3759959751153916},{"$f":"SUMPRODUCT(N37:N38,$V37:$V38)/SUM($V37:$V38)","v":11.456093540129817},{"$f":"SUMPRODUCT(O37:O38,$V37:$V38)/SUM($V37:$V38)","v":1.0543175962691043},{"$f":"SUMPRODUCT(P37:P38,$V37:$V38)/SUM($V37:$V38)","v":0.50077462069965339},{"$f":"SUMPRODUCT(Q37:Q38,$V37:$V38)/SUM($V37:$V38)","v":6.8880199438526688},{"$f":"SUMPRODUCT(R37:R38,$V37:$V38)/SUM($V37:$V38)","v":0.27987951438496428},{"$f":"SUMPRODUCT(S37:S38,$V37:$V38)/SUM($V37:$V38)","v":12.473676426327273},{"$f":"SUMPRODUCT(T37:T38,$V37:$V38)/SUM($V37:$V38)","v":0},{"$f":"SUMPRODUCT(U37:U38,$V37:$V38)/SUM($V37:$V38)","v":10.896797703327726},{"$f":"SUMPRODUCT(V37:V38,$V37:$V38)/SUM($V37:$V38)","v":113.51597934628067},{"$f":"SUMPRODUCT(W37:W38,$V37:$V38)/SUM($V37:$V38)","v":0.19535079106181652}]
[null,"Office","Large",9.7720209400000009,1.8740065020000001,1.0919549449999999,15.600788830000001,5.7481246E-2,15.658270076000001,9.0415736840838523,1.2178684450889312,4.7023385901786652,0,4.7023385901786652,1.6741246447969065,0,3.7199093720667165,0.27344264041653632,0,28.373422517411417,11.164870782868572,88.563803139911599,0.13291298234934712]
[null,null,"Medium",9.7719831740000007,3.9917394229999998,1.4381270799999999,15.315534,0,15.315534,6.0392295032445746,0,1.9822574904900423,0,1.9822574904900423,2.6517312411426866E-3,0,3.0930073842022847,0.59675266894159773,0,0,11.336653317296932,53.567935772416575,0.17520952124105876]
[null,null,"Small",12.22708319,4.4231852519999997,3.1084636520000002,5.8130012109999996,0,5.8130012109999996,4.4886628680479825,0,4.4800473918575063,0,4.4800473918575063,0,0,0,0,0,0,9.097942397310069,43.638385962215558,0.16403312909760792]
["Office",null,"Weighted Average",{"$f":"SUMPRODUCT(D40:D42,$V40:$V42)/SUM($V40:$V42)","v":10.348717171713542},{"$f":"SUMPRODUCT(E40:E42,$V40:$V42)/SUM($V40:$V42)","v":3.0834831464613996},{"$f":"SUMPRODUCT(F40:F42,$V40:$V42)/SUM($V40:$V42)","v":1.6654643401089548},{"$f":"SUMPRODUCT(G40:G42,$V40:$V42)/SUM($V40:$V42)","v":13.219330742780125},{"$f":"SUMPRODUCT(H40:H42,$V40:$V42)/SUM($V40:$V42)","v":2.7403533040733952E-2},{"$f":"SUMPRODUCT(I40:I42,$V40:$V42)/SUM($V40:$V42)","v":13.246734275820859},{"$f":"SUMPRODUCT(J40:J42,$V40:$V42)/SUM($V40:$V42)","v":7.1063267764855782},{"$f":"SUMPRODUCT(K40:K42,$V40:$V42)/SUM($V40:$V42)","v":0.58060498852550635},{"$f":"SUMPRODUCT(L40:L42,$V40:$V42)/SUM($V40:$V42)","v":3.8657694224657226},{"$f":"SUMPRODUCT(M40:M42,$V40:$V42)/SUM($V40:$V42)","v":0},{"$f":"SUMPRODUCT(N40:N42,$V40:$V42)/SUM($V40:$V42)","v":3.8657694224657226},{"$f":"SUMPRODUCT(O40:O42,$V40:$V42)/SUM($V40:$V42)","v":0.79888460721283361},{"$f":"SUMPRODUCT(P40:P42,$V40:$V42)/SUM($V40:$V42)","v":0},{"$f":"SUMPRODUCT(Q40:Q42,$V40:$V42)/SUM($V40:$V42)","v":2.6653119954619569},{"$f":"SUMPRODUCT(R40:R42,$V40:$V42)/SUM($V40:$V42)","v":0.3024379127469079},{"$f":"SUMPRODUCT(S40:S42,$V40:$V42)/SUM($V40:$V42)","v":0},{"$f":"SUMPRODUCT(T40:T42,$V40:$V42)/SUM($V40:$V42)","v":13.526707848931956},{"$f":"SUMPRODUCT(U40:U42,$V40:$V42)/SUM($V40:$V42)","v":10.728872890694692},{"$f":"SUMPRODUCT(V40:V42,$V40:$V42)/SUM($V40:$V42)","v":67.91931537662991},{"$f":"SUMPRODUCT(W40:W42,$V40:$V42)/SUM($V40:$V42)","v":0.15241973165145029}]
[null,"Dining","Restaurant",31.98926148,10.00256735,72.767413770000005,185.7511389,0,185.7511389,16.414204407488189,0,37.609997855325339,0,37.609997855325339,7.7539281715739733E-2,18.340692228482578,0,0,152.90540510521441,0,0,525.85822037822618,0.21684963894285372]
[null,null,"Fast Food",28.46036192,10.37885868,75.298593990000001,249.91523380000001,0,249.91523380000001,20.617462502998801,0,45.897451019592161,0,45.897451019592161,0,40.704379360700173,0,0,269.48507596961235,0,0,740.75741724290356,0.21904769266843488]
["Restaurant",null,"Weighted Average",{"$f":"SUMPRODUCT(D44:D45,$V44:$V45)/SUM($V44:$V45)","v":29.925447923517495},{"$f":"SUMPRODUCT(E44:E45,$V44:$V45)/SUM($V44:$V45)","v":10.222634579128174},{"$f":"SUMPRODUCT(F44:F45,$V44:$V45)/SUM($V44:$V45)","v":74.247729081648146},{"$f":"SUMPRODUCT(G44:G45,$V44:$V45)/SUM($V44:$V45)","v":223.27635792154956},{"$f":"SUMPRODUCT(H44:H45,$V44:$V45)/SUM($V44:$V45)","v":0},{"$f":"SUMPRODUCT(I44:I45,$V44:$V45)/SUM($V44:$V45)","v":223.27635792154956},{"$f":"SUMPRODUCT(J44:J45,$V44:$V45)/SUM($V44:$V45)","v":18.8724044473073},{"$f":"SUMPRODUCT(K44:K45,$V44:$V45)/SUM($V44:$V45)","v":0},{"$f":"SUMPRODUCT(L44:L45,$V44:$V45)/SUM($V44:$V45)","v":42.456766061198472},{"$f":"SUMPRODUCT(M44:M45,$V44:$V45)/SUM($V44:$V45)","v":0},{"$f":"SUMPRODUCT(N44:N45,$V44:$V45)/SUM($V44:$V45)","v":42.456766061198472},{"$f":"SUMPRODUCT(O44:O45,$V44:$V45)/SUM($V44:$V45)","v":3.2191824797793436E-2},{"$f":"SUMPRODUCT(P44:P45,$V44:$V45)/SUM($V44:$V45)","v":31.419693172449371},{"$f":"SUMPRODUCT(Q44:Q45,$V44:$V45)/SUM($V44:$V45)","v":0},{"$f":"SUMPRODUCT(R44:R45,$V44:$V45)/SUM($V44:$V45)","v":0},{"$f":"SUMPRODUCT(S44:S45,$V44:$V45)/SUM($V44:$V45)","v":221.08493275949903},{"$f":"SUMPRODUCT(T44:T45,$V44:$V45)/SUM($V44:$V45)","v":0},{"$f":"SUMPRODUCT(U44:U45,$V44:$V45)/SUM($V44:$V45)","v":0},{"$f":"SUMPRODUCT(V44:V45,$V44:$V45)/SUM($V44:$V45)","v":651.53815777109537},{"$f":"SUMPRODUCT(W44:W45,$V44:$V45)/SUM($V44:$V45)","v":0.21813513120456354}]
[null,"Commercial","Retail Store",18.89221216,4.4165657249999999,3.7702331739999999,29.97799839,0,29.97799839,7.6179327636481453,0,16.027952377288187,0,16.027952377288187,0,0,0,0,0,0,7.4931493277174797,88.19604391765381,0.22481996959711098]
[null,null,"Strip Mall",26.631692269999999,6.0586520549999996,2.9781314920000002,39.269537659999997,0,39.269537659999997,7.6484214533333335,0,10.858297755555556,0,10.858297755555556,0,0,0,0,0,0,5.4236712755555549,98.868403961444429,0.18039157765982777]
["Retail",null,"Weighted Average",{"$f":"SUMPRODUCT(D47:D48,$V47:$V48)/SUM($V47:$V48)","v":22.982727779844531},{"$f":"SUMPRODUCT(E47:E48,$V47:$V48)/SUM($V47:$V48)","v":5.2844508654139313},{"$f":"SUMPRODUCT(F47:F48,$V47:$V48)/SUM($V47:$V48)","v":3.3515869268780962},{"$f":"SUMPRODUCT(G47:G48,$V47:$V48)/SUM($V47:$V48)","v":34.888817460033614},{"$f":"SUMPRODUCT(H47:H48,$V47:$V48)/SUM($V47:$V48)","v":0},{"$f":"SUMPRODUCT(I47:I48,$V47:$V48)/SUM($V47:$V48)","v":34.888817460033614},{"$f":"SUMPRODUCT(J47:J48,$V47:$V48)/SUM($V47:$V48)","v":7.6340468255248224},{"$f":"SUMPRODUCT(K47:K48,$V47:$V48)/SUM($V47:$V48)","v":0},{"$f":"SUMPRODUCT(L47:L48,$V47:$V48)/SUM($V47:$V48)","v":13.295656062956192},{"$f":"SUMPRODUCT(M47:M48,$V47:$V48)/SUM($V47:$V48)","v":0},{"$f":"SUMPRODUCT(N47:N48,$V47:$V48)/SUM($V47:$V48)","v":13.295656062956192},{"$f":"SUMPRODUCT(O47:O48,$V47:$V48)/SUM($V47:$V48)","v":0},{"$f":"SUMPRODUCT(P47:P48,$V47:$V48)/SUM($V47:$V48)","v":0},{"$f":"SUMPRODUCT(Q47:Q48,$V47:$V48)/SUM($V47:$V48)","v":0},{"$f":"SUMPRODUCT(R47:R48,$V47:$V48)/SUM($V47:$V48)","v":0},{"$f":"SUMPRODUCT(S47:S48,$V47:$V48)/SUM($V47:$V48)","v":0},{"$f":"SUMPRODUCT(T47:T48,$V47:$V48)/SUM($V47:$V48)","v":0},{"$f":"SUMPRODUCT(U47:U48,$V47:$V48)/SUM($V47:$V48)","v":6.3993765966065039},{"$f":"SUMPRODUCT(V47:V48,$V47:$V48)/SUM($V47:$V48)","v":93.836662517257693},{"$f":"SUMPRODUCT(W47:W48,$V47:$V48)/SUM($V47:$V48)","v":0.20133841416947751}]
[null,"School","Secondary",14.812607059999999,0.99270096299999999,3.075393118,18.45157283,0,18.45157283,10.662431918515603,0,8.6600369249882636,2.0405170138510198,10.700553938839283,0.7514713021665631,0.94158931181153904,0.34053881146459192,0.35670341306007486,4.0631337714826774,0,9.5406132051762249,74.689309643516566,0.22020832151119527]
[null,null,"Primary",15.51480074,1.0886792359999999,1.9867364750000001,29.49268447,0,29.49268447,8.242454205708567,0,6.3845339363701514,1.3259505498992683,7.7104844862694195,3.2174554144864045E-2,1.7380737608675083,0,0.6153723170946066,6.5470043462519074,0,14.056271833793794,87.024736425130669,0.18425374911816181]
["School",null,"Weighted Average",{"$f":"SUMPRODUCT(D50:D51,$V50:$V51)/SUM($V50:$V51)","v":15.190485305006943},{"$f":"SUMPRODUCT(E50:E51,$V50:$V51)/SUM($V50:$V51)","v":1.0443506750282219},{"$f":"SUMPRODUCT(F50:F51,$V50:$V51)/SUM($V50:$V51)","v":2.4895438382514392},{"$f":"SUMPRODUCT(G50:G51,$V50:$V51)/SUM($V50:$V51)","v":24.393232529143042},{"$f":"SUMPRODUCT(H50:H51,$V50:$V51)/SUM($V50:$V51)","v":0},{"$f":"SUMPRODUCT(I50:I51,$V50:$V51)/SUM($V50:$V51)","v":24.393232529143042},{"$f":"SUMPRODUCT(J50:J51,$V50:$V51)/SUM($V50:$V51)","v":9.3601460149007458},{"$f":"SUMPRODUCT(K50:K51,$V50:$V51)/SUM($V50:$V51)","v":0},{"$f":"SUMPRODUCT(L50:L51,$V50:$V51)/SUM($V50:$V51)","v":7.435498595553188},{"$f":"SUMPRODUCT(M50:M51,$V50:$V51)/SUM($V50:$V51)","v":1.6559804835038574},{"$f":"SUMPRODUCT(N50:N51,$V50:$V51)/SUM($V50:$V51)","v":9.0914790790570432},{"$f":"SUMPRODUCT(O50:O51,$V50:$V51)/SUM($V50:$V51)","v":0.3643892185145971},{"$f":"SUMPRODUCT(P50:P51,$V50:$V51)/SUM($V50:$V51)","v":1.3702091561037755},{"$f":"SUMPRODUCT(Q50:Q51,$V50:$V51)/SUM($V50:$V51)","v":0.15728138249856838},{"$f":"SUMPRODUCT(R50:R51,$V50:$V51)/SUM($V50:$V51)","v":0.49590340058266053},{"$f":"SUMPRODUCT(S50:S51,$V50:$V51)/SUM($V50:$V51)","v":5.3998029559991014},{"$f":"SUMPRODUCT(T50:T51,$V50:$V51)/SUM($V50:$V51)","v":0},{"$f":"SUMPRODUCT(U50:U51,$V50:$V51)/SUM($V50:$V51)","v":11.970668055046806},{"$f":"SUMPRODUCT(V50:V51,$V50:$V51)/SUM($V50:$V51)","v":81.327491610132952},{"$f":"SUMPRODUCT(W50:W51,$V50:$V51)/SUM($V50:$V51)","v":0.20085974133620049}]
["Warehouse","Warehouse",null,8.7793392059999995,2.2465679810000001,0.49037225400000001,17.450251980000001,0,17.450251980000001,0.18543794739168026,0,1.1089845026419445,0,1.1089845026419445,0,0,0,0,0,0,2.5371117206263811,32.798065591660006,0.21414833409843687]
[]
[null,"Climate Zone 6A",null,"Site EUI (kBtu/SF/yr)"]
[null,"Building Type",null,"Lighting, Interior","Lighting, Exterior","DHW","Heating","Humidfy","Heat","Cooling","Heat Rejection","Fan","Heat Recovery","Fans","Pumps","Refrigeration","Elevator","Transformers","Cooking","Data Center","Equipment","Total","Weight"]
[null,"Apartments","Mid Rise",3.400673442,2.0474847039999999,12.28237942,20.619608209999999,0,{"$f":"G57+H57","v":20.619608209999999},2.6737840597492664,0,6.254283248866364,0,{"$f":"L57+M57","v":6.254283248866364},0,0,3.6409424406179123,0,0,0,10.903869648531787,61.82302517376533,4.2799807491917412E-2]
[null,null,"High Rise",3.1704590850000001,2.3959674839999998,13.965785029999999,24.477130639999999,0,{"$f":"G58+H58","v":24.477130639999999},2.5130796957985582,0.11126783982596737,6.954914339908953,0,{"$f":"L58+M58","v":6.954914339908953},0.72987207250569042,0,1.8323394492391682,0.40648052553584979,0,0,10.950199897782836,67.507496059597031,1.3897546597388517E-2]
["Multifamily",null,"Weighted Average",{"$f":"SUMPRODUCT(D57:D58,$V57:$V58)/SUM($V57:$V58)","v":3.2805069519106431},{"$f":"SUMPRODUCT(E57:E58,$V57:$V58)/SUM($V57:$V58)","v":2.2293845345530592},{"$f":"SUMPRODUCT(F57:F58,$V57:$V58)/SUM($V57:$V58)","v":13.161077630600445},{"$f":"SUMPRODUCT(G57:G58,$V57:$V58)/SUM($V57:$V58)","v":22.633144363412299},{"$f":"SUMPRODUCT(H57:H58,$V57:$V58)/SUM($V57:$V58)","v":0},{"$f":"SUMPRODUCT(I57:I58,$V57:$V58)/SUM($V57:$V58)","v":22.633144363412299},{"$f":"SUMPRODUCT(J57:J58,$V57:$V58)/SUM($V57:$V58)","v":2.5899001542898028},{"$f":"SUMPRODUCT(K57:K58,$V57:$V58)/SUM($V57:$V58)","v":5.8079200385018681E-2},{"$f":"SUMPRODUCT(L57:L58,$V57:$V58)/SUM($V57:$V58)","v":6.6199962311286491},{"$f":"SUMPRODUCT(M57:M58,$V57:$V58)/SUM($V57:$V58)","v":0},{"$f":"SUMPRODUCT(N57:N58,$V57:$V58)/SUM($V57:$V58)","v":6.6199962311286491},{"$f":"SUMPRODUCT(O57:O58,$V57:$V58)/SUM($V57:$V58)","v":0.38097608815619277},{"$f":"SUMPRODUCT(P57:P58,$V57:$V58)/SUM($V57:$V58)","v":0},{"$f":"SUMPRODUCT(Q57:Q58,$V57:$V58)/SUM($V57:$V58)","v":2.6968941359368337},{"$f":"SUMPRODUCT(R57:R58,$V57:$V58)/SUM($V57:$V58)","v":0.21217329223007655},{"$f":"SUMPRODUCT(S57:S58,$V57:$V58)/SUM($V57:$V58)","v":0},{"$f":"SUMPRODUCT(T57:T58,$V57:$V58)/SUM($V57:$V58)","v":0},{"$f":"SUMPRODUCT(U57:U58,$V57:$V58)/SUM($V57:$V58)","v":10.928052951041733},{"$f":"SUMPRODUCT(V57:V58,$V57:$V58)/SUM($V57:$V58)","v":64.79018553364476},{"$f":"SUMPRODUCT(W57:W58,$V57:$V58)/SUM($V57:$V58)","v":2.7713505783364952E-2}]
[null,"Healthcare","Hospital",16.420497780000002,1.0251819310000001,5.3043275540000003,67.171587209999998,10.117208979999999,77.288796189999999,10.801448726920384,1.3720518349820499,17.092646548047419,0,17.092646548047419,3.6886528730729897,1.0183931615650086,9.9723134562589788,0.68128138434209373,16.988614125821439,0,21.584459558713572,183.23866512472392,6.4131899422876476E-2]
[null,null,"Clinic",14.15332733,5.2500768420000004,3.2740500529999998,54.3173119,7.6457789409999997,61.963090840999996,15.850485576124651,0,13.441585930249596,0,13.441585930249596,0.57953439188199096,0,15.096741643465389,0,0,0,32.18137152998257,161.79026413770418,7.834475565634956E-2]
["Healthcare/hospital",null,"Weighted Average",{"$f":"SUMPRODUCT(D60:D61,$V60:$V61)/SUM($V60:$V61)","v":15.357380821271866},{"$f":"SUMPRODUCT(E60:E61,$V60:$V61)/SUM($V60:$V61)","v":3.0063110643337105},{"$f":"SUMPRODUCT(F60:F61,$V60:$V61)/SUM($V60:$V61)","v":4.3522939553628621},{"$f":"SUMPRODUCT(G60:G61,$V60:$V61)/SUM($V60:$V61)","v":61.143986561702313},{"$f":"SUMPRODUCT(H60:H61,$V60:$V61)/SUM($V60:$V61)","v":8.9583110300152331},{"$f":"SUMPRODUCT(I60:I61,$V60:$V61)/SUM($V60:$V61)","v":70.102297591717544},{"$f":"SUMPRODUCT(J60:J61,$V60:$V61)/SUM($V60:$V61)","v":13.169032822607733},{"$f":"SUMPRODUCT(K60:K61,$V60:$V61)/SUM($V60:$V61)","v":0.72867207761820674},{"$f":"SUMPRODUCT(L60:L61,$V60:$V61)/SUM($V60:$V61)","v":15.380598624996336},{"$f":"SUMPRODUCT(M60:M61,$V60:$V61)/SUM($V60:$V61)","v":0},{"$f":"SUMPRODUCT(N60:N61,$V60:$V61)/SUM($V60:$V61)","v":15.380598624996336},{"$f":"SUMPRODUCT(O60:O61,$V60:$V61)/SUM($V60:$V61)","v":2.2307313550639596},{"$f":"SUMPRODUCT(P60:P61,$V60:$V61)/SUM($V60:$V61)","v":0.54085031042537635},{"$f":"SUMPRODUCT(Q60:Q61,$V60:$V61)/SUM($V60:$V61)","v":12.375249904907387},{"$f":"SUMPRODUCT(R60:R61,$V60:$V61)/SUM($V60:$V61)","v":0.36181630249972019},{"$f":"SUMPRODUCT(S60:S61,$V60:$V61)/SUM($V60:$V61)","v":9.0223477242594683},{"$f":"SUMPRODUCT(T60:T61,$V60:$V61)/SUM($V60:$V61)","v":0},{"$f":"SUMPRODUCT(U60:U61,$V60:$V61)/SUM($V60:$V61)","v":26.553541978963569},{"$f":"SUMPRODUCT(V60:V61,$V60:$V61)/SUM($V60:$V61)","v":173.1811245340277},{"$f":"SUMPRODUCT(W60:W61,$V60:$V61)/SUM($V60:$V61)","v":7.0796563076096788E-2}]
[null,"Hotel","Large",11.27571893,2.374154265,17.99038367,42.332002420000002,0,42.332002420000002,9.7963557811988196,0,11.149721528005241,3.7251134089420241,14.874834936947265,1.3799936636095644,0.79224080396331509,7.5937691377333767,0.44433994898460527,19.803352735924612,0,7.4458244095061108,136.10297070286768,4.5773999691660947E-2]
[null,null,"Small",10.92771031,2.0886789710000002,14.74401688,19.363453620000001,0,19.363453620000001,4.8130905513633628,0,6.4214040808295918,0,6.4214040808295918,5.7055740012036471E-3,0,5.6869727610347303,0,0,0,16.769679724961289,80.820712473190184,6.1948884988588998E-2]
["Hotel/motel",null,"Weighted Average",{"$f":"SUMPRODUCT(D63:D64,$V63:$V64)/SUM($V63:$V64)","v":11.146059022868588},{"$f":"SUMPRODUCT(E63:E64,$V63:$V64)/SUM($V63:$V64)","v":2.2677928188141188},{"$f":"SUMPRODUCT(F63:F64,$V63:$V64)/SUM($V63:$V64)","v":16.780863007822429},{"$f":"SUMPRODUCT(G63:G64,$V63:$V64)/SUM($V63:$V64)","v":33.774456045570183},{"$f":"SUMPRODUCT(H63:H64,$V63:$V64)/SUM($V63:$V64)","v":0},{"$f":"SUMPRODUCT(I63:I64,$V63:$V64)/SUM($V63:$V64)","v":33.774456045570183},{"$f":"SUMPRODUCT(J63:J64,$V63:$V64)/SUM($V63:$V64)","v":7.9397072105063335},{"$f":"SUMPRODUCT(K63:K64,$V63:$V64)/SUM($V63:$V64)","v":0},{"$f":"SUMPRODUCT(L63:L64,$V63:$V64)/SUM($V63:$V64)","v":9.3880605637204084},{"$f":"SUMPRODUCT(M63:M64,$V63:$V64)/SUM($V63:$V64)","v":2.3372229059498744},{"$f":"SUMPRODUCT(N63:N64,$V63:$V64)/SUM($V63:$V64)","v":11.725283469670282},{"$f":"SUMPRODUCT(O63:O64,$V63:$V64)/SUM($V63:$V64)","v":0.86796592685285145},{"$f":"SUMPRODUCT(P63:P64,$V63:$V64)/SUM($V63:$V64)","v":0.497070330692856},{"$f":"SUMPRODUCT(Q63:Q64,$V63:$V64)/SUM($V63:$V64)","v":6.8833412146512956},{"$f":"SUMPRODUCT(R63:R64,$V63:$V64)/SUM($V63:$V64)","v":0.27878923210833745},{"$f":"SUMPRODUCT(S63:S64,$V63:$V64)/SUM($V63:$V64)","v":12.425084701556392},{"$f":"SUMPRODUCT(T63:T64,$V63:$V64)/SUM($V63:$V64)","v":0},{"$f":"SUMPRODUCT(U63:U64,$V63:$V64)/SUM($V63:$V64)","v":10.91967575924753},{"$f":"SUMPRODUCT(V63:V64,$V63:$V64)/SUM($V63:$V64)","v":115.50608874036121},{"$f":"SUMPRODUCT(W63:W64,$V63:$V64)/SUM($V63:$V64)","v":5.1800385260676304E-2}]
[null,"Office","Large",9.7720209400000009,1.87412059,1.1510190979999999,18.355208059999999,7.3966934999999998E-2,18.429174995,7.743881794186783,0.78260440383643415,4.5808350642213602,0,4.5808350642213602,1.2852563164376198,0,3.7199093720667165,0.27346165511404202,0,28.373422517411417,11.164870782868572,89.15057752914295,4.0012083576556959E-2]
[null,null,"Medium",9.7719831740000007,3.9919162049999999,1.5010462449999999,18.383494469999999,0,18.383494469999999,4.2356986965764154,0,1.8615153287461774,0,1.8615153287461774,2.6517312411426866E-3,0,3.0930073842022847,0.59657588685015295,0,0,11.336653317296932,54.774542438913116,4.9349809930598232E-2]
[null,null,"Small",12.22708319,4.4214621569999997,3.1084636520000002,7.4685698260000004,0,7.4685698260000004,3.0843403198836783,0,4.1543824082151941,0,4.1543824082151941,0,0,0,0,0,0,9.097942397310069,43.562243950408941,4.3007828377301729E-2]
["Office",null,"Weighted Average",{"$f":"SUMPRODUCT(D66:D68,$V66:$V68)/SUM($V66:$V68)","v":10.342437792620954},{"$f":"SUMPRODUCT(E66:E68,$V66:$V68)/SUM($V66:$V68)","v":3.0847045771754642},{"$f":"SUMPRODUCT(F66:F68,$V66:$V68)/SUM($V66:$V68)","v":1.7080873281783875},{"$f":"SUMPRODUCT(G66:G68,$V66:$V68)/SUM($V66:$V68)","v":15.8339874000843},{"$f":"SUMPRODUCT(H66:H68,$V66:$V68)/SUM($V66:$V68)","v":3.5171410144623279E-2},{"$f":"SUMPRODUCT(I66:I68,$V66:$V68)/SUM($V66:$V68)","v":15.869158810228923},{"$f":"SUMPRODUCT(J66:J68,$V66:$V68)/SUM($V66:$V68)","v":5.6363306605753687},{"$f":"SUMPRODUCT(K66:K68,$V66:$V68)/SUM($V66:$V68)","v":0.3721297964870332},{"$f":"SUMPRODUCT(L66:L68,$V66:$V68)/SUM($V66:$V68)","v":3.6872989592342833},{"$f":"SUMPRODUCT(M66:M68,$V66:$V68)/SUM($V66:$V68)","v":0},{"$f":"SUMPRODUCT(N66:N68,$V66:$V68)/SUM($V66:$V68)","v":3.6872989592342833},{"$f":"SUMPRODUCT(O66:O68,$V66:$V68)/SUM($V66:$V68)","v":0.6119163865288002},{"$f":"SUMPRODUCT(P66:P68,$V66:$V68)/SUM($V66:$V68)","v":0},{"$f":"SUMPRODUCT(Q66:Q68,$V66:$V68)/SUM($V66:$V68)","v":2.6724474793062694},{"$f":"SUMPRODUCT(R66:R68,$V66:$V68)/SUM($V66:$V68)","v":0.30432149946175002},{"$f":"SUMPRODUCT(S66:S68,$V66:$V68)/SUM($V66:$V68)","v":0},{"$f":"SUMPRODUCT(T66:T68,$V66:$V68)/SUM($V66:$V68)","v":13.491613253497208},{"$f":"SUMPRODUCT(U66:U68,$V66:$V68)/SUM($V66:$V68)","v":10.734811246309729},{"$f":"SUMPRODUCT(V66:V68,$V66:$V68)/SUM($V66:$V68)","v":68.515257789604163},{"$f":"SUMPRODUCT(W66:W68,$V66:$V68)/SUM($V66:$V68)","v":4.343615995625786E-2}]
[null,"Dining","Restaurant",31.98926148,9.9956749699999996,75.945754039999997,216.9212642,0,216.9212642,9.1961588204289342,0,35.714593184296618,0,35.714593184296618,7.7539281715739733E-2,18.285553184498575,0,0,152.90540510521441,0,0,551.03120426615419,4.7010740075510475E-2]
[null,null,"Fast Food",28.46036192,10.375068000000001,79.262675189999996,297.71917289999999,0,297.71917289999999,11.353061259496201,0,42.739821591363452,0,42.739821591363452,0,40.571705854102817,0,0,269.48507596961235,0,0,779.96694268457486,4.3242658256224711E-2]
["Restaurant",null,"Weighted Average",{"$f":"SUMPRODUCT(D70:D71,$V70:$V71)/SUM($V70:$V71)","v":29.921320959451677},{"$f":"SUMPRODUCT(E70:E71,$V70:$V71)/SUM($V70:$V71)","v":10.217999863812112},{"$f":"SUMPRODUCT(F70:F71,$V70:$V71)/SUM($V70:$V71)","v":77.889474889212465},{"$f":"SUMPRODUCT(G70:G71,$V70:$V71)/SUM($V70:$V71)","v":264.26896184212097},{"$f":"SUMPRODUCT(H70:H71,$V70:$V71)/SUM($V70:$V71)","v":0},{"$f":"SUMPRODUCT(I70:I71,$V70:$V71)/SUM($V70:$V71)","v":264.26896184212097},{"$f":"SUMPRODUCT(J70:J71,$V70:$V71)/SUM($V70:$V71)","v":10.460106937052776},{"$f":"SUMPRODUCT(K70:K71,$V70:$V71)/SUM($V70:$V71)","v":0},{"$f":"SUMPRODUCT(L70:L71,$V70:$V71)/SUM($V70:$V71)","v":39.831387737973472},{"$f":"SUMPRODUCT(M70:M71,$V70:$V71)/SUM($V70:$V71)","v":0},{"$f":"SUMPRODUCT(N70:N71,$V70:$V71)/SUM($V70:$V71)","v":39.831387737973472},{"$f":"SUMPRODUCT(O70:O71,$V70:$V71)/SUM($V70:$V71)","v":3.2101144452861739E-2},{"$f":"SUMPRODUCT(P70:P71,$V70:$V71)/SUM($V70:$V71)","v":31.345272615164589},{"$f":"SUMPRODUCT(Q70:Q71,$V70:$V71)/SUM($V70:$V71)","v":0},{"$f":"SUMPRODUCT(R70:R71,$V70:$V71)/SUM($V70:$V71)","v":0},{"$f":"SUMPRODUCT(S70:S71,$V70:$V71)/SUM($V70:$V71)","v":221.22126991058025},{"$f":"SUMPRODUCT(T70:T71,$V70:$V71)/SUM($V70:$V71)","v":0},{"$f":"SUMPRODUCT(U70:U71,$V70:$V71)/SUM($V70:$V71)","v":0},{"$f":"SUMPRODUCT(V70:V71,$V70:$V71)/SUM($V70:$V71)","v":685.18789589982123},{"$f":"SUMPRODUCT(W70:W71,$V70:$V71)/SUM($V70:$V71)","v":4.4802638386483525E-2}]
[null,"Commercial","Retail Store",18.89221216,4.4138780820000001,3.8385595330000002,35.596497980000002,0,35.596497980000002,4.9863460918516118,0,15.96844027620282,0,15.96844027620282,0,0,0,0,0,0,7.4931493277174797,91.189083450771903,6.2161938286217848E-2]
[null,null,"Strip Mall",26.631692269999999,6.0552812210000004,3.0215309750000001,47.633918430000001,0,47.633918430000001,4.6715540266666666,0,10.897905053333332,0,10.897905053333332,0,0,0,0,0,0,5.4236712755555549,104.33555325155554,2.6924529896460325E-2]
["Retail",null,"Weighted Average",{"$f":"SUMPRODUCT(D73:D74,$V73:$V74)/SUM($V73:$V74)","v":23.022141527344264},{"$f":"SUMPRODUCT(E73:E74,$V73:$V74)/SUM($V73:$V74)","v":5.2897610781521998},{"$f":"SUMPRODUCT(F73:F74,$V73:$V74)/SUM($V73:$V74)","v":3.4025780216213075},{"$f":"SUMPRODUCT(G73:G74,$V73:$V74)/SUM($V73:$V74)","v":42.019887602681699},{"$f":"SUMPRODUCT(H73:H74,$V73:$V74)/SUM($V73:$V74)","v":0},{"$f":"SUMPRODUCT(I73:I74,$V73:$V74)/SUM($V73:$V74)","v":42.019887602681699},{"$f":"SUMPRODUCT(J73:J74,$V73:$V74)/SUM($V73:$V74)","v":4.8183672384743081},{"$f":"SUMPRODUCT(K73:K74,$V73:$V74)/SUM($V73:$V74)","v":0},{"$f":"SUMPRODUCT(L73:L74,$V73:$V74)/SUM($V73:$V74)","v":13.262709138264386},{"$f":"SUMPRODUCT(M73:M74,$V73:$V74)/SUM($V73:$V74)","v":0},{"$f":"SUMPRODUCT(N73:N74,$V73:$V74)/SUM($V73:$V74)","v":13.262709138264386},{"$f":"SUMPRODUCT(O73:O74,$V73:$V74)/SUM($V73:$V74)","v":0},{"$f":"SUMPRODUCT(P73:P74,$V73:$V74)/SUM($V73:$V74)","v":0},{"$f":"SUMPRODUCT(Q73:Q74,$V73:$V74)/SUM($V73:$V74)","v":0},{"$f":"SUMPRODUCT(R73:R74,$V73:$V74)/SUM($V73:$V74)","v":0},{"$f":"SUMPRODUCT(S73:S74,$V73:$V74)/SUM($V73:$V74)","v":0},{"$f":"SUMPRODUCT(T73:T74,$V73:$V74)/SUM($V73:$V74)","v":0},{"$f":"SUMPRODUCT(U73:U74,$V73:$V74)/SUM($V73:$V74)","v":6.3888376606256791},{"$f":"SUMPRODUCT(V73:V74,$V73:$V74)/SUM($V73:$V74)","v":98.204282267163833},{"$f":"SUMPRODUCT(W73:W74,$V73:$V74)/SUM($V73:$V74)","v":4.3358607097352939E-2}]
[null,"School","Secondary",14.812607059999999,0.99211654500000002,3.192473052,22.035971629999999,0,22.035971629999999,7.2558159630513028,0,8.5223840682450795,2.0334590458397153,10.555843114084794,0.53600097730063967,0.93821767060084327,0.34053881146459192,0.35674836827305617,4.0631337714826774,0,9.5406132051762249,74.620080168434129,4.0078616184763494E-2]
[null,null,"Primary",15.51480074,1.0880383090000001,2.0608097490000001,34.61245272,0,34.61245272,5.8775603834556982,0,6.3601786963047093,1.2937759957544044,7.6539546920591137,3.6148303857542689E-2,1.7332027127192098,0,0.6155005025757514,6.5470043462519074,0,14.056271833793794,89.795744292713039,3.3655279363060737E-2]
["School",null,"Weighted Average",{"$f":"SUMPRODUCT(D76:D77,$V76:$V77)/SUM($V76:$V77)","v":15.196110316696192},{"$f":"SUMPRODUCT(E76:E77,$V76:$V77)/SUM($V76:$V77)","v":1.0445042407736838},{"$f":"SUMPRODUCT(F76:F77,$V76:$V77)/SUM($V76:$V77)","v":2.5744148516127963},{"$f":"SUMPRODUCT(G76:G77,$V76:$V77)/SUM($V76:$V77)","v":28.904619971855002},{"$f":"SUMPRODUCT(H76:H77,$V76:$V77)/SUM($V76:$V77)","v":0},{"$f":"SUMPRODUCT(I76:I77,$V76:$V77)/SUM($V76:$V77)","v":28.904619971855002},{"$f":"SUMPRODUCT(J76:J77,$V76:$V77)/SUM($V76:$V77)","v":6.5030813281645141},{"$f":"SUMPRODUCT(K76:K77,$V76:$V77)/SUM($V76:$V77)","v":0},{"$f":"SUMPRODUCT(L76:L77,$V76:$V77)/SUM($V76:$V77)","v":7.3414950551381404},{"$f":"SUMPRODUCT(M76:M77,$V76:$V77)/SUM($V76:$V77)","v":1.6294809601487585},{"$f":"SUMPRODUCT(N76:N77,$V76:$V77)/SUM($V76:$V77)","v":8.9709760152868974},{"$f":"SUMPRODUCT(O76:O77,$V76:$V77)/SUM($V76:$V77)","v":0.2630063127321331},{"$f":"SUMPRODUCT(P76:P77,$V76:$V77)/SUM($V76:$V77)","v":1.3723989532879104},{"$f":"SUMPRODUCT(Q76:Q77,$V76:$V77)/SUM($V76:$V77)","v":0.1545534530829541},{"$f":"SUMPRODUCT(R76:R77,$V76:$V77)/SUM($V76:$V77)","v":0.49806591214809326},{"$f":"SUMPRODUCT(S76:S77,$V76:$V77)/SUM($V76:$V77)","v":5.4197003168207649},{"$f":"SUMPRODUCT(T76:T77,$V76:$V77)/SUM($V76:$V77)","v":0},{"$f":"SUMPRODUCT(U76:U77,$V76:$V77)/SUM($V76:$V77)","v":12.006841312217992},{"$f":"SUMPRODUCT(V76:V77,$V76:$V77)/SUM($V76:$V77)","v":82.908272984678931},{"$f":"SUMPRODUCT(W76:W77,$V76:$V77)/SUM($V76:$V77)","v":3.6570509147998982E-2}]
["Warehouse","Warehouse",null,8.7793392059999995,2.2467501410000001,0.50093748100000002,19.90115462,0,19.90115462,5.064022532423864E-2,0,0.94194462273032953,0,0.94194462273032953,0,0,0,0,0,0,2.5371117206263811,34.957878016680951,2.7870410498406498E-2]

{"sheet":"90.1-2013 Site EUI","index":35,"n_rows":79,"n_cols":23,"rows_kept":79,"cut":false,"hidden":true,"merged":[[78,1,78,2],[2,1,2,2],[2,3,2,22],[3,1,3,2],[26,1,26,2],[28,1,28,2],[28,3,28,22],[29,1,29,2],[52,1,52,2],[54,1,54,2],[54,3,54,22],[55,1,55,2]]}
[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23]
[]
[null,"Climate Zone 4A",null,"Site EUI (kBtu/SF/yr)"]
[null,"Building Type",null,"Lighting, Interior","Lighting, Exterior","DHW","Heating","Humidfy","Heat","Cooling","Heat Rejection","Fan","Heat Recovery","Fans","Pumps","Refrigeration","Elevator","Transformers","Cooking","Data Center","Equipment","Total","Weight"]
[null,"Apartments","Mid Rise",3.1104234489999998,1.127282645,11.063217059999999,5.7990980189999997,0,{"$f":"G5+H5","v":5.7990980189999997},3.5633595477312467,0,5.7221114311964678,0,{"$f":"L5+M5","v":5.7221114311964678},0,0,3.5111295522427404,0,0,0,10.849361147499414,44.745982851669865,0.23138567210488928]
[null,null,"High Rise",3.0074910359999998,1.830636945,12.42582941,6.1439815869999999,0,{"$f":"G6+H6","v":6.1439815869999999},4.5972724452295148,0.22545786537367224,6.4373502963770859,0,{"$f":"L6+M6","v":6.4373502963770859},0.59241695324355093,0,1.7804139861005743,0.23384678608687406,0,0,10.928396368129318,48.20309367854059,0.27946667242036716]
["Multifamily",null,"Weighted Average",{"$f":"SUMPRODUCT(D5:D6,$V5:$V6)/SUM($V5:$V6)","v":3.0570430289720014},{"$f":"SUMPRODUCT(E5:E6,$V5:$V6)/SUM($V5:$V6)","v":1.4920399344506905},{"$f":"SUMPRODUCT(F5:F6,$V5:$V6)/SUM($V5:$V6)","v":11.769863464746564},{"$f":"SUMPRODUCT(G5:G6,$V5:$V6)/SUM($V5:$V6)","v":5.9779535338376331},{"$f":"SUMPRODUCT(H5:H6,$V5:$V6)/SUM($V5:$V6)","v":0},{"$f":"SUMPRODUCT(I5:I6,$V5:$V6)/SUM($V5:$V6)","v":5.9779535338376331},{"$f":"SUMPRODUCT(J5:J6,$V5:$V6)/SUM($V5:$V6)","v":4.0995434681531133},{"$f":"SUMPRODUCT(K5:K6,$V5:$V6)/SUM($V5:$V6)","v":0.1169217275831531},{"$f":"SUMPRODUCT(L5:L6,$V5:$V6)/SUM($V5:$V6)","v":6.093032018122674},{"$f":"SUMPRODUCT(M5:M6,$V5:$V6)/SUM($V5:$V6)","v":0},{"$f":"SUMPRODUCT(N5:N6,$V5:$V6)/SUM($V5:$V6)","v":6.093032018122674},{"$f":"SUMPRODUCT(O5:O6,$V5:$V6)/SUM($V5:$V6)","v":0.30722553639005834},0,2.6135859974281423,0.12127219502291178,0,0,10.89034856002835,46.538829464735294,0.25632032502327123]
[null,"Healthcare","Hospital",13.77987409,0.80746571499999997,4.8175457670000004,27.417104420000001,3.2917310080000002,30.708835428,9.3590886083287437,1.8516085063829966,11.346171088318474,0.97862379327621829,12.324794881594693,2.129818896816162,0.81370947743947719,9.8430027453302475,0.40479827710858335,16.988614125821439,0,20.900455956244016,124.72961247506636,0.17848792406481528]
[null,null,"Clinic",11.655980960000001,2.5735216799999998,2.9212748629999998,20.123237499999998,2.9370330650000001,23.060270565,18.050771364724273,0,8.7858617789283446,0.52188194939676646,9.3077437283251108,0.35332380427880622,0,14.801530674546976,0,0,0,31.916034044839535,114.64045168471472,0.18710373737855782]
["Healthcare/hospital",null,"Weighted Average",{"$f":"SUMPRODUCT(D8:D9,$V8:$V9)/SUM($V8:$V9)","v":12.762687297625098},{"$f":"SUMPRODUCT(E8:E9,$V8:$V9)/SUM($V8:$V9)","v":1.6532751282979818},{"$f":"SUMPRODUCT(F8:F9,$V8:$V9)/SUM($V8:$V9)","v":3.9093730858662661},{"$f":"SUMPRODUCT(G8:G9,$V8:$V9)/SUM($V8:$V9)","v":23.923884826430236},{"$f":"SUMPRODUCT(H8:H9,$V8:$V9)/SUM($V8:$V9)","v":3.1218570827040759},{"$f":"SUMPRODUCT(I8:I9,$V8:$V9)/SUM($V8:$V9)","v":27.045741909134314},{"$f":"SUMPRODUCT(J8:J9,$V8:$V9)/SUM($V8:$V9)","v":13.521757990529828},{"$f":"SUMPRODUCT(K8:K9,$V8:$V9)/SUM($V8:$V9)","v":0.9648257908412754},{"$f":"SUMPRODUCT(L8:L9,$V8:$V9)/SUM($V8:$V9)","v":10.11997341522456},{"$f":"SUMPRODUCT(M8:M9,$V8:$V9)/SUM($V8:$V9)","v":0.75987843148904666},{"$f":"SUMPRODUCT(N8:N9,$V8:$V9)/SUM($V8:$V9)","v":10.879851846713606},{"$f":"SUMPRODUCT(O8:O9,$V8:$V9)/SUM($V8:$V9)","v":1.2790099180951706},0.42400317744230148,12.217768710706922,0.21093001922172483,8.8523319064146264,0,26.176098305580936,119.89765508647007,0.18261425762864519]
[null,"Hotel","Large",7.0987849120000002,1.8233523389999999,16.963551500000001,9.6595541520000001,0,9.6595541520000001,10.527730691123484,0,5.009463946937438,1.5263307500818866,6.535794697019325,0.56865737995414345,0.6590231514175493,7.378572106125123,0.24179699959056669,19.803352735924612,0,6.7716650243840091,88.03183568853882,0.19357586285323519]
[null,null,"Small",7.000519841,1.444388,13.121832769999999,4.9946340380000001,0,4.9946340380000001,5.6314015277070508,0,6.0711696148326473,0,6.0711696148326473,5.7055740012036471E-3,0,5.4842035991132141,0,0,0,16.000745745824521,59.754600710478641,0.18280635362367731]
["Hotel/motel",null,"Weighted Average",{"$f":"SUMPRODUCT(D11:D12,$V11:$V12)/SUM($V11:$V12)","v":7.0590533221162142},{"$f":"SUMPRODUCT(E11:E12,$V11:$V12)/SUM($V11:$V12)","v":1.670125403482621},{"$f":"SUMPRODUCT(F11:F12,$V11:$V12)/SUM($V11:$V12)","v":15.410226483532906},{"$f":"SUMPRODUCT(G11:G12,$V11:$V12)/SUM($V11:$V12)","v":7.7733835023083353},{"$f":"SUMPRODUCT(H11:H12,$V11:$V12)/SUM($V11:$V12)","v":0},{"$f":"SUMPRODUCT(I11:I12,$V11:$V12)/SUM($V11:$V12)","v":7.7733835023083353},{"$f":"SUMPRODUCT(J11:J12,$V11:$V12)/SUM($V11:$V12)","v":8.547994246859604},{"$f":"SUMPRODUCT(K11:K12,$V11:$V12)/SUM($V11:$V12)","v":0},{"$f":"SUMPRODUCT(L11:L12,$V11:$V12)/SUM($V11:$V12)","v":5.4387441962144409},{"$f":"SUMPRODUCT(M11:M12,$V11:$V12)/SUM($V11:$V12)","v":0.90918829272525947},{"$f":"SUMPRODUCT(N11:N12,$V11:$V12)/SUM($V11:$V12)","v":6.3479324889397004},{"$f":"SUMPRODUCT(O11:O12,$V11:$V12)/SUM($V11:$V12)","v":0.3410386538814954},0.39255982615274992,6.6126206663774703,0.14403103733056768,11.796248266141163,0,10.503266156882257,76.598480054005094,0.18922141910629656]
[null,"Office","Large",6.4755104760000002,1.2960376149999999,1.0231006279999999,5.7495469339999996,5.3336055E-2,5.8028829889999995,8.1713498359366845,0.68696078285077056,4.1399807195520149,0.20946523422144137,4.349445953773456,0.95702566327308325,0,3.6145112437523568,0.1518060115365793,0,28.373422517411417,10.143822843487758,71.045876560022094,0.34018675031287815]
[null,null,"Medium",5.7851936500000001,1.8542672630000001,1.348166814,4.5513610340000001,0,4.5513610340000001,4.9981598176325797,0,1.4462542170135004,0,1.4462542170135004,2.6517312411426866E-3,0,2.9238253959374476,0.30152659114641606,0,0,10.336068265955594,33.547474779926688,0.1967408890034183]
[null,null,"Small",7.7918362720000003,2.11768394,3.1032943670000002,1.199210313,0,1.199210313,2.7414443856779354,0,3.2635422155579787,0,3.2635422155579787,0,0,0,0,0,0,8.320826483097056,28.537837976332973,0.16685138805183178]
["Office",null,"Weighted Average",{"$f":"SUMPRODUCT(D14:D16,$V14:$V16)/SUM($V14:$V16)","v":6.5837248324848296},{"$f":"SUMPRODUCT(E14:E16,$V14:$V16)/SUM($V14:$V16)","v":1.6128319360827217},{"$f":"SUMPRODUCT(F14:F16,$V14:$V16)/SUM($V14:$V16)","v":1.5509212079894585},{"$f":"SUMPRODUCT(G14:G16,$V14:$V16)/SUM($V14:$V16)","v":4.472213790931705},{"$f":"SUMPRODUCT(H14:H16,$V14:$V16)/SUM($V14:$V16)","v":2.8462952965335839E-2},{"$f":"SUMPRODUCT(I14:I16,$V14:$V16)/SUM($V14:$V16)","v":4.5006767438970412},{"$f":"SUMPRODUCT(J14:J16,$V14:$V16)/SUM($V14:$V16)","v":6.2077958752173279},{"$f":"SUMPRODUCT(K14:K16,$V14:$V16)/SUM($V14:$V16)","v":0.36659877546833508},{"$f":"SUMPRODUCT(L14:L16,$V14:$V16)/SUM($V14:$V16)","v":3.2733214301421985},{"$f":"SUMPRODUCT(M14:M16,$V14:$V16)/SUM($V14:$V16)","v":0.11178177893955489},{"$f":"SUMPRODUCT(N14:N16,$V14:$V16)/SUM($V14:$V16)","v":3.3851032090817537},{"$f":"SUMPRODUCT(O14:O16,$V14:$V16)/SUM($V14:$V16)","v":0.51138795029364181},0,2.6656644487450758,0.15699286527820899,0,15.141565880316458,9.801491143932326,52.484754868787178,0.26688414595354643]
[null,"Dining","Restaurant",12.25120652,5.7017218539999996,68.831006459999998,92.568071509999996,0,92.568071509999996,13.965686197746274,0,16.539990354416577,0,16.539990354416577,7.7539281715739733E-2,14.308632797164671,0,0,152.90540510521441,0,0,377.14926008025765,0.192721124592207]
[null,null,"Fast Food",12.22112504,5.8452155140000004,70.860793720000004,154.5347409,0,154.5347409,17.751714818072774,0,22.581030359856058,0,22.581030359856058,0,32.114680739704127,0,0,269.48507596961235,0,0,585.39437706124534,0.15169200879179751]
["Restaurant",null,"Weighted Average",{"$f":"SUMPRODUCT(D18:D19,$V18:$V19)/SUM($V18:$V19)","v":12.232911734635278},{"$f":"SUMPRODUCT(E18:E19,$V18:$V19)/SUM($V18:$V19)","v":5.7889910213048683},{"$f":"SUMPRODUCT(F18:F19,$V18:$V19)/SUM($V18:$V19)","v":70.065471062730396},{"$f":"SUMPRODUCT(G18:G19,$V18:$V19)/SUM($V18:$V19)","v":130.25461207438008},{"$f":"SUMPRODUCT(H18:H19,$V18:$V19)/SUM($V18:$V19)","v":0},{"$f":"SUMPRODUCT(I18:I19,$V18:$V19)/SUM($V18:$V19)","v":130.25461207438008},{"$f":"SUMPRODUCT(J18:J19,$V18:$V19)/SUM($V18:$V19)","v":16.26825179603328},{"$f":"SUMPRODUCT(K18:K19,$V18:$V19)/SUM($V18:$V19)","v":0},{"$f":"SUMPRODUCT(L18:L19,$V18:$V19)/SUM($V18:$V19)","v":20.213996097458459},{"$f":"SUMPRODUCT(M18:M19,$V18:$V19)/SUM($V18:$V19)","v":0},{"$f":"SUMPRODUCT(N18:N19,$V18:$V19)/SUM($V18:$V19)","v":20.213996097458459},{"$f":"SUMPRODUCT(O18:O19,$V18:$V19)/SUM($V18:$V19)","v":3.0381877348534963E-2},25.137814915287372,0,0,223.80617382915389,0,0,503.7986044083321,0.16776826764259162]
[null,"Commercial","Retail Store",14.221472179999999,2.3543754699999999,3.6124683769999999,3.9809700920000002,0,3.9809700920000002,5.1495244289648463,0,6.6403985258383278,0.78671156852421831,7.4271100943625461,0,0,0,0,0,0,7.4601297100275392,44.206050352354929,0.16686701421318281]
[null,null,"Strip Mall",20.43483604,2.9895080549999999,2.68402626,13.549572299999999,0,13.549572299999999,4.8620061244444441,0,6.1513499777777776,0,6.1513499777777776,0,0,0,0,0,0,5.3996540844444443,56.07095284166666,0.17783967651747074]
["Retail",null,"Weighted Average",{"$f":"SUMPRODUCT(D21:D22,$V21:$V22)/SUM($V21:$V22)","v":17.695740665149014},{"$f":"SUMPRODUCT(E21:E22,$V21:$V22)/SUM($V21:$V22)","v":2.7095166099165549},{"$f":"SUMPRODUCT(F21:F22,$V21:$V22)/SUM($V21:$V22)","v":3.0933200927438564},{"$f":"SUMPRODUCT(G21:G22,$V21:$V22)/SUM($V21:$V22)","v":9.3313557843939492},{"$f":"SUMPRODUCT(H21:H22,$V21:$V22)/SUM($V21:$V22)","v":0},{"$f":"SUMPRODUCT(I21:I22,$V21:$V22)/SUM($V21:$V22)","v":9.3313557843939492},{"$f":"SUMPRODUCT(J21:J22,$V21:$V22)/SUM($V21:$V22)","v":4.9887555110636326},{"$f":"SUMPRODUCT(K21:K22,$V21:$V22)/SUM($V21:$V22)","v":0},{"$f":"SUMPRODUCT(L21:L22,$V21:$V22)/SUM($V21:$V22)","v":6.3669418288673167},{"$f":"SUMPRODUCT(M21:M22,$V21:$V22)/SUM($V21:$V22)","v":0.34681342783721231},{"$f":"SUMPRODUCT(N21:N22,$V21:$V22)/SUM($V21:$V22)","v":6.7137552567045296},{"$f":"SUMPRODUCT(O21:O22,$V21:$V22)/SUM($V21:$V22)","v":0},0,0,0,0,0,6.3079928495957018,50.840436769567233,0.17300249504143261]
[null,"School","Secondary",8.3244013219999999,0.51878313200000004,2.9313913779999998,2.1259109189999998,0,2.1259109189999998,6.7798301934211205,0,3.8114825845120848,1.3173225395591006,5.1288051240711852,0.20342232845078168,0.8631424687154734,0.29580797088277422,0.18389558313219875,4.0631337714826774,0,8.5700306124975771,39.988554803653784,0.19428622027148637]
[null,null,"Primary",8.8814587970000005,0.58734584499999998,1.863829725,11.82531902,0,11.82531902,6.2358387863546021,0,4.3789440000540845,1.2986470437674928,5.6775910438215771,1.6279555280628459E-2,1.5696380471612656,0,0.31016270190240541,6.5470043462519074,0,11.983640889622023,55.498108757394412,0.17919046104370323]
["School",null,"Weighted Average",{"$f":"SUMPRODUCT(D24:D25,$V24:$V25)/SUM($V24:$V25)","v":8.6481704765469498},{"$f":"SUMPRODUCT(E24:E25,$V24:$V25)/SUM($V24:$V25)","v":0.55863268544411293},{"$f":"SUMPRODUCT(F24:F25,$V24:$V25)/SUM($V24:$V25)","v":2.310910459368483},{"$f":"SUMPRODUCT(G24:G25,$V24:$V25)/SUM($V24:$V25)","v":7.7633348858296269},{"$f":"SUMPRODUCT(H24:H25,$V24:$V25)/SUM($V24:$V25)","v":0},{"$f":"SUMPRODUCT(I24:I25,$V24:$V25)/SUM($V24:$V25)","v":7.7633348858296269},{"$f":"SUMPRODUCT(J24:J25,$V24:$V25)/SUM($V24:$V25)","v":6.463655209956924},{"$f":"SUMPRODUCT(K24:K25,$V24:$V25)/SUM($V24:$V25)","v":0},{"$f":"SUMPRODUCT(L24:L25,$V24:$V25)/SUM($V24:$V25)","v":4.1412986465765025},{"$f":"SUMPRODUCT(M24:M25,$V24:$V25)/SUM($V24:$V25)","v":1.3064680949917891},{"$f":"SUMPRODUCT(N24:N25,$V24:$V25)/SUM($V24:$V25)","v":5.4477667415682918},{"$f":"SUMPRODUCT(O24:O25,$V24:$V25)/SUM($V24:$V25)","v":9.4652479434983214E-2},1.2737670207413692,0.12388047517694195,0.25728369858888295,5.5067921228890153,0,10.554065946333385,49.002912201878964,0.18551236582778888]
["Warehouse","Warehouse",null,5.6305372829999998,1.5046340330000001,0.46341270899999998,7.4089814379999996,0,7.4089814379999996,0.12040715444327024,0,0.40111430262273029,0,0.40111430262273029,0,0,0,0,0,0,2.4864714958209242,18.015558415886925,0.14631429773497143]
[]
[null,"Climate Zone 5A",null,"Site EUI (kBtu/SF/yr)"]
[null,"Building Type",null,"Lighting, Interior","Lighting, Exterior","DHW","Heating","Humidfy","Heat","Cooling","Heat Rejection","Fan","Heat Recovery","Fans","Pumps","Refrigeration","Elevator","Transformers","Cooking","Data Center","Equipment","Total","Weight"]
[null,"Apartments","Mid Rise",3.1104234489999998,1.125877756,11.70384628,10.859403759999999,0,{"$f":"G31+H31","v":10.859403759999999},2.8325364758009544,0,5.7628532023354371,0,{"$f":"L31+M31","v":5.7628532023354371},0,0,3.5111295522427404,0,0,0,10.849361147499414,49.755431622878547,0.15323697055373742]
[null,null,"High Rise",3.0074910359999998,1.828389109,13.23530334,12.214998250000001,0,{"$f":"G32+H32","v":12.214998250000001},3.5634930600341432,0.17229656404116084,6.5013012068474971,0,{"$f":"L32+M32","v":6.5013012068474971},0.60084633511949925,0,1.7804139861005743,0.23373439432378607,0,0,10.928396368129318,54.066663649595974,0.12973302267845771]
["Multifamily",null,"Weighted Average",{"$f":"SUMPRODUCT(D31:D32,$V31:$V32)/SUM($V31:$V32)","v":3.0568200985984624},{"$f":"SUMPRODUCT(E31:E32,$V31:$V32)/SUM($V31:$V32)","v":1.4917193905094084},{"$f":"SUMPRODUCT(F31:F32,$V31:$V32)/SUM($V31:$V32)","v":12.501371831179773},{"$f":"SUMPRODUCT(G31:G32,$V31:$V32)/SUM($V31:$V32)","v":11.565346663037396},{"$f":"SUMPRODUCT(H31:H32,$V31:$V32)/SUM($V31:$V32)","v":0},{"$f":"SUMPRODUCT(I31:I32,$V31:$V32)/SUM($V31:$V32)","v":11.565346663037396},{"$f":"SUMPRODUCT(J31:J32,$V31:$V32)/SUM($V31:$V32)","v":3.2131913227145583},{"$f":"SUMPRODUCT(K31:K32,$V31:$V32)/SUM($V31:$V32)","v":8.9725605629000019E-2},{"$f":"SUMPRODUCT(L31:L32,$V31:$V32)/SUM($V31:$V32)","v":6.1474093007062818},{"$f":"SUMPRODUCT(M31:M32,$V31:$V32)/SUM($V31:$V32)","v":0},{"$f":"SUMPRODUCT(N31:N32,$V31:$V32)/SUM($V31:$V32)","v":6.1474093007062818},{"$f":"SUMPRODUCT(O31:O32,$V31:$V32)/SUM($V31:$V32)","v":0.31289829607793584},0,2.6098376245259143,0.12172012949729576,0,0,10.890519734012758,52.000559996488789,0.14099699368874252]
[null,"Healthcare","Hospital",13.78077699,0.80648430400000004,5.0694717770000004,31.425463019999999,3.4642630620000001,34.889726081999996,8.4423722220611932,1.450250663558329,11.492283559902443,0.93292929677309822,12.425212856675541,2.029283153692945,0.80271767409290706,9.8430027453302475,0.40479827710858335,16.988614125821439,0,20.900455956244016,127.83316682758522,0.23550813259375961]
[null,null,"Clinic",11.657833249999999,2.5813939010000002,3.0900236250000002,24.846139279999999,3.3781089799999999,28.22424826,15.091510850876764,0,8.5978546182777311,0.54573014848825274,9.1435847667659846,0.44223359497875253,0,14.801530674546976,0,0,0,31.916034044839535,116.94839296800802,0.24213976109604499]
["Healthcare/hospital",null,"Weighted Average",{"$f":"SUMPRODUCT(D34:D35,$V34:$V35)/SUM($V34:$V35)","v":12.76650590290579},{"$f":"SUMPRODUCT(E34:E35,$V34:$V35)/SUM($V34:$V35)","v":1.6544763880686697},{"$f":"SUMPRODUCT(F34:F35,$V34:$V35)/SUM($V34:$V35)","v":4.1237580535757212},{"$f":"SUMPRODUCT(G34:G35,$V34:$V35)/SUM($V34:$V35)","v":28.282083515221156},{"$f":"SUMPRODUCT(H34:H35,$V34:$V35)/SUM($V34:$V35)","v":3.4231015404950806},{"$f":"SUMPRODUCT(I34:I35,$V34:$V35)/SUM($V34:$V35)","v":31.705185055716235},{"$f":"SUMPRODUCT(J34:J35,$V34:$V35)/SUM($V34:$V35)","v":11.619106931615423},{"$f":"SUMPRODUCT(K34:K35,$V34:$V35)/SUM($V34:$V35)","v":0.75736969390700637},{"$f":"SUMPRODUCT(L34:L35,$V34:$V35)/SUM($V34:$V35)","v":10.109422802066891},{"$f":"SUMPRODUCT(M34:M35,$V34:$V35)/SUM($V34:$V35)","v":0.74793857202934111},{"$f":"SUMPRODUCT(N34:N35,$V34:$V35)/SUM($V34:$V35)","v":10.857361374096234},{"$f":"SUMPRODUCT(O34:O35,$V34:$V35)/SUM($V34:$V35)","v":1.2710442748852431},0.41920617890276679,12.212020547541837,0.21139928078059494,8.8720259219244504,0,26.1633285196455,122.6327881235655,0.23867650155403075]
[null,"Hotel","Large",7.0995612360000004,1.823507604,17.493186609999999,14.40453838,0,14.40453838,8.5873863085489699,0,5.1544812831640998,1.3960635718964951,6.5505448550605951,0.55274273648869965,0.65871262177457524,7.378572106125123,0.24171936717982312,19.803352735924612,0,6.7716650243840091,91.365489585486429,0.18565490755171163]
[null,null,"Small",6.9996420600000002,1.442632439,13.975048080000001,8.6955509600000003,0,8.6955509600000003,4.5831120295356698,0,6.0854335516874212,0,6.0854335516874212,5.7055740012036471E-3,0,5.4842035991132141,0,0,0,16.000745745824521,63.272074039162035,0.21185128964646066]
["Hotel/motel",null,"Weighted Average",{"$f":"SUMPRODUCT(D37:D38,$V37:$V38)/SUM($V37:$V38)","v":7.0586779386069454},{"$f":"SUMPRODUCT(E37:E38,$V37:$V38)/SUM($V37:$V38)","v":1.6676673212466262},{"$f":"SUMPRODUCT(F37:F38,$V37:$V38)/SUM($V37:$V38)","v":16.053692115049827},{"$f":"SUMPRODUCT(G37:G38,$V37:$V38)/SUM($V37:$V38)","v":12.068628098823611},{"$f":"SUMPRODUCT(H37:H38,$V37:$V38)/SUM($V37:$V38)","v":0},{"$f":"SUMPRODUCT(I37:I38,$V37:$V38)/SUM($V37:$V38)","v":12.068628098823611},{"$f":"SUMPRODUCT(J37:J38,$V37:$V38)/SUM($V37:$V38)","v":6.9489827233125974},{"$f":"SUMPRODUCT(K37:K38,$V37:$V38)/SUM($V37:$V38)","v":0},{"$f":"SUMPRODUCT(L37:L38,$V37:$V38)/SUM($V37:$V38)","v":5.5353931358877322},{"$f":"SUMPRODUCT(M37:M38,$V37:$V38)/SUM($V37:$V38)","v":0.8248450683586368},{"$f":"SUMPRODUCT(N37:N38,$V37:$V38)/SUM($V37:$V38)","v":6.3602382042463699},{"$f":"SUMPRODUCT(O37:O38,$V37:$V38)/SUM($V37:$V38)","v":0.32891499996863882},0.3891913437711485,6.6034653233769687,0.14281658225219404,11.70054012583676,0,10.547869621979656,79.870684398471354,0.1963735155574636]
[null,"Office","Large",6.4861776869999996,1.301133538,1.089540671,10.144914849999999,3.0405354290000002,13.185450278999999,5.2259066022447396,0.49584467275586253,4.1682364677850252,9.9028226230875996E-2,4.2672646940159016,0.88037766412348473,0,3.6145112437523568,0.1518060115365793,0,28.373422517411417,10.143822843487758,75.215258424328098,0.13291298234934712]
[null,null,"Medium",5.8003969089999998,1.858863597,1.4188625050000001,8.6160479369999994,0,8.6160479369999994,4.3239129559185505,0,1.4899193913627209,0,1.4899193913627209,2.6517312411426866E-3,0,2.9238253959374476,0.30134980905497127,0,0,10.336068265955594,37.071898497470436,0.17520952124105876]
[null,null,"Small",7.7970055580000004,2.1245763210000002,3.1032943670000002,2.5171926340000002,0,2.5171926340000002,2.3175629770992368,0,3.3428045928753183,0,3.3428045928753183,0,0,0,0,0,0,8.320826483097056,29.523262933071614,0.16403312909760792]
["Office",null,"Weighted Average",{"$f":"SUMPRODUCT(D40:D42,$V40:$V42)/SUM($V40:$V42)","v":6.5798007121316289},{"$f":"SUMPRODUCT(E40:E42,$V40:$V42)/SUM($V40:$V42)","v":1.6183657271094134},{"$f":"SUMPRODUCT(F40:F42,$V40:$V42)/SUM($V40:$V42)","v":1.5948714183868293},{"$f":"SUMPRODUCT(G40:G42,$V40:$V42)/SUM($V40:$V42)","v":8.1572382895134865},{"$f":"SUMPRODUCT(H40:H42,$V40:$V42)/SUM($V40:$V42)","v":1.6126788022671972},{"$f":"SUMPRODUCT(I40:I42,$V40:$V42)/SUM($V40:$V42)","v":9.7699170917806857},{"$f":"SUMPRODUCT(J40:J42,$V40:$V42)/SUM($V40:$V42)","v":4.384625611969442},{"$f":"SUMPRODUCT(K40:K42,$V40:$V42)/SUM($V40:$V42)","v":0.26299255892357332},{"$f":"SUMPRODUCT(L40:L42,$V40:$V42)/SUM($V40:$V42)","v":3.2962290285290012},{"$f":"SUMPRODUCT(M40:M42,$V40:$V42)/SUM($V40:$V42)","v":5.2523881072215624E-2},{"$f":"SUMPRODUCT(N40:N42,$V40:$V42)/SUM($V40:$V42)","v":3.3487529096012172},{"$f":"SUMPRODUCT(O40:O42,$V40:$V42)/SUM($V40:$V42)","v":0.46763938994988435},0,2.6814542680865872,0.15929533206887653,0,15.049065570878488,9.8145529764828989,55.731333567369525,0.15044893826921191]
[null,"Dining","Restaurant",12.32185342,5.7206759009999999,72.419344379999998,134.6548037,0,134.6548037,10.395433046165031,0,16.086816328607778,0,16.086816328607778,7.7539281715739733E-2,14.224201134133047,0,0,152.90540510521441,0,0,418.80607229683602,0.21684963894285372]
[null,null,"Fast Food",12.27798512,5.8679595429999996,75.347860780000005,216.4479288,0,216.4479288,13.096770167932826,0,21.959360227908835,0,21.959360227908835,0,31.887240447820879,0,0,269.48507596961235,0,0,646.37018105627499,0.21904769266843488]
["Restaurant",null,"Weighted Average",{"$f":"SUMPRODUCT(D44:D45,$V44:$V45)/SUM($V44:$V45)","v":12.295233261200581},{"$f":"SUMPRODUCT(E44:E45,$V44:$V45)/SUM($V44:$V45)","v":5.8100505505441342},{"$f":"SUMPRODUCT(F44:F45,$V44:$V45)/SUM($V44:$V45)","v":74.196426501137722},{"$f":"SUMPRODUCT(G44:G45,$V44:$V45)/SUM($V44:$V45)","v":184.28850226736691},{"$f":"SUMPRODUCT(H44:H45,$V44:$V45)/SUM($V44:$V45)","v":0},{"$f":"SUMPRODUCT(I44:I45,$V44:$V45)/SUM($V44:$V45)","v":184.28850226736691},{"$f":"SUMPRODUCT(J44:J45,$V44:$V45)/SUM($V44:$V45)","v":12.034658253255955},{"$f":"SUMPRODUCT(K44:K45,$V44:$V45)/SUM($V44:$V45)","v":0},{"$f":"SUMPRODUCT(L44:L45,$V44:$V45)/SUM($V44:$V45)","v":19.650393015097997},{"$f":"SUMPRODUCT(M44:M45,$V44:$V45)/SUM($V44:$V45)","v":0},{"$f":"SUMPRODUCT(N44:N45,$V44:$V45)/SUM($V44:$V45)","v":19.650393015097997},{"$f":"SUMPRODUCT(O44:O45,$V44:$V45)/SUM($V44:$V45)","v":3.0486900099266082E-2},24.942485439902079,0,0,223.64827298918493,0,0,556.89650917778965,0.21818346175396397]
[null,"Commercial","Retail Store",14.285591670000001,2.3628223479999999,3.6900072800000001,6.9880976309999996,0,6.9880976309999996,4.1094065000809978,0,6.6741860400129598,0.73564634699497822,7.4098323870079383,0,0,0,0,0,0,7.4601297100275392,46.305887526116472,0.22481996959711098]
[null,null,"Strip Mall",20.43483604,3.0000419100000002,2.7320606390000002,23.025637239999998,0,23.025637239999998,3.7433107208888892,0,6.3405380133333331,0,6.3405380133333331,0,0,0,0,0,0,5.3996540844444443,64.676078647666671,0.18039157765982777]
["Retail",null,"Weighted Average",{"$f":"SUMPRODUCT(D47:D48,$V47:$V48)/SUM($V47:$V48)","v":17.869137954223163},{"$f":"SUMPRODUCT(E47:E48,$V47:$V48)/SUM($V47:$V48)","v":2.7341697292782321},{"$f":"SUMPRODUCT(F47:F48,$V47:$V48)/SUM($V47:$V48)","v":3.1317523271496528},{"$f":"SUMPRODUCT(G47:G48,$V47:$V48)/SUM($V47:$V48)","v":16.33416716668081},{"$f":"SUMPRODUCT(H47:H48,$V47:$V48)/SUM($V47:$V48)","v":0},{"$f":"SUMPRODUCT(I47:I48,$V47:$V48)/SUM($V47:$V48)","v":16.33416716668081},{"$f":"SUMPRODUCT(J47:J48,$V47:$V48)/SUM($V47:$V48)","v":3.8960597715635767},{"$f":"SUMPRODUCT(K47:K48,$V47:$V48)/SUM($V47:$V48)","v":0},{"$f":"SUMPRODUCT(L47:L48,$V47:$V48)/SUM($V47:$V48)","v":6.479748630421744},{"$f":"SUMPRODUCT(M47:M48,$V47:$V48)/SUM($V47:$V48)","v":0.30693957025060259},{"$f":"SUMPRODUCT(N47:N48,$V47:$V48)/SUM($V47:$V48)","v":6.7866882006723461},{"$f":"SUMPRODUCT(O47:O48,$V47:$V48)/SUM($V47:$V48)","v":0},0,0,0,0,0,6.2593627006997412,57.01133785026753,0.19892878862248634]
[null,"School","Secondary",8.336314453,0.52049142999999998,3.0695951500000001,3.9393240340000002,0,3.9393240340000002,5.5259844087117749,0,4.0089708251338392,1.2330315192496457,5.2420023443834847,0.17653911246307263,0.86210849886432095,0.29580797088277422,0.18380567270623605,4.0631337714826774,0,8.5700306124975771,40.785137458991912,0.22020832151119527]
[null,null,"Primary",8.8988920220000001,0.58926862700000004,1.9509747159999999,14.59819575,0,14.59819575,5.2266345434632706,0,4.4230398031341691,1.3041590191863059,5.7271988223204753,2.8969917278492137E-2,1.5672025230195112,0,0.31016270190240541,6.5470043462519074,0,11.983640889622023,57.42814485885809,0.18425374911816181]
["School",null,"Weighted Average",{"$f":"SUMPRODUCT(D50:D51,$V50:$V51)/SUM($V50:$V51)","v":8.665269817940537},{"$f":"SUMPRODUCT(E50:E51,$V50:$V51)/SUM($V50:$V51)","v":0.5607074449736118},{"$f":"SUMPRODUCT(F50:F51,$V50:$V51)/SUM($V50:$V51)","v":2.4155054504222147},{"$f":"SUMPRODUCT(G50:G51,$V50:$V51)/SUM($V50:$V51)","v":10.171874402873907},{"$f":"SUMPRODUCT(H50:H51,$V50:$V51)/SUM($V50:$V51)","v":0},{"$f":"SUMPRODUCT(I50:I51,$V50:$V51)/SUM($V50:$V51)","v":10.171874402873907},{"$f":"SUMPRODUCT(J50:J51,$V50:$V51)/SUM($V50:$V51)","v":5.3509458903030849},{"$f":"SUMPRODUCT(K50:K51,$V50:$V51)/SUM($V50:$V51)","v":0},{"$f":"SUMPRODUCT(L50:L51,$V50:$V51)/SUM($V50:$V51)","v":4.251088924529042},{"$f":"SUMPRODUCT(M50:M51,$V50:$V51)/SUM($V50:$V51)","v":1.2746218242818252},{"$f":"SUMPRODUCT(N50:N51,$V50:$V51)/SUM($V50:$V51)","v":5.5257107488108668},{"$f":"SUMPRODUCT(O50:O51,$V50:$V51)/SUM($V50:$V51)","v":9.0251138802457567E-2},1.2743973543294447,0.12284050048215038,0.25769027981190584,5.5155246885977371,0,10.566067206121943,50.516784923469864,0.19918464382732506]
["Warehouse","Warehouse",null,5.5959270569999999,1.507548578,0.475070891,12.16764439,0,12.16764439,6.1751929426457873E-2,0,0.48472532212508407,0,0.48472532212508407,0,0,0,0,0,0,2.4864714958209242,22.779139663372465,0.21414833409843687]
[]
[null,"Climate Zone 6A",null,"Site EUI (kBtu/SF/yr)"]
[null,"Building Type",null,"Lighting, Interior","Lighting, Exterior","DHW","Heating","Humidfy","Heat","Cooling","Heat Rejection","Fan","Heat Recovery","Fans","Pumps","Refrigeration","Elevator","Transformers","Cooking","Data Center","Equipment","Total","Weight"]
[null,"Apartments","Mid Rise",3.1104234489999998,1.1261587340000001,12.268892490000001,12.770993669999999,0,{"$f":"G57+H57","v":12.770993669999999},1.9112105059126878,0,5.4164076613022729,0,{"$f":"L57+M57","v":5.4164076613022729},0,0,3.5111295522427404,0,0,0,10.849361147499414,50.96457720995712,4.2799807491917412E-2]
[null,null,"High Rise",3.0074910359999998,1.8285015010000001,13.95421148,14.27371559,0,{"$f":"G58+H58","v":14.27371559},2.2045643209408192,0.10373759207843324,6.1721057497154783,0,{"$f":"L58+M58","v":6.1721057497154783},0.53262453836305002,0,1.7804139861005743,0.23384678608687406,0,0,10.928396368129318,55.01960894841455,1.3897546597388517E-2]
["Multifamily",null,"Weighted Average",{"$f":"SUMPRODUCT(D57:D58,$V57:$V58)/SUM($V57:$V58)","v":3.0569881081566592},{"$f":"SUMPRODUCT(E57:E58,$V57:$V58)/SUM($V57:$V58)","v":1.4907661890248842},{"$f":"SUMPRODUCT(F57:F58,$V57:$V58)/SUM($V57:$V58)","v":13.143792747709933},{"$f":"SUMPRODUCT(G57:G58,$V57:$V58)/SUM($V57:$V58)","v":13.551102244623234},{"$f":"SUMPRODUCT(H57:H58,$V57:$V58)/SUM($V57:$V58)","v":0},{"$f":"SUMPRODUCT(I57:I58,$V57:$V58)/SUM($V57:$V58)","v":13.551102244623234},{"$f":"SUMPRODUCT(J57:J58,$V57:$V58)/SUM($V57:$V58)","v":2.0634993781625073},{"$f":"SUMPRODUCT(K57:K58,$V57:$V58)/SUM($V57:$V58)","v":5.3853333749968139E-2},{"$f":"SUMPRODUCT(L57:L58,$V57:$V58)/SUM($V57:$V58)","v":5.808713483657967},{"$f":"SUMPRODUCT(M57:M58,$V57:$V58)/SUM($V57:$V58)","v":0},{"$f":"SUMPRODUCT(N57:N58,$V57:$V58)/SUM($V57:$V58)","v":5.808713483657967},{"$f":"SUMPRODUCT(O57:O58,$V57:$V58)/SUM($V57:$V58)","v":0.27650156951976612},0,2.6126625535172501,0.12139696676179142,0,0,10.890390730211982,53.06966730509594,2.7795766325192605E-2]
[null,"Healthcare","Hospital",13.78434932,0.80652356000000003,5.2932184859999998,33.946940820000002,4.5257964570000002,38.472737277,6.6790907035581633,0.85347426221837586,11.466531335273974,0.93497063200566455,12.401501967279639,1.7074981151216764,0.79255025615260877,9.8430027453302475,0.40479827710858335,16.988614125821439,0,20.900455956244016,128.92781505183473,6.4131899422876476E-2]
[null,null,"Clinic",11.666400080000001,2.5825515810000002,3.2370132869999999,27.14853986,4.5059204160000004,31.654460276000002,11.939380923655547,0,8.6038745518487758,0.53392181678308015,9.1377963686318555,0.47464862306452404,0,14.801530674546976,0,0,0,31.916034044839535,117.40981585873844,7.834475565634956E-2]
["Healthcare/hospital",null,"Weighted Average",{"$f":"SUMPRODUCT(D60:D61,$V60:$V61)/SUM($V60:$V61)","v":12.77488913583176},{"$f":"SUMPRODUCT(E60:E61,$V60:$V61)/SUM($V60:$V61)","v":1.6530167333522632},{"$f":"SUMPRODUCT(F60:F61,$V60:$V61)/SUM($V60:$V61)","v":4.313186840449216},{"$f":"SUMPRODUCT(G60:G61,$V60:$V61)/SUM($V60:$V61)","v":30.706676626920874},{"$f":"SUMPRODUCT(H60:H61,$V60:$V61)/SUM($V60:$V61)","v":4.5163231081446726},{"$f":"SUMPRODUCT(I60:I61,$V60:$V61)/SUM($V60:$V61)","v":35.222999735065549},{"$f":"SUMPRODUCT(J60:J61,$V60:$V61)/SUM($V60:$V61)","v":9.1862582192243512},{"$f":"SUMPRODUCT(K60:K61,$V60:$V61)/SUM($V60:$V61)","v":0.4466900628379345},{"$f":"SUMPRODUCT(L60:L61,$V60:$V61)/SUM($V60:$V61)","v":10.102127510465188},{"$f":"SUMPRODUCT(M60:M61,$V60:$V61)/SUM($V60:$V61)","v":0.74382213645671347},{"$f":"SUMPRODUCT(N60:N61,$V60:$V61)/SUM($V60:$V61)","v":10.845949646921902},{"$f":"SUMPRODUCT(O60:O61,$V60:$V61)/SUM($V60:$V61)","v":1.1198955173824907},0.41480374909354539,12.206343859506562,0.2118627073396796,8.8914750535862286,0,26.150717518713407,123.43808877930488,7.0906052551776982E-2]
[null,"Hotel","Large",7.1015796780000002,1.822498382,17.963602560000002,16.88584475,0,16.88584475,6.0661962684245001,0,5.1764512536848999,1.3643895496233214,6.540840803308221,0.48613413150999019,0.65793629774902662,7.378572106125123,0.24171936717982312,19.803352735924612,0,6.7716650243840091,91.719942104605295,4.5773999691660947E-2]
[null,null,"Small",7.017417118,1.442632439,14.730853359999999,10.301982629999999,0,10.301982629999999,3.4935668441275869,0,6.0435195268737569,0,6.0435195268737569,5.7055740012036471E-3,0,5.4842035991132141,0,0,0,16.000745745824521,64.520626836940281,6.1948884988588998E-2]
["Hotel/motel",null,"Weighted Average",{"$f":"SUMPRODUCT(D63:D64,$V63:$V64)/SUM($V63:$V64)","v":7.066824164984471},{"$f":"SUMPRODUCT(E63:E64,$V63:$V64)/SUM($V63:$V64)","v":1.6656301055824003},{"$f":"SUMPRODUCT(F63:F64,$V63:$V64)/SUM($V63:$V64)","v":16.62861635120904},{"$f":"SUMPRODUCT(G63:G64,$V63:$V64)/SUM($V63:$V64)","v":14.166993213115775},{"$f":"SUMPRODUCT(H63:H64,$V63:$V64)/SUM($V63:$V64)","v":0},{"$f":"SUMPRODUCT(I63:I64,$V63:$V64)/SUM($V63:$V64)","v":14.166993213115775},{"$f":"SUMPRODUCT(J63:J64,$V63:$V64)/SUM($V63:$V64)","v":5.003811100479453},{"$f":"SUMPRODUCT(K63:K64,$V63:$V64)/SUM($V63:$V64)","v":0},{"$f":"SUMPRODUCT(L63:L64,$V63:$V64)/SUM($V63:$V64)","v":5.5345131122377751},{"$f":"SUMPRODUCT(M63:M64,$V63:$V64)/SUM($V63:$V64)","v":0.80095541988456864},{"$f":"SUMPRODUCT(N63:N64,$V63:$V64)/SUM($V63:$V64)","v":6.3354685321223441},{"$f":"SUMPRODUCT(O63:O64,$V63:$V64)/SUM($V63:$V64)","v":0.28773782579485252},0.38623693927174785,6.5962794892933481,0.14189967761567657,11.625420841213396,0,10.58287793348987,80.487796174172374,5.2453530785559199E-2]
[null,"Office","Large",6.4957420490000004,1.303529382,1.1484907639999999,12.170889219999999,3.4892238039999999,15.660113023999999,3.9032294820573297,0.48962688652755382,4.0961519832005582,5.0236669294086503E-2,4.1463886524946449,0.70308519458952079,0,3.6145112437523568,0.15182502617391511,0,28.373422517411417,10.143822843487758,76.133787065494488,4.0012083576556959E-2]
[null,null,"Medium",5.8150698219999999,1.8613385469999999,1.4821351469999999,10.30103768,0,10.30103768,2.9123080275229358,0,1.4276920983441483,0,1.4276920983441483,2.6517312411426866E-3,0,2.9238253959374476,0.30152659114641606,0,0,10.336068265955594,37.36365330614769,4.9349809930598232E-2]
[null,null,"Small",7.8107903189999996,2.1262994160000002,3.1032943670000002,3.5715397260000001,0,3.5715397260000001,1.6782946770265361,0,3.2032338858596874,0,3.2032338858596874,0,0,0,0,0,0,8.320826483097056,29.814278873983284,4.3007828377301729E-2]
["Office",null,"Weighted Average",{"$f":"SUMPRODUCT(D66:D68,$V66:$V68)/SUM($V66:$V68)","v":6.591859901903355},{"$f":"SUMPRODUCT(E66:E68,$V66:$V68)/SUM($V66:$V68)","v":1.6201265433048626},{"$f":"SUMPRODUCT(F66:F68,$V66:$V68)/SUM($V66:$V68)","v":1.6421505511414092},{"$f":"SUMPRODUCT(G66:G68,$V66:$V68)/SUM($V66:$V68)","v":9.8943978741364766},{"$f":"SUMPRODUCT(H66:H68,$V66:$V68)/SUM($V66:$V68)","v":1.8536364193795651},{"$f":"SUMPRODUCT(I66:I68,$V66:$V68)/SUM($V66:$V68)","v":11.748034293516042},{"$f":"SUMPRODUCT(J66:J68,$V66:$V68)/SUM($V66:$V68)","v":3.1820095219693738},{"$f":"SUMPRODUCT(K66:K68,$V66:$V68)/SUM($V66:$V68)","v":0.26011235729116888},{"$f":"SUMPRODUCT(L66:L68,$V66:$V68)/SUM($V66:$V68)","v":3.2146810202545812},{"$f":"SUMPRODUCT(M66:M68,$V66:$V68)/SUM($V66:$V68)","v":2.6688032933024734E-2},{"$f":"SUMPRODUCT(N66:N68,$V66:$V68)/SUM($V66:$V68)","v":3.2413690531876065},{"$f":"SUMPRODUCT(O66:O68,$V66:$V68)/SUM($V66:$V68)","v":0.3742025923827052},0,2.6824828410599717,0.15926924433162812,0,15.073269092233335,9.8146918358601134,56.389577828181565,4.3069806583380374E-2]
[null,"Dining","Restaurant",12.35459223,5.7241220909999999,75.597684229999999,160.0143381,0,160.0143381,5.7344606615776081,0,15.075359474736459,0,15.075359474736459,7.7539281715739733E-2,14.153554233006183,0,0,152.90540510521441,0,0,441.63705540725039,4.7010740075510475E-2]
[null,null,"Fast Food",12.304519819999999,5.8717502149999996,79.338470240000007,252.59837859999999,0,252.59837859999999,6.9596729468212706,0,20.655369220311876,0,20.655369220311876,0,31.648428140743714,0,0,269.48507596961235,0,0,678.86166515248919,4.3242658256224711E-2]
["Restaurant",null,"Weighted Average",{"$f":"SUMPRODUCT(D70:D71,$V70:$V71)/SUM($V70:$V71)","v":12.324255524560643},{"$f":"SUMPRODUCT(E70:E71,$V70:$V71)/SUM($V70:$V71)","v":5.8135635800825707},{"$f":"SUMPRODUCT(F70:F71,$V70:$V71)/SUM($V70:$V71)","v":77.864064523999062},{"$f":"SUMPRODUCT(G70:G71,$V70:$V71)/SUM($V70:$V71)","v":216.1070000077068},{"$f":"SUMPRODUCT(H70:H71,$V70:$V71)/SUM($V70:$V71)","v":0},{"$f":"SUMPRODUCT(I70:I71,$V70:$V71)/SUM($V70:$V71)","v":216.1070000077068},{"$f":"SUMPRODUCT(J70:J71,$V70:$V71)/SUM($V70:$V71)","v":6.4767637422186137},{"$f":"SUMPRODUCT(K70:K71,$V70:$V71)/SUM($V70:$V71)","v":0},{"$f":"SUMPRODUCT(L70:L71,$V70:$V71)/SUM($V70:$V71)","v":18.456045804798617},{"$f":"SUMPRODUCT(M70:M71,$V70:$V71)/SUM($V70:$V71)","v":0},{"$f":"SUMPRODUCT(N70:N71,$V70:$V71)/SUM($V70:$V71)","v":18.456045804798617},{"$f":"SUMPRODUCT(O70:O71,$V70:$V71)/SUM($V70:$V71)","v":3.0561587824237783E-2},24.75294092994649,0,0,223.5359806103784,0,0,585.36117631151546,4.472782243237982E-2]
[null,"Commercial","Retail Store",15.384069849999999,2.3643581450000002,3.7579497829999999,8.2632671080000009,0,8.2632671080000009,2.5993349526162319,0,6.3489812084885795,0.70147488295804306,7.0504560914466223,0,0,0,0,0,0,7.4601297100275392,46.879565640090398,6.2161938286217848E-2]
[null,null,"Strip Mall",20.43483604,3.0017273269999998,2.7733533499999998,28.038957920000001,0,28.038957920000001,2.4063538413333334,0,5.9271895422222221,0,5.9271895422222221,0,0,0,0,0,0,5.3996540844444443,67.982072105,2.6924529896460325E-2]
["Retail",null,"Weighted Average",{"$f":"SUMPRODUCT(D73:D74,$V73:$V74)/SUM($V73:$V74)","v":18.373419105807148},{"$f":"SUMPRODUCT(E73:E74,$V73:$V74)/SUM($V73:$V74)","v":2.7415918196964149},{"$f":"SUMPRODUCT(F73:F74,$V73:$V74)/SUM($V73:$V74)","v":3.1752059965055146},{"$f":"SUMPRODUCT(G73:G74,$V73:$V74)/SUM($V73:$V74)","v":19.967718351252746},{"$f":"SUMPRODUCT(H73:H74,$V73:$V74)/SUM($V73:$V74)","v":0},{"$f":"SUMPRODUCT(I73:I74,$V73:$V74)/SUM($V73:$V74)","v":19.967718351252746},{"$f":"SUMPRODUCT(J73:J74,$V73:$V74)/SUM($V73:$V74)","v":2.4851170459270349},{"$f":"SUMPRODUCT(K73:K74,$V73:$V74)/SUM($V73:$V74)","v":0},{"$f":"SUMPRODUCT(L73:L74,$V73:$V74)/SUM($V73:$V74)","v":6.0993393608506095},{"$f":"SUMPRODUCT(M73:M74,$V73:$V74)/SUM($V73:$V74)","v":0.28629957282593177},{"$f":"SUMPRODUCT(N73:N74,$V73:$V74)/SUM($V73:$V74)","v":6.3856389336765407},{"$f":"SUMPRODUCT(O73:O74,$V73:$V74)/SUM($V73:$V74)","v":0},0,0,0,0,0,6.2406154727340502,59.369306725599451,4.1306306371390648E-2]
[null,"School","Secondary",8.3917442270000002,0.52076116100000003,3.186630139,5.0243696230000001,0,5.0243696230000001,3.7343843982796474,0,3.9247247601796222,1.1838055636430884,5.1085303238227109,0.13054993190666092,0.85963596238743989,0.29580797088277422,0.18380567270623605,4.0631337714826774,0,8.5700306124975771,40.06938379396572,4.0078616184763494E-2]
[null,null,"Primary",8.9596519370000003,0.58965318300000003,2.024919804,17.339802809999998,0,17.339802809999998,3.6666173177030514,0,4.3117748117200065,1.2510902326964939,5.5628650444165002,3.3712779837477523E-2,1.5629724024121479,0,0.31029088738355032,6.5470043462519074,0,11.983640889622023,58.581131401626664,3.3655279363060737E-2]
["School",null,"Weighted Average",{"$f":"SUMPRODUCT(D76:D77,$V76:$V77)/SUM($V76:$V77)","v":8.7289819608075288},{"$f":"SUMPRODUCT(E76:E77,$V76:$V77)/SUM($V76:$V77)","v":0.5616709584329288},{"$f":"SUMPRODUCT(F76:F77,$V76:$V77)/SUM($V76:$V77)","v":2.4967776263158763},{"$f":"SUMPRODUCT(G76:G77,$V76:$V77)/SUM($V76:$V77)","v":12.337580388956898},{"$f":"SUMPRODUCT(H76:H77,$V76:$V77)/SUM($V76:$V77)","v":0},{"$f":"SUMPRODUCT(I76:I77,$V76:$V77)/SUM($V76:$V77)","v":12.337580388956898},{"$f":"SUMPRODUCT(J76:J77,$V76:$V77)/SUM($V76:$V77)","v":3.6941426190644937},{"$f":"SUMPRODUCT(K76:K77,$V76:$V77)/SUM($V76:$V77)","v":0},{"$f":"SUMPRODUCT(L76:L77,$V76:$V77)/SUM($V76:$V77)","v":4.1545647147235867},{"$f":"SUMPRODUCT(M76:M77,$V76:$V77)/SUM($V76:$V77)","v":1.2237608748882203},{"$f":"SUMPRODUCT(N76:N77,$V76:$V77)/SUM($V76:$V77)","v":5.3783255896118058},{"$f":"SUMPRODUCT(O76:O77,$V76:$V77)/SUM($V76:$V77)","v":7.3045620665338651E-2},1.2772946469969308,0.12014983491080329,0.25891574148472896,5.5381179440102564,0,10.597117362137837,51.062120293395424,3.6264278898809933E-2]
["Warehouse","Warehouse",null,7.1940086990000003,1.5091880099999999,0.485271799,11.906309479999999,0,11.906309479999999,1.5847840292054952E-2,0,0.3767049854933231,0,0.3767049854933231,0,0,0,0,0,0,2.4864714958209242,23.973802309606299,2.7870410498406498E-2]

{"sheet":"Revision Notes","index":36,"n_rows":4,"n_cols":2,"rows_kept":4,"cut":false,"hidden":false,"merged":[[3,1,3,6],[5,1,37,6]]}
[null,"Revision Notes"]
[]
[]
[null,"Please provide a narrative describing any additional changes made to the energy models between the review phases not addressed by the responses to the programs review comments. If the projected savings increase or decrease substantially between revisions, a narrative explanation for these results must be provided."]

{"sheet":"Quality Assurance Checks","index":37,"n_rows":190,"n_cols":135,"rows_kept":190,"cut":false,"hidden":false,"merged":[[144,1,144,5],[144,6,144,12],[4,0,4,12],[142,6,142,12],[188,1,188,5],[188,6,188,12],[189,1,189,5],[189,6,189,12],[176,1,176,3],[176,4,176,6],[176,7,176,9],[176,10,176,12],[155,8,155,9],[156,8,156,9],[157,8,157,9],[158,8,158,9],[185,6,185,12],[187,6,187,12],[183,6,183,12],[184,6,184,12],[185,1,185,5],[187,1,187,5],[183,1,183,5],[184,1,184,5],[112,4,112,6],[113,4,113,6],[114,4,114,6],[115,4,115,6],[111,1,111,3],[112,1,112,3],[113,1,113,3],[114,1,114,3],[115,1,115,3],[125,1,125,2],[124,7,124,8],[125,7,125,8],[121,9,121,10],[122,9,122,10],[123,9,123,10],[124,9,124,10],[125,9,125,10],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[116,0,116,5],[116,6,116,12],[112,7,112,10],[113,7,113,10],[114,7,114,10],[115,7,115,10],[104,6,104,12],[105,6,105,12],[111,11,111,12],[109,0,109,12],[110,0,110,12],[96,1,96,3],[97,1,97,3],[98,1,98,3],[99,1,99,3],[100,1,100,3],[96,4,96,6],[100,4,100,6],[102,1,102,5],[103,1,103,5],[102,6,102,12],[103,6,103,12],[98,10,98,12],[99,4,99,6],[99,7,99,9],[99,10,99,12],[111,4,111,6],[97,7,97,9],[97,10,97,12],[98,4,98,6],[98,7,98,9],[111,7,111,10],[96,7,96,9],[96,10,96,12],[97,4,97,6],[106,1,106,5],[104,1,104,5],[105,1,105,5],[107,6,107,12],[108,6,108,12],[169,0,169,12],[170,0,170,5],[170,6,170,12],[173,0,173,12],[182,0,182,5],[182,6,182,12],[167,1,167,5],[167,6,167,12],[166,1,166,5],[166,6,166,12],[168,1,168,5],[168,6,168,12],[155,4,155,5],[156,4,156,5],[157,4,157,5],[158,4,158,5],[154,6,154,7],[155,6,155,7],[156,6,156,7],[157,6,157,7],[163,6,163,12],[154,1,154,2],[155,1,155,2],[162,1,162,5],[162,6,162,12],[161,1,161,5],[161,6,161,12],[160,1,160,5],[160,6,160,12],[123,7,123,8],[158,1,158,2],[154,4,154,5],[107,1,107,5],[108,1,108,5],[106,6,106,12],[164,1,164,5],[164,6,164,12],[165,1,165,5],[165,6,165,12],[140,1,140,5],[140,6,140,12],[152,0,152,12],[153,0,153,12],[159,0,159,5],[159,6,159,12],[163,1,163,5],[66,0,66,2],[67,0,67,2],[66,3,66,4],[67,3,67,4],[66,5,66,6],[66,7,66,8],[67,5,67,6],[67,7,67,8],[112,11,112,12],[113,11,113,12],[114,11,114,12],[115,11,115,12],[82,6,82,7],[83,4,83,5],[83,6,83,7],[84,4,84,5],[126,0,126,5],[126,6,126,12],[82,4,82,5],[94,0,94,12],[95,0,95,12],[151,1,151,5],[151,6,151,12],[147,1,147,5],[147,6,147,12],[148,1,148,5],[148,6,148,12],[149,1,149,5],[149,6,149,12],[133,7,133,8],[186,6,186,12],[172,6,172,12],[171,1,171,5],[186,1,186,5],[172,1,172,5],[171,6,171,12],[174,0,174,12],[154,10,154,11],[155,10,155,11],[156,10,156,11],[157,10,157,11],[158,10,158,11],[158,6,158,7],[154,8,154,9],[141,6,141,12],[142,1,142,5],[156,1,156,2],[157,1,157,2],[92,1,92,5],[76,6,76,12],[134,7,134,8],[135,7,135,8],[136,7,136,8],[150,1,150,5],[150,6,150,12],[139,1,139,5],[139,6,139,12],[141,1,141,5],[117,1,117,5],[118,1,118,5],[129,6,129,12],[127,6,127,12],[128,6,128,12],[129,1,129,5],[127,1,127,5],[128,1,128,5],[117,6,117,12],[118,6,118,12],[120,0,120,12],[131,0,131,12],[132,0,132,12],[138,0,138,5],[138,6,138,12],[119,0,119,12],[137,7,137,8],[133,9,133,10],[134,9,134,10],[135,9,135,10],[136,9,136,10],[137,9,137,10],[61,0,61,5],[61,6,61,12],[68,0,68,5],[68,6,68,12],[76,0,76,5],[66,9,66,12],[67,9,67,12],[146,1,146,5],[121,7,121,8],[122,7,122,8],[62,1,62,5],[62,6,62,12],[69,1,69,5],[71,1,71,5],[69,6,69,12],[71,6,71,12],[70,6,70,12],[70,1,70,5],[77,6,77,12],[78,6,78,12],[77,1,77,5],[78,1,78,5],[87,1,87,5],[88,1,88,5],[101,0,101,5],[101,6,101,12],[91,1,91,5],[90,1,90,5],[93,1,93,5],[87,6,87,12],[88,6,88,12],[89,6,89,12],[49,21,49,22],[50,21,50,22],[57,1,57,2],[58,1,58,2],[48,3,48,4],[52,1,52,2],[53,1,53,2],[54,1,54,2],[48,5,48,8],[48,15,48,16],[49,12,49,13],[47,3,47,8],[49,1,49,2],[50,1,50,2],[51,1,51,2],[55,1,55,2],[56,1,56,2],[54,21,54,22],[55,21,55,22],[51,58,52,58],[57,58,58,58],[57,59,58,59],[57,60,58,61],[57,62,58,62],[51,62,52,62],[51,63,52,63],[51,68,52,68],[57,63,58,63],[47,23,47,25],[48,24,48,25],[53,58,54,58],[53,59,54,59],[53,60,54,61],[53,62,54,62],[53,63,54,63],[53,68,54,68],[2,117,4,117],[5,117,7,117],[8,117,10,117],[11,117,13,117],[14,117,16,117],[47,14,47,16],[45,68,46,68],[47,58,48,58],[37,58,38,58],[41,58,42,58],[37,62,38,62],[41,59,42,59],[43,59,44,59],[45,59,46,59],[43,58,44,58],[41,60,42,61],[37,60,38,61],[19,90,20,90],[19,91,20,91],[19,93,20,93],[19,95,20,95],[41,89,42,89],[41,93,42,93],[41,91,42,91],[17,117,19,117],[20,117,22,117],[23,117,25,117],[41,62,42,62],[41,63,42,63],[41,68,42,68],[43,60,44,61],[43,62,44,62],[39,88,40,88],[29,88,30,88],[31,87,32,87],[31,85,32,85],[31,86,32,86],[35,90,36,90],[35,91,36,91],[27,88,28,88],[29,87,30,87],[29,85,30,85],[29,86,30,86],[33,85,34,85],[33,86,34,86],[33,87,34,87],[33,88,34,88],[33,89,34,89],[27,86,28,86],[19,98,20,98],[19,99,20,99],[21,98,22,98],[13,97,14,97],[15,98,16,98],[35,93,36,93],[21,88,22,88],[23,88,24,88],[27,95,28,95],[29,96,30,96],[29,93,30,93],[31,88,32,88],[35,88,36,88],[35,102,36,102],[31,99,32,99],[31,100,32,100],[31,102,32,102],[35,99,36,99],[31,89,32,89],[31,90,32,90],[31,91,32,91],[31,93,32,93],[31,95,32,95],[31,96,32,96],[27,102,28,102],[29,89,30,89],[29,90,30,90],[31,97,32,97],[31,98,32,98],[31,94,32,94],[27,89,28,89],[27,90,28,90],[2,94,2,102],[5,89,6,89],[5,90,6,90],[5,97,6,97],[5,98,6,98],[5,95,6,95],[5,96,6,96],[5,99,6,99],[5,100,6,100],[5,102,6,102],[5,93,6,93],[5,94,6,94],[2,85,2,93],[5,91,6,91],[5,87,6,87],[17,96,18,96],[15,95,16,95],[15,96,16,96],[15,94,16,94],[13,96,14,96],[11,95,12,95],[11,96,12,96],[11,94,12,94],[11,97,12,97],[13,98,14,98],[13,99,14,99],[11,98,12,98],[11,99,12,99],[11,100,12,100],[11,102,12,102],[15,102,16,102],[15,97,16,97],[9,90,10,90],[9,91,10,91],[19,62,20,62],[21,97,22,97],[17,97,18,97],[23,97,24,97],[21,94,22,94],[21,95,22,95],[21,96,22,96],[17,94,18,94],[17,95,18,95],[25,88,26,88],[23,89,24,89],[17,88,18,88],[17,89,18,89],[17,90,18,90],[17,91,18,91],[19,89,20,89],[19,97,20,97],[9,62,10,62],[9,63,10,63],[9,68,10,68],[25,93,26,93],[23,94,24,94],[11,88,12,88],[9,89,10,89],[19,63,20,63],[17,63,18,63],[15,68,16,68],[25,87,26,87],[19,68,20,68],[25,92,26,92],[27,63,28,63],[27,68,28,68],[29,63,30,63],[29,68,30,68],[27,85,28,85],[25,85,26,85],[25,86,26,86],[17,60,18,61],[5,62,6,62],[3,75,3,79],[3,80,3,84],[4,60,4,61],[9,60,10,61],[7,60,8,61],[21,68,22,68],[19,86,20,86],[5,85,6,85],[17,68,18,68],[15,62,16,62],[25,60,26,61],[5,86,6,86],[5,68,6,68],[7,62,8,62],[7,63,8,63],[7,68,8,68],[5,63,6,63],[19,102,20,102],[21,99,22,99],[21,100,22,100],[21,102,22,102],[17,58,18,58],[5,59,6,59],[7,59,8,59],[5,60,6,61],[15,60,16,61],[35,104,36,104],[23,104,24,104],[27,104,28,104],[29,104,30,104],[31,104,32,104],[19,103,20,103],[17,104,18,104],[15,103,16,103],[21,104,22,104],[19,104,20,104],[21,103,22,103],[35,103,36,103],[33,104,34,104],[23,103,24,103],[27,103,28,103],[15,104,16,104],[7,87,8,87],[7,89,8,89],[5,88,6,88],[7,88,8,88],[23,93,24,93],[17,85,18,85],[17,86,18,86],[5,58,6,58],[7,58,8,58],[9,58,10,58],[11,58,12,58],[15,58,16,58],[11,93,12,93],[11,90,12,90],[7,90,8,90],[7,91,8,91],[11,87,12,87],[5,92,6,92],[7,92,8,92],[9,59,10,59],[11,59,12,59],[11,60,12,61],[11,62,12,62],[15,59,16,59],[15,86,16,86],[15,87,16,87],[15,63,16,63],[7,93,8,93],[13,58,14,58],[13,59,14,59],[13,60,14,61],[13,62,14,62],[13,85,14,85],[7,85,8,85],[7,86,8,86],[9,85,10,85],[9,86,10,86],[11,85,12,85],[11,86,12,86],[13,102,14,102],[13,103,14,103],[13,104,14,104],[13,94,14,94],[7,102,8,102],[9,96,10,96],[9,97,10,97],[9,98,10,98],[11,68,12,68],[11,91,12,91],[13,86,14,86],[15,85,16,85],[13,87,14,87],[13,95,14,95],[9,92,10,92],[11,92,12,92],[13,92,14,92],[15,92,16,92],[9,99,10,99],[9,100,10,100],[7,98,8,98],[7,99,8,99],[9,102,10,102],[9,87,10,87],[9,93,10,93],[7,96,8,96],[7,97,8,97],[7,100,8,100],[15,100,16,100],[15,89,16,89],[15,90,16,90],[15,88,16,88],[17,59,18,59],[17,62,18,62],[13,63,14,63],[13,68,14,68],[13,88,14,88],[13,89,14,89],[13,90,14,90],[13,91,14,91],[13,93,14,93],[15,91,16,91],[15,93,16,93],[21,62,22,62],[23,62,24,62],[19,85,20,85],[21,89,22,89],[21,90,22,90],[21,91,22,91],[21,93,22,93],[17,93,18,93],[23,87,24,87],[21,85,22,85],[21,86,22,86],[23,85,24,85],[23,86,24,86],[19,88,20,88],[17,87,18,87],[19,87,20,87],[23,90,24,90],[23,91,24,91],[21,92,22,92],[23,92,24,92],[5,104,6,104],[7,104,8,104],[9,104,10,104],[11,104,12,104],[5,103,6,103],[7,103,8,103],[9,103,10,103],[11,103,12,103],[25,94,26,94],[25,95,26,95],[25,96,26,96],[25,97,26,97],[25,98,26,98],[25,99,26,99],[25,100,26,100],[23,95,24,95],[23,96,24,96],[15,99,16,99],[17,98,18,98],[13,100,14,100],[17,99,18,99],[17,100,18,100],[17,102,18,102],[17,103,18,103],[25,102,26,102],[25,103,26,103],[25,104,26,104],[23,102,24,102],[5,101,6,101],[7,101,8,101],[7,95,8,95],[7,94,8,94],[9,101,10,101],[11,101,12,101],[27,98,28,98],[29,94,30,94],[27,94,28,94],[27,96,28,96],[27,100,28,100],[21,63,22,63],[29,95,30,95],[27,93,28,93],[29,97,30,97],[29,98,30,98],[25,89,26,89],[25,90,26,90],[25,63,26,63],[25,68,26,68],[23,98,24,98],[23,99,24,99],[23,100,24,100],[25,91,26,91],[23,63,24,63],[23,68,24,68],[27,87,28,87],[9,95,10,95],[11,63,12,63],[9,94,10,94],[19,94,20,94],[19,96,20,96],[19,100,20,100],[11,89,12,89],[21,87,22,87],[9,88,10,88],[31,59,32,59],[33,59,34,59],[35,59,36,59],[37,59,38,59],[39,59,40,59],[31,58,32,58],[33,58,34,58],[35,58,36,58],[29,58,30,58],[29,59,30,59],[27,59,28,59],[25,58,26,58],[23,58,24,58],[27,58,28,58],[27,60,28,61],[19,58,20,58],[19,60,20,61],[39,60,40,61],[23,60,24,61],[21,59,22,59],[23,59,24,59],[25,59,26,59],[21,58,22,58],[21,60,22,61],[19,59,20,59],[39,68,40,68],[39,85,40,85],[39,86,40,86],[39,87,40,87],[45,85,46,85],[45,86,46,86],[45,87,46,87],[31,60,32,61],[33,60,34,61],[29,60,30,61],[33,62,34,62],[33,63,34,63],[33,68,34,68],[31,62,32,62],[31,63,32,63],[31,68,32,68],[25,62,26,62],[27,62,28,62],[29,62,30,62],[37,68,38,68],[35,63,36,63],[35,68,36,68],[41,86,42,86],[43,63,44,63],[43,68,44,68],[35,87,36,87],[37,87,38,87],[35,85,36,85],[35,86,36,86],[37,85,38,85],[37,86,38,86],[41,87,42,87],[45,58,46,58],[45,60,46,61],[45,62,46,62],[45,63,46,63],[47,59,48,59],[49,59,50,59],[51,59,52,59],[51,60,52,61],[47,62,48,62],[47,63,48,63],[49,58,50,58],[47,60,48,61],[49,63,50,63],[51,85,52,85],[51,86,52,86],[51,87,52,87],[35,60,36,61],[49,85,50,85],[49,86,50,86],[49,87,50,87],[39,58,40,58],[37,63,38,63],[49,68,50,68],[47,68,48,68],[47,85,48,85],[47,86,48,86],[47,87,48,87],[39,62,40,62],[39,63,40,63],[35,62,36,62],[49,60,50,61],[49,62,50,62],[43,85,44,85],[43,86,44,86],[43,87,44,87],[43,88,44,88],[43,89,44,89],[35,98,36,98],[35,95,36,95],[35,94,36,94],[35,100,36,100],[37,89,38,89],[37,90,38,90],[37,91,38,91],[37,93,38,93],[43,90,44,90],[43,91,44,91],[43,93,44,93],[35,89,36,89],[41,90,42,90],[37,95,38,95],[39,98,40,98],[39,94,40,94],[37,98,38,98],[37,99,38,99],[37,94,38,94],[37,100,38,100],[39,93,40,93],[41,88,42,88],[41,85,42,85],[37,88,38,88],[39,89,40,89],[39,90,40,90],[39,91,40,91],[29,103,30,103],[31,103,32,103],[27,99,28,99],[29,99,30,99],[41,102,42,102],[37,102,38,102],[39,101,40,101],[41,101,42,101],[29,102,30,102],[39,99,40,99],[39,100,40,100],[33,100,34,100],[33,90,34,90],[33,91,34,91],[33,93,34,93],[33,94,34,94],[33,95,34,95],[35,96,36,96],[35,97,36,97],[29,100,30,100],[33,98,34,98],[33,99,34,99],[41,98,42,98],[41,99,42,99],[41,100,42,100],[41,94,42,94],[27,91,28,91],[29,91,30,91],[27,92,28,92],[29,92,30,92],[31,92,32,92],[33,92,34,92],[43,102,44,102],[43,103,44,103],[43,104,44,104],[43,101,44,101],[43,94,44,94],[43,95,44,95],[43,96,44,96],[43,97,44,97],[43,98,44,98],[43,99,44,99],[43,100,44,100],[33,102,34,102],[33,103,34,103],[37,104,38,104],[41,104,42,104],[37,103,38,103],[41,103,42,103],[39,104,40,104],[39,102,40,102],[39,103,40,103],[41,97,42,97],[45,88,46,88],[45,89,46,89],[45,90,46,90],[45,91,46,91],[45,93,46,93],[45,94,46,94],[45,95,46,95],[45,96,46,96],[45,97,46,97],[47,88,48,88],[47,89,48,89],[47,90,48,90],[47,91,48,91],[47,93,48,93],[47,94,48,94],[47,95,48,95],[47,96,48,96],[47,97,48,97],[49,104,50,104],[51,98,52,98],[51,99,52,99],[51,100,52,100],[49,98,50,98],[49,99,50,99],[49,100,50,100],[49,102,50,102],[49,103,50,103],[47,102,48,102],[47,103,48,103],[47,104,48,104],[45,104,46,104],[47,98,48,98],[47,99,48,99],[45,101,46,101],[47,101,48,101],[49,101,50,101],[51,101,52,101],[47,100,48,100],[45,98,46,98],[45,99,46,99],[45,100,46,100],[57,86,58,86],[57,87,58,87],[53,98,54,98],[53,99,54,99],[53,100,54,100],[57,95,58,95],[57,96,58,96],[57,97,58,97],[57,98,58,98],[57,99,58,99],[57,100,58,100],[57,94,58,94],[57,88,58,88],[53,96,54,96],[53,97,54,97],[55,95,56,95],[55,96,56,96],[53,91,54,91],[53,93,54,93],[55,88,56,88],[55,89,56,89],[55,90,56,90],[55,91,56,91],[55,93,56,93],[57,104,58,104],[49,94,50,94],[55,102,56,102],[55,103,56,103],[55,104,56,104],[57,102,58,102],[57,103,58,103],[53,104,54,104],[53,94,54,94],[53,95,54,95],[53,102,54,102],[53,103,54,103],[55,94,56,94],[33,97,34,97],[27,97,28,97],[37,96,38,96],[37,97,38,97],[39,95,40,95],[39,96,40,96],[39,97,40,97],[41,95,42,95],[41,96,42,96],[33,96,34,96],[53,101,54,101],[55,101,56,101],[57,101,58,101],[55,100,56,100],[45,102,46,102],[45,103,46,103],[51,102,52,102],[51,103,52,103],[51,104,52,104],[1,134,2,134],[1,128,1,130],[1,131,1,133],[64,0,64,12],[65,0,65,12],[1,127,2,127],[57,89,58,89],[57,90,58,90],[57,91,58,91],[57,93,58,93],[55,85,56,85],[55,86,56,86],[55,87,56,87],[51,21,51,22],[56,21,56,22],[57,21,57,22],[58,21,58,22],[52,21,52,22],[53,21,53,22],[53,88,54,88],[53,89,54,89],[1,0,2,11],[53,90,54,90],[39,92,40,92],[41,92,42,92],[43,92,44,92],[45,92,46,92],[47,92,48,92],[49,92,50,92],[51,92,52,92],[17,92,18,92],[19,92,20,92],[13,101,14,101],[15,101,16,101],[17,101,18,101],[19,101,20,101],[21,101,22,101],[23,101,24,101],[25,101,26,101],[27,101,28,101],[29,101,30,101],[31,101,32,101],[33,101,34,101],[35,101,36,101],[37,101,38,101],[51,88,52,88],[51,89,52,89],[51,90,52,90],[51,91,52,91],[49,88,50,88],[49,89,50,89],[49,90,50,90],[49,91,50,91],[51,93,52,93],[51,94,52,94],[51,95,52,95],[51,96,52,96],[51,97,52,97],[49,93,50,93],[49,95,50,95],[49,96,50,96],[49,97,50,97],[35,92,36,92],[37,92,38,92],[74,6,74,12],[75,6,75,12],[81,10,81,12],[53,92,54,92],[55,92,56,92],[57,92,58,92],[55,97,56,97],[55,98,56,98],[55,99,56,99],[59,60,59,61],[57,68,58,68],[55,58,56,58],[55,59,56,59],[55,60,56,61],[55,62,56,62],[55,63,56,63],[55,68,56,68],[72,0,72,12],[73,0,73,12],[79,0,79,12],[80,0,80,12],[81,2,81,3],[81,4,81,5],[81,6,81,7]],"merged_total":1040,"flags":["merged_cut"]}
["Quality Assurance Checks",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Baseline","Baseline","Proposed",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Climate Zone",{"$f":"'General Information'!C46","v":"4A"},null,"Building Type","Multifamily",{"$f":"SUMIF('General Information'!$F$17:F20,DG1,'General Information'!$X$17:X20)","v":0},{"$f":"DH1/$DH$10","v":{"$error":"#DIV/0!"}},null,null,null,null,"Performance Path Review Manual Appendix B: Typical Building Operating Schedules ",null,null,null,null,null,null,null,null,null,"Performance Path Review Table 1: Site EUI kBtu/SF – YR of Common Commercial Building Designs "]
["Note: Please complete all previous worksheets to the fullest. The typical  EUI's and full load hours used in the Quality Assurance Checks are based on the PNNL Prototype Models (link) and the related analysis (link).  The COMNET Appendix-C Schedules are also used for typical  EUI's and full load hours referenced (link). For building types not noted in the 'General Information' tab, the average EFLH of all building types have been used.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Proposed","ASHRAE 90.1-2004","ASHRAE 90.1-2013",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Project Area",{"$f":"BuildingArea","v":0},null,null,"Retail",{"$f":"SUMIF('General Information'!$F$17:F20,DG2,'General Information'!$X$17:X20)","v":0},{"$f":"DH2/$DH$10","v":{"$error":"#DIV/0!"}},null,null,null,"BPF Building Types",null,null,"Occupancy","Lights","Receptacle","Infiltration","HVAC Avail","Service Hot Water",null,null,null,"90.1 2004 Site EUI (PRM)",null,null,"90.1 2013 Site EUI (ECB)",null,null,"Misc. Equipment"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"90.1-2004",null,null,null,null,null,null,null,null,"90.1-2013",null,null,null,null,null,null,null,null,"90.1-2004","90.1-2013",null,null,null,null,null,"Office",{"$f":"SUMIF('General Information'!$F$17:F20,DG3,'General Information'!$X$17:X20)","v":0},{"$f":"DH3/$DH$10","v":{"$error":"#DIV/0!"}},null,null,null,null,"Assembly","Max Sch Fraction",0.8,0.65,0.75,1,"n/a",0.65,null,null,null,"4A","5A","6A","4A","5A","6A"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HIDE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Baseline",null,null,null,null,"Proposed",null,null,null,null,"Office","Retail","School","Healthcare/hospital","Restaurant","Hotel/motel","Warehouse","All Others","Multifamily","Office","Retail","School","Healthcare/hospital","Restaurant","Hotel/motel","Warehouse","All Others","Multifamily","Weighted Average for building types","Weighted Average for building types",null,null,null,null,null,"School",{"$f":"SUMIF('General Information'!$F$17:F20,DG4,'General Information'!$X$17:X20)","v":0},{"$f":"DH4/$DH$10","v":{"$error":"#DIV/0!"}},null,null,null,null,null,"Min Sch Fraction",0,0.05,0.05,0.25,"n/a",0,null,null,"Multifamily NYStretch "]
["Performance Summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Baseline","Baseline","Baseline","Baseline","Baseline","Baseline","Baseline","Proposed","Proposed","Proposed","Proposed","Proposed","Proposed","Proposed","Proposed","Proposed","Proposed","90.1-2004","90.1-2013",null,null,null,"Simple Breakdown used in graphs","PNNL End Use Equivalent","Performance Outputs End Use",null,"Unregulated?","Energy Type","Units of \nAnnual Energy and Peak Demand","Baseline","Proposed","Energy / Demand Savings \nper End-Use","End Use \nPercent Contribution to Total Energy Savings","End Use \nPercent \nContribution to \nTotal Cost Savings","Percent of Total Proposed  \nSite Energy Consumption","Site Energy Conversion Factor","Source Energy Conversion Factor","Baseline $/Energy Type","Proposed $/Energy Type",{"$f":"\"Site Energy Use \"&'12 - Performance_Outputs_1'!PO_SiteUnits","v":"Site Energy Use Btu x 10^6"},"Site EUI (kBtu/sf/yr)",{"$f":"\"Source Energy Use \"&'12 - Performance_Outputs_1'!PO_SourceUnits","v":"Source Energy Use Btu x 10^6"},"Source EUI (kBtu/sf/yr)","Cost $",{"$f":"\"Site Energy Use \"&'12 - Performance_Outputs_1'!PO_SiteUnits","v":"Site Energy Use Btu x 10^6"},"Site EUI (kBtu/sf/yr)",{"$f":"\"Source Energy Use \"&'12 - Performance_Outputs_1'!PO_SourceUnits","v":"Source Energy Use Btu x 10^6"},"Source EUI (kBtu/sf/yr)","Cost $","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)",null,null,null,null,null,"Healthcare/hospital",{"$f":"SUMIF('General Information'!$F$17:F20,DG5,'General Information'!$X$17:X20)","v":0},{"$error":"#DIV/0!"},null,null,null,null,null,"EFLH",2606,3340,3839,3918,6456,312,null,"Multifamily","Multifamily High-rise",54,63,65,46,52,53,13]
["Note: Graphs will only be visable if the Building Type and Area are entered in the 'General Information' tab.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Simple Breakdown",{"$f":"\"Site Energy Use \"&'12 - Performance_Outputs_1'!PO_SiteUnits","v":"Site Energy Use Btu x 10^6"},"Site EUI (kBtu/sf/yr)",{"$f":"\"Source Energy Use \"&'12 - Performance_Outputs_1'!PO_SourceUnits","v":"Source Energy Use Btu x 10^6"},"Source EUI (kBtu/sf/yr)","Cost $","Cost Intensity $/sf","% Energy Site EUI Savings VS 90.1-2004\nper End-Use",{"$f":"\"Site Energy Use \"&'12 - Performance_Outputs_1'!PO_SiteUnits","v":"Site Energy Use Btu x 10^6"},"Site EUI (kBtu/sf/yr)",{"$f":"\"Source Energy Use \"&'12 - Performance_Outputs_1'!PO_SourceUnits","v":"Source Energy Use Btu x 10^6"},"Source EUI (kBtu/sf/yr)","Cost $","Cost Intensity $/sf","% Energy Cost Savings \nper End-Use","% Energy Site EUI Savings \nper End-Use","% Energy Source EUI Savings \nper End-Use","% Energy Site EUI Savings VS 90.1-2013\nper End-Use","Weighted Average for multiple building types Site EUI (kBtu/sf/yr)","Weighted Average for multiple building types Site EUI (kBtu/sf/yr)",null,null,null,"Lighting, Interior","Lighting, Interior",{"$f":"'12 - Performance_Outputs_1'!B209","v":"Interior lighting"},null,{"$f":"'12 - Performance_Outputs_1'!D209","v":0},{"$f":"'12 - Performance_Outputs_1'!E209","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F209","v":""},{"$f":"'12 - Performance_Outputs_1'!G209","v":""},{"$f":"'12 - Performance_Outputs_1'!H209","v":0},{"$f":"'12 - Performance_Outputs_1'!I209","v":""},{"$f":"'12 - Performance_Outputs_1'!J209","v":""},{"$f":"'12 - Performance_Outputs_1'!K209","v":""},{"$f":"'12 - Performance_Outputs_1'!M209","v":""},{"$f":"'12 - Performance_Outputs_1'!Q209","v":""},{"$f":"'12 - Performance_Outputs_1'!R209","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL6,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL6,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},{"$f":"IFERROR(BN6*BT6,\"\")","v":""},{"$f":"IFERROR((BX6*1000)/$DD$2,\"\")","v":""},{"$f":"IFERROR(BN6*BU6,\"\")","v":""},{"$f":"IFERROR((BZ6*1000)/$DD$2,\"\")","v":""},{"$f":"IFERROR(BN6*BV6,\"\")","v":""},{"$f":"IFERROR(BO6*BT6,\"\")","v":""},{"$f":"IFERROR((CC6*1000)/$DD$2,\"\")","v":""},{"$f":"IFERROR(BO6*BU6,\"\")","v":""},{"$f":"IFERROR((CE6*1000)/$DD$2,\"\")","v":""},{"$f":"IFERROR(BO6*BW6,\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":10.346389795103857},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":22.933104120205343},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":15.178241616130954},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":15.334119686091013},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":29.932931024841526},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":11.144597124202233},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":8.7793392059999995},{"$f":"AVERAGE(CH6:CN7,CP6)","v":14.616267591612452},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":3.2814181603246695},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":6.5837248324848296},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":17.695740665149014},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":8.6481704765469498},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":12.762687297625098},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":12.232911734635278},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":7.0590533221162142},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":5.6305372829999998},{"$f":"AVERAGE(CQ6:CW7,CY6)","v":9.2087335800661734},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH6,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH6,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH6,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":3.0570430289720014},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH6:CP7)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH6:CP7)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH6:CP7)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH6:CP7)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH6:CP7)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH6:CP7)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH6:CP7)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH6:CP7)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH6:CP7)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH6:CP7)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ6:CY7)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ6:CY7)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ6:CY7)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ6:CY7)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ6:CY7)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ6:CY7)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ6:CY7)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ6:CY7)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ6:CY7)*$DI$9","v":{"$error":"#DIV/0!"}},null,null,null,null,null,"Restaurant",{"$f":"SUMIF('General Information'!$F$17:F20,DG6,'General Information'!$X$17:X20)","v":0},{"$error":"#DIV/0!"},null,null,null,null,"Health","Max Sch Fraction",0.8,0.9,0.9,0.25,"n/a",0.82,null,"Healthcare/hospital","Hospital",172,174,182,124,127,128,50]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lighting, Interior",{"$f":"SUMIF($BG:$BG,AJ7,$BX:$BX)","v":0},{"$f":"SUMIF($BG:$BG,AJ7,$BY:$BY)","v":0},{"$f":"SUMIF($BG:$BG,AJ7,$BZ:$BZ)","v":0},{"$f":"SUMIF($BG:$BG,AJ7,$CA:$CA)","v":0},{"$f":"SUMIF($BG:$BG,AJ7,$CB:$CB)","v":0},{"$f":"AO7/$DD$2","v":{"$error":"#DIV/0!"}},{"$f":"IFERROR((BB7-AL7)/$AQ$16,\"\")","v":""},{"$f":"SUMIF($BG:$BG,AJ7,$CC:$CC)","v":0},{"$f":"SUMIF($BG:$BG,AJ7,$CD:$CD)","v":0},{"$f":"SUMIF($BG:$BG,AJ7,$CE:$CE)","v":0},{"$f":"SUMIF($BG:$BG,AJ7,$CF:$CF)","v":0},{"$f":"SUMIF($BG:$BG,AJ7,$CG:$CG)","v":0},{"$f":"AV7/$DD$2","v":{"$error":"#DIV/0!"}},{"$f":"IFERROR((AO7-AV7)/$AX$16,\"N/A\")","v":"N/A"},{"$f":"IFERROR((AL7-AS7)/$AY$16,\"\")","v":""},{"$f":"IFERROR((AN7-AU7)/$AZ$16,\"\")","v":""},{"$f":"IFERROR((BC7-AS7)/$BA$16,\"\")","v":""},{"$f":"SUMIF($BG:$BG,AJ7,$CZ:$CZ)","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($BG:$BG,AJ7,$DA:$DA)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F210","v":""},{"$f":"'12 - Performance_Outputs_1'!G210","v":""},{"$f":"'12 - Performance_Outputs_1'!H210","v":0},{"$f":"'12 - Performance_Outputs_1'!I210","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K210","v":0},{"$f":"'12 - Performance_Outputs_1'!M210","v":0},{"$f":"'12 - Performance_Outputs_1'!Q210","v":""},{"$f":"'12 - Performance_Outputs_1'!R210","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL7,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL7,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hotel/motel",{"$f":"SUMIF('General Information'!$F$17:F20,DG7,'General Information'!$X$17:X20)","v":0},{"$error":"#DIV/0!"},null,null,null,null,null,"Min Sch Fraction",0.4,0.5,0.4,0.25,"n/a",0.15,null,"Hotel/motel","Large Hotel",118,132,134,86,90,90,37]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lighting, Exterior",0,0,0,0,0,{"$error":"#DIV/0!"},"",0,0,0,0,0,{"$error":"#DIV/0!"},"N/A","","","",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,null,"Lighting, Interior","Lighting, Interior",{"$f":"'12 - Performance_Outputs_1'!B211","v":"Lighting in Apartments"},null,{"$f":"'12 - Performance_Outputs_1'!D211","v":0},{"$f":"'12 - Performance_Outputs_1'!E211","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F211","v":""},{"$f":"'12 - Performance_Outputs_1'!G211","v":""},{"$f":"'12 - Performance_Outputs_1'!H211","v":0},{"$f":"'12 - Performance_Outputs_1'!I211","v":""},{"$f":"'12 - Performance_Outputs_1'!J211","v":""},{"$f":"'12 - Performance_Outputs_1'!K211","v":""},{"$f":"'12 - Performance_Outputs_1'!M211","v":""},{"$f":"'12 - Performance_Outputs_1'!Q211","v":""},{"$f":"'12 - Performance_Outputs_1'!R211","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL8,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL8,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Warehouse",{"$f":"SUMIF('General Information'!$F$17:F20,DG8,'General Information'!$X$17:X20)","v":0},{"$error":"#DIV/0!"},null,null,null,"Healthcare/hospital",null,"EFLH",4691,5438,5169,2190,8760,2751,null,null,"Large Office",83,87,87,70,74,75,42]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHW",0,0,0,0,0,{"$error":"#DIV/0!"},"",0,0,0,0,0,{"$error":"#DIV/0!"},"N/A","","","",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F212","v":""},{"$f":"'12 - Performance_Outputs_1'!G212","v":""},{"$f":"'12 - Performance_Outputs_1'!H212","v":0},{"$f":"'12 - Performance_Outputs_1'!I212","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K212","v":0},{"$f":"'12 - Performance_Outputs_1'!M212","v":0},{"$f":"'12 - Performance_Outputs_1'!Q212","v":""},{"$f":"'12 - Performance_Outputs_1'!R212","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL9,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL9,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"All Others",{"$f":"SUMIF('General Information'!$F$17:F20,DG9,'General Information'!$X$17:X20)","v":0},{"$error":"#DIV/0!"},null,null,null,null,"Hotel","Max Sch Fraction",0.9,0.9,0.9,0.25,"n/a",0.8,null,null,"Medium Office",45,50,51,32,35,36,16]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heat",0,0,0,0,0,{"$error":"#DIV/0!"},"",0,0,0,0,0,{"$error":"#DIV/0!"},"N/A","","","",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,null,{"$f":"IF(BK10=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Other",{"$f":"'12 - Performance_Outputs_1'!B213","v":"Interior lighting - process"},null,{"$f":"'12 - Performance_Outputs_1'!D213","v":"x"},{"$f":"'12 - Performance_Outputs_1'!E213","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F213","v":""},{"$f":"'12 - Performance_Outputs_1'!G213","v":""},{"$f":"'12 - Performance_Outputs_1'!H213","v":""},{"$f":"'12 - Performance_Outputs_1'!I213","v":""},{"$f":"'12 - Performance_Outputs_1'!J213","v":""},{"$f":"'12 - Performance_Outputs_1'!K213","v":""},{"$f":"'12 - Performance_Outputs_1'!M213","v":""},{"$f":"'12 - Performance_Outputs_1'!Q213","v":""},{"$f":"'12 - Performance_Outputs_1'!R213","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL10,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL10,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(DH1:DH9)","v":0},null,null,null,null,null,null,"Min Sch Fraction",0.2,0.1,0.1,0.25,"n/a",0,null,"Office","Average Office",{"$f":"AVERAGE(DY8:DY9)","v":64},{"$f":"AVERAGE(DZ8:DZ9)","v":68.5},69,51,54.5,55.5,29]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cool",0,0,0,0,0,{"$error":"#DIV/0!"},"",0,0,0,0,0,{"$error":"#DIV/0!"},"N/A","","","",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F214","v":""},{"$f":"'12 - Performance_Outputs_1'!G214","v":""},{"$f":"'12 - Performance_Outputs_1'!H214","v":""},{"$f":"'12 - Performance_Outputs_1'!I214","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K214","v":0},{"$f":"'12 - Performance_Outputs_1'!M214","v":0},{"$f":"'12 - Performance_Outputs_1'!Q214","v":""},{"$f":"'12 - Performance_Outputs_1'!R214","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL11,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL11,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hotel/motel",null,"EFLH",5074,3285,3285,2190,8760,2628,null,null,"Primary School",79,86,89,55,57,58,25]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fans",0,0,0,0,0,{"$error":"#DIV/0!"},"",0,0,0,0,0,{"$error":"#DIV/0!"},"N/A","","","",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,null,"Lighting, Exterior","Lighting, Exterior",{"$f":"'12 - Performance_Outputs_1'!B215","v":"Exterior lighting"},null,{"$f":"'12 - Performance_Outputs_1'!D215","v":0},{"$f":"'12 - Performance_Outputs_1'!E215","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F215","v":""},{"$f":"'12 - Performance_Outputs_1'!G215","v":""},{"$f":"'12 - Performance_Outputs_1'!H215","v":0},{"$f":"'12 - Performance_Outputs_1'!I215","v":""},{"$f":"'12 - Performance_Outputs_1'!J215","v":""},{"$f":"'12 - Performance_Outputs_1'!K215","v":""},{"$f":"'12 - Performance_Outputs_1'!M215","v":""},{"$f":"'12 - Performance_Outputs_1'!Q215","v":""},{"$f":"'12 - Performance_Outputs_1'!R215","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL12,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL12,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":3.0691872327839342},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":5.2735187295148691},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.0425673246761784},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":3.0514922078500155},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":10.221117620326261},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":2.2681461608807667},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":2.2493003680000001},{"$f":"AVERAGE(CH12:CN13,CP12)","v":3.6757269457766624},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":2.2304859221812725},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.6128319360827217},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":2.7095166099165549},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.55863268544411293},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.6532751282979818},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":5.7889910213048683},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.670125403482621},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.5046340330000001},{"$f":"AVERAGE(CQ12:CW13,CY12)","v":2.123755843997444},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH12,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH12,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH12,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.4920399344506905},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH12:CP13)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH12:CP13)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH12:CP13)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH12:CP13)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH12:CP13)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH12:CP13)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH12:CP13)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH12:CP13)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH12:CP13)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH12:CP13)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ12:CY13)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ12:CY13)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ12:CY13)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ12:CY13)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ12:CY13)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ12:CY13)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ12:CY13)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ12:CY13)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ12:CY13)*$DI$9","v":{"$error":"#DIV/0!"}},null,null,"General Info Building Type Options",null,null,"PNNL Building Type Options",null,null,null,null,null,null,"Office","Max Sch Fraction",0.95,0.9,0.9,1,"n/a",0.56999999999999995,null,null,"Secondary School",73,74,74,39,40,40,15]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pumps",0,0,0,0,0,{"$error":"#DIV/0!"},"",0,0,0,0,0,{"$error":"#DIV/0!"},"N/A","","","",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F216","v":""},{"$f":"'12 - Performance_Outputs_1'!G216","v":""},{"$f":"'12 - Performance_Outputs_1'!H216","v":0},{"$f":"'12 - Performance_Outputs_1'!I216","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K216","v":0},{"$f":"'12 - Performance_Outputs_1'!M216","v":0},{"$f":"'12 - Performance_Outputs_1'!Q216","v":""},{"$f":"'12 - Performance_Outputs_1'!R216","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL13,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL13,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Office",null,null,"Apartments","Mid Rise",null,null,null,null,null,null,"Min Sch Fraction",0,0.05,0.4,0.25,"n/a",0.05,null,"School","Average School",{"$f":"AVERAGE(DY11:DY12)","v":76},{"$f":"AVERAGE(DZ11:DZ12)","v":80},{"$f":"AVERAGE(EA11:EA12)","v":81.5},{"$f":"AVERAGE(EB11:EB12)","v":47},{"$f":"AVERAGE(EC11:EC12)","v":48.5},{"$f":"AVERAGE(ED11:ED12)","v":49},{"$f":"AVERAGE(EE11:EE12)","v":20}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Other Regulated",0,0,0,0,0,{"$error":"#DIV/0!"},"",0,0,0,0,0,{"$error":"#DIV/0!"},"N/A","","","",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,null,"Heat","Heating",{"$f":"'12 - Performance_Outputs_1'!B217","v":"Space heating"},null,{"$f":"'12 - Performance_Outputs_1'!D217","v":0},{"$f":"'12 - Performance_Outputs_1'!E217","v":"Natural Gas"},{"$f":"'12 - Performance_Outputs_1'!F217","v":""},{"$f":"'12 - Performance_Outputs_1'!G217","v":""},{"$f":"'12 - Performance_Outputs_1'!H217","v":0},{"$f":"'12 - Performance_Outputs_1'!I217","v":""},{"$f":"'12 - Performance_Outputs_1'!J217","v":""},{"$f":"'12 - Performance_Outputs_1'!K217","v":""},{"$f":"'12 - Performance_Outputs_1'!M217","v":""},{"$f":"'12 - Performance_Outputs_1'!Q217","v":""},{"$f":"'12 - Performance_Outputs_1'!R217","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL14,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL14,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":7.7213184967989559},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":23.399308867478489},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":16.721903298069389},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":47.963188363666639},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":154.40523239224049},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":18.276374822577438},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":12.242857860000001},{"$f":"AVERAGE(CH14:CN15,CP14)","v":36.415650211394087},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":10.595017590321277},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":4.472213790931705},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":9.3313557843939492},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":7.7633348858296269},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":23.923884826430236},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":130.25461207438008},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":7.7733835023083353},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":7.4089814379999996},{"$f":"AVERAGE(CQ14:CW15,CY14)","v":24.613214979513948},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH14,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH14,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH14,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":5.9779535338376331},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH14:CP15)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH14:CP15)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH14:CP15)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH14:CP15)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH14:CP15)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH14:CP15)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH14:CP15)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH14:CP15)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH14:CP15)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH14:CP15)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ14:CY15)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ14:CY15)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ14:CY15)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ14:CY15)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ14:CY15)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ14:CY15)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ14:CY15)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ14:CY15)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ14:CY15)*$DI$9","v":{"$error":"#DIV/0!"}},null,null,"Retail",null,null,null,"High Rise",null,null,null,null,"Office",null,"EFLH",2450,2856,4425,5280,4640,1551]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Other Non-Regulated",0,0,0,0,0,{"$error":"#DIV/0!"},"",0,0,0,0,0,{"$error":"#DIV/0!"},"N/A","","","",{"$error":"#DIV/0!"},{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F218","v":""},{"$f":"'12 - Performance_Outputs_1'!G218","v":""},{"$f":"'12 - Performance_Outputs_1'!H218","v":""},{"$f":"'12 - Performance_Outputs_1'!I218","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K218","v":0},{"$f":"'12 - Performance_Outputs_1'!M218","v":0},{"$f":"'12 - Performance_Outputs_1'!Q218","v":""},{"$f":"'12 - Performance_Outputs_1'!R218","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL15,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL15,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"School",null,null,"Healthcare","Hospital",null,null,null,null,null,"Parking","Max Sch Fraction",0,1,1,1,"n/a","n/a"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AK7:AK15)","v":0},{"$f":"SUM(AL7:AL15)","v":0},{"$f":"SUM(AM7:AM15)","v":0},{"$f":"SUM(AN7:AN15)","v":0},{"$f":"SUM(AO7:AO15)","v":0},null,{"$f":"BB16-AL16","v":{"$error":"#DIV/0!"}},{"$f":"SUM(AR7:AR15)","v":0},{"$f":"SUM(AS7:AS15)","v":0},{"$f":"SUM(AT7:AT15)","v":0},{"$f":"SUM(AU7:AU15)","v":0},{"$f":"SUM(AV7:AV15)","v":0},null,{"$f":"AO16-AV16","v":0},{"$f":"AL16-AS16","v":0},{"$f":"AN16-AU16","v":0},{"$f":"BC16-AS16","v":{"$error":"#DIV/0!"}},{"$f":"SUM(BB7:BB15)","v":{"$error":"#DIV/0!"}},{"$f":"SUM(BC7:BC15)","v":{"$error":"#DIV/0!"}},null,null,null,"Heat","Heating",{"$f":"'12 - Performance_Outputs_1'!B219","v":"Space heating"},null,{"$f":"'12 - Performance_Outputs_1'!D219","v":0},{"$f":"'12 - Performance_Outputs_1'!E219","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F219","v":""},{"$f":"'12 - Performance_Outputs_1'!G219","v":""},{"$f":"'12 - Performance_Outputs_1'!H219","v":0},{"$f":"'12 - Performance_Outputs_1'!I219","v":""},{"$f":"'12 - Performance_Outputs_1'!J219","v":""},{"$f":"'12 - Performance_Outputs_1'!K219","v":""},{"$f":"'12 - Performance_Outputs_1'!M219","v":""},{"$f":"'12 - Performance_Outputs_1'!Q219","v":""},{"$f":"'12 - Performance_Outputs_1'!R219","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL16,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL16,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Healthcare/hospital",null,null,null,"Clinic",null,null,null,null,null,null,"Min Sch Fraction",0,0.5,1,1,"n/a","n/a"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F220","v":""},{"$f":"'12 - Performance_Outputs_1'!G220","v":""},{"$f":"'12 - Performance_Outputs_1'!H220","v":0},{"$f":"'12 - Performance_Outputs_1'!I220","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K220","v":0},{"$f":"'12 - Performance_Outputs_1'!M220","v":0},{"$f":"'12 - Performance_Outputs_1'!Q220","v":""},{"$f":"'12 - Performance_Outputs_1'!R220","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL17,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL17,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Restaurant",null,null,"Hotel","Large",null,null,null,null,null,null,"EFLH",0,6674,8760,8760,"n/a","n/a"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heat","Heating",{"$f":"'12 - Performance_Outputs_1'!B221","v":"Heat Pump Supplementary"},null,{"$f":"'12 - Performance_Outputs_1'!D221","v":0},{"$f":"'12 - Performance_Outputs_1'!E221","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F221","v":""},{"$f":"'12 - Performance_Outputs_1'!G221","v":""},{"$f":"'12 - Performance_Outputs_1'!H221","v":0},{"$f":"'12 - Performance_Outputs_1'!I221","v":""},{"$f":"'12 - Performance_Outputs_1'!J221","v":""},{"$f":"'12 - Performance_Outputs_1'!K221","v":""},{"$f":"'12 - Performance_Outputs_1'!M221","v":""},{"$f":"'12 - Performance_Outputs_1'!Q221","v":""},{"$f":"'12 - Performance_Outputs_1'!R221","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL18,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL18,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hotel/motel",null,null,null,"Small",null,null,null,null,null,"Retail","Max Sch Fraction",0.8,0.9,0.9,1,"n/a",0.62]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F222","v":""},{"$f":"'12 - Performance_Outputs_1'!G222","v":""},{"$f":"'12 - Performance_Outputs_1'!H222","v":0},{"$f":"'12 - Performance_Outputs_1'!I222","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K222","v":0},{"$f":"'12 - Performance_Outputs_1'!M222","v":0},{"$f":"'12 - Performance_Outputs_1'!Q222","v":""},{"$f":"'12 - Performance_Outputs_1'!R222","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL19,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL19,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Warehouse",null,null,"Office","Large",null,null,null,null,null,null,"Min Sch Fraction",0,0.05,0.2,0.25,"n/a",0.04]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cool","Cooling",{"$f":"'12 - Performance_Outputs_1'!B223","v":"Space cooling"},null,{"$f":"'12 - Performance_Outputs_1'!D223","v":0},{"$f":"'12 - Performance_Outputs_1'!E223","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F223","v":""},{"$f":"'12 - Performance_Outputs_1'!G223","v":""},{"$f":"'12 - Performance_Outputs_1'!H223","v":0},{"$f":"'12 - Performance_Outputs_1'!I223","v":""},{"$f":"'12 - Performance_Outputs_1'!J223","v":""},{"$f":"'12 - Performance_Outputs_1'!K223","v":""},{"$f":"'12 - Performance_Outputs_1'!M223","v":""},{"$f":"'12 - Performance_Outputs_1'!Q223","v":""},{"$f":"'12 - Performance_Outputs_1'!R223","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL20,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL20,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":8.7361699158480608},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":9.8860242087130992},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":12.547460266004832},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":21.911569317170738},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":26.734245588787488},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":13.695148470154816},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.30620941992506484},{"$f":"AVERAGE(CH20:CN21,CP20)","v":12.389386466244119},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":5.2982645433488527},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":6.2077958752173279},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":4.9887555110636326},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":6.463655209956924},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":13.521757990529828},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":16.26825179603328},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":8.547994246859604},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.12040715444327024},{"$f":"AVERAGE(CQ20:CW21,CY20)","v":7.5272701565321221},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH20,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH20,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH20,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":4.0995434681531133},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH20:CP21)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH20:CP21)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH20:CP21)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH20:CP21)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH20:CP21)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH20:CP21)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH20:CP21)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH20:CP21)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH20:CP21)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH20:CP21)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ20:CY21)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ20:CY21)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ20:CY21)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ20:CY21)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ20:CY21)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ20:CY21)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ20:CY21)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ20:CY21)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ20:CY21)*$DI$9","v":{"$error":"#DIV/0!"}},null,null,"Multifamily",null,null,null,"Medium",null,null,null,null,"Retail",null,"EFLH",2371,3558,4528,4801,5279,2305]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F224","v":""},{"$f":"'12 - Performance_Outputs_1'!G224","v":""},{"$f":"'12 - Performance_Outputs_1'!H224","v":0},{"$f":"'12 - Performance_Outputs_1'!I224","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K224","v":0},{"$f":"'12 - Performance_Outputs_1'!M224","v":0},{"$f":"'12 - Performance_Outputs_1'!Q224","v":""},{"$f":"'12 - Performance_Outputs_1'!R224","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL21,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL21,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"All Others",null,null,null,"Small",null,null,null,null,null,"School","Max Sch Fraction",0.95,0.9,0.95,1,"n/a",0.83]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cool","Cooling",{"$f":"'12 - Performance_Outputs_1'!B225","v":"Space cooling"},null,{"$f":"'12 - Performance_Outputs_1'!D225","v":0},{"$f":"'12 - Performance_Outputs_1'!E225","v":"Natural Gas"},{"$f":"'12 - Performance_Outputs_1'!F225","v":""},{"$f":"'12 - Performance_Outputs_1'!G225","v":""},{"$f":"'12 - Performance_Outputs_1'!H225","v":0},{"$f":"'12 - Performance_Outputs_1'!I225","v":""},{"$f":"'12 - Performance_Outputs_1'!J225","v":""},{"$f":"'12 - Performance_Outputs_1'!K225","v":""},{"$f":"'12 - Performance_Outputs_1'!M225","v":""},{"$f":"'12 - Performance_Outputs_1'!Q225","v":""},{"$f":"'12 - Performance_Outputs_1'!R225","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL22,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL22,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dining","Restaurant",null,null,null,null,null,null,"Min Sch Fraction",0,0.18,0.35,0.25,"n/a",0.05]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F226","v":""},{"$f":"'12 - Performance_Outputs_1'!G226","v":""},{"$f":"'12 - Performance_Outputs_1'!H226","v":""},{"$f":"'12 - Performance_Outputs_1'!I226","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K226","v":0},{"$f":"'12 - Performance_Outputs_1'!M226","v":0},{"$f":"'12 - Performance_Outputs_1'!Q226","v":""},{"$f":"'12 - Performance_Outputs_1'!R226","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL23,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL23,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fast Food",null,null,null,null,"School",null,"EFLH",2096,4107,4421,6125,3514,1828]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pumps","Pumps",{"$f":"'12 - Performance_Outputs_1'!B227","v":"Pumps"},null,{"$f":"'12 - Performance_Outputs_1'!D227","v":0},{"$f":"'12 - Performance_Outputs_1'!E227","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F227","v":""},{"$f":"'12 - Performance_Outputs_1'!G227","v":""},{"$f":"'12 - Performance_Outputs_1'!H227","v":0},{"$f":"'12 - Performance_Outputs_1'!I227","v":""},{"$f":"'12 - Performance_Outputs_1'!J227","v":""},{"$f":"'12 - Performance_Outputs_1'!K227","v":""},{"$f":"'12 - Performance_Outputs_1'!M227","v":""},{"$f":"'12 - Performance_Outputs_1'!Q227","v":""},{"$f":"'12 - Performance_Outputs_1'!R227","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL24,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL24,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.2797511337267915},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.46532601769583437},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":2.5424969478325656},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":3.2356248378517624E-2},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.1423261966080858},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CH24:CN25,CP24)","v":0.73627989182896947},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.42798259038996028},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.51138795029364181},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":9.4652479434983214E-2},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.2790099180951706},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":3.0381877348534963E-2},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.3410386538814954},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CQ24:CW25,CY24)","v":0.32046205193048555},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH24,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH24,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH24,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.30722553639005834},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH24:CP25)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH24:CP25)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH24:CP25)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH24:CP25)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH24:CP25)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH24:CP25)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH24:CP25)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH24:CP25)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH24:CP25)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH24:CP25)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ24:CY25)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ24:CY25)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ24:CY25)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ24:CY25)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ24:CY25)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ24:CY25)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ24:CY25)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ24:CY25)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ24:CY25)*$DI$9","v":{"$error":"#DIV/0!"}},null,null,null,null,null,"Commercial","Retail Store",null,null,null,null,null,"Residential","Max Sch Fraction",1,1,1,1,"n/a",0.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F228","v":""},{"$f":"'12 - Performance_Outputs_1'!G228","v":""},{"$f":"'12 - Performance_Outputs_1'!H228","v":0},{"$f":"'12 - Performance_Outputs_1'!I228","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K228","v":0},{"$f":"'12 - Performance_Outputs_1'!M228","v":0},{"$f":"'12 - Performance_Outputs_1'!Q228","v":""},{"$f":"'12 - Performance_Outputs_1'!R228","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL25,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL25,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Strip Mall",null,null,null,null,null,null,"Min Sch Fraction",0.25,0.1,0.4,1,"n/a",0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cool","Heat Rejection",{"$f":"'12 - Performance_Outputs_1'!B229","v":"Heat rejection"},null,{"$f":"'12 - Performance_Outputs_1'!D229","v":0},{"$f":"'12 - Performance_Outputs_1'!E229","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F229","v":""},{"$f":"'12 - Performance_Outputs_1'!G229","v":""},{"$f":"'12 - Performance_Outputs_1'!H229","v":0},{"$f":"'12 - Performance_Outputs_1'!I229","v":""},{"$f":"'12 - Performance_Outputs_1'!J229","v":""},{"$f":"'12 - Performance_Outputs_1'!K229","v":""},{"$f":"'12 - Performance_Outputs_1'!M229","v":""},{"$f":"'12 - Performance_Outputs_1'!Q229","v":""},{"$f":"'12 - Performance_Outputs_1'!R229","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL26,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL26,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.74571668046878892},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.2845573801227852},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CH26:CN27,CP26)","v":0.27044274195304824},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.13326787503281215},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.36659877546833508},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.9648257908412754},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CQ26:CW27,CY26)","v":0.18104328673659545},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH26,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH26,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH26,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.1169217275831531},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH26:CP27)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH26:CP27)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH26:CP27)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH26:CP27)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH26:CP27)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH26:CP27)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH26:CP27)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH26:CP27)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH26:CP27)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH26:CP27)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ26:CY27)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ26:CY27)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ26:CY27)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ26:CY27)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ26:CY27)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ26:CY27)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ26:CY27)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ26:CY27)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ26:CY27)*$DI$9","v":{"$error":"#DIV/0!"}},null,null,null,null,null,"School","Secondary",null,null,null,null,"Multifamily",null,"EFLH",6041,2884,5840,8760,8760,2628]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F230","v":""},{"$f":"'12 - Performance_Outputs_1'!G230","v":""},{"$f":"'12 - Performance_Outputs_1'!H230","v":0},{"$f":"'12 - Performance_Outputs_1'!I230","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K230","v":0},{"$f":"'12 - Performance_Outputs_1'!M230","v":0},{"$f":"'12 - Performance_Outputs_1'!Q230","v":""},{"$f":"'12 - Performance_Outputs_1'!R230","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL27,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL27,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Primary",null,null,null,null,null,null,"EFLH AVG",{"$f":"AVERAGE(DP5,DP8,DP11,DP14,DP17,DP20,DP23,DP26)","v":3166.125},{"$f":"AVERAGE(DQ5,DQ8,DQ11,DQ14,DQ17,DQ20,DQ23,DQ26)","v":4017.75},5033.375,5253,6595.5714285714284,2000.4285714285713]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fans","Fans",{"$f":"'12 - Performance_Outputs_1'!B231","v":"Fans - interior ventilation"},null,{"$f":"'12 - Performance_Outputs_1'!D231","v":0},{"$f":"'12 - Performance_Outputs_1'!E231","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F231","v":""},{"$f":"'12 - Performance_Outputs_1'!G231","v":""},{"$f":"'12 - Performance_Outputs_1'!H231","v":0},{"$f":"'12 - Performance_Outputs_1'!I231","v":""},{"$f":"'12 - Performance_Outputs_1'!J231","v":""},{"$f":"'12 - Performance_Outputs_1'!K231","v":""},{"$f":"'12 - Performance_Outputs_1'!M231","v":""},{"$f":"'12 - Performance_Outputs_1'!Q231","v":""},{"$f":"'12 - Performance_Outputs_1'!R231","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL28,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL28,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":3.8095134541658155},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":12.729914269774136},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":9.4561441835324658},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":15.362017124212688},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":49.095887053401192},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":9.7856098171434933},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.83920689941396864},{"$f":"AVERAGE(CH28:CN29,CP28)","v":13.509018899093979},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":6.9938583911080787},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":3.3851032090817537},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":6.7137552567045296},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":5.4477667415682918},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":10.879851846713606},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":20.213996097458459},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":6.3479324889397004},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.40111430262273029},{"$f":"AVERAGE(CQ28:CW29,CY28)","v":7.4353189951514675},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH28,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH28,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH28,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":6.093032018122674},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH28:CP29)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH28:CP29)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH28:CP29)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH28:CP29)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH28:CP29)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH28:CP29)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH28:CP29)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH28:CP29)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH28:CP29)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH28:CP29)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ28:CY29)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ28:CY29)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ28:CY29)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ28:CY29)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ28:CY29)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ28:CY29)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ28:CY29)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ28:CY29)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ28:CY29)*$DI$9","v":{"$error":"#DIV/0!"}},null,null,null,null,null,"Warehouse"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F232","v":""},{"$f":"'12 - Performance_Outputs_1'!G232","v":""},{"$f":"'12 - Performance_Outputs_1'!H232","v":0},{"$f":"'12 - Performance_Outputs_1'!I232","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K232","v":0},{"$f":"'12 - Performance_Outputs_1'!M232","v":0},{"$f":"'12 - Performance_Outputs_1'!Q232","v":""},{"$f":"'12 - Performance_Outputs_1'!R232","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL29,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL29,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK30=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Other",{"$f":"'12 - Performance_Outputs_1'!B233","v":"Fans - parking garage"},null,{"$f":"'12 - Performance_Outputs_1'!D233","v":0},{"$f":"'12 - Performance_Outputs_1'!E233","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F233","v":""},{"$f":"'12 - Performance_Outputs_1'!G233","v":""},{"$f":"'12 - Performance_Outputs_1'!H233","v":""},{"$f":"'12 - Performance_Outputs_1'!I233","v":""},{"$f":"'12 - Performance_Outputs_1'!J233","v":""},{"$f":"'12 - Performance_Outputs_1'!K233","v":""},{"$f":"'12 - Performance_Outputs_1'!M233","v":""},{"$f":"'12 - Performance_Outputs_1'!Q233","v":""},{"$f":"'12 - Performance_Outputs_1'!R233","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL30,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL30,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F234","v":""},{"$f":"'12 - Performance_Outputs_1'!G234","v":""},{"$f":"'12 - Performance_Outputs_1'!H234","v":""},{"$f":"'12 - Performance_Outputs_1'!I234","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K234","v":0},{"$f":"'12 - Performance_Outputs_1'!M234","v":0},{"$f":"'12 - Performance_Outputs_1'!Q234","v":""},{"$f":"'12 - Performance_Outputs_1'!R234","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL31,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL31,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK32=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Other",{"$f":"'12 - Performance_Outputs_1'!B235","v":"Fans - Kitchen Ventilation"},null,{"$f":"'12 - Performance_Outputs_1'!D235","v":0},{"$f":"'12 - Performance_Outputs_1'!E235","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F235","v":""},{"$f":"'12 - Performance_Outputs_1'!G235","v":""},{"$f":"'12 - Performance_Outputs_1'!H235","v":""},{"$f":"'12 - Performance_Outputs_1'!I235","v":""},{"$f":"'12 - Performance_Outputs_1'!J235","v":""},{"$f":"'12 - Performance_Outputs_1'!K235","v":""},{"$f":"'12 - Performance_Outputs_1'!M235","v":""},{"$f":"'12 - Performance_Outputs_1'!Q235","v":""},{"$f":"'12 - Performance_Outputs_1'!R235","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL32,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL32,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F236","v":""},{"$f":"'12 - Performance_Outputs_1'!G236","v":""},{"$f":"'12 - Performance_Outputs_1'!H236","v":""},{"$f":"'12 - Performance_Outputs_1'!I236","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K236","v":0},{"$f":"'12 - Performance_Outputs_1'!M236","v":0},{"$f":"'12 - Performance_Outputs_1'!Q236","v":""},{"$f":"'12 - Performance_Outputs_1'!R236","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL33,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL33,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHW","DHW",{"$f":"'12 - Performance_Outputs_1'!B237","v":"Service water heating"},null,{"$f":"'12 - Performance_Outputs_1'!D237","v":0},{"$f":"'12 - Performance_Outputs_1'!E237","v":"Natural Gas"},{"$f":"'12 - Performance_Outputs_1'!F237","v":""},{"$f":"'12 - Performance_Outputs_1'!G237","v":""},{"$f":"'12 - Performance_Outputs_1'!H237","v":0},{"$f":"'12 - Performance_Outputs_1'!I237","v":""},{"$f":"'12 - Performance_Outputs_1'!J237","v":""},{"$f":"'12 - Performance_Outputs_1'!K237","v":""},{"$f":"'12 - Performance_Outputs_1'!M237","v":""},{"$f":"'12 - Performance_Outputs_1'!Q237","v":""},{"$f":"'12 - Performance_Outputs_1'!R237","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL34,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL34,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.609071482252979},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":3.2928812227832482},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":2.3967516065520873},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":3.9314641937378036},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":70.133199337239688},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":15.535056081233153},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.47871407199999999},{"$f":"AVERAGE(CH34:CN35,CP34)","v":13.644775535899093},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":11.781066291393786},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.5509212079894585},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":3.0933200927438564},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":2.310910459368483},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":3.9093730858662661},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":70.065471062730396},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":15.410226483532906},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.46341270899999998},{"$f":"AVERAGE(CQ34:CW35,CY34)","v":13.571687320747241},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH34,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH34,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH34,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":11.769863464746564},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH34:CP35)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH34:CP35)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH34:CP35)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH34:CP35)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH34:CP35)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH34:CP35)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH34:CP35)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH34:CP35)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH34:CP35)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH34:CP35)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ34:CY35)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ34:CY35)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ34:CY35)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ34:CY35)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ34:CY35)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ34:CY35)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ34:CY35)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ34:CY35)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ34:CY35)*$DI$9","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F238","v":""},{"$f":"'12 - Performance_Outputs_1'!G238","v":""},{"$f":"'12 - Performance_Outputs_1'!H238","v":""},{"$f":"'12 - Performance_Outputs_1'!I238","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K238","v":0},{"$f":"'12 - Performance_Outputs_1'!M238","v":0},{"$f":"'12 - Performance_Outputs_1'!Q238","v":""},{"$f":"'12 - Performance_Outputs_1'!R238","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL35,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL35,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK36=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Equipment",{"$f":"'12 - Performance_Outputs_1'!B239","v":"Service water heating"},null,{"$f":"'12 - Performance_Outputs_1'!D239","v":0},{"$f":"'12 - Performance_Outputs_1'!E239","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F239","v":""},{"$f":"'12 - Performance_Outputs_1'!G239","v":""},{"$f":"'12 - Performance_Outputs_1'!H239","v":0},{"$f":"'12 - Performance_Outputs_1'!I239","v":""},{"$f":"'12 - Performance_Outputs_1'!J239","v":""},{"$f":"'12 - Performance_Outputs_1'!K239","v":""},{"$f":"'12 - Performance_Outputs_1'!M239","v":""},{"$f":"'12 - Performance_Outputs_1'!Q239","v":""},{"$f":"'12 - Performance_Outputs_1'!R239","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL36,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL36,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":10.729671005935613},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":6.4126455853540234},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":11.891931488635418},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":26.662266138571098},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":10.958842983470156},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":2.5371117206263811},{"$f":"AVERAGE(CH36:CN37,CP36)","v":10.015042311810641},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":10.927869571892442},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":9.801491143932326},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":6.3079928495957018},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":10.554065946333385},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":26.176098305580936},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":10.503266156882257},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":2.4864714958209242},{"$f":"AVERAGE(CQ36:CW37,CY36)","v":9.5899668072717361},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH36,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH36,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH36,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":10.89034856002835},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH36:CP37)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH36:CP37)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH36:CP37)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH36:CP37)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH36:CP37)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH36:CP37)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH36:CP37)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH36:CP37)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH36:CP37)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH36:CP37)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ36:CY37)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ36:CY37)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ36:CY37)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ36:CY37)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ36:CY37)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ36:CY37)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ36:CY37)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ36:CY37)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ36:CY37)*$DI$9","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F240","v":""},{"$f":"'12 - Performance_Outputs_1'!G240","v":""},{"$f":"'12 - Performance_Outputs_1'!H240","v":0},{"$f":"'12 - Performance_Outputs_1'!I240","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K240","v":0},{"$f":"'12 - Performance_Outputs_1'!M240","v":0},{"$f":"'12 - Performance_Outputs_1'!Q240","v":""},{"$f":"'12 - Performance_Outputs_1'!R240","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL37,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL37,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK38=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Equipment",{"$f":"'12 - Performance_Outputs_1'!B241","v":"Misc Equipment"},null,{"$f":"'12 - Performance_Outputs_1'!D241","v":"x"},{"$f":"'12 - Performance_Outputs_1'!E241","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F241","v":""},{"$f":"'12 - Performance_Outputs_1'!G241","v":""},{"$f":"'12 - Performance_Outputs_1'!H241","v":0},{"$f":"'12 - Performance_Outputs_1'!I241","v":""},{"$f":"'12 - Performance_Outputs_1'!J241","v":""},{"$f":"'12 - Performance_Outputs_1'!K241","v":""},{"$f":"'12 - Performance_Outputs_1'!M241","v":""},{"$f":"'12 - Performance_Outputs_1'!Q241","v":""},{"$f":"'12 - Performance_Outputs_1'!R241","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL38,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL38,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},{"$f":"IFERROR(BN38*BT38,\"\")","v":""},{"$f":"IFERROR((BX38*1000)/$DD$2,\"\")","v":""},{"$f":"IFERROR(BN38*BU38,\"\")","v":""},{"$f":"IFERROR((BZ38*1000)/$DD$2,\"\")","v":""},{"$f":"IFERROR(BN38*BV38,\"\")","v":""},{"$f":"IFERROR(BO38*BT38,\"\")","v":""},{"$f":"IFERROR((CC38*1000)/$DD$2,\"\")","v":""},{"$f":"IFERROR(BO38*BU38,\"\")","v":""},{"$f":"IFERROR((CE38*1000)/$DD$2,\"\")","v":""},{"$f":"IFERROR(BO38*BW38,\"\")","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F242","v":""},{"$f":"'12 - Performance_Outputs_1'!G242","v":""},{"$f":"'12 - Performance_Outputs_1'!H242","v":""},{"$f":"'12 - Performance_Outputs_1'!I242","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K242","v":0},{"$f":"'12 - Performance_Outputs_1'!M242","v":0},{"$f":"'12 - Performance_Outputs_1'!Q242","v":""},{"$f":"'12 - Performance_Outputs_1'!R242","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL39,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL39,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK40=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Data Center",{"$f":"'12 - Performance_Outputs_1'!B243","v":"Misc Equipment"},null,{"$f":"'12 - Performance_Outputs_1'!D243","v":"x"},{"$f":"'12 - Performance_Outputs_1'!E243","v":"Natural Gas"},{"$f":"'12 - Performance_Outputs_1'!F243","v":""},{"$f":"'12 - Performance_Outputs_1'!G243","v":""},{"$f":"'12 - Performance_Outputs_1'!H243","v":""},{"$f":"'12 - Performance_Outputs_1'!I243","v":""},{"$f":"'12 - Performance_Outputs_1'!J243","v":""},{"$f":"'12 - Performance_Outputs_1'!K243","v":""},{"$f":"'12 - Performance_Outputs_1'!M243","v":""},{"$f":"'12 - Performance_Outputs_1'!Q243","v":""},{"$f":"'12 - Performance_Outputs_1'!R243","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL40,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL40,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","","",{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":13.745458974957227},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CH40:CN41,CP40)","v":1.7181823718696534},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":15.141565880316458},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CQ40:CW41,CY40)","v":1.8926957350395572},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH40,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH40,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH40,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH40:CP41)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH40:CP41)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH40:CP41)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH40:CP41)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH40:CP41)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH40:CP41)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH40:CP41)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH40:CP41)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH40:CP41)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH40:CP41)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ40:CY41)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ40:CY41)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ40:CY41)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ40:CY41)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ40:CY41)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ40:CY41)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ40:CY41)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ40:CY41)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ40:CY41)*$DI$9","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F244","v":""},{"$f":"'12 - Performance_Outputs_1'!G244","v":""},{"$f":"'12 - Performance_Outputs_1'!H244","v":""},{"$f":"'12 - Performance_Outputs_1'!I244","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K244","v":0},{"$f":"'12 - Performance_Outputs_1'!M244","v":0},{"$f":"'12 - Performance_Outputs_1'!Q244","v":""},{"$f":"'12 - Performance_Outputs_1'!R244","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL41,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL41,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK42=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Cooking",{"$f":"'12 - Performance_Outputs_1'!B245","v":"IT equipment"},null,{"$f":"'12 - Performance_Outputs_1'!D245","v":"x"},{"$f":"'12 - Performance_Outputs_1'!E245","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F245","v":""},{"$f":"'12 - Performance_Outputs_1'!G245","v":""},{"$f":"'12 - Performance_Outputs_1'!H245","v":""},{"$f":"'12 - Performance_Outputs_1'!I245","v":""},{"$f":"'12 - Performance_Outputs_1'!J245","v":""},{"$f":"'12 - Performance_Outputs_1'!K245","v":""},{"$f":"'12 - Performance_Outputs_1'!M245","v":""},{"$f":"'12 - Performance_Outputs_1'!Q245","v":""},{"$f":"'12 - Performance_Outputs_1'!R245","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL42,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL42,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","","",{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":5.3564933401596315},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":8.8480447953746655},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":220.83772326130637},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":12.341895684703893},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CH42:CN43,CP42)","v":30.923019635193072},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":5.5067921228890153},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":8.8523319064146264},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":223.80617382915389},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":11.796248266141163},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CQ42:CW43,CY42)","v":31.245193265574837},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH42,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH42,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH42,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH42:CP43)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH42:CP43)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH42:CP43)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH42:CP43)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH42:CP43)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH42:CP43)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH42:CP43)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH42:CP43)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH42:CP43)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH42:CP43)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ42:CY43)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ42:CY43)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ42:CY43)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ42:CY43)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ42:CY43)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ42:CY43)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ42:CY43)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ42:CY43)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ42:CY43)*$DI$9","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F246","v":""},{"$f":"'12 - Performance_Outputs_1'!G246","v":""},{"$f":"'12 - Performance_Outputs_1'!H246","v":""},{"$f":"'12 - Performance_Outputs_1'!I246","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K246","v":0},{"$f":"'12 - Performance_Outputs_1'!M246","v":0},{"$f":"'12 - Performance_Outputs_1'!Q246","v":""},{"$f":"'12 - Performance_Outputs_1'!R246","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL43,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL43,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK44=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Other",{"$f":"'12 - Performance_Outputs_1'!B247","v":"Cooking"},null,{"$f":"'12 - Performance_Outputs_1'!D247","v":"x"},{"$f":"'12 - Performance_Outputs_1'!E247","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F247","v":""},{"$f":"'12 - Performance_Outputs_1'!G247","v":""},{"$f":"'12 - Performance_Outputs_1'!H247","v":""},{"$f":"'12 - Performance_Outputs_1'!I247","v":""},{"$f":"'12 - Performance_Outputs_1'!J247","v":""},{"$f":"'12 - Performance_Outputs_1'!K247","v":""},{"$f":"'12 - Performance_Outputs_1'!M247","v":""},{"$f":"'12 - Performance_Outputs_1'!Q247","v":""},{"$f":"'12 - Performance_Outputs_1'!R247","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL44,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL44,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F248","v":""},{"$f":"'12 - Performance_Outputs_1'!G248","v":""},{"$f":"'12 - Performance_Outputs_1'!H248","v":""},{"$f":"'12 - Performance_Outputs_1'!I248","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K248","v":0},{"$f":"'12 - Performance_Outputs_1'!M248","v":0},{"$f":"'12 - Performance_Outputs_1'!Q248","v":""},{"$f":"'12 - Performance_Outputs_1'!R248","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL45,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL45,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Other Regulated","Refrigeration",{"$f":"'12 - Performance_Outputs_1'!B249","v":"Industrial Process"},null,{"$f":"'12 - Performance_Outputs_1'!D249","v":"x"},{"$f":"'12 - Performance_Outputs_1'!E249","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F249","v":""},{"$f":"'12 - Performance_Outputs_1'!G249","v":""},{"$f":"'12 - Performance_Outputs_1'!H249","v":0},{"$f":"'12 - Performance_Outputs_1'!I249","v":""},{"$f":"'12 - Performance_Outputs_1'!J249","v":""},{"$f":"'12 - Performance_Outputs_1'!K249","v":""},{"$f":"'12 - Performance_Outputs_1'!M249","v":""},{"$f":"'12 - Performance_Outputs_1'!Q249","v":""},{"$f":"'12 - Performance_Outputs_1'!R249","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL46,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL46,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0,{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.3592592062898619},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.54348680817379447},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":31.513891047997841},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.49824187247029539},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CH46:CN47,CP46)","v":4.239359866866474},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":1.2737670207413692},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.42400317744230148},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":25.137814915287372},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.39255982615274992},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CQ46:CW47,CY46)","v":3.4035181174529736},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH46,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH46,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH46,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH46:CP47)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH46:CP47)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH46:CP47)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH46:CP47)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH46:CP47)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH46:CP47)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH46:CP47)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH46:CP47)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH46:CP47)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH46:CP47)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ46:CY47)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ46:CY47)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ46:CY47)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ46:CY47)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ46:CY47)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ46:CY47)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ46:CY47)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ46:CY47)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ46:CY47)*$DI$9","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F250","v":""},{"$f":"'12 - Performance_Outputs_1'!G250","v":""},{"$f":"'12 - Performance_Outputs_1'!H250","v":0},{"$f":"'12 - Performance_Outputs_1'!I250","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K250","v":0},{"$f":"'12 - Performance_Outputs_1'!M250","v":0},{"$f":"'12 - Performance_Outputs_1'!Q250","v":""},{"$f":"'12 - Performance_Outputs_1'!R250","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL47,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL47,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",0]
[null,null,null,"Baseline vs. Proposed",null,null,null,null,null,null,null,null,null,null,"Baseline vs. ASHRAE 90.1-2004",null,null,null,null,null,null,null,null,"Proposed vs. ASHRAE 90.1-2013",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK48=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Refrigeration",{"$f":"'12 - Performance_Outputs_1'!B251","v":"Refrigeration Equipment (Regulated)"},null,{"$f":"'12 - Performance_Outputs_1'!D251","v":0},{"$f":"'12 - Performance_Outputs_1'!E251","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F251","v":""},{"$f":"'12 - Performance_Outputs_1'!G251","v":""},{"$f":"'12 - Performance_Outputs_1'!H251","v":""},{"$f":"'12 - Performance_Outputs_1'!I251","v":""},{"$f":"'12 - Performance_Outputs_1'!J251","v":""},{"$f":"'12 - Performance_Outputs_1'!K251","v":""},{"$f":"'12 - Performance_Outputs_1'!M251","v":""},{"$f":"'12 - Performance_Outputs_1'!Q251","v":""},{"$f":"'12 - Performance_Outputs_1'!R251","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL48,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL48,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,null,null,"Baseline",null,"Proposed",null,null,null,null,null,null,null,null,"Baseline","ASHRAE 90.1-2004",null,null,null,null,null,null,null,"Proposed","ASHRAE 90.1-2013",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F252","v":""},{"$f":"'12 - Performance_Outputs_1'!G252","v":""},{"$f":"'12 - Performance_Outputs_1'!H252","v":""},{"$f":"'12 - Performance_Outputs_1'!I252","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K252","v":0},{"$f":"'12 - Performance_Outputs_1'!M252","v":0},{"$f":"'12 - Performance_Outputs_1'!Q252","v":""},{"$f":"'12 - Performance_Outputs_1'!R252","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL49,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL49,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,"End Use",null,"Site EUI (kBtu/sf/yr)","Cost Intensity $/sf","Site EUI (kBtu/sf/yr)","% Energy Cost Savings \nper End-Use","% Energy Site EUI Savings \nper End-Use","Cost Intensity $/sf",null,"Rank",null,"End Use",null,"Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","% Energy Site EUI Savings VS 90.1-2004\nper End-Use",null,null,null,null,"End Use",null,"Site EUI (kBtu/sf/yr)","Site EUI (kBtu/sf/yr)","% Energy Site EUI Savings VS 90.1-2004\nper End-Use",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK50=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Elevator",{"$f":"'12 - Performance_Outputs_1'!B253","v":"Refrigeration Equipment (Unregulated)"},null,{"$f":"'12 - Performance_Outputs_1'!D253","v":"x"},{"$f":"'12 - Performance_Outputs_1'!E253","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F253","v":""},{"$f":"'12 - Performance_Outputs_1'!G253","v":""},{"$f":"'12 - Performance_Outputs_1'!H253","v":""},{"$f":"'12 - Performance_Outputs_1'!I253","v":""},{"$f":"'12 - Performance_Outputs_1'!J253","v":""},{"$f":"'12 - Performance_Outputs_1'!K253","v":""},{"$f":"'12 - Performance_Outputs_1'!M253","v":""},{"$f":"'12 - Performance_Outputs_1'!Q253","v":""},{"$f":"'12 - Performance_Outputs_1'!R253","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL50,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL50,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","","",{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":2.6730776983694775},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.16321913354436554},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":12.427826462081191},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":6.8753312317948216},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CH50:CN51,CP50)","v":3.1054384086754618},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":2.7040527436138397},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":2.6656644487450758},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.12388047517694195},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":12.217768710706922},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":6.6126206663774703},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CQ50:CW51,CY50)","v":3.029190037304319},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH50,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH50,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH50,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":2.6135859974281423},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH50:CP51)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH50:CP51)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH50:CP51)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH50:CP51)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH50:CP51)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH50:CP51)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH50:CP51)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH50:CP51)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH50:CP51)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH50:CP51)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ50:CY51)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ50:CY51)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ50:CY51)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ50:CY51)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ50:CY51)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ50:CY51)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ50:CY51)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ50:CY51)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ50:CY51)*$DI$9","v":{"$error":"#DIV/0!"}}]
[null,{"$f":"'Quality Assurance Checks'!AJ7","v":"Lighting, Interior"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B51,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B51,'Quality Assurance Checks'!AP:AP)","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B51,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B51,'Quality Assurance Checks'!AX:AX)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B51,'Quality Assurance Checks'!AX:AX))","v":{"$error":"#N/A"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B51,'Quality Assurance Checks'!AY:AY)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B51,'Quality Assurance Checks'!AY:AY))","v":{"$error":"#N/A"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B51,'Quality Assurance Checks'!AW:AW)","v":{"$error":"#DIV/0!"}},{"$f":"IFERROR(100*G51,\"\")","v":""},{"$f":"IFERROR(RANK(J51,$J$51:$J$59,0),\"\")","v":""},"Interior Lighting",{"$f":"'Quality Assurance Checks'!AJ7","v":"Lighting, Interior"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M51,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M51,'Quality Assurance Checks'!BB:BB)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,M51,'Quality Assurance Checks'!AQ:AQ)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,M51,'Quality Assurance Checks'!AQ:AQ))","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"'Quality Assurance Checks'!AJ7","v":"Lighting, Interior"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M51,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M51,'Quality Assurance Checks'!BC:BC)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M51,'Quality Assurance Checks'!BA:BA)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M51,'Quality Assurance Checks'!BA:BA))","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F254","v":""},{"$f":"'12 - Performance_Outputs_1'!G254","v":""},{"$f":"'12 - Performance_Outputs_1'!H254","v":""},{"$f":"'12 - Performance_Outputs_1'!I254","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K254","v":0},{"$f":"'12 - Performance_Outputs_1'!M254","v":0},{"$f":"'12 - Performance_Outputs_1'!Q254","v":""},{"$f":"'12 - Performance_Outputs_1'!R254","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL51,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL51,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,{"$f":"'Quality Assurance Checks'!AJ8","v":"Lighting, Exterior"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B52,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B52,'Quality Assurance Checks'!AP:AP)","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B52,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B52,'Quality Assurance Checks'!AX:AX)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B52,'Quality Assurance Checks'!AX:AX))","v":{"$error":"#N/A"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B52,'Quality Assurance Checks'!AY:AY)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B52,'Quality Assurance Checks'!AY:AY))","v":{"$error":"#N/A"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B52,'Quality Assurance Checks'!AW:AW)","v":{"$error":"#DIV/0!"}},{"$f":"IFERROR(100*G52,\"\")","v":""},{"$f":"IFERROR(RANK(J52,$J$51:$J$59,0),\"\")","v":""},"Exterior Lighting",{"$f":"'Quality Assurance Checks'!AJ8","v":"Lighting, Exterior"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M52,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M52,'Quality Assurance Checks'!BB:BB)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,M52,'Quality Assurance Checks'!AQ:AQ)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,M52,'Quality Assurance Checks'!AQ:AQ))","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"'Quality Assurance Checks'!AJ8","v":"Lighting, Exterior"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M52,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M52,'Quality Assurance Checks'!BC:BC)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M52,'Quality Assurance Checks'!BA:BA)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M52,'Quality Assurance Checks'!BA:BA))","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK52=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Transformers",{"$f":"'12 - Performance_Outputs_1'!B255","v":"Elevators and escalators"},null,{"$f":"'12 - Performance_Outputs_1'!D255","v":0},{"$f":"'12 - Performance_Outputs_1'!E255","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F255","v":""},{"$f":"'12 - Performance_Outputs_1'!G255","v":""},{"$f":"'12 - Performance_Outputs_1'!H255","v":""},{"$f":"'12 - Performance_Outputs_1'!I255","v":""},{"$f":"'12 - Performance_Outputs_1'!J255","v":""},{"$f":"'12 - Performance_Outputs_1'!K255","v":""},{"$f":"'12 - Performance_Outputs_1'!M255","v":""},{"$f":"'12 - Performance_Outputs_1'!Q255","v":""},{"$f":"'12 - Performance_Outputs_1'!R255","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL52,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL52,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","","",{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CH$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.30046128045466697},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CI$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CJ$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.49154820129804683},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CK$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.35484681107352711},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CL$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CM$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.27697105142550343},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CN$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CH52:CN53,CP52)","v":0.2043062465341878},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2004 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2004 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CP$4,'90.1-2004 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2004 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.21062262802175796},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CQ$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.15699286527820899},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CR$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CS$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.25728369858888295},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CT$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.21093001922172483},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CU$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CV$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.14403103733056768},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CW$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0},{"$f":"AVERAGE(CQ52:CW53,CY52)","v":0.11131372693028702},{"$f":"IFERROR(IF($DD$1=\"4A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$3:$W$27,MATCH($BH52,'90.1-2013 Site EUI'!$A$4:$W$4,0),FALSE),IF($DD$1=\"5A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$29:$W$53,MATCH($BH52,'90.1-2013 Site EUI'!$A$30:$W$30,0),FALSE),IF($DD$1=\"6A\",VLOOKUP(CY$4,'90.1-2013 Site EUI'!$A$55:$W$79,MATCH($BH52,'90.1-2013 Site EUI'!$A$56:$W$56,0),FALSE),\"\"))),\"\")","v":0.12127219502291178},{"$f":"SUMIF($CH$4:$CP$4,$DG$1,CH52:CP53)*$DI$1+SUMIF($CH$4:$CP$4,$DG$2,CH52:CP53)*$DI$2+SUMIF($CH$4:$CP$4,$DG$3,CH52:CP53)*$DI$3+SUMIF($CH$4:$CP$4,$DG$4,CH52:CP53)*$DI$4+SUMIF($CH$4:$CP$4,$DG$5,CH52:CP53)*$DI$5+SUMIF($CH$4:$CP$4,$DG$6,CH52:CP53)*$DI$6+SUMIF($CH$4:$CP$4,$DG$7,CH52:CP53)*$DI$7+SUMIF($CH$4:$CP$4,$DG$8,CH52:CP53)*$DI$8+SUMIF($CH$4:$CP$4,$DG$8,CH52:CP53)*$DI$8+SUMIF($CH$4:$CP$4,$DG$9,CH52:CP53)*$DI$9","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF($CQ$4:$CY$4,$DG$1,CQ52:CY53)*$DI$1+SUMIF($CQ$4:$CY$4,$DG$2,CQ52:CY53)*$DI$2+SUMIF($CQ$4:$CY$4,$DG$3,CQ52:CY53)*$DI$3+SUMIF($CQ$4:$CY$4,$DG$4,CQ52:CY53)*$DI$4+SUMIF($CQ$4:$CY$4,$DG$5,CQ52:CY53)*$DI$5+SUMIF($CQ$4:$CY$4,$DG$6,CQ52:CY53)*$DI$6+SUMIF($CQ$4:$CY$4,$DG$7,CQ52:CY53)*$DI$7+SUMIF($CQ$4:$CY$4,$DG$8,CQ52:CY53)*$DI$8+SUMIF($CQ$4:$CY$4,$DG$9,CQ52:CY53)*$DI$9","v":{"$error":"#DIV/0!"}}]
[null,{"$f":"'Quality Assurance Checks'!AJ9","v":"SHW"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B53,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B53,'Quality Assurance Checks'!AP:AP)","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B53,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B53,'Quality Assurance Checks'!AX:AX)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B53,'Quality Assurance Checks'!AX:AX))","v":{"$error":"#N/A"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B53,'Quality Assurance Checks'!AY:AY)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B53,'Quality Assurance Checks'!AY:AY))","v":{"$error":"#N/A"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B53,'Quality Assurance Checks'!AW:AW)","v":{"$error":"#DIV/0!"}},"","","Service Hot Water",{"$f":"'Quality Assurance Checks'!AJ9","v":"SHW"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M53,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M53,'Quality Assurance Checks'!BB:BB)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,M53,'Quality Assurance Checks'!AQ:AQ)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,M53,'Quality Assurance Checks'!AQ:AQ))","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"'Quality Assurance Checks'!AJ9","v":"SHW"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M53,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M53,'Quality Assurance Checks'!BC:BC)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M53,'Quality Assurance Checks'!BA:BA)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M53,'Quality Assurance Checks'!BA:BA))","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F256","v":""},{"$f":"'12 - Performance_Outputs_1'!G256","v":""},{"$f":"'12 - Performance_Outputs_1'!H256","v":""},{"$f":"'12 - Performance_Outputs_1'!I256","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K256","v":0},{"$f":"'12 - Performance_Outputs_1'!M256","v":0},{"$f":"'12 - Performance_Outputs_1'!Q256","v":""},{"$f":"'12 - Performance_Outputs_1'!R256","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL53,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL53,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,{"$f":"'Quality Assurance Checks'!AJ10","v":"Heat"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B54,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B54,'Quality Assurance Checks'!AP:AP)","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B54,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B54,'Quality Assurance Checks'!AX:AX)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B54,'Quality Assurance Checks'!AX:AX))","v":{"$error":"#N/A"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B54,'Quality Assurance Checks'!AY:AY)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B54,'Quality Assurance Checks'!AY:AY))","v":{"$error":"#N/A"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B54,'Quality Assurance Checks'!AW:AW)","v":{"$error":"#DIV/0!"}},"","","Heating",{"$f":"'Quality Assurance Checks'!AJ10","v":"Heat"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M54,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M54,'Quality Assurance Checks'!BB:BB)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,M54,'Quality Assurance Checks'!AQ:AQ)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,M54,'Quality Assurance Checks'!AQ:AQ))","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"'Quality Assurance Checks'!AJ10","v":"Heat"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M54,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M54,'Quality Assurance Checks'!BC:BC)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M54,'Quality Assurance Checks'!BA:BA)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M54,'Quality Assurance Checks'!BA:BA))","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK54=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Other",{"$f":"'12 - Performance_Outputs_1'!B257","v":"Building Transformers"},null,{"$f":"'12 - Performance_Outputs_1'!D257","v":0},{"$f":"'12 - Performance_Outputs_1'!E257","v":"Electricity"},{"$f":"'12 - Performance_Outputs_1'!F257","v":""},{"$f":"'12 - Performance_Outputs_1'!G257","v":""},{"$f":"'12 - Performance_Outputs_1'!H257","v":""},{"$f":"'12 - Performance_Outputs_1'!I257","v":""},{"$f":"'12 - Performance_Outputs_1'!J257","v":""},{"$f":"'12 - Performance_Outputs_1'!K257","v":""},{"$f":"'12 - Performance_Outputs_1'!M257","v":""},{"$f":"'12 - Performance_Outputs_1'!Q257","v":""},{"$f":"'12 - Performance_Outputs_1'!R257","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL54,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL54,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,{"$f":"'Quality Assurance Checks'!AJ11","v":"Cool"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B55,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B55,'Quality Assurance Checks'!AP:AP)","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B55,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B55,'Quality Assurance Checks'!AX:AX)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B55,'Quality Assurance Checks'!AX:AX))","v":{"$error":"#N/A"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B55,'Quality Assurance Checks'!AY:AY)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B55,'Quality Assurance Checks'!AY:AY))","v":{"$error":"#N/A"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B55,'Quality Assurance Checks'!AW:AW)","v":{"$error":"#DIV/0!"}},"","","Cooling",{"$f":"'Quality Assurance Checks'!AJ11","v":"Cool"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M55,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M55,'Quality Assurance Checks'!BB:BB)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,M55,'Quality Assurance Checks'!AQ:AQ)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,M55,'Quality Assurance Checks'!AQ:AQ))","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"'Quality Assurance Checks'!AJ11","v":"Cool"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M55,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M55,'Quality Assurance Checks'!BC:BC)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M55,'Quality Assurance Checks'!BA:BA)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M55,'Quality Assurance Checks'!BA:BA))","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F258","v":""},{"$f":"'12 - Performance_Outputs_1'!G258","v":""},{"$f":"'12 - Performance_Outputs_1'!H258","v":""},{"$f":"'12 - Performance_Outputs_1'!I258","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K258","v":0},{"$f":"'12 - Performance_Outputs_1'!M258","v":0},{"$f":"'12 - Performance_Outputs_1'!Q258","v":""},{"$f":"'12 - Performance_Outputs_1'!R258","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL55,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL55,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,{"$f":"'Quality Assurance Checks'!AJ12","v":"Fans"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B56,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B56,'Quality Assurance Checks'!AP:AP)","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B56,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B56,'Quality Assurance Checks'!AX:AX)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B56,'Quality Assurance Checks'!AX:AX))","v":{"$error":"#N/A"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B56,'Quality Assurance Checks'!AY:AY)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B56,'Quality Assurance Checks'!AY:AY))","v":{"$error":"#N/A"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B56,'Quality Assurance Checks'!AW:AW)","v":{"$error":"#DIV/0!"}},"","","Fans",{"$f":"'Quality Assurance Checks'!AJ12","v":"Fans"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M56,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M56,'Quality Assurance Checks'!BB:BB)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,M56,'Quality Assurance Checks'!AQ:AQ)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,M56,'Quality Assurance Checks'!AQ:AQ))","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"'Quality Assurance Checks'!AJ12","v":"Fans"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M56,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M56,'Quality Assurance Checks'!BC:BC)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M56,'Quality Assurance Checks'!BA:BA)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M56,'Quality Assurance Checks'!BA:BA))","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK56=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Other",{"$f":"'12 - Performance_Outputs_1'!B259","v":0},null,{"$f":"'12 - Performance_Outputs_1'!D259","v":0},{"$f":"'12 - Performance_Outputs_1'!E259","v":0},{"$f":"'12 - Performance_Outputs_1'!F259","v":""},{"$f":"'12 - Performance_Outputs_1'!G259","v":""},{"$f":"'12 - Performance_Outputs_1'!H259","v":""},{"$f":"'12 - Performance_Outputs_1'!I259","v":""},{"$f":"'12 - Performance_Outputs_1'!J259","v":""},{"$f":"'12 - Performance_Outputs_1'!K259","v":""},{"$f":"'12 - Performance_Outputs_1'!M259","v":""},{"$f":"'12 - Performance_Outputs_1'!Q259","v":""},{"$f":"'12 - Performance_Outputs_1'!R259","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL56,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL56,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,{"$f":"'Quality Assurance Checks'!AJ13","v":"Pumps"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B57,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B57,'Quality Assurance Checks'!AP:AP)","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B57,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B57,'Quality Assurance Checks'!AX:AX)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B57,'Quality Assurance Checks'!AX:AX))","v":{"$error":"#N/A"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B57,'Quality Assurance Checks'!AY:AY)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B57,'Quality Assurance Checks'!AY:AY))","v":{"$error":"#N/A"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B57,'Quality Assurance Checks'!AW:AW)","v":{"$error":"#DIV/0!"}},"","","Pumps",{"$f":"'Quality Assurance Checks'!AJ13","v":"Pumps"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M57,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M57,'Quality Assurance Checks'!BB:BB)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,M57,'Quality Assurance Checks'!AQ:AQ)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,M57,'Quality Assurance Checks'!AQ:AQ))","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"'Quality Assurance Checks'!AJ13","v":"Pumps"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M57,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M57,'Quality Assurance Checks'!BC:BC)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M57,'Quality Assurance Checks'!BA:BA)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M57,'Quality Assurance Checks'!BA:BA))","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F260","v":""},{"$f":"'12 - Performance_Outputs_1'!G260","v":""},{"$f":"'12 - Performance_Outputs_1'!H260","v":""},{"$f":"'12 - Performance_Outputs_1'!I260","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K260","v":0},{"$f":"'12 - Performance_Outputs_1'!M260","v":0},{"$f":"'12 - Performance_Outputs_1'!Q260","v":""},{"$f":"'12 - Performance_Outputs_1'!R260","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL57,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL57,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,{"$f":"'Quality Assurance Checks'!AJ14","v":"Other Regulated"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B58,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B58,'Quality Assurance Checks'!AP:AP)","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B58,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B58,'Quality Assurance Checks'!AX:AX)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B58,'Quality Assurance Checks'!AX:AX))","v":{"$error":"#N/A"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B58,'Quality Assurance Checks'!AY:AY)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B58,'Quality Assurance Checks'!AY:AY))","v":{"$error":"#N/A"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B58,'Quality Assurance Checks'!AW:AW)","v":{"$error":"#DIV/0!"}},"","","Other Regulated Loads",{"$f":"'Quality Assurance Checks'!AJ14","v":"Other Regulated"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M58,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M58,'Quality Assurance Checks'!BB:BB)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,M58,'Quality Assurance Checks'!AQ:AQ)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,M58,'Quality Assurance Checks'!AQ:AQ))","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"'Quality Assurance Checks'!AJ14","v":"Other Regulated"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M58,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M58,'Quality Assurance Checks'!BC:BC)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M58,'Quality Assurance Checks'!BA:BA)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M58,'Quality Assurance Checks'!BA:BA))","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK58=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Other",{"$f":"'12 - Performance_Outputs_1'!B261","v":0},null,{"$f":"'12 - Performance_Outputs_1'!D261","v":0},{"$f":"'12 - Performance_Outputs_1'!E261","v":0},{"$f":"'12 - Performance_Outputs_1'!F261","v":""},{"$f":"'12 - Performance_Outputs_1'!G261","v":""},{"$f":"'12 - Performance_Outputs_1'!H261","v":""},{"$f":"'12 - Performance_Outputs_1'!I261","v":""},{"$f":"'12 - Performance_Outputs_1'!J261","v":""},{"$f":"'12 - Performance_Outputs_1'!K261","v":""},{"$f":"'12 - Performance_Outputs_1'!M261","v":""},{"$f":"'12 - Performance_Outputs_1'!Q261","v":""},{"$f":"'12 - Performance_Outputs_1'!R261","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL58,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL58,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,{"$f":"'Quality Assurance Checks'!AJ15","v":"Other Non-Regulated"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B59,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B59,'Quality Assurance Checks'!AP:AP)","v":{"$error":"#DIV/0!"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B59,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B59,'Quality Assurance Checks'!AX:AX)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B59,'Quality Assurance Checks'!AX:AX))","v":{"$error":"#N/A"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,B59,'Quality Assurance Checks'!AY:AY)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,B59,'Quality Assurance Checks'!AY:AY))","v":{"$error":"#N/A"}},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,B59,'Quality Assurance Checks'!AW:AW)","v":{"$error":"#DIV/0!"}},"","","Other Non-Regulated Loads",{"$f":"'Quality Assurance Checks'!AJ15","v":"Other Non-Regulated"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M59,'Quality Assurance Checks'!AL:AL)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,M59,'Quality Assurance Checks'!BB:BB)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,M59,'Quality Assurance Checks'!AQ:AQ)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,M59,'Quality Assurance Checks'!AQ:AQ))","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"'Quality Assurance Checks'!AJ15","v":"Other Non-Regulated"},null,{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M59,'Quality Assurance Checks'!AS:AS)","v":0},{"$f":"SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M59,'Quality Assurance Checks'!BC:BC)","v":{"$error":"#DIV/0!"}},{"$f":"IF(SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M59,'Quality Assurance Checks'!BA:BA)<0.001,#N/A,SUMIF('Quality Assurance Checks'!AJ:AJ,'Quality Assurance Checks'!M59,'Quality Assurance Checks'!BA:BA))","v":{"$error":"#N/A"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'12 - Performance_Outputs_1'!F262","v":""},{"$f":"'12 - Performance_Outputs_1'!G262","v":""},{"$f":"'12 - Performance_Outputs_1'!H262","v":""},{"$f":"'12 - Performance_Outputs_1'!I262","v":""},null,{"$f":"'12 - Performance_Outputs_1'!K262","v":0},{"$f":"'12 - Performance_Outputs_1'!M262","v":0},{"$f":"'12 - Performance_Outputs_1'!Q262","v":""},{"$f":"'12 - Performance_Outputs_1'!R262","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL59,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL59,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BK60=\"\",\"Other Regulated\",\"Other Non-Regulated\")","v":"Other Non-Regulated"},"Other",{"$f":"'12 - Performance_Outputs_1'!B263","v":0},null,{"$f":"'12 - Performance_Outputs_1'!D263","v":0},{"$f":"'12 - Performance_Outputs_1'!E263","v":0},{"$f":"'12 - Performance_Outputs_1'!F263","v":""},{"$f":"'12 - Performance_Outputs_1'!G263","v":""},{"$f":"'12 - Performance_Outputs_1'!H263","v":""},{"$f":"'12 - Performance_Outputs_1'!I263","v":""},{"$f":"'12 - Performance_Outputs_1'!J263","v":""},{"$f":"'12 - Performance_Outputs_1'!K263","v":""},{"$f":"'12 - Performance_Outputs_1'!M263","v":""},{"$f":"'12 - Performance_Outputs_1'!Q263","v":""},{"$f":"'12 - Performance_Outputs_1'!R263","v":""},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL60,'12 - Performance_Outputs_1'!$E$282:$G$286)","v":0},{"$f":"SUMIF('12 - Performance_Outputs_1'!$B$282:$B$287,BL60,'12 - Performance_Outputs_1'!$H$282:$H$286)","v":0},"","","","","","","","","",""]
[]
["Issue",null,null,null,null,null,"Project Team Response"]
[{"$f":"\"Please Explain\"","v":"Please Explain"},{"$f":"IFERROR(\"The three largest end use contributors to the cost savings are \"&CONCATENATE(VLOOKUP(1,$K$51:$L$59,2,FALSE),\", \", VLOOKUP(2,$K$51:$L$59,2,FALSE), \", and \",VLOOKUP(3,$K$51:$L$59,2,FALSE))&\" (as reported in the 12 - Performance_Outputs_1 tab). Please provide a narrative to justify the savings of these end uses, such as the energy efficiency measures which contribute to the savings claimed.\",\"-\")","v":"-"}]
[]
["General"]
["Input/Output Summary"]
["Building Area, SF (General Information tab)",null,null,"Building Area, SF \n(6a - Lighting Counts tab)",null,"Baseline Unmet Load Hours \n(12 - Performance_Outputs_1 tab)",null,"Proposed Desing Unmet Load Hours \n(12 - Performance_Outputs_1 tab)",null,"Number of Thermal Blocks \n(6a - Lighting Counts tab)"]
[{"$f":"'General Information'!F23","v":0},null,null,{"$f":"'6a - Lighting Counts'!H26","v":0},null,{"$f":"'12 - Performance_Outputs_1'!F434","v":0},null,{"$f":"'12 - Performance_Outputs_1'!I434","v":0},null,{"$f":"SUM('6a - Lighting Counts'!F29:F551)","v":0}]
["Issue",null,null,null,null,null,"Project Team Response"]
[{"$f":"IFERROR(IF(ABS(A68-D68)/MIN(A68,D68)>0.1,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},{"$f":"\"The total building area reported in the \"&IF(MultipleBuildingsExist=\"No\",\"General Information\", \"Multiple Building Details\")& \" tab differs from the total building area reported in the Lighting tab (Interior Lighting section) by more than 10%. Please check for consistency and verify that the building areas reported are accurate.\"","v":"The total building area reported in the General Information tab differs from the total building area reported in the Lighting tab (Interior Lighting section) by more than 10%. Please check for consistency and verify that the building areas reported are accurate."}]
[{"$f":"IFERROR(IF(J68<10,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},"Based on the Lighting Counts tab, less than 10 thermal blocks were modeled, which is lower than expected. Please verify that the thermal blocks were modeled as required in Table G 3.1 #7, and provide a narrative justifying the number of modeled thermal blocks."]
[{"$f":"IFERROR(IF(MAX(F68:I68)>300,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},"The unmet load hours exceed 300 hours for the baseline and/or proposed (as reported in the Performance Outputs tab), which is not in compliance with G3.1.2.3.  Please correct."]
["Envelope"]
["Input/Output Summary"]
["Modeled Baseline Vertical Glazing %\n(4 - Shading and Fenestration tab)",null,null,"Calculated Baseline Vertical Glazing % based on Table G3.1 #5c\n(4 - Shading and Fenestration tab)",null,null,"Has the baseline model been rotated?\n(Energy Modeling Output Reporting Method of the 12 - Performance_Outputs_1 tab)"]
[{"$f":"IFERROR(ROUND('4 - Shading and Fenestration'!D53,3),\"-\")","v":0},null,null,{"$f":"IFERROR(ROUND('4 - Shading and Fenestration'!B53,3),\"-\")","v":"-"},null,null,{"$f":"IF('12 - Performance_Outputs_1'!R99=1,\"Yes\",\"No\")","v":"Yes"}]
["Issue",null,null,null,null,null,"Project Team Response"]
[{"$f":"IFERROR(IF(A76=D76,\"Pass\",\"Please Explain\"),\"Pass\")","v":"Please Explain"},"The vertical glazing areas in the baseline differs from what is required in Table G3.1.1-1.  Please correct or provide justification."]
[{"$f":"IFERROR(IF(G76=\"No\",\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},"The Energy Modeling Output Reporting Method (as reported in the Performance Outputs tab) indicates that the baseline has not been rotated because the building orientation is dictated by site considerations, as allowed by Table G3.1 #5 (a) (baseline) Exception 1. Provide a detailed narrative (and additional documentation as necessary) describing why this exception has been applied."]
["Interior Lighting"]
["Input/Output Summary"]
[null,"Interior Lighting Power [W] \n(6b - General Lighting tab)","Lighting Power [W]  Adjusted for OS \n(6b - General Lighting tab)",null,"Non-coincident Lighting Peak Demand [W] \n(12 - Performance_Outputs_1 tab)",null,"Annual Lighting Use [kWh] \n(12 - Performance_Outputs_1 tab) ",null,"Effective Full Load Hours (EFLH)",{"$f":"\"Typical EFLH for \"&IF(INDEX('General Information'!$F$17:$F$21,2,1)=\"\",INDEX('General Information'!$F$17:$F$21,1,1),INDEX('General Information'!$F$17:$F$21,1,1)&\" and \"&INDEX('General Information'!$F$17:$F$21,2,1))","v":"Typical EFLH for "},"Diversity Factor"]
[null,"A","B",null,"C",null,"D",null,"E=D/(A/1000)","F","G=C/A"]
["Baseline Design",{"$f":"'6b - General Lighting'!F60","v":0},{"$f":"'6b - General Lighting'!F60","v":0},null,{"$f":"IFERROR('12 - Performance_Outputs_1'!G210*1000+'12 - Performance_Outputs_1'!G212*1000,\"-\")","v":"-"},null,{"$f":"IFERROR('12 - Performance_Outputs_1'!G209+'12 - Performance_Outputs_1'!G211,\"-\")","v":"-"},null,{"$f":"IFERROR(G84/(B84/1000),\"-\")","v":"-"},{"$f":"IFERROR(SUM('General Information'!U17:U20),$DQ$27)","v":4017.75},{"$f":"IFERROR(E84/B84,\"-\")","v":"-"}]
["Proposed Design",{"$f":"'6b - General Lighting'!E60","v":0},{"$f":"'6b - General Lighting'!L60","v":0},null,{"$f":"IFERROR('12 - Performance_Outputs_1'!H210*1000+'12 - Performance_Outputs_1'!H212*1000,\"-\")","v":0},null,{"$f":"IFERROR('12 - Performance_Outputs_1'!H209+'12 - Performance_Outputs_1'!H211,\"-\")","v":0},null,{"$f":"IFERROR(G85/(B85/1000),\"-\")","v":"-"},"NA",{"$f":"IFERROR(E85/B85,\"-\")","v":"-"}]
["Proposed/Baseline",{"$f":"IFERROR(B85/B84,\"-\")","v":"-"},{"$f":"IFERROR(C85/C84,\"-\")","v":"-"},null,{"$f":"IFERROR(E85/E84,\"-\")","v":"-"},null,{"$f":"IFERROR(G85/G84,\"-\")","v":"-"},null,{"$f":"IFERROR(I85/I84,\"-\")","v":"-"},"NA",{"$f":"IFERROR(K85/K84,\"-\")","v":"-"}]
["Issue",null,null,null,null,null,"Project Team Response"]
[{"$f":"IF(E84>B84,\"Please Explain\",\"Pass\")","v":"Please Explain"},"The baseline lighting non-coincident peak demand reported on the Performance Outputs tab exceeds the baseline lighting power on the General Lighting tab (B>A). Please correct the lighting inputs in the baseline model, or update the inputs on the Lighting Counts tab."]
[{"$f":"IF(E85>B85,\"Please Explain\",\"Pass\")","v":"Pass"},"The proposed lighting non-coincident peak demand reported on the Performance Outputs tab exceeds the proposed lighting power on the General Lighting tab (B>A). Please correct the lighting inputs in the proposed model, or update the inputs on the Lighting Counts tab."]
[{"$f":"IF((E86<0.9*C86),\"Please Explain\",\"Pass\")","v":{"$error":"#VALUE!"}},{"$f":"AJ90&TEXT(C86,\"00%\")&AJ93&TEXT(E86,\"00%\")&AJ92","v":"Based on the General Lighting tab, the proposed lighting power adjusted for occupancy sensors is - of the baseline. A similar relationship is expected for the non-coincident peak demand. However, based on the modeling results in the Performance Outputs tab, the proposed non-coincident lighting peak demand is - of the baseline, which is less  than expected. Please review and correct the lighting inputs in the proposed and / or baseline model, update the inputs on the Lighting Counts tab, or explain."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Based on the General Lighting tab, the proposed lighting power adjusted for occupancy sensors is "]
[{"$f":"IFERROR(IF(AND(RatingSystemSelection=\"ENERGY STAR MFHR\",'6b - General Lighting'!X60=1),\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},"The proposed in-unit lighting is reported as <0.6 w/sf in the General Lighting tab. For ENERGY STAR MFHR projects, if the proposed in-unit lighting is below 0.6 W/SF, the savings in excess of these limits may be modeled only if the proposed fixtures are demonstrated to meet the recommended weighted average footcandles based on the 10th edition of the Illuminating Engineering Society (IESNA) Lighting Handbook for the given space type. Please provide external calculations showing these requirements are met, and also note the modeled in-unit LPD."]
[{"$f":"IF(((C85*0.9)/(C84))>(G85/G84),\"Please Explain\",\"Pass\")","v":{"$error":"#DIV/0!"}},"The difference between the baseline and proposed annual lighting energy use is higher than expected based on the baseline and proposed lighting wattages and OS entered on the Lighting Counts tab, and an estimated additional 10% savings from daylighting controls. Please verify that the modeled lighting wattages and controls reflect the values reported on the Lighting Counts tab. 0.9 * (B prop / B base > D prop / D base) ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," of the baseline, which is less  than expected. Please review and correct the lighting inputs in the proposed and / or baseline model, update the inputs on the Lighting Counts tab, or explain."]
[{"$f":"IF((I84>1.2*J84),\"Please Explain\",\"Pass\")","v":"Please Explain"},"The effective full load hours (E) exceed the typical (F) by more than 20%. Ensure that the model reflects the mandatory lighting controls, and is based on the anticipated schedule of operation for the building. Please describe operating schedule if different than typical for the building type.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," of the baseline. A similar relationship is expected for the non-coincident peak demand. However, based on the modeling results in the Performance Outputs tab, the proposed non-coincident lighting peak demand is "]
[{"$f":"IFERROR(IF(AND(RatingSystemSelection=\"ENERGY STAR MFHR\",'6b - General Lighting'!X60>0),\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},"Some space types in the General Lighting tab show an LPD reduction of >30% compared to the space-by-space lighting power allowance in the reference edition of 90.1. For ENERGY STAR MFHR projects, if a proposed common space lighting power reduction is >30%, the savings in excess of these limits may be modeled only if the proposed fixtures are demonstrated to meet the recommended weighted average footcandles based on the 10th edition of the Illuminating Engineering Society (IESNA) Lighting Handbook for the given space type. Please provide external calculations showing these requirements are met, and also note the modeled common space LPDs for any spaces with >30% LPD reduction."]
["Exterior Lighting"]
["Input/Output Summary"]
[null,"Exterior Lighting Power [W] \n(6b - General Lighting tab)",null,null,"Non-coincident Lighting Peak Demand [W] \n(12 - Performance_Outputs_1 tab)",null,null,"Annual Lighting Use [kWh] \n(12 - Performance_Outputs_1 tab) ",null,null,"Effective Full Load Hours (EFLH)"]
[null,"A",null,null,"B",null,null,"C",null,null,"D=C / (A/1000)"]
["Baseline Design",{"$f":"'6b - General Lighting'!J172*1000","v":0},null,null,{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G216=\"\",0,'12 - Performance_Outputs_1'!G216*1000),\"-\")","v":0},null,null,{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G215=\"\",0,'12 - Performance_Outputs_1'!G215),\"-\")","v":0},null,null,{"$f":"IFERROR(H99/(B99/1000),\"-\")","v":"-"}]
["Proposed Design",{"$f":"'6b - General Lighting'!M172*1000","v":0},null,null,{"$f":"IFERROR('12 - Performance_Outputs_1'!H216*1000,\"-\")","v":0},null,null,{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H215=\"\",0,'12 - Performance_Outputs_1'!H215),\"-\")","v":0},null,null,{"$f":"IFERROR(H100/(B100/1000),\"-\")","v":"-"}]
["Proposed/Baseline",{"$f":"IFERROR(B100/B99,\"-\")","v":"-"},null,null,{"$f":"IFERROR(E100/E99,\"-\")","v":"-"},null,null,{"$f":"IFERROR(H100/H99,\"-\")","v":"-"},null,null,{"$f":"IFERROR(K100/K99,\"-\")","v":"-"}]
["Issue",null,null,null,null,null,"Project Team Response"]
[{"$f":"IF(B99<E99,\"Please Explain\",\"Pass\")","v":"Pass"},"The baseline exterior Lighting Power reported on the General Lighting tab is less than the modeled baseline exterior lighting non-coincident peak demand (A<B). Please review and correct the inputs on the General Lighting tab or the baseline model."]
[{"$f":"IF(B100>B99,\"Please Explain\",\"Pass\")","v":"Pass"},"Based on the General Lighting tab, proposed exterior lighting wattage exceeds the baseline (A prop > A base). The exterior lighting requirements are mandatory and cannot be exceeded by the proposed design. Please review the exterior lighting inputs in the General Lighting tab, and the fixtures specified for the proposed design."]
[{"$f":"IFERROR(IF(K99=\"-\",\"Pass\",IF(K99>2920,\"Please Explain\",\"Pass\")),\"Please Explain\")","v":"Pass"},"The baseline EFLH (D) exceed 2920 (8 hours per day). Please verify that the exterior lighting controls required in Section 9.4.1.4 were modeled."]
[{"$f":"IFERROR(IF(AND(K99=\"-\",K100=\"-\"),\"Pass\",IF((ABS(K99-K100)/MIN(K100,K99))>0.01,\"Please Explain\",\"Pass\")),\"Please Explain\")","v":"Pass"},"EFLH for the baseline differ from the EFLH for the proposed design (D base not equal to D prop). Since exterior lighting schedules and controls must be the same in the baseline and proposed design, the EFLH are expected to be equal. Please review and correct the baseline and / proposed design models."]
[{"$f":"IF(E100=0,\"Please Explain\",\"Pass\")","v":"Please Explain"},"The Performance Outputs tab shows zero consumption for exterior lighting power in the proposed model. Confirm that no exterior lighting is included in the building site."]
[{"$f":"IFERROR(IF(AND(B99=0,B100=0,H99=0,H100=0),\"Pass\",IF((B99/B100)<>(H99/H100),\"Please Explain\",\"Pass\")),\"Please Explain\")","v":"Pass"},"Since the same schedules and controls must be modeled for the baseline and proposed design, the change in the annual exterior lighting energy use of the baseline versus proposed design is expected to be proportional to the change in the exterior lighting power between the baseline and proposed design (A base / A prop = C base / C prop). Please review and correct the inputs in the baseline and/or proposed design models."]
[{"$f":"IFERROR(IF(AND(H99=0,H100=0),\"Pass\",IF((ABS(H99-H100)/MIN(H100,H99))<0.01,\"Please Explain\",\"Pass\")),\"Please Explain\")","v":"Pass"},"The baseline and proposed exterior lighting consumption values are within 1% of each other, indicating that the lighting has been modeled nearly identically. Verify that the proposed exterior lighting reflects the actual building design, and the baseline reflects the allowed lighting power from Table G3.6. Ensure that no credit is taken in the proposed design for non‐tradable surfaces. Note that additional lighting power allowance cannot be claimed in the baseline for surfaces that are not provided with lighting in the actual design, and  that lighting fixtures cannot be double counted for different exterior surfaces."]
["Miscellaneous Loads"]
["Input/Output Summary"]
[null,"Miscellaneous Unregulated Loads [kBtu/SF] \n(12 - Performance_Outputs_1 tab)",null,null,"Total Miscellaneous Loads  [kBtu/SF] \n(12 - Performance_Outputs_1 tab)",null,null,{"$f":"\"Typical Miscellaneous Loads for \"&IF(INDEX('General Information'!$S$17:$S$21,2,1)=\"\",INDEX('General Information'!$S$17:$S$21,1,1),INDEX('General Information'!$S$17:$S$21,1,1)&\" and \"&INDEX('General Information'!$S$17:$S$21,2,1))&\" [kBtu/SF] \"","v":"Typical Miscellaneous Loads for Office and Office [kBtu/SF] "},null,null,null,{"$f":"\"Typical EFLH for \"&IF(INDEX('General Information'!$F$17:$F$21,2,1)=\"\",INDEX('General Information'!$F$17:$F$21,1,1),INDEX('General Information'!$F$17:$F$21,1,1)&\" and \"&INDEX('General Information'!$F$17:$F$21,2,1))","v":"Typical EFLH for "}]
[null,"A",null,null,"B",null,null,"C",null,null,null,"E"]
["Baseline Design",{"$f":"IFERROR(SUMIF('12 - Performance_Outputs_1'!AI209:AI264,1,'12 - Performance_Outputs_1'!U209:U264)*1000/BuildingArea,\"-\")","v":"-"},null,null,{"$f":"IFERROR(SUMIF('12 - Performance_Outputs_1'!AJ209:AJ264,1,'12 - Performance_Outputs_1'!U209:U264)*1000/BuildingArea,\"-\")","v":"-"},null,null,{"$f":"IFERROR(SUM('General Information'!T17:T20),\"-\")","v":"-"},null,null,null,{"$f":"IFERROR(SUM('General Information'!U17:U20),$DR$27)","v":5033.375}]
["Proposed Design",{"$f":"IFERROR(SUMIF('12 - Performance_Outputs_1'!AI209:AI264,1,'12 - Performance_Outputs_1'!V209:V264)*1000/BuildingArea,\"-\")","v":"-"},null,null,{"$f":"IFERROR(SUMIF('12 - Performance_Outputs_1'!AJ209:AJ264,1,'12 - Performance_Outputs_1'!V209:V264)*1000/BuildingArea,\"-\")","v":"-"},null,null,"NA",null,null,null,"NA"]
["Proposed/Baseline",{"$f":"IFERROR(B115/B114,\"-\")","v":"-"},null,null,{"$f":"IFERROR(E115/E114,\"-\")","v":"-"},null,null,"NA",null,null,null,"NA"]
["Issue",null,null,null,null,null,"Project Team Response"]
[{"$f":"IFERROR(IF(SUM('12 - Performance_Outputs_1'!$AK$209:$AK$264)>0.01,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},"One (or more) of the unregulated end uses differs by more than 1% between the baseline and proposed as reported in the Performance Outputs tab. If savings are being documented for an unregulated end use, the Exceptional Calculation Method documentation must be included in the submittal."]
[{"$f":"IFERROR(IF((ABS(E114-H114)/MIN(E114,H114))>0.2,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},{"$f":"\"Modeled Miscellaneous Loads differs from typical for \"&J114&\" building type(s) by more than 20%. Please review model inputs related to plug and process loads, and explain the sources of the relevant assumptions, such as plug and process loads.\"","v":"Modeled Miscellaneous Loads differs from typical for  building type(s) by more than 20%. Please review model inputs related to plug and process loads, and explain the sources of the relevant assumptions, such as plug and process loads."}]
["Service Water Heating (SWH)"]
["Input/Output Summary"]
[null,"Annual Service Water Heating Use MMBtu/Yr\n(12 - Performance_Outputs_1)",null,"Heater Capacity [kBtu/Hr] \n(8 - Service Water Heating)","Annual Effective Full Load Hours","Typical Effective Full Load Hours","Heater Efficiency","Annual Service Water Heating Load MMBtu/Yr \n(12 - Performance Outputs 1 tab)",null,"Annual Service Water Heating Site EUI [kBtu/SF] \n(12 - Performance Outputs tab)",null,{"$f":"\"Typical EFLH for \"&IF(INDEX('General Information'!$F$17:$F$21,2,1)=\"\",INDEX('General Information'!$F$17:$F$21,1,1),INDEX('General Information'!$F$17:$F$21,1,1)&\" and \"&INDEX('General Information'!$F$17:$F$21,2,1))&\"  [kBtu/SF]\"","v":"Typical EFLH for   [kBtu/SF]"}]
[null,"A",null,"B","C = A / B","D","E","F = A * E",null,"G=A*1000 / Conditioned Floor Area",null,"H"]
["Baseline Design",{"$f":"IFERROR('12 - Performance_Outputs_1'!G237*'12 - Performance_Outputs_1'!Q237+'12 - Performance_Outputs_1'!G239*'12 - Performance_Outputs_1'!Q239,\"-\")","v":"-"},null,{"$f":"IFERROR('8 - Service Water Heating'!BD15,\"-\")","v":"-"},{"$f":"IFERROR(B124/D124*1000,\"-\")","v":"-"},{"$f":"IFERROR(SUM('General Information'!V17:V20),$DU$27)","v":2000.4285714285713},{"$f":"IFERROR('8 - Service Water Heating'!BE15,\"-\")","v":"-"},{"$f":"IFERROR(B124*G124,\"-\")","v":"-"},null,{"$f":"IFERROR(B124*1000/BuildingArea,\"-\")","v":"-"},null,{"$f":"IFERROR(Y53,\"-\")","v":"-"}]
["Proposed Design",{"$f":"IFERROR('12 - Performance_Outputs_1'!H237*'12 - Performance_Outputs_1'!Q237+'12 - Performance_Outputs_1'!H239*'12 - Performance_Outputs_1'!Q239,\"-\")","v":"-"},null,{"$f":"IFERROR('8 - Service Water Heating'!BD16,\"-\")","v":"-"},"NA","NA",{"$f":"'8 - Service Water Heating'!BE16","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(B125*G125,\"-\")","v":"-"},null,{"$f":"IFERROR(B125*1000/BuildingArea,\"-\")","v":"-"},null,"NA"]
["Proposed/Baseline",{"$f":"IFERROR(B125/B124,\"-\")","v":"-"},null,{"$f":"IFERROR(D125/D124,\"-\")","v":"-"},"NA","NA",{"$f":"IFERROR(G125/G124,\"-\")","v":"-"},{"$f":"IFERROR(H125/H124,\"-\")","v":"-"},null,{"$f":"IFERROR(J125/J124,\"-\")","v":"-"},null,{"$f":"IFERROR(L125/L124,\"-\")","v":"-"}]
["Issue",null,null,null,null,null,"Project Team Response"]
[{"$f":"IFERROR(IF(((J124-L124)/L124)>0.25,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},"The baseline SWH site EUI differs from typical by more than 25%. Please review the inputs related to service water heating use, such as the amount of hot water used in the building (the design flow rate and schedule), temperature of water entering water heater, water heater efficiency, and stand-by losses."]
[{"$f":"IFERROR(IF(ABS((H124-H125)/H125)>0.02,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},"Annual Service Water Heating Load differs between baseline and proposed design. Please explain what factors other than heater efficiency affected SWH energy use in the baseline and proposed design. "]
[{"$f":"IFERROR(IF(((E124-F124)/F124)>0.25,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},"Effective full load hours (C) exceed typical by more than 25%, which may indicate that the modeled demand is high relative to the specified service water heater capacity. Please review the service water heater capacity and hot water demand (e.g. flow rate and schedule) to justify the result. The modeled service water heater energy use may be exaggerated."]
[{"$f":"IFERROR((IF(OR(J124<0.75*L124,J124>1.25*L124),\"Please Explain\",\"Pass\")),\"Please Explain\")","v":"Please Explain"},"The modeled annual service water heating use (G) differs from typical (H) by more than 25%. Please provide an explanation to justify the difference, or adjust the modeled hot water load."]
["Air-Side HVAC"]
["Input/Output Summary"]
[null,"Hours per Year HVAC Runs in Occupied Mode (Schedules tab, average specified) ","Total Fan kW of Constant Volume (CV) systems (10 - Air-side HVAC) ","Total Fan kW of VAV systems (10 - Air-side HVAC) ","Total Fan kW (10 - Air-side HVAC) ","Fan Peak Demand\n(12 - Performance Outputs 1 tab, Fan - Interior Ventilation kW)","Total Supply CFM (10 - Air-side HVAC)","Total OA CFM (10 - Air-side HVAC) ",null,"Total Indoor Fan Energy Use (12- Performance Outputs tab, Fans - Interior Ventilation) kWh",null,"Indoor Fans Effective Full Load Hours (EFLH), hr/yr","Total Cooling Capacity (10 - Air-side HVAC) Ton"]
[null,"A","B","C","D = B + C","E","F","G",null,"H",null,"I = H / E","J"]
["Baseline Design",{"$f":"AVERAGE('2a - Schedules'!O12:O19)","v":8760},{"$f":"'10a - Baseline Air-Side HVAC'!G64","v":0},{"$f":"'10a - Baseline Air-Side HVAC'!G65","v":0},{"$f":"C136+D136","v":0},{"$f":"'12 - Performance_Outputs_1'!G232","v":""},{"$f":"'10a - Baseline Air-Side HVAC'!E23","v":"0"},{"$f":"'10a - Baseline Air-Side HVAC'!E24","v":"0"},null,{"$f":"'12 - Performance_Outputs_1'!G231","v":""},null,{"$f":"IFERROR(J136/F136,\"-\")","v":"-"},{"$f":"'10a - Baseline Air-Side HVAC'!E14/DropdownData!G8","v":0}]
["Proposed Design",{"$f":"AVERAGE('2a - Schedules'!O12:O19)","v":8760},{"$f":"'10b - Proposed Air-Side HVAC'!F34","v":0},{"$f":"'10b - Proposed Air-Side HVAC'!F35","v":0},{"$f":"C137+D137","v":0},{"$f":"'12 - Performance_Outputs_1'!H232","v":0},{"$f":"'10b - Proposed Air-Side HVAC'!D22","v":"0"},{"$f":"'10b - Proposed Air-Side HVAC'!D23","v":"0"},null,{"$f":"'12 - Performance_Outputs_1'!H231","v":0},null,{"$f":"IFERROR(J137/F137,\"-\")","v":"-"},{"$f":"'10b - Proposed Air-Side HVAC'!D14/DropdownData!G8","v":0}]
["Proposed/Baseline",{"$f":"IFERROR(B137/B136,\"-\")","v":1},"-","-","-",{"$f":"IFERROR(F137/F136,\"-\")","v":"-"},"-","-",null,{"$f":"IFERROR(J137/J136,\"-\")","v":"-"},null,{"$f":"IFERROR(L137/L136,\"-\")","v":"-"},{"$f":"IFERROR(M137/M136,\"-\")","v":"-"}]
["Issue",null,null,null,null,null,"Project Team Response"]
[{"$f":"IFERROR(IF(OR(AND('General Information'!N16=\"Multifamily\",('General Information'!G23+'General Information'!H23)/'Quality Assurance Checks'!M136<400),AND('General Information'!N15=FALSE,('General Information'!G23+'General Information'!H23)/'Quality Assurance Checks'!M136<280)),\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},{"$f":"AB140&ROUND(('General Information'!G23+'General Information'!H23)/'Quality Assurance Checks'!M136,0)&\" sf/ton\"&AB142","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Baseline cooling capacity appears unrealistically high. Cooling capacity in square feet per Ton is typically 400-450 for residential and 280 – 360 for non-residential buildings such as offices.  Based on the inputs on “10 - Air-Side HVAC” tab, the cooling capacity of all baseline systems is "]
[{"$f":"IFERROR(IF(AND(VLOOKUP('General Information'!C46,AF153:AG187,2,FALSE)=\"no\",'12 - Performance_Outputs_1'!G219=\"\"),\"Pass\",IF(AND(VLOOKUP('General Information'!C46,AF153:AG187,2,FALSE)=\"only\",'12 - Performance_Outputs_1'!G2107=\"\"),\"Pass\",\"Please Explain\")),\"Please Explain\")","v":"Pass"},{"$f":"AB154&'General Information'!C46&'Quality Assurance Checks'!AC154&VLOOKUP('General Information'!C46,AF153:AG187,2,FALSE)&'Quality Assurance Checks'!AD154","v":"Project is located in climate zone 4A, thus the baseline is expected to have no electric heating based on Table G3.1.1-3. However, based on the information shown on the Performance Outputs tab, other fuels are shown under Space Heating end use for the baseline. Please review and update the baseline model to use the appropriate heating fuel source."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,". Exaggerated cooling load may be due to higher than expected modeled peak equipment load (e.g. equipment schedule that turns unrealistically high fraction of equipment design load during a particular hour), cooling thermostat schedule leading to higher than expected load when the building switches from un-occupied to occupied, or incorrect cooling system sizing. ",null,null,null,"CZ","Electric Heat Table G3.1.1-3"]
[{"$f":"IFERROR(IF(OR(AND('General Information'!N16=\"Multifamily\",'Quality Assurance Checks'!G136/('General Information'!G23+'General Information'!H23)>0.8),AND('General Information'!N15=FALSE,('Quality Assurance Checks'!G136/'General Information'!G23+'General Information'!H23)>1.6)),\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},"Baseline supply air flow CFM appears unrealistically high. Typical ranges are 0.5 CFM/SF - 0.8 CFM/SF in apartments, and 0.8 CFM/SF – 1.6 CFM/SF in offices. Please confirm that the supply flow was sized based on supply-air-to-room temperature difference of 20°F or the minimum baseline ventilation rate, whichever is greater (G3.1.2.8), and that the over-sizing factor was not applied to the flow rate (G3.1.2.2).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,". Exaggerated cooling load may be due to higher than expected modeled peak equipment load (e.g. equipment schedule that turns unrealistically high fraction of equipment design load during a particular hour), cooling thermostat schedule leading to higher than expected load when the building switches from un-occupied to occupied temperature, or incorrect cooling system sizing. "]
[{"$f":"IF(AND('10a - Baseline Air-Side HVAC'!E30='10b - Proposed Air-Side HVAC'!D30,'10a - Baseline Air-Side HVAC'!E31='10b - Proposed Air-Side HVAC'!D31,'10a - Baseline Air-Side HVAC'!E32='10b - Proposed Air-Side HVAC'!D32),\"Pass\",\"Please Explain\")","v":{"$error":"#DIV/0!"}},"Based on the inputs on Tabs 10a and 10b, the baseline system fan power is not distributed to the supply, return, exhaust and relief fans in the same proportion as the proposed design, and does not meet G3.1.2.9.1. Please update the inputs in these tabs and the model, or explain."]
[{"$f":"IF(F136>1.01*E136,\"Please Explain\",\"Pass\")","v":"Please Explain"},"Modeled Baseline fan peak demand (E) exceeds the total baseline fan power listed in the Air-side HVAC tabs. Please review and adjust the inputs in the Air-side HVAC tabs and/or in the model to eliminate the discrepancy."]
[{"$f":"IF((C136*B136/E136+D136*0.3/E136)<L137*0.85,\"Please Explain\",\"Pass\")","v":{"$error":"#DIV/0!"}},{"$f":"AB145&IFERROR((C133*B133/E133+D133*0.3/E133),B133)&AB146","v":"The baseline fan EFLH appears low. EFLH for CV systems is expected to be similar to the number of hours per year the building is occupied. Average flow rate of VAV systems is typically 50% of the design, with the fan system drawing ~ 30% of the design power, and thus the EFLH approximately equal to 30% of hours the building is occupied. Based on this rule of thumb, the estimated EFLH for the project are  (B*A/D+C*0.3/D), and are more than 15% lower than reported. Please review the baseline fan power inputs, flow controls (CV vs VAV), and operation mode (continuous versus cycling)."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"The baseline fan EFLH appears low. EFLH for CV systems is expected to be similar to the number of hours per year the building is occupied. Average flow rate of VAV systems is typically 50% of the design, with the fan system drawing ~ 30% of the design power, and thus the EFLH approximately equal to 30% of hours the building is occupied. Based on this rule of thumb, the estimated EFLH for the project are "]
[{"$f":"IFERROR(IF(AND('9 - General HVAC'!I24>=1,'12 - Performance_Outputs_1'!AN219<1),\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},"Based on the inputs on “10 - Air-Side HVAC” tab, the proposed design has heating systems that use electricity, however no electricity space heating use is shown on the Performance Outputs tab. Please update the model to ensure that all specified heating systems are included, and that their use is realistically captured. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," (B*A/D+C*0.3/D), and are more than 15% lower than reported. Please review the baseline fan power inputs, flow controls (CV vs VAV), and operation mode (continuous versus cycling)."]
[{"$f":"IF(F137>E137,\"Please Explain\",\"Pass\")","v":"Pass"},"Modeled Proposed fan peak demand (E) exceeds the total proposed fan power listed in the Air-side HVAC tabs. Please review and adjust the inputs in the Air-side HVAC tabs and/or in the model to eliminate the discrepancy."]
[{"$f":"IF(F137<E137*(1-0.15),\"Please Explain\",\"Pass\")","v":"Pass"},"Proposed fan peak demand (E) in the Performance Outputs tab is low relative to the total fan system power listed on “10 - Air-Side HVAC” tab. The fan peak demand for Constant Volume (CV) systems is expected to be approximately equal to 100% of fan power.  The fan peak demand for Variable Air Volume systems (VAV) is expected to be approximately equal to 50% of fan power (assuming peak flow of ~70%). However, the reported peak demand is 15% below this estimated value. Please review the fan power inputs and confirm that all proposed fans including supply, return, exhaust, and relief were properly modeled.  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Long Comments"]
[{"$f":"IF((C137*B137/E137+D137*0.3/E137)>L137*1.15,\"Please Explain\",\"Pass\")","v":{"$error":"#DIV/0!"}},{"$f":"AB149&IFERROR((C137*B137/E137+D137*0.3/E137),B137)&AB150","v":"The proposed fan EFLH appears low. EFLH for CV systems is expected to be similar to the number of hours per year the building is occupied. Average flow rate of VAV systems is typically 50% of the design, with the fan system drawing ~ 30% of the design power, and thus the EFLH approximately equal to 30% of hours the building is occupied. Based on this rule of thumb, the estimated EFLH for the project are 8760 (B*A/D+C*0.3/D), and are more than 15% higher than reported. Please review the proposed fan power inputs, flow controls (CV vs VAV), and operation mode (continuous versus cycling)."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"The proposed fan EFLH appears low. EFLH for CV systems is expected to be similar to the number of hours per year the building is occupied. Average flow rate of VAV systems is typically 50% of the design, with the fan system drawing ~ 30% of the design power, and thus the EFLH approximately equal to 30% of hours the building is occupied. Based on this rule of thumb, the estimated EFLH for the project are "]
[{"$f":"IFERROR(IF(OR(ABS((L136-L137)/L136)>0.25,B136>8760,B137>8760,L136>8760,L137>8760),\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},"The baseline and proposed fan EFLH differs by more than 25%, which is unexpected. Please ensure that the HVAC system models reflect all mandatory controls from Section 6, continuous versus cycling fan operation is correctly captured for each model, and that the same occupied hours were modeled for the baseline and proposed design, based on the anticipated building operation.  In addition, EFLH cannot exceed 8760 hours per year.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," (B*A/D+C*0.3/D), and are more than 15% higher than reported. Please review the proposed fan power inputs, flow controls (CV vs VAV), and operation mode (continuous versus cycling)."]
[{"$f":"IFERROR(IF(ABS(G136-G137)/G136>0.35,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},"The total baseline and proposed air flow rates differ by more than 35% (as reported in the Air-Side HVAC tab). Please confirm that the baseline fan air flow rate was sized based on a 20 deg. F supply-air-to-room-air temperature difference, as required by G3.1.2.8.1 for each baseline system, and that the over-sizing factor was not applied to the flow (G3.1.2.2). Verify that the proposed flow rate has been modeled as shown in the design documents."]
[{"$f":"IF(ABS(H136-H137)/H137>0.01,\"Please Explain\",IF(ABS(H137-H136)/H136>0.01,\"Please Explain\",\"Pass\"))","v":{"$error":"#DIV/0!"}},"The outdoor airflow rate (G) differs between the baseline and proposed design. Please explain which of the exceptions to G3.1.2.4 apply to the project."]
["Water-Side HVAC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,". Exaggerated cooling load may be due to higher than expected modeled peak equipment load (e.g. equipment schedule that turns unrealistically high fraction of equipment design load during a particular hour), cooling thermostat schedule leading to higher than expected load when the building switches from un-occupied to occupied, or incorrect cooling system sizing. ",null,null,null,"1A","only"]
["Input/Output Summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Project is located in climate zone ",", thus the baseline is expected to have "," electric heating based on Table G3.1.1-3. However, based on the information shown on the Performance Outputs tab, other fuels are shown under Space Heating end use for the baseline. Please review and update the baseline model to use the appropriate heating fuel source.",null,"1B","only"]
[null,"Hours per Year HVAC Runs in Occupied Mode (Schedules tab, average specified) ",null,"Total Pump  kW (from 11-Water-side HVAC","Total Pump peak demand kW (from 12 - Performance Outputs)",null,"Total Pump energy kWh (from 12 - Performance Outputs)",null,"Total Heat Rejection peak demand kW (from 12 - Performance Outputs)",null,"Total Heat Rejection energy kWh (from 12 - Performance Outputs)",null,"Pump Effective Full Load Hours (EFLH), hr/yr",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Based on “11 – Water Side HVAC” tab, the total baseline design pump power (B) including chilled water pumps, hot water pumps, and condenser loop pumps is ",null,null,null,"2A","only"]
[null,"A",null,"B","C",null,"D",null,"E",null,"F",null,"G=D/E",null,null,null,null,null,null,null,null,null,null,null,null,null,null,". This exceeds 85% of peak demand for pump end use (C) reported on the “Performance Outputs” tab. Please review baseline model inputs related to pump power and loop controls.",null,null,null,"2B","only"]
["Baseline Design",{"$f":"AVERAGE('2a - Schedules'!O12:O18)","v":8760},null,{"$f":"'11 - Water-Side HVAC'!Z11","v":0},{"$f":"'12 - Performance_Outputs_1'!G228","v":""},null,{"$f":"'12 - Performance_Outputs_1'!G227","v":""},null,{"$f":"IF('12 - Performance_Outputs_1'!G230=\"\",\"-\")","v":"-"},null,{"$f":"IF('12 - Performance_Outputs_1'!G229=\"\",\"-\")","v":"-"},null,{"$f":"IFERROR(G157/E157,\"-\")","v":"-"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3A","only"]
["Proposed Design",{"$f":"AVERAGE('2a - Schedules'!O12:O18)","v":8760},null,{"$f":"'11 - Water-Side HVAC'!Z12","v":0},{"$f":"'12 - Performance_Outputs_1'!H228","v":0},null,{"$f":"'12 - Performance_Outputs_1'!H227","v":0},null,{"$f":"'12 - Performance_Outputs_1'!H230","v":0},null,{"$f":"'12 - Performance_Outputs_1'!H229","v":0},null,{"$f":"IFERROR(G158/E158,\"-\")","v":"-"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3B","no"]
["Proposed/Baseline",{"$f":"IFERROR(B158/B157,\"-\")","v":1},null,{"$f":"IFERROR(D158/D157,\"-\")","v":"-"},{"$f":"IFERROR(E158/E157,\"-\")","v":"-"},null,{"$f":"IFERROR(G158/G157,\"-\")","v":"-"},null,{"$f":"IFERROR(I158/I157,\"-\")","v":"-"},null,{"$f":"IFERROR(K158/K157,\"-\")","v":"-"},null,{"$f":"IFERROR(M158/M157,\"-\")","v":"-"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3C","no"]
["Issue",null,null,null,null,null,"Project Team Response",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Baseline systems",null,null,null,"4A","no"]
[{"$f":"IFERROR(IF(AND('9 - General HVAC'!Q27>0,'11 - Water-Side HVAC'!G58=\"\"),\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},"Projects with baseline System 1, 5, 7 or 10 are expected to have a baseline heating pump entered  on the 11 - Water-Side HVAC tab. Currently there is no entry, or the baseline heating pump power is equal to 0 kW. Please revise the heating pump power input on the 11- Water-Side HVAC tab.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('9 - General HVAC'!J28=\"\",\"\",'9 - General HVAC'!J28)","v":""},{"$f":"IF(AB161=0,\"\",\"System \"&AB161)","v":"System "},null,null,"4B","no"]
[{"$f":"IFERROR(IF(AND('9 - General HVAC'!R27>0,'11 - Water-Side HVAC'!G21=\"\"),\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},"Projects with baseline System 7, 8, 11 or 12 are expected to have a baseline chilled water pump entered  on the 11 - Water-Side HVAC tab. Currently there is no entry, or the baseline chilled water pump power is equal to 0 kW. Please revise the chilled water pump power input on the 11- Water-Side HVAC tab.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('9 - General HVAC'!J29=\"\",\"\",'9 - General HVAC'!J29)","v":""},{"$f":"IF(AB162=0,\"\",\"System \"&AB162)","v":"System "},null,null,"4B","no"]
[{"$f":"IFERROR(IF(AND('9 - General HVAC'!R27>0,'11 - Water-Side HVAC'!G42=\"\"),\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},"Projects with baseline System 7, 8, 11 or 12 are expected to have a baseline condenser water pump entered  on the 11 - Water-Side HVAC tab. Currently there is no entry, or the baseline condenser water pump power is equal to 0 kW. Please revise the condenser water pump power input on the 11- Water-Side HVAC tab.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('9 - General HVAC'!J30=\"\",\"\",'9 - General HVAC'!J30)","v":0},"",null,null,"4B","no"]
[{"$f":"IFERROR(IF('9 - General HVAC'!M31=TRUE,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},{"$f":"\"Project baseline includes Systems \"&AC164&\" \"&AC165&\" \"&AC166&\" \"&AC168&\" \"&AC167&\" \"&AC169&\". These systems do not have pumps, however pump energy is reported on the Performance Output tab for the baseline. Please review the baseline model inputs, or explain.\"","v":"Project baseline includes Systems    System   System . These systems do not have pumps, however pump energy is reported on the Performance Output tab for the baseline. Please review the baseline model inputs, or explain."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('9 - General HVAC'!J31=\"\",\"\",'9 - General HVAC'!J31)","v":0},"",null,null,"4B","no"]
[{"$f":"IFERROR(IF('9 - General HVAC'!O31=TRUE,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},{"$f":"\"Project baseline includes \"&AC164&\" \"&AC165&\" \"&AC166&\" \"&AC168&\" \"&AC167&\" \"&AC169&\". These systems do not have cooling tower, however Heat rejection energy is reported on the Performance Output tab for the baseline. Please review the baseline model inputs, or explain. \"","v":"Project baseline includes    System   System . These systems do not have cooling tower, however Heat rejection energy is reported on the Performance Output tab for the baseline. Please review the baseline model inputs, or explain. "},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('9 - General HVAC'!J32=\"\",\"\",'9 - General HVAC'!J32)","v":0},"",null,null,"4C","no"]
[{"$f":"IFERROR(IF(D157>0.85*E157,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},{"$f":"AB155&D157&AB156","v":"Based on “11 – Water Side HVAC” tab, the total baseline design pump power (B) including chilled water pumps, hot water pumps, and condenser loop pumps is 0. This exceeds 85% of peak demand for pump end use (C) reported on the “Performance Outputs” tab. Please review baseline model inputs related to pump power and loop controls."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('9 - General HVAC'!J33=\"\",\"\",'9 - General HVAC'!J33)","v":0},"",null,null,"5A","no"]
[{"$f":"IFERROR(IF(M157>0.75*B157,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},{"$f":"AJ167&ROUND(B157,0)&AK167","v":"The baseline pump EFLH appear high. The building is occupied 8760 hours per year when HVAC system are running in occupied mode. Assuming that pumps run at 100% of design load 1% of the time, at 75% of the design load 42% of the time, 50% of design load 45% of the time, and 25% of design load 12% of design, the weighted average Watt of the pump riding pump curve is ~ 78% of the design, and pumps with VSD is 43% of design. However, based on the simulation results, the EFLH of the pumps exceeds 75% of the hours the building is occupied, which is unexpected. Please review the baseline pump power input, flow control (i.e. whether VSD is specified), and confirm that two-way valves were modeled to reflect the continuous variable flow (G3.1.3.5, G3.1.3.10)."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('9 - General HVAC'!J34=\"\",\"\",'9 - General HVAC'!J34)","v":0},"",null,null,"5C","no",null,null,"The baseline pump EFLH appear high. The building is occupied "," hours per year when HVAC system are running in occupied mode. Assuming that pumps run at 100% of design load 1% of the time, at 75% of the design load 42% of the time, 50% of design load 45% of the time, and 25% of design load 12% of design, the weighted average Watt of the pump riding pump curve is ~ 78% of the design, and pumps with VSD is 43% of design. However, based on the simulation results, the EFLH of the pumps exceeds 75% of the hours the building is occupied, which is unexpected. Please review the baseline pump power input, flow control (i.e. whether VSD is specified), and confirm that two-way valves were modeled to reflect the continuous variable flow (G3.1.3.5, G3.1.3.10)."]
[{"$f":"IFERROR(IF(D158>0.85*E158,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},{"$f":"\"Based on “11 – Water Side HVAC” tab, the total proposed design pump power (B) including chilled water pumps, hot water pumps, and condenser loop pumps is \"&D158&\". This exceeds 85% of peak demand for pump end use (C) reported on the “Performance Outputs” tab. Please review baseline model inputs related to pump power and loop controls.\"","v":"Based on “11 – Water Side HVAC” tab, the total proposed design pump power (B) including chilled water pumps, hot water pumps, and condenser loop pumps is 0. This exceeds 85% of peak demand for pump end use (C) reported on the “Performance Outputs” tab. Please review baseline model inputs related to pump power and loop controls."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('9 - General HVAC'!J35=\"\",\"\",'9 - General HVAC'!J35)","v":""},"System ",null,null,"5B","no"]
[{"$f":"IFERROR(IF(M158<0.35*B158,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},{"$f":"AJ169&ROUND(B158,0)&AK169","v":"The proposed pump EFLH appears low. The building is occupied 8760 hours per year when HVAC system are running in occupied mode. Assuming that pumps run at 100% of design load 1% of the time, at 75% of the design load 42% of the time, 50% of design load 45% of the time, and 25% of design load 12% of design, the weighted average Watt of the pump riding pump curve is ~ 78% of the design, and pumps with VSD is 43% of design, and pump with VSD and differential pressure reset controls is 34%. However, based on the simulation results, the EFLH of the proposed pumps is less than 35% of the hours the building is occupied, which is unexpected. Please review the proposed pump power input, flow control (i.e. whether VSD is specified), and confirm that CHW, CW, and HW loop design (primary/secondary, and  variable / constant flow) is reflected in the proposed design model. "},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('9 - General HVAC'!J36=\"\",\"\",'9 - General HVAC'!J36)","v":""},"System ",null,null,"6A","no",null,null,"The proposed pump EFLH appears low. The building is occupied "," hours per year when HVAC system are running in occupied mode. Assuming that pumps run at 100% of design load 1% of the time, at 75% of the design load 42% of the time, 50% of design load 45% of the time, and 25% of design load 12% of design, the weighted average Watt of the pump riding pump curve is ~ 78% of the design, and pumps with VSD is 43% of design, and pump with VSD and differential pressure reset controls is 34%. However, based on the simulation results, the EFLH of the proposed pumps is less than 35% of the hours the building is occupied, which is unexpected. Please review the proposed pump power input, flow control (i.e. whether VSD is specified), and confirm that CHW, CW, and HW loop design (primary/secondary, and  variable / constant flow) is reflected in the proposed design model. "]
["Other",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,". Exaggerated cooling load may be due to higher than expected modeled peak equipment load (e.g. equipment schedule that turns unrealistically high fraction of equipment design load during a particular hour), cooling thermostat schedule leading to higher than expected load when the building switches from un-occupied to occupied, or incorrect cooling system sizing. ",null,null,null,"6B","no"]
["Issue",null,null,null,null,null,"Project Team Response",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"7A","no"]
[{"$f":"IF('12 - Performance_Outputs_1'!AD29=FALSE,\"Pass\",IFERROR(IF((IFERROR(MAX(IFERROR(OFFSET(PO_renewable_table,MATCH(\"Photovoltaic system\",PO_renewable_Index,0)-2,MATCH($S$35,PO_renewable_hdr,0)-1,1,1),0),\nIFERROR(OFFSET(PO_renewable_table,MATCH(\"Solar thermal system\",PO_renewable_Index,0)-2,MATCH($S$35,PO_renewable_hdr,0)-1,1,1),0)),\"\"))=\"\",\"Please Explain\",IF('12 - Performance_Outputs_1'!G449>1500,\"Please Explain\",\"Pass\")),\"Please Explain\"))","v":"Pass"},"The equivalent full load hours (determined by dividing the total annual consumption by the total rated capacity/power as reported in the Performance Outputs tab) for the photovoltaic system is greater than 1,500 hours/year, which is unexpectedly high. Provide documentation explaining the calculation method used to estimate the annual energy generated, and indicate all factors influencing the performance, such as derate factor, tilt, orientation, etc.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"7B","no"]
[{"$f":"IF(RatingSystemSelection=\"LEED v4 BD+C: Data Centers\",\"Please Explain\",\"Pass\")","v":"Pass"},"The rating system requires that a minimum of 2% of the energy savings must come from building power and cooling infrastructure. Provide a narrative describing how this requirement has been met. If necessary, include additional modeling output reports.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"no"]
["Utility Rates",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,". Exaggerated cooling load may be due to higher than expected modeled peak equipment load (e.g. equipment schedule that turns unrealistically high fraction of equipment design load during a particular hour), cooling thermostat schedule leading to higher than expected load when the building switches from un-occupied to occupied, or incorrect cooling system sizing. "]
["Input/Output Summary",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Project is located in climate zone ",", thus the baseline is expected to have "," electric heating based on Table G3.1.1-3. However, based on the information shown on the Performance Outputs tab, other fuels are shown under Space Heating end use for the baseline. Please review and update the baseline model to use the appropriate heating fuel source.",null,"1B","only"]
[null,null,null,{"$f":"IF('12 - Performance_Outputs_1'!C17=\"\",\"-\",'12 - Performance_Outputs_1'!B17)","v":"-"},null,null,{"$f":"IF('12 - Performance_Outputs_1'!C18=\"\",\"-\",'12 - Performance_Outputs_1'!B18)","v":"-"},null,null,{"$f":"IF('12 - Performance_Outputs_1'!C19=\"\",\"-\",'12 - Performance_Outputs_1'!B19)","v":"-"},null,null,{"$f":"IF('12 - Performance_Outputs_1'!C20=\"\",\"-\",'12 - Performance_Outputs_1'!B20)","v":"-"}]
[null,{"$f":"IF('12 - Performance_Outputs_1'!C17=\"\",\"-\",'12 - Performance_Outputs_1'!B17&\" Virtual Rate\")","v":"-"},null,null,{"$f":"IF('12 - Performance_Outputs_1'!C18=\"\",\"-\",'12 - Performance_Outputs_1'!B18&\" Virtual Rate\")","v":"-"},null,null,{"$f":"IF('12 - Performance_Outputs_1'!C19=\"\",\"-\",'12 - Performance_Outputs_1'!B19&\" Virtual Rate\")","v":"-"},null,null,{"$f":"IF('12 - Performance_Outputs_1'!C20=\"\",\"-\",'12 - Performance_Outputs_1'!B20&\" Virtual Rate\")","v":"-"}]
[null,{"$f":"IF('12 - Performance_Outputs_1'!C17=\"\",\"-\",\"$/\"&'12 - Performance_Outputs_1'!C17&\" (Performance Outputs tab, Table 12.8)\")","v":"-"},{"$f":"IF('12 - Performance_Outputs_1'!C17=\"\",\"-\",'12 - Performance_Outputs_1'!C17&\" to Site MMBtu Conversion (Performance Outputs tab Table 12.1)\")","v":"-"},{"$f":"IF('12 - Performance_Outputs_1'!C17=\"\",\"-\",\"$/MMBtu\")","v":"-"},{"$f":"IF('12 - Performance_Outputs_1'!C18=\"\",\"-\",\"$/\"&'12 - Performance_Outputs_1'!C18&\" (Performance Outputs tab, Table 12.8)\")","v":"-"},{"$f":"IF('12 - Performance_Outputs_1'!C18=\"\",\"-\",'12 - Performance_Outputs_1'!C18&\" to Site MMBtu Conversion (Performance Outputs tab Table 12.1)\")","v":"-"},{"$f":"IF('12 - Performance_Outputs_1'!C18=\"\",\"-\",\"$/MMBtu\")","v":"-"},{"$f":"IF('12 - Performance_Outputs_1'!C19=\"\",\"-\",\"$/\"&'12 - Performance_Outputs_1'!C19&\" (Performance Outputs tab, Table 12.8)\")","v":"-"},{"$f":"IF('12 - Performance_Outputs_1'!C19=\"\",\"-\",'12 - Performance_Outputs_1'!C19&\" to Site MMBtu Conversion (Performance Outputs tab Table 12.1)\")","v":"-"},{"$f":"IF('12 - Performance_Outputs_1'!C19=\"\",\"-\",\"$/MMBtu\")","v":"-"},{"$f":"IF('12 - Performance_Outputs_1'!C20=\"\",\"-\",\"$/\"&'12 - Performance_Outputs_1'!C20&\" (Performance Outputs tab, Table 12.8)\")","v":"-"},{"$f":"IF('12 - Performance_Outputs_1'!C20=\"\",\"-\",'12 - Performance_Outputs_1'!C20&\" to Site MMBtu Conversion (Performance Outputs tab Table 12.1)\")","v":"-"},{"$f":"IF('12 - Performance_Outputs_1'!C20=\"\",\"-\",\"$/MMBtu\")","v":"-"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Based on “11 – Water Side HVAC” tab, the total baseline design pump power (TPW) including chilled water pumps, hot water pumps, and condenser loop pumps is ",null,null,null,"2A","only"]
[null,"A","B","C","D","E","F","G","H","I","J","K","L",null,null,null,null,null,null,null,null,null,null,null,null,null,null,". This exceeds 85% of peak demand for pump end use (PD) reported on the “Performance Outputs” tab. Please review baseline model inputs related to pump power and loop controls.",null,null,null,"2B","only"]
["Baseline Design",{"$f":"IFERROR('12 - Performance_Outputs_1'!E282,\"-\")","v":""},{"$f":"IFERROR('12 - Performance_Outputs_1'!K17,\"-\")","v":""},{"$f":"IFERROR(B180/C180,\"-\")","v":"-"},{"$f":"IFERROR('12 - Performance_Outputs_1'!E283,\"-\")","v":""},{"$f":"IFERROR('12 - Performance_Outputs_1'!K18,\"-\")","v":""},{"$f":"IFERROR(E180/F180,\"-\")","v":"-"},{"$f":"IFERROR('12 - Performance_Outputs_1'!E284,\"-\")","v":""},{"$f":"IFERROR('12 - Performance_Outputs_1'!K19,\"-\")","v":""},{"$f":"IFERROR(H180/I180,\"-\")","v":"-"},{"$f":"IFERROR('12 - Performance_Outputs_1'!E285,\"-\")","v":""},{"$f":"IFERROR('12 - Performance_Outputs_1'!K20,\"-\")","v":""},{"$f":"IFERROR(K180/L180,\"-\")","v":"-"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3A","only"]
["Proposed Design",{"$f":"IFERROR('12 - Performance_Outputs_1'!H282,\"-\")","v":""},{"$f":"IFERROR('12 - Performance_Outputs_1'!K17,\"-\")","v":""},{"$f":"IFERROR(B181/C181,\"-\")","v":"-"},{"$f":"IFERROR('12 - Performance_Outputs_1'!H283,\"-\")","v":""},{"$f":"IFERROR('12 - Performance_Outputs_1'!K18,\"-\")","v":""},{"$f":"IFERROR(E181/F181,\"-\")","v":"-"},{"$f":"IFERROR('12 - Performance_Outputs_1'!E284,\"-\")","v":""},{"$f":"IFERROR('12 - Performance_Outputs_1'!K19,\"-\")","v":""},{"$f":"IFERROR(H181/I181,\"-\")","v":"-"},{"$f":"IFERROR('12 - Performance_Outputs_1'!E285,\"-\")","v":""},{"$f":"IFERROR('12 - Performance_Outputs_1'!K20,\"-\")","v":""},{"$f":"IFERROR(K181/L181,\"-\")","v":"-"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3B","no"]
["Proposed/Baseline",{"$f":"IFERROR((B181/B180),\"-\")","v":"-"},{"$f":"IFERROR((C181/C180),\"-\")","v":"-"},"-","-","-","-","-","-","-","-","-","-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3C","no"]
["Issue",null,null,null,null,null,"Project Team Response"]
[{"$f":"IFERROR(IF(OR('12 - Performance_Outputs_1'!I449<0.06,'12 - Performance_Outputs_1'!I449>0.25),\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},"The proposed virtual energy rate for electricity is less than $0.06 per kWh or greater than $0.25 per kWh (as reported in the Performance Outputs tab), which is unexpected. Please correct or provide justification."]
[{"$f":"IFERROR(IF(OR('12 - Performance_Outputs_1'!J449<0.5,'12 - Performance_Outputs_1'!J449>2),\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Please Explain"},"The proposed virtual energy rate for natural gas is less than $0.50 per therm or greater than $2.00 per therm (as reported in the Performance Outputs tab), which is unexpected.  Please correct or provide justification."]
[{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,IF(COUNTIF(INDEX(PO_renewable_table,,MATCH('12 - Performance_Outputs_1'!$U$35,PO_renewable_hdr,0)),\">0.05\")+COUNTIF(INDEX(PO_renewable_table,,MATCH('12 - Performance_Outputs_1'!$U$35,PO_renewable_hdr,0)),\"<-0.05\")>0,\"Please Explain\",\"Pass\"),\"Pass\"),\"Please Explain\")","v":"Pass"},"The virtual energy rate for the renewable energy varies from the virtual energy rate for the proposed by more than 5% (as reported in the Performance Outputs tab), which is unexpected.  Please correct or provide justification."]
[{"$f":"IFERROR(IF(COUNTIF(INDEX(PO_Enrgy_8_Table,,MATCH('12 - Performance_Outputs_1'!$K$281,PO_Enrgy_8_Hdr,0)),\">0.1\")+COUNTIF(INDEX(PO_Enrgy_8_Table,,MATCH('12 - Performance_Outputs_1'!$K$281,PO_Enrgy_8_Hdr,0)),\"<-0.1\")>0,\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},"The virtual energy rate for one or more of the energy types varies by more than 10% (as reported in the Performance Outputs tab). Ensure that the energy rates have been determined using either actual rates or state average energy prices published by DOE's Energy Information Administration. Provide information regarding the utility rate structure including all demand and energy charges and the seasonal and time-of-use structure of the utility tariff."]
[{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,IF(COUNTIF(INDEX(PO_ExCalc_Table,,MATCH('12 - Performance_Outputs_1'!$U$64,PO_ExCalc_Hdr,0)),\">0.05\")+COUNTIF(INDEX(PO_ExCalc_Table,,MATCH('12 - Performance_Outputs_1'!$U$64,PO_ExCalc_Hdr,0)),\"<-0.05\")>0,\"Please Explain\",\"Pass\"),\"Pass\"),\"Please Explain\")","v":"Pass"},"The virtual energy rate for one or more exceptional calculation measures varies from the virtual energy rate for the proposed by more than 10% (as reported in the Performance Outputs tab), which is unexpected.  Please correct or provide justification."]
[{"$f":"IFERROR(IF((SUMIF(176:176,\"Electricity\",180:180))>5*(SUMIF(176:176,\"Natural Gas\",180:180)),\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},"The equivalent cost of 1 MMBtu (site energy) of electricity is more than 5 time greater than the cost of 1 MMBtu (site energy) of natural gas, which appears high. Please confirm that utility rates from the same source (i.e. either Energy Information Administration website, or actual utility rates at the project location) are used, and are modeled correctly."]
[{"$f":"IFERROR(IF((SUMIF(176:176,\"Electricity\",180:180))<2*(SUMIF(176:176,\"Natural Gas\",180:180)),\"Please Explain\",\"Pass\"),\"Please Explain\")","v":"Pass"},"The equivalent cost of 1 MMBtu (site energy) of electricity is less than 2 time greater than the cost of 1 MMBtu (site energy) of natural gas, which appears low. Please confirm that utility rates from the same source (i.e. either Energy Information Administration website, or actual utility rates at the project location) are used, and are modeled correctly."]

{"sheet":"Performance_Outputs_0 old","index":38,"n_rows":394,"n_cols":55,"rows_kept":394,"cut":false,"hidden":true,"merged":[[242,2,242,3],[242,10,242,11],[264,2,264,3],[264,10,264,11],[275,2,275,3],[275,10,275,11],[284,2,284,3],[284,10,284,11],[293,2,293,3],[293,10,293,11],[250,1,250,3],[251,2,251,3],[252,2,252,3],[254,1,254,3],[255,2,255,3],[256,2,256,3],[243,1,243,3],[243,10,243,11],[245,1,245,11],[246,1,246,12],[247,1,248,1],[247,2,248,3],[247,4,247,6],[247,7,247,9],[389,8,389,12],[388,8,388,12],[391,8,391,12],[392,8,392,12],[393,8,393,12],[387,8,387,12],[372,8,372,12],[373,8,373,12],[374,8,374,12],[375,8,375,12],[376,8,376,12],[377,8,377,12],[378,8,378,12],[379,8,379,12],[382,8,382,12],[390,8,390,12],[365,8,365,12],[366,8,366,12],[367,8,367,12],[368,8,368,12],[370,8,370,12],[371,8,371,12],[383,8,383,12],[384,8,384,12],[386,8,386,12],[369,8,369,12],[380,8,380,12],[381,8,381,12],[385,8,385,12],[350,1,351,1],[352,1,355,1],[358,8,358,12],[359,8,359,12],[360,8,360,12],[361,8,361,12],[362,8,362,12],[363,8,363,12],[364,8,364,12],[358,1,358,7],[359,1,359,7],[360,1,360,7],[361,1,361,7],[362,1,362,7],[363,1,363,7],[364,1,364,7],[4,7,4,12],[6,1,6,12],[7,1,7,12],[8,1,8,12],[9,1,9,12],[10,1,10,12],[11,1,11,12],[12,1,12,12],[13,1,14,1],[13,2,14,3],[13,4,14,4],[13,5,14,6],[13,7,14,9],[13,10,13,12],[14,10,14,11],[19,1,19,10],[19,11,19,12],[20,1,20,10],[20,11,20,12],[27,1,27,12],[28,1,28,12],[15,2,15,3],[16,2,16,3],[16,5,16,6],[16,7,16,9],[16,10,16,11],[17,2,17,3],[17,5,17,6],[17,7,17,9],[17,10,17,11],[18,2,18,3],[18,5,18,6],[18,7,18,9],[18,10,18,11],[33,1,33,3],[33,9,33,12],[34,1,34,12],[35,1,36,3],[35,4,35,6],[35,7,36,8],[35,9,36,12],[36,4,36,5],[30,1,30,3],[30,5,30,6],[30,7,30,8],[30,9,30,12],[32,1,32,3],[32,9,32,12],[41,1,41,5],[41,7,41,8],[41,9,41,12],[42,1,42,8],[42,9,42,12],[43,1,43,11],[38,1,38,3],[38,7,38,8],[38,9,38,12],[39,1,39,3],[39,7,39,8],[39,9,39,12],[40,1,40,3],[40,7,40,8],[40,9,40,12],[55,3,55,4],[56,3,56,4],[56,9,56,10],[56,11,56,12],[58,3,58,4],[58,9,58,10],[58,11,58,12],[48,1,48,12],[51,1,51,12],[53,1,54,1],[53,2,54,2],[53,3,54,4],[53,6,53,10],[53,11,54,12],[54,6,54,7],[54,9,54,10],[53,5,54,5],[57,3,57,4],[57,9,57,10],[57,11,57,12],[63,1,63,5],[63,9,63,10],[63,11,63,12],[65,1,65,4],[67,1,67,5],[67,9,67,10],[67,11,67,12],[59,3,59,4],[59,9,59,10],[59,11,59,12],[60,1,60,4],[62,1,62,5],[62,9,62,10],[62,11,62,12],[64,1,64,5],[64,9,64,10],[64,11,64,12],[72,1,72,12],[75,1,75,12],[76,1,76,12],[78,1,78,12],[80,1,80,12],[82,1,82,12],[68,1,68,5],[68,9,68,10],[68,11,68,12],[70,1,70,5],[70,9,70,10],[70,11,70,12],[69,1,69,5],[69,9,69,10],[69,11,69,12],[92,1,92,12],[94,1,94,2],[94,10,94,12],[96,1,97,2],[96,3,97,3],[96,4,97,4],[96,10,96,12],[97,10,97,12],[83,1,83,12],[87,1,87,12],[88,1,88,12],[89,1,89,12],[90,1,90,12],[91,1,91,12],[98,1,99,2],[98,3,99,3],[98,4,99,4],[98,10,98,12],[99,10,99,12],[100,1,101,2],[100,3,101,3],[100,4,101,4],[100,10,100,12],[101,10,101,12],[102,1,103,2],[102,3,103,3],[102,4,103,4],[102,10,102,12],[103,10,103,12],[104,1,105,2],[104,3,105,3],[104,4,105,4],[104,10,104,12],[105,10,105,12],[106,1,107,2],[106,3,107,3],[106,4,107,4],[106,10,106,12],[107,10,107,12],[108,1,109,2],[108,3,109,3],[108,4,109,4],[108,10,108,12],[109,10,109,12],[110,1,111,2],[110,3,111,3],[110,4,111,4],[110,10,110,12],[111,10,111,12],[112,1,113,2],[112,3,113,3],[112,4,113,4],[112,10,112,12],[113,10,113,12],[114,1,115,2],[114,3,115,3],[114,4,115,4],[114,10,114,12],[115,10,115,12],[116,1,117,2],[116,3,117,3],[116,4,117,4],[116,10,116,12],[117,10,117,12],[118,1,119,2],[118,3,119,3],[118,4,119,4],[118,10,118,12],[119,10,119,12],[120,1,121,2],[120,3,121,3],[120,4,121,4],[120,10,120,12],[121,10,121,12],[122,1,123,2],[122,3,123,3],[122,4,123,4],[122,10,122,12],[123,10,123,12],[124,1,125,2],[124,3,125,3],[124,4,125,4],[124,10,124,12],[125,10,125,12],[126,1,127,2],[126,3,127,3],[126,4,127,4],[126,10,126,12],[127,10,127,12],[128,1,129,2],[128,3,129,3],[128,4,129,4],[128,10,128,12],[129,10,129,12],[130,1,131,2],[130,3,131,3],[130,4,131,4],[130,10,130,12],[131,10,131,12],[132,1,133,2],[132,3,133,3],[132,4,133,4],[132,10,132,12],[133,10,133,12],[134,1,135,2],[134,3,135,3],[134,4,135,4],[134,10,134,12],[135,10,135,12],[136,1,137,2],[136,3,137,3],[136,4,137,4],[136,10,136,12],[137,10,137,12],[138,1,139,2],[138,3,139,3],[138,4,139,4],[138,10,138,12],[139,10,139,12],[140,1,141,2],[140,3,141,3],[140,4,141,4],[140,10,140,12],[141,10,141,12],[146,1,146,3],[146,10,146,12],[148,1,148,5],[148,10,148,12],[149,1,149,5],[149,10,149,12],[142,1,143,2],[142,3,143,3],[142,4,143,4],[142,10,142,12],[143,10,143,12],[145,1,145,3],[145,10,145,12],[147,1,147,3],[147,10,147,12],[157,1,157,5],[157,10,157,12],[161,1,161,12],[162,1,162,12],[163,1,163,12],[164,1,164,12],[152,1,152,5],[152,10,152,12],[154,1,154,4],[154,10,154,12],[155,1,155,4],[155,10,155,12],[156,1,156,4],[156,10,156,12],[170,31,171,32],[172,1,173,2],[172,3,173,3],[172,4,173,4],[172,9,173,9],[172,10,173,11],[172,12,173,12],[172,31,173,32],[165,1,165,12],[166,1,166,12],[168,1,168,2],[168,10,168,11],[170,1,171,2],[170,3,171,3],[170,4,171,4],[170,9,171,9],[170,10,171,11],[170,12,171,12],[174,31,175,32],[176,1,177,2],[176,3,177,3],[176,4,177,4],[176,9,177,9],[176,10,177,11],[176,12,177,12],[176,31,177,32],[174,1,175,2],[174,3,175,3],[174,4,175,4],[174,9,175,9],[174,10,175,11],[174,12,175,12],[178,31,179,32],[180,1,181,2],[180,3,181,3],[180,4,181,4],[180,9,181,9],[180,10,181,11],[180,12,181,12],[180,31,181,32],[178,1,179,2],[178,3,179,3],[178,4,179,4],[178,9,179,9],[178,10,179,11],[178,12,179,12],[182,31,183,32],[184,1,185,2],[184,3,185,3],[184,4,185,4],[184,9,185,9],[184,10,185,11],[184,12,185,12],[184,31,185,32],[182,1,183,2],[182,3,183,3],[182,4,183,4],[182,9,183,9],[182,10,183,11],[182,12,183,12],[186,31,187,32],[188,1,189,2],[188,3,189,3],[188,4,189,4],[188,9,189,9],[188,10,189,11],[188,12,189,12],[188,31,189,32],[186,1,187,2],[186,3,187,3],[186,4,187,4],[186,9,187,9],[186,10,187,11],[186,12,187,12],[190,31,191,32],[192,1,193,2],[192,3,193,3],[192,4,193,4],[192,9,193,9],[192,10,193,11],[192,12,193,12],[192,31,193,32],[190,1,191,2],[190,3,191,3],[190,4,191,4],[190,9,191,9],[190,10,191,11],[190,12,191,12],[194,31,195,32],[196,1,197,2],[196,3,197,3],[196,4,197,4],[196,9,197,9],[196,10,197,11],[196,12,197,12],[196,31,197,32],[194,1,195,2],[194,3,195,3],[194,4,195,4],[194,9,195,9],[194,10,195,11],[194,12,195,12],[198,31,199,32],[200,1,201,2],[200,3,201,3],[200,4,201,4],[200,9,201,9],[200,10,201,11],[200,12,201,12],[200,31,201,32],[198,1,199,2],[198,3,199,3],[198,4,199,4],[198,9,199,9],[198,10,199,11],[198,12,199,12],[202,31,203,32],[204,1,205,2],[204,3,205,3],[204,4,205,4],[204,9,205,9],[204,10,205,11],[204,12,205,12],[204,31,205,32],[202,1,203,2],[202,3,203,3],[202,4,203,4],[202,9,203,9],[202,10,203,11],[202,12,203,12],[206,31,207,32],[208,1,209,2],[208,3,209,3],[208,4,209,4],[208,9,209,9],[208,10,209,11],[208,12,209,12],[208,31,209,32],[206,1,207,2],[206,3,207,3],[206,4,207,4],[206,9,207,9],[206,10,207,11],[206,12,207,12],[210,31,211,32],[212,1,213,2],[212,3,213,3],[212,4,213,4],[212,9,213,9],[212,10,213,11],[212,12,213,12],[212,31,213,32],[210,1,211,2],[210,3,211,3],[210,4,211,4],[210,9,211,9],[210,10,211,11],[210,12,211,12],[214,31,215,32],[216,1,217,2],[216,3,217,3],[216,4,217,4],[216,9,217,9],[216,10,217,11],[216,12,217,12],[216,31,217,32],[214,1,215,2],[214,3,215,3],[214,4,215,4],[214,9,215,9],[214,10,215,11],[214,12,215,12],[223,2,223,3],[223,10,223,11],[224,2,224,3],[224,10,224,11],[226,1,226,3],[226,10,226,11],[220,1,221,1],[220,2,221,3],[220,4,220,6],[220,7,220,9],[220,10,220,12],[221,10,221,11],[225,2,225,3],[225,10,225,11],[229,1,229,11],[230,1,230,3],[230,4,230,6],[230,7,230,9],[230,10,230,12],[232,2,232,3],[232,4,232,6],[232,7,232,9],[232,10,232,12],[237,13,237,15],[238,10,238,11],[240,2,240,3],[240,10,240,11],[241,2,241,3],[241,10,241,11],[233,2,233,3],[233,4,233,6],[233,7,233,9],[233,10,233,12],[236,1,236,11],[237,1,238,1],[237,2,238,3],[237,4,237,6],[237,7,237,9],[237,10,237,12],[234,2,234,3],[234,4,234,6],[234,7,234,9],[234,10,234,12],[259,13,259,15],[260,10,260,11],[262,2,262,3],[262,10,262,11],[263,2,263,3],[263,10,263,11],[258,1,258,3],[259,1,260,1],[259,2,260,3],[259,4,259,6],[259,7,259,9],[259,10,259,12],[270,13,270,15],[271,10,271,11],[273,2,273,3],[273,10,273,11],[274,2,274,3],[274,10,274,11],[265,1,265,3],[265,10,265,11],[266,1,266,3],[268,1,268,12],[270,1,271,1],[270,2,271,3],[270,4,270,6],[270,7,270,9],[270,10,270,12],[279,13,279,15],[280,10,280,11],[282,2,282,3],[282,10,282,11],[283,2,283,3],[283,10,283,11],[276,1,276,3],[276,10,276,11],[277,1,277,11],[279,1,280,1],[279,2,280,3],[279,4,279,6],[279,7,279,9],[279,10,279,12],[288,13,288,15],[289,10,289,11],[291,2,291,3],[291,10,291,11],[292,2,292,3],[292,10,292,11],[285,1,285,3],[285,10,285,11],[286,1,286,11],[288,1,289,1],[288,2,289,3],[288,4,288,6],[288,7,288,9],[288,10,288,12],[294,1,294,3],[294,10,294,11],[295,1,295,11],[296,1,296,9],[296,10,296,12],[299,1,300,1],[299,2,300,3],[299,4,299,6],[299,7,299,9],[299,10,299,12],[305,1,305,3],[305,10,305,11],[308,1,308,12],[309,1,310,1],[309,2,310,3],[309,4,309,7],[309,8,309,12],[299,13,299,15],[300,10,300,11],[302,2,302,3],[302,10,302,11],[303,2,303,3],[303,10,303,11],[304,2,304,3],[304,10,304,11],[313,1,313,3],[313,6,313,7],[313,10,313,12],[314,2,314,3],[314,6,314,7],[314,10,314,12],[309,13,309,15],[310,6,310,7],[310,10,310,12],[312,2,312,3],[312,6,312,7],[312,10,312,12],[320,1,321,1],[320,2,321,3],[320,4,320,6],[320,7,320,9],[320,10,320,12],[321,10,321,11],[315,2,315,3],[315,6,315,7],[315,10,315,12],[317,1,317,3],[317,6,317,7],[317,10,317,12],[316,2,316,3],[316,6,316,7],[316,10,316,12],[331,5,331,7],[331,8,331,12],[332,1,332,4],[332,5,332,7],[332,8,332,12],[323,2,323,3],[323,10,323,11],[324,2,324,3],[324,10,324,11],[326,1,326,3],[326,10,326,11],[325,2,325,3],[325,10,325,11],[247,10,247,11],[365,1,365,7],[366,1,366,7],[367,1,367,7],[368,1,368,7],[369,1,369,7],[370,1,370,7],[371,1,371,7],[372,1,372,7],[338,1,339,1],[340,1,341,1],[342,1,343,1],[344,1,349,1],[335,1,335,4],[335,5,335,12],[336,2,336,6],[333,1,333,4],[333,5,333,7],[333,8,333,12],[334,1,334,4],[334,5,334,7],[334,8,334,12],[327,1,327,11],[331,1,331,4],[373,1,373,7],[374,1,374,7],[375,1,375,7],[376,1,376,7],[377,1,377,7],[378,1,378,7],[379,1,379,7],[380,1,380,7],[381,1,381,7],[382,1,382,7],[392,1,392,7],[393,1,393,7],[383,1,383,7],[384,1,384,7],[385,1,385,7],[386,1,386,7],[387,1,387,7],[388,1,388,7],[389,1,389,7],[390,1,390,7],[391,1,391,7]]}
["G"]
["G","Performance Rating Method Outputs"]
["G"]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Multiplier"]
["G","Energy Model ID",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(INDEX(MBD_EMI_Table,MATCH($H$5,MBD_EMI_Index,0),MATCH('1 - Multiple Buildings Details'!$J$16,MBD_EMI_Hdr,0)),\"ERROR\")","v":0}]
["G"]
["G","Energy Sources"]
["G"]
["G","Enter each energy source serving the project, the units for the energy consumption and demand, and the associated utility rate name and tariff structure. Default EIA Rates may be used in lieu of local utility rates at the discretion of the energy modeler.  All project energy types and the demand and consumption units must be entered before entering energy simulation output data. Also enter the units used to report energy consumption totals (the sum of all energy types) for site energy consumption and source energy consumption (generally, the IP units are Btu x 10^6, the SI site energy units are kWh, and the SI source energy units are MJ).\n\n\n",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","DES Path 1: If the project is using campus or district thermal energy using ASHRAE 90.1-2010 without Addenda (District Energy Modeling Path 1), select District Cooling, District Hot Water, or District Steam as applicable and all other energy sources serving the building "]
["G","DES Path 2: If the project is modeling campus or district thermal energy using the Full DES Performance Accounting method (District Energy Modeling Path 2) include each energy source serving the building except District Energy, AND include each energy source in the district or campus plant (e.g. electricity, natural gas, etc.) if different from the energy sources serving the building. Do not select District Cooling, District Hot Water, or District Steam. "]
["G","DES Path 3: If the project is modeling campus or district thermal energy using the Streamlined DES Accounting Method (District Energy Modeling Path 3), select District Cooling, District Hot Water, or District Steam as applicable, AND each energy source serving the building, AND each energy source in the district or campus plant if different from the energy sources serving the building (e.g. electricity, natural gas, etc.).\n"]
["G"]
["G","Energy Type","Energy Consumption Units",null,"Demand Units","Utility Rate Name",null,"Utility Rate Structure",null,null,"Unit Conversion Factors"]
["G",null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Energy Type Consumption Units to Site Energy Consumption (\",PO_SiteUnits,\")\")","v":"Energy Type Consumption Units to Site Energy Consumption (Btu x 10^6)"},null,{"$f":"CONCATENATE(\"Energy Type Consumption Units to Source Energy Consumption (\",PO_SourceUnits,\")\")","v":"Energy Type Consumption Units to Source Energy Consumption (Btu x 10^6)"}]
["G","Energy_Type","Energy_Consumption_Units",null,"Demand_Units","Utility_Rate_Name",null,"Utility_Rate_Structure",null,null,"Site_Energy_Conversion_Factor",null,"Source_Energy_Conversion_Factor"]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B17<>\"\",'12 - Performance_Outputs_1'!B17,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C17<>\"\",'12 - Performance_Outputs_1'!C17,\"\"),\"\")","v":""},"",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E17<>\"\",'12 - Performance_Outputs_1'!E17,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H17<>\"\",'12 - Performance_Outputs_1'!H17,\"\"),\"\")","v":""},"",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F17<>\"\",'12 - Performance_Outputs_1'!F17,\"\"),\"\")","v":""},"","",{"$f":"IFERROR(VLOOKUP(\"kBtu\",EnergyUnitsTable,3,FALSE)/VLOOKUP(PO_SiteUnits,EnergyUnitsTable,3,FALSE)*VLOOKUP($C17,EnergyUnitsTable,3,FALSE),\"\")","v":""},null,{"$f":"IFERROR(VLOOKUP(\"kBtu\",EnergyUnitsTable,3,FALSE)/VLOOKUP(PO_SourceUnits,EnergyUnitsTable,3,FALSE)*VLOOKUP($C17,EnergyUnitsTable,3,FALSE)*VLOOKUP($B17,FuelTypesTable,2,FALSE),\"\")","v":""}]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B18<>\"\",'12 - Performance_Outputs_1'!B18,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C18<>\"\",'12 - Performance_Outputs_1'!C18,\"\"),\"\")","v":""},"",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E18<>\"\",'12 - Performance_Outputs_1'!E18,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H18<>\"\",'12 - Performance_Outputs_1'!H18,\"\"),\"\")","v":""},"",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F18<>\"\",'12 - Performance_Outputs_1'!F18,\"\"),\"\")","v":""},"","",{"$f":"IFERROR(VLOOKUP(\"kBtu\",EnergyUnitsTable,3,FALSE)/VLOOKUP(PO_SiteUnits,EnergyUnitsTable,3,FALSE)*VLOOKUP($C18,EnergyUnitsTable,3,FALSE),\"\")","v":""},null,{"$f":"IFERROR(VLOOKUP(\"kBtu\",EnergyUnitsTable,3,FALSE)/VLOOKUP(PO_SourceUnits,EnergyUnitsTable,3,FALSE)*VLOOKUP($C18,EnergyUnitsTable,3,FALSE)*VLOOKUP($B18,FuelTypesTable,2,FALSE),\"\")","v":""}]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B19<>\"\",'12 - Performance_Outputs_1'!B19,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C19<>\"\",'12 - Performance_Outputs_1'!C19,\"\"),\"\")","v":""},"",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E19<>\"\",'12 - Performance_Outputs_1'!E19,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H19<>\"\",'12 - Performance_Outputs_1'!H19,\"\"),\"\")","v":""},"",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F19<>\"\",'12 - Performance_Outputs_1'!F19,\"\"),\"\")","v":""},"","",{"$f":"IFERROR(VLOOKUP(\"kBtu\",EnergyUnitsTable,3,FALSE)/VLOOKUP(PO_SiteUnits,EnergyUnitsTable,3,FALSE)*VLOOKUP($C19,EnergyUnitsTable,3,FALSE),\"\")","v":""},null,{"$f":"IFERROR(VLOOKUP(\"kBtu\",EnergyUnitsTable,3,FALSE)/VLOOKUP(PO_SourceUnits,EnergyUnitsTable,3,FALSE)*VLOOKUP($C19,EnergyUnitsTable,3,FALSE)*VLOOKUP($B19,FuelTypesTable,2,FALSE),\"\")","v":""}]
["G","Site energy consumption units used to report energy consumption totals (sum of energy types)",null,null,null,null,null,null,null,null,null,{"$f":"IF(SI_IP_Units=\"SI\",\"MWh\",\"Btu x 10^6\")","v":"Btu x 10^6"}]
["G","Source energy consumption units used to report energy consumption totals (sum of energy types)",null,null,null,null,null,null,null,null,null,{"$f":"IF(SI_IP_Units=\"SI\",\"MWh\",\"Btu x 10^6\")","v":"Btu x 10^6"}]
["G"]
["G"]
["G","On-Site Renewable Energy Production"]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Site-generated renewable energy?"]
["G","The project building uses on-site renewable energy systems. (Optional)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,true]
["G"]
["G","Table: On-Site Renewable energy source summary"]
["G","Renewable energy production should be reported in the table below. Note: This calculator will automatically reduce the proposed energy consumption and cost to accurately reflect the revised results. Therefore, any site-generated renewable energy production should NOT be included in the Performance Rating Method tables below.\n\nSelect the site-generated renewable energy source. Enter the rated capacity of the site-generated renewable source including the units (e.g. for photovoltaics 10 kW). Include all relevant capacities (i.e for solar thermal, both the storage tank capacity and the solar thermal panel capacity).\n\nThe cost of the Site-generated renewable cost will be automatically determined using the virtual rate once the output data (consumption and cost) is entered below. The cost may be overridden by the user, however this may generate an issue on the Quality Checks and the user should be prepared to justify the entered cost value."]
["G"]
["G","On-Site Renewable Source",null,null,"Offset \nEnergy Type","Rated Capacity ",null,"Annual Site Energy Generated",null,"Annual Energy Cost Offset with \nSite-Generated Renewables \n($/year)",null,null,null,null,null,null,null,null,null,"Default_Cost","Rate_Variance"]
["G","Renewable_Source",null,null,"Offset_Energy_Type","Rated_Capacity",null,"Annual_Site_Energy",null,"Cost",null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion","EFLH","Default_Cost","Rate_Variance"]
["A","Photovoltaic system",null,null,"Electricity",null,{"$f":"IFERROR(IF(ISBLANK($E33),\"\",VLOOKUP($E33,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR(IF(ISBLANK($E33),\"\",VLOOKUP($E33,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($H33*VLOOKUP($E33,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},"","","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E33),\"\",VLOOKUP($E33,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E33),\"\",VLOOKUP($E33,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR((H33*VLOOKUP(I33,EnergyUnitsTable,3,FALSE))/(F33*VLOOKUP(G33,DemandTable,3,FALSE)),\"\")","v":""},{"$f":"IFERROR($H33*VLOOKUP($E33,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(1-$J33/$T33,0)","v":0}]
[null,"Solar thermal system",null,null,"Natural Gas",null,{"$f":"IFERROR(IF(ISBLANK($E34),\"\",VLOOKUP($E34,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR(IF(ISBLANK($E34),\"\",VLOOKUP($E34,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},"","","","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E34),\"\",VLOOKUP($E34,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E34),\"\",VLOOKUP($E34,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR((H34*VLOOKUP(I34,EnergyUnitsTable,3,FALSE))/(F34*VLOOKUP(G34,DemandTable,3,FALSE)),\"\")","v":""},{"$f":"IFERROR($H34*VLOOKUP($E34,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(1-$J34/$T34,0)","v":0}]
[null,"Renewable Summary"]
[null,"Offset Energy Type",null,null,"Annual Site Energy Generated",null,null,{"$f":"CONCATENATE(\"Annual Source Energy Generated\n (\", PO_SourceUnits, \")\")","v":"Annual Source Energy Generated\n (Btu x 10^6)"},null,"Annual Energy Cost Offset with \nSite-Generated Renewables \n($/year)"]
[null,null,null,null,"Units per Energy Type",null,{"$f":"CONCATENATE(\"Units = \", PO_SiteUnits,\")\")","v":"Units = Btu x 10^6)"}]
[null,"Energy_Type",null,null,"Site_Energy_Ind_Units","Site_Ind_Units","Site_Energy_Same_Units","Source_Energy",null,"Cost",null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
[null,{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},null,null,{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,SUMIF(INDEX(PO_renewable_table,0,MATCH($E$32,PO_renewable_hdr,0)),$B39,INDEX(PO_renewable_table,0,MATCH($H$32,PO_renewable_hdr,0))),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(ISBLANK($B39),\"\",VLOOKUP($B39,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($E39*$Q39,\"\")","v":""},{"$f":"IFERROR($E39*$R39,\"\")","v":""},null,{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,SUMIF($E$33:$E$34,$B39,$J$33:$J$34),0),\"\")","v":0},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B39),\"\",VLOOKUP($B39,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B39),\"\",VLOOKUP($B39,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
[null,{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},null,null,{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,SUMIF(INDEX(PO_renewable_table,0,MATCH($E$32,PO_renewable_hdr,0)),$B40,INDEX(PO_renewable_table,0,MATCH($H$32,PO_renewable_hdr,0))),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(ISBLANK($B40),\"\",VLOOKUP($B40,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($E40*$Q40,\"\")","v":""},{"$f":"IFERROR($E40*$R40,\"\")","v":""},null,{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,SUMIF($E$33:$E$34,$B40,$J$33:$J$34),0),\"\")","v":0},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B40),\"\",VLOOKUP($B40,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B40),\"\",VLOOKUP($B40,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
[null,{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},null,null,{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,SUMIF(INDEX(PO_renewable_table,0,MATCH($E$32,PO_renewable_hdr,0)),$B41,INDEX(PO_renewable_table,0,MATCH($H$32,PO_renewable_hdr,0))),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(ISBLANK($B41),\"\",VLOOKUP($B41,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($E41*$Q41,\"\")","v":""},{"$f":"IFERROR($E41*$R41,\"\")","v":""},null,{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,SUMIF($E$33:$E$34,$B41,$J$33:$J$34),0),\"\")","v":0},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B41),\"\",VLOOKUP($B41,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B41),\"\",VLOOKUP($B41,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
[null,"Total",null,null,null,null,{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_2_Table,0,MATCH($G$38,PO_Enrgy_2_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_2_Table,0,MATCH($H$38,PO_Enrgy_2_Hdr,0))),\"\")","v":0},{"$f":"SUM(I38:I40)","v":0},{"$f":"IFERROR(SUM(J32:J34),\"\")","v":0}]
[null,"Percent renewable energy (by cost)",null,null,null,null,null,null,null,{"$f":"IF(Datacenter_Avg=TRUE,IFERROR($J42/$J$295,\"\"),IFERROR($J42/$J$266,\"\"))","v":""}]
["G"]
["G"]
["G","Exceptional Calculation Methods",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Exceptional Calculations?"]
["G",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,true]
["G","The building energy analysis includes exceptional calculation methods. (Optional)"]
["G","Data Centers:  If using the Data Center Calculator to document energy improvements in IT loads, the checkbox stating that the building energy analysis includes exceptional calculation methods must be checked.  In the table below, select the checkbox “Apply to Baseline?” for each end-use impacted, and provide:\n•  The completed Data Center Calculator (found under the prerequisite's \"Resources\" tab in the Credit Library), as well as copies of any other spreadsheets used to perform the calculations\n•  If energy efficiency credit is applied for any future IT equipment, electrical infrastructure, and/or for future server room cooling equipment that will serve unfinished spaces (meaning that the IT equipment, electrical infrastructure, and/or unfinished space cooling equipment will not be installed during Startup Occupancy), provide a binding Owner commitment letter and (for any tenants) sample lease agreements with binding tenant requirements that confirms that the future installed IT equipment will be at least as efficient as the equipment modeled in the Data Center Calculator. Note that the future equipment may not be modeled as being more efficient than the equipment installed for Startup occupancy.\n•  If taking credit for the impact of IT equipment load reductions on HVAC energy consumption, upload the simulation input summary and simulation output reports, and Performance Rating summary with the baseline model revised to include the baseline IT and electrical infrastructure from the Data Center Calculator.\n"]
["G"]
["G","Table: Exceptional calculation methods energy summary"]
["G","Report Exceptional calculation methods in the table below.\n\nSelect \"Add to Baseline\" if the exceptional calculation adjusts the Baseline building energy consumption and cost up, or \"Subtract from Proposed\" if the exceptional calculation adjusts the Proposed building energy consumption and cost down.\n\nThis calculator will automatically reduce the proposed energy consumption and cost, or increase the baseline energy consumption and cost to accurately reflect the revised results. Therefore, any exceptional calculation methods should NOT be included in the Performance Rating Method Compliance report below.  If any single Exceptional Calculation Method results in energy penalties for a given energy type (i.e. increased proposed case electricity energy usage, or decreased baseline case fossil fuel energy usage), that penalty should be entered as a negative number. If any single Exceptional Calculation Method affects more than one energy type, please add additional rows to capture the method's impact to that energy type. If taking credit for Data Center Equipment or Retail Process Loads, those savings must be recorded here and the supplemental spreadsheets associated with that equipment must be uploaded as part of the submittal documents.\n\nThe cost of the Exceptional Calculation Method will be automatically determined using the virtual rate once the output data (consumption and cost) is entered below. The cost may be overridden by the user, however this may generate an issue on the Quality Checks and the user should be prepared to justify the entered cost value."]
["G"]
["G","Exceptional \nCalculation \nNumber","Exceptional \nCalculation \nMethod ID","Energy Type(s)",null,"Add to Baseline?\nSubtract from Proposed?","Annual Energy Difference by Energy Type",null,null,null,null,"Annual Energy Cost Difference"]
["G",null,null,null,null,null,"Site Energy \n(Units per Energy Type)",null,{"$f":"CONCATENATE(\"Site Energy \n(Units = \", PO_SiteUnits,\")\")","v":"Site Energy \n(Units = Btu x 10^6)"},{"$f":"\"Source Energy Consumption \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Consumption \n(Btu x 10^6)"}]
["G","Ex_Calc_Number","Ex_Calc_ID","Energy_Type",null,"Add_Baseline_Subtract_Proposed","Site_Energy_Ind_Units","Site_Ind_Units","Site_Energy_Same_Units","Source_Energy",null,"Cost",null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",null,"Default_Cost","Rate_Variance"]
["B",null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D57),\"\",VLOOKUP($D57,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D57,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)*$G57,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D57,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)*$G57,\"\")","v":""},null,{"$f":"IFERROR($G57*IF($F57=\"Subtract from Proposed\",VLOOKUP($D57,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D57,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D57),\"\",VLOOKUP($D57,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($D57),\"\",VLOOKUP($D57,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR($G57*IF($F57=\"Subtract from Proposed\",VLOOKUP($D57,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D57,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(1-$J57/$T57,0)","v":0},null,null,null,null,null,null,""]
[null,1,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D58),\"\",VLOOKUP($D58,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D58,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)*$G58,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D58,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)*$G58,\"\")","v":""},null,{"$f":"IFERROR($G58*IF($F58=\"Subtract from Proposed\",VLOOKUP($D58,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D58,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D58),\"\",VLOOKUP($D58,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($D58),\"\",VLOOKUP($D58,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR($G58*IF($F58=\"Subtract from Proposed\",VLOOKUP($D58,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D58,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(1-$J58/$T58,0)","v":0}]
[null,2,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D59),\"\",VLOOKUP($D59,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D59,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)*$G59,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D59,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)*$G59,\"\")","v":""},null,{"$f":"IFERROR($G59*IF($F59=\"Subtract from Proposed\",VLOOKUP($D59,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D59,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D59),\"\",VLOOKUP($D59,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($D59),\"\",VLOOKUP($D59,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR($G59*IF($F59=\"Subtract from Proposed\",VLOOKUP($D59,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D59,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(1-$J59/$T59,0)","v":0},null,null,null,null,null,null,""]
[null,3,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D60),\"\",VLOOKUP($D60,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D60,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)*$G60,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($D60,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)*$G60,\"\")","v":""},null,{"$f":"IFERROR($G60*IF($F60=\"Subtract from Proposed\",VLOOKUP($D60,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D60,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($D60),\"\",VLOOKUP($D60,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($D60),\"\",VLOOKUP($D60,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR($G60*IF($F60=\"Subtract from Proposed\",VLOOKUP($D60,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),VLOOKUP($D60,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(1-$J60/$T60,0)","v":0},null,null,null,null,null,null,""]
[null,"Subtotals added to baseline"]
[null,"Energy_Type",null,null,null,null,"Site_Energy_Ind_Units","Site_Ind_Units","Site_Energy_Same_Units","Source_Energy",null,"Cost",null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
[null,{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($G$56,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$56,PO_ExCalc_Hdr,0)),$B63,INDEX(PO_ExCalc_Table,0,MATCH($F$56,PO_ExCalc_Hdr,0)),\"Add to Baseline\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(ISBLANK($B63),\"\",VLOOKUP($B63,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($G63*$Q63,\"\")","v":""},{"$f":"IFERROR($G63*$R63,\"\")","v":""},{"$f":"IFERROR($G63*$Q63,\"\")","v":""},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($L$56,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$56,PO_ExCalc_Hdr,0)),$B63,INDEX(PO_ExCalc_Table,0,MATCH($F$56,PO_ExCalc_Hdr,0)),\"Add to Baseline\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(M$57:M$60,$D$57:$D$60,$B63,$F$57:$F$60,\"Add to Baseline\"),\"\"),\"\")","v":0},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B63),\"\",VLOOKUP($B63,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B63),\"\",VLOOKUP($B63,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
[null,{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($G$56,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$56,PO_ExCalc_Hdr,0)),$B64,INDEX(PO_ExCalc_Table,0,MATCH($F$56,PO_ExCalc_Hdr,0)),\"Add to Baseline\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(ISBLANK($B64),\"\",VLOOKUP($B64,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($G64*$Q64,\"\")","v":""},{"$f":"IFERROR($G64*$R64,\"\")","v":""},{"$f":"IFERROR($G64*$Q64,\"\")","v":""},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($L$56,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$56,PO_ExCalc_Hdr,0)),$B64,INDEX(PO_ExCalc_Table,0,MATCH($F$56,PO_ExCalc_Hdr,0)),\"Add to Baseline\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(M$57:M$60,$D$57:$D$60,$B64,$F$57:$F$60,\"Add to Baseline\"),\"\"),\"\")","v":0},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B64),\"\",VLOOKUP($B64,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B64),\"\",VLOOKUP($B64,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
[null,{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($G$56,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$56,PO_ExCalc_Hdr,0)),$B65,INDEX(PO_ExCalc_Table,0,MATCH($F$56,PO_ExCalc_Hdr,0)),\"Add to Baseline\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(ISBLANK($B65),\"\",VLOOKUP($B65,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($G65*$Q65,\"\")","v":""},{"$f":"IFERROR($G65*$R65,\"\")","v":""},{"$f":"IFERROR($G65*$Q65,\"\")","v":""},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($L$56,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$56,PO_ExCalc_Hdr,0)),$B65,INDEX(PO_ExCalc_Table,0,MATCH($F$56,PO_ExCalc_Hdr,0)),\"Add to Baseline\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(M$57:M$60,$D$57:$D$60,$B65,$F$57:$F$60,\"Add to Baseline\"),\"\"),\"\")","v":0},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B65),\"\",VLOOKUP($B65,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B65),\"\",VLOOKUP($B65,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
[null,"Subtotals subtracted from proposed"]
[null,"Energy_Type",null,null,null,null,"Site_Energy_Ind_Units","Site_Ind_Units","Site_Energy_Same_Units","Source_Energy",null,"Cost",null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
[null,{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($G$56,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$56,PO_ExCalc_Hdr,0)),$B68,INDEX(PO_ExCalc_Table,0,MATCH($F$56,PO_ExCalc_Hdr,0)),\"Subtract from Proposed\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(ISBLANK($B68),\"\",VLOOKUP($B68,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($G68*$Q68,\"\")","v":""},{"$f":"IFERROR($G68*$R68,\"\")","v":""},{"$f":"IFERROR($G68*$Q68,\"\")","v":""},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($L$56,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$56,PO_ExCalc_Hdr,0)),$B68,INDEX(PO_ExCalc_Table,0,MATCH($F$56,PO_ExCalc_Hdr,0)),\"Subtract from Proposed\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(M$57:M$60,$D$57:$D$60,$B68,$F$57:$F$60,\"Add to Baseline\"),\"\"),\"\")","v":0},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B68),\"\",VLOOKUP($B68,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B68),\"\",VLOOKUP($B68,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
[null,{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($G$56,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$56,PO_ExCalc_Hdr,0)),$B69,INDEX(PO_ExCalc_Table,0,MATCH($F$56,PO_ExCalc_Hdr,0)),\"Subtract from Proposed\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(ISBLANK($B69),\"\",VLOOKUP($B69,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($G69*$Q69,\"\")","v":""},{"$f":"IFERROR($G69*$R69,\"\")","v":""},{"$f":"IFERROR($G69*$Q69,\"\")","v":""},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($L$56,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$56,PO_ExCalc_Hdr,0)),$B69,INDEX(PO_ExCalc_Table,0,MATCH($F$56,PO_ExCalc_Hdr,0)),\"Subtract from Proposed\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(M$57:M$60,$D$57:$D$60,$B69,$F$57:$F$60,\"Add to Baseline\"),\"\"),\"\")","v":0},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B69),\"\",VLOOKUP($B69,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B69),\"\",VLOOKUP($B69,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
[null,{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($G$56,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$56,PO_ExCalc_Hdr,0)),$B70,INDEX(PO_ExCalc_Table,0,MATCH($F$56,PO_ExCalc_Hdr,0)),\"Subtract from Proposed\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(ISBLANK($B70),\"\",VLOOKUP($B70,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR($G70*$Q70,\"\")","v":""},{"$f":"IFERROR($G70*$R70,\"\")","v":""},{"$f":"IFERROR($G70*$Q70,\"\")","v":""},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(INDEX(PO_ExCalc_Table,0,MATCH($L$56,PO_ExCalc_Hdr,0)),INDEX(PO_ExCalc_Table,0,MATCH($D$56,PO_ExCalc_Hdr,0)),$B70,INDEX(PO_ExCalc_Table,0,MATCH($F$56,PO_ExCalc_Hdr,0)),\"Subtract from Proposed\"),\"\"),\"\")","v":0},{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,SUMIFS(M$57:M$60,$D$57:$D$60,$B70,$F$57:$F$60,\"Add to Baseline\"),\"\"),\"\")","v":0},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B70),\"\",VLOOKUP($B70,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B70),\"\",VLOOKUP($B70,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
[null,"Total Exceptional Calculation Method Adjustment",null,null,null,null,null,null,{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_3_Table,0,MATCH($I62,PO_Enrgy_3_Hdr,0)),INDEX(PO_Enrgy_4_Table,0,MATCH($I67,PO_Enrgy_4_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_3_Table,0,MATCH($J62,PO_Enrgy_3_Hdr,0)),INDEX(PO_Enrgy_4_Table,0,MATCH($J67,PO_Enrgy_4_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(K$35:K$69),0)","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_3_Table,0,MATCH($L62,PO_Enrgy_3_Hdr,0)),INDEX(PO_Enrgy_4_Table,0,MATCH($L67,PO_Enrgy_4_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(M$35:M$69),0)","v":0}]
["G"]
["G","Upload: Exceptional calculation \nProvide a detailed narrative explaining the exceptional calculation method(s) performed, including all end-uses affected by the exceptional calculation method. If more than one exceptional calculation method is used, the exceptional calculation ID in the narrative must match the values listed in the table above.  The exceptional calculation method must include:\n•  Step-by-step documentation of the exceptional calculation method(s) performed detailed enough to reproduce the results\n•  Copies of all spreadsheets used to perform the calculations, or simulation energy model input and output summaries documenting the calculations performed\n•  For methods that significantly impact HVAC or refrigeration energy, the calculations shall be performed on a time step basis consistent with the simulation program used\n•  The Performance Rating calculated with and without the exceptional calculation method\n•  Documentation of the baseline and proposed assumptions. Documentation of baseline assumptions verify that the efficiency measure is not conventional practice by including, but not limited to:\n    ○  a recently published study (published within five years of the project registration date) with researched tabulations or monitored data establishing standard practice for the given application in similar newly constructed facilities\n    ○  a new construction utility or government program that incentivizes the measure\n    ○  a document showing the systems used to perform the same function in other newly constructed facilities (for example, three similar facilities built within the past five years). These systems would be treated as the baseline system in the analysis, and evidence must be provided to demonstrate how the energy for the baseline and proposed buildings are determined \n    ○  use any of the prescriptive requirements from 90.1-2010 as the baseline requirement without further justification to substantiate conventional practice, but only for the specific component addressed by the prescriptive requirement"]
["G"]
["G","Energy Modeling Output Reporting Method"]
["G","Select one of the following before entering any simulation output data:"]
["G","Complete the baseline results for each of the four building orientations, in addition to the proposed results.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5]
["G"]
["G","Report the averaged baseline results, in addition to the proposed results. In the EAp2 form uploads, provide simulation output summaries from the simulation output software that include the energy consumption by end-use, total energy consumption by energy type, and total energy cost by energy type, reported separately  for each of the four baseline rotations, and the average baseline energy consumption by end-use, energy consumption by energy type, and energy cost by energy type. (The simulation software must report this average as a standard report in order to use this option)."]
["G"]
["G","The project is not required to simulate four baseline orientations because (a) the vertical fenestration area on each orientation varies by less than 5%, (b) the energy code used does not require simulation of four baseline orientations, or (c) the building is more than 50% existing based on conditioned floor area. Report the non-rotated baseline results, in addition to the proposed results.\n"]
["G"]
["G","The project is not required to simulate four baseline orientations because the building orientation is dictated by site consideration, as allowed by Table G3.1.5 (a) (baseline) Exception 1. Report the non-rotated baseline results, in addition to the proposed results."]
["G"]
["G"]
["G","Performance Rating Method Compliance Report"]
["G","Table: Baseline energy summary by end use"]
["G","Complete the table below for the proposed, providing information on baseline energy consumption and peak demand by end-use. This data will be used to autopopulate the Performance tables below. If an end-use has two energy types (e.g. proposed space heating includes both fossil fuel and electric), enter the end-use twice in the table, and list the two different energy types."]
["G","ASHRAE 90.1-2010 without Addenda (District Energy Modeling Path 1): Report the district energy type (District Cooling, District Hot Water, or District Steam) for the cooling and heating end-uses as applicable for both the baseline and proposed.  "]
["G","Full DES Performance Accounting method (District Energy Modeling Path 2): Report the baseline energy as if the thermal energy is produced in the building.  Report the proposed energy used to generate and distribute the district thermal energy serving the building based on calculated average district thermal efficiencies (e.g. report the electricity used to generate and distribute chilled water to the building).\n"]
["G","Streamlined DES Accounting Method (District Energy Modeling Path 3): Report the energy type (District Cooling, District Hot Water, or District Steam for the cooling and heating end-uses as applicable for both the baseline and proposed. "]
["G","Data Centers: The energy consumption for IT equipment must be metered and reported separately from other end-uses in the energy model, and in the tables below to allow the proper determination of the PUE. Complete the table below for the baseline using the full build-out IT loads for the proposed design.\n"]
["G","Retail: The energy consumption for cooking, refrigeration, and kitchen ventilation fans must be metered and reported separately from other end-uses in the energy model and in the tables below. Energy savings or consumption attributable to unregulated equipment, other than Commercial Kitchen Equipment, Supermarket Refrigeration, Walk-in Coolers and Freezers, or Commercial Kitchen Ventilation listed in Tables 1 – 4 of the LEED v4 BD+C:Retail and ID+C: Retail Rating System Appendix 3 must be claimed via Exceptional Calculation Methodology."]
["G"]
["G","End Use",null,"Unregulated?","Energy Type","Units of \nAnnual Energy and Peak Demand","Baseline 0° rotation","Baseline 90° rotation","Baseline 180° rotation","Baseline 270° rotation","Baseline Design Total\n (Average of 4 rotations)"]
["G","End_Use",null,"Unregulated","Energy_Type","Energy_Units","Baseline_0_Rotation","Baseline_90_Rotation","Baseline_180_Rotation","Baseline_270_Rotation","Base_Consumption_Demand",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion","EFLH"]
["G","Interior lighting",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E97),\"\",\"Consumption (\" & VLOOKUP($E97,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,{"$f":"IFERROR(AVERAGE(G97,H97,I97,J97),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($E97),\"\",VLOOKUP($E97,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E97),\"\",VLOOKUP($E97,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F97),(K97*VLOOKUP(MID(F97,FIND(\"(\",F97)+1,LEN(F97)-FIND(\"(\",F97)-1),EnergyUnitsTable,3,FALSE))/(K98*VLOOKUP(MID(F98,FIND(\"(\",F98)+1,LEN(F98)-FIND(\"(\",F98)-1),DemandTable,3,FALSE)),1),\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E97),\"\",\"Demand (\" & VLOOKUP($E97,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Exterior lighting",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E99),\"\",\"Consumption (\" & VLOOKUP($E99,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E99),\"\",\"Demand (\" & VLOOKUP($E99,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Space heating",null,null,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E101),\"\",\"Consumption (\" & VLOOKUP($E101,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E101),\"\",\"Demand (\" & VLOOKUP($E101,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Space cooling",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E103),\"\",\"Consumption (\" & VLOOKUP($E103,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E103),\"\",\"Demand (\" & VLOOKUP($E103,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Pumps",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E105),\"\",\"Consumption (\" & VLOOKUP($E105,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E105),\"\",\"Demand (\" & VLOOKUP($E105,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Heat rejection",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E107),\"\",\"Consumption (\" & VLOOKUP($E107,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E107),\"\",\"Demand (\" & VLOOKUP($E107,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Fans - interior ventilation",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E109),\"\",\"Consumption (\" & VLOOKUP($E109,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E109),\"\",\"Demand (\" & VLOOKUP($E109,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Fans - parking garage",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E111),\"\",\"Consumption (\" & VLOOKUP($E111,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E111),\"\",\"Demand (\" & VLOOKUP($E111,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Service water heating",null,null,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E113),\"\",\"Consumption (\" & VLOOKUP($E113,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E113),\"\",\"Demand (\" & VLOOKUP($E113,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Receptacle equipment",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E115),\"\",\"Consumption (\" & VLOOKUP($E115,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E115),\"\",\"Demand (\" & VLOOKUP($E115,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","IT equipment",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E117),\"\",\"Consumption (\" & VLOOKUP($E117,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E117),\"\",\"Demand (\" & VLOOKUP($E117,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Interior lighting - process",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E119),\"\",\"Consumption (\" & VLOOKUP($E119,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E119),\"\",\"Demand (\" & VLOOKUP($E119,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Refrigeration equipment",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E121),\"\",\"Consumption (\" & VLOOKUP($E121,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E121),\"\",\"Demand (\" & VLOOKUP($E121,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Fans - Kitchen Ventilation",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E123),\"\",\"Consumption (\" & VLOOKUP($E123,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E123),\"\",\"Demand (\" & VLOOKUP($E123,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Cooking",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E125),\"\",\"Consumption (\" & VLOOKUP($E125,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E125),\"\",\"Demand (\" & VLOOKUP($E125,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Industrial Process",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E127),\"\",\"Consumption (\" & VLOOKUP($E127,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E127),\"\",\"Demand (\" & VLOOKUP($E127,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Elevators and escalators",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E129),\"\",\"Consumption (\" & VLOOKUP($E129,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E129),\"\",\"Demand (\" & VLOOKUP($E129,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G","Heat Pump Supplementary",null,null,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E131),\"\",\"Consumption (\" & VLOOKUP($E131,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E131),\"\",\"Demand (\" & VLOOKUP($E131,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E133),\"\",\"Consumption (\" & VLOOKUP($E133,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E133),\"\",\"Demand (\" & VLOOKUP($E133,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E135),\"\",\"Consumption (\" & VLOOKUP($E135,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E135),\"\",\"Demand (\" & VLOOKUP($E135,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E137),\"\",\"Consumption (\" & VLOOKUP($E137,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E137),\"\",\"Demand (\" & VLOOKUP($E137,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E139),\"\",\"Consumption (\" & VLOOKUP($E139,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E139),\"\",\"Demand (\" & VLOOKUP($E139,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E141),\"\",\"Consumption (\" & VLOOKUP($E141,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E141),\"\",\"Demand (\" & VLOOKUP($E141,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E143),\"\",\"Consumption (\" & VLOOKUP($E143,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E143),\"\",\"Demand (\" & VLOOKUP($E143,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},null,null,null,null,"",null,null,null,null,null,"","",""]
["G",null,null,null,"Energy_Type","Energy_Units","Baseline_0_Rotation","Baseline_90_Rotation","Baseline_180_Rotation","Baseline_270_Rotation","Baseline_Total",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",""]
["G","Total energy consumption by energy type ",null,null,{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK(E146),\"\",VLOOKUP($E146,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IFERROR(SUMIFS(INDEX(PO_baseline_table,0,MATCH(G$96,PO_baseline_hdr,0)),INDEX(PO_baseline_table,0,MATCH($E$96,PO_baseline_hdr,0)),$E146,INDEX(PO_baseline_table,0,MATCH($F$96,PO_baseline_hdr,0)),\"=Con*\"),\"\")","v":0},0,0,0,0,"","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E146),\"\",VLOOKUP($E146,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E146),\"\",VLOOKUP($E146,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",null,null,null,{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK(E147),\"\",VLOOKUP($E147,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},0,0,0,0,0,"","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E147),\"\",VLOOKUP($E147,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E147),\"\",VLOOKUP($E147,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",null,null,null,{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK(E148),\"\",VLOOKUP($E148,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},0,0,0,0,0,"","",null,null,null,{"$f":"IFERROR(IF(ISBLANK($E148),\"\",VLOOKUP($E148,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E148),\"\",VLOOKUP($E148,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"\"Total site energy (\" & PO_SiteUnits & \")\"","v":"Total site energy (Btu x 10^6)"},null,null,null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_5_Table,0,MATCH(G$145,PO_Enrgy_5_Hdr,0)),INDEX(PO_Enrgy_5_Table,0,MATCH($Q145,PO_Enrgy_5_Hdr,0))),\"\")","v":0},0,0,0,0,"",""]
["G",{"$f":"\"Total source energy (\" & PO_SourceUnits & \")\"","v":"Total source energy (Btu x 10^6)"},null,null,null,null,{"$f":"IFERROR(SUMPRODUCT(G$146:G$147,$R$146:$R$147),0)","v":0},0,0,0,0,0,0]
["G"]
["G","Table: Baseline building annual energy cost by energy type "]
["G","Energy Type",null,null,null,null,"Baseline 0° rotation","Baseline 90° rotation","Baseline 180° rotation","Baseline 270° rotation","Baseline Design Total"]
["G","Energy_Type",null,null,null,null,"Baseline_0_Rotation","Baseline_90_Rotation","Baseline_180_Rotation","Baseline_270_Rotation","Base_Cost",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B155),\"\",VLOOKUP($B155,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},null,null,null,null,{"$f":"IFERROR((AVERAGE(G155:J155)),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B155),\"\",VLOOKUP($B155,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B155),\"\",VLOOKUP($B155,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B156),\"\",VLOOKUP($B156,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},null,null,null,null,{"$f":"IFERROR((AVERAGE(G156:J156)),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B156),\"\",VLOOKUP($B156,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B156),\"\",VLOOKUP($B156,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B157),\"\",VLOOKUP($B157,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},null,null,null,null,{"$f":"IFERROR((AVERAGE(G157:J157)),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B157),\"\",VLOOKUP($B157,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B157),\"\",VLOOKUP($B157,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","Baseline annual energy cost",null,null,null,null,{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_6_Table,0,MATCH(G$154,PO_Enrgy_6_Hdr,0))),\"\")","v":0},0,0,0,0,"",""]
["G"]
["G"]
["G","Table: Proposed energy summary by end use"]
["G","Complete the table below, providing information on energy consumption and demand by end-use. If an end-use has two energy types (e.g. proposed case space heating includes both fossil fuel and electric), enter the end-use twice in the table, and list the two different energy types."]
["G","ASHRAE 90.1-2010 without Addenda (District Energy Modeling Path 1): Report the district energy type (District Cooling, District Hot Water, or District Steam) for the cooling and heating end-uses as applicable for both the baseline and proposed."]
["G","Full DES Performance Accounting method (District Energy Modeling Path 2): Report the baseline energy as if the thermal energy is produced in the building.  Report the proposed energy used to generate and distribute the district thermal energy serving the building based on calculated average district thermal efficiencies (e.g. report the electricity used to generate and distribute chilled water to the building).\n"]
["G","Streamlined DES Accounting Method (District Energy Modeling Path 3): Report the energy type (District Cooling, District Hot Water, or District Steam for the cooling and heating end-uses as applicable for both the baseline and proposed. "]
["G","Data Centers: The energy consumption for IT equipment must be metered and reported separately from other end-uses in the energy model, and in the tables below to allow the proper determination of the PUE. Complete the table below for the baseline using the full build-out IT loads for the proposed design.\n"]
["G","Retail: The energy consumption for cooking, refrigeration, and kitchen ventilation fans must be metered and reported separately from other end-uses in the energy model and in the tables below. Energy savings or consumption attributable to unregulated equipment, other than Commercial Kitchen Equipment, Supermarket Refrigeration, Walk-in Coolers and Freezers, or Commercial Kitchen Ventilation listed in Tables 1 – 4 of the LEED v4 BD+C: Retail and ID+C: Retail Rating System Appendix 3 must be claimed via Exceptional Calculation Methodology."]
["G"]
["G","End Use",null,"Unregulated?","Energy Type","Units of \nAnnual Energy and Peak Demand","Baseline","Proposed","Energy / Demand Savings \nper End-Use","End Use \nPercent Contribution to Total Energy Savings","End Use \nPercent \nContribution to \nTotal Cost Savings",null,"Percent of Total Proposed  \nSite Energy Consumption",null,null,null,null,null,null,null,null,null,"contribution rank",null,"Rank with ties","rank no ties",null,null,null,null,null,null,"QC_EFLH"]
["G","End_Use",null,"Unregulated","Energy_Type","Energy_Units","Base_Consumption_Demand","Design_Consumption_Demand","End_Use_Savings","End_Use_Contribution_to_Energy_Savings","End_Use_Contribution_to_Cost_Savings",null,"Percent_Design_Site_Consumption",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion","Base_EFLH","Design_EFLH",null,null,"contribution rank",null,"Rank with ties","rank no ties"]
["G","Interior lighting",null,{"$f":"INDEX(PO_baseline_table,1, 3)","v":0},{"$f":"INDEX(PO_baseline_table,1, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E171),\"\",\"Consumption (\" & VLOOKUP($E171,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,1, 10)","v":""},null,{"$f":"IFERROR(1-H171/G171,\"\")","v":""},{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G171-$H171)*VLOOKUP($E171,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G171*VLOOKUP($E171,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H171*VLOOKUP($E171,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H171*VLOOKUP($E171,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($E171),\"\",VLOOKUP($E171,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E171),\"\",VLOOKUP($E171,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",F171),(G171*VLOOKUP(MID(F171,FIND(\"(\",F171)+1,LEN(F171)-FIND(\"(\",F171)-1),EnergyUnitsTable,3,FALSE))/(G172*VLOOKUP(MID(F172,FIND(\"(\",F172)+1,LEN(F172)-FIND(\"(\",F172)-1),DemandTable,3,FALSE)),1),\"\")","v":""},{"$f":"IFERROR(IF(FIND(\"Consumption\",$F171),(H171*VLOOKUP(MID($F171,FIND(\"(\",$F171)+1,LEN($F171)-FIND(\"(\",$F171)-1),EnergyUnitsTable,3,FALSE))/(H172*VLOOKUP(MID($F172,FIND(\"(\",$F172)+1,LEN($F172)-FIND(\"(\",$F172)-1),DemandTable,3,FALSE)),1),\"\")","v":""},null,{"$f":"IFERROR($AN171*H171,0)","v":0},{"$f":"IFERROR(G171*VLOOKUP($AE171,PO_Enrgy_8_Table,4,FALSE),0)","v":0},{"$f":"IFERROR(H171*VLOOKUP($AE171,PO_Enrgy_8_Table,7,FALSE),0)","v":0},{"$f":"IFERROR(IF(D171=\"x\",IF(OR(G171/H171>1.03,G171/H171<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J171*100,)","v":0},null,{"$f":"RANK(Z171,$Z$171:$Z$218,0)","v":1},{"$f":"AB171","v":1},{"$f":"B171","v":"Interior lighting"},null,{"$f":"IFERROR(G171/'6b - General Lighting'!#REF!,\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E171),\"\",\"Demand (\" & VLOOKUP($E171,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,2, 10)","v":""},null,{"$f":"IFERROR(1-H172/G172,\"\")","v":""},null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Exterior lighting",null,{"$f":"INDEX(PO_baseline_table,3, 3)","v":0},{"$f":"INDEX(PO_baseline_table,3, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E173),\"\",\"Consumption (\" & VLOOKUP($E173,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,3, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G173-$H173)*VLOOKUP($E173,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G173*VLOOKUP($E173,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H173*VLOOKUP($E173,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H173*VLOOKUP($E173,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D173=\"x\",IF(OR(G173/H173>1.03,G173/H173<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J173*100,)","v":0},null,{"$f":"RANK(Z173,$Z$171:$Z$218,0)","v":1},{"$f":"AB173+COUNTIF($AB$171:$AB172,AB173)","v":2},{"$f":"B173","v":"Exterior lighting"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E173),\"\",\"Demand (\" & VLOOKUP($E173,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,4, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Space heating",null,{"$f":"INDEX(PO_baseline_table,5, 3)","v":0},{"$f":"INDEX(PO_baseline_table,5, 4)","v":"Natural Gas"},{"$f":"IFERROR(IF(ISBLANK(E175),\"\",\"Consumption (\" & VLOOKUP($E175,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,5, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G175-$H175)*VLOOKUP($E175,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G175*VLOOKUP($E175,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H175*VLOOKUP($E175,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H175*VLOOKUP($E175,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D175=\"x\",IF(OR(G175/H175>1.03,G175/H175<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J175*100,)","v":0},null,{"$f":"RANK(Z175,$Z$171:$Z$218,0)","v":1},{"$f":"AB175+COUNTIF($AB$171:$AB174,AB175)","v":3},{"$f":"B175","v":"Space heating"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E175),\"\",\"Demand (\" & VLOOKUP($E175,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,6, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Space cooling",null,{"$f":"INDEX(PO_baseline_table,7, 3)","v":0},{"$f":"INDEX(PO_baseline_table,7, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E177),\"\",\"Consumption (\" & VLOOKUP($E177,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,7, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G177-$H177)*VLOOKUP($E177,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G177*VLOOKUP($E177,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H177*VLOOKUP($E177,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H177*VLOOKUP($E177,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D177=\"x\",IF(OR(G177/H177>1.03,G177/H177<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J177*100,)","v":0},null,{"$f":"RANK(Z177,$Z$171:$Z$218,0)","v":1},{"$f":"AB177+COUNTIF($AB$171:$AB176,AB177)","v":4},{"$f":"B177","v":"Space cooling"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E177),\"\",\"Demand (\" & VLOOKUP($E177,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,8, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Pumps",null,{"$f":"INDEX(PO_baseline_table,9, 3)","v":0},{"$f":"INDEX(PO_baseline_table,9, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E179),\"\",\"Consumption (\" & VLOOKUP($E179,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,9, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G179-$H179)*VLOOKUP($E179,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G179*VLOOKUP($E179,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H179*VLOOKUP($E179,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H179*VLOOKUP($E179,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D179=\"x\",IF(OR(G179/H179>1.03,G179/H179<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J179*100,)","v":0},null,{"$f":"RANK(Z179,$Z$171:$Z$218,0)","v":1},{"$f":"AB179+COUNTIF($AB$171:$AB178,AB179)","v":5},{"$f":"B179","v":"Pumps"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E179),\"\",\"Demand (\" & VLOOKUP($E179,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,10, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Heat rejection",null,{"$f":"INDEX(PO_baseline_table,11, 3)","v":0},{"$f":"INDEX(PO_baseline_table,11, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E181),\"\",\"Consumption (\" & VLOOKUP($E181,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,11, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G181-$H181)*VLOOKUP($E181,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G181*VLOOKUP($E181,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H181*VLOOKUP($E181,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H181*VLOOKUP($E181,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D181=\"x\",IF(OR(G181/H181>1.03,G181/H181<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J181*100,)","v":0},null,{"$f":"RANK(Z181,$Z$171:$Z$218,0)","v":1},{"$f":"AB181+COUNTIF($AB$171:$AB180,AB181)","v":6},{"$f":"B181","v":"Heat rejection"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E181),\"\",\"Demand (\" & VLOOKUP($E181,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,12, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Fans - interior ventilation",null,{"$f":"INDEX(PO_baseline_table,13, 3)","v":0},{"$f":"INDEX(PO_baseline_table,13, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E183),\"\",\"Consumption (\" & VLOOKUP($E183,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,13, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G183-$H183)*VLOOKUP($E183,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G183*VLOOKUP($E183,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H183*VLOOKUP($E183,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H183*VLOOKUP($E183,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D183=\"x\",IF(OR(G183/H183>1.03,G183/H183<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J183*100,)","v":0},null,{"$f":"RANK(Z183,$Z$171:$Z$218,0)","v":1},{"$f":"AB183+COUNTIF($AB$171:$AB182,AB183)","v":7},{"$f":"B183","v":"Fans - interior ventilation"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E183),\"\",\"Demand (\" & VLOOKUP($E183,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,14, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Fans - parking garage",null,{"$f":"INDEX(PO_baseline_table,15, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,15, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E185),\"\",\"Consumption (\" & VLOOKUP($E185,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,15, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G185-$H185)*VLOOKUP($E185,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G185*VLOOKUP($E185,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H185*VLOOKUP($E185,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H185*VLOOKUP($E185,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D185=\"x\",IF(OR(G185/H185>1.03,G185/H185<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J185*100,)","v":0},null,{"$f":"RANK(Z185,$Z$171:$Z$218,0)","v":1},{"$f":"AB185+COUNTIF($AB$171:$AB184,AB185)","v":8},{"$f":"B185","v":"Fans - parking garage"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E185),\"\",\"Demand (\" & VLOOKUP($E185,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,16, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Service water heating",null,{"$f":"INDEX(PO_baseline_table,17, 3)","v":0},{"$f":"INDEX(PO_baseline_table,17, 4)","v":"Natural Gas"},{"$f":"IFERROR(IF(ISBLANK(E187),\"\",\"Consumption (\" & VLOOKUP($E187,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,17, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G187-$H187)*VLOOKUP($E187,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G187*VLOOKUP($E187,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H187*VLOOKUP($E187,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H187*VLOOKUP($E187,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D187=\"x\",IF(OR(G187/H187>1.03,G187/H187<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J187*100,)","v":0},null,{"$f":"RANK(Z187,$Z$171:$Z$218,0)","v":1},{"$f":"AB187+COUNTIF($AB$171:$AB186,AB187)","v":9},{"$f":"B187","v":"Service water heating"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E187),\"\",\"Demand (\" & VLOOKUP($E187,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,18, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Receptacle equipment",null,{"$f":"INDEX(PO_baseline_table,19, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,19, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E189),\"\",\"Consumption (\" & VLOOKUP($E189,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,19, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G189-$H189)*VLOOKUP($E189,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G189*VLOOKUP($E189,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H189*VLOOKUP($E189,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H189*VLOOKUP($E189,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D189=\"x\",IF(OR(G189/H189>1.03,G189/H189<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J189*100,)","v":0},null,{"$f":"RANK(Z189,$Z$171:$Z$218,0)","v":1},{"$f":"AB189+COUNTIF($AB$171:$AB188,AB189)","v":10},{"$f":"B189","v":"Receptacle equipment"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E189),\"\",\"Demand (\" & VLOOKUP($E189,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,20, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","IT equipment",null,{"$f":"INDEX(PO_baseline_table,21, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,21, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E191),\"\",\"Consumption (\" & VLOOKUP($E191,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,21, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G191-$H191)*VLOOKUP($E191,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G191*VLOOKUP($E191,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H191*VLOOKUP($E191,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H191*VLOOKUP($E191,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D191=\"x\",IF(OR(G191/H191>1.03,G191/H191<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J191*100,)","v":0},null,{"$f":"RANK(Z191,$Z$171:$Z$218,0)","v":1},{"$f":"AB191+COUNTIF($AB$171:$AB190,AB191)","v":11},{"$f":"B191","v":"IT equipment"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E191),\"\",\"Demand (\" & VLOOKUP($E191,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,22, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Interior lighting - process",null,{"$f":"INDEX(PO_baseline_table,23, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,23, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E193),\"\",\"Consumption (\" & VLOOKUP($E193,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,23, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G193-$H193)*VLOOKUP($E193,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G193*VLOOKUP($E193,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H193*VLOOKUP($E193,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H193*VLOOKUP($E193,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D193=\"x\",IF(OR(G193/H193>1.03,G193/H193<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J193*100,)","v":0},null,{"$f":"RANK(Z193,$Z$171:$Z$218,0)","v":1},{"$f":"AB193+COUNTIF($AB$171:$AB192,AB193)","v":12},{"$f":"B193","v":"Interior lighting - process"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E193),\"\",\"Demand (\" & VLOOKUP($E193,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,24, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Refrigeration equipment",null,{"$f":"INDEX(PO_baseline_table,25, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,25, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E195),\"\",\"Consumption (\" & VLOOKUP($E195,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,25, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G195-$H195)*VLOOKUP($E195,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G195*VLOOKUP($E195,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H195*VLOOKUP($E195,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H195*VLOOKUP($E195,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D195=\"x\",IF(OR(G195/H195>1.03,G195/H195<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J195*100,)","v":0},null,{"$f":"RANK(Z195,$Z$171:$Z$218,0)","v":1},{"$f":"AB195+COUNTIF($AB$171:$AB194,AB195)","v":13},{"$f":"B195","v":"Refrigeration equipment"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E195),\"\",\"Demand (\" & VLOOKUP($E195,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,26, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Fans - Kitchen Ventilation",null,{"$f":"INDEX(PO_baseline_table,27, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,27, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E197),\"\",\"Consumption (\" & VLOOKUP($E197,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,27, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G197-$H197)*VLOOKUP($E197,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G197*VLOOKUP($E197,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H197*VLOOKUP($E197,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H197*VLOOKUP($E197,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D197=\"x\",IF(OR(G197/H197>1.03,G197/H197<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J197*100,)","v":0},null,{"$f":"RANK(Z197,$Z$171:$Z$218,0)","v":1},{"$f":"AB197+COUNTIF($AB$171:$AB196,AB197)","v":14},{"$f":"B197","v":"Fans - Kitchen Ventilation"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E197),\"\",\"Demand (\" & VLOOKUP($E197,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,28, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Cooking",null,{"$f":"INDEX(PO_baseline_table,29, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,29, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E199),\"\",\"Consumption (\" & VLOOKUP($E199,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,29, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G199-$H199)*VLOOKUP($E199,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G199*VLOOKUP($E199,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H199*VLOOKUP($E199,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H199*VLOOKUP($E199,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D199=\"x\",IF(OR(G199/H199>1.03,G199/H199<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J199*100,)","v":0},null,{"$f":"RANK(Z199,$Z$171:$Z$218,0)","v":1},{"$f":"AB199+COUNTIF($AB$171:$AB198,AB199)","v":15},{"$f":"B199","v":"Cooking"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E199),\"\",\"Demand (\" & VLOOKUP($E199,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,30, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Industrial Process",null,{"$f":"INDEX(PO_baseline_table,31, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,31, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E201),\"\",\"Consumption (\" & VLOOKUP($E201,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,31, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G201-$H201)*VLOOKUP($E201,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G201*VLOOKUP($E201,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H201*VLOOKUP($E201,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H201*VLOOKUP($E201,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D201=\"x\",IF(OR(G201/H201>1.03,G201/H201<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J201*100,)","v":0},null,{"$f":"RANK(Z201,$Z$171:$Z$218,0)","v":1},{"$f":"AB201+COUNTIF($AB$171:$AB200,AB201)","v":16},{"$f":"B201","v":"Industrial Process"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E201),\"\",\"Demand (\" & VLOOKUP($E201,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,32, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Elevators and escalators",null,{"$f":"INDEX(PO_baseline_table,33, 3)","v":"x"},{"$f":"INDEX(PO_baseline_table,33, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E203),\"\",\"Consumption (\" & VLOOKUP($E203,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,33, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G203-$H203)*VLOOKUP($E203,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G203*VLOOKUP($E203,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H203*VLOOKUP($E203,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H203*VLOOKUP($E203,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D203=\"x\",IF(OR(G203/H203>1.03,G203/H203<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J203*100,)","v":0},null,{"$f":"RANK(Z203,$Z$171:$Z$218,0)","v":1},{"$f":"AB203+COUNTIF($AB$171:$AB202,AB203)","v":17},{"$f":"B203","v":"Elevators and escalators"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E203),\"\",\"Demand (\" & VLOOKUP($E203,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,34, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G","Heat Pump Supplementary",null,{"$f":"INDEX(PO_baseline_table,35, 3)","v":0},{"$f":"INDEX(PO_baseline_table,35, 4)","v":"Electricity"},{"$f":"IFERROR(IF(ISBLANK(E205),\"\",\"Consumption (\" & VLOOKUP($E205,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,35, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G205-$H205)*VLOOKUP($E205,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G205*VLOOKUP($E205,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H205*VLOOKUP($E205,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H205*VLOOKUP($E205,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D205=\"x\",IF(OR(G205/H205>1.03,G205/H205<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J205*100,)","v":0},null,{"$f":"RANK(Z205,$Z$171:$Z$218,0)","v":1},{"$f":"AB205+COUNTIF($AB$171:$AB204,AB205)","v":18},{"$f":"B205","v":"Heat Pump Supplementary"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E205),\"\",\"Demand (\" & VLOOKUP($E205,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,36, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G",{"$f":"INDEX(PO_base_Add_EndUses,1, 1)","v":0},null,{"$f":"INDEX(PO_baseline_table,37, 3)","v":0},{"$f":"INDEX(PO_baseline_table,37, 4)","v":0},{"$f":"IFERROR(IF(ISBLANK(E207),\"\",\"Consumption (\" & VLOOKUP($E207,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,37, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G207-$H207)*VLOOKUP($E207,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G207*VLOOKUP($E207,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H207*VLOOKUP($E207,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H207*VLOOKUP($E207,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D207=\"x\",IF(OR(G207/H207>1.03,G207/H207<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J207*100,)","v":0},null,{"$f":"RANK(Z207,$Z$171:$Z$218,0)","v":1},{"$f":"AB207+COUNTIF($AB$171:$AB206,AB207)","v":19},{"$f":"B207","v":0}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E207),\"\",\"Demand (\" & VLOOKUP($E207,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,38, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G",{"$f":"INDEX(PO_base_Add_EndUses,3, 1)","v":0},null,{"$f":"INDEX(PO_baseline_table,39, 3)","v":0},{"$f":"INDEX(PO_baseline_table,39, 4)","v":0},{"$f":"IFERROR(IF(ISBLANK(E209),\"\",\"Consumption (\" & VLOOKUP($E209,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,39, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G209-$H209)*VLOOKUP($E209,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G209*VLOOKUP($E209,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H209*VLOOKUP($E209,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H209*VLOOKUP($E209,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D209=\"x\",IF(OR(G209/H209>1.03,G209/H209<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J209*100,)","v":0},null,{"$f":"RANK(Z209,$Z$171:$Z$218,0)","v":1},{"$f":"AB209+COUNTIF($AB$171:$AB208,AB209)","v":20},{"$f":"B209","v":0}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E209),\"\",\"Demand (\" & VLOOKUP($E209,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,40, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G",{"$f":"INDEX(PO_base_Add_EndUses,5, 1)","v":0},null,{"$f":"INDEX(PO_baseline_table,41, 3)","v":0},{"$f":"INDEX(PO_baseline_table,41, 4)","v":0},{"$f":"IFERROR(IF(ISBLANK(E211),\"\",\"Consumption (\" & VLOOKUP($E211,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,41, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G211-$H211)*VLOOKUP($E211,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G211*VLOOKUP($E211,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H211*VLOOKUP($E211,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H211*VLOOKUP($E211,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D211=\"x\",IF(OR(G211/H211>1.03,G211/H211<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J211*100,)","v":0},null,{"$f":"RANK(Z211,$Z$171:$Z$218,0)","v":1},{"$f":"AB211+COUNTIF($AB$171:$AB210,AB211)","v":21},{"$f":"B211","v":0}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E211),\"\",\"Demand (\" & VLOOKUP($E211,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,42, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G",{"$f":"INDEX(PO_base_Add_EndUses,7, 1)","v":0},null,{"$f":"INDEX(PO_baseline_table,43, 3)","v":0},{"$f":"INDEX(PO_baseline_table,43, 4)","v":0},{"$f":"IFERROR(IF(ISBLANK(E213),\"\",\"Consumption (\" & VLOOKUP($E213,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,43, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G213-$H213)*VLOOKUP($E213,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G213*VLOOKUP($E213,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H213*VLOOKUP($E213,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H213*VLOOKUP($E213,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D213=\"x\",IF(OR(G213/H213>1.03,G213/H213<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J213*100,)","v":0},null,{"$f":"RANK(Z213,$Z$171:$Z$218,0)","v":1},{"$f":"AB213+COUNTIF($AB$171:$AB212,AB213)","v":22},{"$f":"B213","v":0}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E213),\"\",\"Demand (\" & VLOOKUP($E213,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,44, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G",{"$f":"INDEX(PO_base_Add_EndUses,9, 1)","v":0},null,{"$f":"INDEX(PO_baseline_table,45, 3)","v":0},{"$f":"INDEX(PO_baseline_table,45, 4)","v":0},{"$f":"IFERROR(IF(ISBLANK(E215),\"\",\"Consumption (\" & VLOOKUP($E215,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,45, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G215-$H215)*VLOOKUP($E215,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G215*VLOOKUP($E215,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H215*VLOOKUP($E215,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H215*VLOOKUP($E215,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D215=\"x\",IF(OR(G215/H215>1.03,G215/H215<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J215*100,)","v":0},null,{"$f":"RANK(Z215,$Z$171:$Z$218,0)","v":1},{"$f":"AB215+COUNTIF($AB$171:$AB214,AB215)","v":23},{"$f":"B215","v":0}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E215),\"\",\"Demand (\" & VLOOKUP($E215,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,46, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G",{"$f":"INDEX(PO_base_Add_EndUses,11, 1)","v":0},null,{"$f":"INDEX(PO_baseline_table,47, 3)","v":0},{"$f":"INDEX(PO_baseline_table,47, 4)","v":0},{"$f":"IFERROR(IF(ISBLANK(E217),\"\",\"Consumption (\" & VLOOKUP($E217,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,47, 10)","v":""},null,"",{"$f":"IFERROR(IF($E$327-$H$327<0,\"\",($G217-$H217)*VLOOKUP($E217,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)/($E$327-$H$327)),\"\")","v":""},{"$f":"IFERROR(IF($G$327-$J$327<0,\"\",($G217*VLOOKUP($E217,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)-($H217*VLOOKUP($E217,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)))/($G$327-$J$327)),\"\")","v":""},null,{"$f":"IFERROR(H217*VLOOKUP($E217,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0))/$H$227,\"\")","v":""},null,null,null,"","","","",null,0,0,0,{"$f":"IFERROR(IF(D217=\"x\",IF(OR(G217/H217>1.03,G217/H217<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J217*100,)","v":0},null,{"$f":"RANK(Z217,$Z$171:$Z$218,0)","v":1},{"$f":"AB217+COUNTIF($AB$171:$AB216,AB217)","v":24},{"$f":"B217","v":0}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E217),\"\",\"Demand (\" & VLOOKUP($E217,PO_Enrgy_1_Table,MATCH($E$16,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},{"$f":"INDEX(PO_baseline_table,48, 10)","v":""},null,"",null,null,null,null,null,null,null,"","","","",null,0,0,0]
["G"]
["G","Table: Performance rating energy consumption and cost by fuel type"]
["G","Energy Type","Site Energy Units",null,"Baseline",null,null,"Proposed",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site_Energy",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B224),\"\",VLOOKUP($B224,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C224=\"\",\"\",VLOOKUP(C224,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(SUMIFS(G$171:G$218,$F$171:$F$218,\"=Con*\",$E$171:$E$218,$B224), 0)","v":0},{"$f":"IFERROR(SUMIFS(G$171:G$218,$F$171:$F$218,\"=Con*\",$E$171:$E$218,$B224)*VLOOKUP($B224,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE), 0)","v":0},{"$f":"INDEX(PO_Enrgy_6_Table,1, 10)","v":""},{"$f":"IFERROR(SUMIFS(H$171:H$218,$F$171:$F$218,\"=Con*\",$E$171:$E$218,$B224), 0)","v":0},{"$f":"IFERROR(SUMIFS(H$171:H$218,$F$171:$F$218,\"=Con*\",$E$171:$E$218,$B224)*VLOOKUP($B224,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE), 0)","v":0},null,{"$f":"IFERROR(1-H224/E224,\"\")","v":""},null,{"$f":"IFERROR(1-J224/G224,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B224),\"\",VLOOKUP($B224,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B224),\"\",VLOOKUP($B224,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B225),\"\",VLOOKUP($B225,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C225=\"\",\"\",VLOOKUP(C225,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(SUMIFS(G$171:G$218,$F$171:$F$218,\"=Con*\",$E$171:$E$218,$B225), 0)","v":0},{"$f":"IFERROR(SUMIFS(G$171:G$218,$F$171:$F$218,\"=Con*\",$E$171:$E$218,$B225)*VLOOKUP($B225,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE), 0)","v":0},{"$f":"INDEX(PO_Enrgy_6_Table,2, 10)","v":""},{"$f":"IFERROR(SUMIFS(H$171:H$218,$F$171:$F$218,\"=Con*\",$E$171:$E$218,$B225), 0)","v":0},{"$f":"IFERROR(SUMIFS(H$171:H$218,$F$171:$F$218,\"=Con*\",$E$171:$E$218,$B225)*VLOOKUP($B225,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE), 0)","v":0},null,{"$f":"IFERROR(1-H225/E225,\"\")","v":""},null,{"$f":"IFERROR(1-J225/G225,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B225),\"\",VLOOKUP($B225,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B225),\"\",VLOOKUP($B225,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B226),\"\",VLOOKUP($B226,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C226=\"\",\"\",VLOOKUP(C226,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(SUMIFS(G$171:G$218,$F$171:$F$218,\"=Con*\",$E$171:$E$218,$B226), 0)","v":0},{"$f":"IFERROR(SUMIFS(G$171:G$218,$F$171:$F$218,\"=Con*\",$E$171:$E$218,$B226)*VLOOKUP($B226,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE), 0)","v":0},{"$f":"INDEX(PO_Enrgy_6_Table,2, 10)","v":""},{"$f":"IFERROR(SUMIFS(H$171:H$218,$F$171:$F$218,\"=Con*\",$E$171:$E$218,$B226), 0)","v":0},{"$f":"IFERROR(SUMIFS(H$171:H$218,$F$171:$F$218,\"=Con*\",$E$171:$E$218,$B226)*VLOOKUP($B226,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE), 0)","v":0},null,{"$f":"IFERROR(1-H226/E226,\"\")","v":""},null,{"$f":"IFERROR(1-J226/G226,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B226),\"\",VLOOKUP($B226,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B226),\"\",VLOOKUP($B226,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_7_Table,0,MATCH(E$223,PO_Enrgy_7_Hdr,0)),INDEX(PO_Enrgy_7_Table,0,MATCH($Q$223,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(F$223,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(G$223,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_7_Table,0,MATCH(H$223,PO_Enrgy_7_Hdr,0)),INDEX(PO_Enrgy_7_Table,0,MATCH($Q$223,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(I$223,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(J$223,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H227/E227,\"\")","v":""},null,{"$f":"IFERROR(1-J227/G227,\"\")","v":""}]
["G"]
["G"]
["G","Table: Virtual rate (average energy cost per unit energy)"]
["G","Energy Type",null,null,"Baseline",null,null,"Proposed",null,null,"Percent Variance"]
["G","Energy_Type","Units",null,"Base_Virtual_Rate",null,null,"Design_Virtual_Rate",null,null,"Percent_Variance",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",null,"Default_Base","Default_Proposed"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(CONCATENATE(\"$ / \",VLOOKUP($B233,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":"$ / "},{"$f":"IF(C233=\"\",\"\",VLOOKUP(C233,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B233=\"District Cooling\",$B233=\"District Steam\",$B233=\"District Hot Water\")),IF($B233=\"District Cooling\",$V$251,$W$251),VLOOKUP($B233,PO_Enrgy_7_Table,MATCH($G$223,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B233,PO_Enrgy_7_Table,MATCH($E$223,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},"","",{"$f":"IFERROR(IF(AND(DESPath=3,OR($B233=\"District Cooling\",$B233=\"District Steam\",$B233=\"District Hot Water\")),IF($B233=\"District Cooling\",$V$255,$W$255),VLOOKUP($B233,PO_Enrgy_7_Table,MATCH($J$223,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B233,PO_Enrgy_7_Table,MATCH($H$223,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},"","",{"$f":"IFERROR(ABS(1-H233/E233),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B233),\"\",VLOOKUP($B233,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B233),\"\",VLOOKUP($B233,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B233=\"District Cooling\",$B233=\"District Steam\",$B233=\"District Hot Water\")),IF($B233=\"District Cooling\",$V$251,$W$251),VLOOKUP($B233,PO_Enrgy_7_Table,MATCH($G$223,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B233,PO_Enrgy_7_Table,MATCH($E$223,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B233=\"District Cooling\",$B233=\"District Steam\",$B233=\"District Hot Water\")),IF($B233=\"District Cooling\",$V$255,$W$255),VLOOKUP($B233,PO_Enrgy_7_Table,MATCH($J$223,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B233,PO_Enrgy_7_Table,MATCH($H$223,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},{"$f":"IFERROR(CONCATENATE(\"$ / \",VLOOKUP($B234,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":"$ / "},{"$f":"IF(C234=\"\",\"\",VLOOKUP(C234,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","",{"$f":"IFERROR(ABS(1-H234/E234),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B234),\"\",VLOOKUP($B234,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B234),\"\",VLOOKUP($B234,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B234=\"District Cooling\",$B234=\"District Steam\",$B234=\"District Hot Water\")),IF($B234=\"District Cooling\",$V$251,$W$251),VLOOKUP($B234,PO_Enrgy_7_Table,MATCH($G$223,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B234,PO_Enrgy_7_Table,MATCH($E$223,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B234=\"District Cooling\",$B234=\"District Steam\",$B234=\"District Hot Water\")),IF($B234=\"District Cooling\",$V$255,$W$255),VLOOKUP($B234,PO_Enrgy_7_Table,MATCH($J$223,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B234,PO_Enrgy_7_Table,MATCH($H$223,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},{"$f":"IFERROR(CONCATENATE(\"$ / \",VLOOKUP($B235,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":"$ / "},{"$f":"IF(C235=\"\",\"\",VLOOKUP(C235,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},"","","","","","",{"$f":"IFERROR(ABS(1-H235/E235),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B235),\"\",VLOOKUP($B235,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B235),\"\",VLOOKUP($B235,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B235=\"District Cooling\",$B235=\"District Steam\",$B235=\"District Hot Water\")),IF($B235=\"District Cooling\",$V$251,$W$251),VLOOKUP($B235,PO_Enrgy_7_Table,MATCH($G$223,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B235,PO_Enrgy_7_Table,MATCH($E$223,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B235=\"District Cooling\",$B235=\"District Steam\",$B235=\"District Hot Water\")),IF($B235=\"District Cooling\",$V$255,$W$255),VLOOKUP($B235,PO_Enrgy_7_Table,MATCH($J$223,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B235,PO_Enrgy_7_Table,MATCH($H$223,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""}]
["G"]
["G","Table: Exceptional calculation methods"]
["G","Energy Type","Site Energy Units",null,"Baseline Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site_Energy",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B241),\"\",VLOOKUP($B241,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C241=\"\",\"\",VLOOKUP(C241,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(VLOOKUP($B241,PO_Enrgy_7_Table,MATCH($E$223,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B241,PO_Enrgy_3_Table,MATCH($G$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B241,PO_Enrgy_7_Table,MATCH($F$223,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B241,PO_Enrgy_3_Table,MATCH($J$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B241,PO_Enrgy_7_Table,MATCH($G$223,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B241,PO_Enrgy_3_Table,MATCH($L$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B241,PO_Enrgy_7_Table,MATCH($H$223,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B241,PO_Enrgy_4_Table,MATCH($G$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B241,PO_Enrgy_7_Table,MATCH($I$223,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B241,PO_Enrgy_4_Table,MATCH($J$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B241,PO_Enrgy_7_Table,MATCH($J$223,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B241,PO_Enrgy_4_Table,MATCH($L$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(1-H241/E241,\"\")","v":""},null,{"$f":"IFERROR(1-J241/G241,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B241),\"\",VLOOKUP($B241,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B241),\"\",VLOOKUP($B241,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B242),\"\",VLOOKUP($B242,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C242=\"\",\"\",VLOOKUP(C242,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(VLOOKUP($B242,PO_Enrgy_7_Table,MATCH($E$223,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B242,PO_Enrgy_3_Table,MATCH($G$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B242,PO_Enrgy_7_Table,MATCH($F$223,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B242,PO_Enrgy_3_Table,MATCH($J$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B242,PO_Enrgy_7_Table,MATCH($G$223,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B242,PO_Enrgy_3_Table,MATCH($L$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B242,PO_Enrgy_7_Table,MATCH($H$223,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B242,PO_Enrgy_4_Table,MATCH($G$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B242,PO_Enrgy_7_Table,MATCH($I$223,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B242,PO_Enrgy_4_Table,MATCH($J$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B242,PO_Enrgy_7_Table,MATCH($J$223,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B242,PO_Enrgy_4_Table,MATCH($L$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(1-H242/E242,\"\")","v":""},null,{"$f":"IFERROR(1-J242/G242,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B242),\"\",VLOOKUP($B242,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B242),\"\",VLOOKUP($B242,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B243),\"\",VLOOKUP($B243,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C243=\"\",\"\",VLOOKUP(C243,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(VLOOKUP($B243,PO_Enrgy_7_Table,MATCH($E$223,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B243,PO_Enrgy_3_Table,MATCH($G$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B243,PO_Enrgy_7_Table,MATCH($F$223,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B243,PO_Enrgy_3_Table,MATCH($J$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B243,PO_Enrgy_7_Table,MATCH($G$223,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B243,PO_Enrgy_3_Table,MATCH($L$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B243,PO_Enrgy_7_Table,MATCH($H$223,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B243,PO_Enrgy_4_Table,MATCH($G$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B243,PO_Enrgy_7_Table,MATCH($I$223,PO_Enrgy_7_Hdr,0),FALSE)-IF(PO_ShowExCalc=TRUE,VLOOKUP($B243,PO_Enrgy_4_Table,MATCH($J$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(VLOOKUP($B243,PO_Enrgy_7_Table,MATCH($J$223,PO_Enrgy_7_Hdr,0),FALSE)+IF(PO_ShowExCalc=TRUE,VLOOKUP($B243,PO_Enrgy_4_Table,MATCH($L$62,PO_Enrgy_3_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(1-H243/E243,\"\")","v":""},null,{"$f":"IFERROR(1-J243/G243,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B243),\"\",VLOOKUP($B243,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B243),\"\",VLOOKUP($B243,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_9_Table,0,MATCH(E$240,PO_Enrgy_9_Hdr,0)),INDEX(PO_Enrgy_9_Table,0,MATCH($Q$240,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(F$240,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(G$240,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_9_Table,0,MATCH(H$240,PO_Enrgy_9_Hdr,0)),INDEX(PO_Enrgy_9_Table,0,MATCH($Q$240,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(I$240,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(J$240,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H244/E244,\"\")","v":""},null,{"$f":"IFERROR(1-J244/G244,\"\")","v":""}]
["G"]
["G","Table: Streamlined DES Accounting Method (DES Path 3) - District Energy Allocation to Project Based on Average Efficiencies"]
["G","Select the fossil fuel energy type used to generate any district heating or cooling.  Enter the proposed average District Cooling and District Heating efficiencies as applicable. For District Cooling, include chillers, cooling towers, chilled water and condenser water pumps, thermal distribution losses, and any other end-uses contributing towards the energy used to generate and distribute chilled water to the building. For District Heating, include boilers, pumps, thermal distribution losses, and any other end-uses contributing towards the energy used to generate and distribute heating to the building. In the Uploads section of the form, provide details regarding the calculations and or monitoring used to determine the proposed District Energy average efficiency, including any energy simulation outputs for the district plant if using the modeling method.\n\n* Average DES efficiency (COP) per energy source is equal to one unit of thermal energy divided by the input energy for the energy source associated with generating one unit of thermal energy and delivering it to the building. Baseline average efficiency is determined based on chilled water or hot water capacity and ASHRAE 90.1 Appendix G Baseline requirements for on-site CHW and HHW generation equipment (see District Energy Path 3 tab for details)."]
["G","Fuel Source for District Cooling and/or Heating","Site Energy Units",null,"District Cooling ",null,null,"District Heating"]
["G",null,null,null,"Average \nEfficiency \n(COP)*","Site Energy Use \n(Units shown per energy type)","Cost","Average \nEfficiency \n(COP)*","Site Energy Use (Units shown per energy type)","Cost"]
["G","Energy_Type","Energy_Units",null,"Cooling_Avg_Efficiency","Cooling_Site_Energy","Cooling_Cost","Heating_Avg_Effiicency","Heating_Site_Energy","Heating_Cost",null,null,null,null,null,null,null,null,null,null,"Total Baseline","Cost/Unit District Cooling","Cost/Unit District Heating"]
["G","Baseline",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",null,null,null,{"$f":"IFERROR(V253+V252,\"\")","v":""},{"$f":"IFERROR(W253+W252,\"\")","v":""}]
["G",{"$f":"IFERROR(IF(DESPath=3,\"Electricity\",\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B252),\"\",VLOOKUP($B252,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C252=\"\",\"\",VLOOKUP(C252,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(AND(DESPath=3,DistrictCooling,$B$252=\"Electricity\"),DESPath3_Cooling_COP,\"\"),\"\")","v":""},{"$f":"IFERROR(IF(DESPath=3,VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($E$240,PO_Enrgy_9_Hdr,0),FALSE)/$E252*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C252,EnergyUnitsTable,3,FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(F252*VLOOKUP($B252,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(IF(AND(DESPath=3,DistrictHeating,$B$252=\"Electricity\"),DESPath3_Heating_eCOP,\"\"),\"\")","v":""},{"$f":"IF(DESPath = 3,IFERROR(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($E$240,PO_Enrgy_9_Hdr,0),FALSE)/$H252*VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C252,EnergyUnitsTable,3,FALSE),0)+IFERROR(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($E$240,PO_Enrgy_9_Hdr,0),FALSE)/$H252*VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($H252,EnergyUnitsTable,3,FALSE),0),0)","v":0},{"$f":"IFERROR(I252*VLOOKUP($B252,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B252),\"\",VLOOKUP($B252,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B252),\"\",VLOOKUP($B252,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,null,"Elec",{"$f":"IFERROR(VLOOKUP($B252,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)/$E$252*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C252,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B252,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)/$H$252*(IFERROR(VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1)+IFERROR(VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1))/VLOOKUP($C252,EnergyUnitsTable,3,FALSE),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(DESPath=3,IF(MATCH(\"Natural Gas\",PO_Enrgy_1_Index,0)>0,\"Natural Gas\",IF(MATCH(\"Fuel Oil / Diesel\",PO_Enrgy_1_Table,0)>1,\"Fuel Oil / Diesel\",\"\")),\"\"),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B253),\"\",VLOOKUP($B253,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C253=\"\",\"\",VLOOKUP(C253,ProjectEnergyTypeTable,3,FALSE))","v":""},null,null,null,{"$f":"IFERROR(IF(AND(DESPath=3,DistrictHeating,$B$252=\"Electricity\"),DESPath3_Heating_fCOP,\"\"),\"\")","v":""},{"$f":"IF(DESPath = 3,IFERROR(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($E$240,PO_Enrgy_9_Hdr,0),FALSE)/$H253*VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C253,EnergyUnitsTable,3,FALSE),0)+IFERROR(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($E$240,PO_Enrgy_9_Hdr,0),FALSE)/$H253*VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($H253,EnergyUnitsTable,3,FALSE),0),0)","v":0},{"$f":"IFERROR(I253*VLOOKUP($B253,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B253),\"\",VLOOKUP($B253,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B253),\"\",VLOOKUP($B253,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,null,"Fuel",{"$f":"IFERROR(VLOOKUP($B253,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)/$E$252*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C253,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B253,PO_Enrgy_8_Table,MATCH($E$232,PO_Enrgy_8_Hdr,0),FALSE)/$H$252*(IFERROR(VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1)+IFERROR(VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1))/VLOOKUP($C253,EnergyUnitsTable,3,FALSE),\"\")","v":""}]
["G","Energy_Type","Energy_Units",null,"Cooling_Avg_Efficiency","Cooling_Site_Energy","Cooling_Cost","Heating_Avg_Effiicency","Heating_Site_Energy","Heating_Cost",null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",null,null,null,"Cost/Unit District Cooling","Cost/Unit District Heating"]
["G","Proposed",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Total Proposed",{"$f":"IFERROR(V256+V257,\"\")","v":""},{"$f":"IFERROR(W256+W257,\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B256),\"\",VLOOKUP($B256,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C256=\"\",\"\",VLOOKUP(C256,ProjectEnergyTypeTable,3,FALSE))","v":""},null,{"$f":"IFERROR(VLOOKUP($B256,PO_Enrgy_9_Table,MATCH($E$240,PO_Enrgy_9_Hdr,0),FALSE)/$E$256*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C256,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(F256*VLOOKUP($B256,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,{"$f":"IF(DESPath = 3,IFERROR(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($H$240,PO_Enrgy_9_Hdr,0),FALSE)/$H256*VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C256,EnergyUnitsTable,3,FALSE),0)+IFERROR(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($H$240,PO_Enrgy_9_Hdr,0),FALSE)/$H256*VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($H256,EnergyUnitsTable,3,FALSE),0),0)","v":0},{"$f":"IFERROR(I256*VLOOKUP($B256,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B256),\"\",VLOOKUP($B256,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B256),\"\",VLOOKUP($B256,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,null,"Elec",{"$f":"IFERROR(VLOOKUP($B256,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)/$E$256*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C256,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B256,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)/$H$256*(IFERROR(VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1)+IFERROR(VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1))/VLOOKUP($C256,EnergyUnitsTable,3,FALSE),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK($B$253),\"\",$B$253),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B257),\"\",VLOOKUP($B257,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C257=\"\",\"\",VLOOKUP(C257,ProjectEnergyTypeTable,3,FALSE))","v":""},null,{"$f":"IFERROR(VLOOKUP($B257,PO_Enrgy_9_Table,MATCH($E$240,PO_Enrgy_9_Hdr,0),FALSE)/$E$256*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C257,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(F257*VLOOKUP($B257,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,{"$f":"IF(DESPath = 3,IFERROR(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($H$240,PO_Enrgy_9_Hdr,0),FALSE)/$H257*VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C257,EnergyUnitsTable,3,FALSE),0)+IFERROR(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($H$240,PO_Enrgy_9_Hdr,0),FALSE)/$H257*VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($H257,EnergyUnitsTable,3,FALSE),0),0)","v":0},{"$f":"IFERROR(I257*VLOOKUP($B257,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE),\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B257),\"\",VLOOKUP($B257,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B257),\"\",VLOOKUP($B257,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,null,"Fuel",{"$f":"IFERROR(VLOOKUP($B257,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)/$E$256*VLOOKUP(VLOOKUP(\"District Cooling\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE)/VLOOKUP($C257,EnergyUnitsTable,3,FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B257,PO_Enrgy_8_Table,MATCH($H$232,PO_Enrgy_8_Hdr,0),FALSE)/$H$256*(IFERROR(VLOOKUP(VLOOKUP(\"District Hot Water\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1)+IFERROR(VLOOKUP(VLOOKUP(\"District Steam\",PO_Enrgy_9_Table,MATCH($C$240,PO_Enrgy_9_Hdr,0),FALSE),EnergyUnitsTable,3,FALSE),1))/VLOOKUP($C257,EnergyUnitsTable,3,FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(G257/E257,\"\")","v":""},{"$f":"IFERROR(J257/H257,\"\")","v":""}]
["G",null,null,null,null,null,null,null,"("]
["G"]
["G","Energy Type","Site Energy Units",null,"Baseline Energy Consumption \nwith District Energy Average Efficiencies \n(if DES Path 3 is used)",null,null,"Proposed Energy Consumption \nwith District Energy Average Efficiencies \n(if DES Path 3 is used)",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B263),\"\",VLOOKUP($B263,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C263=\"\",\"\",VLOOKUP(C263,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B263,PO_DESbase_Enrgy_Table,MATCH($F$250,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B263,PO_DESbase_Enrgy_Table,MATCH($I$250,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B263<>\"District Cooling\",B263<>\"District Hot Water\",B263<>\"District Steam\")),VLOOKUP($B263,PO_Enrgy_9_Table,MATCH($E$240,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E263*$R263,\"\")","v":""},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B263,PO_DESbase_Enrgy_Table,MATCH($G$250,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B263,PO_DESbase_Enrgy_Table,MATCH($J$250,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B263<>\"District Cooling\",B263<>\"District Hot Water\",B263<>\"District Steam\")),VLOOKUP($B263,PO_Enrgy_9_Table,MATCH($G$240,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B263,PO_DESdesign_Enrgy_Table,MATCH($F$254,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B263,PO_DESdesign_Enrgy_Table,MATCH($I$254,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B263<>\"District Cooling\",B263<>\"District Hot Water\",B263<>\"District Steam\")),VLOOKUP($B263,PO_Enrgy_9_Table,MATCH($H$240,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(H263*$R263,\"\")","v":""},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B263,PO_DESdesign_Enrgy_Table,MATCH($G$254,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B263,PO_DESdesign_Enrgy_Table,MATCH($J$254,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B263<>\"District Cooling\",B263<>\"District Hot Water\",B263<>\"District Steam\")),VLOOKUP($B263,PO_Enrgy_9_Table,MATCH($J$240,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(1-H263/E263,\"\")","v":""},null,{"$f":"IFERROR(1-J263/G263,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B263),\"\",VLOOKUP($B263,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B263),\"\",VLOOKUP($B263,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B264),\"\",VLOOKUP($B264,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C264=\"\",\"\",VLOOKUP(C264,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B264,PO_DESbase_Enrgy_Table,MATCH($F$250,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B264,PO_DESbase_Enrgy_Table,MATCH($I$250,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B264<>\"District Cooling\",B264<>\"District Hot Water\",B264<>\"District Steam\")),VLOOKUP($B264,PO_Enrgy_9_Table,MATCH($E$240,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E264*$R264,\"\")","v":""},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B264,PO_DESbase_Enrgy_Table,MATCH($G$250,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B264,PO_DESbase_Enrgy_Table,MATCH($J$250,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B264<>\"District Cooling\",B264<>\"District Hot Water\",B264<>\"District Steam\")),VLOOKUP($B264,PO_Enrgy_9_Table,MATCH($G$240,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B264,PO_DESdesign_Enrgy_Table,MATCH($F$254,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B264,PO_DESdesign_Enrgy_Table,MATCH($I$254,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B264<>\"District Cooling\",B264<>\"District Hot Water\",B264<>\"District Steam\")),VLOOKUP($B264,PO_Enrgy_9_Table,MATCH($H$240,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(H264*$R264,\"\")","v":""},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B264,PO_DESdesign_Enrgy_Table,MATCH($G$254,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B264,PO_DESdesign_Enrgy_Table,MATCH($J$254,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B264<>\"District Cooling\",B264<>\"District Hot Water\",B264<>\"District Steam\")),VLOOKUP($B264,PO_Enrgy_9_Table,MATCH($J$240,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(1-H264/E264,\"\")","v":""},null,{"$f":"IFERROR(1-J264/G264,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B264),\"\",VLOOKUP($B264,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B264),\"\",VLOOKUP($B264,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B265),\"\",VLOOKUP($B265,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C265=\"\",\"\",VLOOKUP(C265,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B265,PO_DESbase_Enrgy_Table,MATCH($F$250,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B265,PO_DESbase_Enrgy_Table,MATCH($I$250,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B265<>\"District Cooling\",B265<>\"District Hot Water\",B265<>\"District Steam\")),VLOOKUP($B265,PO_Enrgy_9_Table,MATCH($E$240,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E265*$R265,\"\")","v":""},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B265,PO_DESbase_Enrgy_Table,MATCH($G$250,PO_DESbase_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B265,PO_DESbase_Enrgy_Table,MATCH($J$250,PO_DESbase_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B265<>\"District Cooling\",B265<>\"District Hot Water\",B265<>\"District Steam\")),VLOOKUP($B265,PO_Enrgy_9_Table,MATCH($G$240,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B265,PO_DESdesign_Enrgy_Table,MATCH($F$254,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B265,PO_DESdesign_Enrgy_Table,MATCH($I$254,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B265<>\"District Cooling\",B265<>\"District Hot Water\",B265<>\"District Steam\")),VLOOKUP($B265,PO_Enrgy_9_Table,MATCH($H$240,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(H265*$R265,\"\")","v":""},{"$f":"IFERROR(IFERROR(IFERROR(VLOOKUP($B265,PO_DESdesign_Enrgy_Table,MATCH($G$254,PO_DESdesign_Enrgy_Hdr,0),FALSE),0)+IFERROR(VLOOKUP($B265,PO_DESdesign_Enrgy_Table,MATCH($J$254,PO_DESdesign_Enrgy_Hdr,0),FALSE),0),0)+IF(OR(DESPath<>3,AND(B265<>\"District Cooling\",B265<>\"District Hot Water\",B265<>\"District Steam\")),VLOOKUP($B265,PO_Enrgy_9_Table,MATCH($J$240,PO_Enrgy_9_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(1-H265/E265,\"\")","v":""},null,{"$f":"IFERROR(1-J265/G265,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B265),\"\",VLOOKUP($B265,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B265),\"\",VLOOKUP($B265,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"\"Energy Model Subtotal (\" & PO_SiteUnits & \")\"","v":"Energy Model Subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_10_Table,0,MATCH(E$262,PO_Enrgy_10_Hdr,0)),INDEX(PO_Enrgy_10_Table,0,MATCH($Q$262,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_10_Table,0,MATCH(F$262,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_10_Table,0,MATCH(G$262,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_10_Table,0,MATCH(H$262,PO_Enrgy_10_Hdr,0)),INDEX(PO_Enrgy_10_Table,0,MATCH($Q$262,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_10_Table,0,MATCH(I$262,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_10_Table,0,MATCH(J$262,PO_Enrgy_10_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H266/E266,\"\")","v":""},null,{"$f":"IFERROR(1-J266/G266,\"\")","v":""}]
["G"]
["G","Data Center - Performance Rating Method Results"]
["G",{"$f":"CONCATENATE(\"Startup IT Loads: Enter the simulated energy consumption and cost for the Data Center based on Startup IT Loads as defined in the LEED Reference Guide.\",\" Report exceptional calculations and results from the Data Center calculator in the startup load results below,\",\" but do not include renewable energy in these reported results. Provide separate exceptional calculation method uploads as applicable for Startup Loads and for Full build-out.\", \" Also upload simulation outputs and performance rating method calculations with and without the exceptional calculation methods for both Startup IT Loads, and the full buildout IT loads.\",\"\n\n\",IF(DESPath=3,\" Note: The calculations using DES Path 3 must be performed manually for the Startup IT Load method, and supplemental documentation uploaded for the project must show these calculations.\",\"\"))","v":"Startup IT Loads: Enter the simulated energy consumption and cost for the Data Center based on Startup IT Loads as defined in the LEED Reference Guide. Report exceptional calculations and results from the Data Center calculator in the startup load results below, but do not include renewable energy in these reported results. Provide separate exceptional calculation method uploads as applicable for Startup Loads and for Full build-out. Also upload simulation outputs and performance rating method calculations with and without the exceptional calculation methods for both Startup IT Loads, and the full buildout IT loads.\n\n"}]
["G","Table: Performance rating data center - Startup IT loads"]
["G","Energy Type","Site Energy Units",null,"Baseline Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B274),\"\",VLOOKUP($B274,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C274=\"\",\"\",VLOOKUP(C274,ProjectEnergyTypeTable,3,FALSE))","v":""},null,{"$f":"IFERROR(E274*$Q274,\"\")","v":""},null,null,{"$f":"IFERROR(H274*$Q274,\"\")","v":""},null,{"$f":"IFERROR(1-H274/E274,\"\")","v":""},null,{"$f":"IFERROR(1-J274/G274,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B274),\"\",VLOOKUP($B274,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B274),\"\",VLOOKUP($B274,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B275),\"\",VLOOKUP($B275,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C275=\"\",\"\",VLOOKUP(C275,ProjectEnergyTypeTable,3,FALSE))","v":""},null,{"$f":"IFERROR(E275*$Q275,\"\")","v":""},null,null,{"$f":"IFERROR(H275*$Q275,\"\")","v":""},null,{"$f":"IFERROR(1-H275/E275,\"\")","v":""},null,{"$f":"IFERROR(1-J275/G275,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B275),\"\",VLOOKUP($B275,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B275),\"\",VLOOKUP($B275,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B276),\"\",VLOOKUP($B276,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C276=\"\",\"\",VLOOKUP(C276,ProjectEnergyTypeTable,3,FALSE))","v":""},null,{"$f":"IFERROR(E276*$Q276,\"\")","v":""},null,null,{"$f":"IFERROR(H276*$Q276,\"\")","v":""},null,{"$f":"IFERROR(1-H276/E276,\"\")","v":""},null,{"$f":"IFERROR(1-J276/G276,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B276),\"\",VLOOKUP($B276,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B276),\"\",VLOOKUP($B276,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_11_Table,0,MATCH(E$273,PO_Enrgy_11_Hdr,0)),INDEX(PO_Enrgy_11_Table,0,MATCH($Q$273,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_11_Table,0,MATCH(F$273,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_11_Table,0,MATCH(G$273,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_11_Table,0,MATCH(H$273,PO_Enrgy_11_Hdr,0)),INDEX(PO_Enrgy_11_Table,0,MATCH($Q$273,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_11_Table,0,MATCH(I$273,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_11_Table,0,MATCH(J$273,PO_Enrgy_11_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H277/E277,\"\")","v":""},null,{"$f":"IFERROR(1-J277/G277,\"\")","v":""}]
["G"]
["G","Table: Performance rating data center - Full load IT loads (tabulated from spreadsheet data entered above)"]
["G","Energy Type","Site Energy Units",null,"Baseline Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B283),\"\",VLOOKUP($B283,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C283=\"\",\"\",VLOOKUP(C283,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(VLOOKUP($B283,PO_Enrgy_10_Table,MATCH($E$262,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(E283*$R283,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B283,PO_Enrgy_10_Table,MATCH($G$262,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B283,PO_Enrgy_10_Table,MATCH($H$262,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(H283*$R283,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B283,PO_Enrgy_10_Table,MATCH($J$262,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(1-H283/E283,\"\")","v":""},null,{"$f":"IFERROR(1-J283/G283,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B283),\"\",VLOOKUP($B283,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B283),\"\",VLOOKUP($B283,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B284),\"\",VLOOKUP($B284,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C284=\"\",\"\",VLOOKUP(C284,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(VLOOKUP($B284,PO_Enrgy_10_Table,MATCH($E$262,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(E284*$R284,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B284,PO_Enrgy_10_Table,MATCH($G$262,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B284,PO_Enrgy_10_Table,MATCH($H$262,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(H284*$R284,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B284,PO_Enrgy_10_Table,MATCH($J$262,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(1-H284/E284,\"\")","v":""},null,{"$f":"IFERROR(1-J284/G284,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B284),\"\",VLOOKUP($B284,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B284),\"\",VLOOKUP($B284,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B285),\"\",VLOOKUP($B285,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C285=\"\",\"\",VLOOKUP(C285,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(VLOOKUP($B285,PO_Enrgy_10_Table,MATCH($E$262,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(E285*$R285,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B285,PO_Enrgy_10_Table,MATCH($G$262,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B285,PO_Enrgy_10_Table,MATCH($H$262,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(H285*$R285,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B285,PO_Enrgy_10_Table,MATCH($J$262,PO_Enrgy_10_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(1-H285/E285,\"\")","v":""},null,{"$f":"IFERROR(1-J285/G285,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B285),\"\",VLOOKUP($B285,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B285),\"\",VLOOKUP($B285,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_12_Table,0,MATCH(E$282,PO_Enrgy_12_Hdr,0)),INDEX(PO_Enrgy_12_Table,0,MATCH($Q$282,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_12_Table,0,MATCH(F$282,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_12_Table,0,MATCH(G$282,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_12_Table,0,MATCH(H$282,PO_Enrgy_12_Hdr,0)),INDEX(PO_Enrgy_12_Table,0,MATCH($Q$282,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_12_Table,0,MATCH(I$282,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_12_Table,0,MATCH(J$282,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H286/E286,\"\")","v":""},null,{"$f":"IFERROR(1-J286/G286,\"\")","v":""}]
["G"]
["G","Table: Performance rating data center - Average between full Load IT loads and startup IT loads"]
["G","Energy Type","Site Energy Units",null,"Baseline Building Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Building Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B292),\"\",VLOOKUP($B292,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C292=\"\",\"\",VLOOKUP(C292,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B292,PO_Enrgy_11_Table,MATCH($E$273,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B292,PO_Enrgy_12_Table,MATCH($E$282,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B292,PO_Enrgy_12_Table,MATCH($E$282,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(E292*$R292,\"\")","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B292,PO_Enrgy_11_Table,MATCH($G$273,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B292,PO_Enrgy_12_Table,MATCH($G$282,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B292,PO_Enrgy_12_Table,MATCH($G$282,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B292,PO_Enrgy_11_Table,MATCH($H$273,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B292,PO_Enrgy_12_Table,MATCH($H$282,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B292,PO_Enrgy_12_Table,MATCH($H$282,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(H292*$R292,\"\")","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B292,PO_Enrgy_11_Table,MATCH($J$273,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B292,PO_Enrgy_12_Table,MATCH($J$282,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B292,PO_Enrgy_12_Table,MATCH($J$282,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(1-H292/E292,\"\")","v":""},null,{"$f":"IFERROR(1-J292/G292,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B292),\"\",VLOOKUP($B292,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B292),\"\",VLOOKUP($B292,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B293),\"\",VLOOKUP($B293,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C293=\"\",\"\",VLOOKUP(C293,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B293,PO_Enrgy_11_Table,MATCH($E$273,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B293,PO_Enrgy_12_Table,MATCH($E$282,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B293,PO_Enrgy_12_Table,MATCH($E$282,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(E293*$R293,\"\")","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B293,PO_Enrgy_11_Table,MATCH($G$273,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B293,PO_Enrgy_12_Table,MATCH($G$282,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B293,PO_Enrgy_12_Table,MATCH($G$282,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B293,PO_Enrgy_11_Table,MATCH($H$273,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B293,PO_Enrgy_12_Table,MATCH($H$282,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B293,PO_Enrgy_12_Table,MATCH($H$282,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(H293*$R293,\"\")","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B293,PO_Enrgy_11_Table,MATCH($J$273,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B293,PO_Enrgy_12_Table,MATCH($J$282,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B293,PO_Enrgy_12_Table,MATCH($J$282,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(1-H293/E293,\"\")","v":""},null,{"$f":"IFERROR(1-J293/G293,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B293),\"\",VLOOKUP($B293,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B293),\"\",VLOOKUP($B293,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B294),\"\",VLOOKUP($B294,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C294=\"\",\"\",VLOOKUP(C294,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B294,PO_Enrgy_11_Table,MATCH($E$273,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B294,PO_Enrgy_12_Table,MATCH($E$282,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B294,PO_Enrgy_12_Table,MATCH($E$282,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(E294*$R294,\"\")","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B294,PO_Enrgy_11_Table,MATCH($G$273,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B294,PO_Enrgy_12_Table,MATCH($G$282,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B294,PO_Enrgy_12_Table,MATCH($G$282,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B294,PO_Enrgy_11_Table,MATCH($H$273,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B294,PO_Enrgy_12_Table,MATCH($H$282,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B294,PO_Enrgy_12_Table,MATCH($H$282,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(H294*$R294,\"\")","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,AVERAGE(VLOOKUP($B294,PO_Enrgy_11_Table,MATCH($J$273,PO_Enrgy_11_Hdr,0),FALSE),VLOOKUP($B294,PO_Enrgy_12_Table,MATCH($J$282,PO_Enrgy_12_Hdr,0),FALSE)),VLOOKUP($B294,PO_Enrgy_12_Table,MATCH($J$282,PO_Enrgy_12_Hdr,0),FALSE)),\"\")","v":0},{"$f":"IFERROR(1-H294/E294,\"\")","v":""},null,{"$f":"IFERROR(1-J294/G294,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B294),\"\",VLOOKUP($B294,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B294),\"\",VLOOKUP($B294,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"\"Energy Model Subtotal (\" & PO_SiteUnits & \")\"","v":"Energy Model Subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_13_Table,0,MATCH(E$291,PO_Enrgy_13_Hdr,0)),INDEX(PO_Enrgy_13_Table,0,MATCH($Q$291,PO_Enrgy_13_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(F$291,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(G$291,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_13_Table,0,MATCH(H$291,PO_Enrgy_13_Hdr,0)),INDEX(PO_Enrgy_13_Table,0,MATCH($Q$291,PO_Enrgy_13_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(I$291,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(J$291,PO_Enrgy_12_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H295/E295,\"\")","v":""},null,{"$f":"IFERROR(1-J295/G295,\"\")","v":""}]
["G"]
["G","Total energy cost savings (excluding site-generated renewable energy) (%)",null,null,null,null,null,null,null,null,{"$f":"$M$295","v":""}]
["G"]
["G","Table: Renewable energy production"]
["G","Energy Type","Site Energy Units",null,"On-Site Renewable Savings",null,null,"Proposed with On-Site Renewable Energy",null,null,"Percent Cost Savings"]
["G",null,null,null,"Site Energy Use Savings ",{"$f":"\"Source Energy Use Savings \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use Savings \n(Btu x 10^6)"},"Cost Savings","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Renewable_Site_Savings","Renewable_Source_Savings","Renewable_Cost_Savings","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion","Virtual Rate"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B303),\"\",VLOOKUP($B303,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C303=\"\",\"\",VLOOKUP(C303,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,VLOOKUP($B303,PO_Enrgy_2_Table,MATCH($E$38,PO_Enrgy_2_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E303*$R303,\"\")","v":""},{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,VLOOKUP($B303,PO_Enrgy_2_Table,MATCH($J$38,PO_Enrgy_2_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B303,PO_Enrgy_13_Table,MATCH($H$291,PO_Enrgy_13_Hdr,0),FALSE)-IF(PO_SiteRenewable=TRUE,VLOOKUP($B303,PO_Enrgy_2_Table,MATCH($E$38,PO_Enrgy_2_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(H303*$R303,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B303,PO_Enrgy_13_Table,MATCH($J$291,PO_Enrgy_13_Hdr,0),FALSE)-IF(PO_SiteRenewable=TRUE,VLOOKUP($B303,PO_Enrgy_2_Table,MATCH($J$38,PO_Enrgy_2_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(1-$H303/VLOOKUP($B303,PO_Enrgy_13_Table,MATCH($E$291,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},null,{"$f":"IFERROR(1-$J303/VLOOKUP($B303,PO_Enrgy_13_Table,MATCH($G$291,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B303),\"\",VLOOKUP($B303,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B303),\"\",VLOOKUP($B303,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(G303/E303,\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B304),\"\",VLOOKUP($B304,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C304=\"\",\"\",VLOOKUP(C304,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,VLOOKUP($B304,PO_Enrgy_2_Table,MATCH($E$38,PO_Enrgy_2_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E304*$R304,\"\")","v":""},{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,VLOOKUP($B304,PO_Enrgy_2_Table,MATCH($J$38,PO_Enrgy_2_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B304,PO_Enrgy_13_Table,MATCH($H$291,PO_Enrgy_13_Hdr,0),FALSE)-IF(PO_SiteRenewable=TRUE,VLOOKUP($B304,PO_Enrgy_2_Table,MATCH($E$38,PO_Enrgy_2_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(H304*$R304,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B304,PO_Enrgy_13_Table,MATCH($J$291,PO_Enrgy_13_Hdr,0),FALSE)-IF(PO_SiteRenewable=TRUE,VLOOKUP($B304,PO_Enrgy_2_Table,MATCH($J$38,PO_Enrgy_2_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(1-$H304/VLOOKUP($B304,PO_Enrgy_13_Table,MATCH($E$291,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},null,{"$f":"IFERROR(1-$J304/VLOOKUP($B304,PO_Enrgy_13_Table,MATCH($G$291,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B304),\"\",VLOOKUP($B304,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B304),\"\",VLOOKUP($B304,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(G304/E304,\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B305),\"\",VLOOKUP($B305,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C305=\"\",\"\",VLOOKUP(C305,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,VLOOKUP($B305,PO_Enrgy_2_Table,MATCH($E$38,PO_Enrgy_2_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(E305*$R305,\"\")","v":""},{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,VLOOKUP($B305,PO_Enrgy_2_Table,MATCH($J$38,PO_Enrgy_2_Hdr,0),FALSE),0),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B305,PO_Enrgy_13_Table,MATCH($H$291,PO_Enrgy_13_Hdr,0),FALSE)-IF(PO_SiteRenewable=TRUE,VLOOKUP($B305,PO_Enrgy_2_Table,MATCH($E$38,PO_Enrgy_2_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(H305*$R305,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B305,PO_Enrgy_13_Table,MATCH($J$291,PO_Enrgy_13_Hdr,0),FALSE)-IF(PO_SiteRenewable=TRUE,VLOOKUP($B305,PO_Enrgy_2_Table,MATCH($J$38,PO_Enrgy_2_Hdr,0),FALSE),0),0)","v":0},{"$f":"IFERROR(1-$H305/VLOOKUP($B305,PO_Enrgy_13_Table,MATCH($E$291,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},null,{"$f":"IFERROR(1-$J305/VLOOKUP($B305,PO_Enrgy_13_Table,MATCH($G$291,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B305),\"\",VLOOKUP($B305,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B305),\"\",VLOOKUP($B305,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(G305/E305,\"\")","v":""}]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_14_Table,0,MATCH(E$302,PO_Enrgy_14_Hdr,0)),INDEX(PO_Enrgy_14_Table,0,MATCH($Q$302,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(F$302,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(G$302,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_14_Table,0,MATCH(H$302,PO_Enrgy_14_Hdr,0)),INDEX(PO_Enrgy_14_Table,0,MATCH($Q$302,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(I$302,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(J$302,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-$H306/$E$295,\"\")","v":""},null,{"$f":"IFERROR(1-$J306/$G$295,\"\")","v":""}]
["G"]
["G","Table: Data center PUE3 of startup and full buildout IT loads "]
["G",{"$f":"\"Enter the IT equipment energy consumption \" & IF(Datacenter_Avg=FALSE, \" and total building consumption by end-use including renewable energy \",\"\") & \"for the Startup IT loads.  The information for the full buildout loads is tabulated from the data above.  PUE3 is calculated based on source energy.\"","v":"Enter the IT equipment energy consumption  and total building consumption by end-use including renewable energy for the Startup IT loads.  The information for the full buildout loads is tabulated from the data above.  PUE3 is calculated based on source energy."}]
["G","Energy Type","Site Energy Units",null,"Startup IT Loads\nBuilding energy consumption with Startup IT loads \nincluding Data Center Calculator and exceptional calculation measures",null,null,null,"Full Buildout IT Loads\nBuilding energy consumption with Full Buildout IT loads \nincluding Data Center Calculator and exceptional calculation measures"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"PUE3",null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"PUE3"]
["G","Energy_Type","Energy_Units",null,"Startup_Site_Energy","Startup_Source_Energy","Startup_PUE",null,"Buildout_Site_Energy","Buildout_Source_Energy","Buildoout_PUE",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"B191","v":"IT equipment"},"kWh",{"$f":"IF(C313=\"\",\"\",VLOOKUP(C313,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},null,{"$f":"IFERROR(E313*$R313,\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP(B313,PO_design_table,MATCH($H$170,PO_design_hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(I313*$R313,\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(VLOOKUP(\"Electricity\",PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(\"electricity\",PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE),\"\")","v":""}]
["G","Total building consumption by end-use",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B315),\"\",VLOOKUP($B315,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C315=\"\",\"\",VLOOKUP(C315,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B315,PO_Enrgy_11_Table,MATCH($H$273,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B315,PO_Enrgy_14_Table,MATCH($E302,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(E315*$R315,\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP($B315,PO_Enrgy_12_Table,MATCH($H$282,PO_Enrgy_12_Hdr,0),FALSE)-VLOOKUP($B315,PO_Enrgy_14_Table,MATCH($E$302,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(I315*$R315,\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B315),\"\",VLOOKUP($B315,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B315),\"\",VLOOKUP($B315,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B316),\"\",VLOOKUP($B316,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C316=\"\",\"\",VLOOKUP(C316,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B316,PO_Enrgy_11_Table,MATCH($H$273,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B316,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(E316*$R316,\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP($B316,PO_Enrgy_12_Table,MATCH($H$282,PO_Enrgy_12_Hdr,0),FALSE)-VLOOKUP($B316,PO_Enrgy_14_Table,MATCH($E$302,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(I316*$R316,\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B316),\"\",VLOOKUP($B316,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B316),\"\",VLOOKUP($B316,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B317),\"\",VLOOKUP($B317,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C317=\"\",\"\",VLOOKUP(C317,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(Datacenter_Avg=TRUE,VLOOKUP($B317,PO_Enrgy_11_Table,MATCH($H$273,PO_Enrgy_11_Hdr,0),FALSE)-VLOOKUP($B317,PO_Enrgy_14_Table,MATCH(#REF!,PO_Enrgy_14_Hdr,0),FALSE),\"\"),\"\")","v":""},{"$f":"IFERROR(E317*$R317,\"\")","v":""},null,null,{"$f":"IFERROR(VLOOKUP($B317,PO_Enrgy_12_Table,MATCH($H$282,PO_Enrgy_12_Hdr,0),FALSE)-VLOOKUP($B317,PO_Enrgy_14_Table,MATCH($E$302,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(I317*$R317,\"\")","v":""},null,null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B317),\"\",VLOOKUP($B317,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B317),\"\",VLOOKUP($B317,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_15_Table,0,MATCH(E$312,PO_Enrgy_15_Hdr,0)),INDEX(PO_Enrgy_15_Table,0,MATCH($Q$312,PO_Enrgy_15_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_15_Table,0,MATCH(F$312,PO_Enrgy_15_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(F318/F313,\"\")","v":""},null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_15_Table,0,MATCH(I$312,PO_Enrgy_15_Hdr,0)),INDEX(PO_Enrgy_15_Table,0,MATCH($Q$312,PO_Enrgy_15_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_15_Table,0,MATCH(J$312,PO_Enrgy_15_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(J318/J313,\"\")","v":""}]
["G"]
["G","Table: Total energy usage"]
["G","Energy Type","Site Energy Units",null,"Baseline",null,null,"Proposed",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B17),\"\",B17),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B324),\"\",VLOOKUP($B324,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C324=\"\",\"\",VLOOKUP(C324,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(VLOOKUP($B324,PO_Enrgy_13_Table,MATCH($E$291,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(E324*$R324,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B324,PO_Enrgy_13_Table,MATCH($G$291,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B324,PO_Enrgy_14_Table,MATCH($H$291,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(H324*$R324,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B324,PO_Enrgy_14_Table,MATCH($J$291,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(1-H324/E324,\"\")","v":""},null,{"$f":"IFERROR(1-J324/G324,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B324),\"\",VLOOKUP($B324,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B324),\"\",VLOOKUP($B324,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B18),\"\",B18),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B325),\"\",VLOOKUP($B325,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C325=\"\",\"\",VLOOKUP(C325,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(VLOOKUP($B325,PO_Enrgy_13_Table,MATCH($E$291,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(E325*$R325,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B325,PO_Enrgy_13_Table,MATCH($G$291,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B325,PO_Enrgy_14_Table,MATCH($H$291,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(H325*$R325,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B325,PO_Enrgy_14_Table,MATCH($J$291,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(1-H325/E325,\"\")","v":""},null,{"$f":"IFERROR(1-J325/G325,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B325),\"\",VLOOKUP($B325,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B325),\"\",VLOOKUP($B325,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G",{"$f":"IFERROR(IF(ISBLANK(B19),\"\",B19),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B326),\"\",VLOOKUP($B326,PO_Enrgy_1_Table,MATCH($C$16,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C326=\"\",\"\",VLOOKUP(C326,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(VLOOKUP($B326,PO_Enrgy_13_Table,MATCH($E$291,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(E326*$R326,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B326,PO_Enrgy_13_Table,MATCH($G$291,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(VLOOKUP($B326,PO_Enrgy_14_Table,MATCH($H$291,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(H326*$R326,\"\")","v":""},{"$f":"IFERROR(VLOOKUP($B326,PO_Enrgy_14_Table,MATCH($J$291,PO_Enrgy_14_Hdr,0),FALSE),\"\")","v":0},{"$f":"IFERROR(1-H326/E326,\"\")","v":""},null,{"$f":"IFERROR(1-J326/G326,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B326),\"\",VLOOKUP($B326,PO_Enrgy_1_Table,MATCH($K$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B326),\"\",VLOOKUP($B326,PO_Enrgy_1_Table,MATCH($M$16,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","Totals",null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_16_Table,0,MATCH(E$323,PO_Enrgy_16_Hdr,0)),INDEX(PO_Enrgy_16_Table,0,MATCH($Q$323,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(F$323,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(G$323,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_16_Table,0,MATCH(H$323,PO_Enrgy_16_Hdr,0)),INDEX(PO_Enrgy_16_Table,0,MATCH($Q$323,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(I$323,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(J$323,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-H327/E327,\"\")","v":""},null,{"$f":"IFERROR(1-J327/G327,\"\")","v":""}]
["G","Total energy cost savings (including site-generated renewable energy) (%)",null,null,null,null,null,null,null,null,null,null,{"$f":"$M$327","v":""}]
["G"]
["G","Unmet Loads"]
[null,"Enter the non-coincident unmet load hours, consistent with the energy simulation output reports."]
["G","Unmet Loads",null,null,null,"Baseline",null,null,"Proposed"]
["G","Number of hours heating loads not met"]
["G","Number of hours cooling loads not met"]
["G","Totals",null,null,null,{"$f":"IF(ISERROR(F333+F334),0,F333+F334)","v":0},null,null,{"$f":"IF(ISERROR(I333+I334),0,I333+I334)","v":0}]
["G","Compliance",null,null,null,{"$f":"IF(ISERROR(OR(F333+F334,I333+I334)),\"Enter numbers only\",\n     IF(OR(F335>300,I335>300),\"No\",\"Yes\"))","v":"Yes"}]
[null,null,{"$f":"IF(ISERROR(F335+I335),\"\",IF(OR(I335>300,F335>300),\"Revise the model so that the unmet load hours for both the baseline and proposed case are 300 hours or less\",\"\"))","v":""}]
[null,"Quality Assurance Checks"]
[null,{"$f":"IF(MultipleBuildingsExist=\"No\",\"General information\",\"Multiple Building Details\")","v":"General information"},{"$f":"\"Total Area \"&IF(SI_IP_Units=\"IP\",\"(sq ft)\",\"(sq m)\")","v":"Total Area (sq ft)"}]
[null,null,{"$f":"IFERROR(IF(MultipleBuildingsExist=\"No\",\nGI_BldgArea,\nSUMIF(MBD_BS_Index,$H$5,OFFSET(MBD_BS_Index,0,MATCH('1 - Multiple Buildings Details'!$G$22,MBD_BS_Hdr,0)-1,1,1))+SUMIF(MBD_BS_Index,$H$5,OFFSET(MBD_BS_Index,0,MATCH('1 - Multiple Buildings Details'!$H$22,MBD_BS_Hdr,0)-1,1,1))),\"\")","v":0}]
[null,"Lighting",{"$f":"\"Total Area \"&IF(SI_IP_Units=\"IP\",\"(sq ft)\",\"(sq m)\")","v":"Total Area (sq ft)"},"Base Lighting Demand",null,"Design Lighting Demand","Base Exterior Lighting Demand","Design Exterior Lighting Demand","Base Non Tradeable Exterior Lighting Maximum","Design Non Tradeable Exterior Lighting Maximum"]
[null,null,{"$f":"IFERROR(IF(L_LPDmethod=1,SUMIF(L_BAMInput_Index,$H$5,OFFSET(L_BAMInput_Index,0,MATCH('6b - General Lighting'!$D$32,Lighting_Residential_Hdr,0)-1)),SUMIF(L_SxSInput_Index,$H$5,OFFSET(L_SxSInput_Index,0,MATCH('6b - General Lighting'!$E$61,Lighting_SxS_Residential_Hdr,0)-1))),\"\")","v":""},{"$f":"IFERROR(OFFSET(L_IL_SumTable,MATCH($H$5,L_IL_SumIndex,0)-1,MATCH('6b - General Lighting'!$L$107,L_IL_SumHdr,0)-1,1,1),\"\")","v":"Base_Power"},null,{"$f":"IFERROR(OFFSET(L_IL_SumTable,MATCH($H$5,L_IL_SumIndex,0)-1,MATCH('6b - General Lighting'!$O$107,L_IL_SumHdr,0)-1,1,1),\"\")","v":"Design_Power"},{"$f":"IFERROR(OFFSET(L_ExtSum_Table,1,MATCH('6b - General Lighting'!$J$171,L_ExtSum_Hdr,0)-1,1,1),\"\")","v":0},{"$f":"IFERROR(OFFSET(L_ExtSum_Table,1,MATCH('6b - General Lighting'!$M$171,L_ExtSum_Hdr,0)-1,1,1),\"\")","v":0},{"$f":"IFERROR(OFFSET(L_LtgZone_Table,1,MATCH('6b - General Lighting'!$M$134,L_LtgZone_Hdr,0)-1,1,1)+OFFSET(L_NTSurface_Table,MATCH('6b - General Lighting'!$B$165,L_NTSurface_Index,0)-1,MATCH('6b - General Lighting'!$J$158,L_NTSurface_Hdr,0)-1,1,1),\"\")","v":""},{"$f":"IFERROR(OFFSET(L_NTSurface_Table,MATCH('6b - General Lighting'!$B$165,L_NTSurface_Index,0)-1,MATCH('6b - General Lighting'!$M$158,L_NTSurface_Hdr,0)-1,1,1),\"\")","v":0}]
[null,"Shading and Fenestration","Glazing Differential","Baseline Above 40%",null,"Zones Modeled"]
[null,null,{"$f":"IFERROR(SUMIF('4 - Shading and Fenestration'!S:S,$H$5,'4 - Shading and Fenestration'!T:T),\"\")","v":0},{"$f":"IF(IFERROR(COUNTIFS('4 - Shading and Fenestration'!S:S,$H$5,'4 - Shading and Fenestration'!U:U,TRUE),\"\")>0,TRUE,FALSE)","v":false},null,{"$f":"IFERROR(OFFSET('4 - Shading and Fenestration'!S:U,MATCH(CONCATENATE($H$5, \" zones\"),'4 - Shading and Fenestration'!S:S,0)-1,1,1,1),\"\")","v":""}]
[null,"Performance Outputs","Baseline Lighting EFLHs","Design Lighting EFLHs",null,"Base Lighting Demand","Design Lighting Demand","Base Exterior Lighitng Consumption","Design Exterior Lighting Consumption","Base Exterior EFLH","Design Ext EFLH"]
[null,null,{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$171,PO_design_index,0)-2,MATCH($S$170,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$171,PO_design_index,0)-2,MATCH($T$170,PO_design_hdr,0)-1,1,1)),\"\")","v":0},null,{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$171,PO_design_index,0)-1,MATCH($G$170,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$171,PO_design_index,0)-1,MATCH($H$170,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$173,PO_design_index,0)-2,MATCH($G$170,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$173,PO_design_index,0)-2,MATCH($H$170,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$173,PO_design_index,0)-2,MATCH($S$170,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$173,PO_design_index,0)-2,MATCH($T$170,PO_design_hdr,0)-1,1,1)),\"\")","v":0}]
[null,null,"Base Exterior Lighting Demand","Design Exterior Lighting Demand",null,"Base Miscellaneous % of Total","Design Miscellaneous % of Total","Unregulated Load Difference","Base Service Hot Waters % of Total","Design Service Hot Water % of Total","Base Pump Consumption",null,"Base Fan EFLH"]
[null,null,{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$173,PO_design_index,0)-1,MATCH($G$170,PO_design_hdr,0)-1,1,1)),\"\")","v":0},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$173,PO_design_index,0)-1,MATCH($H$170,PO_design_hdr,0)-1,1,1)),\"\")","v":0},null,{"$f":"IFERROR((OFFSET(PO_design_table,MATCH($B$189,PO_design_index,0)-2,MATCH($G$170,PO_design_hdr,0)-1,1,1)*OFFSET(PO_design_table,MATCH($B$189,PO_design_index,0)-2,MATCH($Q$170,PO_design_hdr,0)-1,1,1))/OFFSET(PO_ModelSubtotal,0,4,1,1),\"\")","v":""},{"$f":"IFERROR((OFFSET(PO_design_table,MATCH($B$189,PO_design_index,0)-2,MATCH($H$170,PO_design_hdr,0)-1,1,1)*OFFSET(PO_design_table,MATCH($B$189,PO_design_index,0)-2,MATCH($Q$170,PO_design_hdr,0)-1,1,1))/OFFSET(PO_ModelSubtotal,0,7,1,1),\"\")","v":""},null,{"$f":"IFERROR((OFFSET(PO_design_table,MATCH($B$187,PO_design_index,0)-2,MATCH($G$170,PO_design_hdr,0)-1,1,1)*OFFSET(PO_design_table,MATCH($B$187,PO_design_index,0)-2,MATCH($Q$170,PO_design_hdr,0)-1,1,1))/OFFSET(PO_ModelSubtotal,0,4,1,1),\"\")","v":""},{"$f":"IFERROR((OFFSET(PO_design_table,MATCH($B$187,PO_design_index,0)-2,MATCH($H$170,PO_design_hdr,0)-1,1,1)*OFFSET(PO_design_table,MATCH($B$187,PO_design_index,0)-2,MATCH($Q$170,PO_design_hdr,0)-1,1,1))/OFFSET(PO_ModelSubtotal,0,7,1,1),\"\")","v":""},{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$179,PO_design_index,0)-2,MATCH($G$170,PO_design_hdr,0)-1,1,1)),\"\")","v":0},null,{"$f":"IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$183,PO_design_index,0)-2,MATCH($S$170,PO_design_hdr,0)-1,1,1)),\"\")","v":0}]
[null,null,"Design Fan EFLH","Base Fan Demand",null,"Design Fan Demand","PV EFLH","Renewable Rate Difference","Proposed Electric Rate","Proposed Gas Rate","Total Baseline Exterior Lighting Demand",null,"Total Design Exterior Lighting Demand"]
[null,null,{"$f":"IFERROR(IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$183,PO_design_index,0)-2,MATCH($T$170,PO_design_hdr,0)-1,1,1)),\"\"),\"\")","v":0},{"$f":"IFERROR(IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$183,PO_design_index,0)-1,MATCH($G$170,PO_design_hdr,0)-1,1,1)),\"\"),\"\")","v":0},null,{"$f":"IFERROR(IFERROR(MAX(OFFSET(PO_design_table,MATCH($B$183,PO_design_index,0)-1,MATCH($H$170,PO_design_hdr,0)-1,1,1)),\"\"),\"\")","v":0},{"$f":"IFERROR(MAX(IFERROR(OFFSET(PO_renewable_table,MATCH(\"Photovoltaic system\",PO_renewable_Index,0)-2,MATCH($S$32,PO_renewable_hdr,0)-1,1,1),0),\nIFERROR(OFFSET(PO_renewable_table,MATCH(\"Solar thermal system\",PO_renewable_Index,0)-2,MATCH($S$32,PO_renewable_hdr,0)-1,1,1),0)),\"\")","v":""},null,{"$f":"IFERROR(OFFSET(PO_Enrgy_8_Table,MATCH(\"Electricity\",PO_Enrgy_8_Index,0)-2,MATCH($H$232,PO_Enrgy_8_Hdr,0)-1,1,1),\"\")","v":""},{"$f":"IFERROR(OFFSET(PO_Enrgy_8_Table,MATCH(\"Natural Gas\",PO_Enrgy_8_Index,0)-2,MATCH($H$232,PO_Enrgy_8_Hdr,0)-1,1,1),\"\")","v":""},{"$f":"IFERROR(GetPerformanceOutputRangeSums(\"PO_QA_BaseExtLtgDem\"),\"\")","v":"Error"},null,{"$f":"IFERROR(GetPerformanceOutputRangeSums(\"PO_QA_DesignExtLtgDem\"),\"\")","v":"Error"}]
[null,"General HVAC","Base non-water systems","Base water systems"]
[null,null,{"$f":"COUNTIFS(OFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$D$29,GHVAC_BSysType_Hdr,0)-1),\"System 2 - PTHP\",\nOFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$B$29,GHVAC_BSysType_Hdr,0)-1),$H$5)+\nCOUNTIFS(OFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$D$29,GHVAC_BSysType_Hdr,0)-1),\"System 3 - PSZ-AC\",\nOFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$B$29,GHVAC_BSysType_Hdr,0)-1),$H$5)+\nCOUNTIFS(OFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$D$29,GHVAC_BSysType_Hdr,0)-1),\"System 4 - PSZ-HP\",\nOFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$B$29,GHVAC_BSysType_Hdr,0)-1),$H$5)+\nCOUNTIFS(OFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$D$29,GHVAC_BSysType_Hdr,0)-1),\"System 6 - Packaged VAV with PFP Boxes\",\nOFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$B$29,GHVAC_BSysType_Hdr,0)-1),$H$5)+\nCOUNTIFS(OFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$D$29,GHVAC_BSysType_Hdr,0)-1),\"System 8 - VAV with PFP Boxes\",\nOFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$B$29,GHVAC_BSysType_Hdr,0)-1),$H$5)+\nCOUNTIFS(OFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$D$29,GHVAC_BSysType_Hdr,0)-1),\"System 9 - Heating and Ventilation\",\nOFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$B$29,GHVAC_BSysType_Hdr,0)-1),$H$5)+\nCOUNTIFS(OFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$D$29,GHVAC_BSysType_Hdr,0)-1),\"System 10 - Heating and Ventilation\",\nOFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$B$29,GHVAC_BSysType_Hdr,0)-1),$H$5)","v":0},{"$f":"COUNTIFS(OFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$D$29,GHVAC_BSysType_Hdr,0)-1),\"System 1 - PTAC\",\nOFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$B$29,GHVAC_BSysType_Hdr,0)-1),$H$5)+\nCOUNTIFS(OFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$D$29,GHVAC_BSysType_Hdr,0)-1),\"System 5 - Packaged VAV with Reheat\",\nOFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$B$29,GHVAC_BSysType_Hdr,0)-1),$H$5)+\nCOUNTIFS(OFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$D$29,GHVAC_BSysType_Hdr,0)-1),\"System 7 - VAV with Reheat\",\nOFFSET(GHVAC_BHVACST_Index,0,MATCH('9 - General HVAC'!$B$29,GHVAC_BSysType_Hdr,0)-1),$H$5)","v":0}]
[null,"Air-Side HVAC","Base Fan Flow","Design Fan Flow",null,"Base Fan Power","Design Fan Power","Base Cooling Capacity","Design Cooling Capacity","Base Heating Capacity","Design Heating Capacity"]
[null,null,{"$f":"IFERROR(SUMIFS(AHVAC_Base_FanFlow,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_FanFlow,AHVAC_Design_ID,$H$5),\"\")","v":0},null,{"$f":"IFERROR(SUMIFS(AHVAC_Base_FanPower,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_FanPower,AHVAC_Design_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Base_CoolingCap,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_CoolingCap,AHVAC_Design_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Base_HeatingCap,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_HeatingCap,AHVAC_Design_ID,$H$5),\"\")","v":0}]
[null,null,"Base OA","Design OA"]
[null,null,{"$f":"IFERROR(SUMIFS(AHVAC_Base_OAFlow,AHVAC_Base_ID,$H$5),\"\")","v":0},{"$f":"IFERROR(SUMIFS(AHVAC_Design_OAFlow,AHVAC_Design_ID,$H$5),\"\")","v":0}]
[]
[null,"Issue",null,null,null,null,null,null,"Project Team Respone",null,null,null,null,null,null,null,"Trigger","Issue Applicable"]
[null,{"$f":"\"The total building area reported in the \"&IF(MultipleBuildingsExist=\"No\",\"General Information\", \"Multiple Building Details\")& \" tab differs from the total building area reported in the Lighting tab (Interior Lighting section) by more than 10%. Please check for consistency and verify that the building areas reported are accurate.\"","v":"The total building area reported in the General Information tab differs from the total building area reported in the Lighting tab (Interior Lighting section) by more than 10%. Please check for consistency and verify that the building areas reported are accurate."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ABS(C340-C342)/MIN(C340,C342)>0.1,TRUE,FALSE),TRUE)","v":true}]
[null,"The vertical glazing areas in the proposed and baseline differ from one another (as reported on the Shading and Fenestration tab, Shading section), which is inconsistent with the requirement of Table G3.1.5(c) (baseline).  Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(C344>0.01,TRUE,FALSE),TRUE)","v":false}]
[null,"The baseline vertical glazing area is greater than 40% (as reported in the Shading and Fenestration tab, Shading section), which is inconsistent with the requirement of Table G3.1.5(c) (baseline).  Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(D344=TRUE,TRUE,FALSE),TRUE)","v":false}]
[null,"The baseline and/or proposed interior lighting equivalent full load hours (determined by dividing the total annual lighting consumption by the total lighting power as reported in the Performance Outputs tab) is greater than 4,000 hours/year, which is unexpectedly high. Ensure that the lighting models reflect all mandatory controls from Section 9 and reflect the anticipated schedule of operation for the building.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(C346>4000,D346>4000),TRUE,FALSE),TRUE)","v":false}]
[null,"The baseline and/or proposed interior lighting equivalent full load hours (determined by dividing the total annual lighting consumption by the total lighting power as reported in the Performance Outputs tab) differs by more than 10%, which is unexpected.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(ABS(C346-D346)/MIN(C346,D346)>0.1,MIN(C346,D346)=0),TRUE,FALSE),TRUE)","v":true}]
[null,"The interior lighting demand (as reported in the Performance Outputs tab for the baseline and/or proposed) exceeds the lighting power as reported in the Lighting sheet (Summary section) by more than 5%. Ensure that the values reflected in the Lighting sheet are accurate and appropriately reflect the modeled interior lighting power density.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(((F346-D342)/MIN(F346,D342))>0.05,((G346-F342)/MIN(G346,F342))>0.05),TRUE,FALSE),TRUE)","v":true}]
[null,"The Performance Outputs tab shows zero consumption for exterior lighting power in the baseline and/or proposed model.  Confirm that no exterior lighting is included in the building site. Verify that the proposed exterior lighting reflects the actual building design, and the baseline reflects the allowed lighting power from Section 9.4.3. Ensure that no credit is taken in the proposed for lighting reductions on non‐tradable surfaces.  (Note that additional lighting power allowance cannot be claimed in the baseline for surfaces that are not provided with lighting in the actual design, and that lighting fixtures cannot be double counted for different exterior surfaces).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(H346=0,I346=0),TRUE,FALSE),TRUE)","v":true}]
[null,"The baseline and/or proposed exterior lighting equivalent full load hours (determined by dividing the total annual lighting consumption by the total lighting power as reported in the Performance Outputs tab) is greater than 5,110 hours/year (approximately 14 hours per day) or less than 3,650 hours/year (approximately 10 hours per day). Ensure that the lighting models reflect all mandatory controls from Section 9.4.1.7.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(J346>5110,K346>5110),TRUE,FALSE),TRUE)","v":false}]
[null,"The baseline and/or proposed exterior lighting equivalent full load hours (determined by dividing the total annual lighting consumption by the total lighting power as reported in the Performance Outputs tab) differs by more than 5%, which is unexpected. Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ABS(J346-K346)/MIN(J346,K346)>0.05,TRUE,FALSE),TRUE)","v":true}]
[null,"The baseline and proposed exterior lighting consumption values are within 1% of each other, as reported in the Performance Outputs tab, indicating that the lighting has been modeled nearly identically. Verify that the proposed exterior lighting reflects the actual building design, and the baseline reflects the allowed lighting power from Section 9.4.3. Ensure that no credit is taken in the proposed for lighting reductions on non‐tradable surfaces. (Note that additional lighting power allowance cannot be claimed in the baseline for surfaces that are not provided with lighting in the actual design, and  that lighting fixtures cannot be double counted for different exterior surfaces.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ABS(H346-I346)/MIN(H346,I346)<0.01,TRUE,FALSE),TRUE)","v":true}]
[null,"The receptacle equipment consumption for the baseline and/or proposed building (as reported in the Performance Outputs tab) is greater than 40% (less than 10%) of the total building site energy usage, which is unexpectedly high (low). This check was made using the Performance rating energy consumption and cost by fuel type table (i.e. before adjustments were made for renewable energy production or an exceptional calculation method). Verify that the receptacle equipment has been modeled as accurately as possible.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(F348>0.4,G348>0.4,F348<0.1,G348<0.1),TRUE,FALSE),TRUE)","v":true}]
[null,"One (or more) of the unregulated end uses differs by more than 3% between the baseline and proposed as reported in the Performance Outputs tab. If savings are being attempted for an unregulated end use, the Exceptional Calculation Method must be followed.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(COUNTIFS(INDEX(PO_design_table,,MATCH($D$170,PO_design_hdr,0)),\"x\",INDEX(PO_design_table,,MATCH($I$170,PO_design_hdr,0)),\">0.03\")+COUNTIFS(INDEX(PO_design_table,,MATCH($D$170,PO_design_hdr,0)),\"x\",INDEX(PO_design_table,,MATCH($I$170,PO_design_hdr,0)),\"<-0.03\")>0,TRUE,FALSE),TRUE)","v":false}]
[null,"The service water heating consumption for the baseline and/or proposed building constitutes more than 15% of the total building site energy usage (as reported in the Performance Outputs tab), which is unexpected. This check was made using the Performance Rating - Energy Consumption and Cost by Fuel Type table (i.e. before any adjustments were made for renewable energy production or an exceptional calculation method). Verify that the service water heating has been modeled as designed, in accordance with Table G3.1.11 (b) (proposed) and that the schedule is typical of the building type in accordance with Table G3.1.4 (proposed).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(I348>0.15,J348>0.15),TRUE,FALSE),TRUE)","v":true}]
[null,"Pump consumption is reflected in the baseline outputs (as reported in the Performance Outputs tab), even though the baseline HVAC system type is 2, 3, 4, 6, 8, 9, or 10, none of which include an HVAC circulation loop.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AND(C352>0,D352<1),TRUE,FALSE),TRUE)","v":false}]
[null,"The total baseline and proposed air flow rates differ by more than 35% (as reported in the Air-Side HVAC sheet), making it unclear whether the baseline fan air flow rate was sized based on a 20 deg. F supply-air-to-room-air temperature difference, as required by G3.1.2.9.1 for each baseline system. Verify that the proposed has been modeled as designed in accordance with Table G3.1.10(b) (proposed) and that the baseline has been correctly sized in accordance with Appendix G requirements.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ABS(C354-D354)/MIN(C354,D354),TRUE,FALSE),TRUE)","v":true}]
[null,"The baseline and/or proposed fans equivalent full load hours (determined by dividing the total annual fan consumption by the total fan power as reported in the Performance Outputs tab) is greater than 4,000 hours/year, which is unexpectedly high. Ensure that the HVAC system models reflect all mandatory controls from Section 6, and reflect the anticipated schedule of operation for the building. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(M348>4000,C350>4000),TRUE,FALSE),TRUE)","v":false}]
[null,"The baseline and/or proposed fan equivalent full load hours (determined by dividing the total annual fan consumption by the total fan power as reported in the Performance Outputs tab) differs by more than 25%, which is unexpected. Ensure that the HVAC system models reflect all mandatory controls from Section 6, and reflect the anticipated schedule of operation for the building. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(ABS(M348-C350)/MIN(M348,C350)>0.25,TRUE,FALSE),TRUE)","v":true}]
[null,"The fan demand (as reported in the Performance Outputs tab) for the baseline and/or proposed exceeds the fan power as reported in the Air-Side HVAC tab (total system fan power) by more than 5%. Ensure that the values reflected in the Air-Side HVAC sheet are accurate and appropriately reflect the modeled fans.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(((D350-F354)/MIN(D350,F354))>0.05,((F350-G354)/MIN(F350,G354))>0.05),TRUE,FALSE),TRUE)","v":true}]
[null,"The fan demand (as reported in the Performance Outputs tab) for the baseline and/or proposed is 60% less than the fan power as reported in the Air-Side HVAC tab, which is unexpected. Ensure that the values reflected in the Air-Side HVAC tab are accurate and appropriately reflect the modeled fans.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(1-(D350/F354)>0.6,1-(F350/G354)>0.6),TRUE,FALSE),TRUE)","v":true}]
[null,"The total baseline and proposed capacities for the cooling and/or heating (as reported in the Air-Side HVAC tab) differ by more than 35%, making it unclear whether the baseline cooling and heating capacities have been met the G3.1.2.2 requirement for oversizing by 15% for cooling and 25% for heating. Verify that the proposed has been modeled as designed in accordance with Table G3.1.10(b) (proposed) and that the baseline has been sized in accordance with Appendix G requirements. Additionally, verify that the baseline capacities were oversized either at the system level or plant level, but not both, and that any other safety factors have been excluded from the baseline.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(ABS(H354-I354)/MIN(H354,I354)>0.35,ABS(J354-K354)/MIN(J354,K354)>0.35),TRUE,FALSE),TRUE)","v":true}]
[null,"The outdoor airflow rate is higher in the baseline model compared to the proposed (as reported in the Air-Side HVAC tab). Section G3.1.2.6 exception (c) requires that if the proposed design has more outdoor air than required by the rating authority (in this case USGBC/GBCI), then the baseline must be modeled with the amount required per EQ Prerequisite Minimum Indoor Air Quality Performance, and will be less than the rate modeled in the proposed. Ensure that the baseline outdoor airflow rate is consistent with that required by EQ Prerequisite Minimum Indoor Air Quality Performance. If applying G3.1.2.6 exception (b), and using an Ez value of 1.0 for the Baseline Case, upload baseline design ventilation rate procedure calculations as described in Standard 62.1 and as required by ASHRAE 90.1 in order to claim credit for this exception.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(C356>D356,TRUE,FALSE),TRUE)","v":false}]
[null,"The equivalent full load hours (determined by dividing the total annual consumption by the total rated capacity/power as reported in the Performance Outputs tab) for the photovoltaic system is greater than 1,500 hours/year, which is unexpectedly high. Provide documentation explaining the calculation method used to estimate the annual energy generated, and indicate all factors influencing the performance, such as derate factor, tilt, orientation, etc.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(G350>1500,TRUE,FALSE),TRUE)","v":true}]
[null,"The virtual energy rate for one or more of the energy types varies by more than 10% (as reported in the Performance Outputs tab). Ensure that the energy rates have been determined using either actual rates or state average energy prices published by DOE's Energy Information Administration. Provide information regarding the utility rate structure including all demand and energy charges and the seasonal and time-of-use structure of the utility tariff.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(COUNTIF(INDEX(PO_Enrgy_8_Table,,MATCH($K$232,PO_Enrgy_8_Hdr,0)),\">0.1\")+COUNTIF(INDEX(PO_Enrgy_8_Table,,MATCH($K$232,PO_Enrgy_8_Hdr,0)),\"<-0.1\")>0,TRUE,FALSE),TRUE)","v":false}]
[null,"The virtual energy rate for the renewable energy varies from the virtual energy rate for the proposed by more than 5% (as reported in the Performance Outputs tab), which is unexpected.  Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(PO_SiteRenewable=TRUE,IF(COUNTIF(INDEX(PO_renewable_table,,MATCH($U$32,PO_renewable_hdr,0)),\">0.05\")+COUNTIF(INDEX(PO_renewable_table,,MATCH($U$32,PO_renewable_hdr,0)),\"<-0.05\")>0,TRUE,FALSE),FALSE),TRUE)","v":false}]
[null,"The virtual energy rate for one or more exceptional calculation measures varies from the virtual energy rate for the proposed by more than 10% (as reported in the Performance Outputs tab), which is unexpected.  Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(PO_ShowExCalc=TRUE,IF(COUNTIF(INDEX(PO_ExCalc_Table,,MATCH($U$56,PO_ExCalc_Hdr,0)),\">0.05\")+COUNTIF(INDEX(PO_ExCalc_Table,,MATCH($U$56,PO_ExCalc_Hdr,0)),\"<-0.05\")>0,TRUE,FALSE),FALSE),TRUE)","v":false}]
[null,"The proposed virtual energy rate for electricity is less than $0.06 per kWh or greater than $0.25 per kWh (as reported in the Performance Outputs tab), which is unexpected. Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(I350<0.06,I350>0.25),TRUE,FALSE),TRUE)","v":true}]
[null,"The proposed virtual energy rate for natural gas is less than $0.50 per therm or greater than $2.00 per therm (as reported in the Performance Outputs tab), which is unexpected.  Please correct or provide justification.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR(J350<0.5,J350>2),TRUE,FALSE),TRUE)","v":true}]
[null,"The Energy Modeling Output Reporting Method (as reported in the Performance Outputs tab) indicates that the baseline has not been rotated because the building orientation is dictated by site considerations, as allowed by Table G3.1.5 (a) (baseline) Exception 1. Provide a detailed narrative (and additional documentation as necessary) describing why this exception has been applied.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(PO_EnergyReportingMethod>2,TRUE,FALSE),FALSE)","v":true}]
[null,"Two different types of heating consumption (e.g. electricity and natural gas) are reported in the baseline results in the Performance Outputs tab, which is unexpected. If modeling system type 3, note that there should be no crankcase heating or electric space heaters modeled in the baseline. If modeling system type 1, 5, or 7, note that the hot water boiler must be modeled as a natural draft boiler and there should be no electric space heaters modeled in the baseline. Please note that there are some exceptions (e.g. G3.1.1 (a)) which allow this situation; therefore, please be cautious before changing the model as a result of this comment.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AND(COUNTIFS(INDEX(PO_design_table,,MATCH($E$170,PO_design_hdr,0)),\"Electricity\",INDEX(PO_design_table,,MATCH($B$170,PO_design_hdr,0)),\"Space Heating\",INDEX(PO_design_table,,MATCH($G$170,PO_design_hdr,0)),\">0\")>0,COUNTIFS(INDEX(PO_design_table,,MATCH($E$170,PO_design_hdr,0)),\"<>Electricity\",INDEX(PO_design_table,,MATCH($B$170,PO_design_hdr,0)),\"Space Heating\",INDEX(PO_design_table,,MATCH($G$170,PO_design_hdr,0)),\">0\")>0),TRUE,FALSE),TRUE)","v":false}]
[null,"The unmet load hours exceed 300 hours for the baseline and/or proposed (as reported in the Performance Outputs tab), which is not in compliance with G3.1.2.3.  Please correct.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(MAX(F335:M335)>300,TRUE,FALSE),TRUE)","v":false}]
[null,{"$f":"\"The three largest end use contributors to the cost savings are \"&CONCATENATE(VLOOKUP(1,QCEnSaveRank,2,FALSE),\", \", VLOOKUP(2,QCEnSaveRank,2,FALSE), \", \",VLOOKUP(3,QCEnSaveRank,2,FALSE))&\" (as reported in the Performance Outputs tab). Please provide a narrative to justify the savings of these end uses, such as the energy conservation measures which contribute to the savings claimed.\"","v":"The three largest end use contributors to the cost savings are Interior lighting, Exterior lighting, Space heating (as reported in the Performance Outputs tab). Please provide a narrative to justify the savings of these end uses, such as the energy conservation measures which contribute to the savings claimed."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"TRUE","v":true}]
[null,"The rating system requires that a minimum of 2% of the energy savings must come from building power and cooling infrastructure. Provide a narrative describing how this requirement has been met. If necessary, include additional modeling output reports.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(RatingSystemSelection=\"LEED v4 BD+C: Data Centers\",TRUE,FALSE)","v":false}]
[null,"Inputs for the Shading and Fenestration tab indicate that less than 10 zones were modeled for the building.  This is unusually low for a standard submission.  Revise the quantity of zones input or provide a narrative justifying the number of zones used.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(F344<10,TRUE,FALSE),TRUE)","v":false}]
[null,"The exterior lighting demand as reported in the Performance Outputs tab for the baseline and/or proposed exceeds the lighting power reported on the Lighting sheet (Summary section) by more than 5%. Ensure that the values reflected in the Lighting sheet are accurate and appropriately reflect the modeled exterior lighting power density.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR((K350-G342)/MIN(K350,G342)>0.05,(M350-G342)/MIN(M350,G342)>0.05),TRUE,FALSE),TRUE)","v":true}]
[null,"The total exterior lighting power allowance, including the base site allowance, is less than the designed lighting power as reported in the Lighting tab, violating mandatory Section 9.4.3. Verify that the inputs are accurate and modify the exterior lighting design as necessary to show compliance.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(H342>G342,TRUE,FALSE),TRUE)","v":false}]
[null,"The value for nontradable exterior lighting power (building facades, ATMs and night depositories, entrances and gatehouse inspection stations at guarded facilities, loading areas for law enforcement, fire, ambulance, and other emergency service vehicles, drive-through windows at fast food restaurants, and/or parking near 24-hour retail entrances) is less than the designed lighting power after adding in the unrestricted lighting power allowance as reported in the Lighting sheet, violating mandatory Section 9.4.3. Verify that the inputs are accurate and modify the exterior lighting design as necessary to show compliance.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(J342>I342,TRUE,FALSE),TRUE)","v":false}]

{"sheet":"Performance_Outputs_Summary","index":39,"n_rows":220,"n_cols":55,"rows_kept":220,"cut":false,"hidden":true,"merged":[[178,2,178,3],[178,10,178,11],[174,2,174,3],[174,10,174,11],[195,2,195,3],[195,10,195,11],[129,2,129,3],[129,10,129,11],[130,2,130,3],[130,10,130,11],[151,2,151,3],[150,2,150,3],[131,2,131,3],[131,10,131,11],[153,2,153,3],[153,10,153,11],[151,10,151,11],[135,2,135,3],[135,10,135,11],[175,2,175,3],[175,10,175,11],[176,2,176,3],[176,10,176,11],[150,10,150,11],[12,2,12,3],[12,5,12,6],[12,7,12,9],[12,10,12,11],[87,2,87,3],[87,10,87,11],[108,2,108,3],[108,4,108,6],[108,7,108,9],[108,10,108,12],[13,2,13,3],[13,5,13,6],[13,7,13,9],[13,10,13,11],[88,2,88,3],[88,10,88,11],[103,7,103,9],[99,10,99,11],[14,2,14,3],[14,5,14,6],[14,7,14,9],[14,10,14,11],[89,2,89,3],[89,10,89,11],[11,7,11,9],[11,10,11,11],[86,2,86,3],[86,10,86,11],[107,2,107,3],[107,4,107,6],[107,7,107,9],[107,10,107,12],[127,2,127,3],[127,10,127,11],[126,2,126,3],[126,10,126,11],[106,2,106,3],[106,4,106,6],[106,7,106,9],[106,10,106,12],[121,1,121,11],[122,1,123,1],[102,1,102,11],[103,1,103,3],[103,4,103,6],[122,2,123,3],[122,4,122,6],[122,7,122,9],[219,9,219,12],[166,13,166,15],[167,10,167,11],[169,2,169,3],[169,10,169,11],[170,2,170,3],[170,10,170,11],[218,9,218,12],[218,1,218,8],[219,1,219,8],[205,1,205,3],[205,10,205,11],[194,2,194,3],[194,10,194,11],[193,2,193,3],[193,10,193,11],[192,2,192,3],[192,10,192,11],[166,7,166,9],[166,10,166,12],[217,9,217,12],[215,1,215,8],[215,9,215,12],[216,1,216,8],[217,1,217,8],[210,1,211,1],[212,1,213,1],[216,9,216,12],[209,1,209,12],[184,1,184,3],[184,10,184,11],[206,1,206,11],[190,2,190,3],[190,10,190,11],[191,2,191,3],[191,10,191,11],[187,1,188,1],[187,2,188,3],[187,4,187,6],[187,7,187,9],[187,10,187,12],[188,10,188,11],[198,2,198,3],[198,10,198,11],[196,2,196,3],[196,10,196,11],[197,2,197,3],[197,10,197,11],[143,13,143,15],[144,10,144,11],[146,10,146,11],[147,2,147,3],[147,10,147,11],[146,2,146,3],[141,1,141,11],[143,1,144,1],[143,2,144,3],[143,4,143,6],[143,7,143,9],[143,10,143,12],[75,31,76,32],[77,1,78,2],[77,3,78,3],[77,4,78,4],[77,9,78,9],[77,10,78,11],[77,12,78,12],[77,31,78,32],[75,1,76,2],[75,3,76,3],[75,4,76,4],[75,9,76,9],[75,10,76,11],[75,12,76,12],[122,13,122,15],[123,10,123,11],[125,2,125,3],[125,10,125,11],[71,31,72,32],[73,1,74,2],[73,3,74,3],[73,4,74,4],[73,9,74,9],[73,10,74,11],[73,12,74,12],[73,31,74,32],[71,1,72,2],[71,3,72,3],[71,4,72,4],[71,9,72,9],[71,10,72,11],[71,12,72,12],[103,10,103,12],[84,2,84,3],[84,10,84,11],[85,2,85,3],[85,10,85,11],[99,1,99,3],[67,31,68,32],[69,1,70,2],[69,3,70,3],[69,4,70,4],[69,9,70,9],[69,10,70,11],[69,12,70,12],[69,31,70,32],[67,1,68,2],[67,3,68,3],[67,4,68,4],[67,9,68,9],[67,10,68,11],[67,12,68,12],[63,31,64,32],[65,1,66,2],[65,3,66,3],[65,4,66,4],[65,9,66,9],[65,10,66,11],[65,12,66,12],[65,31,66,32],[63,1,64,2],[63,3,64,3],[63,4,64,4],[63,9,64,9],[63,10,64,11],[63,12,64,12],[59,31,60,32],[61,1,62,2],[61,3,62,3],[61,4,62,4],[61,9,62,9],[61,10,62,11],[61,12,62,12],[61,31,62,32],[59,1,60,2],[59,3,60,3],[59,4,60,4],[59,9,60,9],[59,10,60,11],[59,12,60,12],[55,31,56,32],[57,1,58,2],[57,3,58,3],[57,4,58,4],[57,9,58,9],[57,10,58,11],[57,12,58,12],[57,31,58,32],[55,1,56,2],[55,3,56,3],[55,4,56,4],[55,9,56,9],[55,10,56,11],[55,12,56,12],[51,31,52,32],[53,1,54,2],[53,3,54,3],[53,4,54,4],[53,9,54,9],[53,10,54,11],[53,12,54,12],[53,31,54,32],[51,1,52,2],[51,3,52,3],[51,4,52,4],[51,9,52,9],[51,10,52,11],[51,12,52,12],[47,31,48,32],[49,1,50,2],[49,3,50,3],[49,4,50,4],[49,9,50,9],[49,10,50,11],[49,12,50,12],[49,31,50,32],[47,1,48,2],[47,3,48,3],[47,4,48,4],[47,9,48,9],[47,10,48,11],[47,12,48,12],[43,31,44,32],[45,1,46,2],[45,3,46,3],[45,4,46,4],[45,9,46,9],[45,10,46,11],[45,12,46,12],[45,31,46,32],[43,1,44,2],[43,3,44,3],[43,4,44,4],[43,9,44,9],[43,10,44,11],[43,12,44,12],[39,31,40,32],[41,1,42,2],[41,3,42,3],[41,4,42,4],[41,9,42,9],[41,10,42,11],[41,12,42,12],[41,31,42,32],[39,1,40,2],[39,3,40,3],[39,4,40,4],[39,9,40,9],[39,10,40,11],[39,12,40,12],[35,31,36,32],[37,1,38,2],[37,3,38,3],[37,4,38,4],[37,9,38,9],[37,10,38,11],[37,12,38,12],[37,31,38,32],[35,1,36,2],[35,3,36,3],[35,4,36,4],[35,9,36,9],[35,10,36,11],[35,12,36,12],[31,31,32,32],[33,1,34,2],[33,3,34,3],[33,4,34,4],[33,9,34,9],[33,10,34,11],[33,12,34,12],[33,31,34,32],[29,1,29,2],[29,10,29,11],[31,1,32,2],[31,3,32,3],[31,4,32,4],[31,9,32,9],[31,10,32,11],[31,12,32,12],[4,1,4,12],[5,1,5,12],[24,1,24,10],[24,11,24,12],[25,1,25,10],[25,11,25,12],[8,2,8,3],[9,2,9,3],[9,5,9,6],[9,7,9,9],[9,10,9,11],[10,2,10,3],[10,5,10,6],[10,7,10,9],[10,10,10,11],[6,1,7,1],[6,2,7,3],[6,4,7,4],[6,5,7,6],[6,7,7,9],[6,10,6,12],[7,10,7,11],[11,2,11,3],[11,5,11,6],[81,1,82,1],[81,2,82,3],[81,4,81,6],[81,7,81,9],[81,10,81,12],[82,10,82,11],[105,10,105,12],[149,10,149,11],[172,2,172,3],[172,10,172,11],[122,10,122,12],[105,2,105,3],[105,4,105,6],[105,7,105,9],[140,1,140,3],[140,10,140,11],[148,2,148,3],[148,10,148,11],[171,2,171,3],[171,10,171,11],[128,2,128,3],[128,10,128,11],[149,2,149,3],[162,1,162,11],[91,2,91,3],[91,10,91,11],[111,2,111,3],[111,4,111,6],[111,7,111,9],[111,10,111,12],[112,2,112,3],[112,4,112,6],[112,7,112,9],[109,2,109,3],[109,4,109,6],[109,7,109,9],[109,10,109,12],[110,2,110,3],[110,4,110,6],[110,7,110,9],[110,10,110,12],[92,2,92,3],[92,10,92,11],[112,10,112,12],[93,2,93,3],[93,10,93,11],[94,2,94,3],[94,10,94,11],[15,2,15,3],[15,5,15,6],[15,7,15,9],[15,10,15,11],[16,2,16,3],[16,5,16,6],[16,7,16,9],[16,10,16,11],[90,2,90,3],[90,10,90,11],[17,2,17,3],[17,5,17,6],[17,7,17,9],[17,10,17,11],[18,2,18,3],[18,5,18,6],[18,7,18,9],[18,10,18,11],[19,2,19,3],[19,5,19,6],[19,7,19,9],[19,10,19,11],[21,2,21,3],[21,5,21,6],[118,2,118,3],[118,4,118,6],[118,7,118,9],[118,10,118,12],[119,2,119,3],[114,2,114,3],[114,4,114,6],[114,7,114,9],[114,10,114,12],[119,4,119,6],[119,7,119,9],[119,10,119,12],[173,2,173,3],[173,10,173,11],[161,1,161,3],[161,10,161,11],[163,1,163,9],[163,10,163,12],[166,1,167,1],[166,2,167,3],[166,4,166,6],[156,2,156,3],[156,10,156,11],[158,2,158,3],[158,10,158,11],[159,2,159,3],[159,10,159,11],[160,2,160,3],[160,10,160,11],[152,2,152,3],[152,10,152,11],[155,2,155,3],[155,10,155,11],[179,2,179,3],[179,10,179,11],[200,2,200,3],[200,10,200,11],[20,2,20,3],[20,5,20,6],[20,7,20,9],[20,10,20,11],[95,2,95,3],[95,10,95,11],[116,2,116,3],[116,4,116,6],[116,7,116,9],[116,10,116,12],[136,2,136,3],[136,10,136,11],[157,2,157,3],[157,10,157,11],[180,2,180,3],[180,10,180,11],[154,2,154,3],[154,10,154,11],[177,2,177,3],[177,10,177,11],[21,7,21,9],[21,10,21,11],[22,2,22,3],[22,5,22,6],[22,7,22,9],[22,10,22,11],[23,2,23,3],[23,5,23,6],[23,7,23,9],[23,10,23,11],[96,2,96,3],[96,10,96,11],[97,2,97,3],[97,10,97,11],[98,2,98,3],[98,10,98,11],[117,2,117,3],[117,4,117,6],[117,7,117,9],[117,10,117,12],[113,2,113,3],[113,4,113,6],[113,7,113,9],[113,10,113,12],[115,2,115,3],[115,4,115,6],[115,7,115,9],[115,10,115,12],[137,2,137,3],[137,10,137,11],[138,2,138,3],[138,10,138,11],[139,2,139,3],[139,10,139,11],[132,2,132,3],[132,10,132,11],[134,2,134,3],[134,10,134,11],[133,2,133,3],[133,10,133,11],[204,2,204,3],[204,10,204,11],[181,2,181,3],[181,10,181,11],[182,2,182,3],[182,10,182,11],[183,2,183,3],[183,10,183,11],[202,2,202,3],[202,10,202,11],[203,2,203,3],[203,10,203,11],[201,2,201,3],[201,10,201,11],[199,2,199,3],[199,10,199,11]]}
["G"]
["G","Performance Rating Method Outputs"]
["G"]
["G"]
["G","Energy Sources"]
["G"]
["G","Energy Type","Energy Consumption Units",null,"Demand Units","Utility Rate Name",null,"Utility Rate Structure",null,null,"Unit Conversion Factors"]
["G",null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"Energy Type Consumption Units to Site Energy Consumption (\",PO_SiteUnits,\")\")","v":"Energy Type Consumption Units to Site Energy Consumption (Btu x 10^6)"},null,{"$f":"CONCATENATE(\"Energy Type Consumption Units to Source Energy Consumption (\",PO_SourceUnits,\")\")","v":"Energy Type Consumption Units to Source Energy Consumption (Btu x 10^6)"}]
["G","Energy_Type","Energy_Consumption_Units",null,"Demand_Units","Utility_Rate_Name",null,"Utility_Rate_Structure",null,null,"Site_Energy_Conversion_Factor",null,"Source_Energy_Conversion_Factor"]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B17<>\"\",'12 - Performance_Outputs_1'!B17,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C17<>\"\",'12 - Performance_Outputs_1'!C17,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D17<>\"\",'12 - Performance_Outputs_1'!D17,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E17<>\"\",'12 - Performance_Outputs_1'!E17,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H17<>\"\",'12 - Performance_Outputs_1'!H17,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I17<>\"\",'12 - Performance_Outputs_1'!I17,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F17<>\"\",'12 - Performance_Outputs_1'!F17,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G17<>\"\",'12 - Performance_Outputs_1'!G17,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J17<>\"\",'12 - Performance_Outputs_1'!J17,\"\"),\"\")","v":""},{"$f":"IFERROR(VLOOKUP(\"kBtu\",EnergyUnitsTable,3,FALSE)/VLOOKUP(PO_SiteUnits,EnergyUnitsTable,3,FALSE)*VLOOKUP($C10,EnergyUnitsTable,3,FALSE),\"\")","v":""},null,{"$f":"IFERROR(VLOOKUP(\"kBtu\",EnergyUnitsTable,3,FALSE)/VLOOKUP(PO_SourceUnits,EnergyUnitsTable,3,FALSE)*VLOOKUP($C10,EnergyUnitsTable,3,FALSE)*VLOOKUP($B10,FuelTypesTable,2,FALSE),\"\")","v":""}]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B18<>\"\",'12 - Performance_Outputs_1'!B18,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C18<>\"\",'12 - Performance_Outputs_1'!C18,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D18<>\"\",'12 - Performance_Outputs_1'!D18,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E18<>\"\",'12 - Performance_Outputs_1'!E18,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H18<>\"\",'12 - Performance_Outputs_1'!H18,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I18<>\"\",'12 - Performance_Outputs_1'!I18,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F18<>\"\",'12 - Performance_Outputs_1'!F18,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G18<>\"\",'12 - Performance_Outputs_1'!G18,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J18<>\"\",'12 - Performance_Outputs_1'!J18,\"\"),\"\")","v":""},"",null,""]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B19<>\"\",'12 - Performance_Outputs_1'!B19,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C19<>\"\",'12 - Performance_Outputs_1'!C19,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D19<>\"\",'12 - Performance_Outputs_1'!D19,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E19<>\"\",'12 - Performance_Outputs_1'!E19,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H19<>\"\",'12 - Performance_Outputs_1'!H19,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I19<>\"\",'12 - Performance_Outputs_1'!I19,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F19<>\"\",'12 - Performance_Outputs_1'!F19,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G19<>\"\",'12 - Performance_Outputs_1'!G19,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J19<>\"\",'12 - Performance_Outputs_1'!J19,\"\"),\"\")","v":""},"",null,""]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B23<>\"\",'12 - Performance_Outputs_1'!B23,\"\"),\"\")","v":"Site energy consumption units used to report energy consumption totals (sum of energy types)"},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C23<>\"\",'12 - Performance_Outputs_1'!C23,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D23<>\"\",'12 - Performance_Outputs_1'!D23,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E23<>\"\",'12 - Performance_Outputs_1'!E23,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F23<>\"\",'12 - Performance_Outputs_1'!F23,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G23<>\"\",'12 - Performance_Outputs_1'!G23,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H23<>\"\",'12 - Performance_Outputs_1'!H23,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I23<>\"\",'12 - Performance_Outputs_1'!I23,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J23<>\"\",'12 - Performance_Outputs_1'!J23,\"\"),\"\")","v":""},"",null,""]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B24<>\"\",'12 - Performance_Outputs_1'!B24,\"\"),\"\")","v":"Source energy consumption units used to report energy consumption totals (sum of energy types)"},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C24<>\"\",'12 - Performance_Outputs_1'!C24,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D24<>\"\",'12 - Performance_Outputs_1'!D24,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E24<>\"\",'12 - Performance_Outputs_1'!E24,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F24<>\"\",'12 - Performance_Outputs_1'!F24,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G24<>\"\",'12 - Performance_Outputs_1'!G24,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H24<>\"\",'12 - Performance_Outputs_1'!H24,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I24<>\"\",'12 - Performance_Outputs_1'!I24,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J24<>\"\",'12 - Performance_Outputs_1'!J24,\"\"),\"\")","v":""},"",null,""]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B25<>\"\",'12 - Performance_Outputs_1'!B25,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C25<>\"\",'12 - Performance_Outputs_1'!C25,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D25<>\"\",'12 - Performance_Outputs_1'!D25,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E25<>\"\",'12 - Performance_Outputs_1'!E25,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F25<>\"\",'12 - Performance_Outputs_1'!F25,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G25<>\"\",'12 - Performance_Outputs_1'!G25,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H25<>\"\",'12 - Performance_Outputs_1'!H25,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I25<>\"\",'12 - Performance_Outputs_1'!I25,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J25<>\"\",'12 - Performance_Outputs_1'!J25,\"\"),\"\")","v":""},"",null,""]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B26<>\"\",'12 - Performance_Outputs_1'!B26,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C26<>\"\",'12 - Performance_Outputs_1'!C26,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D26<>\"\",'12 - Performance_Outputs_1'!D26,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E26<>\"\",'12 - Performance_Outputs_1'!E26,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F26<>\"\",'12 - Performance_Outputs_1'!F26,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G26<>\"\",'12 - Performance_Outputs_1'!G26,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H26<>\"\",'12 - Performance_Outputs_1'!H26,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I26<>\"\",'12 - Performance_Outputs_1'!I26,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J26<>\"\",'12 - Performance_Outputs_1'!J26,\"\"),\"\")","v":""},"",null,""]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B27<>\"\",'12 - Performance_Outputs_1'!B27,\"\"),\"\")","v":"Table 12.2: On-Site Renewable Energy Production"},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C27<>\"\",'12 - Performance_Outputs_1'!C27,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D27<>\"\",'12 - Performance_Outputs_1'!D27,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E27<>\"\",'12 - Performance_Outputs_1'!E27,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F27<>\"\",'12 - Performance_Outputs_1'!F27,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G27<>\"\",'12 - Performance_Outputs_1'!G27,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H27<>\"\",'12 - Performance_Outputs_1'!H27,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I27<>\"\",'12 - Performance_Outputs_1'!I27,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J27<>\"\",'12 - Performance_Outputs_1'!J27,\"\"),\"\")","v":""},"",null,""]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B28<>\"\",'12 - Performance_Outputs_1'!B28,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C28<>\"\",'12 - Performance_Outputs_1'!C28,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D28<>\"\",'12 - Performance_Outputs_1'!D28,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E28<>\"\",'12 - Performance_Outputs_1'!E28,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F28<>\"\",'12 - Performance_Outputs_1'!F28,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G28<>\"\",'12 - Performance_Outputs_1'!G28,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H28<>\"\",'12 - Performance_Outputs_1'!H28,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I28<>\"\",'12 - Performance_Outputs_1'!I28,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J28<>\"\",'12 - Performance_Outputs_1'!J28,\"\"),\"\")","v":""},"",null,""]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B29<>\"\",'12 - Performance_Outputs_1'!B29,\"\"),\"\")","v":"The project building uses on-site renewable energy systems. (Optional)"},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C29<>\"\",'12 - Performance_Outputs_1'!C29,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D29<>\"\",'12 - Performance_Outputs_1'!D29,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E29<>\"\",'12 - Performance_Outputs_1'!E29,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F29<>\"\",'12 - Performance_Outputs_1'!F29,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G29<>\"\",'12 - Performance_Outputs_1'!G29,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H29<>\"\",'12 - Performance_Outputs_1'!H29,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I29<>\"\",'12 - Performance_Outputs_1'!I29,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J29<>\"\",'12 - Performance_Outputs_1'!J29,\"\"),\"\")","v":""},"",null,""]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B30<>\"\",'12 - Performance_Outputs_1'!B30,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C30<>\"\",'12 - Performance_Outputs_1'!C30,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D30<>\"\",'12 - Performance_Outputs_1'!D30,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E30<>\"\",'12 - Performance_Outputs_1'!E30,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F30<>\"\",'12 - Performance_Outputs_1'!F30,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G30<>\"\",'12 - Performance_Outputs_1'!G30,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H30<>\"\",'12 - Performance_Outputs_1'!H30,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I30<>\"\",'12 - Performance_Outputs_1'!I30,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J30<>\"\",'12 - Performance_Outputs_1'!J30,\"\"),\"\")","v":""},"",null,""]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B31<>\"\",'12 - Performance_Outputs_1'!B31,\"\"),\"\")","v":"Table: On-Site Renewable energy source summary"},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C31<>\"\",'12 - Performance_Outputs_1'!C31,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D31<>\"\",'12 - Performance_Outputs_1'!D31,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E31<>\"\",'12 - Performance_Outputs_1'!E31,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F31<>\"\",'12 - Performance_Outputs_1'!F31,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G31<>\"\",'12 - Performance_Outputs_1'!G31,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H31<>\"\",'12 - Performance_Outputs_1'!H31,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I31<>\"\",'12 - Performance_Outputs_1'!I31,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J31<>\"\",'12 - Performance_Outputs_1'!J31,\"\"),\"\")","v":""},"",null,""]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B32<>\"\",'12 - Performance_Outputs_1'!B32,\"\"),\"\")","v":"Renewable energy production should be reported in the table below. Note: This calculator will automatically reduce the proposed energy consumption and cost to accurately reflect the revised results. Therefore, any site-generated renewable energy production should NOT be included in the Performance Rating Method tables below.\n\nSelect the site-generated renewable energy source. Enter the rated capacity of the site-generated renewable source including the units (e.g. for photovoltaics 10 kW). Include all relevant capacities (i.e for solar thermal, both the storage tank capacity and the solar thermal panel capacity).\n\nThe cost of the Site-generated renewable cost will be automatically determined using the virtual rate once the output data (consumption and cost) is entered below. The cost may be overridden by the user, however this may generate an issue on the Quality Checks and the user should be prepared to justify the entered cost value."},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C32<>\"\",'12 - Performance_Outputs_1'!C32,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D32<>\"\",'12 - Performance_Outputs_1'!D32,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E32<>\"\",'12 - Performance_Outputs_1'!E32,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F32<>\"\",'12 - Performance_Outputs_1'!F32,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G32<>\"\",'12 - Performance_Outputs_1'!G32,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H32<>\"\",'12 - Performance_Outputs_1'!H32,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I32<>\"\",'12 - Performance_Outputs_1'!I32,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J32<>\"\",'12 - Performance_Outputs_1'!J32,\"\"),\"\")","v":""},"",null,""]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B33<>\"\",'12 - Performance_Outputs_1'!B33,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C33<>\"\",'12 - Performance_Outputs_1'!C33,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D33<>\"\",'12 - Performance_Outputs_1'!D33,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E33<>\"\",'12 - Performance_Outputs_1'!E33,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F33<>\"\",'12 - Performance_Outputs_1'!F33,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G33<>\"\",'12 - Performance_Outputs_1'!G33,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H33<>\"\",'12 - Performance_Outputs_1'!H33,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I33<>\"\",'12 - Performance_Outputs_1'!I33,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J33<>\"\",'12 - Performance_Outputs_1'!J33,\"\"),\"\")","v":""},"",null,""]
["G",{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!B34<>\"\",'12 - Performance_Outputs_1'!B34,\"\"),\"\")","v":"On-Site Renewable Source"},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!C34<>\"\",'12 - Performance_Outputs_1'!C34,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!D34<>\"\",'12 - Performance_Outputs_1'!D34,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!E34<>\"\",'12 - Performance_Outputs_1'!E34,\"\"),\"\")","v":"Offset \nEnergy Type"},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!F34<>\"\",'12 - Performance_Outputs_1'!F34,\"\"),\"\")","v":"Rated Capacity "},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!G34<>\"\",'12 - Performance_Outputs_1'!G34,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!H34<>\"\",'12 - Performance_Outputs_1'!H34,\"\"),\"\")","v":"Annual Site Energy Generated"},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!I34<>\"\",'12 - Performance_Outputs_1'!I34,\"\"),\"\")","v":""},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!J34<>\"\",'12 - Performance_Outputs_1'!J34,\"\"),\"\")","v":"Annual Energy Cost Offset with \nSite-Generated Renewables \n($/year)"},"",null,""]
["G","Site energy consumption units used to report energy consumption totals (sum of energy types)",null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!L23<>\"\",'12 - Performance_Outputs_1'!L23,\"\"),\"\")","v":"Btu x 10^6"},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!M23<>\"\",'12 - Performance_Outputs_1'!M23,\"\"),\"\")","v":""}]
["G","Source energy consumption units used to report energy consumption totals (sum of energy types)",null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!L24<>\"\",'12 - Performance_Outputs_1'!L24,\"\"),\"\")","v":"Btu x 10^6"},{"$f":"IFERROR(IF('12 - Performance_Outputs_1'!M24<>\"\",'12 - Performance_Outputs_1'!M24,\"\"),\"\")","v":""}]
["G"]
["G","Table: Proposed energy summary by end use"]
["G"]
["G","End Use",null,"Unregulated?","Energy Type","Units of \nAnnual Energy and Peak Demand","Baseline","Proposed","Energy / Demand Savings \nper End-Use","End Use \nPercent Contribution to Total Energy Savings","End Use \nPercent \nContribution to \nTotal Cost Savings",null,"Percent of Total Proposed  \nSite Energy Consumption",null,null,null,null,null,null,null,null,null,"contribution rank",null,"Rank with ties","rank no ties",null,null,null,null,null,null,"QC_EFLH"]
["G","End_Use",null,"Unregulated","Energy_Type","Energy_Units","Base_Consumption_Demand","Design_Consumption_Demand","End_Use_Savings","End_Use_Contribution_to_Energy_Savings","End_Use_Contribution_to_Cost_Savings",null,"Percent_Design_Site_Consumption",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion",null,null,null,null,"contribution rank",null,"Rank with ties","rank no ties"]
["G","Interior lighting",null,0,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E32),\"\",\"Consumption (\" & VLOOKUP($E32,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,{"$f":"IFERROR(1-H32/G32,\"\")","v":""},{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G32-$H32)*VLOOKUP($E32,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G32*VLOOKUP($E32,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H32*VLOOKUP($E32,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H32*VLOOKUP($E32,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($E32),\"\",VLOOKUP($E32,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($E32),\"\",VLOOKUP($E32,PO_Enrgy_1_Table,MATCH($M$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},null,null,null,{"$f":"IFERROR($AN32*H32,0)","v":0},{"$f":"IFERROR(G32*VLOOKUP($AE32,PO_Enrgy_8_Table,4,FALSE),0)","v":0},{"$f":"IFERROR(H32*VLOOKUP($AE32,PO_Enrgy_8_Table,7,FALSE),0)","v":0},{"$f":"IFERROR(IF(D32=\"x\",IF(OR(G32/H32>1.03,G32/H32<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J32*100,)","v":0},null,{"$f":"RANK(Z32,$Z$32:$Z$79,0)","v":1},{"$f":"AB32","v":1},{"$f":"B32","v":"Interior lighting"},null,{"$f":"IFERROR(G32/'6b - General Lighting'!#REF!,\"\")","v":""}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E32),\"\",\"Demand (\" & VLOOKUP($E32,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,{"$f":"IFERROR(1-H33/G33,\"\")","v":""},null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Lighting in Apartments",null,0,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E34),\"\",\"Consumption (\" & VLOOKUP($E34,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G34-$H34)*VLOOKUP($E34,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G34*VLOOKUP($E34,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H34*VLOOKUP($E34,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H34*VLOOKUP($E34,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D34=\"x\",IF(OR(G34/H34>1.03,G34/H34<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J34*100,)","v":0},null,{"$f":"RANK(Z34,$Z$32:$Z$79,0)","v":1},{"$f":"AB34+COUNTIF($AB$32:$AB33,AB34)","v":2},{"$f":"B34","v":"Lighting in Apartments"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E34),\"\",\"Demand (\" & VLOOKUP($E34,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Exterior lighting",null,0,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E36),\"\",\"Consumption (\" & VLOOKUP($E36,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G36-$H36)*VLOOKUP($E36,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G36*VLOOKUP($E36,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H36*VLOOKUP($E36,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H36*VLOOKUP($E36,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D36=\"x\",IF(OR(G36/H36>1.03,G36/H36<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J36*100,)","v":0},null,{"$f":"RANK(Z36,$Z$32:$Z$79,0)","v":1},{"$f":"AB36+COUNTIF($AB$32:$AB35,AB36)","v":3},{"$f":"B36","v":"Exterior lighting"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E36),\"\",\"Demand (\" & VLOOKUP($E36,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Space heating",null,0,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E38),\"\",\"Consumption (\" & VLOOKUP($E38,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G38-$H38)*VLOOKUP($E38,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G38*VLOOKUP($E38,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H38*VLOOKUP($E38,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H38*VLOOKUP($E38,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D38=\"x\",IF(OR(G38/H38>1.03,G38/H38<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J38*100,)","v":0},null,{"$f":"RANK(Z38,$Z$32:$Z$79,0)","v":1},{"$f":"AB38+COUNTIF($AB$32:$AB37,AB38)","v":4},{"$f":"B38","v":"Space heating"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E38),\"\",\"Demand (\" & VLOOKUP($E38,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Space cooling",null,0,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E40),\"\",\"Consumption (\" & VLOOKUP($E40,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G40-$H40)*VLOOKUP($E40,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G40*VLOOKUP($E40,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H40*VLOOKUP($E40,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H40*VLOOKUP($E40,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D40=\"x\",IF(OR(G40/H40>1.03,G40/H40<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J40*100,)","v":0},null,{"$f":"RANK(Z40,$Z$32:$Z$79,0)","v":1},{"$f":"AB40+COUNTIF($AB$32:$AB39,AB40)","v":5},{"$f":"B40","v":"Space cooling"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E40),\"\",\"Demand (\" & VLOOKUP($E40,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Pumps",null,0,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E42),\"\",\"Consumption (\" & VLOOKUP($E42,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G42-$H42)*VLOOKUP($E42,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G42*VLOOKUP($E42,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H42*VLOOKUP($E42,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H42*VLOOKUP($E42,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D42=\"x\",IF(OR(G42/H42>1.03,G42/H42<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J42*100,)","v":0},null,{"$f":"RANK(Z42,$Z$32:$Z$79,0)","v":1},{"$f":"AB42+COUNTIF($AB$32:$AB41,AB42)","v":6},{"$f":"B42","v":"Pumps"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E42),\"\",\"Demand (\" & VLOOKUP($E42,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Heat rejection",null,0,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E44),\"\",\"Consumption (\" & VLOOKUP($E44,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G44-$H44)*VLOOKUP($E44,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G44*VLOOKUP($E44,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H44*VLOOKUP($E44,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H44*VLOOKUP($E44,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D44=\"x\",IF(OR(G44/H44>1.03,G44/H44<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J44*100,)","v":0},null,{"$f":"RANK(Z44,$Z$32:$Z$79,0)","v":1},{"$f":"AB44+COUNTIF($AB$32:$AB43,AB44)","v":7},{"$f":"B44","v":"Heat rejection"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E44),\"\",\"Demand (\" & VLOOKUP($E44,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Fans - interior ventilation",null,0,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E46),\"\",\"Consumption (\" & VLOOKUP($E46,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G46-$H46)*VLOOKUP($E46,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G46*VLOOKUP($E46,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H46*VLOOKUP($E46,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H46*VLOOKUP($E46,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D46=\"x\",IF(OR(G46/H46>1.03,G46/H46<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J46*100,)","v":0},null,{"$f":"RANK(Z46,$Z$32:$Z$79,0)","v":1},{"$f":"AB46+COUNTIF($AB$32:$AB45,AB46)","v":8},{"$f":"B46","v":"Fans - interior ventilation"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E46),\"\",\"Demand (\" & VLOOKUP($E46,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Fans - parking garage",null,0,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E48),\"\",\"Consumption (\" & VLOOKUP($E48,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G48-$H48)*VLOOKUP($E48,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G48*VLOOKUP($E48,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H48*VLOOKUP($E48,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H48*VLOOKUP($E48,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D48=\"x\",IF(OR(G48/H48>1.03,G48/H48<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J48*100,)","v":0},null,{"$f":"RANK(Z48,$Z$32:$Z$79,0)","v":1},{"$f":"AB48+COUNTIF($AB$32:$AB47,AB48)","v":9},{"$f":"B48","v":"Fans - parking garage"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E48),\"\",\"Demand (\" & VLOOKUP($E48,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Service water heating",null,0,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E50),\"\",\"Consumption (\" & VLOOKUP($E50,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G50-$H50)*VLOOKUP($E50,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G50*VLOOKUP($E50,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H50*VLOOKUP($E50,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H50*VLOOKUP($E50,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D50=\"x\",IF(OR(G50/H50>1.03,G50/H50<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J50*100,)","v":0},null,{"$f":"RANK(Z50,$Z$32:$Z$79,0)","v":1},{"$f":"AB50+COUNTIF($AB$32:$AB49,AB50)","v":10},{"$f":"B50","v":"Service water heating"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E50),\"\",\"Demand (\" & VLOOKUP($E50,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Receptacle equipment",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E52),\"\",\"Consumption (\" & VLOOKUP($E52,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G52-$H52)*VLOOKUP($E52,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G52*VLOOKUP($E52,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H52*VLOOKUP($E52,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H52*VLOOKUP($E52,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D52=\"x\",IF(OR(G52/H52>1.03,G52/H52<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J52*100,)","v":0},null,{"$f":"RANK(Z52,$Z$32:$Z$79,0)","v":1},{"$f":"AB52+COUNTIF($AB$32:$AB51,AB52)","v":11},{"$f":"B52","v":"Receptacle equipment"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E52),\"\",\"Demand (\" & VLOOKUP($E52,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","IT equipment",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E54),\"\",\"Consumption (\" & VLOOKUP($E54,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G54-$H54)*VLOOKUP($E54,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G54*VLOOKUP($E54,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H54*VLOOKUP($E54,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H54*VLOOKUP($E54,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D54=\"x\",IF(OR(G54/H54>1.03,G54/H54<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J54*100,)","v":0},null,{"$f":"RANK(Z54,$Z$32:$Z$79,0)","v":1},{"$f":"AB54+COUNTIF($AB$32:$AB53,AB54)","v":12},{"$f":"B54","v":"IT equipment"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E54),\"\",\"Demand (\" & VLOOKUP($E54,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Interior lighting - process",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E56),\"\",\"Consumption (\" & VLOOKUP($E56,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G56-$H56)*VLOOKUP($E56,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G56*VLOOKUP($E56,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H56*VLOOKUP($E56,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H56*VLOOKUP($E56,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D56=\"x\",IF(OR(G56/H56>1.03,G56/H56<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J56*100,)","v":0},null,{"$f":"RANK(Z56,$Z$32:$Z$79,0)","v":1},{"$f":"AB56+COUNTIF($AB$32:$AB55,AB56)","v":13},{"$f":"B56","v":"Interior lighting - process"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E56),\"\",\"Demand (\" & VLOOKUP($E56,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Refrigeration equipment",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E58),\"\",\"Consumption (\" & VLOOKUP($E58,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G58-$H58)*VLOOKUP($E58,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G58*VLOOKUP($E58,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H58*VLOOKUP($E58,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H58*VLOOKUP($E58,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D58=\"x\",IF(OR(G58/H58>1.03,G58/H58<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J58*100,)","v":0},null,{"$f":"RANK(Z58,$Z$32:$Z$79,0)","v":1},{"$f":"AB58+COUNTIF($AB$32:$AB57,AB58)","v":14},{"$f":"B58","v":"Refrigeration equipment"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E58),\"\",\"Demand (\" & VLOOKUP($E58,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Fans - Kitchen Ventilation",null,0,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E60),\"\",\"Consumption (\" & VLOOKUP($E60,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G60-$H60)*VLOOKUP($E60,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G60*VLOOKUP($E60,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H60*VLOOKUP($E60,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H60*VLOOKUP($E60,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D60=\"x\",IF(OR(G60/H60>1.03,G60/H60<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J60*100,)","v":0},null,{"$f":"RANK(Z60,$Z$32:$Z$79,0)","v":1},{"$f":"AB60+COUNTIF($AB$32:$AB59,AB60)","v":15},{"$f":"B60","v":"Fans - Kitchen Ventilation"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E60),\"\",\"Demand (\" & VLOOKUP($E60,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Cooking",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E62),\"\",\"Consumption (\" & VLOOKUP($E62,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G62-$H62)*VLOOKUP($E62,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G62*VLOOKUP($E62,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H62*VLOOKUP($E62,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H62*VLOOKUP($E62,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D62=\"x\",IF(OR(G62/H62>1.03,G62/H62<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J62*100,)","v":0},null,{"$f":"RANK(Z62,$Z$32:$Z$79,0)","v":1},{"$f":"AB62+COUNTIF($AB$32:$AB61,AB62)","v":16},{"$f":"B62","v":"Cooking"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E62),\"\",\"Demand (\" & VLOOKUP($E62,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Industrial Process",null,"x","Electricity",{"$f":"IFERROR(IF(ISBLANK(E64),\"\",\"Consumption (\" & VLOOKUP($E64,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G64-$H64)*VLOOKUP($E64,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G64*VLOOKUP($E64,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H64*VLOOKUP($E64,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H64*VLOOKUP($E64,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D64=\"x\",IF(OR(G64/H64>1.03,G64/H64<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J64*100,)","v":0},null,{"$f":"RANK(Z64,$Z$32:$Z$79,0)","v":1},{"$f":"AB64+COUNTIF($AB$32:$AB63,AB64)","v":17},{"$f":"B64","v":"Industrial Process"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E64),\"\",\"Demand (\" & VLOOKUP($E64,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Elevators and escalators",null,0,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E66),\"\",\"Consumption (\" & VLOOKUP($E66,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G66-$H66)*VLOOKUP($E66,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G66*VLOOKUP($E66,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H66*VLOOKUP($E66,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H66*VLOOKUP($E66,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D66=\"x\",IF(OR(G66/H66>1.03,G66/H66<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J66*100,)","v":0},null,{"$f":"RANK(Z66,$Z$32:$Z$79,0)","v":1},{"$f":"AB66+COUNTIF($AB$32:$AB65,AB66)","v":18},{"$f":"B66","v":"Elevators and escalators"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E66),\"\",\"Demand (\" & VLOOKUP($E66,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Heat Pump Supplementary",null,0,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E68),\"\",\"Consumption (\" & VLOOKUP($E68,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G68-$H68)*VLOOKUP($E68,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G68*VLOOKUP($E68,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H68*VLOOKUP($E68,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H68*VLOOKUP($E68,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D68=\"x\",IF(OR(G68/H68>1.03,G68/H68<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J68*100,)","v":0},null,{"$f":"RANK(Z68,$Z$32:$Z$79,0)","v":1},{"$f":"AB68+COUNTIF($AB$32:$AB67,AB68)","v":19},{"$f":"B68","v":"Heat Pump Supplementary"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E68),\"\",\"Demand (\" & VLOOKUP($E68,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Space Heating",null,0,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E70),\"\",\"Consumption (\" & VLOOKUP($E70,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G70-$H70)*VLOOKUP($E70,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G70*VLOOKUP($E70,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H70*VLOOKUP($E70,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H70*VLOOKUP($E70,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D70=\"x\",IF(OR(G70/H70>1.03,G70/H70<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J70*100,)","v":0},null,{"$f":"RANK(Z70,$Z$32:$Z$79,0)","v":1},{"$f":"AB70+COUNTIF($AB$32:$AB69,AB70)","v":20},{"$f":"B70","v":"Space Heating"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E70),\"\",\"Demand (\" & VLOOKUP($E70,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Misc Equipment (Gas)",null,0,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E72),\"\",\"Consumption (\" & VLOOKUP($E72,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G72-$H72)*VLOOKUP($E72,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G72*VLOOKUP($E72,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H72*VLOOKUP($E72,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H72*VLOOKUP($E72,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D72=\"x\",IF(OR(G72/H72>1.03,G72/H72<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J72*100,)","v":0},null,{"$f":"RANK(Z72,$Z$32:$Z$79,0)","v":1},{"$f":"AB72+COUNTIF($AB$32:$AB71,AB72)","v":21},{"$f":"B72","v":"Misc Equipment (Gas)"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E72),\"\",\"Demand (\" & VLOOKUP($E72,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Auxiliary (Gas)",null,0,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E74),\"\",\"Consumption (\" & VLOOKUP($E74,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G74-$H74)*VLOOKUP($E74,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G74*VLOOKUP($E74,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H74*VLOOKUP($E74,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H74*VLOOKUP($E74,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D74=\"x\",IF(OR(G74/H74>1.03,G74/H74<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J74*100,)","v":0},null,{"$f":"RANK(Z74,$Z$32:$Z$79,0)","v":1},{"$f":"AB74+COUNTIF($AB$32:$AB73,AB74)","v":22},{"$f":"B74","v":"Auxiliary (Gas)"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E74),\"\",\"Demand (\" & VLOOKUP($E74,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Cooling (Gas)",null,0,"Natural Gas",{"$f":"IFERROR(IF(ISBLANK(E76),\"\",\"Consumption (\" & VLOOKUP($E76,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G76-$H76)*VLOOKUP($E76,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G76*VLOOKUP($E76,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H76*VLOOKUP($E76,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H76*VLOOKUP($E76,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D76=\"x\",IF(OR(G76/H76>1.03,G76/H76<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J76*100,)","v":0},null,{"$f":"RANK(Z76,$Z$32:$Z$79,0)","v":1},{"$f":"AB76+COUNTIF($AB$32:$AB75,AB76)","v":23},{"$f":"B76","v":"Cooling (Gas)"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E76),\"\",\"Demand (\" & VLOOKUP($E76,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G","Refrigeration Equipment (Regulated)",null,0,"Electricity",{"$f":"IFERROR(IF(ISBLANK(E78),\"\",\"Consumption (\" & VLOOKUP($E78,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",{"$f":"IFERROR(IF($E$206-$H$206<0,\"\",($G78-$H78)*VLOOKUP($E78,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)/($E$206-$H$206)),\"\")","v":""},{"$f":"IFERROR(IF($G$206-$J$206<0,\"\",($G78*VLOOKUP($E78,PO_Enrgy_8_Table,MATCH($E$105,PO_Enrgy_8_Hdr,0),FALSE)-($H78*VLOOKUP($E78,PO_Enrgy_8_Table,MATCH($H$105,PO_Enrgy_8_Hdr,0),FALSE)))/($G$206-$J$206)),\"\")","v":""},null,{"$f":"IFERROR(H78*VLOOKUP($E78,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0))/$H$100,\"\")","v":""},null,null,null,"","",null,null,null,0,0,0,{"$f":"IFERROR(IF(D78=\"x\",IF(OR(G78/H78>1.03,G78/H78<0.97),TRUE,FALSE),FALSE),FALSE)","v":false},{"$f":"IFERROR(J78*100,)","v":0},null,{"$f":"RANK(Z78,$Z$32:$Z$79,0)","v":1},{"$f":"AB78+COUNTIF($AB$32:$AB77,AB78)","v":24},{"$f":"B78","v":"Refrigeration Equipment (Regulated)"}]
["G",null,null,null,null,{"$f":"IFERROR(IF(ISBLANK(E78),\"\",\"Demand (\" & VLOOKUP($E78,PO_Enrgy_1_Table,MATCH($E$9,PO_Enrgy_1_Hdr,0),FALSE) & \")\"),\"\")","v":""},0,0,"",null,null,null,null,null,null,null,"","",null,null,null,0,0,0]
["G"]
["G","Table: Performance rating energy consumption and cost by fuel type",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Notes (Optional):"]
["G","Energy Type","Site Energy Units",null,"Baseline",null,null,"Proposed",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site_Energy",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B10),\"\",B10),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B85),\"\",VLOOKUP($B85,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C85=\"\",\"\",VLOOKUP(C85,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H85/E85,\"\")","v":""},null,{"$f":"IFERROR(1-J85/G85,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B85),\"\",VLOOKUP($B85,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B85),\"\",VLOOKUP($B85,PO_Enrgy_1_Table,MATCH($M$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C86=\"\",\"\",VLOOKUP(C86,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C87=\"\",\"\",VLOOKUP(C87,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","Site energy consumption units used to report energy consumption totals (sum of energy types)","",{"$f":"IF(C88=\"\",\"\",VLOOKUP(C88,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","Source energy consumption units used to report energy consumption totals (sum of energy types)","",{"$f":"IF(C89=\"\",\"\",VLOOKUP(C89,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C90=\"\",\"\",VLOOKUP(C90,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H90/E90,\"\")","v":""},null,{"$f":"IFERROR(1-J90/G90,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C91=\"\",\"\",VLOOKUP(C91,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H91/E91,\"\")","v":""},null,{"$f":"IFERROR(1-J91/G91,\"\")","v":""},null,null,null,"",""]
["G","Table 12.2: On-Site Renewable Energy Production","",{"$f":"IF(C92=\"\",\"\",VLOOKUP(C92,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C93=\"\",\"\",VLOOKUP(C93,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H93/E93,\"\")","v":""},null,{"$f":"IFERROR(1-J93/G93,\"\")","v":""},null,null,null,"",""]
["G","The project building uses on-site renewable energy systems. (Optional)","",{"$f":"IF(C94=\"\",\"\",VLOOKUP(C94,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H94/E94,\"\")","v":""},null,{"$f":"IFERROR(1-J94/G94,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C95=\"\",\"\",VLOOKUP(C95,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H95/E95,\"\")","v":""},null,{"$f":"IFERROR(1-J95/G95,\"\")","v":""},null,null,null,"",""]
["G","Table: On-Site Renewable energy source summary","",{"$f":"IF(C96=\"\",\"\",VLOOKUP(C96,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H96/E96,\"\")","v":""},null,{"$f":"IFERROR(1-J96/G96,\"\")","v":""},null,null,null,"",""]
["G",{"$f":"IFERROR(IF(ISBLANK(B22),\"\",B22),\"\")","v":"Renewable energy production should be reported in the table below. Note: This calculator will automatically reduce the proposed energy consumption and cost to accurately reflect the revised results. Therefore, any site-generated renewable energy production should NOT be included in the Performance Rating Method tables below.\n\nSelect the site-generated renewable energy source. Enter the rated capacity of the site-generated renewable source including the units (e.g. for photovoltaics 10 kW). Include all relevant capacities (i.e for solar thermal, both the storage tank capacity and the solar thermal panel capacity).\n\nThe cost of the Site-generated renewable cost will be automatically determined using the virtual rate once the output data (consumption and cost) is entered below. The cost may be overridden by the user, however this may generate an issue on the Quality Checks and the user should be prepared to justify the entered cost value."},"",{"$f":"IF(C97=\"\",\"\",VLOOKUP(C97,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H97/E97,\"\")","v":""},null,{"$f":"IFERROR(1-J97/G97,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C98=\"\",\"\",VLOOKUP(C98,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","On-Site Renewable Source","",{"$f":"IF(C99=\"\",\"\",VLOOKUP(C99,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_7_Table,0,MATCH(E$84,PO_Enrgy_7_Hdr,0)),INDEX(PO_Enrgy_7_Table,0,MATCH($Q$84,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(F$84,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(G$84,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_7_Table,0,MATCH(H$84,PO_Enrgy_7_Hdr,0)),INDEX(PO_Enrgy_7_Table,0,MATCH($Q$84,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(I$84,PO_Enrgy_7_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_7_Table,0,MATCH(J$84,PO_Enrgy_7_Hdr,0))),\"\")","v":0},"",null,""]
["G"]
["G"]
["G","Table: Virtual rate (average energy cost per unit energy)"]
["G","Energy Type",null,null,"Baseline",null,null,"Proposed",null,null,"Percent Variance"]
["G","Energy_Type","Units",null,"Base_Virtual_Rate",null,null,"Design_Virtual_Rate",null,null,"Percent_Variance",null,null,null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B10),\"\",B10),\"\")","v":""},{"$f":"IFERROR(CONCATENATE(\"$ / \",VLOOKUP($B106,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":"$ / "},{"$f":"IF(C106=\"\",\"\",VLOOKUP(C106,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B106=\"District Cooling\",$B106=\"District Steam\",$B106=\"District Hot Water\")),IF($B106=\"District Cooling\",#REF!,#REF!),VLOOKUP($B106,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B106,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B106=\"District Cooling\",$B106=\"District Steam\",$B106=\"District Hot Water\")),IF($B106=\"District Cooling\",#REF!,#REF!),VLOOKUP($B106,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B106,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(ABS(1-H106/E106),\"\")","v":""},null,null,null,null,null,{"$f":"IFERROR(IF(ISBLANK($B106),\"\",VLOOKUP($B106,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B106),\"\",VLOOKUP($B106,PO_Enrgy_1_Table,MATCH($M$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","$ / ",{"$f":"IF(C107=\"\",\"\",VLOOKUP(C107,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B107=\"District Cooling\",$B107=\"District Steam\",$B107=\"District Hot Water\")),IF($B107=\"District Cooling\",#REF!,#REF!),VLOOKUP($B107,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B107,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B107=\"District Cooling\",$B107=\"District Steam\",$B107=\"District Hot Water\")),IF($B107=\"District Cooling\",#REF!,#REF!),VLOOKUP($B107,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B107,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,"",null,null,null,null,null,"",""]
["G","","$ / ",{"$f":"IF(C108=\"\",\"\",VLOOKUP(C108,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B108=\"District Cooling\",$B108=\"District Steam\",$B108=\"District Hot Water\")),IF($B108=\"District Cooling\",#REF!,#REF!),VLOOKUP($B108,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B108,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B108=\"District Cooling\",$B108=\"District Steam\",$B108=\"District Hot Water\")),IF($B108=\"District Cooling\",#REF!,#REF!),VLOOKUP($B108,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B108,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,"",null,null,null,null,null,"",""]
["G","Site energy consumption units used to report energy consumption totals (sum of energy types)","$ / ",{"$f":"IF(C109=\"\",\"\",VLOOKUP(C109,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B109=\"District Cooling\",$B109=\"District Steam\",$B109=\"District Hot Water\")),IF($B109=\"District Cooling\",#REF!,#REF!),VLOOKUP($B109,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B109,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B109=\"District Cooling\",$B109=\"District Steam\",$B109=\"District Hot Water\")),IF($B109=\"District Cooling\",#REF!,#REF!),VLOOKUP($B109,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B109,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,"",null,null,null,null,null,"",""]
["G","Source energy consumption units used to report energy consumption totals (sum of energy types)","$ / ",{"$f":"IF(C110=\"\",\"\",VLOOKUP(C110,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B110=\"District Cooling\",$B110=\"District Steam\",$B110=\"District Hot Water\")),IF($B110=\"District Cooling\",#REF!,#REF!),VLOOKUP($B110,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B110,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B110=\"District Cooling\",$B110=\"District Steam\",$B110=\"District Hot Water\")),IF($B110=\"District Cooling\",#REF!,#REF!),VLOOKUP($B110,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B110,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,"",null,null,null,null,null,"",""]
["G","","$ / ",{"$f":"IF(C111=\"\",\"\",VLOOKUP(C111,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B111=\"District Cooling\",$B111=\"District Steam\",$B111=\"District Hot Water\")),IF($B111=\"District Cooling\",#REF!,#REF!),VLOOKUP($B111,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B111,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B111=\"District Cooling\",$B111=\"District Steam\",$B111=\"District Hot Water\")),IF($B111=\"District Cooling\",#REF!,#REF!),VLOOKUP($B111,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B111,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,"",null,null,null,null,null,"",""]
["G","","$ / ",{"$f":"IF(C112=\"\",\"\",VLOOKUP(C112,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B112=\"District Cooling\",$B112=\"District Steam\",$B112=\"District Hot Water\")),IF($B112=\"District Cooling\",#REF!,#REF!),VLOOKUP($B112,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B112,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B112=\"District Cooling\",$B112=\"District Steam\",$B112=\"District Hot Water\")),IF($B112=\"District Cooling\",#REF!,#REF!),VLOOKUP($B112,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B112,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(ABS(1-H112/E112),\"\")","v":""},null,null,null,null,null,"",""]
["G","Table 12.2: On-Site Renewable Energy Production","$ / ",{"$f":"IF(C113=\"\",\"\",VLOOKUP(C113,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B113=\"District Cooling\",$B113=\"District Steam\",$B113=\"District Hot Water\")),IF($B113=\"District Cooling\",#REF!,#REF!),VLOOKUP($B113,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B113,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B113=\"District Cooling\",$B113=\"District Steam\",$B113=\"District Hot Water\")),IF($B113=\"District Cooling\",#REF!,#REF!),VLOOKUP($B113,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B113,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,"",null,null,null,null,null,"",""]
["G","","$ / ",{"$f":"IF(C114=\"\",\"\",VLOOKUP(C114,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B114=\"District Cooling\",$B114=\"District Steam\",$B114=\"District Hot Water\")),IF($B114=\"District Cooling\",#REF!,#REF!),VLOOKUP($B114,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B114,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B114=\"District Cooling\",$B114=\"District Steam\",$B114=\"District Hot Water\")),IF($B114=\"District Cooling\",#REF!,#REF!),VLOOKUP($B114,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B114,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(ABS(1-H114/E114),\"\")","v":""},null,null,null,null,null,"",""]
["G","The project building uses on-site renewable energy systems. (Optional)","$ / ",{"$f":"IF(C115=\"\",\"\",VLOOKUP(C115,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B115=\"District Cooling\",$B115=\"District Steam\",$B115=\"District Hot Water\")),IF($B115=\"District Cooling\",#REF!,#REF!),VLOOKUP($B115,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B115,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B115=\"District Cooling\",$B115=\"District Steam\",$B115=\"District Hot Water\")),IF($B115=\"District Cooling\",#REF!,#REF!),VLOOKUP($B115,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B115,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(ABS(1-H115/E115),\"\")","v":""},null,null,null,null,null,"",""]
["G","","$ / ",{"$f":"IF(C116=\"\",\"\",VLOOKUP(C116,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B116=\"District Cooling\",$B116=\"District Steam\",$B116=\"District Hot Water\")),IF($B116=\"District Cooling\",#REF!,#REF!),VLOOKUP($B116,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B116,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B116=\"District Cooling\",$B116=\"District Steam\",$B116=\"District Hot Water\")),IF($B116=\"District Cooling\",#REF!,#REF!),VLOOKUP($B116,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B116,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(ABS(1-H116/E116),\"\")","v":""},null,null,null,null,null,"",""]
["G","Table: On-Site Renewable energy source summary","$ / ",{"$f":"IF(C117=\"\",\"\",VLOOKUP(C117,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B117=\"District Cooling\",$B117=\"District Steam\",$B117=\"District Hot Water\")),IF($B117=\"District Cooling\",#REF!,#REF!),VLOOKUP($B117,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B117,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B117=\"District Cooling\",$B117=\"District Steam\",$B117=\"District Hot Water\")),IF($B117=\"District Cooling\",#REF!,#REF!),VLOOKUP($B117,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B117,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(ABS(1-H117/E117),\"\")","v":""},null,null,null,null,null,"",""]
["G",{"$f":"IFERROR(IF(ISBLANK(B22),\"\",B22),\"\")","v":"Renewable energy production should be reported in the table below. Note: This calculator will automatically reduce the proposed energy consumption and cost to accurately reflect the revised results. Therefore, any site-generated renewable energy production should NOT be included in the Performance Rating Method tables below.\n\nSelect the site-generated renewable energy source. Enter the rated capacity of the site-generated renewable source including the units (e.g. for photovoltaics 10 kW). Include all relevant capacities (i.e for solar thermal, both the storage tank capacity and the solar thermal panel capacity).\n\nThe cost of the Site-generated renewable cost will be automatically determined using the virtual rate once the output data (consumption and cost) is entered below. The cost may be overridden by the user, however this may generate an issue on the Quality Checks and the user should be prepared to justify the entered cost value."},"",{"$f":"IF(C118=\"\",\"\",VLOOKUP(C118,ProjectEnergyTypeTable,3,FALSE))","v":""},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B118=\"District Cooling\",$B118=\"District Steam\",$B118=\"District Hot Water\")),IF($B118=\"District Cooling\",#REF!,#REF!),VLOOKUP($B118,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B118,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B118=\"District Cooling\",$B118=\"District Steam\",$B118=\"District Hot Water\")),IF($B118=\"District Cooling\",#REF!,#REF!),VLOOKUP($B118,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B118,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(ABS(1-H118/E118),\"\")","v":""},null,null,null,null,null,"",""]
["G","","$ / ",{"$f":"IF(C119=\"\",\"\",VLOOKUP(C119,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B119=\"District Cooling\",$B119=\"District Steam\",$B119=\"District Hot Water\")),IF($B119=\"District Cooling\",#REF!,#REF!),VLOOKUP($B119,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B119,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B119=\"District Cooling\",$B119=\"District Steam\",$B119=\"District Hot Water\")),IF($B119=\"District Cooling\",#REF!,#REF!),VLOOKUP($B119,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B119,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,"",null,null,null,null,null,"",""]
["G","On-Site Renewable Source","$ / ",{"$f":"IF(C120=\"\",\"\",VLOOKUP(C120,ProjectEnergyTypeTable,3,FALSE))","v":{"$error":"#NAME?"}},{"$f":"IFERROR(IF(AND(DESPath=3,OR($B120=\"District Cooling\",$B120=\"District Steam\",$B120=\"District Hot Water\")),IF($B120=\"District Cooling\",#REF!,#REF!),VLOOKUP($B120,PO_Enrgy_7_Table,MATCH($G$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B120,PO_Enrgy_7_Table,MATCH($E$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,{"$f":"IFERROR(IF(AND(DESPath=3,OR($B120=\"District Cooling\",$B120=\"District Steam\",$B120=\"District Hot Water\")),IF($B120=\"District Cooling\",#REF!,#REF!),VLOOKUP($B120,PO_Enrgy_7_Table,MATCH($J$84,PO_Enrgy_7_Hdr,0),FALSE)/VLOOKUP($B120,PO_Enrgy_7_Table,MATCH($H$84,PO_Enrgy_7_Hdr,0),FALSE)),\"\")","v":""},null,null,"",null,null,null,null,null,"",""]
["G"]
["G","Table: Exceptional calculation methods"]
["G","Energy Type","Site Energy Units",null,"Baseline Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site_Energy",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B10),\"\",B10),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B126),\"\",VLOOKUP($B126,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C126=\"\",\"\",VLOOKUP(C126,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H126/E126,\"\")","v":""},null,{"$f":"IFERROR(1-J126/G126,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B126),\"\",VLOOKUP($B126,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B126),\"\",VLOOKUP($B126,PO_Enrgy_1_Table,MATCH($M$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C127=\"\",\"\",VLOOKUP(C127,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C128=\"\",\"\",VLOOKUP(C128,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","Site energy consumption units used to report energy consumption totals (sum of energy types)","",{"$f":"IF(C129=\"\",\"\",VLOOKUP(C129,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","Source energy consumption units used to report energy consumption totals (sum of energy types)","",{"$f":"IF(C130=\"\",\"\",VLOOKUP(C130,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C131=\"\",\"\",VLOOKUP(C131,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H131/E131,\"\")","v":""},null,{"$f":"IFERROR(1-J131/G131,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C132=\"\",\"\",VLOOKUP(C132,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H132/E132,\"\")","v":""},null,{"$f":"IFERROR(1-J132/G132,\"\")","v":""},null,null,null,"",""]
["G","Table 12.2: On-Site Renewable Energy Production","",{"$f":"IF(C133=\"\",\"\",VLOOKUP(C133,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C134=\"\",\"\",VLOOKUP(C134,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H134/E134,\"\")","v":""},null,{"$f":"IFERROR(1-J134/G134,\"\")","v":""},null,null,null,"",""]
["G","The project building uses on-site renewable energy systems. (Optional)","",{"$f":"IF(C135=\"\",\"\",VLOOKUP(C135,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H135/E135,\"\")","v":""},null,{"$f":"IFERROR(1-J135/G135,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C136=\"\",\"\",VLOOKUP(C136,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H136/E136,\"\")","v":""},null,{"$f":"IFERROR(1-J136/G136,\"\")","v":""},null,null,null,"",""]
["G","Table: On-Site Renewable energy source summary","",{"$f":"IF(C137=\"\",\"\",VLOOKUP(C137,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H137/E137,\"\")","v":""},null,{"$f":"IFERROR(1-J137/G137,\"\")","v":""},null,null,null,"",""]
["G",{"$f":"IFERROR(IF(ISBLANK(B22),\"\",B22),\"\")","v":"Renewable energy production should be reported in the table below. Note: This calculator will automatically reduce the proposed energy consumption and cost to accurately reflect the revised results. Therefore, any site-generated renewable energy production should NOT be included in the Performance Rating Method tables below.\n\nSelect the site-generated renewable energy source. Enter the rated capacity of the site-generated renewable source including the units (e.g. for photovoltaics 10 kW). Include all relevant capacities (i.e for solar thermal, both the storage tank capacity and the solar thermal panel capacity).\n\nThe cost of the Site-generated renewable cost will be automatically determined using the virtual rate once the output data (consumption and cost) is entered below. The cost may be overridden by the user, however this may generate an issue on the Quality Checks and the user should be prepared to justify the entered cost value."},"",{"$f":"IF(C138=\"\",\"\",VLOOKUP(C138,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H138/E138,\"\")","v":""},null,{"$f":"IFERROR(1-J138/G138,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C139=\"\",\"\",VLOOKUP(C139,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","On-Site Renewable Source","",{"$f":"IF(C140=\"\",\"\",VLOOKUP(C140,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_9_Table,0,MATCH(E$125,PO_Enrgy_9_Hdr,0)),INDEX(PO_Enrgy_9_Table,0,MATCH($Q$125,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(F$125,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(G$125,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_9_Table,0,MATCH(H$125,PO_Enrgy_9_Hdr,0)),INDEX(PO_Enrgy_9_Table,0,MATCH($Q$125,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(I$125,PO_Enrgy_9_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_9_Table,0,MATCH(J$125,PO_Enrgy_9_Hdr,0))),\"\")","v":0},"",null,""]
["G"]
["G","Table: Subtotal including DES Path 3 Streamlined calculations"]
["G","Energy Type","Site Energy Units",null,"Baseline Building Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Proposed Building Energy Consumption \nwith Exceptional Calculation Methods",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use (\"  & PO_SourceUnits & \")\"","v":"Source Energy Use (Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B10),\"\",B10),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B147),\"\",VLOOKUP($B147,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},null,0,0,0,0,0,0,{"$f":"IFERROR(1-H147/E147,\"\")","v":""},null,{"$f":"IFERROR(1-J147/G147,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B147),\"\",VLOOKUP($B147,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B147),\"\",VLOOKUP($B147,PO_Enrgy_1_Table,MATCH($M$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C148=\"\",\"\",VLOOKUP(C148,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C149=\"\",\"\",VLOOKUP(C149,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","Site energy consumption units used to report energy consumption totals (sum of energy types)","",{"$f":"IF(C150=\"\",\"\",VLOOKUP(C150,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","Source energy consumption units used to report energy consumption totals (sum of energy types)","",{"$f":"IF(C151=\"\",\"\",VLOOKUP(C151,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C152=\"\",\"\",VLOOKUP(C152,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H152/E152,\"\")","v":""},null,{"$f":"IFERROR(1-J152/G152,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C153=\"\",\"\",VLOOKUP(C153,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H153/E153,\"\")","v":""},null,{"$f":"IFERROR(1-J153/G153,\"\")","v":""},null,null,null,"",""]
["G","Table 12.2: On-Site Renewable Energy Production","",{"$f":"IF(C154=\"\",\"\",VLOOKUP(C154,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C155=\"\",\"\",VLOOKUP(C155,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H155/E155,\"\")","v":""},null,{"$f":"IFERROR(1-J155/G155,\"\")","v":""},null,null,null,"",""]
["G","The project building uses on-site renewable energy systems. (Optional)","",{"$f":"IF(C156=\"\",\"\",VLOOKUP(C156,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H156/E156,\"\")","v":""},null,{"$f":"IFERROR(1-J156/G156,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C157=\"\",\"\",VLOOKUP(C157,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H157/E157,\"\")","v":""},null,{"$f":"IFERROR(1-J157/G157,\"\")","v":""},null,null,null,"",""]
["G","Table: On-Site Renewable energy source summary","",{"$f":"IF(C158=\"\",\"\",VLOOKUP(C158,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H158/E158,\"\")","v":""},null,{"$f":"IFERROR(1-J158/G158,\"\")","v":""},null,null,null,"",""]
["G",{"$f":"IFERROR(IF(ISBLANK(B22),\"\",B22),\"\")","v":"Renewable energy production should be reported in the table below. Note: This calculator will automatically reduce the proposed energy consumption and cost to accurately reflect the revised results. Therefore, any site-generated renewable energy production should NOT be included in the Performance Rating Method tables below.\n\nSelect the site-generated renewable energy source. Enter the rated capacity of the site-generated renewable source including the units (e.g. for photovoltaics 10 kW). Include all relevant capacities (i.e for solar thermal, both the storage tank capacity and the solar thermal panel capacity).\n\nThe cost of the Site-generated renewable cost will be automatically determined using the virtual rate once the output data (consumption and cost) is entered below. The cost may be overridden by the user, however this may generate an issue on the Quality Checks and the user should be prepared to justify the entered cost value."},"",{"$f":"IF(C159=\"\",\"\",VLOOKUP(C159,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H159/E159,\"\")","v":""},null,{"$f":"IFERROR(1-J159/G159,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C160=\"\",\"\",VLOOKUP(C160,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","On-Site Renewable Source","",{"$f":"IF(C161=\"\",\"\",VLOOKUP(C161,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G",{"$f":"\"Energy Model Subtotal (\" & PO_SiteUnits & \")\"","v":"Energy Model Subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_13_Table,0,MATCH(E$146,PO_Enrgy_13_Hdr,0)),INDEX(PO_Enrgy_13_Table,0,MATCH($Q$146,PO_Enrgy_13_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(F$146,PO_Enrgy_12_Hdr,0))),\"\")","v":""},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(G$146,PO_Enrgy_12_Hdr,0))),\"\")","v":""},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_13_Table,0,MATCH(H$146,PO_Enrgy_13_Hdr,0)),INDEX(PO_Enrgy_13_Table,0,MATCH($Q$146,PO_Enrgy_13_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(I$146,PO_Enrgy_12_Hdr,0))),\"\")","v":""},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_13_Table,0,MATCH(J$146,PO_Enrgy_12_Hdr,0))),\"\")","v":""},"",null,""]
["G"]
["G","Total energy cost savings (excluding site-generated renewable energy) (%)",null,null,null,null,null,null,null,null,{"$f":"$M$162","v":""}]
["G"]
["G","Table: Renewable energy production"]
["G","Energy Type","Site Energy Units",null,"On-Site Renewable Savings",null,null,"Proposed with On-Site Renewable Energy",null,null,"Percent Cost Savings"]
["G",null,null,null,"Site Energy Use Savings ",{"$f":"\"Source Energy Use Savings \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use Savings \n(Btu x 10^6)"},"Cost Savings","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Renewable_Site_Savings","Renewable_Source_Savings","Renewable_Cost_Savings","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B10),\"\",B10),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B170),\"\",VLOOKUP($B170,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C170=\"\",\"\",VLOOKUP(C170,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-$H170/VLOOKUP($B170,PO_Enrgy_13_Table,MATCH($E$146,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},null,{"$f":"IFERROR(1-$J170/VLOOKUP($B170,PO_Enrgy_13_Table,MATCH($G$146,PO_Enrgy_13_Hdr,0),FALSE),\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B170),\"\",VLOOKUP($B170,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B170),\"\",VLOOKUP($B170,PO_Enrgy_1_Table,MATCH($M$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C171=\"\",\"\",VLOOKUP(C171,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C172=\"\",\"\",VLOOKUP(C172,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","Site energy consumption units used to report energy consumption totals (sum of energy types)","",{"$f":"IF(C173=\"\",\"\",VLOOKUP(C173,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","Source energy consumption units used to report energy consumption totals (sum of energy types)","",{"$f":"IF(C174=\"\",\"\",VLOOKUP(C174,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C175=\"\",\"\",VLOOKUP(C175,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C176=\"\",\"\",VLOOKUP(C176,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","Table 12.2: On-Site Renewable Energy Production","",{"$f":"IF(C177=\"\",\"\",VLOOKUP(C177,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C178=\"\",\"\",VLOOKUP(C178,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","The project building uses on-site renewable energy systems. (Optional)","",{"$f":"IF(C179=\"\",\"\",VLOOKUP(C179,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C180=\"\",\"\",VLOOKUP(C180,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","Table: On-Site Renewable energy source summary","",{"$f":"IF(C181=\"\",\"\",VLOOKUP(C181,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G",{"$f":"IFERROR(IF(ISBLANK(B22),\"\",B22),\"\")","v":"Renewable energy production should be reported in the table below. Note: This calculator will automatically reduce the proposed energy consumption and cost to accurately reflect the revised results. Therefore, any site-generated renewable energy production should NOT be included in the Performance Rating Method tables below.\n\nSelect the site-generated renewable energy source. Enter the rated capacity of the site-generated renewable source including the units (e.g. for photovoltaics 10 kW). Include all relevant capacities (i.e for solar thermal, both the storage tank capacity and the solar thermal panel capacity).\n\nThe cost of the Site-generated renewable cost will be automatically determined using the virtual rate once the output data (consumption and cost) is entered below. The cost may be overridden by the user, however this may generate an issue on the Quality Checks and the user should be prepared to justify the entered cost value."},"",{"$f":"IF(C182=\"\",\"\",VLOOKUP(C182,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C183=\"\",\"\",VLOOKUP(C183,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","On-Site Renewable Source","",{"$f":"IF(C184=\"\",\"\",VLOOKUP(C184,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G",{"$f":"\"Energy model subtotal (\" & PO_SiteUnits & \")\"","v":"Energy model subtotal (Btu x 10^6)"},null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_14_Table,0,MATCH(E$169,PO_Enrgy_14_Hdr,0)),INDEX(PO_Enrgy_14_Table,0,MATCH($Q$169,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(F$169,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(G$169,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_14_Table,0,MATCH(H$169,PO_Enrgy_14_Hdr,0)),INDEX(PO_Enrgy_14_Table,0,MATCH($Q$169,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(I$169,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_14_Table,0,MATCH(J$169,PO_Enrgy_14_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(1-$H185/$E$162,\"\")","v":""},null,{"$f":"IFERROR(1-$J185/$G$162,\"\")","v":""}]
["G"]
["G","Table: Total energy usage"]
["G","Energy Type","Site Energy Units",null,"Baseline",null,null,"Proposed",null,null,"Percent Savings"]
["G",null,null,null,"Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use (Units shown per energy type)",{"$f":"\"Source Energy Use \n(\"  & PO_SourceUnits & \")\"","v":"Source Energy Use \n(Btu x 10^6)"},"Cost","Site Energy Use",null,"Cost"]
["G","Energy_Type","Energy_Units",null,"Base_Site_Energy","Base_Source_Energy","Base_Cost","Design_Site_Energy","Design_Source_Energy","Design_Cost","Percent_Savings_Site",null,"Percent_Savings_Cost",null,null,null,"Site_Unit_Conversion","Source_Unit_Conversion"]
["G",{"$f":"IFERROR(IF(ISBLANK(B10),\"\",B10),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B191),\"\",VLOOKUP($B191,PO_Enrgy_1_Table,MATCH($C$9,PO_Enrgy_1_Hdr,0),FALSE) ),\"\")","v":""},{"$f":"IF(C191=\"\",\"\",VLOOKUP(C191,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H191/E191,\"\")","v":""},null,{"$f":"IFERROR(1-J191/G191,\"\")","v":""},null,null,null,{"$f":"IFERROR(IF(ISBLANK($B191),\"\",VLOOKUP($B191,PO_Enrgy_1_Table,MATCH($K$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""},{"$f":"IFERROR(IF(ISBLANK($B191),\"\",VLOOKUP($B191,PO_Enrgy_1_Table,MATCH($M$9,PO_Enrgy_1_Hdr,0),FALSE)),\"\")","v":""}]
["G","","",{"$f":"IF(C192=\"\",\"\",VLOOKUP(C192,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C193=\"\",\"\",VLOOKUP(C193,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","Site energy consumption units used to report energy consumption totals (sum of energy types)","",{"$f":"IF(C194=\"\",\"\",VLOOKUP(C194,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","Source energy consumption units used to report energy consumption totals (sum of energy types)","",{"$f":"IF(C195=\"\",\"\",VLOOKUP(C195,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C196=\"\",\"\",VLOOKUP(C196,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H196/E196,\"\")","v":""},null,{"$f":"IFERROR(1-J196/G196,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C197=\"\",\"\",VLOOKUP(C197,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H197/E197,\"\")","v":""},null,{"$f":"IFERROR(1-J197/G197,\"\")","v":""},null,null,null,"",""]
["G","Table 12.2: On-Site Renewable Energy Production","",{"$f":"IF(C198=\"\",\"\",VLOOKUP(C198,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","","",{"$f":"IF(C199=\"\",\"\",VLOOKUP(C199,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H199/E199,\"\")","v":""},null,{"$f":"IFERROR(1-J199/G199,\"\")","v":""},null,null,null,"",""]
["G","The project building uses on-site renewable energy systems. (Optional)","",{"$f":"IF(C200=\"\",\"\",VLOOKUP(C200,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H200/E200,\"\")","v":""},null,{"$f":"IFERROR(1-J200/G200,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C201=\"\",\"\",VLOOKUP(C201,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H201/E201,\"\")","v":""},null,{"$f":"IFERROR(1-J201/G201,\"\")","v":""},null,null,null,"",""]
["G","Table: On-Site Renewable energy source summary","",{"$f":"IF(C202=\"\",\"\",VLOOKUP(C202,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H202/E202,\"\")","v":""},null,{"$f":"IFERROR(1-J202/G202,\"\")","v":""},null,null,null,"",""]
["G",{"$f":"IFERROR(IF(ISBLANK(B22),\"\",B22),\"\")","v":"Renewable energy production should be reported in the table below. Note: This calculator will automatically reduce the proposed energy consumption and cost to accurately reflect the revised results. Therefore, any site-generated renewable energy production should NOT be included in the Performance Rating Method tables below.\n\nSelect the site-generated renewable energy source. Enter the rated capacity of the site-generated renewable source including the units (e.g. for photovoltaics 10 kW). Include all relevant capacities (i.e for solar thermal, both the storage tank capacity and the solar thermal panel capacity).\n\nThe cost of the Site-generated renewable cost will be automatically determined using the virtual rate once the output data (consumption and cost) is entered below. The cost may be overridden by the user, however this may generate an issue on the Quality Checks and the user should be prepared to justify the entered cost value."},"",{"$f":"IF(C203=\"\",\"\",VLOOKUP(C203,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,{"$f":"IFERROR(1-H203/E203,\"\")","v":""},null,{"$f":"IFERROR(1-J203/G203,\"\")","v":""},null,null,null,"",""]
["G","","",{"$f":"IF(C204=\"\",\"\",VLOOKUP(C204,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","On-Site Renewable Source","",{"$f":"IF(C205=\"\",\"\",VLOOKUP(C205,ProjectEnergyTypeTable,3,FALSE))","v":""},0,0,0,0,0,0,"",null,"",null,null,null,"",""]
["G","Totals",null,null,{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_16_Table,0,MATCH(E$190,PO_Enrgy_16_Hdr,0)),INDEX(PO_Enrgy_16_Table,0,MATCH($Q$190,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(F$190,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(G$190,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUMPRODUCT(INDEX(PO_Enrgy_16_Table,0,MATCH(H$190,PO_Enrgy_16_Hdr,0)),INDEX(PO_Enrgy_16_Table,0,MATCH($Q$190,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(I$190,PO_Enrgy_16_Hdr,0))),\"\")","v":0},{"$f":"IFERROR(SUM(INDEX(PO_Enrgy_16_Table,0,MATCH(J$190,PO_Enrgy_16_Hdr,0))),\"\")","v":0},"",null,""]
["G","Total energy cost savings (including site-generated renewable energy) (%)",null,null,null,null,null,null,null,null,null,null,{"$f":"$M$206","v":""}]
["G"]
[null,"Quality Assurance Checks"]
[null,"The issues listed below were automatically generated based upon information provided in the input and output sections. The intent is to address common review issues before submitting for certification via changing the model and/or actual design. This section is not meant to catch all potential issues present within the submittal. Although responses are not required, the project team is strongly encouraged to address each issue noted, as this will reduce the number of review comments and increase the likelihood of awarding this prerequisite at the preliminary review stage."]
[null,"Lighting","BExt Ltg Demand","DExt Ltg Demand",null,"BNT Ext Ltg Max","DNT Ext Ltg Max","Exterior Compliant"]
[null,null,{"$f":"OFFSET(L_ExtSum_Table,1,MATCH('6b - General Lighting'!$J$171,L_ExtSum_Hdr,0)-1,1,1)","v":0},{"$f":"OFFSET(L_ExtSum_Table,1,MATCH('6b - General Lighting'!$M$171,L_ExtSum_Hdr,0)-1,1,1)","v":0},null,{"$f":"OFFSET(L_LtgZone_Table,1,MATCH('6b - General Lighting'!$M$134,L_LtgZone_Hdr,0)-1,1,1)+OFFSET(L_NTSurface_Table,MATCH('6b - General Lighting'!$B$165,L_NTSurface_Index,0)-1,MATCH('6b - General Lighting'!$J$158,L_NTSurface_Hdr,0)-1,1,1)","v":{"$error":"#N/A"}},{"$f":"OFFSET(L_NTSurface_Table,MATCH('6b - General Lighting'!$B$165,L_NTSurface_Index,0)-1,MATCH('6b - General Lighting'!$M$158,L_NTSurface_Hdr,0)-1,1,1)","v":0},{"$f":"L_ELR_Response","v":0}]
[null,"Performace Outputs","Base Ext Ltg Demand","Design Ext Ltg Demand"]
[null,null,{"$f":"GetPerformanceOutputRangeSums(\"PO_QA_BaseExtLtgDem\")","v":"Error"},{"$f":"GetPerformanceOutputRangeSums(\"PO_QA_DesignExtLtgDem\")","v":"Error"},null,null,null,null,null,null,null,"z"]
[]
[null,"Issue",null,null,null,null,null,null,null,"Project Team Response",null,null,null,null,null,null,"Trigger","Issue Applicable to Project"]
[null,"The exterior lighting demand as reported in the Performance Outputs tab for the baseline and/or proposed exceeds the lighting power reported on the Lighting sheet (Summary section) by more than 5%. Ensure that the values reflected in the Lighting sheet are accurate and appropriately reflect the modeled exterior lighting power density.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(OR((C214-C212)/MIN(C214,C212)>0.05,(D214-D212)/MIN(D214,D212)>0.05),TRUE,FALSE),TRUE)","v":true}]
[null,"The total exterior lighting power allowance, including the base site allowance, is less than the designed lighting power as reported in the Lighting tab, violating mandatory Section 9.4.3. Verify that the inputs are accurate and modify the exterior lighting design as necessary to show compliance.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(D212>C212,TRUE,FALSE),TRUE)","v":false}]
[null,"The value for nontradable exterior lighting power (building facades, ATMs and night depositories, entrances and gatehouse inspection stations at guarded facilities, loading areas for law enforcement, fire, ambulance, and other emergency service vehicles, drive-through windows at fast food restaurants, and/or parking near 24-hour retail entrances) is less than the designed lighting power after adding in the unrestricted lighting power allowance as reported in the Lighting sheet, violating mandatory Section 9.4.3. Verify that the inputs are accurate and modify the exterior lighting design as necessary to show compliance.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(G212>F212,TRUE,FALSE),TRUE)","v":true}]
[null,"The exterior lighting inputs indicate that additional lighting power allowance has been claimed in the baseline for surfaces that are not provided with lighting in the actual design and/or lighting fixtures have been double-counted for different exterior surfaces.  Please review selection in LIghting tab or provide a narrative which explains the reasoning for this choice.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(H212<>\"Yes\",TRUE,FALSE),TRUE)","v":true}]

{"sheet":"BPF 2013BM","index":40,"n_rows":12,"n_cols":20,"rows_kept":12,"cut":false,"hidden":true,"merged":[[1,1,1,19]]}
[]
[null,"Table 4.2.1.1 Building Performance Factors (BPF) for Compliance with Standard 90.1-2013BM"]
[null,"Building Type","1A","1B","2A","2B","3A","3B","3C","4A","4B","4C","5A","5B","5C","6A","6B",7,8,"Average"]
[null,"Multifamily",0.73,0.73,0.71,0.69,0.74,0.73,0.68,0.78,0.81,0.81,0.76,0.8,0.81,0.76,0.79,0.74,0.8,{"$f":"AVERAGE(C4:S4)","v":0.7570588235294119}]
[null,"Healthcare/hospital",0.64,0.56000000000000005,0.6,0.56000000000000005,0.6,0.56000000000000005,0.54,0.56999999999999995,0.53,0.55000000000000004,0.59,0.52,0.55000000000000004,0.56999999999999995,0.52,0.56000000000000005,0.56000000000000005,{"$f":"AVERAGE(C5:S5)","v":0.56352941176470595}]
[null,"Hotel/motel",0.64,0.65,0.62,0.6,0.63,0.65,0.64,0.62,0.64,0.62,0.6,0.61,0.6,0.59,0.61,0.56999999999999995,0.57999999999999996,0.61588235294117644]
[null,"Office",0.57999999999999996,0.62,0.56999999999999995,0.62,0.6,0.64,0.54,0.57999999999999996,0.6,0.57999999999999996,0.6,0.61,0.57999999999999996,0.61,0.61,0.56999999999999995,0.61,0.59529411764705875]
[null,"Restaurant",0.62,0.62,0.57999999999999996,0.61,0.6,0.6,0.61,0.57999999999999996,0.55000000000000004,0.6,0.62,0.57999999999999996,0.6,0.63,0.6,0.65,0.68,0.60764705882352943]
[null,"Retail",0.52,0.57999999999999996,0.53,0.57999999999999996,0.54,0.62,0.6,0.55000000000000004,0.6,0.6,0.55000000000000004,0.59,0.61,0.55000000000000004,0.57999999999999996,0.53,0.53,0.56823529411764695]
[null,"School",0.46,0.53,0.47,0.53,0.49,0.52,0.5,0.49,0.5,0.49,0.5,0.5,0.5,0.49,0.5,0.47,0.51,0.49705882352941183]
[null,"Warehouse",0.51,0.52,0.56000000000000005,0.57999999999999996,0.56999999999999995,0.59,0.63,0.57999999999999996,0.6,0.63,0.6,0.61,0.65,0.66,0.66,0.67,0.67,0.60529411764705876]
[null,"All Others",0.62,0.61,0.55000000000000004,0.56999999999999995,0.56000000000000005,0.61,0.59,0.57999999999999996,0.56999999999999995,0.61,0.6,0.56999999999999995,0.61,0.56000000000000005,0.56000000000000005,0.53,0.52,0.5776470588235294]

{"sheet":"BPF 2007","index":41,"n_rows":12,"n_cols":20,"rows_kept":12,"cut":false,"hidden":true,"merged":[[1,1,1,19]]}
[]
[null,"Table 2.2 Building Performance Factors (BPF) for Compliance with Standard 90.1-2010"]
[null,"Building Type","1A","1B","2A","2B","3A","3B","3C","4A","4B","4C","5A","5B","5C","6A","6B",7,8,"Average"]
[null,"Office"]
[null,"Retail"]
[null,"School"]
[null,"Healthcare/hospital"]
[null,"Restaurant"]
[null,"Hotel/motel"]
[null,"Warehouse"]
[null,"Multifamily",0.96,0.96,0.93,0.91,0.93,0.92,0.85,0.97,0.97,0.97,0.97,0.97,0.97,0.97,0.97,0.93,0.95,{"$f":"AVERAGE(C11:S11)","v":0.94705882352941206}]
[null,"All Others"]

{"sheet":"BPF 2010","index":42,"n_rows":12,"n_cols":20,"rows_kept":12,"cut":false,"hidden":true,"merged":[[1,1,1,19]]}
[]
[null,"Table 2.2 Building Performance Factors (BPF) for Compliance with Standard 90.1-2010"]
[null,"Building Type","1A","1B","2A","2B","3A","3B","3C","4A","4B","4C","5A","5B","5C","6A","6B",7,8,"Average"]
[null,"Office",0.74,0.77,0.73,0.76,0.72,0.76,0.66,0.7,0.73,0.7,0.72,0.73,0.7,0.71,0.72,0.7,0.75,0.72]
[null,"Retail",0.71,0.75,0.68,0.71,0.68,0.74,0.75,0.69,0.74,0.75,0.69,0.73,0.76,0.69,0.74,0.66,0.69,0.72]
[null,"School",0.68,0.68,0.64,0.67,0.63,0.67,0.68,0.63,0.67,0.64,0.63,0.63,0.63,0.63,0.62,0.61,0.64,0.65]
[null,"Healthcare/hospital",0.72,0.75,0.7,0.7,0.69,0.72,0.64,0.66,0.73,0.66,0.69,0.7,0.66,0.69,0.68,0.69,0.71,0.69]
[null,"Restaurant",0.76,0.73,0.71,0.72,0.72,0.72,0.78,0.7,0.71,0.76,0.74,0.72,0.75,0.75,0.74,0.78,0.79,0.74]
[null,"Hotel/motel",0.8,0.82,0.76,0.77,0.77,0.81,0.8,0.76,0.81,0.78,0.72,0.77,0.73,0.71,0.73,0.69,0.7,0.76]
[null,"Warehouse",0.63,0.62,0.67,0.69,0.67,0.69,0.73,0.69,0.71,0.72,0.7,0.71,0.74,0.74,0.73,0.73,0.76,0.7]
[null,"Multifamily",0.92,0.91,0.88,0.86,0.87,0.87,0.8,0.9,0.93,0.92,0.88,0.92,0.92,0.88,0.91,0.83,0.89,0.89]
[null,"All Others",0.81,0.76,0.7,0.71,0.69,0.74,0.72,0.71,0.73,0.73,0.69,0.72,0.73,0.69,0.7,0.67,0.67,0.72]

{"sheet":"BPF 2013","index":43,"n_rows":12,"n_cols":20,"rows_kept":12,"cut":false,"hidden":true,"merged":[[1,1,1,19]]}
[]
[null,"Table 2.3 Building Performance Factors (BPF) for Compliance with Standard 90.1-2013"]
[null,"Building Type","1A","1B","2A","2B","3A","3B","3C","4A","4B","4C","5A","5B","5C","6A","6B",7,8,"Average"]
[null,"Office",0.63,0.67,0.62,0.67,0.65,0.69,0.59,0.63,0.65,0.63,0.65,0.66,0.63,0.66,0.66,0.62,0.66,0.65]
[null,"Retail",0.56999999999999995,0.63,0.57999999999999996,0.63,0.59,0.67,0.65,0.6,0.65,0.65,0.6,0.64,0.66,0.6,0.63,0.57999999999999996,0.57999999999999996,0.62]
[null,"School",0.51,0.57999999999999996,0.52,0.57999999999999996,0.54,0.56999999999999995,0.55000000000000004,0.54,0.55000000000000004,0.54,0.55000000000000004,0.55000000000000004,0.55000000000000004,0.54,0.55000000000000004,0.52,0.56000000000000005,0.55000000000000004]
[null,"Healthcare/hospital",0.69,0.61,0.65,0.61,0.65,0.61,0.59,0.62,0.57999999999999996,0.6,0.64,0.56999999999999995,0.6,0.62,0.56999999999999995,0.61,0.61,0.61]
[null,"Restaurant",0.67,0.67,0.63,0.66,0.65,0.65,0.66,0.63,0.6,0.65,0.67,0.63,0.65,0.68,0.65,0.7,0.73,0.66]
[null,"Hotel/motel",0.69,0.7,0.67,0.65,0.68,0.7,0.69,0.67,0.69,0.67,0.65,0.66,0.65,0.64,0.66,0.62,0.63,0.67]
[null,"Warehouse",0.56000000000000005,0.56999999999999995,0.61,0.63,0.62,0.64,0.68,0.63,0.65,0.68,0.65,0.66,0.7,0.71,0.71,0.72,0.72,0.66]
[null,"Multifamily",0.78,0.78,0.76,0.74,0.79,0.78,0.73,0.83,0.86,0.86,0.81,0.85,0.86,0.81,0.84,0.79,0.85,0.81]
[null,"All Others",0.67,0.66,0.6,0.62,0.61,0.66,0.64,0.63,0.62,0.66,0.62,0.62,0.66,0.61,0.61,0.57999999999999996,0.56999999999999995,0.63]

{"sheet":"BPF 2016","index":44,"n_rows":12,"n_cols":20,"rows_kept":12,"cut":false,"hidden":true,"merged":[[1,1,1,19]]}
[]
[null,"Table 2.4 Building Performance Factors (BPF) for Compliance with Standard 90.1-2016"]
[null,"Building Type","1A","1B","2A","2B","3A","3B","3C","4A","4B","4C","5A","5B","5C","6A","6B",7,8,"Average"]
[null,"Office",0.57999999999999996,0.62,0.56999999999999995,0.62,0.6,0.64,0.54,0.57999999999999996,0.6,0.57999999999999996,0.6,0.61,0.57999999999999996,0.61,0.61,0.56999999999999995,0.61,0.6]
[null,"Retail",0.52,0.57999999999999996,0.53,0.57999999999999996,0.54,0.62,0.6,0.55000000000000004,0.6,0.6,0.55000000000000004,0.59,0.61,0.55000000000000004,0.57999999999999996,0.53,0.53,0.56999999999999995]
[null,"School",0.46,0.53,0.47,0.53,0.49,0.52,0.5,0.49,0.5,0.49,0.5,0.5,0.5,0.49,0.5,0.47,0.51,0.5]
[null,"Healthcare/hospital",0.64,0.56000000000000005,0.6,0.56000000000000005,0.6,0.56000000000000005,0.54,0.56999999999999995,0.53,0.55000000000000004,0.59,0.52,0.55000000000000004,0.56999999999999995,0.52,0.56000000000000005,0.56000000000000005,0.56000000000000005]
[null,"Restaurant",0.62,0.62,0.57999999999999996,0.61,0.6,0.6,0.61,0.57999999999999996,0.55000000000000004,0.6,0.62,0.57999999999999996,0.6,0.63,0.6,0.65,0.68,0.61]
[null,"Hotel/motel",0.64,0.65,0.62,0.6,0.63,0.65,0.64,0.62,0.64,0.62,0.6,0.61,0.6,0.59,0.61,0.56999999999999995,0.57999999999999996,0.62]
[null,"Warehouse",0.51,0.52,0.56000000000000005,0.57999999999999996,0.56999999999999995,0.59,0.63,0.57999999999999996,0.6,0.63,0.6,0.61,0.65,0.66,0.66,0.67,0.67,0.61]
[null,"Multifamily",0.73,0.73,0.71,0.69,0.74,0.73,0.68,0.78,0.81,0.81,0.76,0.8,0.81,0.76,0.79,0.74,0.8,0.76]
[null,"All Others",0.62,0.61,0.55000000000000004,0.56999999999999995,0.56000000000000005,0.61,0.59,0.57999999999999996,0.56999999999999995,0.61,0.56999999999999995,0.56999999999999995,0.61,0.56000000000000005,0.56000000000000005,0.53,0.52,0.57999999999999996]

{"sheet":"Summary","index":45,"n_rows":23,"n_cols":33,"rows_kept":23,"cut":false,"hidden":false,"merged":[[19,31,19,32],[13,2,13,32],[5,31,5,32],[10,31,10,32],[15,2,15,32],[14,2,14,32]]}
[]
[]
[null,null,"Summary "]
[null,null,"Note: All information in this section is READ-ONLY. To edit, see previous tabs. "]
[]
[null,null,"Total energy cost savings (excluding site-generated renewable energy) (%)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(MultipleBuildingsExist=\"Yes\",ROUNDUP(Performance_Outputs_Summary!$K$164,3),ROUNDUP('12 - Performance_Outputs_1'!$M$362,3)),\"\")","v":""}]
[]
[]
[null,null,"For projects pursuing EA Credit Optimize Energy Performance"]
[]
[null,null,"Total energy cost savings (including site-generated renewable energy) (%)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(MultipleBuildingsExist=\"Yes\",ROUNDUP(Performance_Outputs_Summary!$M$207,3),ROUNDUP('12 - Performance_Outputs_1'!$M$411,3)),\"\")","v":""}]
[]
[]
[null,null,"Performance Threshold"]
[null,null,{"$f":"IF(proj_RatingSystem=\"Data Centers - New Construction\",\"Thresholds are based on the major renovation area as a percentage of total conditioned building area.  A minimum 2% of energy savings must come from building power and cooling infrastructure.\",IF(OR(\"A\"=1,proj_RatingSystem=\"Core and Shell\"),\"\",IF(proj_RatingSystem=\"Homes\",\"The performance thresholds in the table below are used in combination with the point adjustment on the multifamily details tab for a maximum of 30 points\",\"Thresholds are based on the major renovation area as a percentage of total conditioned building area.\")))","v":"The performance thresholds in the table below are used in combination with the point adjustment on the multifamily details tab for a maximum of 30 points"}]
[null,null,"Performance Improvement  Threshold"]
[null,null,{"$f":"IF(proj_RatingSystem=\"Core and Shell\",0.02,IF(proj_RatingSystem=\"Homes\",0.05,IF(RatingSystem_IDC=TRUE,0.03,5*(pctNew/100)+3*(PctRenovation/100))))","v":0.05},{"$f":"C17+1%","v":6.0000000000000005E-2},{"$f":"IF(OR(RatingSystem_IDC=TRUE,proj_RatingSystem=\"Homes\"),D17+1%,D17+2%)","v":7.0000000000000007E-2},0.08,0.09,9.9999999999999992E-2,0.10999999999999999,0.11999999999999998,0.12999999999999998,0.13999999999999999,0.15,0.16,{"$f":"IF(OR(RatingSystem_IDC=TRUE,proj_RatingSystem=\"Homes\"),N17+1%,N17+3%)","v":0.17},{"$f":"IF(OR(RatingSystem_IDC=TRUE,proj_RatingSystem=\"Homes\"),O17+1%,O17+3%)","v":0.18000000000000002},{"$f":"IF(OR(RatingSystem_IDC=TRUE,proj_RatingSystem=\"Homes\"),P17+1%,P17+3%)","v":0.19000000000000003},{"$f":"IF(OR(RatingSystem_IDC=TRUE,proj_RatingSystem=\"Homes\"),Q17+1%,Q17+3%)","v":0.20000000000000004},{"$f":"IF(proj_RatingSystem=\"Homes\",R17+2%,IF(RatingSystem_IDC=TRUE,R17+2%,R17+4%))","v":0.22000000000000003},{"$f":"IF(proj_RatingSystem=\"Homes\",S17+2%,IF(RatingSystem_IDC=TRUE,S17+2%,IF(proj_RatingSystem=\"Schools - New Construction\",\"\",S17+4%)))","v":0.24000000000000002},{"$f":"IF(proj_RatingSystem=\"Homes\",T17+2%,IF(RatingSystem_IDC=TRUE,T17+2%,IF(proj_RatingSystem=\"Schools - New Construction\",\"\",T17+4%)))","v":0.26},{"$f":"IF(proj_RatingSystem=\"Homes\",U17+2%,IF(RatingSystem_IDC=TRUE,U17+4%,\"\"))","v":0.28000000000000003},{"$f":"IF(proj_RatingSystem=\"Homes\",V17+2%,\"\")","v":0.30000000000000004},{"$f":"IF(proj_RatingSystem=\"Homes\",W17+3%,\"\")","v":0.33000000000000007},0.3600000000000001,0.39000000000000012,0.42000000000000015,0.45000000000000018,0.4800000000000002,0.51000000000000023,0.54000000000000026,0.57000000000000028,{"$f":"IF(proj_RatingSystem=\"Homes\",AF17+3%,MAX(C17:AF17)+4%)","v":0.60000000000000031}]
[null,null,"Y",{"$f":"IF(proj_RatingSystem=\"Healthcare\",3,IF(RatingSystem_IDC=TRUE,4,1))","v":1},{"$f":"IF(RatingSystem_IDC=TRUE,D18+2,D18+1)","v":2},{"$f":"IF(RatingSystem_IDC=TRUE,E18+2,E18+1)","v":3},{"$f":"IF(RatingSystem_IDC=TRUE,F18+2,F18+1)","v":4},{"$f":"G18+1","v":5},6,7,8,9,10,11,12,{"$f":"O18+1","v":13},{"$f":"P18+1","v":14},{"$f":"Q18+1","v":15},{"$f":"R18+1","v":16},{"$f":"IF(proj_RatingSystem=\"Schools - New Construction\",\"\",S18+1)","v":17},{"$f":"IF(proj_RatingSystem=\"Schools - New Construction\",\"\",T18+1)","v":18},{"$f":"IF(OR(proj_RatingSystem=\"Homes\",RatingSystem_IDC=TRUE),U18+1,\"\")","v":19},{"$f":"IF(proj_RatingSystem=\"Homes\",V18+1,\"\")","v":20},21,22,23,24,25,26,27,28,29,{"$f":"IF(proj_RatingSystem=\"Homes\",AF18+1,\"EP\")","v":30}]
[]
[null,null,"Total points documented:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF(AF11>=D17,MIN(MAX(HLOOKUP($AF$11+0.00005,$D$17:$AG$18,2,TRUE)+Homes_Point_Adjustment,0),30),0),\"-\")","v":"-"}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]

{"sheet":"Revision Log","index":46,"n_rows":79,"n_cols":3,"rows_kept":79,"cut":false,"hidden":true,"merged":[[73,0,74,0],[73,1,74,1],[54,1,60,1],[54,0,60,0],[51,1,52,1],[51,0,52,0],[12,1,15,1],[31,0,47,0],[31,1,47,1],[48,1,50,1],[48,0,50,0]]}
["Date","Editor","Change"]
[null,null,"V3.0 released"]
[null,null,"Instructions: Added instructions for activating Macro to Instructions tab"]
[null,null,"3A - Added conditional formatting to highlight input in \"area where prop. lighting must be equal to baseline\" if it is greater than the total area of thermal block"]
[null,null,"3A - Changed conditional formatting in column AN to compare values after rounding"]
[null,null,"3A - Limited decorative allowance to 1 W/SF"]
[null,null,"3A - fixed bug where additional lighting allowance was being double counted"]
[null,null,"3A - adjusted calculations for non-qualified LED fixtures"]
[null,null,"3A - removed \"Remove Fixture\" button to increase robustness of the spreadsheet"]
[null,null,"3C - Added floating tip and changed label for Fixture Wattage to reference NYSERDA default wattages"]
[null,null,"3C - Expanded Legend on include conditional formatting for values that do not meet mandatory code requirements."]
[null,null,"V3A Released"]
[null,"Maria","Added Helpful Hints in Row 10 (General HVAC tab)"]
[null,null,"Added Notes label above the cell at the bottom of the tab (General HVAC tab)"]
[null,null,"Added fourth bullet to Proposed HVAC System Type helpful hints. (General HVAC tab)"]
[null,null,"Expanded helpful hints and tooltips for the Baseline HVAC System Types (General HVAC tab)"]
["2013-08-22","Mike","Demand control ventilation marked with an asterisk in column B of Tab 7"]
["2013-08-23","Mike","Helpful Hints on Tab 7 cell C30 – removed reference to Table 1.4.4, referenced Tab 4 instead"]
[null,null,"V3B Released"]
["2013-10-10","Mike","8 - Revised SHW tab to match simulation guidelines"]
["2015-08-27","Mike","8 - Limited pump power fields on Tab 8 to kW for QC purposes"]
["2015-08-27","Mike","3C - Added non-qualifying LED support for exterior lighting"]
["2015-08-27","Mike","7 - Updated fan power calculator to use average fan motor size instead of total when determining compliance"]
["2015-08-31","Mike","7 - added unitary efficiency and capacity range lookup"]
["2015-08-31","Mike","8 - added baseline boiler and chiller lookup tables"]
["2015-08-31","Mike","9 - added QC tab (new)"]
["2015-09-04","Mike","3A - fixes to conditional formatting to improve performance"]
["2015-09-04","Mike","3A - split classroom space type into OS required and no OS required"]
[null,null,"V3C Released"]
["2016-05-12","Mike/Eva","Updated per ASHRAE 90.1–2013, plus various performance improvements"]
[null,null,"V4 Released"]
["2017-04-05","Nick/Eva/Maria","Column added to tabs to identify ECMs (for example cell O53 of the ‘Shading and Fenestration’ tab)."]
[null,null,"Column added to tabs to show prescriptive requirements of 90.1-2013 applicable to App. G baseline (for example cell N53 of the ‘Shading and Fenestration’ tab)."]
[null,null,"90.1 2010  look-up functionality for the third (prescriptive) column is set up, but currently filled out with the 2013 values as the placeholders. The following tabs must be updated to support LEED 90.1 – 2010 lookups:\n• Envelope Lookup 90.1-2010\n• Lighting Assumptions 90.1-2010\n• HVAC Lookup 90.1-2010"]
[null,null,"Conditional formatting of proposed entries to show if they are better or worse than prescriptive requirements if present (green font if better, red font if worse) and baseline requirements (green cell outline if better, red cell outline if worse)\no ‘Shading and Fenestration’ tab proposed U-values\no ‘Opaque Assemblies’ tab proposed U-values, C-value and F-values\no ‘General Lighting’ Average LPD "]
[null,null,"Added conditional formatting to the PCI in the ‘Performance_Outputs_1’ tab to show green font if better than BPF and red font if worse."]
[null,null,"Added BBUEC, BBREC, BBP, BBF, PCI target and % Improvement beyond code with/without unregulated loads to ‘Performance_Outputs_1’ tab rows 299-305 and 338-344."]
[null,null,"‘Performance_Outputs_1’ tab updates to Quality Assurance Checks:\no Baseline Non-Tradable exterior lighting max cell I358 updated formula to reference correct cells."]
[null,null,"Quality Assurance Checklist moved to new tab named “Quality Assurance Checks’\no Flag in row 14 and 15 formula updated so it would not flag if there was no design exterior lighting.\no Flag in row 27 formula updated so it will not flag if there is no PV in the project.\no Flag in rows 39, 40 and 41 are updated from always being TRUE to include conditional formulas."]
[null,null,"In the ‘Multifamily Details’ tab, the Homes Laundry Room Equipment Calculator (rows 48-59) reported 1.0/0.0 sensible/latent ratio for Clothes dryer commercial gas. This was updated to report 0.10/0.05 to be consistent with EPA HRMF Simulation Guidelines."]
[null,null,"General Information tab VBA Code: Updated the 'Worksheet_Change' Sub to make the General Information tab run smoother. Updates made are marked with \"KC UPDATE:\" followed by what change was made on the line. Updates also made in 'NDInGeneralInformation' sub, and are marked with \"KC UPDATE:\"."]
[null,null,"Results from eQUEST tab table was extended for entire row (this enables users to copy and paste an entire row from the PARMS file rather than making a defined selection). Will make process faster for users. "]
[null,null,"Multiple Building Type capability added in the ‘General Information’ tab row 22-24."]
[null,null,"Moved ‘Opaque Assemblies’ tab after ‘Shading and Fenestration’ so that values from previous tab can be used in the new infiltration calculator (rows 30-38)"]
[null,null,"Updated exterior surface area table in the ‘Shading and Fenestration’ tab (rows 18-32). Made majority of inputs equal to proposed. "]
[null,null,"‘General Lighting’ exterior lighting zone selection added to row 114 for exterior lighting table calculations. "]
[null,null,"‘Service Water Heating’ tab baseline inputs set to lookup values (rows 15-19)."]
[null,null,"‘Air-Side HVAC’ some baseline values updated to be automatic lookups (now white cells). Some overall units in column F now set to automatically populate based on row inputs. "]
["2017-08-22","Eva","Service Water Heater tab Update: Add system now also carried over the formulas but not the text."]
[null,null,"General Lighting tab Update: Exterior Lighting table baseline now references App. G rather than Section 9, and exterior table \"add row\" rows formulas updated to work when new rows are added."]
[null,null,"Updated QC Assurance Checks rows 27, 39-41for formula accuracy"]
["2017-09-11","Eva","Updated General Info BPF reference to keep the year cell constant."]
[null,null,"Updated baseline Air Side Fan Power formula in the Air-Side HVAC tab"]
["2017-09-18","Eva","Multifamily Details tab row 46 sensible and latent equations updated to not show error."]
["2017-11-22","Eva","90.1-2016 COP cooling conversions are added as cell notes to the proposed EER and COP in rows 21 and 22 of the 'Air Side HVAC' tab."]
[null,null,"Updated cells AC38:AC42 to include a delta T calculation for the Hot Water Consumption formula in the 'Service Hot Water' tab."]
[null,null,"Row 68 of the 'Air-Side HVAC' tab baseline BHP formula updated to show value. Previously the value would always show as \"-\"."]
[null,null,"Row 40 and 44 have been added to the 'Opaque Assemblies' tab to include building Volume input and ACH calculation."]
[null,null,"Opaque Assemblies' tab Table 5.1 updated to include 50Pa and 75Pa pressure differential. Instructions row 30 updated, rows 36, 37, 39, 41, 42, and 43 have been added for calculation."]
[null,null,"Cell E12, DHW FLH, of the  'Schedules' tab has been updated to 2,628 hours to be consistent with COMNET."]
[null,null,"Reviewed/updated references to be consistent with 90.1-2016."]
["2017-12-26","Eva","V1.1: Updated Template to allow entering custom site-to-source conversions for different energy sources, and added performance rating calculations based on source energy."]
["2017-12-26",null,"V1.1 Released to EPA"]
["2018-02-01","Eva","V1.2: Number tabs based on the table numbers within tabs.\nAdded 2016 NYS Energy Code ASHRAE 90.1 Appendix G as a Rating System (No multiple buildings, Version of ASHRAE to exceed is 2013, and 2016 BPF's are used.\n\nGeneral Information tab was updated to include new construction and renovation conditioned area and %, as well as above and below grade floors.\nSpace to add simulation program version type is added.\n\"Are there error or warning messages noted in the simulation program output?\" warning added.\n\nEntire workbook in proposed inputs, a space for drawings/specs have been added, as well as area values for some items (for example windows sf area)\n\nPerformance Summary tab added with comparison graphs and QC Checks. The QC Checks at the bottom of the Performance Outputs tab have been hidden.\n\nOpaque Assemblies and Fenestration, unconditioned baseline description and U-values are set to equal the proposed design values. The conditional formatting as updated to allow the proposed design to select a type of each component. On these tabs the initial checks on the top of the tab have been reworded or added/removed.\n\nGeneral Lighting tab OS credits and OS types have been adjusted.\n\nMultifamily Details tab EPD calculations for common equipment have been updated to reflect the quantity.\n\nService Water Heating tab has been adjusted to have automatic calculations.\n\nAir-Side HVAC tab has now been split into two tabs, one for Proposed and one for Baseline. The tab structure has been changed slightly to have a more compact format.\n"]
["2018-03-13","Eva","Updated the exceptional calculations formulas and Table 12.9 of the 12-Performance Outputs 1 tab to be consistent with Add to Proposed (new), Add to Baseline, and Subtract from proposed."]
["2018-04-19","Eva","Updated tab colors and legend on the Instructions tab. All hidden tabs are now red, with the exception of the two blue tabs which Karpman Consulting is using as logs."]
["2018-04-23","Eva","Table 3.6 of the 3-Multifamily Details tab, now includes an input for baseline shower and sink GPMS for the calculations. 2.5 GPM is automatically filled out in the template but can be changed."]
["2018-04-25",null,"V1.2 Submitted the EPA and LEED (but not posted)"]
[null,"Eva","Summary of Recent changes added to the background section of the instructions tab. Title of Instructions tab updated."]
["2018-06-15","Eva","Temperature and humidity control set points and schedules as well as temperature control throttling range are the same for proposed design and baseline building design. (Table G3.1 No 4). Check added to General HVAC tab."]
["2018-06-20","Eva","Background section in Instruction tab is now hidden. "]
[null,null,"V1.2 Submitted to EPA (posted)"]
["2018-08-02","Eva","Added \"restore formula\" buttons to Table 12.4 and 12.6 of the 12 - Performance_Outputs_1 tab."]
["2018-08-02","Eva","Added \"restore formula\" buttons to Table 12.4 and 12.6 of the 12 - Performance_Outputs_1 tab."]
[null,null,"Added P4P - LEED Inputs tab for use of the P4P Program. "]
[null,null,"V1.3 Released to EPA (not posted)"]
["2019-06-03","CML","Fixed the coefficients for gas dryers on the \"Dropdown data\" tab. I also revised the envelope reference values for the baseline and for ASHRAE 2013. Also, modified cells V365:375 on the 12-Performance Outputs tab. Revised LEED instructions on the Instructions tab."]
[null,null,"V1.3 Released to EPA (posted)"]
["2020-04-29","CML","Adjusted the General Information tab so that ASHRAE 90.1-2016 can be selected and such that the 2016 BPFs are used."]

{"sheet":"Version Update Checklist","index":47,"n_rows":11,"n_cols":5,"rows_kept":11,"cut":false,"hidden":true,"merged":[]}
["Version Update Checklist"]
[]
[]
["Version","V1.1","V1.2","V1.3","V1.4"]
["Update Release Date in Instructions Tab","x","x","x","X"]
["Update version number in the file name","x","x","x","X"]
["Add changes made in this version to the Revision Log tab in the template and in the LEED changes word document.","x","x","x","X"]
["Lock the template","x","x","x","X"]
["Save the template so that it opens on the “Instructions” tab.","x","x","x","X"]
["Hide and lock this tab","x","x","x","X"]
["Notes"]

{"sheet":"Rating System Descriptions","index":48,"n_rows":7,"n_cols":4,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[null,"Rating System","BPF","Other"]
[null,"ENERGY STAR MFHR","BPF values are selected based on building type and climate zone.","ES MFHR Rating System Selection triggers EPA specific LPD's, fixture GPM's, DHW baseline system type. Version to exceed of 90.1-2007 is only allowed in this rating system."]
[null,"ECCCNYS ASHRAE Standard 90.1 Appendix G","BPF values are selected based on building type and climate zone per 90.1 2016 Section 4."]
[null,"LEED v4 BD+C: Core and Shell","BPF values are based on the building type average for all climate zones."]

{"sheet":"HVAC Lookup","index":49,"n_rows":58,"n_cols":36,"rows_kept":58,"cut":false,"hidden":true,"merged":[[35,16,35,19],[7,6,8,6],[7,20,8,20],[6,16,6,20],[7,7,8,7],[7,8,8,8],[6,10,6,14],[7,17,8,17],[7,18,8,18],[7,19,8,19],[7,10,7,11],[7,12,8,12],[7,13,8,13],[7,16,8,16],[32,26,34,26],[42,26,44,26],[45,26,49,26],[52,26,54,26],[55,26,57,26]]}
["District Cooling",{"$f":"'General Information'!K61","v":false}]
["District Heating",{"$f":"'General Information'!L61","v":false}]
["ASHRAE 90.1-2010 (Path 1)",{"$f":"'General Information'!K62","v":false},null,null,null,null,null,null,null,null,null,null,null,"Q = fan flow"]
["Full DES (Path 2)",{"$f":"'General Information'!L62","v":false}]
["Streamlined DES (Path 3)",{"$f":"'General Information'!M62","v":false},3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20]
["California Title-24 (Path 4)",{"$f":"'General Information'!N62","v":false}]
[null,null,null,null,null,null,null,null,null,null,"Allowed Fan Power: Power = p x Q + A",null,null,null,null,null,"Motor Horsepower Nominal Efficiency",null,null,null,null,null,null,null,"System ","Equipment type","Size Category","Heating Section Type","Lookup Value","FL Eff",null,"PL Eff","Units",null,"kBtu/h","(British thermal unit per hour) x 1,000"]
["Applicability to Project",{"$f":"IF(AND(C8=FALSE,D8=FALSE,E8=FALSE,F8=FALSE),TRUE,FALSE)","v":true},{"$f":"AND(B1=TRUE,B2=FALSE,OR(B3=TRUE,B5=TRUE))","v":false},{"$f":"AND(B1=FALSE,B2=TRUE,OR(B3=TRUE,B5=TRUE))","v":false},{"$f":"AND(B1=TRUE,B2=TRUE,OR(B3=TRUE,B5=TRUE))","v":false},{"$f":"B6","v":false},"System Number","Project-Specific \nPrimary Systems","Project-Specific \nSecondary System",null,"Fan Power Multiplier (p)",null,"Multiply\nx A","Multiplier \nx Motor Efficiency","Additional fan power for non-mechanical coolling",null,"Motor Horsepower (IP)","Motor \nKilowatts (SI)","Min. Nominal Full-load Efficiency*","Next Motor Size Up HP","Multiplier to convert from input power to allowable fan power",null,null,null,"System 1 - PTAC","PTAC (cooling mode)\nnew construction","All capacities",null,{"$f":"Y8&AA8","v":"System 1 - PTACAll capacities"},"12.5-(0.213*CAP/1000)","EER","-","-",null,"tons","tons"]
["Systems","• No DES\n• ASHRAE 90.1 (Path 1)\n• Full DES (Path 2)","• ASHRAE 90.1 (Path 1)\n• Streamlined DES (Path 3)\n• District Cooling Only","• ASHRAE 90.1 (Path 1)\n• Streamlined DES (Path 3)\n• District Heating Only","• ASHRAE 90.1 (Path 1)\n• Streamlined DES (Path 3)\n• District Cooling and Heating","California Title-24 Baseline default efficiencies (Path 4)",null,null,null,null,"cfm (IP)","L/s (SI)",null,null,"IP",null,null,null,null,null,null,null,null,null,"System 2 - PTHP","PTHP (cooling mode)\nnew construction","All capacities",null,{"$f":"Y9&AA9","v":"System 2 - PTHPAll capacities"},"12.3-(0.213*CAP/1000)","EER","-","-",null,"kW","Kilowatt"]
[{"$f":"IF($C$8=TRUE,C10,IF($D$8=TRUE,D10,IF($E$8=TRUE,E10,IF($F$8=TRUE,F10,B10))))","v":"System 1 - PTAC"},"System 1 - PTAC","System 1 (District Cooling) - 4-pipe CV Fan Coil with HW Boiler","System 1 (District Heating) - PTAC","System 1 (District Heating & Cooling) - 4-pipe CV Fan Coil","Describe the California Title-24 Baseline System Type",1,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A1)),1),\"\")","v":"System 1 - PTAC"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A1)),1),\"\")","v":"System 1 - PTAC"},1,2.9999999999999997E-4,6.4000000000000005E-4,0,0,0,null,0,0,null,{"$f":"S11","v":0.82499999999999996},{"$f":"IF(SI_IP_Units=\"SI\",1/T10,0.746/T10)","v":0.90424242424242429},null,null,null,"System 2 - PTHP","PTHP (cooling mode)\nreplacements","All capacities",null,"System 2 - PTHPAll capacities","12.3-(0.213*CAP/1000)","COP","-","-",null,"Btuh","British thermal unit per hour"]
[{"$f":"IF($C$8=TRUE,C11,IF($D$8=TRUE,D11,IF($E$8=TRUE,E11,IF($F$8=TRUE,F11,B11))))","v":"System 2 - PTHP"},"System 2 - PTHP","System 2 (District Cooling) - 4-pipe CV Fan Coil with HW Boiler",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},2,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A2)),1),\"\")","v":"System 2 - PTHP"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A2)),1),\"\")","v":"System 2 - PTHP"},2,2.9999999999999997E-4,{"$f":"L10/K10*K11","v":6.4000000000000005E-4},0,0,0,null,1,0.8,0.82499999999999996,{"$f":"S12","v":0.84},0.88809523809523816,null,null,null,"System 3 - PSZ-AC","Air conditioners,\nair cooled","<65,000 Btu/h","All","System 3 - PSZ-AC<65,000 Btu/h","-","-",9.6999999999999993,"SEER"]
["System 3 - PSZ-AC","System 3 - PSZ-AC","System 3 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 3 (District Heating) - PSZ-AC with District Heating","System 3 (District Heating & Cooling) - 4-pipe CV AHU",{"$f":"\"\"","v":""},3,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A3)),1),\"\")","v":"System 3 - PSZ-AC"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A3)),1),\"\")","v":"System 3 - PSZ-AC"},3,9.3999999999999997E-4,1.5E-3,1,1,0,null,1.5,1.1000000000000001,0.84,0.84,0.88809523809523816,null,null,null,"System 3 - PSZ-AC",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 3 - PSZ-AC≥65,000 Btu/h and\n<135,000 Btu/h",10.1,"EER","-","IEER"]
["System 4 - PSZ-HP","System 4 - PSZ-HP","System 4 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},4,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A4)),1),\"\")","v":"System 4 - PSZ-HP"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A4)),1),\"\")","v":"System 4 - PSZ-HP"},4,9.3999999999999997E-4,1.5E-3,1,1,0,null,2,1.5,0.84,0.875,0.85257142857142854,null,null,null,"System 3 - PSZ-AC",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 3 - PSZ-AC≥135,000 Btu/h and\n<240,000 Btu/h",9.5,"EER","-","IEER"]
["System 5 - Packaged VAV with Reheat","System 5 - Packaged VAV with Reheat","System 5 (District Cooling) - Change to System 7 - VAV with Reheat","System 5 (District Heating) - Packaged VAV with Reheat","System 5 (District Heating & Cooling) - Change to System 7 - VAV with Reheat",{"$f":"\"\"","v":""},5,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A5)),1),\"\")","v":"System 5 - Packaged VAV with Reheat"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A5)),1),\"\")","v":"System 5 - Packaged VAV with Reheat"},5,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,3,2.2000000000000002,0.875,0.875,0.85257142857142854,null,null,null,"System 3 - PSZ-AC",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 3 - PSZ-AC≥240,000 Btu/h and\n<760,000 Btu/h",9.3000000000000007,"EER",9.4,"IEER"]
["System 6 - Packaged VAV with PFP Boxes","System 6 - Packaged VAV with PFP Boxes","System 6 (District Cooling) - Change to System 8 - VAV with PFP Boxes",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},6,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A6)),1),\"\")","v":"System 6 - Packaged VAV with PFP Boxes"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A6)),1),\"\")","v":"System 6 - Packaged VAV with PFP Boxes"},6,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,5,3.7,0.875,0.89500000000000002,0.83351955307262571,null,null,null,"System 3 - PSZ-AC",null,"≥760,000 Btu/h","All other","System 3 - PSZ-AC≥760,000 Btu/h",9,"EER",9.1,"IEER"]
["System 7 - VAV with Reheat","System 7 - VAV with Reheat","System 7 (District Cooling) - VAV with Reheat","System 7 (District Heating) - VAV with Reheat","System 7 (District Heating & Cooling) - VAV with Reheat",{"$f":"\"\"","v":""},7,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A7)),1),\"\")","v":"System 7 - VAV with Reheat"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A7)),1),\"\")","v":"System 7 - VAV with Reheat"},7,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,7.5,5.6,0.89500000000000002,0.89500000000000002,0.83351955307262571,null,null,null,"System 4 - PSZ-HP","Air cooled\n(cooling mode)","<65,000 Btu/h","All","System 4 - PSZ-HP<65,000 Btu/h","-",null,9.6999999999999993,"SEER"]
["System 8 - VAV with PFP Boxes","System 8 - VAV with PFP Boxes","System 8 (District Cooling) - VAV with PFP Boxes",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},8,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A8)),1),\"\")","v":"System 8 - VAV with PFP Boxes"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A8)),1),\"\")","v":"System 8 - VAV with PFP Boxes"},8,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,10,7.5,0.89500000000000002,0.91,0.81978021978021975,null,null,null,"System 4 - PSZ-HP",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All","System 4 - PSZ-HP≥65,000 Btu/h and\n<135,000 Btu/h",9.9,"EER","-","IEER"]
["System 9 - Heating and Ventilation","System 9 - Heating and Ventilation","System 9 - Heating and Ventilation","System 9 (District Heating) - Heating and Ventilation","System 9 (District Heating) - Heating and Ventilation",{"$f":"\"\"","v":""},9,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A9)),1),\"\")","v":"System 9 - Heating and Ventilation"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A9)),1),\"\")","v":"System 9 - Heating and Ventilation"},9,2.9999999999999997E-4,6.4000000000000005E-4,0,0,1,null,15,11.1,0.91,0.91,0.81978021978021975,null,null,null,"System 4 - PSZ-HP",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All","System 4 - PSZ-HP≥135,000 Btu/h and\n<240,000 Btu/h",9.1,"EER","-","IEER"]
["System 10 - Heating and Ventilation","System 10 - Heating and Ventilation","System 10 - Heating and Ventilation",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},10,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A10)),1),\"\")","v":"System 10 - Heating and Ventilation"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A10)),1),\"\")","v":"System 10 - Heating and Ventilation"},10,2.9999999999999997E-4,6.4000000000000005E-4,0,0,1,null,20,14.9,0.91,0.92400000000000004,0.80735930735930728,null,null,null,"System 4 - PSZ-HP",null,"≥240,000 Btu/h","All","System 4 - PSZ-HP≥240,000 Btu/h",8.8000000000000007,"EER",8.9,"IEER"]
["System 11 - SZ-VAV","System 11 - SZ-VAV","System 11 (District Cooling) - SZ-VAV","System 11 (District Heating) - SZ-VAV","System 11 (District Heating & Cooling) - SZ-VAV",{"$f":"\"\"","v":""},11,{"$f":"A20","v":"System 11 - SZ-VAV"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A11)),1),\"\")","v":"System 11 - SZ-VAV"},11,6.2E-4,{"$f":"L10/K10*K20","v":1.3226666666666669E-3},1,1,0,null,25,18.7,0.92400000000000004,0.92400000000000004,{"$f":"IF(SI_IP_Units=\"SI\",1/T20,0.746/T20)","v":0.80735930735930728},null,null,null,"System 5 - Packaged VAV with Reheat","Air conditioners,\nair cooled","<65,000 Btu/h","All","System 5 - Packaged VAV with Reheat<65,000 Btu/h",9.6999999999999993,"SEER","-","SEER"]
["System 12 - SZ-CV-HW","System 12 - SZ-CV-HW","System 12 (District Cooling) - SZ-CV-HW","System 12 (District Heating) - SZ-CV-HW","System 12 (District Heating & Cooling) - SZ-CV-HW",{"$f":"\"\"","v":""},12,{"$f":"A21","v":"System 12 - SZ-CV-HW"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A12)),1),\"\")","v":"System 12 - SZ-CV-HW"},12,2.9999999999999997E-4,6.4000000000000005E-4,1,1,0,null,30,22.4,0.92400000000000004,0.93,0.80215053763440858,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥65,000 Btu/h and\n<135,000 Btu/h",10.1,"EER","-","IEER"]
["System 13 - SZ-CV-ER","System 13 - SZ-CV-ER","System 13 (District Cooling) - SZ-CV-ER","System 13 (District Heating) - SZ-CV-ER","System 13 (District Heating & Cooling) - SZ-CV-ER",{"$f":"\"\"","v":""},13,{"$f":"A22","v":"System 13 - SZ-CV-ER"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A13)),1),\"\")","v":"System 13 - SZ-CV-ER"},13,2.9999999999999997E-4,6.4000000000000005E-4,1,1,0,null,40,29.8,0.93,0.93,0.80215053763440858,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥135,000 Btu/h and\n<240,000 Btu/h",9.5,"EER","-","IEER"]
[null,null,"System 1 - PTAC","System 1 - PTAC","System 1 - PTAC",{"$f":"\"\"","v":""},1,null,null,null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,0,null,50,37.299999999999997,0.93,0.93600000000000005,0.79700854700854695,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥240,000 Btu/h and\n<760,000 Btu/h",9.3000000000000007,"EER",9.4,"IEER"]
[null,null,"System 2 - PTHP","System 2 - PTHP","System 2 - PTHP",{"$f":"\"\"","v":""},2,null,null,null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,0,null,60,44.8,0.93600000000000005,0.94099999999999995,0.7927736450584485,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥760,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥760,000 Btu/h",9,"EER",9.1,"IEER"]
[null,null,"System 3 - PSZ-AC","System 3 - PSZ-AC","System 3 - PSZ-AC",{"$f":"\"\"","v":""},3,null,null,null,9.3999999999999997E-4,1.5E-3,1,1,0,null,75,56,0.94099999999999995,0.94499999999999995,0.78941798941798946,null,null,null,"System 6 - Packaged VAV with PFP Boxes","Air conditioners,\nair cooled","<65,000 Btu/h","All","System 6 - Packaged VAV with PFP Boxes<65,000 Btu/h","-","-",9.6999999999999993,"SEER"]
[{"$f":"IF($C$8=TRUE,C23,IF($D$8=TRUE,D23,IF($E$8=TRUE,E23,IF($F$8=TRUE,F23,B26))))","v":""},{"$f":"\"\"","v":""},"System 4 - PSZ-HP","System 4 - PSZ-HP","System 4 - PSZ-HP",{"$f":"\"\"","v":""},4,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A14)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A14)),1),\"\")","v":""},null,9.3999999999999997E-4,1.5E-3,1,1,0,null,100,74.599999999999994,0.94499999999999995,0.94499999999999995,0.78941798941798946,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥65,000 Btu/h and\n<135,000 Btu/h",10.1,"EER","-","IEER"]
["",{"$f":"\"\"","v":""},"System 5 - Packaged VAV with Reheat","System 5 - Packaged VAV with Reheat","System 5 - Packaged VAV with Reheat",{"$f":"\"\"","v":""},5,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A15)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A15)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,125,93.3,0.94499999999999995,0.95,0.78526315789473689,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥135,000 Btu/h and\n<240,000 Btu/h",9.5,"EER","-","IEER"]
["",{"$f":"\"\"","v":""},"System 6 - Packaged VAV with PFP Boxes","System 6 - Packaged VAV with PFP Boxes","System 6 - Packaged VAV with PFP Boxes",{"$f":"\"\"","v":""},6,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A16)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A16)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,150,111.9,0.95,0.95,0.78526315789473689,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥240,000 Btu/h and\n<760,000 Btu/h",9.3000000000000007,"EER",9.4,"IEER"]
["",{"$f":"\"\"","v":""},"System 7 - VAV with Reheat","System 7 - VAV with Reheat","System 7 - VAV with Reheat",{"$f":"\"\"","v":""},7,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A17)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A17)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,200,149.19999999999999,0.95,0.95,0.78526315789473689,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥760,000 Btu/h",9,"EER",9.1,"IEER"]
["",{"$f":"\"\"","v":""},"System 8 - VAV with PFP Boxes","System 8 - VAV with PFP Boxes","System 8 - VAV with PFP Boxes",{"$f":"\"\"","v":""},8,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A18)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A18)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,null,null,0.95]
["",{"$f":"\"\"","v":""},null,"System 9 - Heating and Ventilation","System 9 - Heating and Ventilation",{"$f":"\"\"","v":""},9,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A19)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A19)),1),\"\")","v":""},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,1]
["",{"$f":"\"\"","v":""},null,"System 10 - Heating and Ventilation","System 10 - Heating and Ventilation",{"$f":"\"\"","v":""},10,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A20)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A20)),1),\"\")","v":""},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,1,null,null,null,null,null,null,null,null,null,"System ","Equipment type","Size Category","Heating Section Type","Lookup Value","Minimum Efficiency",null,"Size Category"]
[null,null,"System 11 - SZ-VAV","System 11 - SZ-VAV","System 11 - SZ-VAV",null,11,null,null,null,6.2E-4,1.32E-3,1,1,0,null,null,null,null,null,null,null,null,null,"System 1 - PTAC","Boilers, gas fired","N/A",null,{"$f":"Y33&AA33","v":"System 1 - PTACN/A"},0.8,"AFUE","<300,000 Btu/h"]
[null,null,"System 12 - SZ-CV-HW","System 12 - SZ-CV-HW","System 12 - SZ-CV-HW",null,12,null,null,null,2.9999999999999997E-4,6.4000000000000005E-4,1,1,0,null,null,null,null,null,null,null,null,null,"System 1 - PTAC",null,null,null,{"$f":"Y34&AA33","v":"System 1 - PTACN/A"},0.75,"Et","≥300,000 Btu/h and\n≤2,500,000 Btu/h"]
[null,null,"System 13 - SZ-CV-ER","System 13 - SZ-CV-ER","System 13 - SZ-CV-ER",null,13,null,null,null,2.9999999999999997E-4,6.4000000000000005E-4,1,1,0,null,null,null,null,null,null,null,null,null,"System 1 - PTAC",null,null,null,{"$f":"Y35&AA33","v":"System 1 - PTACN/A"},0.8,"Ec",">2,500,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"*Note: Values provided for enclosed motors @ 1800 rpm as specified in ASHRAE 90.1-2016 Appendix G, Section G3.9.1",null,null,null,null,null,null,null,"System 2 - PTHP","PTHP (heating mode)\nnew construction","All capacities",null,{"$f":"Y36&AA36","v":"System 2 - PTHPAll capacities"},"<enter average eff>",null,"All capacities"]
[null,null,"Unitary Cooling","Unitary Heating","No Pressure Adjustment","HeatingOnly","UnitaryHeatingSize","NoEconomizer","SATreset",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 2 - PTHP","PTHP (heating mode)\nreplacements","All capacities",null,"System 2 - PTHPAll capacities","<enter average eff>",null,"All capacities"]
[null,null,"System 1 - PTAC","System 2 - PTHP","System 1 - PTAC","System 9 - Heating and Ventilation","System 3 - PSZ-AC","System 1 - PTAC","System 5 - Packaged VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 3 - PSZ-AC","Warm air furnace, gas-fired","<225,000 Btu/h",null,"System 3 - PSZ-AC<225,000 Btu/h","78% or 80%","AFUE or Et","<225,000 Btu/h"]
[null,null,"System 2 - PTHP","System 3 - PSZ-AC","System 1 (District Cooling) - 4-pipe Fan Coil with HW Boiler","System 10 - Heating and Ventilation","System 4 - PSZ-HP","System 1 (District Cooling) - 4-pipe Fan Coil with HW Boiler","System 5 (District Cooling) - Change to System 7 - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 3 - PSZ-AC","Warm air furnace, gas-fired","≥225,000 Btu/h",null,"System 3 - PSZ-AC≥225,000 Btu/h",0.8,"Ec","≥225,000 Btu/h"]
[null,null,"System 3 - PSZ-AC","System 3 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 1 (District Heating) - PTAC","System 9 (District Heating) - Heating and Ventilation","System 9 - Heating and Ventilation","System 1 (District Heating) - PTAC","System 5 (District Heating) - Packaged VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 4 - PSZ-HP","Electric Heat Pump","<65,000 Btu/h\n(cooling capacity)",null,"System 4 - PSZ-HP<65,000 Btu/h\n(cooling capacity)",6.6,"HSPF","<65,000 Btu/h\n(cooling capacity)"]
[null,null,"System 4 - PSZ-HP","System 4 - PSZ-HP","System 1 (District Heating & Cooling) - 4-pipe Fan Coil",null,"System 10 - Heating and Ventilation","System 1 (District Heating & Cooling) - 4-pipe Fan Coil","System 5 (District Heating & Cooling) - Change to System 7 - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 4 - PSZ-HP",null,"≥65,000 Btu/h and\n<135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air",null,"System 4 - PSZ-HP≥65,000 Btu/h and\n<135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air",3.2,"COP","≥65,000 Btu/h and\n<135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air"]
[null,null,"System 5 - Packaged VAV with Reheat","System 4 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 1 (District Heating) - PTAC",null,"System 3 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 2 - PTHP","System 6 - Packaged VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 4 - PSZ-HP",null,"≥135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air",null,"System 4 - PSZ-HP≥135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air",3.1,"COP","≥135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air"]
[null,null,"System 6 - Packaged VAV with PFP Boxes","System 9 - Heating and Ventilation","System 1 (District Heating & Cooling) - 4-pipe Fan Coil",null,"System 4 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 2 (District Cooling) - 4-pipe Fan Coil with HW Boiler","System 6 (District Cooling) - Change to System 8 - VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 5 - Packaged VAV with Reheat","Boilers, gas fired","N/A",null,{"$f":"Y43&AA43","v":"System 5 - Packaged VAV with ReheatN/A"},0.8,"AFUE","<300,000 Btu/h"]
[null,null,"System 1 (District Heating) - PTAC",null,"System 2 - PTHP",null,null,"System 9 - Heating and Ventilation","System 7 - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 5 - Packaged VAV with Reheat",null,null,null,{"$f":"Y44&AA43","v":"System 5 - Packaged VAV with ReheatN/A"},0.75,"Et","≥300,000 Btu/h and\n≤2,500,000 Btu/h"]
[null,null,"System 3 (District Heating) - PSZ-AC with District Heating",null,"System 2 (District Cooling) - 4-pipe Fan Coil with HW Boiler",null,null,"System 9 - Heating and Ventilation","System 7 (District Cooling) - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 5 - Packaged VAV with Reheat",null,null,null,{"$f":"Y45&AA43","v":"System 5 - Packaged VAV with ReheatN/A"},0.8,"Ec",">2,500,000 Btu/h"]
[null,null,"System 5 (District Heating) - Packaged VAV with Reheat",null,"System 9 - Heating and Ventilation",null,null,"System 9 (District Heating) - Heating and Ventilation","System 7 (District Heating) - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes","Electric Resistance","N/A","All","System 6 - Packaged VAV with PFP BoxesN/A",null,null,"<65,000 Btu/h"]
[null,null,null,null,"System 9 (District Heating) - Heating and Ventilation",null,null,"System 9 (District Heating) - Heating and Ventilation","System 7 (Heating & Cooling) - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,null,"All other",{"$f":"Y47&AA46","v":"System 6 - Packaged VAV with PFP BoxesN/A"},null,null,"≥65,000 Btu/h and\n<135,000 Btu/h"]
[null,null,null,null,"System 10 - Heating and Ventilation",null,null,"System 10 - Heating and Ventilation","System 8 - VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,null,"All other",{"$f":"Y48&AA46","v":"System 6 - Packaged VAV with PFP BoxesN/A"},null,null,"≥135,000 Btu/h and\n<240,000 Btu/h"]
[null,null,null,null,null,null,null,"System 10 - Heating and Ventilation","System 8 (District Cooling)- VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,null,"All other",{"$f":"Y49&AA46","v":"System 6 - Packaged VAV with PFP BoxesN/A"},null,null,"≥240,000 Btu/h and\n<760,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,null,"All other",{"$f":"Y50&AA46","v":"System 6 - Packaged VAV with PFP BoxesN/A"},null,null,"≥760,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 9 - Heating and Ventilation","Warm air furnace, gas-fired","<225,000 Btu/h",null,"System 9 - Heating and Ventilation<225,000 Btu/h","78% or 80%","AFUE or Et","<225,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 9 - Heating and Ventilation","Warm air furnace, gas-fired","≥225,000 Btu/h",null,"System 9 - Heating and Ventilation≥225,000 Btu/h",0.8,"Ec","≥225,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 7 - VAV with Reheat","Boilers, gas fired","N/A",null,{"$f":"Y53&AA53","v":"System 7 - VAV with ReheatN/A"},0.8,"AFUE","<300,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 7 - VAV with Reheat",null,null,null,{"$f":"Y54&AA53","v":"System 7 - VAV with ReheatN/A"},0.75,"Et","≥300,000 Btu/h and\n≤2,500,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 7 - VAV with Reheat",null,null,null,{"$f":"Y55&AA53","v":"System 7 - VAV with ReheatN/A"},0.8,"Ec",">2,500,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 12 - SZ-CV-HW","Boilers, gas fired","N/A",null,"System 12 - SZ-CV-HWN/A",0.8,"AFUE","<300,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 12 - SZ-CV-HW",null,null,null,{"$f":"Y57&AA56","v":"System 12 - SZ-CV-HWN/A"},0.75,"Et","≥300,000 Btu/h and\n≤2,500,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 12 - SZ-CV-HW",null,null,null,{"$f":"Y58&AA56","v":"System 12 - SZ-CV-HWN/A"},0.8,"Ec",">2,500,000 Btu/h"]

{"sheet":"HVAC Lookup 90.1-2007","index":50,"n_rows":58,"n_cols":36,"rows_kept":58,"cut":false,"hidden":true,"merged":[[7,18,8,18],[7,19,8,19],[7,20,8,20],[35,16,35,19],[6,10,6,14],[6,16,6,20],[7,13,8,13],[7,16,8,16],[7,17,8,17],[7,6,8,6],[7,7,8,7],[7,8,8,8],[7,10,7,11],[7,12,8,12]]}
["District Cooling",{"$f":"'General Information'!K61","v":false},"*** THESE ARE NOT 2007 VALUES. THESE TABLES ARE HERE AS A PLACEHOLDER."]
["District Heating",{"$f":"'General Information'!L61","v":false}]
["ASHRAE 90.1-2010 (Path 1)",{"$f":"'General Information'!K62","v":false},null,null,null,null,null,null,null,null,null,null,null,"Q = fan flow"]
["Full DES (Path 2)",{"$f":"'General Information'!L62","v":false}]
["Streamlined DES (Path 3)",{"$f":"'General Information'!M62","v":false},3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20]
["California Title-24 (Path 4)",{"$f":"'General Information'!N62","v":false}]
[null,null,null,null,null,null,null,null,null,null,"Allowed Fan Power: Power = p x Q + A",null,null,null,null,null,"Motor Horsepower Nominal Efficiency",null,null,null,null,null,null,null,"System ","Equipment type","Size Category","Heating Section Type","Lookup Value","FL Eff",null,"PL Eff","Units",null,"kBtu/h","(British thermal unit per hour) x 1,000"]
["Applicability to Project",{"$f":"IF(AND(C8=FALSE,D8=FALSE,E8=FALSE,F8=FALSE),TRUE,FALSE)","v":true},{"$f":"AND(B1=TRUE,B2=FALSE,OR(B3=TRUE,B5=TRUE))","v":false},{"$f":"AND(B1=FALSE,B2=TRUE,OR(B3=TRUE,B5=TRUE))","v":false},{"$f":"AND(B1=TRUE,B2=TRUE,OR(B3=TRUE,B5=TRUE))","v":false},{"$f":"B6","v":false},"System Number","Project-Specific \nPrimary Systems","Project-Specific \nSecondary System",null,"Fan Power Multiplier (p)",null,"Multiply\nx A","Multiplier \nx Motor Efficiency","Additional fan power for non-mechanical coolling",null,"Motor Horsepower (IP)","Motor \nKilowatts (SI)","Min. Nominal Full-load Efficiency*","Next Motor Size Up HP","Multiplier to convert from input power to allowable fan power",null,null,null,"System 1 - PTAC","PTAC (cooling mode)\nnew construction","All capacities",null,{"$f":"Y8&AA8","v":"System 1 - PTACAll capacities"},"14-(0.3*CAP/1000)","EER","-","-",null,"tons","tons"]
["Systems","• No DES\n• ASHRAE 90.1 (Path 1)\n• Full DES (Path 2)","• ASHRAE 90.1 (Path 1)\n• Streamlined DES (Path 3)\n• District Cooling Only","• ASHRAE 90.1 (Path 1)\n• Streamlined DES (Path 3)\n• District Heating Only","• ASHRAE 90.1 (Path 1)\n• Streamlined DES (Path 3)\n• District Cooling and Heating","California Title-24 Baseline default efficiencies (Path 4)",null,null,null,null,"cfm (IP)","L/s (SI)",null,null,"IP",null,null,null,null,null,null,null,null,null,"System 2 - PTHP","PTHP (cooling mode)\nnew construction","All capacities",null,{"$f":"Y9&AA9","v":"System 2 - PTHPAll capacities"},"14-(0.3*CAP/1000)","EER","-","-",null,"kW","Kilowatt"]
[{"$f":"IF($C$8=TRUE,C10,IF($D$8=TRUE,D10,IF($E$8=TRUE,E10,IF($F$8=TRUE,F10,B10))))","v":"System 1 - PTAC"},"System 1 - PTAC","System 1 (District Cooling) - 4-pipe CV Fan Coil with HW Boiler","System 1 (District Heating) - PTAC","System 1 (District Heating & Cooling) - 4-pipe CV Fan Coil","Describe the California Title-24 Baseline System Type",1,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A1)),1),\"\")","v":"System 1 - PTAC"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A1)),1),\"\")","v":"System 1 - PTAC"},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,0,null,0,0,null,0.82499999999999996,{"$f":"IF(SI_IP_Units=\"SI\",1/T10,0.746/T10)","v":0.90424242424242429},null,null,null,"System 2 - PTHP","PTHP (cooling mode)\nreplacements","All capacities",null,"System 2 - PTHPAll capacities","14-(0.3*CAP/1000)","EER","-","-",null,"Btuh","British thermal unit per hour"]
[{"$f":"IF($C$8=TRUE,C11,IF($D$8=TRUE,D11,IF($E$8=TRUE,E11,IF($F$8=TRUE,F11,B11))))","v":"System 2 - PTHP"},"System 2 - PTHP","System 2 (District Cooling) - 4-pipe CV Fan Coil with HW Boiler",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},2,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A2)),1),\"\")","v":"System 2 - PTHP"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A2)),1),\"\")","v":"System 2 - PTHP"},null,2.9999999999999997E-4,{"$f":"L10/K10*K11","v":6.4000000000000005E-4},0,0,0,null,1,0.8,0.82499999999999996,0.84,0.88809523809523816,null,null,null,"System 3 - PSZ-AC","Air conditioners,\nair cooled","<65,000 Btu/h","All","System 3 - PSZ-AC<65,000 Btu/h","-","-",14,"SEER"]
["System 3 - PSZ-AC","System 3 - PSZ-AC","System 3 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 3 (District Heating) - PSZ-AC with District Heating","System 3 (District Heating & Cooling) - 4-pipe CV AHU",{"$f":"\"\"","v":""},3,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A3)),1),\"\")","v":"System 3 - PSZ-AC"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A3)),1),\"\")","v":"System 3 - PSZ-AC"},null,9.3999999999999997E-4,1.5E-3,1,1,0,null,1.5,1.1000000000000001,0.84,0.84,0.88809523809523816,null,null,null,"System 3 - PSZ-AC",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 3 - PSZ-AC≥65,000 Btu/h and\n<135,000 Btu/h",11,"EER",12.7,"IEER"]
["System 4 - PSZ-HP","System 4 - PSZ-HP","System 4 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},4,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A4)),1),\"\")","v":"System 4 - PSZ-HP"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A4)),1),\"\")","v":"System 4 - PSZ-HP"},null,9.3999999999999997E-4,1.5E-3,1,1,0,null,2,1.5,0.84,0.875,0.85257142857142854,null,null,null,"System 3 - PSZ-AC",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 3 - PSZ-AC≥135,000 Btu/h and\n<240,000 Btu/h",10.8,"EER",12.2,"IEER"]
["System 5 - Packaged VAV with Reheat","System 5 - Packaged VAV with Reheat","System 5 (District Cooling) - Change to System 7 - VAV with Reheat","System 5 (District Heating) - Packaged VAV with Reheat","System 5 (District Heating & Cooling) - Change to System 7 - VAV with Reheat",{"$f":"\"\"","v":""},5,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A5)),1),\"\")","v":"System 5 - Packaged VAV with Reheat"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A5)),1),\"\")","v":"System 5 - Packaged VAV with Reheat"},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,3,2.2000000000000002,0.86499999999999999,0.875,0.85257142857142854,null,null,null,"System 3 - PSZ-AC",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 3 - PSZ-AC≥240,000 Btu/h and\n<760,000 Btu/h",9.8000000000000007,"EER",11.4,"IEER"]
["System 6 - Packaged VAV with PFP Boxes","System 6 - Packaged VAV with PFP Boxes","System 6 (District Cooling) - Change to System 8 - VAV with PFP Boxes",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},6,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A6)),1),\"\")","v":"System 6 - Packaged VAV with PFP Boxes"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A6)),1),\"\")","v":"System 6 - Packaged VAV with PFP Boxes"},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,5,3.7,0.875,0.89500000000000002,0.83351955307262571,null,null,null,"System 3 - PSZ-AC",null,"≥760,000 Btu/h","All other","System 3 - PSZ-AC≥760,000 Btu/h",9.5,"EER",11,"IEER"]
["System 7 - VAV with Reheat","System 7 - VAV with Reheat","System 7 (District Cooling) - VAV with Reheat","System 7 (District Heating) - VAV with Reheat","System 7 (District Heating & Cooling) - VAV with Reheat",{"$f":"\"\"","v":""},7,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A7)),1),\"\")","v":"System 7 - VAV with Reheat"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A7)),1),\"\")","v":"System 7 - VAV with Reheat"},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,7.5,5.6,0.88500000000000001,0.89500000000000002,0.83351955307262571,null,null,null,"System 4 - PSZ-HP","Air cooled\n(cooling mode)","<65,000 Btu/h","All","System 4 - PSZ-HP<65,000 Btu/h","-","-",14,"SEER"]
["System 8 - VAV with PFP Boxes","System 8 - VAV with PFP Boxes","System 8 (District Cooling) - VAV with PFP Boxes",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},8,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A8)),1),\"\")","v":"System 8 - VAV with PFP Boxes"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A8)),1),\"\")","v":"System 8 - VAV with PFP Boxes"},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,10,7.5,0.89500000000000002,0.91,0.81978021978021975,null,null,null,"System 4 - PSZ-HP",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All","System 4 - PSZ-HP≥65,000 Btu/h and\n<135,000 Btu/h",10.8,"EER",12,"IEER"]
["System 9 - Heating and Ventilation","System 9 - Heating and Ventilation","System 9 - Heating and Ventilation","System 9 (District Heating) - Heating and Ventilation","System 9 (District Heating) - Heating and Ventilation",{"$f":"\"\"","v":""},9,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A9)),1),\"\")","v":"System 9 - Heating and Ventilation"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A9)),1),\"\")","v":"System 9 - Heating and Ventilation"},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,5.3999999999999998E-5,null,15,11.1,0.91,0.91,0.81978021978021975,null,null,null,"System 4 - PSZ-HP",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All","System 4 - PSZ-HP≥135,000 Btu/h and\n<240,000 Btu/h",10.4,"EER",11.4,"IEER"]
["System 10 - Heating and Ventilation","System 10 - Heating and Ventilation","System 10 - Heating and Ventilation",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},10,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A10)),1),\"\")","v":"System 10 - Heating and Ventilation"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A10)),1),\"\")","v":"System 10 - Heating and Ventilation"},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,5.3999999999999998E-5,null,20,14.9,0.91,0.92400000000000004,0.80735930735930728,null,null,null,"System 4 - PSZ-HP",null,"≥240,000 Btu/h","All","System 4 - PSZ-HP≥240,000 Btu/h",9.3000000000000007,"EER",0.4,"IEER"]
["System 11 - SZ-VAV","System 11 - SZ-VAV","System 11 (District Cooling) - SZ-VAV","System 11 (District Heating) - SZ-VAV","System 11 (District Heating & Cooling) - SZ-VAV",{"$f":"\"\"","v":""},11,{"$f":"A20","v":"System 11 - SZ-VAV"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A11)),1),\"\")","v":"System 11 - SZ-VAV"},null,6.2E-4,1.3226666666666669E-3,1,1,0,null,25,18.7,0.91700000000000004,0.92400000000000004,0.80735930735930728,null,null,null,"System 5 - Packaged VAV with Reheat","Air conditioners,\nair cooled","<65,000 Btu/h","All","System 5 - Packaged VAV with Reheat<65,000 Btu/h","-","-",14,"SEER"]
["System 12 - SZ-CV-HW","System 12 - SZ-CV-HW","System 12 (District Cooling) - SZ-CV-HW","System 12 (District Heating) - SZ-CV-HW","System 12 (District Heating & Cooling) - SZ-CV-HW",{"$f":"\"\"","v":""},12,{"$f":"A21","v":"System 12 - SZ-CV-HW"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A12)),1),\"\")","v":"System 12 - SZ-CV-HW"},null,9.3999999999999997E-4,2.0053333333333338E-3,1,1,0,null,30,22.4,0.92400000000000004,0.93,0.80215053763440858,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥65,000 Btu/h and\n<135,000 Btu/h",11,"EER",12.7,"IEER"]
["System 13 - SZ-CV-ER","System 13 - SZ-CV-ER","System 13 (District Cooling) - SZ-CV-ER","System 13 (District Heating) - SZ-CV-ER","System 13 (District Heating & Cooling) - SZ-CV-ER",{"$f":"\"\"","v":""},13,{"$f":"A22","v":"System 13 - SZ-CV-ER"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A13)),1),\"\")","v":"System 13 - SZ-CV-ER"},null,9.3999999999999997E-4,2.0053333333333338E-3,1,1,0,null,40,29.8,0.93,0.93,0.80215053763440858,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥135,000 Btu/h and\n<240,000 Btu/h",10.8,"EER",12.2,"IEER"]
[null,null,"System 1 - PTAC","System 1 - PTAC","System 1 - PTAC",{"$f":"\"\"","v":""},1,null,null,null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,0,null,50,37.299999999999997,0.93,0.93600000000000005,0.79700854700854695,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥240,000 Btu/h and\n<760,000 Btu/h",9.8000000000000007,"EER",11.4,"IEER"]
[null,null,"System 2 - PTHP","System 2 - PTHP","System 2 - PTHP",{"$f":"\"\"","v":""},2,null,null,null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,0,null,60,44.8,0.93600000000000005,0.94099999999999995,0.7927736450584485,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥760,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥760,000 Btu/h",9.5,"EER",11,"IEER"]
[null,null,"System 3 - PSZ-AC","System 3 - PSZ-AC","System 3 - PSZ-AC",{"$f":"\"\"","v":""},3,null,null,null,9.3999999999999997E-4,1.5E-3,1,1,0,null,75,56,0.94099999999999995,0.94499999999999995,0.78941798941798946,null,null,null,"System 6 - Packaged VAV with PFP Boxes","Air conditioners,\nair cooled","<65,000 Btu/h","All","System 6 - Packaged VAV with PFP Boxes<65,000 Btu/h","-","-",13,"SEER"]
[{"$f":"IF($C$8=TRUE,C23,IF($D$8=TRUE,D23,IF($E$8=TRUE,E23,IF($F$8=TRUE,F23,B26))))","v":""},{"$f":"\"\"","v":""},"System 4 - PSZ-HP","System 4 - PSZ-HP","System 4 - PSZ-HP",{"$f":"\"\"","v":""},4,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A14)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A14)),1),\"\")","v":""},null,9.3999999999999997E-4,1.5E-3,1,1,0,null,100,74.599999999999994,0.94099999999999995,0.94499999999999995,0.78941798941798946,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥65,000 Btu/h and\n<135,000 Btu/h",11.2,"EER",12.9,"IEER"]
["",{"$f":"\"\"","v":""},"System 5 - Packaged VAV with Reheat","System 5 - Packaged VAV with Reheat","System 5 - Packaged VAV with Reheat",{"$f":"\"\"","v":""},5,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A15)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A15)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,125,93.3,0.94499999999999995,0.95,0.78526315789473689,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥135,000 Btu/h and\n<240,000 Btu/h",11,"EER",12.4,"IEER"]
["",{"$f":"\"\"","v":""},"System 6 - Packaged VAV with PFP Boxes","System 6 - Packaged VAV with PFP Boxes","System 6 - Packaged VAV with PFP Boxes",{"$f":"\"\"","v":""},6,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A16)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A16)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,150,111.9,0.95,0.95,0.78526315789473689,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥240,000 Btu/h and\n<760,000 Btu/h",10,"EER",11.6,"IEER"]
["",{"$f":"\"\"","v":""},"System 7 - VAV with Reheat","System 7 - VAV with Reheat","System 7 - VAV with Reheat",{"$f":"\"\"","v":""},7,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A17)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A17)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,200,149.19999999999999,0.95,0.95,0.78526315789473689,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥760,000 Btu/h",9.6999999999999993,"EER",11.2,"IEER"]
["",{"$f":"\"\"","v":""},"System 8 - VAV with PFP Boxes","System 8 - VAV with PFP Boxes","System 8 - VAV with PFP Boxes",{"$f":"\"\"","v":""},8,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A18)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A18)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0]
["",{"$f":"\"\"","v":""},null,"System 9 - Heating and Ventilation","System 9 - Heating and Ventilation",{"$f":"\"\"","v":""},9,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A19)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A19)),1),\"\")","v":""},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,5.3999999999999998E-5]
["",{"$f":"\"\"","v":""},null,"System 10 - Heating and Ventilation","System 10 - Heating and Ventilation",{"$f":"\"\"","v":""},10,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A20)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A20)),1),\"\")","v":""},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,5.3999999999999998E-5,null,null,null,null,null,null,null,null,null,"System ","Equipment type","Size Category","Heating Section Type","Lookup Value","Minimum Efficiency"]
[null,null,"System 11 - SZ-VAV","System 11 - SZ-VAV","System 11 - SZ-VAV",null,11,null,null,null,6.2E-4,1.3226666666666669E-3,1,1,0,null,null,null,null,null,null,null,null,null,"System 1 - PTAC","Boilers, gas fired","<300,000 Btu/h",null,{"$f":"Y33&AA33","v":"System 1 - PTAC<300,000 Btu/h"},"82% AFUE"]
[null,null,"System 12 - SZ-CV-HW","System 12 - SZ-CV-HW","System 12 - SZ-CV-HW",null,12,null,null,null,9.3999999999999997E-4,2.0053333333333338E-3,1,1,0,null,null,null,null,null,null,null,null,null,"System 1 - PTAC",null,"≥300,000 Btu/h and\n≤2,500,000 Btu/h",null,{"$f":"Y34&AA34","v":"System 1 - PTAC≥300,000 Btu/h and\n≤2,500,000 Btu/h"},"80% Et"]
[null,null,"System 13 - SZ-CV-ER","System 13 - SZ-CV-ER","System 13 - SZ-CV-ER",null,13,null,null,null,9.3999999999999997E-4,2.0053333333333338E-3,1,1,0,null,null,null,null,null,null,null,null,null,"System 1 - PTAC",null,">2,500,000 Btu/h",null,{"$f":"Y35&AA35","v":"System 1 - PTAC>2,500,000 Btu/h"},"82% Ec"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"*Note: Values provided for enclosed motors @ 1800 rpm as specified in ASHRAE 90.1-2013 Appendix G, Section G3.1.2.9",null,null,null,null,null,null,null,"System 2 - PTHP","PTHP (heating mode)\nnew construction","All capacities",null,{"$f":"Y36&AA36","v":"System 2 - PTHPAll capacities"},"<enter average eff>"]
[null,null,"Unitary Cooling","Unitary Heating","No Pressure Adjustment","HeatingOnly","UnitaryHeatingSize","NoEconomizer","SATreset",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 2 - PTHP","PTHP (heating mode)\nreplacements","All capacities",null,"System 2 - PTHPAll capacities","<enter average eff>"]
[null,null,"System 1 - PTAC","System 2 - PTHP","System 1 - PTAC","System 9 - Heating and Ventilation","System 3 - PSZ-AC","System 1 - PTAC","System 5 - Packaged VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 3 - PSZ-AC","Warm air furnace, gas-fired","<225,000 Btu/h",null,"System 3 - PSZ-AC<225,000 Btu/h","78% AFUE or 80% Et"]
[null,null,"System 2 - PTHP","System 3 - PSZ-AC","System 1 (District Cooling) - 4-pipe Fan Coil with HW Boiler","System 10 - Heating and Ventilation","System 4 - PSZ-HP","System 1 (District Cooling) - 4-pipe Fan Coil with HW Boiler","System 5 (District Cooling) - Change to System 7 - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 3 - PSZ-AC","Warm air furnace, gas-fired","≥225,000 Btu/h",null,"System 3 - PSZ-AC≥225,000 Btu/h","80 %Ec"]
[null,null,"System 3 - PSZ-AC","System 3 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 1 (District Heating) - PTAC","System 9 (District Heating) - Heating and Ventilation","System 9 - Heating and Ventilation","System 1 (District Heating) - PTAC","System 5 (District Heating) - Packaged VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 4 - PSZ-HP","Electric Heat Pump","<65,000 Btu/h\n(cooling capacity)",null,"System 4 - PSZ-HP<65,000 Btu/h\n(cooling capacity)","6.6 HSPF"]
[null,null,"System 4 - PSZ-HP","System 4 - PSZ-HP","System 1 (District Heating & Cooling) - 4-pipe Fan Coil",null,"System 10 - Heating and Ventilation","System 1 (District Heating & Cooling) - 4-pipe Fan Coil","System 5 (District Heating & Cooling) - Change to System 7 - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 4 - PSZ-HP",null,"≥65,000 Btu/h and\n<135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air",null,"System 4 - PSZ-HP≥65,000 Btu/h and\n<135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air","3.2 COP"]
[null,null,"System 5 - Packaged VAV with Reheat","System 4 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 1 (District Heating) - PTAC",null,"System 3 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 2 - PTHP","System 6 - Packaged VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 4 - PSZ-HP",null,"≥135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air",null,"System 4 - PSZ-HP≥135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air","3.1 COP"]
[null,null,"System 6 - Packaged VAV with PFP Boxes","System 9 - Heating and Ventilation","System 1 (District Heating & Cooling) - 4-pipe Fan Coil",null,"System 4 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 2 (District Cooling) - 4-pipe Fan Coil with HW Boiler","System 6 (District Cooling) - Change to System 8 - VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 5 - Packaged VAV with Reheat","Boilers, gas fired","<300,000 Btu/h",null,"System 5 - Packaged VAV with Reheat<300,000 Btu/h","82% AFUE"]
[null,null,"System 1 (District Heating) - PTAC",null,"System 2 - PTHP",null,null,"System 9 - Heating and Ventilation","System 7 - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥300,000 Btu/h and\n≤2,500,000 Btu/h",null,"System 5 - Packaged VAV with Reheat≥300,000 Btu/h and\n≤2,500,000 Btu/h","80% Et"]
[null,null,"System 3 (District Heating) - PSZ-AC with District Heating",null,"System 2 (District Cooling) - 4-pipe Fan Coil with HW Boiler",null,null,"System 9 - Heating and Ventilation","System 7 (District Cooling) - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 5 - Packaged VAV with Reheat",null,">2,500,000 Btu/h",null,"System 5 - Packaged VAV with Reheat>2,500,000 Btu/h","82% Ec"]
[null,null,"System 5 (District Heating) - Packaged VAV with Reheat",null,"System 9 - Heating and Ventilation",null,null,"System 9 (District Heating) - Heating and Ventilation","System 7 (District Heating) - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes","Electric Resistance","<65,000 Btu/h","All","System 6 - Packaged VAV with PFP Boxes<65,000 Btu/h"]
[null,null,null,null,"System 9 (District Heating) - Heating and Ventilation",null,null,"System 9 (District Heating) - Heating and Ventilation","System 7 (Heating & Cooling) - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥65,000 Btu/h and\n<135,000 Btu/h"]
[null,null,null,null,"System 10 - Heating and Ventilation",null,null,"System 10 - Heating and Ventilation","System 8 - VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥135,000 Btu/h and\n<240,000 Btu/h"]
[null,null,null,null,null,null,null,"System 10 - Heating and Ventilation","System 8 (District Cooling)- VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥240,000 Btu/h and\n<760,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥760,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 9 - Heating and Ventilation","Warm air furnace, gas-fired","<225,000 Btu/h",null,"System 9 - Heating and Ventilation<225,000 Btu/h","78% AFUE or 80% Et"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 9 - Heating and Ventilation","Warm air furnace, gas-fired","≥225,000 Btu/h",null,"System 9 - Heating and Ventilation≥225,000 Btu/h","80 %Ec"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 7 - VAV with Reheat","Boilers, gas fired","<300,000 Btu/h",null,"System 7 - VAV with Reheat<300,000 Btu/h","82% AFUE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 7 - VAV with Reheat",null,"≥300,000 Btu/h and\n≤2,500,000 Btu/h",null,"System 7 - VAV with Reheat≥300,000 Btu/h and\n≤2,500,000 Btu/h","80% Et"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 7 - VAV with Reheat",null,">2,500,000 Btu/h",null,"System 7 - VAV with Reheat>2,500,000 Btu/h","82% Ec"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 12 - SZ-CV-HW","Boilers, gas fired","<300,000 Btu/h",null,"System 12 - SZ-CV-HW<300,000 Btu/h","82% AFUE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 12 - SZ-CV-HW",null,"≥300,000 Btu/h and\n≤2,500,000 Btu/h",null,"System 12 - SZ-CV-HW≥300,000 Btu/h and\n≤2,500,000 Btu/h","80% Et"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 12 - SZ-CV-HW",null,">2,500,000 Btu/h",null,"System 12 - SZ-CV-HW>2,500,000 Btu/h","82% Ec"]

{"sheet":"HVAC Lookup 90.1-2013","index":51,"n_rows":58,"n_cols":36,"rows_kept":58,"cut":false,"hidden":true,"merged":[[7,18,8,18],[7,19,8,19],[7,20,8,20],[35,16,35,19],[6,10,6,14],[6,16,6,20],[7,13,8,13],[7,16,8,16],[7,17,8,17],[7,6,8,6],[7,7,8,7],[7,8,8,8],[7,10,7,11],[7,12,8,12]]}
["District Cooling",{"$f":"'General Information'!K61","v":false}]
["District Heating",{"$f":"'General Information'!L61","v":false}]
["ASHRAE 90.1-2010 (Path 1)",{"$f":"'General Information'!K62","v":false},null,null,null,null,null,null,null,null,null,null,null,"Q = fan flow"]
["Full DES (Path 2)",{"$f":"'General Information'!L62","v":false}]
["Streamlined DES (Path 3)",{"$f":"'General Information'!M62","v":false},3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20]
["California Title-24 (Path 4)",{"$f":"'General Information'!N62","v":false}]
[null,null,null,null,null,null,null,null,null,null,"Allowed Fan Power: Power = p x Q + A",null,null,null,null,null,"Motor Horsepower Nominal Efficiency",null,null,null,null,null,null,null,"System ","Equipment type","Size Category","Heating Section Type","Lookup Value","FL Eff",null,"PL Eff","Units",null,"kBtu/h","(British thermal unit per hour) x 1,000"]
["Applicability to Project",{"$f":"IF(AND(C8=FALSE,D8=FALSE,E8=FALSE,F8=FALSE),TRUE,FALSE)","v":true},{"$f":"AND(B1=TRUE,B2=FALSE,OR(B3=TRUE,B5=TRUE))","v":false},{"$f":"AND(B1=FALSE,B2=TRUE,OR(B3=TRUE,B5=TRUE))","v":false},{"$f":"AND(B1=TRUE,B2=TRUE,OR(B3=TRUE,B5=TRUE))","v":false},{"$f":"B6","v":false},"System Number","Project-Specific \nPrimary Systems","Project-Specific \nSecondary System",null,"Fan Power Multiplier (p)",null,"Multiply\nx A","Multiplier \nx Motor Efficiency","Additional fan power for non-mechanical coolling",null,"Motor Horsepower (IP)","Motor \nKilowatts (SI)","Min. Nominal Full-load Efficiency*","Next Motor Size Up HP","Multiplier to convert from input power to allowable fan power",null,null,null,"System 1 - PTAC","PTAC (cooling mode)\nnew construction","All capacities",null,{"$f":"Y8&AA8","v":"System 1 - PTACAll capacities"},"14-(0.3*CAP/1000)","EER","-","-",null,"tons","tons"]
["Systems","• No DES\n• ASHRAE 90.1 (Path 1)\n• Full DES (Path 2)","• ASHRAE 90.1 (Path 1)\n• Streamlined DES (Path 3)\n• District Cooling Only","• ASHRAE 90.1 (Path 1)\n• Streamlined DES (Path 3)\n• District Heating Only","• ASHRAE 90.1 (Path 1)\n• Streamlined DES (Path 3)\n• District Cooling and Heating","California Title-24 Baseline default efficiencies (Path 4)",null,null,null,null,"cfm (IP)","L/s (SI)",null,null,"IP",null,null,null,null,null,null,null,null,null,"System 2 - PTHP","PTHP (cooling mode)\nnew construction","All capacities",null,{"$f":"Y9&AA9","v":"System 2 - PTHPAll capacities"},"14-(0.3*CAP/1000)","EER","-","-",null,"kW","Kilowatt"]
[{"$f":"IF($C$8=TRUE,C10,IF($D$8=TRUE,D10,IF($E$8=TRUE,E10,IF($F$8=TRUE,F10,B10))))","v":"System 1 - PTAC"},"System 1 - PTAC","System 1 (District Cooling) - 4-pipe CV Fan Coil with HW Boiler","System 1 (District Heating) - PTAC","System 1 (District Heating & Cooling) - 4-pipe CV Fan Coil","Describe the California Title-24 Baseline System Type",1,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A1)),1),\"\")","v":"System 1 - PTAC"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A1)),1),\"\")","v":"System 1 - PTAC"},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,0,null,0,0,null,0.82499999999999996,{"$f":"IF(SI_IP_Units=\"SI\",1/T10,0.746/T10)","v":0.90424242424242429},null,null,null,"System 2 - PTHP","PTHP (cooling mode)\nreplacements","All capacities",null,"System 2 - PTHPAll capacities","14-(0.3*CAP/1000)","EER","-","-",null,"Btuh","British thermal unit per hour"]
[{"$f":"IF($C$8=TRUE,C11,IF($D$8=TRUE,D11,IF($E$8=TRUE,E11,IF($F$8=TRUE,F11,B11))))","v":"System 2 - PTHP"},"System 2 - PTHP","System 2 (District Cooling) - 4-pipe CV Fan Coil with HW Boiler",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},2,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A2)),1),\"\")","v":"System 2 - PTHP"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A2)),1),\"\")","v":"System 2 - PTHP"},null,2.9999999999999997E-4,{"$f":"L10/K10*K11","v":6.4000000000000005E-4},0,0,0,null,1,0.8,0.82499999999999996,0.84,0.88809523809523816,null,null,null,"System 3 - PSZ-AC","Air conditioners,\nair cooled","<65,000 Btu/h","All","System 3 - PSZ-AC<65,000 Btu/h","-","-",14,"SEER"]
["System 3 - PSZ-AC","System 3 - PSZ-AC","System 3 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 3 (District Heating) - PSZ-AC with District Heating","System 3 (District Heating & Cooling) - 4-pipe CV AHU",{"$f":"\"\"","v":""},3,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A3)),1),\"\")","v":"System 3 - PSZ-AC"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A3)),1),\"\")","v":"System 3 - PSZ-AC"},null,9.3999999999999997E-4,1.5E-3,1,1,0,null,1.5,1.1000000000000001,0.84,0.84,0.88809523809523816,null,null,null,"System 3 - PSZ-AC",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 3 - PSZ-AC≥65,000 Btu/h and\n<135,000 Btu/h",11,"EER",12.7,"IEER"]
["System 4 - PSZ-HP","System 4 - PSZ-HP","System 4 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},4,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A4)),1),\"\")","v":"System 4 - PSZ-HP"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A4)),1),\"\")","v":"System 4 - PSZ-HP"},null,9.3999999999999997E-4,1.5E-3,1,1,0,null,2,1.5,0.84,0.875,0.85257142857142854,null,null,null,"System 3 - PSZ-AC",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 3 - PSZ-AC≥135,000 Btu/h and\n<240,000 Btu/h",10.8,"EER",12.2,"IEER"]
["System 5 - Packaged VAV with Reheat","System 5 - Packaged VAV with Reheat","System 5 (District Cooling) - Change to System 7 - VAV with Reheat","System 5 (District Heating) - Packaged VAV with Reheat","System 5 (District Heating & Cooling) - Change to System 7 - VAV with Reheat",{"$f":"\"\"","v":""},5,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A5)),1),\"\")","v":"System 5 - Packaged VAV with Reheat"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A5)),1),\"\")","v":"System 5 - Packaged VAV with Reheat"},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,3,2.2000000000000002,0.86499999999999999,0.875,0.85257142857142854,null,null,null,"System 3 - PSZ-AC",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 3 - PSZ-AC≥240,000 Btu/h and\n<760,000 Btu/h",9.8000000000000007,"EER",11.4,"IEER"]
["System 6 - Packaged VAV with PFP Boxes","System 6 - Packaged VAV with PFP Boxes","System 6 (District Cooling) - Change to System 8 - VAV with PFP Boxes",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},6,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A6)),1),\"\")","v":"System 6 - Packaged VAV with PFP Boxes"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A6)),1),\"\")","v":"System 6 - Packaged VAV with PFP Boxes"},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,5,3.7,0.875,0.89500000000000002,0.83351955307262571,null,null,null,"System 3 - PSZ-AC",null,"≥760,000 Btu/h","All other","System 3 - PSZ-AC≥760,000 Btu/h",9.5,"EER",11,"IEER"]
["System 7 - VAV with Reheat","System 7 - VAV with Reheat","System 7 (District Cooling) - VAV with Reheat","System 7 (District Heating) - VAV with Reheat","System 7 (District Heating & Cooling) - VAV with Reheat",{"$f":"\"\"","v":""},7,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A7)),1),\"\")","v":"System 7 - VAV with Reheat"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A7)),1),\"\")","v":"System 7 - VAV with Reheat"},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,7.5,5.6,0.88500000000000001,0.89500000000000002,0.83351955307262571,null,null,null,"System 4 - PSZ-HP","Air cooled\n(cooling mode)","<65,000 Btu/h","All","System 4 - PSZ-HP<65,000 Btu/h","-","-",14,"SEER"]
["System 8 - VAV with PFP Boxes","System 8 - VAV with PFP Boxes","System 8 (District Cooling) - VAV with PFP Boxes",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},8,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A8)),1),\"\")","v":"System 8 - VAV with PFP Boxes"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A8)),1),\"\")","v":"System 8 - VAV with PFP Boxes"},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,10,7.5,0.89500000000000002,0.91,0.81978021978021975,null,null,null,"System 4 - PSZ-HP",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All","System 4 - PSZ-HP≥65,000 Btu/h and\n<135,000 Btu/h",10.8,"EER",12,"IEER"]
["System 9 - Heating and Ventilation","System 9 - Heating and Ventilation","System 9 - Heating and Ventilation","System 9 (District Heating) - Heating and Ventilation","System 9 (District Heating) - Heating and Ventilation",{"$f":"\"\"","v":""},9,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A9)),1),\"\")","v":"System 9 - Heating and Ventilation"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A9)),1),\"\")","v":"System 9 - Heating and Ventilation"},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,5.3999999999999998E-5,null,15,11.1,0.91,0.91,0.81978021978021975,null,null,null,"System 4 - PSZ-HP",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All","System 4 - PSZ-HP≥135,000 Btu/h and\n<240,000 Btu/h",10.4,"EER",11.4,"IEER"]
["System 10 - Heating and Ventilation","System 10 - Heating and Ventilation","System 10 - Heating and Ventilation",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},10,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A10)),1),\"\")","v":"System 10 - Heating and Ventilation"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A10)),1),\"\")","v":"System 10 - Heating and Ventilation"},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,5.3999999999999998E-5,null,20,14.9,0.91,0.92400000000000004,0.80735930735930728,null,null,null,"System 4 - PSZ-HP",null,"≥240,000 Btu/h","All","System 4 - PSZ-HP≥240,000 Btu/h",9.3000000000000007,"EER",0.4,"IEER"]
["System 11 - SZ-VAV","System 11 - SZ-VAV","System 11 (District Cooling) - SZ-VAV","System 11 (District Heating) - SZ-VAV","System 11 (District Heating & Cooling) - SZ-VAV",{"$f":"\"\"","v":""},11,{"$f":"A20","v":"System 11 - SZ-VAV"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A11)),1),\"\")","v":"System 11 - SZ-VAV"},null,6.2E-4,1.3226666666666669E-3,1,1,0,null,25,18.7,0.91700000000000004,0.92400000000000004,0.80735930735930728,null,null,null,"System 5 - Packaged VAV with Reheat","Air conditioners,\nair cooled","<65,000 Btu/h","All","System 5 - Packaged VAV with Reheat<65,000 Btu/h","-","-",14,"SEER"]
["System 12 - SZ-CV-HW","System 12 - SZ-CV-HW","System 12 (District Cooling) - SZ-CV-HW","System 12 (District Heating) - SZ-CV-HW","System 12 (District Heating & Cooling) - SZ-CV-HW",{"$f":"\"\"","v":""},12,{"$f":"A21","v":"System 12 - SZ-CV-HW"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A12)),1),\"\")","v":"System 12 - SZ-CV-HW"},null,9.3999999999999997E-4,2.0053333333333338E-3,1,1,0,null,30,22.4,0.92400000000000004,0.93,0.80215053763440858,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥65,000 Btu/h and\n<135,000 Btu/h",11,"EER",12.7,"IEER"]
["System 13 - SZ-CV-ER","System 13 - SZ-CV-ER","System 13 (District Cooling) - SZ-CV-ER","System 13 (District Heating) - SZ-CV-ER","System 13 (District Heating & Cooling) - SZ-CV-ER",{"$f":"\"\"","v":""},13,{"$f":"A22","v":"System 13 - SZ-CV-ER"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A13)),1),\"\")","v":"System 13 - SZ-CV-ER"},null,9.3999999999999997E-4,2.0053333333333338E-3,1,1,0,null,40,29.8,0.93,0.93,0.80215053763440858,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥135,000 Btu/h and\n<240,000 Btu/h",10.8,"EER",12.2,"IEER"]
[null,null,"System 1 - PTAC","System 1 - PTAC","System 1 - PTAC",{"$f":"\"\"","v":""},1,null,null,null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,0,null,50,37.299999999999997,0.93,0.93600000000000005,0.79700854700854695,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥240,000 Btu/h and\n<760,000 Btu/h",9.8000000000000007,"EER",11.4,"IEER"]
[null,null,"System 2 - PTHP","System 2 - PTHP","System 2 - PTHP",{"$f":"\"\"","v":""},2,null,null,null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,0,null,60,44.8,0.93600000000000005,0.94099999999999995,0.7927736450584485,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥760,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥760,000 Btu/h",9.5,"EER",11,"IEER"]
[null,null,"System 3 - PSZ-AC","System 3 - PSZ-AC","System 3 - PSZ-AC",{"$f":"\"\"","v":""},3,null,null,null,9.3999999999999997E-4,1.5E-3,1,1,0,null,75,56,0.94099999999999995,0.94499999999999995,0.78941798941798946,null,null,null,"System 6 - Packaged VAV with PFP Boxes","Air conditioners,\nair cooled","<65,000 Btu/h","All","System 6 - Packaged VAV with PFP Boxes<65,000 Btu/h","-","-",13,"SEER"]
[{"$f":"IF($C$8=TRUE,C23,IF($D$8=TRUE,D23,IF($E$8=TRUE,E23,IF($F$8=TRUE,F23,B26))))","v":""},{"$f":"\"\"","v":""},"System 4 - PSZ-HP","System 4 - PSZ-HP","System 4 - PSZ-HP",{"$f":"\"\"","v":""},4,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A14)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A14)),1),\"\")","v":""},null,9.3999999999999997E-4,1.5E-3,1,1,0,null,100,74.599999999999994,0.94099999999999995,0.94499999999999995,0.78941798941798946,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥65,000 Btu/h and\n<135,000 Btu/h",11.2,"EER",12.9,"IEER"]
["",{"$f":"\"\"","v":""},"System 5 - Packaged VAV with Reheat","System 5 - Packaged VAV with Reheat","System 5 - Packaged VAV with Reheat",{"$f":"\"\"","v":""},5,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A15)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A15)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,125,93.3,0.94499999999999995,0.95,0.78526315789473689,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥135,000 Btu/h and\n<240,000 Btu/h",11,"EER",12.4,"IEER"]
["",{"$f":"\"\"","v":""},"System 6 - Packaged VAV with PFP Boxes","System 6 - Packaged VAV with PFP Boxes","System 6 - Packaged VAV with PFP Boxes",{"$f":"\"\"","v":""},6,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A16)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A16)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,150,111.9,0.95,0.95,0.78526315789473689,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥240,000 Btu/h and\n<760,000 Btu/h",10,"EER",11.6,"IEER"]
["",{"$f":"\"\"","v":""},"System 7 - VAV with Reheat","System 7 - VAV with Reheat","System 7 - VAV with Reheat",{"$f":"\"\"","v":""},7,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A17)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A17)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,200,149.19999999999999,0.95,0.95,0.78526315789473689,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥760,000 Btu/h",9.6999999999999993,"EER",11.2,"IEER"]
["",{"$f":"\"\"","v":""},"System 8 - VAV with PFP Boxes","System 8 - VAV with PFP Boxes","System 8 - VAV with PFP Boxes",{"$f":"\"\"","v":""},8,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A18)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A18)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0]
["",{"$f":"\"\"","v":""},null,"System 9 - Heating and Ventilation","System 9 - Heating and Ventilation",{"$f":"\"\"","v":""},9,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A19)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A19)),1),\"\")","v":""},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,5.3999999999999998E-5]
["",{"$f":"\"\"","v":""},null,"System 10 - Heating and Ventilation","System 10 - Heating and Ventilation",{"$f":"\"\"","v":""},10,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A20)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A20)),1),\"\")","v":""},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,5.3999999999999998E-5,null,null,null,null,null,null,null,null,null,"System ","Equipment type","Size Category","Heating Section Type","Lookup Value","Minimum Efficiency"]
[null,null,"System 11 - SZ-VAV","System 11 - SZ-VAV","System 11 - SZ-VAV",null,11,null,null,null,6.2E-4,1.3226666666666669E-3,1,1,0,null,null,null,null,null,null,null,null,null,"System 1 - PTAC","Boilers, gas fired","<300,000 Btu/h",null,{"$f":"Y33&AA33","v":"System 1 - PTAC<300,000 Btu/h"},"82% AFUE"]
[null,null,"System 12 - SZ-CV-HW","System 12 - SZ-CV-HW","System 12 - SZ-CV-HW",null,12,null,null,null,9.3999999999999997E-4,2.0053333333333338E-3,1,1,0,null,null,null,null,null,null,null,null,null,"System 1 - PTAC",null,"≥300,000 Btu/h and\n≤2,500,000 Btu/h",null,{"$f":"Y34&AA34","v":"System 1 - PTAC≥300,000 Btu/h and\n≤2,500,000 Btu/h"},"80% Et"]
[null,null,"System 13 - SZ-CV-ER","System 13 - SZ-CV-ER","System 13 - SZ-CV-ER",null,13,null,null,null,9.3999999999999997E-4,2.0053333333333338E-3,1,1,0,null,null,null,null,null,null,null,null,null,"System 1 - PTAC",null,">2,500,000 Btu/h",null,{"$f":"Y35&AA35","v":"System 1 - PTAC>2,500,000 Btu/h"},"82% Ec"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"*Note: Values provided for enclosed motors @ 1800 rpm as specified in ASHRAE 90.1-2013 Appendix G, Section G3.1.2.9",null,null,null,null,null,null,null,"System 2 - PTHP","PTHP (heating mode)\nnew construction","All capacities",null,{"$f":"Y36&AA36","v":"System 2 - PTHPAll capacities"},"<enter average eff>"]
[null,null,"Unitary Cooling","Unitary Heating","No Pressure Adjustment","HeatingOnly","UnitaryHeatingSize","NoEconomizer","SATreset",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 2 - PTHP","PTHP (heating mode)\nreplacements","All capacities",null,"System 2 - PTHPAll capacities","<enter average eff>"]
[null,null,"System 1 - PTAC","System 2 - PTHP","System 1 - PTAC","System 9 - Heating and Ventilation","System 3 - PSZ-AC","System 1 - PTAC","System 5 - Packaged VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 3 - PSZ-AC","Warm air furnace, gas-fired","<225,000 Btu/h",null,"System 3 - PSZ-AC<225,000 Btu/h","78% AFUE or 80% Et"]
[null,null,"System 2 - PTHP","System 3 - PSZ-AC","System 1 (District Cooling) - 4-pipe Fan Coil with HW Boiler","System 10 - Heating and Ventilation","System 4 - PSZ-HP","System 1 (District Cooling) - 4-pipe Fan Coil with HW Boiler","System 5 (District Cooling) - Change to System 7 - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 3 - PSZ-AC","Warm air furnace, gas-fired","≥225,000 Btu/h",null,"System 3 - PSZ-AC≥225,000 Btu/h","80 %Ec"]
[null,null,"System 3 - PSZ-AC","System 3 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 1 (District Heating) - PTAC","System 9 (District Heating) - Heating and Ventilation","System 9 - Heating and Ventilation","System 1 (District Heating) - PTAC","System 5 (District Heating) - Packaged VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 4 - PSZ-HP","Electric Heat Pump","<65,000 Btu/h\n(cooling capacity)",null,"System 4 - PSZ-HP<65,000 Btu/h\n(cooling capacity)","6.6 HSPF"]
[null,null,"System 4 - PSZ-HP","System 4 - PSZ-HP","System 1 (District Heating & Cooling) - 4-pipe Fan Coil",null,"System 10 - Heating and Ventilation","System 1 (District Heating & Cooling) - 4-pipe Fan Coil","System 5 (District Heating & Cooling) - Change to System 7 - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 4 - PSZ-HP",null,"≥65,000 Btu/h and\n<135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air",null,"System 4 - PSZ-HP≥65,000 Btu/h and\n<135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air","3.2 COP"]
[null,null,"System 5 - Packaged VAV with Reheat","System 4 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 1 (District Heating) - PTAC",null,"System 3 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 2 - PTHP","System 6 - Packaged VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 4 - PSZ-HP",null,"≥135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air",null,"System 4 - PSZ-HP≥135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air","3.1 COP"]
[null,null,"System 6 - Packaged VAV with PFP Boxes","System 9 - Heating and Ventilation","System 1 (District Heating & Cooling) - 4-pipe Fan Coil",null,"System 4 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 2 (District Cooling) - 4-pipe Fan Coil with HW Boiler","System 6 (District Cooling) - Change to System 8 - VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 5 - Packaged VAV with Reheat","Boilers, gas fired","<300,000 Btu/h",null,{"$f":"Y43&AA43","v":"System 5 - Packaged VAV with Reheat<300,000 Btu/h"},"82% AFUE"]
[null,null,"System 1 (District Heating) - PTAC",null,"System 2 - PTHP",null,null,"System 9 - Heating and Ventilation","System 7 - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥300,000 Btu/h and\n≤2,500,000 Btu/h",null,"System 5 - Packaged VAV with Reheat≥300,000 Btu/h and\n≤2,500,000 Btu/h","80% Et"]
[null,null,"System 3 (District Heating) - PSZ-AC with District Heating",null,"System 2 (District Cooling) - 4-pipe Fan Coil with HW Boiler",null,null,"System 9 - Heating and Ventilation","System 7 (District Cooling) - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 5 - Packaged VAV with Reheat",null,">2,500,000 Btu/h",null,"System 5 - Packaged VAV with Reheat>2,500,000 Btu/h","82% Ec"]
[null,null,"System 5 (District Heating) - Packaged VAV with Reheat",null,"System 9 - Heating and Ventilation",null,null,"System 9 (District Heating) - Heating and Ventilation","System 7 (District Heating) - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes","Electric Resistance","<65,000 Btu/h","All","System 6 - Packaged VAV with PFP Boxes<65,000 Btu/h"]
[null,null,null,null,"System 9 (District Heating) - Heating and Ventilation",null,null,"System 9 (District Heating) - Heating and Ventilation","System 7 (Heating & Cooling) - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥65,000 Btu/h and\n<135,000 Btu/h"]
[null,null,null,null,"System 10 - Heating and Ventilation",null,null,"System 10 - Heating and Ventilation","System 8 - VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥135,000 Btu/h and\n<240,000 Btu/h"]
[null,null,null,null,null,null,null,"System 10 - Heating and Ventilation","System 8 (District Cooling)- VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥240,000 Btu/h and\n<760,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥760,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 9 - Heating and Ventilation","Warm air furnace, gas-fired","<225,000 Btu/h",null,"System 9 - Heating and Ventilation<225,000 Btu/h","78% AFUE or 80% Et"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 9 - Heating and Ventilation","Warm air furnace, gas-fired","≥225,000 Btu/h",null,"System 9 - Heating and Ventilation≥225,000 Btu/h","80 %Ec"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 7 - VAV with Reheat","Boilers, gas fired","<300,000 Btu/h",null,"System 7 - VAV with Reheat<300,000 Btu/h","82% AFUE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 7 - VAV with Reheat",null,"≥300,000 Btu/h and\n≤2,500,000 Btu/h",null,"System 7 - VAV with Reheat≥300,000 Btu/h and\n≤2,500,000 Btu/h","80% Et"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 7 - VAV with Reheat",null,">2,500,000 Btu/h",null,"System 7 - VAV with Reheat>2,500,000 Btu/h","82% Ec"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 12 - SZ-CV-HW","Boilers, gas fired","<300,000 Btu/h",null,"System 12 - SZ-CV-HW<300,000 Btu/h","82% AFUE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 12 - SZ-CV-HW",null,"≥300,000 Btu/h and\n≤2,500,000 Btu/h",null,"System 12 - SZ-CV-HW≥300,000 Btu/h and\n≤2,500,000 Btu/h","80% Et"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 12 - SZ-CV-HW",null,">2,500,000 Btu/h",null,"System 12 - SZ-CV-HW>2,500,000 Btu/h","82% Ec"]

{"sheet":"HVAC Lookup 90.1-2010","index":52,"n_rows":58,"n_cols":36,"rows_kept":58,"cut":false,"hidden":true,"merged":[[7,18,8,18],[7,19,8,19],[7,20,8,20],[35,16,35,19],[6,10,6,14],[6,16,6,20],[7,13,8,13],[7,16,8,16],[7,17,8,17],[7,6,8,6],[7,7,8,7],[7,8,8,8],[7,10,7,11],[7,12,8,12]]}
["District Cooling",{"$f":"'General Information'!K61","v":false}]
["District Heating",{"$f":"'General Information'!L61","v":false}]
["ASHRAE 90.1-2010 (Path 1)",{"$f":"'General Information'!K62","v":false},null,null,null,null,null,null,null,null,null,null,null,"Q = fan flow"]
["Full DES (Path 2)",{"$f":"'General Information'!L62","v":false}]
["Streamlined DES (Path 3)",{"$f":"'General Information'!M62","v":false},3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20]
["California Title-24 (Path 4)",{"$f":"'General Information'!N62","v":false}]
[null,null,null,null,null,null,null,null,null,null,"Allowed Fan Power: Power = p x Q + A",null,null,null,null,null,"Motor Horsepower Nominal Efficiency",null,null,null,null,null,null,null,"System ","Equipment type","Size Category","Heating Section Type","Lookup Value","FL Eff",null,"PL Eff","Units",null,"kBtu/h","(British thermal unit per hour) x 1,000"]
["Applicability to Project",{"$f":"IF(AND(C8=FALSE,D8=FALSE,E8=FALSE,F8=FALSE),TRUE,FALSE)","v":true},{"$f":"AND(B1=TRUE,B2=FALSE,OR(B3=TRUE,B5=TRUE))","v":false},{"$f":"AND(B1=FALSE,B2=TRUE,OR(B3=TRUE,B5=TRUE))","v":false},{"$f":"AND(B1=TRUE,B2=TRUE,OR(B3=TRUE,B5=TRUE))","v":false},{"$f":"B6","v":false},"System Number","Project-Specific \nPrimary Systems","Project-Specific \nSecondary System",null,"Fan Power Multiplier (p)",null,"Multiply\nx A","Multiplier \nx Motor Efficiency","Additional fan power for non-mechanical coolling",null,"Motor Horsepower (IP)","Motor \nKilowatts (SI)","Min. Nominal Full-load Efficiency*","Next Motor Size Up HP","Multiplier to convert from input power to allowable fan power",null,null,null,"System 1 - PTAC","PTAC (cooling mode)\nnew construction","All capacities",null,{"$f":"Y8&AA8","v":"System 1 - PTACAll capacities"},"13.8-(0.3*CAP/1000)","EER","-","EER",null,"tons","tons"]
["Systems","• No DES\n• ASHRAE 90.1 (Path 1)\n• Full DES (Path 2)","• ASHRAE 90.1 (Path 1)\n• Streamlined DES (Path 3)\n• District Cooling Only","• ASHRAE 90.1 (Path 1)\n• Streamlined DES (Path 3)\n• District Heating Only","• ASHRAE 90.1 (Path 1)\n• Streamlined DES (Path 3)\n• District Cooling and Heating","California Title-24 Baseline default efficiencies (Path 4)",null,null,null,null,"cfm (IP)","L/s (SI)",null,null,"IP",null,null,null,null,null,null,null,null,null,"System 2 - PTHP","PTHP (cooling mode)\nnew construction","All capacities",null,{"$f":"Y9&AA9","v":"System 2 - PTHPAll capacities"},"14-(0.3*CAP/1000)","EER","-","EER",null,"kW","Kilowatt"]
[{"$f":"IF($C$8=TRUE,C10,IF($D$8=TRUE,D10,IF($E$8=TRUE,E10,IF($F$8=TRUE,F10,B10))))","v":"System 1 - PTAC"},"System 1 - PTAC","System 1 (District Cooling) - 4-pipe CV Fan Coil with HW Boiler","System 1 (District Heating) - PTAC","System 1 (District Heating & Cooling) - 4-pipe CV Fan Coil","Describe the California Title-24 Baseline System Type",1,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A1)),1),\"\")","v":"System 1 - PTAC"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A1)),1),\"\")","v":"System 1 - PTAC"},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,0,null,0,0,null,0.82499999999999996,{"$f":"IF(SI_IP_Units=\"SI\",1/T10,0.746/T10)","v":0.90424242424242429},null,null,null,"System 2 - PTHP","PTHP (cooling mode)\nreplacements","All capacities",null,"System 2 - PTHPAll capacities","14-(0.3*CAP/1000)","EER","-","EER",null,"Btuh","British thermal unit per hour"]
[{"$f":"IF($C$8=TRUE,C11,IF($D$8=TRUE,D11,IF($E$8=TRUE,E11,IF($F$8=TRUE,F11,B11))))","v":"System 2 - PTHP"},"System 2 - PTHP","System 2 (District Cooling) - 4-pipe CV Fan Coil with HW Boiler",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},2,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A2)),1),\"\")","v":"System 2 - PTHP"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A2)),1),\"\")","v":"System 2 - PTHP"},null,2.9999999999999997E-4,{"$f":"L10/K10*K11","v":6.4000000000000005E-4},0,0,0,null,1,0.8,0.82499999999999996,0.84,0.88809523809523816,null,null,null,"System 3 - PSZ-AC","Air conditioners,\nair cooled","<65,000 Btu/h","All","System 3 - PSZ-AC<65,000 Btu/h","-","-",14,"SEER"]
["System 3 - PSZ-AC","System 3 - PSZ-AC","System 3 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 3 (District Heating) - PSZ-AC with District Heating","System 3 (District Heating & Cooling) - 4-pipe CV AHU",{"$f":"\"\"","v":""},3,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A3)),1),\"\")","v":"System 3 - PSZ-AC"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A3)),1),\"\")","v":"System 3 - PSZ-AC"},null,9.3999999999999997E-4,1.5E-3,1,1,0,null,1.5,1.1000000000000001,0.84,0.84,0.88809523809523816,null,null,null,"System 3 - PSZ-AC",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 3 - PSZ-AC≥65,000 Btu/h and\n<135,000 Btu/h",11,"EER",12.7,"IEER"]
["System 4 - PSZ-HP","System 4 - PSZ-HP","System 4 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},4,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A4)),1),\"\")","v":"System 4 - PSZ-HP"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A4)),1),\"\")","v":"System 4 - PSZ-HP"},null,9.3999999999999997E-4,1.5E-3,1,1,0,null,2,1.5,0.84,0.875,0.85257142857142854,null,null,null,"System 3 - PSZ-AC",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 3 - PSZ-AC≥135,000 Btu/h and\n<240,000 Btu/h",10.8,"EER",12.2,"IEER"]
["System 5 - Packaged VAV with Reheat","System 5 - Packaged VAV with Reheat","System 5 (District Cooling) - Change to System 7 - VAV with Reheat","System 5 (District Heating) - Packaged VAV with Reheat","System 5 (District Heating & Cooling) - Change to System 7 - VAV with Reheat",{"$f":"\"\"","v":""},5,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A5)),1),\"\")","v":"System 5 - Packaged VAV with Reheat"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A5)),1),\"\")","v":"System 5 - Packaged VAV with Reheat"},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,3,2.2000000000000002,0.86499999999999999,0.875,0.85257142857142854,null,null,null,"System 3 - PSZ-AC",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 3 - PSZ-AC≥240,000 Btu/h and\n<760,000 Btu/h",9.8000000000000007,"EER",11.4,"IEER"]
["System 6 - Packaged VAV with PFP Boxes","System 6 - Packaged VAV with PFP Boxes","System 6 (District Cooling) - Change to System 8 - VAV with PFP Boxes",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},6,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A6)),1),\"\")","v":"System 6 - Packaged VAV with PFP Boxes"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A6)),1),\"\")","v":"System 6 - Packaged VAV with PFP Boxes"},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,5,3.7,0.875,0.89500000000000002,0.83351955307262571,null,null,null,"System 3 - PSZ-AC",null,"≥760,000 Btu/h","All other","System 3 - PSZ-AC≥760,000 Btu/h",9.5,"EER",11,"IEER"]
["System 7 - VAV with Reheat","System 7 - VAV with Reheat","System 7 (District Cooling) - VAV with Reheat","System 7 (District Heating) - VAV with Reheat","System 7 (District Heating & Cooling) - VAV with Reheat",{"$f":"\"\"","v":""},7,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A7)),1),\"\")","v":"System 7 - VAV with Reheat"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A7)),1),\"\")","v":"System 7 - VAV with Reheat"},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,7.5,5.6,0.88500000000000001,0.89500000000000002,0.83351955307262571,null,null,null,"System 4 - PSZ-HP","Air cooled\n(cooling mode)","<65,000 Btu/h","All","System 4 - PSZ-HP<65,000 Btu/h","-","-",14,"SEER"]
["System 8 - VAV with PFP Boxes","System 8 - VAV with PFP Boxes","System 8 (District Cooling) - VAV with PFP Boxes",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},8,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A8)),1),\"\")","v":"System 8 - VAV with PFP Boxes"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A8)),1),\"\")","v":"System 8 - VAV with PFP Boxes"},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,10,7.5,0.89500000000000002,0.91,0.81978021978021975,null,null,null,"System 4 - PSZ-HP",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All","System 4 - PSZ-HP≥65,000 Btu/h and\n<135,000 Btu/h",10.8,"EER",12,"IEER"]
["System 9 - Heating and Ventilation","System 9 - Heating and Ventilation","System 9 - Heating and Ventilation","System 9 (District Heating) - Heating and Ventilation","System 9 (District Heating) - Heating and Ventilation",{"$f":"\"\"","v":""},9,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A9)),1),\"\")","v":"System 9 - Heating and Ventilation"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A9)),1),\"\")","v":"System 9 - Heating and Ventilation"},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,5.3999999999999998E-5,null,15,11.1,0.91,0.91,0.81978021978021975,null,null,null,"System 4 - PSZ-HP",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All","System 4 - PSZ-HP≥135,000 Btu/h and\n<240,000 Btu/h",10.4,"EER",11.4,"IEER"]
["System 10 - Heating and Ventilation","System 10 - Heating and Ventilation","System 10 - Heating and Ventilation",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},10,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A10)),1),\"\")","v":"System 10 - Heating and Ventilation"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A10)),1),\"\")","v":"System 10 - Heating and Ventilation"},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,5.3999999999999998E-5,null,20,14.9,0.91,0.92400000000000004,0.80735930735930728,null,null,null,"System 4 - PSZ-HP",null,"≥240,000 Btu/h","All","System 4 - PSZ-HP≥240,000 Btu/h",9.3000000000000007,"EER",0.4,"IEER"]
["System 11 - SZ-VAV","System 11 - SZ-VAV","System 11 (District Cooling) - SZ-VAV","System 11 (District Heating) - SZ-VAV","System 11 (District Heating & Cooling) - SZ-VAV",{"$f":"\"\"","v":""},11,{"$f":"A20","v":"System 11 - SZ-VAV"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A11)),1),\"\")","v":"System 11 - SZ-VAV"},null,6.2E-4,1.3226666666666669E-3,1,1,0,null,25,18.7,0.91700000000000004,0.92400000000000004,0.80735930735930728,null,null,null,"System 5 - Packaged VAV with Reheat","Air conditioners,\nair cooled","<65,000 Btu/h","All","System 5 - Packaged VAV with Reheat<65,000 Btu/h","-","-",14,"SEER"]
["System 12 - SZ-CV-HW","System 12 - SZ-CV-HW","System 12 (District Cooling) - SZ-CV-HW","System 12 (District Heating) - SZ-CV-HW","System 12 (District Heating & Cooling) - SZ-CV-HW",{"$f":"\"\"","v":""},12,{"$f":"A21","v":"System 12 - SZ-CV-HW"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A12)),1),\"\")","v":"System 12 - SZ-CV-HW"},null,9.3999999999999997E-4,2.0053333333333338E-3,1,1,0,null,30,22.4,0.92400000000000004,0.93,0.80215053763440858,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥65,000 Btu/h and\n<135,000 Btu/h",11,"EER",12.7,"IEER"]
["System 13 - SZ-CV-ER","System 13 - SZ-CV-ER","System 13 (District Cooling) - SZ-CV-ER","System 13 (District Heating) - SZ-CV-ER","System 13 (District Heating & Cooling) - SZ-CV-ER",{"$f":"\"\"","v":""},13,{"$f":"A22","v":"System 13 - SZ-CV-ER"},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A13)),1),\"\")","v":"System 13 - SZ-CV-ER"},null,9.3999999999999997E-4,2.0053333333333338E-3,1,1,0,null,40,29.8,0.93,0.93,0.80215053763440858,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥135,000 Btu/h and\n<240,000 Btu/h",10.8,"EER",12.2,"IEER"]
[null,null,"System 1 - PTAC","System 1 - PTAC","System 1 - PTAC",{"$f":"\"\"","v":""},1,null,null,null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,0,null,50,37.299999999999997,0.93,0.93600000000000005,0.79700854700854695,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥240,000 Btu/h and\n<760,000 Btu/h",9.8000000000000007,"EER",11.4,"IEER"]
[null,null,"System 2 - PTHP","System 2 - PTHP","System 2 - PTHP",{"$f":"\"\"","v":""},2,null,null,null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,0,null,60,44.8,0.93600000000000005,0.94099999999999995,0.7927736450584485,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥760,000 Btu/h","All other","System 5 - Packaged VAV with Reheat≥760,000 Btu/h",9.5,"EER",11,"IEER"]
[null,null,"System 3 - PSZ-AC","System 3 - PSZ-AC","System 3 - PSZ-AC",{"$f":"\"\"","v":""},3,null,null,null,9.3999999999999997E-4,1.5E-3,1,1,0,null,75,56,0.94099999999999995,0.94499999999999995,0.78941798941798946,null,null,null,"System 6 - Packaged VAV with PFP Boxes","Air conditioners,\nair cooled","<65,000 Btu/h","All","System 6 - Packaged VAV with PFP Boxes<65,000 Btu/h","-","-",13,"SEER"]
[{"$f":"IF($C$8=TRUE,C23,IF($D$8=TRUE,D23,IF($E$8=TRUE,E23,IF($F$8=TRUE,F23,B26))))","v":""},{"$f":"\"\"","v":""},"System 4 - PSZ-HP","System 4 - PSZ-HP","System 4 - PSZ-HP",{"$f":"\"\"","v":""},4,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A14)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A14)),1),\"\")","v":""},null,9.3999999999999997E-4,1.5E-3,1,1,0,null,100,74.599999999999994,0.94099999999999995,0.94499999999999995,0.78941798941798946,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥65,000 Btu/h and\n<135,000 Btu/h",11.2,"EER",12.9,"IEER"]
["",{"$f":"\"\"","v":""},"System 5 - Packaged VAV with Reheat","System 5 - Packaged VAV with Reheat","System 5 - Packaged VAV with Reheat",{"$f":"\"\"","v":""},5,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A15)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A15)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,125,93.3,0.94499999999999995,0.95,0.78526315789473689,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥135,000 Btu/h and\n<240,000 Btu/h",11,"EER",12.4,"IEER"]
["",{"$f":"\"\"","v":""},"System 6 - Packaged VAV with PFP Boxes","System 6 - Packaged VAV with PFP Boxes","System 6 - Packaged VAV with PFP Boxes",{"$f":"\"\"","v":""},6,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A16)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A16)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,150,111.9,0.95,0.95,0.78526315789473689,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥240,000 Btu/h and\n<760,000 Btu/h",10,"EER",11.6,"IEER"]
["",{"$f":"\"\"","v":""},"System 7 - VAV with Reheat","System 7 - VAV with Reheat","System 7 - VAV with Reheat",{"$f":"\"\"","v":""},7,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A17)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A17)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0,null,200,149.19999999999999,0.95,0.95,0.78526315789473689,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥760,000 Btu/h",9.6999999999999993,"EER",11.2,"IEER"]
["",{"$f":"\"\"","v":""},"System 8 - VAV with PFP Boxes","System 8 - VAV with PFP Boxes","System 8 - VAV with PFP Boxes",{"$f":"\"\"","v":""},8,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A18)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A18)),1),\"\")","v":""},null,1.2999999999999999E-3,2.0999999999999999E-3,1,1,0]
["",{"$f":"\"\"","v":""},null,"System 9 - Heating and Ventilation","System 9 - Heating and Ventilation",{"$f":"\"\"","v":""},9,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A19)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A19)),1),\"\")","v":""},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,5.3999999999999998E-5]
["",{"$f":"\"\"","v":""},null,"System 10 - Heating and Ventilation","System 10 - Heating and Ventilation",{"$f":"\"\"","v":""},10,{"$f":"IFERROR(INDEX($A$10:$A$19,SMALL((IF(LEN($A$10:$A$19),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$19))))),ROW(A20)),1),\"\")","v":""},{"$f":"IFERROR(INDEX($A$10:$A$32,SMALL((IF(LEN($A$10:$A$32),ROW(INDIRECT(\"1:\"&ROWS($A$10:$A$32))))),ROW(A20)),1),\"\")","v":""},null,2.9999999999999997E-4,6.4000000000000005E-4,0,0,5.3999999999999998E-5,null,null,null,null,null,null,null,null,null,"System ","Equipment type","Size Category","Heating Section Type","Lookup Value","Minimum Efficiency"]
[null,null,"System 11 - SZ-VAV","System 11 - SZ-VAV","System 11 - SZ-VAV",null,11,null,null,null,6.2E-4,1.3226666666666669E-3,1,1,0,null,null,null,null,null,null,null,null,null,"System 1 - PTAC","Boilers, gas fired","<300,000 Btu/h",null,{"$f":"Y33&AA33","v":"System 1 - PTAC<300,000 Btu/h"},"82% AFUE"]
[null,null,"System 12 - SZ-CV-HW","System 12 - SZ-CV-HW","System 12 - SZ-CV-HW",null,12,null,null,null,9.3999999999999997E-4,2.0053333333333338E-3,1,1,0,null,null,null,null,null,null,null,null,null,"System 1 - PTAC",null,"≥300,000 Btu/h and\n≤2,500,000 Btu/h",null,{"$f":"Y34&AA34","v":"System 1 - PTAC≥300,000 Btu/h and\n≤2,500,000 Btu/h"},"80% Et"]
[null,null,"System 13 - SZ-CV-ER","System 13 - SZ-CV-ER","System 13 - SZ-CV-ER",null,13,null,null,null,9.3999999999999997E-4,2.0053333333333338E-3,1,1,0,null,null,null,null,null,null,null,null,null,"System 1 - PTAC",null,">2,500,000 Btu/h",null,{"$f":"Y35&AA35","v":"System 1 - PTAC>2,500,000 Btu/h"},"82% Ec"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"*Note: Values provided for enclosed motors @ 1800 rpm as specified in ASHRAE 90.1-2013 Appendix G, Section G3.1.2.9",null,null,null,null,null,null,null,"System 2 - PTHP","PTHP (heating mode)\nnew construction","All capacities",null,{"$f":"Y36&AA36","v":"System 2 - PTHPAll capacities"},"<enter average eff>"]
[null,null,"Unitary Cooling","Unitary Heating","No Pressure Adjustment","HeatingOnly","UnitaryHeatingSize","NoEconomizer","SATreset",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 2 - PTHP","PTHP (heating mode)\nreplacements","All capacities",null,"System 2 - PTHPAll capacities","<enter average eff>"]
[null,null,"System 1 - PTAC","System 2 - PTHP","System 1 - PTAC","System 9 - Heating and Ventilation","System 3 - PSZ-AC","System 1 - PTAC","System 5 - Packaged VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 3 - PSZ-AC","Warm air furnace, gas-fired","<225,000 Btu/h",null,"System 3 - PSZ-AC<225,000 Btu/h","78% AFUE or 80% Et"]
[null,null,"System 2 - PTHP","System 3 - PSZ-AC","System 1 (District Cooling) - 4-pipe Fan Coil with HW Boiler","System 10 - Heating and Ventilation","System 4 - PSZ-HP","System 1 (District Cooling) - 4-pipe Fan Coil with HW Boiler","System 5 (District Cooling) - Change to System 7 - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 3 - PSZ-AC","Warm air furnace, gas-fired","≥225,000 Btu/h",null,"System 3 - PSZ-AC≥225,000 Btu/h","80 %Ec"]
[null,null,"System 3 - PSZ-AC","System 3 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 1 (District Heating) - PTAC","System 9 (District Heating) - Heating and Ventilation","System 9 - Heating and Ventilation","System 1 (District Heating) - PTAC","System 5 (District Heating) - Packaged VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 4 - PSZ-HP","Electric Heat Pump","<65,000 Btu/h\n(cooling capacity)",null,"System 4 - PSZ-HP<65,000 Btu/h\n(cooling capacity)","6.6 HSPF"]
[null,null,"System 4 - PSZ-HP","System 4 - PSZ-HP","System 1 (District Heating & Cooling) - 4-pipe Fan Coil",null,"System 10 - Heating and Ventilation","System 1 (District Heating & Cooling) - 4-pipe Fan Coil","System 5 (District Heating & Cooling) - Change to System 7 - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 4 - PSZ-HP",null,"≥65,000 Btu/h and\n<135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air",null,"System 4 - PSZ-HP≥65,000 Btu/h and\n<135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air","3.2 COP"]
[null,null,"System 5 - Packaged VAV with Reheat","System 4 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 1 (District Heating) - PTAC",null,"System 3 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 2 - PTHP","System 6 - Packaged VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 4 - PSZ-HP",null,"≥135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air",null,"System 4 - PSZ-HP≥135,000 Btu/h\n(cooling capacity)\n47°F db/43°F wb\noutdoor air","3.1 COP"]
[null,null,"System 6 - Packaged VAV with PFP Boxes","System 9 - Heating and Ventilation","System 1 (District Heating & Cooling) - 4-pipe Fan Coil",null,"System 4 (District Cooling) - 2-pipe CV AHU with Fossil Fuel Furnace","System 2 (District Cooling) - 4-pipe Fan Coil with HW Boiler","System 6 (District Cooling) - Change to System 8 - VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 5 - Packaged VAV with Reheat","Boilers, gas fired","<300,000 Btu/h",null,{"$f":"Y43&AA43","v":"System 5 - Packaged VAV with Reheat<300,000 Btu/h"},"82% AFUE"]
[null,null,"System 1 (District Heating) - PTAC",null,"System 2 - PTHP",null,null,"System 9 - Heating and Ventilation","System 7 - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 5 - Packaged VAV with Reheat",null,"≥300,000 Btu/h and\n≤2,500,000 Btu/h",null,"System 5 - Packaged VAV with Reheat≥300,000 Btu/h and\n≤2,500,000 Btu/h","80% Et"]
[null,null,"System 3 (District Heating) - PSZ-AC with District Heating",null,"System 2 (District Cooling) - 4-pipe Fan Coil with HW Boiler",null,null,"System 9 - Heating and Ventilation","System 7 (District Cooling) - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 5 - Packaged VAV with Reheat",null,">2,500,000 Btu/h",null,"System 5 - Packaged VAV with Reheat>2,500,000 Btu/h","82% Ec"]
[null,null,"System 5 (District Heating) - Packaged VAV with Reheat",null,"System 9 - Heating and Ventilation",null,null,"System 9 (District Heating) - Heating and Ventilation","System 7 (District Heating) - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes","Electric Resistance","<65,000 Btu/h","All","System 6 - Packaged VAV with PFP Boxes<65,000 Btu/h"]
[null,null,null,null,"System 9 (District Heating) - Heating and Ventilation",null,null,"System 9 (District Heating) - Heating and Ventilation","System 7 (Heating & Cooling) - VAV with Reheat",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥65,000 Btu/h and\n<135,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥65,000 Btu/h and\n<135,000 Btu/h"]
[null,null,null,null,"System 10 - Heating and Ventilation",null,null,"System 10 - Heating and Ventilation","System 8 - VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥135,000 Btu/h and\n<240,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥135,000 Btu/h and\n<240,000 Btu/h"]
[null,null,null,null,null,null,null,"System 10 - Heating and Ventilation","System 8 (District Cooling)- VAV with PFP Boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥240,000 Btu/h and\n<760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥240,000 Btu/h and\n<760,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 6 - Packaged VAV with PFP Boxes",null,"≥760,000 Btu/h","All other","System 6 - Packaged VAV with PFP Boxes≥760,000 Btu/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 9 - Heating and Ventilation","Warm air furnace, gas-fired","<225,000 Btu/h",null,"System 9 - Heating and Ventilation<225,000 Btu/h","78% AFUE or 80% Et"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 9 - Heating and Ventilation","Warm air furnace, gas-fired","≥225,000 Btu/h",null,"System 9 - Heating and Ventilation≥225,000 Btu/h","80 %Ec"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 7 - VAV with Reheat","Boilers, gas fired","<300,000 Btu/h",null,"System 7 - VAV with Reheat<300,000 Btu/h","82% AFUE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 7 - VAV with Reheat",null,"≥300,000 Btu/h and\n≤2,500,000 Btu/h",null,"System 7 - VAV with Reheat≥300,000 Btu/h and\n≤2,500,000 Btu/h","80% Et"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 7 - VAV with Reheat",null,">2,500,000 Btu/h",null,"System 7 - VAV with Reheat>2,500,000 Btu/h","82% Ec"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 12 - SZ-CV-HW","Boilers, gas fired","<300,000 Btu/h",null,"System 12 - SZ-CV-HW<300,000 Btu/h","82% AFUE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 12 - SZ-CV-HW",null,"≥300,000 Btu/h and\n≤2,500,000 Btu/h",null,"System 12 - SZ-CV-HW≥300,000 Btu/h and\n≤2,500,000 Btu/h","80% Et"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"System 12 - SZ-CV-HW",null,">2,500,000 Btu/h",null,"System 12 - SZ-CV-HW>2,500,000 Btu/h","82% Ec"]

{"sheet":"District Energy Path 3","index":53,"n_rows":126,"n_cols":18,"rows_kept":126,"cut":false,"hidden":true,"merged":[[57,1,57,2],[57,6,57,15],[112,1,113,2],[112,3,112,4],[112,6,112,7],[112,8,114,8],[113,3,113,4],[113,6,113,7]]}
["Chilled Water Assumptions Used to Derive Average Efficiencies:"]
[]
[null,"3,000 Hours of CHW Plant Operation per year"]
[null,"1500 Equivalent full load hours of CHW operation per year"]
[null,"2 gpm/ton Chilled Water (ARI conditions)"]
[null,"90% fan motor efficiency for cooling tower"]
[null,"3 gpm/ton Chilled Water (ARI conditions)"]
[null,"Assume IPLV = Average chiller efficiency (kWh/ton-hr)"]
[null,"Assume 2-speed cooling towers use 38% of the energy that a 1-speed cooling tower would use"]
[null,"   (source: VSDs and their Effect on System Components (http://www.trane.com/Commercial/Uploads/PDF/ContinuingEducation/ENL_VSDsystemeffects_handouts.pdf)"]
[null,"Assume 50% of CHW pump power is used in primary loop, 50% in secondary loop"]
[null,"Assume average part-load performance of 72% for secondary CHW pumps riding the curve (up to 300 tons capacity)"]
[null,"Assume average part-load performance of 42% for secondary CHW pumps with VSD (above 300 tons capacity)"]
[]
[null,"Hours of Operation Assumed:"]
[null,null,"Total Annual Hours:",null,3000]
[null,null,"EFLH:",null,1500]
[]
[]
[null,null,null,"Chiller 1","Chiller 2","Chiller 3","PCHWP1","PCHWP2","PCHWP3+","SCHWP","CWP1","CWP2","CWP3+"]
[null,null,"1 Chiller",{"$f":"$E$16","v":3000},null,null,{"$f":"$E$16","v":3000},null,null,{"$f":"$E$16","v":3000},3000]
[null,null,"2 Chillers",{"$f":"$E$16","v":3000},{"$f":"40%*D21","v":1200},null,{"$f":"$E$16","v":3000},{"$f":"40%*G21","v":1200},null,3000,3000,{"$f":"40%*K21","v":1200}]
[null,null,"3 Chillers",{"$f":"$E$16","v":3000},{"$f":"50%*D22","v":1500},{"$f":"20%*D23","v":600},{"$f":"$E$16","v":3000},{"$f":"50%*G22","v":1500},{"$f":"20%*G23","v":600},3000,3000,{"$f":"50%*K22","v":1500},{"$f":"20%*K23","v":600}]
[]
[null,"ASHRAE 90.1 Appendix G requirement (assume Chiller Path A, Use IPLV)"]
[]
[null,"Cooling Tower Fans",38.200000000000003,"gpm/hp"]
[]
[null,null,"Calculated","kW/ton","=",3,"gpm/ton","/",{"$f":"C27","v":38.200000000000003},"gpm/hp","/",0.9,"fan motor efficiency",null,null,"x",0.746,"kW/hp"]
[null,null,{"$f":"3/38.2/90%*0.746","v":6.5095986038394421E-2},"kW/ton"]
[]
[null,null,"Calculated","kWh/ton-hr","=",{"$f":"C30","v":6.5095986038394421E-2},"kW/ton","x",0.38,"Average efficiency",null,"x",{"$f":"$E$16","v":3000},"Hours of Operation",null,"/",{"$f":"$E$17","v":1500},"Equivalent Full Load Hours of Operation"]
[null,null,{"$f":"F32*I32*M32/Q32","v":4.9472949389179753E-2},"kWh/ton-hr"]
[]
[]
[null,"CW Pump Power"]
[null,null,19,"W/gpm"]
[]
[null,null,"Calculated","kW/ton","-",{"$f":"C37","v":19},"W/gpm","x",3,"gpm/ton","/","1000 W/kW"]
[null,null,{"$f":"F39*I39/1000","v":5.7000000000000002E-2},"kW/ton"]
[]
[null,"Primary CHW Pump Power"]
[null,null,11,"W/gpm"]
[]
[null,null,"Calculated","kW/ton","-",{"$f":"C43","v":11},"W/gpm","x",2,"gpm/ton","/","1000 W/kW"]
[null,null,{"$f":"F45*I45/1000","v":2.1999999999999999E-2},"kW/ton"]
[]
[null,"Secondary CHW Pump Power"]
[null,null,11,"W/gpm"]
[]
[null,null,"Calculated","kW/ton","-",{"$f":"C49","v":11},"W/gpm","x",2,"gpm/ton","/","1000 W/kW"]
[null,null,{"$f":"F51*I51/1000","v":2.1999999999999999E-2},"kW/ton"]
[]
[null,"Chiller Type, Quantity, and Efficiency, and Pump Consumption"]
[null,"*Peak CHW Load assumes baseline chilled water system is 15% oversized, so it is 15% less than the chiller equipment thresholds in ASHRAE 90.1 Table 6.8"]
[null,null,"Oversize factor",1.1499999999999999,null,null,null,"*columns below include conversion factor of 0.2844 to convert from kWh/ton-hr to kWh/kWh",null,null,null,null,null,null,null,{"$f":"3413/12000","v":0.28441666666666665}]
[]
[null,"Min CHW Peak Load in this Range",null,null,null,null,"Average chilled water system efficiency Cooling Energy Input Ratio (kWh/kWh)",null,null,null,null,null,null,null,null,null,"Average COP"]
[null,"tons","kW","Qty Chillers","Type Chillers","IPLV (kW/kW)","Chillers","PCHWP1","PCHWP2","PCHWP3","SCHWP","CWP1","CWP2","CWP3","Tower Fans","Total:"]
[null,0,0,1,"Screw",5.5819999999999999,{"$f":"1/F60","v":0.1791472590469366},{"$f":"C$46*$G$21/$E$17*$P56","v":1.2514333333333332E-2},null,null,{"$f":"0.72*$C$52*$J$21/$E$17*$P56","v":9.0103199999999987E-3},{"$f":"$C$40/$D60*K$21/$E$17*$P56","v":3.2423500000000001E-2},null,null,{"$f":"$C$33*$P56","v":1.4070931355439208E-2},{"$f":"SUM(G60:O60)","v":0.24716634373570912},{"$f":"1/P60","v":4.0458582867143251}]
[null,{"$f":"75/$D$56","v":65.217391304347828},{"$f":"264/$D$56","v":229.56521739130437},1,"Screw",5.718,0.17488632388947184,{"$f":"C$46*$G$21/$E$17*$P56","v":1.2514333333333332E-2},null,null,{"$f":"0.72*$C$52*$J$21/$E$17*$P56","v":9.0103199999999987E-3},{"$f":"$C$40/$D61*K$21/$E$17*$P56","v":3.2423500000000001E-2},null,null,{"$f":"$C$33*$P56","v":1.4070931355439208E-2},0.24290540857824436,4.1168288752939866]
[null,{"$f":"150/$D$56","v":130.43478260869566},{"$f":"528/$D$56","v":459.13043478260875},1,"Screw",6.0640000000000001,0.16490765171503957,{"$f":"C$46*$G$21/$E$17*$P56","v":1.2514333333333332E-2},null,null,{"$f":"0.72*$C$52*$J$21/$E$17*$P56","v":9.0103199999999987E-3},{"$f":"$C$40/$D62*K$21/$E$17*$P56","v":3.2423500000000001E-2},null,null,{"$f":"$C$33*$P56","v":1.4070931355439208E-2},0.23292673640381209,4.2931954289109848]
[null,{"$f":"300/$D$56","v":260.86956521739131},{"$f":"1055/$D$56","v":917.39130434782612},2,"Screw",6.0640000000000001,0.16490765171503957,{"$f":"C$46/D63*$G$22/$E$17*$P56","v":6.2571666666666661E-3},{"$f":"C$46/D63*$H$22/$E$17*$P56","v":2.5028666666666662E-3},null,{"$f":"$C$52*0.42*$J$22/$E$17*$P56","v":5.2560199999999993E-3},{"$f":"$C$40/$D63*K$22/$E$17*$P56","v":1.621175E-2},{"$f":"$C$40/$D63*L$22/$E$17*$P56","v":6.4846999999999995E-3},null,{"$f":"$C$33*$P56","v":1.4070931355439208E-2},0.21569108640381213,4.6362602028338893]
[null,{"$f":"600/$D$56","v":521.73913043478262},{"$f":"2110/$D$56","v":1834.7826086956522},2,"Centrifugal",5.9009999999999998,0.16946280291476021,{"$f":"C$46/D64*$G$22/$E$17*$P56","v":6.2571666666666661E-3},{"$f":"C$46/D64*$H$22/$E$17*$P56","v":2.5028666666666662E-3},null,{"$f":"$C$52*0.42*$J$22/$E$17*$P56","v":5.2560199999999993E-3},{"$f":"$C$40/$D64*K$22/$E$17*$P56","v":1.621175E-2},{"$f":"$C$40/$D64*L$22/$E$17*$P56","v":6.4846999999999995E-3},null,{"$f":"$C$33*$P56","v":1.4070931355439208E-2},0.22024623760353276,4.5403726796010426]
[null,{"$f":"1200/$D$56","v":1043.4782608695652},{"$f":"4220/$D$56","v":3669.5652173913045},3,"Centrifugal",6.4059999999999997,0.15610365282547611,{"$f":"C$46/D65*$G$23/$E$17*$P56","v":4.1714444444444438E-3},{"$f":"C$46/D65*$H$23/$E$17*$P56","v":2.0857222222222219E-3},{"$f":"C$46/D65*$I$23/$E$17*$P56","v":8.3428888888888891E-4},{"$f":"$C$52*0.42*$J$23/$E$17*$P56","v":5.2560199999999993E-3},{"$f":"$C$40/$D65*K$23/$E$17*$P56","v":1.0807833333333332E-2},{"$f":"$C$40/D$65*L$23/$E$17*$P56","v":5.4039166666666662E-3},{"$f":"$C$40/D$65*M$23/$E$17*$P56","v":2.1615666666666665E-3},{"$f":"$C$33*$P56","v":1.4070931355439208E-2},0.20089537640313757,4.977715355645099]
[]
[null,"BUILDING SPECIFIC DES CHW Average Efficiency:"]
[]
[null,null,"Building CHW Peak Baseline Load from PRM Outputs (use 1,200 tons if not yet entered, or if units are not entered for District Chilled Water Demand)"]
[null,null,{"$f":"IF(OR(SUMIF('12 - Performance_Outputs_1'!$R$209:$R$264,\"District Cooling\",'12 - Performance_Outputs_1'!$G$209:$G$264)=0,ISERROR(VLOOKUP(VLOOKUP(\"District Cooling\",'12 - Performance_Outputs_1'!$B$17:$H$18,5,FALSE),DemandTable,3,FALSE)/12)),1200,(SUMIF('12 - Performance_Outputs_1'!$R$209:$R$264,\"District Cooling\",'12 - Performance_Outputs_1'!$G$209:$G$264)*VLOOKUP(VLOOKUP(\"District Cooling\",'12 - Performance_Outputs_1'!$B$17:$H$18,5,FALSE),DemandTable,3,FALSE)/12))","v":1200},"tons"]
[]
[null,null,"Average CHW Plant Efficiency for Project based on Building CHW Peak Load (includes chillers, cooling towers, condenser water pumps and chilled water pumps)"]
[null,null,{"$f":"IF(ISERROR(VLOOKUP($C$70,DESBaseCHWTable,16)),$Q$65,VLOOKUP($C$70,DESBaseCHWTable,16))","v":4.977715355645099},"COP"]
[]
["Hot Water Assumptions Used to Derive Average Efficiencies:"]
[]
[null,"3,000 Hours of HHW Plant Operation per year"]
[null,"1500 Equivalent full load hours of HHW operation per year"]
[null,"40 gpm / (Btuh*10^6) hot water flow (or 0.1366 gpm/kW) (based on 50 deg. loop delta T required by ASHRAE 90.1-2010)"]
[null,"Assume Average thermal efficiency (including part-load operation) = AFUE = Et = Ec)"]
[null,"Assume average part-load performance of 72% for secondary CHW pumps riding the curve (up to 300 tons capacity)"]
[null,"Assume average part-load performance of 42% for secondary CHW pumps with VSD (above 300 tons capacity)"]
[null,"Assume a capacity of 300,000 Btuh is roughly equivalent to a building size of 120,000 square feet (to allow average efficiency based on capacity range only rather than building size)"]
[]
[]
[null,"Relevant ASHRAE 90.1-2010 Requirements:"]
[null,"19 W/gpm pump power"]
[null,"Variable primary pumping"]
[null,"Variable speed pumps for buildings with 120,000 square feet or more"]
[null,"Riding the pump curve for buildings less than 120,000 square feet"]
[]
[null,"Boiler Efficiencies:"]
[null,"Gas-Fired:","<300,000 Btuh","80% AFUE"]
[null,null,"300,000 to 2,500,000","80% Et"]
[null,null,">=2500000","82% Ec"]
[]
[null,"Oil-Fired:","<300,000 Btuh","80% AFUE"]
[null,null,"300,000 to 2,500,000","82% Et"]
[null,null,">=2500000","84% Ec"]
[]
[]
[null,"HHW Pump Power"]
[null,null,19,"W/gpm"]
[null,null,"."]
[null,null,"Calculated","kW/kW","=",{"$f":"C103","v":19},"W/gpm","x",0.1366,"gpm/kW","/","1000 W/kW"]
[null,null,{"$f":"F105*I105/1000","v":2.5954000000000003E-3},"kW/kW"]
[]
[]
[null,"Boiler and HHW Loop Pump Average Efficiency"]
[null,"*Peak HHW Load assumes baseline HHW water system is 25% oversized, so it is 25% less than the chiller equipment thresholds in ASHRAE 90.1 Table 6.8"]
[null,null,"Oversize factor",1.25]
[]
[null,"Min HHW Peak Load in this Range",null,"Average Fuel Efficiency",null,"Average Pump Efficiency \n(electricity kWh/chilled water kWh)","Average Fuel COP",null,"Average Electrical COP"]
[null,null,null,"Fuel-type",null,"PHHWP","Fuel-type"]
[null,"Btuh","kW","Gas-Fired","Oil-Fired",null,"Gas-Fired","Oil-Fired"]
[null,0,0,0.8,0.8,{"$f":"$C$106*3000/1500*0.72","v":3.7373760000000002E-3},{"$f":"D116","v":0.8},0.8,{"$f":"1/F116","v":267.5674055808139}]
[null,{"$f":"300000/$D$111","v":240000},88,0.8,0.82,{"$f":"$C$106*3000/1500*0.42","v":2.1801360000000001E-3},0.8,0.82,{"$f":"1/F117","v":458.68698099568098}]
[null,{"$f":"2500000/$D$111","v":2000000},733,0.82,0.84,{"$f":"$C$106*3000/1500*0.42","v":2.1801360000000001E-3},0.82,0.84,{"$f":"1/F118","v":458.68698099568098}]
[]
[null,"BUILDING SPECIFIC DES Heating Average Efficiency:"]
[]
[null,null,"Building Heating Peak Baseline Load from PRM Outputs (use 2,000,000 Btuh if not yet entered, or if units are not entered for District Heating Demand)"]
[null,null,{"$f":"IF(SUMIF('12 - Performance_Outputs_1'!$R$209:$R$264,\"District Hot Water\",'12 - Performance_Outputs_1'!$G$209:$G$264)+SUMIF('12 - Performance_Outputs_1'!$R$209:$R$264,\"District Steam\",'12 - Performance_Outputs_1'!$G$209:$G$264)=0,3000000,IF(ISERROR(VLOOKUP(VLOOKUP(\"District Hot Water\",'12 - Performance_Outputs_1'!$B$17:$H$18,5,FALSE),DemandTable,3,FALSE)),IF(ISERROR(VLOOKUP(VLOOKUP(\"District Steam\",'12 - Performance_Outputs_1'!$B$17:$H$18,5,FALSE),DemandTable,3,FALSE)),3000000,(SUMIF('12 - Performance_Outputs_1'!$R$209:$R$264,\"District Steam\",'12 - Performance_Outputs_1'!$G$209:$G$264)*(VLOOKUP(VLOOKUP(\"District Steam\",'12 - Performance_Outputs_1'!$B$17:$H$18,5,FALSE),DemandTable,3,FALSE))/VLOOKUP(\"Btuh\",DemandTable,3,FALSE))),(SUMIF('12 - Performance_Outputs_1'!$R$209:$R$264,\"District Hot Water\",'12 - Performance_Outputs_1'!$G$209:$G$264)*(VLOOKUP(VLOOKUP(\"District Hot Water\",'12 - Performance_Outputs_1'!$B$17:$H$18,5,FALSE),DemandTable,3,FALSE))/VLOOKUP(\"Btuh\",DemandTable,3,FALSE))))","v":3000000},"Btuh"]
[]
[null,null,"Average District Heating Plant Efficiency for Project based on Building District Heating Peak Load (includes boilers, pumps). Use Max efficiency if central plant fuel source isn't defined, or maximum capacity is not listed."]
[null,null,{"$f":"(IF(ISERROR(VLOOKUP('12 - Performance_Outputs_1'!$B$308,DropdownData!$B$2:$D$14,3,FALSE)),$H$118,IF(VLOOKUP('12 - Performance_Outputs_1'!$B$308,DropdownData!$B$2:$D$14,3,FALSE)=\"Yes\",IF(ISERROR(VLOOKUP($C$123,DESBaseHHWTable,6)),$H$118,VLOOKUP($C$123,DESBaseHHWTable,6)),IF(ISERROR(VLOOKUP($C$123,DESBaseHHWTable,7)),$H$118,VLOOKUP($C$123,DESBaseHHWTable,7)))))","v":0.84},"Average Fuel COP",null,{"$f":"IF(ISERROR(VLOOKUP($C$123,DESBaseHHWTable,8)),$I$118,VLOOKUP($C$123,DESBaseHHWTable,8))","v":458.68698099568098},"Average Electrical COP"]